**3GPP TSG-CT3 Meeting #122e C3-223734**

**E-Meeting, 12th – 20th May 2022**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **29.675** | **CR** | **0032** | **rev** | **-** | **Current version:** | **17.5.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **x** |

|  |
| --- |
|  |
| ***Title:***  | Update of info and externalDocs fields |
|  |  |
| ***Source to WG:*** | Ericsson |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | TEI17 |  | ***Date:*** | 2022-05-20 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | No CRs modifying Nucmf\_Provisioning API have been agreed during CT3#121e and CT3#122e meetings. However, since the present release will be frozen for OpenAPI, the API version number needs to be modified in accordance with the rules specified in TS 29.501, clause 4.3.1.As a draft version number was already assigned for the present release, only the additional Pre-Release version field needs to be removed.Since a new TS version will be provided with changes to the OpenAPI specification file, the TS version number included in the "description" field of the "externalDocs" object also needs to be updated. |
|  |  |
| ***Summary of change:*** | The Nucmf\_Provisioning API version number set to value "1.1.0".The TS version number in the "description" field of the "externalDocs" object is changed to "17.6.0". |
|  |  |
| ***Consequences if not approved:*** | Incorrect API version number and incorrect TS version number in the "description" field of the "externalDocs" object. |
|  |  |
| ***Clauses affected:*** | A.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\*\*\* First Change \*\*\*

# A.2 Nucmf\_Provisioning API

openapi: 3.0.0

info:

 title: Nucmf\_Provisioning

 version: 1.1.0

 description: |

 UCMF\_Provisioning Service.

 © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: >

 3GPP TS 29.675 V17.6.0; User Equipment (UE) radio capability provisioning service; Stage 3.

 url: https://www.3gpp.org/ftp/Specs/archive/29\_series/29.675/

servers:

 - url: '{apiRoot}/nucmf-provisioning/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in clause 4.4 of 3GPP TS 29.501

security:

 - {}

 - oAuth2ClientCredentials:

 - nucmf-provisioning

paths:

 /provisionings:

 post:

 summary: Create an Individual UE radio capability provisioning

 operationId: CreateProvisioning

 tags:

 - UE radio capability provisionings (Collection)

 requestBody:

 description: Create new provisionings for a given SCS/AS.

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/RacsData'

 responses:

 '201':

 description: >

 Created. The creation of an Individual UE radio capability provisioning

 resource is confirmed and a representation of that resource is returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/RacsData'

 headers:

 Location:

 description: Contains the URI of the newly created resource.

 required: true

 schema:

 type: string

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 description: The RACS data for all RACS IDs were not provisioned successfully.

 content:

 application/json:

 schema:

 type: array

 items:

 $ref: 'TS29122\_RacsParameterProvisioning.yaml#/components/schemas/RacsFailureReport'

 minItems: 1

 application/problem+json:

 schema:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/ProblemDetails'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 /provisionings/{provisioningId}:

 parameters:

 - name: provisioningId

 in: path

 description: Provisioning ID

 required: true

 schema:

 type: string

 get:

 summary: Get an Individual UE radio capability provisioning

 operationId: GetProvisioning

 tags:

 - Individual UE radio capability provisioning (Document)

 responses:

 '200':

 description: OK. The provisioning information related to the request URI is returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/RacsData'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/406'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 patch:

 summary: Update (PATCH) an Individual UE radio capability provisioning

 operationId: UpdateProvisioning

 tags:

 - Individual UE radio capability provisioning (Document)

 requestBody:

 description: Update an existing parameter provisioning.

 required: true

 content:

 application/merge-patch+json:

 schema:

 $ref: '#/components/schemas/RacsDataPatch'

 responses:

 '200':

 description: >

 OK. The Individual UE radio capability provisioning resource is modified

 and a representation of that resource is returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/RacsData'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 description: The RACS data for all RACS IDs were not provisioned successfully.

 content:

 application/json:

 schema:

 type: array

 items:

 $ref: 'TS29122\_RacsParameterProvisioning.yaml#/components/schemas/RacsFailureReport'

 minItems: 1

 application/problem+json:

 schema:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/ProblemDetails'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 put:

 summary: Replace (PUT) an Individual UE radio capability provisioning

 operationId: ReplaceProvisioning

 tags:

 - Individual UE radio capability provisioning (Document)

 requestBody:

 description: Update an existing parameter provisioning.

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/RacsData'

 responses:

 '200':

 description: >

 OK. The Individual UE radio capability provisioning resource is modified and a

 representation of that resource is returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/RacsData'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 description: The RACS data for all RACS IDs were not provisioned successfully.

 content:

 application/json:

 schema:

 type: array

 items:

 $ref: 'TS29122\_RacsParameterProvisioning.yaml#/components/schemas/RacsFailureReport'

 minItems: 1

 application/problem+json:

 schema:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/ProblemDetails'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 delete:

 summary: Remove an Individual UE radio capability provisioning

 operationId: RemoveProvisioning

 tags:

 - Individual UE radio capability provisioning (Document)

 responses:

 '204':

 description: >

 No Content. The Individual UE radio capability resource was successfully removed.

 The payload body shall be empty.

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{tokenUrl}'

 scopes:

 nucmf-provisioning: Access to the Nucmf\_Provisioning API

 schemas:

 RacsData:

 description: Represents a UE radio capability data provided by the NF service consumer.

 type: object

 properties:

 suppFeat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 racsConfigs:

 type: object

 additionalProperties:

 $ref: 'TS29122\_RacsParameterProvisioning.yaml#/components/schemas/RacsConfiguration'

 minProperties: 1

 description: >

 Identifies the configuration related to manufacturer specific UE radio capability.

 Each element uniquely identifies an RACS configuration for an RACS ID and is

 identified in the map via the RACS ID as key. The response shall include

 successfully provisioned RACS data.

 racsReports:

 type: object

 additionalProperties:

 $ref: 'TS29122\_RacsParameterProvisioning.yaml#/components/schemas/RacsFailureReport'

 minProperties: 1

 description: >

 Contains the RACS IDs for which the RACS data are not provisioned successfully. The

 failure reason is also included. Any string value can be used as a key of the map.

 readOnly: true

 required:

 - racsConfigs

 RacsDataPatch:

 description: >

 Represents a modification of a UE radio capability data provided by the NF service

 consumer.

 type: object

 properties:

 racsConfigs:

 type: object

 additionalProperties:

 $ref: 'TS29122\_RacsParameterProvisioning.yaml#/components/schemas/RacsConfigurationRm'

 minProperties: 1

 description: >

 Identifies the configuration related to manufacturer specific UE radio

 capability. Each element uniquely identifies an RACS configuration for an RACS ID

 and is identified in the map via the RACS ID as key.

\*\*\* End of Changes \*\*\*