**3GPP TSG-CT3 Meeting #122e C3-223106**

**E-Meeting, 12th – 20th May 2022 *(revison of C3-222452)***

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **29.507** | **CR** | **0213** | **rev** | **2** | **Current version:** | **17.6.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Correction to access stratum time distribution |
|  |  |
| ***Source to WG:*** | Huawei |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | IIoT |  | ***Date:*** | 2022-05-20 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | Current description does not indicate the condition where the PCF removes the access stratum time distribution from the AMF and the behaviour of the AMF to remove the access stratum time distribution from the NG-RAN. As the PCF may receives multiple access stratum time distribution parameters for a UE, the PCF shall remove the access stratum time distribution parameters from the AMF when all the access stratum time distribution parameters for the UE are removed. |
|  |  |
| ***Summary of change:*** | Describe the condition where the PCF removes the access stratum time distribution from the AMF and the behaviour of the AMF to remove the access stratum time distribution from the NG-RAN. |
|  |  |
| ***Consequences if not approved:*** | Incompleted specification. |
|  |  |
| ***Clauses affected:*** | 4.2.2.1, 4.2.2.3.6, 4.2.4.2, 5.6.2.10 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR doesn’t impact the OpenAPI file. |
|  |  |
| ***This CR's revision history:*** | C3-222452 agreed in CT3#121e is revised:Clarify that if the PCF receives the removal of the access stratum time distribution parameters from the TSCTSF and all the access stratum time distribution parameters for the UE are removed the PCF shall provide the "asTimeDisParam" attribute set to NULL.Undo the change for the the 5G access stratum time distribution in clause 4.2.2.3.6 and 4.2.4.2 |

\* \* \* \* Start of Changes \* \* \* \*

#### 4.2.2.1 General

The procedure in the present subclause is applicable when the NF service consumer (e.g. AMF) creates an AM policy association when the UE registers to the network, and when the AMF is relocated (between the different AMF sets) and the new AMF selects a new PCF. The procedure for the case where the AMF is relocated and the new AMF selects the old PCF is defined in subclause 4.2.3.1.

The creation of an AM policy association only applies for normally registered UEs, i.e., it does not apply for Emergency Registered UEs.

Figure 4.2.2.1-1 illustrates the creation of a policy association.



Figure 4.2.2.1-1: Creation of a policy association

When a UE registers and a UE context is being established, the AMF can obtain Service Area Restrictions, RFSP index, subscribed UE-AMBR, subscribed UE-Slice-MBR(s) and GPSI(s) from the UDM during the Access and Mobility Subscription Data retrieval procedure, the list of NWDAF instance IDs used for the UE and their associated Analytic ID(s) consumed by the AMF and the allowed NSSAI and the Target NSSAI from local configuration or from the NSSF during the slice selection procedure and shall decide based on local policies whether to request policies from the PCF.

To request policies from the PCF, the NF service consumer (e.g. AMF) shall send an HTTP POST request with: "{apiRoot}/npcf-am-policy-control/v1/policies" as Resource URI and the PolicyAssociationRequest data structure as request body that shall include:

- Notification URI encoded as "notificationUri" attribute;

- SUPI encoded as "supi" attribute; and

- if the feature "SliceSupport" or the feature "DNNReplacementControl" is supported in the NF service consumer and the UE is registered via a 3GPP access, the allowed NSSAI in the 3GPP access encoded in the "allowedSnssais" attribute;

and that shall include when available:

- GPSI encoded as "gpsi" attribute;

- if the feature "MultipleAccessTypes" is not supported, the access type encoded as "accessType" attribute;

NOTE 1: In this Release, for SNPN-enabled UE registered in the SNPN, direct access to the SNPN is specified for 3GPP access only.

- Permanent Equipment Identifier (PEI) encoded as "pei" attribute;

- User Location Information encoded as "userLoc" attribute;

- UE Time Zone encoded as "timeZone" attribute;

- the identifier of the serving network (the PLMN Identifier or the SNPN Identifier)encoded as "servingPlmn" attribute;

NOTE 2: The SNPN Identifier consists of the PLMN Identifier and the NID.

- if the feature "MultipleAccessTypes" is not supported, the RAT type encoded as "ratType" attribute;

- Service Area Restrictions (see subclause 4.2.2.3.1) derived from the Service Area Restrictions obtained from the UDM by mapping any service areas denoted by geographical information into Tracking Area Identities (TAIs) and encoded as "servAreaRes" attribute;

- RFSP index (see subclause 4.2.2.3.2) as obtained from the UDM encoded as "rfsp" attribute;

- a list of Internal Group Identifiers encoded as "groupIds" attribute;

- if the NF service consumer is an AMF, the GUAMI encoded as "guami" attribute;

- if the NF service consumer is an AMF, the name of a service produced by the AMF that expects to receive information within Npcf\_AMPolicyControl\_UpdateNotify service operation encoded as "serviceName" attribute;

- Alternate or backup IPv4 Address(es) where to send Notifications encoded as "altNotifIpv4Addrs" attribute;

- Alternate or backup IPv6 Address(es) where to send Notifications encoded as "altNotifIpv6Addrs" attribute;

- Alternate or backup FQDN(s) where to send Notifications encoded as "altNotifFqdns" attribute;

- trace control and configuration parameters information encoded as "traceReq" attribute;

- if the feature "UE-AMBR\_Authorization" is supported in the NF service consumer, the subscribed UE-AMBR (see subclause 4.2.2.3.3) in the "ueAmbr" attribute;

- if the feature "DNNReplacementControl" is supported, the mapping of each S-NSSAI of the Allowed NSSAI to the corresponding S-NSSAI of the HPLMN encoded in the "mappingSnssais" attribute;

- if the feature "UE-Slice-MBR\_Authorization" is supported in the NF service consumer, the subscribed UE-Slice-MBR(s) for the allowed NSSAI (see subclause 4.2.2.3.5) in the "ueSliceMbrs" attribute; and.

- when the "EneNA" feature is supported, the list of NWDAF instance IDs used for the UE within the "nwdafInstanceIds" and their associated Analytic ID(s) within "nwdafEvents" consumed by the NF service consumer, included within the "nwdafDatas" attribute; and

- if the feature "TargetNSSAI" is supported in the NF service consumer, the Target NSSAI generated by the NF service consumer or received from the NSSF encoded in the "targetSnssais" attribute.Upon the reception of this HTTP POST request, the PCF shall:

- assign a policy association ID;

- determine the applicable policy (taking into consideration and optionally modifying the possibly received UE-AMBR, UE-Slice-MBR(s) for the allowed NSSAI, Service Area Restrictions and/or RFSP index);

- for the successful case, send a HTTP "201 Created" response with the URI for the created resource in the "Location" header field

NOTE 3: The assigned policy association ID is part of the URI for the created resource and is thus associated with the SUPI.

and the PolicyAssociation data type as response body including:

- conditionally AMF Access and Mobility Policy (see subclause 4.2.2.3), i.e.:

a) if the PCF received the "servAreaRes" attribute in the request, Service Area Restrictions encoded as "servAreaRes" attribute; and/or

b) if the PCF received the "rfsp" attribute in the request, RAT Frequency Selection Priority (RFSP) Index encoded as "rfsp" attribute; and/or

c) if the feature "UE-AMBR\_Authorization" is supported and the PCF received the "ueAmbr" attribute in the request, the authorized UE-AMBR encoded as "ueAmbr" attribute;

d) if the feature "UE-Slice-MBR\_Authorization" is supported and the PCF received the "ueSliceMbrs" attribute in the request, the authorized UE-Slice-MBR(s) for the allowed NSSAI encoded as "ueSliceMbrs" attribute; and/or

e) if the feature "AMInfluence" is supported, the PCF for the UE determines that the access and mobility policies may be influenced by the traffic of PDU session(s) and local operator policies indicate that the PCF for the UE shall subscribe with the PCF for the PDU session for established/terminated PDU session(s) event notifications via the AMF and the SMF, the PCF for the UE information within the "pcfUeInfo" attribute, and the DNN and S-NSSAI of the concerned PDU session(s) within the "matchPdus" attribute. The "pcfUeInfo" attribute shall include the PCF for the UE callback URI via which the PCF(s) for the PDU session shall send notifications about the related PDU session(s) established/terminated events within the "callbackUri" attribute, and if available, the associated PCF for the UE instance ID, PCF set ID, and the level of SBA binding within the "bindingInfo" attribute;

f) if the feature "5GAccessStratumTime" is supported and the PCF receives the access stratum time distribution parameters from the TSCTSF as defined in 3GPP TS 29.534 [31], the 5G access stratum time distribution parameters encoded as "asTimeDisParam" attribute as defined in subclause 4.2.2.3.6;

- optionally one or several of the following Policy Control Request Trigger(s) encoded as "triggers" attribute (see subclause 4.2.3.2):

a) Location change (tracking area);

b) Change of UE presence in PRA;

c) if the "SliceSupport" feature or the "DNNReplacementControl" feature is supported, change of allowed NSSAI;

d) if the "DNNReplacementControl" feature is supported, change of SMF selection information; and

e) if the "EneNA" feature is supported, change of NWDAF data;

f) if the "TargetNSSAI" feature is supported, Generation of Target NSSAI; and

- if the Policy Control Request Trigger "Change of UE presence in PRA" is provided, the presence reporting areas for which reporting is required encoded as "pras" attribute;

NOTE 4: If the PCF uses a Presence Reporting Area identifier referring to a Set of Core Network predefined Presence Reporting Areas as defined in 3GPP TS 23.501 [2], the PCF includes the identifier of this Presence Reporting Area set within the "praId" attribute.

- if the Policy Control Request Trigger "Change of SMF selection information" is provided, the SMF selection information representing the conditions upon which the AMF shall request a DNN replacement (see subclause 4.2.2.3.4) encoded as "smfSelInfo" attribute;

- if the Policy Control Request Trigger "Generation of Target NSSAI" is provided, the RFSP Index associated with the Target NSSAI encoded as "targetRfsp" attribute;

Editor’s note: It is FFS whether the PCF can subscribe to the "Generation of Target NSSAI" Trigger when the "targetRfsp" attribute is provided in the response to the AM Policy Association creation.

- if errors occur when processing the HTTP POST request, apply error handling procedures as specified in subclause 5.7 and according to the following provisions:

- if the user information received within the "supi" attribute is unknown, the PCF shall reject the request and include in an HTTP "400 Bad Request" response message the "cause" attribute of the ProblemDetails data structure set to "USER\_UNKNOWN";

- if the PCF is, due to incomplete, erroneous or missing information in the request, not able to provision an AM policy decision, the PCF may reject the request and include in an HTTP "400 Bad Request" response message the "cause" attribute of the ProblemDetails data structure set to "ERROR\_REQUEST\_PARAMETERS".

- if the PCF rejects the AM policy association establishment, the NF service consumer shall apply the policy retrieved from the UDM if available; otherwise, the NF service consumer shall apply the operator configured policy.

If the PCF received a GUAMI, the PCF may subscribe to GUAMI changes using the AMFStatusChange service operation of the Namf\_Communication service specified in 3GPP TS 29.518 [14], and it may use the Nnrf\_NFDiscovery Service specified in 3GPP TS 29.510 [13] (using the obtained GUAMI and possibly service name) to query the other AMFs within the AMF set.

If the PCF received a "traceReq" attribute, it shall perform trace procedures as defined in 3GPP TS 32.422 [18].

If the PCF received the list of NWDAF instance IDs used for the UE in "nwdafInstanceIds" attribute and their associated Analytic IDs in "nwdafEvents" attribute included within the "nwdafDatas" attribute the PCF may select those NWDAF instances as described in 3GPP TS 29.513 [7].

The PCF may retrieve AF requirements on Access and Mobility policies from the UDR as specified in 3GPP TS 29.519 [17] and consider them for determining the Access and Mobility policies to be provisioned.

\* \* \* \* Next change \* \* \* \*

##### 4.2.2.3.6 5G access stratum time distribution

If the feature "5GAccessStratumTime" is supported and the PCF receives the access stratum time distribution parametersfrom the TSCTSF as defined in 3GPP TS 29.534 [31], the 5G access stratum time distribution parameters are encoded using the "asTimeDisParam" attribute of the "AsTimeDistributionParam" data type, which consists of:

* an indication of whether the 5G access stratum time distribution is enabled encoded in the "asTimeDistInd" attribute if applicable; and
* the Uu Time synchronization error budget encoded in the "uuErrorBudget" if applicable.

If the PCF receives the removal of the access stratum time distribution parameters from the TSCTSF as defined in 3GPP TS 29.534 [26] and there are no other AS time distribution parameters from other requests for the same UE, the PCF shall provide the "asTimeDisParam" attribute set to NULL.

\* \* \* \* Next change \* \* \* \*

#### 4.2.4.2 Policy update notification

Figure 4.2.4.2-1 illustrates the policy update notification.



Figure 4.2.4.2-1: policy update notification

The PCF may decide to update policy control request trigger(s) and/or Access and Mobility policies related to an Individual AM Policy Association, e.g. in response to information provided to the PCF via the Npcf\_AMPolicyAuthorization service (see 3GPP TS 29.534 [26]), to notification provided by the Nbsf\_Management Service about the registration/deregistration of the PCF for a PDU session (see 3GPP TS 29.521 [30]) or to notifications provided by the Npcf\_PolicyAuthorization service (see 3GPP TS 29.514 [25]), in response to a notification received from UDR about new or updated AF requirements on Access and Mobility polices (see 3GPP TS 29.519 [17]), or in response to an internal trigger within the PCF. The PCF shall send for this purpose an HTTP POST request with "{notificationUri}/update" as URI (where the Notification URI was previously supplied by the NF service consumer) and the PolicyUpdate data structure as request body encoded as described in subclause 4.2.3.3.

Upon the reception of the HTTP POST request, the NF service consumer shall enforce the received updated policy.

In case of a successful update notification:

- if the feature "ImmediateReport" is supported and the PCF provisioned the policy control request triggers related to access type change, PRA change, allowed NSSAI change or location change, a "200 OK" response code and a response body with the corresponding available information in the "AmRequestedValueRep" data structure shall be returned in the response;

- otherwise, a "204 No Content" response code shall be returned in the response.

If errors occur when processing the HTTP POST request, the NF service consumer shall send an HTTP error response as specified in subclause 5.7.

If the feature "ES3XX" is supported, and the NF service consumer determines the received HTTP POST request needs to be redirected, the NF service consumer shall send an HTTP redirect response as specified in subclause 6.10.9 of 3GPP TS 29.500 [5].

If the AMF as NF service consumer is not able to handle the notification but knows by implementation specific means that another AMF is able to handle the notification, it shall reply with an HTTP "307 Temporary redirect" response pointing to the URI of the new AMF. If the AMF is not able to handle the notification but another unknown AMF could possibly handle the notification, it shall reply with an HTTP "404 Not found" error response.

If the PCF receives a "307 Temporary redirect" response, the PCF shall resend the failed policy update notification request using the received URI in the Location header field as Notification URI. Subsequent policy update notifications, triggered after the failed one, shall be sent to the Notification URI provided by the NF service consumer during the corresponding policy association creation/update.

If the PCF becomes aware that a new AMF is requiring notifications (e.g. via the "404 Not found" response, via Namf\_Communication service AMFStatusChange Notifications, see 3GPP TS 29.518 [14], or via link level failures), and the PCF knows alternate or backup IPv4, IPv6 Addess(es) or FQDN(s) where to send Notifications (e.g. via "altNotifIpv4Addrs", "altNotifIpv6Addrs" or "altNotifFqdns" attributes received when the policy association was created, via AMFStatusChange Notifications or via the Nnrf\_NFDiscovery Service specified in 3GPP TS 29.510 [13] (using the service name and GUAMI obtained during the creation of the subscription) to discover the other AMFs within the AMF set), the PCF shall exchange the authority part of the corresponding Notification URI with one of those addresses and shall use that URI in any subsequent communication.

If the PCF received a "404 Not found" response, the PCF should resend the failed policy update notification request to that URI.

If the feature "DNNReplacementControl" is supported and the AMF received the update of the SMF selection information within the "smfSelInfo" attribute in the request, the AMF shall apply the updated SMF selection information to the new PDU Sessions only, i.e. already established PDU Sessions are not affected.

If the feature "AMInfluence" is supported, the PCF determines that the access and mobility policies may be influenced by the traffic of a PDU session(s) based on an AF request, UDR notification or other internal policies, and local operator policies indicate the PCF for the UE shall subscribe with the PCF for the PDU session for established/terminated PDU session(s) event notifications, the PCF for the UE shall provision/update the AMF with the PCF for the UE information within the "pcfUeInfo" attribute and the complete list of S-NSSAI and DNN combinations within the "matchPdus" attribute. The AMF shall update the affected established PDU sesssions, forwarding the received PCF for the UE information for the PDU session(s) matching the new S-NSSAI and DNN combination(s), and removing the previously provided PCF for the UE information for the PDU session(s) matching the removed S-NSSAI and DNN combination(s).

When the feature "AMInfluence" is supported, and the SBA binding indication information for the PCF instance changes, the PCF may update the previously provided information in the AMF. The AMF shall apply the updated PCF callback information to the new PDU Sessions only, i.e., already established PDU sessions are not affected.

If the PCF changed the Service Area Restrictions as part of the policy update, it shall send notifications to any NF Service Consumer(s) (e.g. AF) that have subscribed to the related event by using the Npcf\_AMPolicyAuthorization service (see TS 29.534 [26]) and/or the Npcf\_EventExposure service ((see TS 29.523 [28]).

If the feature "5GAccessStratumTime" is supported and the PCF receives the access stratum time distribution parameters or removal of the access stratum time distribution parameters from the TSCTSF as defined in 3GPP TS 29.534 [31], the PCF may provision, update or remove the 5G access stratum time distribution parameters by provisioning the "asTimeDisParam" attribute as defined in subclause 4.2.2.3.6. The AMF shall provision the 5G access stratum time distribution parameters to the NG-RAN when receiving it from the PCF.

\* \* \* \* Next change \* \* \* \*

#### 5.6.2.10 Type: AsTimeDistributionParam

Table 5.6.2.10-1: Definition of type AsTimeDistributionParam

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| asTimeDistInd | boolean | O | 0..1 | When this attribute is included and set to true, it indicates that the access stratum time distribution via Uu reference point is activated. When present it shall be set as follows:- true: activated.- false (default): deactivated. |  |
| uuErrorBudget | Uinteger | O | 0..1 | Indicates the time synchronization error budget in terms of time units of nanoseconds. |  |

\* \* \* \* End of changes \* \* \* \*