**3GPP TSG- Meeting #**

**, , -**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  |  |
|  |  |
| ***Source to WG:*** | Nokia, Nokia Shanghai Bell, Ericsson |
| ***Source to TSG:*** | C3 |
|  |  |
| ***Work item code:*** |  |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | Although a resource may have more than one custom operation associated with it, the current data model allows for defining only one, while the only information that can currently be provided for this custom operation is its name, which may not be sufficient. |
|  |  |
| ***Summary of change:*** | Added a feature-dependent array to enable the modelling of more than one custom operations associated with a resource. |
|  |  |
| ***Consequences if not approved:*** | Inability to model certain 3gpp APIs and unclear specification. |
|  |  |
| ***Clauses affected:*** | 8.2.4.2.6, 8.2.4.2.7, 8.2.6, A.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR is a backwards compatible feature in the OpenAPI file of the CAPIF\_Publish\_Service API. |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* \* First change \* \* \* \*

#### 8.2.4.1 General

This clause specifies the application data model supported by the API. Data types listed in clause 7.2 also apply to this API.

Table 8.2.4.1-1 specifies the data types defined specifically for the CAPIF\_Publish\_Service\_API service.

Table 8.2.4.1-1: CAPIF\_Publish\_Service\_API specific Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Section defined | Description | Applicability |
| AefLocation | Clause 8.2.4.2.10 | Represents the location information (e.g. civic address, GPS coordinates, data center ID) where the AEF providing the service API is located. |  |
| AefProfile | Clause 8.2.4.2.4 | Represents the AEF profile data. |  |
| CommunicationType | Clause 8.2.4.3.5 | Indicates a communication type of the resource or a custom operation. |  |
| CustomOperation | Clause 8.2.4.2.7 | Represents the description of a custom operation. |  |
| DataFormat | Clause 8.2.4.3.4 | Indicates a data format, e.g., JSON. |  |
| InterfaceDescription | Clause 8.2.4.2.3 | Represents the description of the API interface. |  |
| Operation | Clause 8.2.4.3.7 | Indicates an HTTP method (e.g. PUT). |  |
| Protocol | Clause 8.2.4.3.3 | Indicates a protocol and protocol version used by the API. |  |
| PublishedApiPath | Clause 8.2.4.2.9 | Represents the published API path within the same CAPIF provider domain. |  |
| Resource | Clause 8.2.4.2.6 | Represents the API resource data. |  |
| SecurityMethod | Clause 8.2.4.3.6 | Indicates the security method (e.g. PKI). |  |
| ServiceAPIDescription | Clause 8.2.4.2.2 | Represents the description of a service API as published by the APF. |  |
| ServiceAPIDescriptionPatch | Clause 8.2.4.2.11 | Represents the parameters to request the modification of an APF published API resource. | PatchUpdate |
| ShareableInformation | Clause 8.2.4.2.8 | Indicates whether the service API and/or the service API category can be shared to the list of CAPIF provider domains. |  |
| Version | Clause 8.2.4.2.5 | Represents the API version information |  |

Table 8.2.4.1-2 specifies data types re-used by the CAPIF\_Publish\_Service\_API service:

Table 8.2.4.1-2: Re-used Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Reference | Comments | Applicability |
| CivicAddress | 3GPP TS 29.572 [30] | Used to indicate a civic address. |  |
| DateTime | 3GPP TS 29.122 [14] | Used to indicate an expiration timer. |  |
| GeographicArea | 3GPP TS 29.572 [30] | Used to indicate a geographic area. |  |
| Ipv4Addr | 3GPP TS 29.122 [14] | Used to indicate an IPv4 address. |  |
| Ipv6Addr | 3GPP TS 29.122 [14] | Used to indicate an IPv6 address. |  |
| Port | 3GPP TS 29.122 [14] | Used to indicate a port. |  |
| SupportedFeatures | 3GPP TS 29.571 [19] | Used to negotiate the applicability of optional features defined in table 8.2.6-1. | ApiSupportedFeaturePublishing |

\* \* \* \* Next change \* \* \* \*

##### 8.2.4.2.6 Type: Resource

Table 8.2.4.2.6-1: Definition of type Resource

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| resourceName | string | M | 1 | Resource name. |  |
| commType | CommunicationType | M | 1 | Communication type used by the API resource. (NOTE 1) |  |
| uri | string | M | 1 | Relative URI of the API resource, it is set as {apiSpecificSuffixes} part of the URI structure as defined in clause 5.2.4 of 3GPP TS 29.122 [14]. |  |
| custOpName | string | O | 0..1 | it is set as {custOpName} part of the URI structure for the case where there is only a single custom operation associated with this resource as defined in clause 5.2.4 of 3GPP TS 29.122 [14]. (NOTE 2) |  |
| custOperations | array(CustomOperation) | O | 1..N | List of custom operations associated to this resource. (NOTE 2) | MultipleCustomOperations |
| operations | array(Operation) | C | 1..N | Supported HTTP methods for the API resource. Only applicable when the protocol in AefProfile indicates HTTP. |  |
| description | string | O | 0..1 | Text description of the API resource. |  |
| NOTE 1: The communication type refers to the semantics of the resource or custom operation and is independent of the HTTP methods that are supported (e.g. if a resource is used for subscriptions then its CommunicationType shall be SUBSCRIBE\_NOTIFY even if it supports also the GET method for retrieving the subscriptions).NOTE 2: The attributes "custOpName" and "custOperations" are mutually exclusive.  |

\* \* \* \* Next change \* \* \* \*

##### 8.2.4.2.7 Type: CustomOperation

Table 8.2.4.2.7-1: Definition of type CustomOperation

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| commType | CommunicationType | M | 1 | Communication type used by the custom operation. |  |
| custOpName | string | M | 1 | it is set as {custOpName} part of the URI structure for a custom operation without resource association as defined in clause 5.2.4 of 3GPP TS 29.122 [14]. |  |
| operations | array(Operation) | C | 1..N | Supported HTTP methods for the custom operation. Only applicable when the protocol in AefProfile indicates HTTP. |  |
| description | string | O | 0..1 | Text description of the custom operation. |  |

\* \* \* \* Next change \* \* \* \*

### 8.2.6 Feature negotiation

General feature negotiation procedures are defined in clause 7.8.

Table 8.2.6-1: Supported Features

|  |  |  |
| --- | --- | --- |
| **Feature number** | **Feature Name** | **Description** |
| 1 | ApiSupportedFeaturePublishing | Indicates the support of publishing with supported feature for a service API. |
| 2 | PatchUpdate | Indicates the support of the PATCH method for updating an APF published API resource. |
| X | MultipleCustomOperations | Indicates the support of modelling multiple custom operations associated with a resource. |

\* \* \* \* Next change \* \* \* \*

# A.3 CAPIF\_Publish\_Service\_API

openapi: 3.0.0

info:

 title: CAPIF\_Publish\_Service\_API

 description: |

 API for publishing service APIs.

 © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

 version: "1.2.1"

externalDocs:

 description: 3GPP TS 29.222 V17.6.0 Common API Framework for 3GPP Northbound APIs

 url: https://www.3gpp.org/ftp/Specs/archive/29\_series/29.222/

servers:

 - url: '{apiRoot}/published-apis/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in clause 7.5 of 3GPP TS 29.222.

paths:

# APF published API

 /{apfId}/service-apis:

 post:

 description: Publish a new API.

 parameters:

 - name: apfId

 in: path

 required: true

 schema:

 type: string

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ServiceAPIDescription'

 responses:

 '201':

 description: >

 Service API published successfully The URI of the created resource

 shall be returned in the "Location" HTTP header.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ServiceAPIDescription'

 headers:

 Location:

 description: >

 Contains the URI of the newly created resource, according to the structure

 {apiRoot}/published-apis/v1/{apfId}/service-apis/{serviceApiId}

 required: true

 schema:

 type: string

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 get:

 description: Retrieve all published APIs.

 parameters:

 - name: apfId

 in: path

 required: true

 schema:

 type: string

 responses:

 '200':

 description: Definition of all service API(s) published by the API publishing function.

 content:

 application/json:

 schema:

 type: array

 items:

 $ref: '#/components/schemas/ServiceAPIDescription'

 minItems: 0

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/406'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

# Individual APF published API

 /{apfId}/service-apis/{serviceApiId}:

 get:

 description: Retrieve a published service API.

 parameters:

 - name: serviceApiId

 in: path

 required: true

 schema:

 type: string

 - name: apfId

 in: path

 required: true

 schema:

 type: string

 responses:

 '200':

 description: >

 Definition of individual service API published by the API publishing function.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ServiceAPIDescription'

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/406'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 put:

 description: Update a published service API.

 parameters:

 - name: serviceApiId

 in: path

 required: true

 schema:

 type: string

 - name: apfId

 in: path

 required: true

 schema:

 type: string

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ServiceAPIDescription'

 responses:

 '200':

 description: Definition of service API updated successfully.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ServiceAPIDescription'

 '204':

 description: No Content

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 patch:

 description: Modify an existing published service API.

 operationId: ModifyIndAPFPubAPI

 tags:

 - Individual APF published API

 parameters:

 - name: serviceApiId

 in: path

 required: true

 schema:

 type: string

 - name: apfId

 in: path

 required: true

 schema:

 type: string

 requestBody:

 required: true

 content:

 application/merge-patch+json:

 schema:

 $ref: '#/components/schemas/ServiceAPIDescriptionPatch'

 responses:

 '200':

 description: >

 The definition of the service API is modified successfully and a

 representation of the updated service API is returned in the request body.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ServiceAPIDescription'

 '204':

 description: No Content. The definition of the service API is modified successfully.

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 delete:

 description: Unpublish a published service API.

 parameters:

 - name: serviceApiId

 in: path

 required: true

 schema:

 type: string

 - name: apfId

 in: path

 required: true

 schema:

 type: string

 responses:

 '204':

 description: The individual published service API matching the serviceAPiId is deleted.

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

# Components

components:

 schemas:

# Data Type for representations

 ServiceAPIDescription:

 type: object

 description: Represents the description of a service API as published by the APF.

 properties:

 apiName:

 type: string

 description: API name, it is set as {apiName} part of the URI structure as defined in clause 5.2.4 of 3GPP TS 29.122.

 apiId:

 type: string

 description: >

 API identifier assigned by the CAPIF core function to the published service API.

 Shall not be present in the HTTP POST request from the API publishing function

 to the CAPIF core function. Shall be present in the HTTP POST response from the

 CAPIF core function to the API publishing function and in the HTTP GET response

 from the CAPIF core function to the API invoker (discovery API).

 aefProfiles:

 type: array

 items:

 $ref: '#/components/schemas/AefProfile'

 minItems: 1

 description: >

 AEF profile information, which includes the exposed API details (e.g. protocol).

 description:

 type: string

 description: Text description of the API

 supportedFeatures:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 shareableInfo:

 $ref: '#/components/schemas/ShareableInformation'

 serviceAPICategory:

 type: string

 apiSuppFeats:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 pubApiPath:

 $ref: '#/components/schemas/PublishedApiPath'

 ccfId:

 type: string

 description: CAPIF core function identifier.

 required:

 - apiName

 InterfaceDescription:

 type: object

 description: Represents the description of an API's interface.

 properties:

 ipv4Addr:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv4Addr'

 ipv6Addr:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv6Addr'

 port:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Port'

 securityMethods:

 type: array

 items:

 $ref: '#/components/schemas/SecurityMethod'

 minItems: 1

 description: >

 Security methods supported by the interface, it take precedence over

 the security methods provided in AefProfile, for this specific interface.

 oneOf:

 - required: [ipv4Addr]

 - required: [ipv6Addr]

 AefProfile:

 type: object

 description: Represents the AEF profile data.

 properties:

 aefId:

 type: string

 description: Identifier of the API exposing function

 versions:

 type: array

 items:

 $ref: '#/components/schemas/Version'

 minItems: 1

 description: API version

 protocol:

 $ref: '#/components/schemas/Protocol'

 dataFormat:

 $ref: '#/components/schemas/DataFormat'

 securityMethods:

 type: array

 items:

 $ref: '#/components/schemas/SecurityMethod'

 minItems: 1

 description: Security methods supported by the AEF

 domainName:

 type: string

 description: Domain to which API belongs to

 interfaceDescriptions:

 type: array

 items:

 $ref: '#/components/schemas/InterfaceDescription'

 minItems: 1

 description: Interface details

 aefLocation:

 $ref: '#/components/schemas/AefLocation'

 required:

 - aefId

 - versions

 oneOf:

 - required: [domainName]

 - required: [interfaceDescriptions]

 Resource:

 type: object

 description: Represents the API resource data.

 properties:

 resourceName:

 type: string

 description: Resource name

 commType:

 $ref: '#/components/schemas/CommunicationType'

 uri:

 type: string

 description: >

 Relative URI of the API resource, it is set as {apiSpecificSuffixes} part

 of the URI structure as defined in clause 5.2.4 of 3GPP TS 29.122.

 custOpName:

 type: string

 description: >

 it is set as {custOpName} part of the URI structure for a custom operation

 associated with a resource as defined in clause 5.2.4 of 3GPP TS 29.122.

 custOperations:

 type: array

 items:

 $ref: '#/components/schemas/CustomOperation'

 minItems: 1

 description: >

 Custom operations associated with this resource.

 operations:

 type: array

 items:

 $ref: '#/components/schemas/Operation'

 minItems: 1

 description: >

 Supported HTTP methods for the API resource. Only applicable when the

 protocol in AefProfile indicates HTTP.

 description:

 type: string

 description: Text description of the API resource

 required:

 - resourceName

 - commType

 - uri

 CustomOperation:

 type: object

 description: Represents the description of a custom operation.

 properties:

 commType:

 $ref: '#/components/schemas/CommunicationType'

 custOpName:

 type: string

 description: >

 it is set as {custOpName} part of the URI structure for a custom operation

 without resource association as defined in clause 5.2.4 of 3GPP TS 29.122.

 operations:

 type: array

 items:

 $ref: '#/components/schemas/Operation'

 minItems: 1

 description: >

 Supported HTTP methods for the API resource. Only applicable when the

 protocol in AefProfile indicates HTTP.

 description:

 type: string

 description: Text description of the custom operation

 required:

 - commType

 - custOpName

 Version:

 type: object

 description: Represents the API version information.

 properties:

 apiVersion:

 type: string

 description: API major version in URI (e.g. v1)

 expiry:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

 resources:

 type: array

 items:

 $ref: '#/components/schemas/Resource'

 minItems: 1

 description: Resources supported by the API.

 custOperations:

 type: array

 items:

 $ref: '#/components/schemas/CustomOperation'

 minItems: 1

 description: Custom operations without resource association.

 required:

 - apiVersion

 ShareableInformation:

 type: object

 description: >

 Indicates whether the service API and/or the service API category can be shared

 to the list of CAPIF provider domains.

 properties:

 isShareable:

 type: boolean

 description: >

 Set to "true" indicates that the service API and/or the service API

 category can be shared to the list of CAPIF provider domain information.

 Otherwise set to "false".

 capifProvDoms:

 type: array

 items:

 type: string

 minItems: 1

 description: >

 List of CAPIF provider domains to which the service API information to be shared.

 required:

 - isShareable

 PublishedApiPath:

 type: object

 description: Represents the published API path within the same CAPIF provider domain.

 properties:

 ccfIds:

 type: array

 items:

 type: string

 minItems: 1

 description: A list of CCF identifiers where the service API is already published.

 AefLocation:

 description: >

 The location information (e.g. civic address, GPS coordinates, data center ID)

 where the AEF providing the service API is located.

 type: object

 properties:

 civicAddr:

 $ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/CivicAddress'

 geoArea:

 $ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/GeographicArea'

 dcId:

 type: string

 description: >

 Identifies the data center where the AEF providing the service API is located.

 ServiceAPIDescriptionPatch:

 type: object

 description: >

 Represents the parameters to request the modification of an APF published API resource.

 properties:

 aefProfiles:

 type: array

 items:

 $ref: '#/components/schemas/AefProfile'

 minItems: 1

 description:

 type: string

 description: Text description of the API

 shareableInfo:

 $ref: '#/components/schemas/ShareableInformation'

 serviceAPICategory:

 type: string

 apiSuppFeats:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 pubApiPath:

 $ref: '#/components/schemas/PublishedApiPath'

 ccfId:

 type: string

 description: CAPIF core function identifier.

 Protocol:

 anyOf:

 - type: string

 enum:

 - HTTP\_1\_1

 - HTTP\_2

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Possible values are:

 - HTTP\_1\_1: HTTP version 1.1

 - HTTP\_2: HTTP version 2

 CommunicationType:

 anyOf:

 - type: string

 enum:

 - REQUEST\_RESPONSE

 - SUBSCRIBE\_NOTIFY

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Possible values are:

 - REQUEST\_RESPONSE: The communication is of the type request-response

 - SUBSCRIBE\_NOTIFY: The communication is of the type subscribe-notify

 DataFormat:

 anyOf:

 - type: string

 enum:

 - JSON

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Possible values are:

 - JSON: JavaScript Object Notation

 SecurityMethod:

 anyOf:

 - type: string

 enum:

 - PSK

 - PKI

 - OAUTH

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Possible values are:

 - PSK: Security method 1 (Using TLS-PSK) as described in 3GPP TS 33.122

 - PKI: Security method 2 (Using PKI) as described in 3GPP TS 33.122

 - OAUTH: Security method 3 (TLS with OAuth token) as described in 3GPP TS 33.122

 Operation:

 anyOf:

 - type: string

 enum:

 - GET

 - POST

 - PUT

 - PATCH

 - DELETE

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Possible values are:

 - GET: HTTP GET method

 - POST: HTTP POST method

 - PUT: HTTP PUT method

 - PATCH: HTTP PATCH method

 - DELETE: HTTP DELETE method

\* \* \* \* End of changes \* \* \* \*