**3GPP TSG- WG3 Meeting #****125 C3-225245\_r1**

**Toulouse, France, - , November, 2022**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.522** | **CR** | **0752** | **rev** | **-** | **Current version:** | **17.7.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **x** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Enumeration definitions in the OpenAPI files | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Ericsson | | | | | | | | | |
| ***Source to TSG:*** | CT3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NBI18 | | | | |  | ***Date:*** | | | 2022-11-01 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | TS 29.122 specifies in clause 5.2.9.10 for the enumeration definition in the OpenAPI file that the schema:  - shall contain the "anyOf" keyword listing as alternatives:  1. the "type: string" keyword and the "enum" keyword with a list of all defined values for the enumeration; and  2. the "type: string" keyword and the "description" keyword with a description stating that the string is only provided for extensibility and is not used to encode contents defined in the present version of the specification. And  - may contain a description listing the defined values of the enumeration together with explanations of those values.  However, the OpenAPI files of the 5GLANParameterProvision, ServiceParameter and TimeSyncExposure APIs are not aligned with the above requirement from TS 29.122 i.e. in definitions of enumerations, descriptions of the string data type provided for forward compatibility with future extensions are incorrect. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Definitions of enumerations:  descriptions of the string data type provided for forward compatibility with future extensions corrected and specified in accordance with TS 29.122. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The OpenAPI files of the 5GLANParameterProvision, ServiceParameter and TimeSyncExposure APIs will remain not fully compliant with the OpenAPI requirements specified in TS 29.122. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | A.5, A.9, A.13 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR introduces backward compatible corrections to the OpenAPI files of the 5GLANParameterProvision, ServiceParameter and TimeSyncExposure APIs. | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

\*\*\* First Change \*\*\*

# A.5 5GLANParameterProvision API

openapi: 3.0.0

info:

title: 3gpp-5glan-pp

version: 1.1.1

description: |

API for 5G LAN Parameter Provision.

© 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: >

3GPP TS 29.522 V17.7.0; 5G System; Network Exposure Function Northbound APIs.

url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.522/'

security:

- {}

- oAuth2ClientCredentials: []

servers:

- url: '{apiRoot}/3gpp-5glan-pp/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 5.2.4 of 3GPP TS 29.122.

paths:

/{afId}/subscriptions:

get:

summary: read all of the active subscriptions for the AF

operationId: RealAllSubscriptions

tags:

- 5GLAN Parameters Provision Subscriptions

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

responses:

'200':

description: OK (Successful get all of the active subscriptions for the AF)

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/5GLanParametersProvision'

minItems: 0

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

post:

summary: Creates a new subscription resource

operationId: CreateAnSubscription

tags:

- 5GLAN Parameters Provision Subscriptions

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

requestBody:

description: new subscription creation

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/5GLanParametersProvision'

responses:

'201':

description: Created (Successful creation)

content:

application/json:

schema:

$ref: '#/components/schemas/5GLanParametersProvision'

headers:

Location:

description: Contains the URI of the newly created resource.

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{afId}/subscriptions/{subscriptionId}:

get:

summary: read an active subscription for the AF and the subscription Id

operationId: ReadAnSubscription

tags:

- Individual 5GLAN Parameters Provision Subscription

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

responses:

'200':

description: OK (Successful get the active subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/5GLanParametersProvision'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

put:

summary: Fully updates/replaces an existing subscription resource

operationId: FullyUpdateAnSubscription

tags:

- Individual 5GLAN Parameters Provision Subscription

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

requestBody:

description: Parameters to update/replace the existing subscription

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/5GLanParametersProvision'

responses:

'200':

description: OK (Successful deletion of the existing subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/5GLanParametersProvision'

'204':

description: >

Successful case. The resource has been successfully updated and no additional

content is to be sent in the response message.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

patch:

summary: Partial updates an existing subscription resource

operationId: PartialUpdateAnSubscription

tags:

- Individual 5GLAN Parameters Provision Subscription

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

requestBody:

required: true

content:

application/merge-patch+json:

schema:

$ref: '#/components/schemas/5GLanParametersProvisionPatch'

responses:

'200':

description: OK. The subscription was modified successfully.

content:

application/json:

schema:

$ref: '#/components/schemas/5GLanParametersProvision'

'204':

description: >

Successful case. The resource has been successfully updated and no additional

content is to be sent in the response message.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

summary: Deletes an already existing subscription

operationId: DeleteAnSubscription

tags:

- Individual 5GLAN Parameters Provision Subscription

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

responses:

'204':

description: No Content (Successful deletion of the existing subscription)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{tokenUrl}'

scopes: {}

schemas:

5GLanParametersProvision:

description: Represents an individual 5G LAN parameters provision subscription resource.

type: object

properties:

self:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

5gLanParams:

$ref: '#/components/schemas/5GLanParameters'

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

required:

- 5gLanParams

- suppFeat

5GLanParametersProvisionPatch:

description: >

Represents the 5G LAN parameters to request the modification of a subscription

to provision parameters.

type: object

properties:

5gLanParamsPatch:

$ref: '#/components/schemas/5GLanParametersPatch'

5GLanParameters:

description: Represents 5G LAN service related parameters that need to be provisioned.

type: object

properties:

exterGroupId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalGroupId'

gpsis:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

minProperties: 1

description: >

Contains the list of 5G VN Group members, each member is identified by GPSI.

Any string value can be used as a key of the map.

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

aaaIpv4Addr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

aaaIpv6Addr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

aaaUsgs:

type: array

items:

$ref: '#/components/schemas/AaaUsage'

minItems: 1

mtcProviderId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MtcProviderInformation'

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

sessionType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionType'

sessionTypes:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionType'

minItems: 1

description: Further allowed PDU Session types.

appDesps:

type: object

additionalProperties:

$ref: '#/components/schemas/AppDescriptor'

minProperties: 1

description: Describes the operation systems and the corresponding applications for each operation systems. The key of map is osId.

required:

- exterGroupId

- gpsis

- dnn

- snssai

- sessionType

- appDesps

5GLanParametersPatch:

description: Represents 5G LAN service related parameters that need to be modified.

type: object

properties:

gpsis:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GpsiRm'

minProperties: 1

description: >

Contains the list of 5G VN Group members, each member is identified by GPSI.

Any string value can be used as a key of the map.

appDesps:

type: object

additionalProperties:

$ref: '#/components/schemas/AppDescriptorRm'

minProperties: 1

description: >

Describes the operation systems and the corresponding applications for

each operation systems. The key of map is osId.

AppDescriptor:

description: Represents an operation system and the corresponding applications.

type: object

properties:

osId:

$ref: 'TS29519\_Policy\_Data.yaml#/components/schemas/OsId'

appIds:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

minProperties: 1

description: >

Identifies applications that are running on the UE's operating system.

Any string value can be used as a key of the map.

required:

- osId

- appIds

AppDescriptorRm:

description: >

Represents the same as the AppDescriptor data type but with the nullable:true

property.

type: object

properties:

appIds:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationIdRm'

minProperties: 1

description: >

Identifies applications that are running on the UE's operating system.

Any string value can be used as a key of the map.

AaaUsage:

anyOf:

- type: string

enum:

- AUTH

- IP\_ALLOC

- type: string

description: >

This string provides forward-compatibility with future extensions to the enumeration

and is not used to encode content defined in the present version of this API.

description: |

Possible values are:

- AUTH: secondary authentication/authorization needed from DN-AAA server

- IP\_ALLOC: UE IP address allocation needed from DN-AAA server

\*\*\* Next Change \*\*\*

# A.9 ServiceParameter API

openapi: 3.0.0

info:

title: 3gpp-service-parameter

version: 1.1.1

description: |

API for AF service paramter

© 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: >

3GPP TS 29.522 V17.7.0; 5G System; Network Exposure Function Northbound APIs.

url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.522/'

security:

- {}

- oAuth2ClientCredentials: []

servers:

- url: '{apiRoot}/3gpp-service-parameter/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 5.2.4 of 3GPP TS 29.122.

paths:

/{afId}/subscriptions:

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

get:

summary: read all of the active subscriptions for the AF

operationId: ReadAllSubscriptions

tags:

- Service Parameter Subscriptions

parameters:

- name: gpsis

in: query

description: The GPSI of the requested UE(s).

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

minItems: 1

- name: ip-addrs

in: query

description: The IP address(es) of the requested UE(s).

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/IpAddr'

minItems: 1

- name: ip-domain

in: query

description: >

The IPv4 address domain identifier. The attribute may only be provided

if IPv4 address is included in the ip-addrs query parameter.

required: false

schema:

type: string

- name: mac-addrs

in: query

description: The MAC address(es) of the requested UE(s).

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

minItems: 1

responses:

'200':

description: OK.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/ServiceParameterData'

minItems: 0

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

post:

summary: Creates a new subscription resource

operationId: CreateAnSubscription

tags:

- Service Parameter Subscriptions

requestBody:

description: Request to create a new subscription resource

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/ServiceParameterData'

responses:

'201':

description: Created (Successful creation of subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/ServiceParameterData'

headers:

Location:

description: Contains the URI of the newly created resource.

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

callbacks:

notificationDestination:

'{$request.body#/notificationDestination}':

post:

requestBody:

description: >

Notifications upon AF Service Parameter Authorization Update,

and/or AF subscribed event notification of the outcome related

to the invocation of service parameters provisioning.

required: true

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/AfNotification'

minItems: 1

responses:

'204':

description: Expected response to a successful callback processing without a body

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{afId}/subscriptions/{subscriptionId}:

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

get:

summary: read an active subscriptions for the SCS/AS and the subscription Id

operationId: ReadAnSubscription

tags:

- Individual Service Parameter Subscription

responses:

'200':

description: OK (Successful get the active subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/ServiceParameterData'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

put:

summary: Fully updates/replaces an existing subscription resource

operationId: FullyUpdateAnSubscription

tags:

- Individual Service Parameter Subscription

requestBody:

description: Parameters to update/replace the existing subscription

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/ServiceParameterData'

responses:

'200':

description: OK (Successful update of the subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/ServiceParameterData'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

patch:

summary: Partial updates/replaces an existing subscription resource

operationId: PartialUpdateAnSubscription

tags:

- Individual Service Parameter Subscription

requestBody:

required: true

content:

application/merge-patch+json:

schema:

$ref: '#/components/schemas/ServiceParameterDataPatch'

responses:

'200':

description: OK. The subscription was modified successfully.

content:

application/json:

schema:

$ref: '#/components/schemas/ServiceParameterData'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

summary: Deletes an already existing subscription

operationId: DeleteAnSubscription

tags:

- Individual Service Parameter Subscription

responses:

'204':

description: No Content (Successful deletion of the existing subscription)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{tokenUrl}'

scopes: {}

schemas:

ServiceParameterData:

description: Represents an individual Service Parameter subscription resource.

type: object

properties:

afServiceId:

type: string

description: Identifies a service on behalf of which the AF is issuing the request.

appId:

type: string

description: Identifies an application.

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

externalGroupId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalGroupId'

anyUeInd:

type: boolean

description: >

Identifies whether the AF request applies to any UE. This attribute

shall set to "true" if applicable for any UE, otherwise, set to "false".

gpsi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

ueIpv4:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

ueIpv6:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

ueMac:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

self:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

subNotifEvents:

type: array

items:

$ref: '#/components/schemas/Event'

minItems: 1

notificationDestination:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

requestTestNotification:

type: boolean

description: >

Set to true by the AF to request the NEF to send a test notification

as defined in clause 5.2.5.3 of 3GPP TS 29.122. Set to false or omitted otherwise.

websockNotifConfig:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/WebsockNotifConfig'

paramOverPc5:

$ref: '#/components/schemas/ParameterOverPc5'

paramOverUu:

$ref: '#/components/schemas/ParameterOverUu'

paramForProSeDd:

$ref: '#/components/schemas/ParamForProSeDd'

paramForProSeDc:

$ref: '#/components/schemas/ParamForProSeDc'

paramForProSeU2NRelUe:

$ref: '#/components/schemas/ParamForProSeU2NRelUe'

paramForProSeRemUe:

$ref: '#/components/schemas/ParamForProSeRemUe'

urspGuidance:

type: array

items:

$ref: '#/components/schemas/UrspRuleRequest'

minItems: 1

description: Contains the service parameter used to guide the URSP.

mtcProviderId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MtcProviderInformation'

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

ServiceParameterDataPatch:

description: >

Represents the parameters to request the modification of a service parameter

subscription resource.

type: object

properties:

paramOverPc5:

$ref: '#/components/schemas/ParameterOverPc5Rm'

paramOverUu:

$ref: '#/components/schemas/ParameterOverUuRm'

paramForProSeDd:

$ref: '#/components/schemas/ParamForProSeDdRm'

paramForProSeDc:

$ref: '#/components/schemas/ParamForProSeDcRm'

paramForProSeU2NRelUe:

$ref: '#/components/schemas/ParamForProSeU2NRelUeRm'

paramForProSeRemUe:

$ref: '#/components/schemas/ParamForProSeRemUeRm'

urspGuidance:

type: array

items:

$ref: '#/components/schemas/UrspRuleRequest'

minItems: 1

description: Contains the service parameter used to guide the URSP.

subNotifEvents:

type: array

items:

$ref: '#/components/schemas/Event'

minItems: 1

nullable: true

notificationDestination:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

ParameterOverPc5:

description: >

Represents configuration parameters for V2X communications over PC5 reference point.

type: string

ParameterOverPc5Rm:

description: >

Represents the same as the ParameterOverPc5 data type but with the nullable:true property.

type: string

nullable: true

ParameterOverUu:

description: >

Represents configuration parameters for V2X communications over Uu reference point.

type: string

ParameterOverUuRm:

description: >

Represents the same as the ParameterOverUu data type but with the nullable:true property.

type: string

nullable: true

ParamForProSeDd:

description: Represents the service parameters for 5G ProSe direct discovery.

type: string

ParamForProSeDdRm:

description: >

This data type is defined in the same way as the ParamForProSeDd data type,

but with the OpenAPI nullable property set to true.

type: string

nullable: true

ParamForProSeDc:

description: Represents the service parameters for 5G ProSe direct communications.

type: string

ParamForProSeDcRm:

description: >

This data type is defined in the same way as the ParamForProSeDc data type,

but with the OpenAPI nullable property set to true.

type: string

nullable: true

ParamForProSeU2NRelUe:

description: Represents the service parameters for 5G ProSe UE-to-network relay UE.

type: string

ParamForProSeU2NRelUeRm:

description: >

This data type is defined in the same way as the ParamForProSeU2NRelay data type,

but with the OpenAPI nullable property set to true.

type: string

nullable: true

ParamForProSeRemUe:

description: Represents the service parameters for 5G ProSe Remate UE.

type: string

ParamForProSeRemUeRm:

description: >

This data type is defined in the same way as the ParamForProSeRemUe data type,

but with the OpenAPI nullable property set to true.

type: string

nullable: true

UrspRuleRequest:

description: Contains parameters that can be used to guide the URSP.

type: object

properties:

trafficDesc:

$ref: '#/components/schemas/TrafficDescriptorComponents'

relatPrecedence:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

routeSelParamSets:

type: array

items:

$ref: '#/components/schemas/RouteSelectionParameterSet'

minItems: 1

description: Sets of parameters that may be used to guide the Route Selection Descriptors of the URSP.

RouteSelectionParameterSet:

description: >

Contains parameters that can be used to guide the Route Selection

Descriptors of the URSP.

type: object

properties:

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

precedence:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

spatialValidityAreas:

type: array

items:

$ref: 'TS29522\_AMPolicyAuthorization.yaml#/components/schemas/GeographicalArea'

minItems: 1

description: >

Indicates where the route selection parameters apply. It may correspond

to a geographical area, for example using a geographic shape that

is known to the AF and is configured by the operator to correspond to a list

of or TAIs.

spatialValidityTais:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Tai'

minItems: 1

description: Indicates the TAIs in which the route selection parameters apply. This attribute is applicable only within the 5GC and it shall not be included in the request messages of untrusted AFs for URSP guidance.

Event:

anyOf:

- type: string

enum:

- SUCCESS\_UE\_POL\_DEL\_SP

- UNSUCCESS\_UE\_POL\_DEL\_SP

- type: string

description: >

This string provides forward-compatibility with future extensions to the enumeration

and is not used to encode content defined in the present version of this API.

description: |

Possible values are:

- SUCCESS\_UE\_POL\_DEL\_SP: Successful UE Policy Delivery related to the invocation of AF provisioned Service Parameters.

- UNSUCCESS\_UE\_POL\_DEL\_SP: Unsuccessful UE Policy Delivery related to the invocation of AF provisioned Service Parameters.

AfNotification:

description: >

Notifications upon AF Service Parameter Authorization Update e.g. to

revoke the authorization, and/or AF subscribed event notification of the

outcome related to the invocation of service parameter provisioning.

type: object

properties:

subscription:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

reportEvent:

$ref: '#/components/schemas/Event'

authResult:

$ref: '#/components/schemas/AuthorizationResult'

gpsis:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

minItems: 1

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

eventInfo:

$ref: '#/components/schemas/EventInfo'

required:

- subscription

anyOf:

- required: [reportEvent]

- required: [authResult]

TrafficDescriptorComponents:

description: Traffic descriptor components for the requested URSP.

type: object

properties:

appDescs:

type: object

additionalProperties:

$ref: 'TS29522\_5GLANParameterProvision.yaml#/components/schemas/AppDescriptor'

minProperties: 1

description: Describes the operation systems and the corresponding applications for each operation systems. The key of map is osId.

flowDescs:

type: array

items:

type: string

minItems: 1

description: Represents a 3-tuple with protocol, server ip and server port for UL/DL application traffic. The content of the string has the same encoding as the IPFilterRule AVP value as defined in IETF RFC 6733.

domainDescs:

type: array

items:

type: string

minItems: 1

description: FQDN(s) or a regular expression which are used as a domain name matching criteria.

ethFlowDescs:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EthFlowDescription'

minItems: 1

description: Descriptor(s) for destination information of non-IP traffic in which only ethernet flow description is defined.

dnns:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

minItems: 1

description: This is matched against the DNN information provided by the application.

connCaps:

type: array

items:

$ref: '#/components/schemas/ConnectionCapabilities'

minItems: 1

description: This is matched against the information provided by a UE application when it requests a network connection with certain capabilities.

anyOf:

- required: [appDescs]

- required: [flowDescs]

- required: [domainDescs]

- required: [ethFlowDescs]

- required: [dnns]

- required: [connCaps]

AuthorizationResult:

anyOf:

- type: string

enum:

- AUTH\_REVOKED

- type: string

description: >

This string provides forward-compatibility with future extensions to the enumeration

and is not used to encode content defined in the present version of this API.

description: |

Possible values are:

- AUTH\_REVOKED: Indicated the service parameters authorization is revoked.

EventInfo:

description: Indicates the event information.

type: object

properties:

failureCause:

$ref: '#/components/schemas/Failure'

Failure:

oneOf:

- type: string

enum:

- UNSPECIFIED

- UE\_NOT\_REACHABLE

- UNKNOWN

- UE\_TEMP\_UNREACHABLE

- type: string

description: >

This string provides forward-compatibility with future extensions to the enumeration

and is not used to encode content defined in the present version of this API.

description: |

Possible values are:

- UNSPECIFIED: Indicates the PCF received the UE sent UE policy delivery service cause #111 (Protocol error, unspecified).

- UE\_NOT\_REACHABLE: Indicates the PCF received the notification from the AMF that the UE is not reachable.

- UNKNOWN: Indicates unknown reasons upon no response from the UE, e.g. UPDS message type is not defined or not implemented by the UE, or not compatible with the UPDS state, in which the UE shall ignore the UPDS message.

- UE\_TEMP\_UNREACHABLE: Indicates the PCF received the notification from the AMF that the UE is not reachable but the PCF will retry again.

ConnectionCapabilities:

anyOf:

- type: string

enum:

- IMS

- MMS

- SUPL

- INTERNET

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration and is not used to encode

content defined in the present version of this API.

description: |

Possible values are:

- IMS: Indicates the connection capability to support IMS service.

- MMS: Indicates the connection capability to support MMS service.

- SUPL: Indicates the connection capability to support SUPL service.

- INTERNET: Indicates the connection capability to support Internet service.

\*\*\* Next Change \*\*\*

# A.13 TimeSyncExposure API

openapi: 3.0.0

info:

title: 3gpp-time-sync-exposure

version: 1.0.1

description: |

API for time synchronization exposure.

© 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: >

3GPP TS 29.522 V17.7.0; 5G System; Network Exposure Function Northbound APIs.

url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.522/'

security:

- {}

- oAuth2ClientCredentials: []

servers:

- url: '{apiRoot}/3gpp-time-sync/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 5.2.4 of 3GPP TS 29.122.

paths:

/{afId}/subscriptions:

get:

summary: read all of the active subscriptions for the AF

operationId: ReadAllSubscriptions

tags:

- Time Synchronization Exposure Subscriptions

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

responses:

'200':

description: OK (Successful get all of the active subscriptions for the AF)

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/TimeSyncExposureSubsc'

minItems: 0

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

post:

summary: Creates a new subscription resource

operationId: CreateNewSubscription

tags:

- Time Synchronization Exposure Subscriptions

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

requestBody:

description: new subscription creation

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureSubsc'

responses:

'201':

description: Created (Successful creation)

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureSubsc'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

callbacks:

timeSyncSubsNotification:

'{$request.body#/subsNotifUri}':

post:

requestBody:

description: Notification for Time Synchronization Capability for a list of UEs.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureSubsNotif'

responses:

'204':

description: Expected response to a successful callback processing without a body

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{afId}/subscriptions/{subscriptionId}:

get:

summary: read an active subscription for the AF and the subscription Id

operationId: ReadAnSubscription

tags:

- Individual Time Synchronization Exposure Subscription

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

responses:

'200':

description: OK (Successful get the active subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureSubsc'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

put:

summary: Fully updates/replaces an existing subscription resource

operationId: FullyUpdateAnSubscription

tags:

- Individual Time Synchronization Exposure Subscription

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

requestBody:

description: Parameters to update/replace the existing subscription

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureSubsc'

responses:

'200':

description: OK (Successful deletion of the existing subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureSubsc'

'204':

description: >

Successful case. The resource has been successfully updated and no additional

content is to be sent in the response message.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

summary: Deletes an already existing subscription

operationId: DeleteAnSubscription

tags:

- Individual Time Synchronization Exposure Subscription

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

responses:

'204':

description: No Content (Successful deletion of the existing subscription)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{afId}/subscriptions/{subscriptionId}/configurations:

get:

summary: read all of the active configurations for the AF

operationId: ReadAllConfirguations

tags:

- Time Synchronization Exposure Configurations

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

- name: subscriptionId

description: String identifying the individual synchronization Exposure Subscription resource in the NEF

in: path

required: true

schema:

type: string

responses:

'200':

description: OK (Successful get all of the active configurations for the AF)

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/TimeSyncExposureConfig'

minItems: 0

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

post:

summary: Creates a new configuration resource

operationId: CreateNewConfirguation

tags:

- Time Synchronization Exposure Configurations

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

- name: subscriptionId

description: >

String identifying the individual synchronization Exposure Subscription

resource in the NEF.

in: path

required: true

schema:

type: string

requestBody:

description: new configuration creation

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureConfig'

responses:

'201':

description: Created (Successful creation)

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureConfig'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

callbacks:

timeSyncConfigNotification:

'{$request.body#/configNotifUri}':

post:

requestBody:

description: Notification for Time Synchronization Service status.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureConfigNotif'

responses:

'204':

description: Expected response to a successful callback processing without a body

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{afId}/subscriptions/{subscriptionId}/configurations/{instanceReference}:

get:

summary: read an active subscription for the AF and the subscription Id

operationId: ReadTimeSynSubscription

tags:

- Individual Time Synchronization Exposure Subscription

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

- name: instanceReference

in: path

description: Identifier of the configuration resource

required: true

schema:

type: string

responses:

'200':

description: OK (Successful get the active subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureConfig'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

put:

summary: Fully updates/replaces an existing configuration resource

operationId: FullyUpdateAnConfiguration

tags:

- Individual Time Synchronization Exposure Configuration

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

- name: instanceReference

in: path

description: Identifier of the configuration resource

required: true

schema:

type: string

requestBody:

description: Parameters to update/replace the existing configuration

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureConfig'

responses:

'200':

description: OK (Successful deletion of the existing configuration)

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureConfig'

'204':

description: >

Successful case. The resource has been successfully updated and no additional

content is to be sent in the response message.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

summary: Deletes an already existing configuration

operationId: DeleteAnConfiguration

tags:

- Individual Time Synchronization Exposure Configuration

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

- name: instanceReference

in: path

description: Identifier of the configuration resource

required: true

schema:

type: string

responses:

'204':

description: No Content (Successful deletion of the existing configuration)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{tokenUrl}'

scopes: {}

schemas:

TimeSyncExposureSubsc:

description: >

Contains requested parameters for the subscription to the notification

of time synchronization capability.

type: object

properties:

exterGroupId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalGroupId'

gpsis:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

minItems: 1

description: >

Contains a list of UE for which the time synchronization capabilities is requested.

anyUeInd:

type: boolean

description: >

Any UE indication. This IE shall be present if the event subscription

is applicable to any UE. Default value "false" is used, if not present.

afServiceId:

type: string

description: Identifies a service on behalf of which the AF is issuing the request.

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

subsNotifId:

type: string

description: Notification Correlation ID assigned by the NF service consumer.

subsNotifUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

subscribedEvents:

type: array

items:

$ref: '#/components/schemas/SubscribedEvent'

minItems: 1

description: Subscribed events

eventFilters:

type: array

items:

$ref: '#/components/schemas/EventFilter'

minItems: 1

description: >

Contains the filter conditions to match for notifying the event(s)

of time synchronization capabilities for a list of UE(s).

notifMethod:

$ref: 'TS29508\_Nsmf\_EventExposure.yaml#/components/schemas/NotificationMethod'

maxReportNbr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

expiry:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

repPeriod:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

requestTestNotification:

type: boolean

description: >

Set to true by the SCS/AS to request the SCEF to send a test notification

as defined in clause 5.2.5.3 of 3GPP TS 29.122. Set to false or omitted otherwise.

websockNotifConfig:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/WebsockNotifConfig'

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

required:

- subsNotifUri

- subsNotifId

TimeSyncCapability:

description: Contains time synchronization capability.

type: object

properties:

upNodeId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

gmCapables:

type: array

items:

$ref: '#/components/schemas/GmCapable'

asTimeRes:

$ref: '#/components/schemas/AsTimeResource'

ptpCapForUes:

type: object

additionalProperties:

$ref: '#/components/schemas/PtpCapabilitiesPerUe'

minProperties: 1

description: >

Contains the PTP capabilities supported by each of the UE(s).

The key of the map is the gpsi.

required:

- upNodeId

anyOf:

- required: [gmCapables]

- required: [asTimeRes]

TimeSyncExposureConfig:

description: Contains the Time Synchronization Configuration parameters.

type: object

properties:

upNodeId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

reqPtpIns:

$ref: '#/components/schemas/PtpInstance'

gmEnable:

type: boolean

description: >

Indicates that the AF requests 5GS to act as a grandmaster for PTP

or gPTP if it is included and set to true.

gmPrio:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

timeDom:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

timeSyncErrBdgt:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

configNotifId:

type: string

description: Notification Correlation ID assigned by the NF service consumer.

configNotifUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

tempValidity:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TemporalValidity'

required:

- upNodeId

- reqPtpIns

- timeDom

- configNotifId

- configNotifUri

TimeSyncExposureSubsNotif:

description: Contains the notification of time synchronization capability.

type: object

properties:

subsNotifId:

type: string

description: Notification Correlation ID assigned by the NF service consumer.

eventNotifs:

type: array

items:

$ref: '#/components/schemas/SubsEventNotification'

minItems: 1

required:

- subsNotifId

- eventNotifs

SubsEventNotification:

description: Notifications about subscribed Individual Events.

type: object

properties:

event:

$ref: '#/components/schemas/SubscribedEvent'

timeSyncCapas:

type: array

items:

$ref: '#/components/schemas/TimeSyncCapability'

minItems: 1

required:

- event

TimeSyncExposureConfigNotif:

description: Contains the notification of time synchronization service state.

type: object

properties:

configNotifId:

type: string

description: Notification Correlation ID assigned by the NF service consumer.

stateOfConfig:

$ref: '#/components/schemas/StateOfConfiguration'

required:

- configNotifId

- stateOfConfig

PtpCapabilitiesPerUe:

description: Contains the supported PTP capabilities per UE.

type: object

properties:

gpsi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

ptpCaps:

type: array

items:

$ref: '#/components/schemas/EventFilter'

minItems: 1

required:

- gpsi

- ptpCaps

EventFilter:

description: >

Contains the filter conditions to match for notifying the event(s) of time

synchronization capabilities.

type: object

properties:

instanceTypes:

type: array

items:

$ref: '#/components/schemas/InstanceType'

minItems: 1

transProtocols:

type: array

items:

$ref: '#/components/schemas/Protocol'

minItems: 1

ptpProfiles:

type: array

items:

type: string

minItems: 1

PtpInstance:

description: Contains PTP instance configuration and activation requested by the AF.

type: object

properties:

instanceType:

$ref: '#/components/schemas/InstanceType'

protocol:

$ref: '#/components/schemas/Protocol'

ptpProfile:

type: string

portConfigs:

type: array

items:

$ref: '#/components/schemas/ConfigForPort'

minItems: 1

required:

- instanceType

- protocol

- ptpProfile

ConfigForPort:

description: Contains configuration for each port.

type: object

properties:

gpsi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

n6Ind:

type: boolean

ptpEnable:

type: boolean

logSyncInter:

type: integer

logSyncInterInd:

type: boolean

logAnnouInter:

type: integer

logAnnouInterInd:

type: boolean

StateOfConfiguration:

description: Contains the state of the time synchronization configuration.

type: object

properties:

stateOfNwtt:

type: boolean

description: >

When the PTP port state is Leader, Follower or Passive, it is included and set to true

to indicate the state of configuration for NW-TT port is active; when PTP port state is

in any other case, it is included and set to false to indicate the state of

configuration for NW-TT port is inactive. Default value is false.

stateOfDstts:

description: >

Contains the PTP port states of the DS-TT(s).

type: array

items:

$ref: '#/components/schemas/StateOfDstt'

minItems: 1

StateOfDstt:

description: Contains the PTP port state of a DS-TT.

type: object

properties:

gpsi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

state:

type: boolean

description: >

When the PTP port state is Leader, Follower or Passive, it is included and set to true

to indicate the state of configuration for DS-TT port is active; when PTP port state is

in any other case, it is included and set to false to indicate the state of

configuration for DS port is inactive. Default value is false.

required:

- gpsi

- state

Protocol:

anyOf:

- type: string

enum:

- ETH

- IPV4

- IPV6

- type: string

description: >

This string provides forward-compatibility with future extensions to the enumeration

and is not used to encode content defined in the present version of this API.

description: |

Possible values are:

- ETH: Indicates Ethernet as defined in IEEE Std 1588 [45] Annex E is supported.

- IPV4: Indicates IPv4 as defined in IEEE Std 1588 [45] Annex C is supported.

- IPV6: Indicates IPv6 as defined in IEEE Std 1588 [45] Annex D is supported.

GmCapable:

anyOf:

- type: string

enum:

- GPTP

- PTP

- type: string

description: >

This string provides forward-compatibility with future extensions to the enumeration

and is not used to encode content defined in the present version of this API.

description: |

Possible values are:

- GPTP: gPTP grandmaster is supported.

- PTP: PTP grandmaste is supported.

InstanceType:

anyOf:

- type: string

enum:

- BOUNDARY\_CLOCK

- E2E\_TRANS\_CLOCK

- P2P\_TRANS\_CLOCK

- P2P\_RELAY\_INSTANCE

- type: string

description: >

This string provides forward-compatibility with future extensions to the enumeration

and is not used to encode content defined in the present version of this API.

description: |

Possible values are:

- BOUNDARY\_CLOCK: Indicates Boundary Clock as defined in IEEE Std 1588.

- E2E\_TRANS\_CLOCK: Indicates End-to-End Transparent Clock as defined in IEEE Std 1588.

- P2P\_TRANS\_CLOCK: Indicates Peer-to-Peer Transparent Clock as defined in IEEE Std 1588.

- P2P\_RELAY\_INSTANCE: Indicates PTP Relay instance as defined in IEEE Std 802.1AS.

SubscribedEvent:

anyOf:

- type: string

enum:

- AVAILABILITY\_FOR\_TIME\_SYNC\_SERVICE

- type: string

description: >

This string provides forward-compatibility with future extensions to the enumeration

and is not used to encode content defined in the present version of this API.

description: |

Possible values are:

- AVAILABILITY\_FOR\_TIME\_SYNC\_SERVICE: The UE is availability for time synchronization service.

AsTimeResource:

anyOf:

- type: string

enum:

- ATOMIC\_CLOCK

- GNSS

- TERRESTRIAL\_RADIO

- SERIAL\_TIME\_CODE

- PTP

- NTP

- HAND\_SET

- INTERNAL\_OSCILLATOR

- OTHER

- type: string

description: >

This string provides forward-compatibility with future extensions to the enumeration

and is not used to encode content defined in the present version of this API.

description: |

Possible values are:

- ATOMIC\_CLOCK: Indicates atomic clock is supported.

- GNSS: Indicates Global Navigation Satellite System is supported.

- TERRESTRIAL\_RADIO: Indicates terrestrial radio is supported.

- SERIAL\_TIME\_CODE: Indicates serial time code is supported.

- PTP: Indicates PTP is supported.

- NTP: Indicates NTP is supported.

- HAND\_SET: Indicates hand set is supported.

- INTERNAL\_OSCILLATOR: Indicates internal oscillator is supported.

- OTHER: Indicates other source of time is supported.

\*\*\* End of Changes \*\*\*