**3GPP TSG- WG3 Meeting #C3-230594**

**Athens, Greece, 27th February - 3rd** **March, 2023**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  |  |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** |  |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | SA2 has agreed in CR 3740 to TS 23.502 clause 4.11.0a.2 (see S2-2301622) to support URSP provisioning in EPS, when the SMF+PGW-C receives the UE Policy Container in ePCO in Create Session Request during initial Attach procedure, it forwards transparently the UE Policy Container in ePCO to PCF for the PDU Session in the Npcf\_SMPolicyControl\_Create Request. When the PCF for Session Management receives UE Policy Container from PCF for the UE, it forwards the UE Policy Container to SMF+PGW-C in Npcf\_SMPolicyControl\_UpdateNotify Request. The PCF for the PDU Session retrieves the PCRTs for UE Policy from PCF for the UE and subscribe to the applicable PCRTs in EPC to SMF+PGW-C.*“- To Support URSP provisioning in EPS, when the SMF+PGW-C receives the UE Policy Container in ePCO in Create Session Request during initial Attach procedure, it forwards transparently the UE Policy Container in ePCO to PCF for the PDU Session in the Npcf\_SMPolicyControl\_Create Request. When the PCF for Session Management receives UE Policy Container from PCF for the UE, it forwards the UE Policy Container to SMF+PGW-C in Npcf\_SMPolicyControl\_UpdateNotify Request. The PCF for the PDU Session retrieves the PCRTs for UE Policy from PCF for the UE and subscribe to the applicable PCRTs in EPC to SMF+PGW-C.”*Furthermore, when URSP Provisioning is supported in EPS, the PCF for the PDU Session establishes the UE Policy Association with PCF for the UE when a UE Policy Container is received from the UE and forwards the UE Policy Container to PCF for the UE in Npcf\_UEPolicyControl\_Create Request. The PCF for the UE generates the URSP and sends it to the PCF for the PDU Session in the UE Policy Container via Npcf\_UEPolicyControl\_UpdateNotify Request. The PCF for the UE triggers the re-evaluation of applicable URSPs and determines an update of URSP is needed for the UE when an event as described in TS 23.503[20] clause 6.1.2.2.X happens in the PCF for the PDU Session.*“When URSP Provisioning is supported in EPS, the PCF for the PDU Session establishes the UE Policy Association with PCF for the UE when a UE Policy Container is received from the UE and forwards the UE Policy Container to PCF for the UE in Npcf\_UEPolicyControl\_Create Request. The PCF for the UE generates the URSP and sends it to the PCF for the PDU Session in the UE Policy Container via Npcf\_UEPolicyControl\_UpdateNotify Request. The PCF for the UE triggers the re-evaluation of applicable URSPs and determines an update of URSP is needed for the UE when an event as described in TS 23.503[20] clause 6.1.2.2.X happens in the PCF for the PDU Session”*Accordingly, this CR adds support for URSP provisioning in EPS |
|  |  |
| ***Summary of change:*** | Add support for URSP provisioning in EPS |
|  |  |
| ***Consequences if not approved:*** | Stage 3 not aligned with stage 2 |
|  |  |
| ***Clauses affected:*** | 2, 5.6.1, 5.6.2.3, 5.6.2.4, 5.6.2.19, 5.6.3.2, 5.6.2.6, 5.8, B.3.2.0, B.3.2.X (new), B.3.3.Y (new), B.3.4.0, B.3.4.Z (new), A2, C2.1.5 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **X** |  |  Other core specifications  | TS 23.502 CR 3740  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR introduces a backwards compatible new feature to the OpenAPI description of the Npcf\_SMPolicyControl. |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* First Change \* \* \* \*

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 23.501: "System Architecture for the 5G System; Stage 2".

[3] 3GPP TS 23.502: "Procedures for the 5G System; Stage 2".

[4] 3GPP TS 29.500: "5G System; Technical Realization of Service Based Architecture; Stage 3".

[5] 3GPP TS 29.501: "5G System; Principles and Guidelines for Services Definition; Stage 3".

[6] 3GPP TS 23.503: "Policy and Charging Control Framework for the 5G System; Stage 2".

[7] 3GPP TS 29.513: "5G System; Policy and Charging Control signalling flows and QoS parameter mapping; Stage 3".

[8] IETF RFC 7540: "Hypertext Transfer Protocol Version 2 (HTTP/2)".

[9] IETF RFC 8259: "The JavaScript Object Notation (JSON) Data Interchange Format".

[10] OpenAPI: "OpenAPI Specification Version 3.0.0", <https://spec.openapis.org/oas/v3.0.0>.

[11] 3GPP TS 29.571: "5G System; Common Data Types for Service Based Interfaces; Stage 3".

[12] 3GPP TS 29.508: "5G System; Session Management Event Exposure Service; Stage 3".

[13] 3GPP TS 29.244: "Interface between the Control Plane and the User Plane of EPC Nodes".

[14] Void.

[15] 3GPP TS 29.519: "5G System; Usage of the Unified Data Repository service for Policy Control Data, Application Data and Structured Data for Exposure; Stage 3".

[16] 3GPP TS 23.228: "IP multimedia subsystem; Stage 2".

[17] 3GPP TS 29.514: "5G System; Policy Authorization Service; Stage 3".

[18] 3GPP TS 29.214: "Policy and Charging Control over Rx reference point 5".

[19] 3GPP TS 32.291: "5G System; Charging service; Stage 3".

[20] 3GPP TS 24.501: "Non-Access-Stratum (NAS) protocol for 5G System (5GS); Stage 3".

[21] 3GPP TS 23.380: "IMS Restoration Procedures".

[22] 3GPP TS 29.502: "5G System; Session Management Services; Stage 3".

[23] 3GPP TS 29.212: "Policy and Charging Control (PCC); Reference points".

[24] 3GPP TS 32.422: "Telecommunication management; Subscriber and equipment trace; Trace control and configuration management".

[25] 3GPP TS 29.507: "5G System; Access and Mobility Policy Control Service; Stage 3".

[26] 3GPP TS 23.060: "General Packet Radio Service (GPRS); Service description; Stage 2".

[27] 3GPP TS 33.501: "Security architecture and procedures for 5G system".

[28] IETF RFC 6749: "The OAuth 2.0 Authorization Framework".

[29] 3GPP TS 29.510: "Network Function Repository Services; Stage 3".

[30] 3GPP TS 32.290: "5G system; Services, operations and procedures of charging using Service Based Interface (SBI)".

[31] IETF RFC 7807: "Problem Details for HTTP APIs".

[32] 3GPP TS 29.122: "T8 reference point for Northbound APIs".

[33] 3GPP TS 23.527: "5G System; Restoration Procedures".

[34] 3GPP TS 29.503: "5G System; Unified Data Management Services; Stage 3".

[35] 3GPP TS 32.255: "Charging management; 5G data connectivity domain charging; stage 2".

[36] 3GPP TS 29.518: "5G System; Access and Mobility Management Services; Stage 3".

[37] 3GPP TS 29.274: "3GPP Evolved Packet System (EPS); Evolved General Packet Radio Service (GPRS) Tunnelling Protocol for Control plane (GTPv2-C); Stage 3".

[38] 3GPP TR 21.900: "Technical Specification Group working methods".

[39] 3GPP TS 29.521: "5G System; Binding Support Management Service; Stage 3".

[40] 3GPP TS 29.524: "Cause codes mapping between 5GC interfaces; Stage 3".

[41] 3GPP TS 24.008: "Mobile radio interface Layer 3 specification".

[42] 3GPP TS 23.316: "Wireless and wireline convergence access support for the 5G System (5GS)".

[43] 3GPP TS 24.193: "Access Traffic Steering, Switching and Splitting (ATSSS); Stage 3".

[44] 3GPP TS 24.519: "Time-Sensitive Networking (TSN) Application Function (AF) to Device-Side TSN Translator (DS-TT) and Network-Side TSN Translator (NW-TT) protocol aspects; Stage 3".

[45] IEEE Std 802.1Q-2018: "IEEE Standard for Local and metropolitan area networks--Bridges and Bridged Networks".

[46] 3GPP TS 29.551: "5G System; Packet Flow Description Management Service; Stage 3".

[47] BBF TR-456: "AGF Functional Requirements".

[48] CableLabs WR-TR-5WWC-ARCH: "5G Wireless Wireline Converged Core Architecture".

[49] 3GPP TS 24.539: "5G System (5GS); Network to TSN translator (TT) protocol aspects; Stage 3".

[50] 3GPP TS 29.564: "5G System; User Plane Function Services; Stage 3".

[51] 3GPP TS 29.520: "5G System; Network Data Analytics Services; Stage 3".

[52] 3GPP TS 24.301: "Non-Access-Stratum (NAS) protocol for Evolved Packet System (EPS); Stage 3".

[53] 3GPP TS 29.565: "5G System; Time Sensitive Communication and Time Synchronization Function Services; Stage 3".

[54] 3GPP TS 38.413: "NG Radio Access Network (NG-RAN); NG Application Protocol (NGAP)".

[55] 3GPP TS 29.525: "5G System; UE Policy Control Service; Stage 3".

\* \* \* Next Change \* \* \* \*

### 5.6.1 General

This clause specifies the application data model supported by the API.

The Npcf\_SMPolicyControl API allows the NF service consumer to retrieve the session management related policy from the PCF as defined in 3GPP TS 23.503 [6].

Table 5.6.1-1 specifies the data types defined for the Npcf\_SMPolicyControl service based interface protocol.

Table 5.6.1-1: Npcf\_SMPolicyControl specific Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Section defined | Description | Applicability |
| 5GSmCause | 5.6.3.2 | Indicates the 5GSM cause code value. | RAN-NAS-Cause |
| AdditionalAccessInfo | 5.6.2.43 | Indicates the combination of additional Access Type and RAT Type for MA PDU session | ATSSS |
| AccNetChargingAddress | 5.6.2.35 | Identifies the address of the network node performing charging and used for charging applications. |  |
| AccNetChId | 5.6.2.23 | Contains the access network charging identifier for the PCC rule(s) or whole PDU session. |  |
| AccuUsageReport | 5.6.2.18 | Contains the accumulated usage report information. | UMC |
| AfSigProtocol | 5.6.3.10 | Indicates the protocol used for signalling between the UE and the AF. | ProvAFsignalFlow |
| AppDetectionInfo | 5.6.2.22 | Contains the detected application's traffic information. | ADC |
| ApplicationDescriptor | 5.6.3.2 | Defines the Application Descriptor for an ATSSS rule. | ATSSS |
| AtsssCapability | 5.6.3.26 | Contains the ATSSS capability supported for the MA PDU Session. | ATSSS |
| AuthorizedDefaultQos | 5.6.2.34 | Authorized Default QoS. |  |
| BridgeManagementContainer | 5.6.2.47 | Contains the UMIC. | TimeSensitiveNetworking |
| ChargingData | 5.6.2.11 | Contains charging related parameters. |  |
| ChargingInformation | 5.6.2.17 | Contains the addresses, and if available, the instance ID and set ID, of the charging functions. |  |
| ConditionData | 5.6.2.9 | Contains conditions for applicability of a rule. |  |
| CreditManagementStatus | 5.6.3.16 | Indicates the reason of the credit management session failure. |  |
| DownlinkDataNotificationControl | 5.6.2.48 | Contains the downlink data notification control information. | DDNEventPolicyControl |
| DownlinkDataNotificationControlRm | 5.6.2.49 | This data type is defined in the same way as the "DownlinkDataNotificationControl" data type, but with the OpenAPI "nullable: true" property. | DDNEventPolicyControl2 |
| EpsRanNasRelCause | 5.6.3.2 | Indicates the RAN or NAS release cause code information in 3GPP-EPS access type or indicates the TWAN or untrusted WLAN release cause code information in Non-3GPP-EPS access type. | RAN-NAS-Cause |
| ErrorReport | 5.6.2.36 | Contains the PCC rule and/or session rule and/or policy decision and/or condition data reports. |  |
| FailureCause | 5.6.3.14 | Indicates the cause of the failure in a Partial Success Report. |  |
| FailureCode | 5.6.3.9 | Indicates the reason of the PCC rule failure. |  |
| FlowDescription | 5.6.3.2 | Defines a packet filter for an IP flow. |  |
| FlowDirection | 5.6.3.3 | Indicates the direction of the service data flow. |  |
| FlowDirectionRm | 5.6.3.15 | This data type is defined in the same way as the "FlowDirection" data type, but allows null value. |  |
| FlowInformation | 5.6.2.14 | Contains the flow information. |  |
| IpMulticastAddressInfo | 5.6.2.46 | Contains the IP multicast addressing information | WWC |
| MaPduIndication | 5.6.3.25 | Contains the MA PDU session indication, i.e., MA PDU Request or MA PDU Network-Upgrade Allowed. | ATSSS |
| MeteringMethod | 5.6.3.5 | Indicates the metering method. |  |
| MulticastAccessControl | 5.6.3.20 | Indicates whether the service data flow, corresponding to the service data flow template, is allowed or not allowed. | WWC |
| NetLocAccessSupport | 5.6.3.27 | Indicates the access network support of the report of the requested access network information. | NetLoc |
| NotificationControlIndication | 5.6.3.29 | Indicates the notification of DDD Status is requested and/or notification of DDN Failure is requested. | DDNEventPolicyControl |
| NwdafData | 5.6.2.53 | Indicates the list of NWDAF instance IDs used for the PDU Session and their associated Analytics ID(s) consumed by the NF service consumer. | EneNA |
| PacketFilterContent | 5.6.3.2 | Defines a packet filter for an IP flow. |  |
| PacketFilterInfo | 5.6.2.30 | Contains the information from a single packet filter sent from the NF service consumer to the PCF. |  |
| PartialSuccessReport | 5.6.2.33 | Includes the information reported by the NF service consumer when some of the PCC rules and/or session rules and/or policy decisions and/or condition data are not successfully installed/activated or stored. |  |
| PccRule | 5.6.2.6 | Contains the PCC rule information. |  |
| PduSessionRelCause | 5.6.3.24 | Contains the NF service consumer PDU Session release cause.  | PDUSessionRelCause,ImmediateTermination |
| PolicyControlRequestTrigger | 5.6.3.6 | Contains the policy control request trigger(s). |  |
| PolicyDecisionFailureCode | 5.6.3.28 | Indicates the type of the failed policy decision and/or condition data. | PolicyDecisionErrorHandling |
| PortManagementContainer | 5.6.2.45 | Contains the port management information container for a port. | TimeSensitiveNetworking |
| QosCharacteristics | 5.6.2.16 | Contains QoS characteristics for a non-standardized or non-configured 5QI. |  |
| QosData | 5.6.2.8 | Contains the QoS parameters. |  |
| QosFlowUsage | 5.6.3.13 | Indicates a QoS flow usage information. |  |
| QosMonitoringData | 5.6.2.40 | Contains QoS monitoring related control information. | QosMonitoring |
| QosMonitoringReport | 5.6.2.42 | Contains QoS monitoring reporting information. | QosMonitoring |
| QosNotificationControlInfo | 5.6.2.32 | Contains the QoS Notification Control Information. |  |
| RanNasRelCause | 5.6.2.28 | Contains the RAN/NAS release cause. | RAN-NAS-Cause |
| RedirectAddressType | 5.6.3.12 | Indicates the redirect address type. | ADC |
| RedirectInformation | 5.6.2.13 | Contains the redirect information. | ADC |
| ReportingFrequency | 5.6.3.22 | Indicates the frequency for the reporting | QosMonitoring |
| ReportingLevel | 5.6.3.4 | Indicates the reporting level. |  |
| RequestedQos | 5.6.2.31 | Contains the QoS information requested by the UE. |  |
| RequestedQosMonitoringParameter | 5.6.3.21 | Indicates the requested QoS monitoring parameters to be measured. | QosMonitoring |
| RequestedRuleData | 5.6.2.24 | Contains rule data requested by the PCF to receive information associated with PCC rules.  |  |
| RequestedRuleDataType | 5.6.3.7 | Contains the type of rule data requested by the PCF. |  |
| RequestedUsageData | 5.6.2.25 | Contains usage data requested by the PCF requesting usage reports for the corresponding usage monitoring data instances.  | UMC |
| RuleOperation | 5.6.3.11 | Indicates a UE initiated resource operation that causes a request for PCC rules. |  |
| RuleReport | 5.6.2.27 | Reports the status of PCC rule(s). |  |
| RuleStatus | 5.6.3.8 | Indicates the status of PCC or session rule. |  |
| ServingNfIdenty | 5.6.2.38 | Contains the serving Network Function identity. |  |
| SessionRule | 5.6.2.7 | Contains session level policy information. |  |
| SessionRuleFailureCode | 5.6.3.17 | Indicates the reason of the session rule failure. | SessionRuleErrorHandling |
| SessionRuleReport | 5.6.2.37 | Reports the status of session rule. | SessionRuleErrorHandling |
| SgsnAddress | 5.6.2.50 | Contains the serving SGSN address. | 2G3GIWK |
| SmPolicyAssociationReleaseCause | 5.6.3.23 | Represents the cause why the PCF requests the termination of the SM policy association. |  |
| SmPolicyControl | 5.6.2.2 | Contains the parameters to request the SM policies and the SM policies authorized by the PCF. |  |
| SmPolicyContextData | 5.6.2.3 | Contains the parameters to create individual SM policy resource. |  |
| SmPolicyDecision | 5.6.2.4 | Contains the SM policies authorized by the PCF. |  |
| SmPolicyNotification | 5.6.2.5 | Contains the update of the SM policies. |  |
| SmPolicyDeleteData | 5.6.2.15 | Contains the parameters to be sent to the PCF when the individual SM policy is deleted. |  |
| SmPolicyUpdateContextData | 5.6.2.19 | Contains the met policy control request trigger(s) and corresponding new value(s) or the error report of the policy enforcement. |  |
| SteeringFunctionality | 5.6.3.18 | Indicates functionality to support traffic steering, switching and splitting determined by the PCF. | ATSSS |
| SteeringMode | 5.6.2.39 | Contains the steering mode value and parameters determined by the PCF. | ATSSS |
| SteerModeIndicator | 5.6.3.31 | Contains Autonomous load-balance indicator or UE-assistance indicator. | EnATSSS |
| SteerModeValue | 5.6.3.19 | Indicates the steering mode value determined by the PCF. | ATSSS |
| TerminationNotification | 5.6.2.21 | Termination Notification. |  |
| ThresholdValue | 5.6.2.52 | Contains the threshold value(s) for RTT and/or Packet Loss Rate. | EnATSSS |
| TrafficControlData | 5.6.2.10 | Contains parameters determining how flows associated with a PCCRule are treated (blocked, redirected, etc). |  |
| TsnBridgeInfo | 5.6.2.41 | Contains parameters that describe and identify the TSC user plane node. | TimeSensitiveNetworking |
| TsnPortNumber | 5.6.3.2 | Contains a port number. | TimeSensitiveNetworking |
| UeCampingRep | 5.6.2.26 | Contains the current applicable values corresponding to the policy control request triggers. |  |
| UeInitiatedResourceRequest | 5.6.2.29 | Indicates a UE requests specific QoS handling for selected SDF. |  |
| UePolicyContainer | 5.6.3.2 | Contains a UE policy container | EpsUrsp |
| UpPathChgEvent | 5.6.2.20 | Contains the UP path change event subscription from the AF. | TSC |
| UsageMonitoringData | 5.6.2.12 | Contains usage monitoring related control information. | UMC |

Table 5.6.1-2 specifies data types re-used by the Npcf\_SMPolicyControl service based interface protocol from other specifications, including a reference to their respective specifications and when needed, a short description of their use within the Npcf\_SMPolicyControl service based interface.

Table 5.6.1-2: Npcf\_SMPolicyControl re-used Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Reference | Comments | Applicability |
| 5GMmCause | 3GPP TS 29.571 [11] | Contains the cause value of 5GMM protocol. | RAN-NAS-Cause |
| 5Qi | 3GPP TS 29.571 [11] | Unsigned integer representing a 5G QoS Identifier (see clause 5.7.2.1 of 3GPP TS 23.501 [2]), within the range 0 to 255. |  |
| 5QiPriorityLevel | 3GPP TS 29.571 [11] | Unsigned integer indicating the 5QI Priority Level (see clauses 5.7.3.3 and 5.7.4 of 3GPP TS 23.501 [2]), within the range 1 to 127.Values are ordered in decreasing order of priority, i.e. with 1 as the highest priority and 127 as the lowest priority. |  |
| 5QiPriorityLevelRm | 3GPP TS 29.571 [11] | This data type is defined in the same way as the "5QiPriorityLevel" data type, but with the OpenAPI "nullable: true" property. |  |
| AccessType | 3GPP TS 29.571 [11] | The identification of the type of access network. |  |
| AccessTypeRm | 3GPP TS 29.571 [11] | This data type is defined in the same way as the "AccessType" data type, but with the OpenAPI "nullable: true" property. | ATSSS |
| Ambr | 3GPP TS 29.571 [11] | Session-AMBR. |  |
| AnGwAddress | 3GPP TS 29.514 [17] | Carries the control plane address of the access network gateway. (NOTE 1) |  |
| ApplicationChargingId | 3GPP TS 29.571 [11] | Application provided charging identifier allowing correlation of charging information. | AF\_Charging\_Identifier |
| Arp | 3GPP TS 29.571 [11] | ARP. |  |
| AverWindow | 3GPP TS 29.571 [11] | Averaging Window. |  |
| AverWindowRm | 3GPP TS 29.571 [11] | This data type is defined in the same way as the "AverWindow" data type, but with the OpenAPI "nullable: true" property. |  |
| BitRate | 3GPP TS 29.571 [11] | String representing a bit rate that shall be formatted as follows:pattern: "^\d+(\.\d+)? (bps|Kbps|Mbps|Gbps|Tbps)$"Examples: "125 Mbps", "0.125 Gbps", "125000 Kbps". |  |
| BitRateRm | 3GPP TS 29.571 [11] | This data type is defined in the same way as the "BitRate" data type, but with the OpenAPI "nullable: true" property. |  |
| Bytes | 3GPP TS 29.571 [11] | String with format "byte". | TimeSensitiveNetworking |
| ChargingId | 3GPP TS 29.571 [11] | Charging identifier allowing correlation of charging information. |  |
| ContentVersion | 3GPP TS 29.514 [17] | Indicates the content version of a PCC rule. It uniquely identifies a version of the PCC rule as defined in clause 4.2.6.2.14. | RuleVersioning |
| DateTime | 3GPP TS 29.571 [11] | String with format "date-time" as defined in OpenAPI Specification [10]. |  |
| DateTimeRm | 3GPP TS 29.571 [11] | This data type is defined in the same way as the "DateTime" data type, but with the OpenAPI "nullable: true" property. |  |
| DddTrafficDescriptor | 3GPP TS 29.571 [11] | Traffic Descriptor | DDNEventPolicyControl |
| DlDataDeliveryStatus | 3GPP TS 29.571 [11] | Downlink data delivery status. | DDNEventPolicyControl |
| DnaiChangeType | 3GPP TS 29.571 [11] | Describes the types of DNAI change. |  |
| Dnn | 3GPP TS 29.571 [11] | The DNN the user is connected to. |  |
| DnnSelectionMode | 3GPP TS 29.502 [22] | DNN selection mode. | DNNSelectionMode |
| DurationSec | 3GPP TS 29.571 [11] | Identifies a period of time in units of seconds. |  |
| DurationSecRm | 3GPP TS 29.571 [11] | This data type is defined in the same way as the "DurationSec" data type, but with the OpenAPI "nullable: true" property. |  |
| EasIpReplacementInfo | 3GPP TS 29.571 [11] | Contains EAS IP replacement information for a Source and a Target EAS. | EASIPreplacement |
| EthFlowDescription | 3GPP TS 29.514 [17] | Defines a packet filter for an Ethernet flow. (NOTE 2) |  |
| ExtMaxDataBurstVol | 3GPP TS 29.571 [11] | Maximum Data Burst Volume. | EMDBV |
| ExtMaxDataBurstVolRm | 3GPP TS 29.571 [11] | This data type is defined in the same way as the "ExtMaxDataBurstVol" data type, but with the OpenAPI "nullable: true" property. | EMDBV |
| FinalUnitAction | 3GPP TS 32.291 [19] | Indicates the action to be taken when the user's account cannot cover the service cost. |  |
| FlowStatus | 3GPP TS 29.514 [17] | Describes whether the IP flow(s) are enabled or disabled. The value "REMOVED" is not applicable to Npcf\_SMPolicyControl service. |  |
| Gpsi | 3GPP TS 29.571 [11] | Identifies a GPSI. |  |
| GroupId | 3GPP TS 29.571 [11] | Identifies a group of internal globally unique ID. |  |
| Guami | 3GPP TS 29.571 [11] | Globally Unique AMF Identifier. |  |
| InvalidParam | 3GPP TS 29.571 [11] | Invalid Parameters for the reported failed policy decisions | ExtPolicyDecisionErrorHandling |
| IpIndex | 3GPP TS 29.519 [15] | Information that identifies which IP pool or external server is used to allocate the IP address. |  |
| Ipv4Addr | 3GPP TS 29.571 [11]  | Identifies an Ipv4 address. |  |
| Ipv4AddrMask | 3GPP TS 29.571 [11] | String identifying an IPv4 address mask. |  |
| Ipv6Addr | 3GPP TS 29.571 [11] | Identifies an IPv6 address. |  |
| Ipv6Prefix | 3GPP TS 29.571 [11] | The Ipv6 prefix allocated for the user. |  |
| MacAddr48 | 3GPP TS 29.571 [11] | MAC Address. |  |
| MaxDataBurstVol | 3GPP TS 29.571 [11] | Maximum Data Burst Volume. |  |
| MaxDataBurstVolRm | 3GPP TS 29.571 [11] | This data type is defined in the same way as the "MaxDataBurstVol" data type, but with the OpenAPI "nullable: true" property. |  |
| NfInstanceId | 3GPP TS 29.571 [11] | The NF instance identifier. |  |
| NfSetId | 3GPP TS 29.571 [11] | The NF set identifier. |  |
| NgApCause | 3GPP TS 29.571 [11] | Contains the cause value of NgAP protocol. | RAN-NAS-Cause |
| NullValue | 3GPP TS 29.571 [11] | JSON's null value, used as an explicit value of an enumeration. |  |
| NwdafEvent | 3GPP TS 29.520 [51] | Analytics ID consumed by the NF service consumer. | EneNA |
| PacketDelBudget | 3GPP TS 29.571 [11] | Packet Delay Budget. |  |
| PacketErrRate | 3GPP TS 29.571 [11] | Packet Error Rate. |  |
| PacketLossRateRm | 3GPP TS 29.571 [11] | This data type is defined in the same way as the "PacketLossRate" data type, but with the OpenAPI "nullable: true" property. |  |
| PcfUeCallbackInfo | 3GPP TS 29.571 [11] | Contains the PCF for the UE callback URI and SBA binding information, if available | AMInfluence  |
| PduSessionId | 3GPP TS 29.571 [11] | The identification of the PDU session. |  |
| PduSessionType | 3GPP TS 29.571 [11] | Indicate the type of a PDU session. |  |
| Pei | 3GPP TS 29.571 [11] | The Identification of a Permanent Equipment. |  |
| PlmnIdNid | 3GPP TS 29.571 [11] | The identification of the Network: The PLMN Identifier (the mobile country code and the mobile network code) or the SNPN Identifier (the PLMN Identifier and the NID). |  |
| PresenceInfo  | 3GPP TS 29.571 [11] | Contains the information which describes a Presence Reporting Area. | PRA |
| PresenceInfoRm | 3GPP TS 29.571 [11] | This data type is defined in the same way as the "PresenceInfo" data type, but with the OpenAPI "nullable: true" property. | PRA |
| ProblemDetails | 3GPP TS 29.571 [11] | Contains a detailed information about an error. |  |
| QosNotifType | 3GPP TS 29.514 [17] | Indicates whether the GBR targets for the indicated SDFs are "NOT\_GUARANTEED" or "GUARANTEED" again. |  |
| QosResourceType | 3GPP TS 29.571 [11] | Indicates whether the resource type is GBR, delay critical GBR, or non-GBR. |  |
| RatingGroup | 3GPP TS 29.571 [11] | Identifier of a rating group. |  |
| RatType | 3GPP TS 29.571 [11] | The identification of the RAT type. |  |
| RedirectResponse | 3GPP TS 29.571 [11] | Contains redirection related information. | ES3XX |
| RouteToLocation | 3GPP TS 29.571 [11] | A traffic routes to applications location. | TSC |
| SatelliteBackhaulCategory | 3GPP TS 29.571 [11] | Indicates the satellite backhaul category or non-satellite backhaul. | SatBackhaulCategoryChg |
| ServerAddressingInfo | 3GPP TS 29.571 [11] | Contains the Provisioning Server information that provisions the UE with credentials and other data to enable SNPN access. | PvsSupport |
| ServiceId | 3GPP TS 29.571 [11] | Identifier of a service. |  |
| Snssai | 3GPP TS 29.571 [11] | Identifies the S-NSSAI. |  |
| SubscribedDefaultQos | 3GPP TS 29.571 [11] | Subscribed Default QoS. |  |
| Supi | 3GPP TS 29.571 [11] | The identification of the user (i.e. IMSI, NAI). |  |
| SupportedFeatures | 3GPP TS 29.571 [11] | Used to negotiate the applicability of the optional features defined in table 5.8-1. |  |
| TraceData | 3GPP TS 29.571 [11] |  |  |
| TimeZone | 3GPP TS 29.571 [11] | Contains the user time zone information. |  |
| TscaiInputContainer | 3GPP TS 29.514 [17] | TSCAI Input information. | TimeSensitiveNetworking |
| Uinteger | 3GPP TS 29.571 [11] | Unsigned Integer. |  |
| UintegerRm | 3GPP TS 29.571 [11] | This data type is defined in the same way as the "Uinteger" data type, but with the OpenAPI "nullable: true" property. | EnATSSS,AF\_latency |
| Uint64 | 3GPP TS 29.571 [11] | Unsigned 64-bit integers. | TimeSensitiveNetworking |
| Uri | 3GPP TS 29.571 [11] | URI. |  |
| UserLocation | 3GPP TS 29.571 [11] | Contains the user location(s). |  |
| Volume | 3GPP TS 29.122 [32] | Unsigned integer identifying a volume in units of bytes. |  |
| VolumeRm | 3GPP TS 29.122 [32] | This data type is defined in the same way as the "Volume" data type, but with the OpenAPI "nullable: true" property. |  |
| VplmnQos | 3GPP TS 29.502 [22] | QoS constraints in the VPLMN. | VPLMN-QoS-Control |
| NOTE 1: "AnGwAddr" data structure is only applicable to the 5GS and EPC/E-UTRAN interworking scenario as defined in Annex B.NOTE 2: In order to support a set of MAC addresses with a specific range in the traffic filter, feature MacAddressRange as specified in clause 5.8 shall be supported. |

\* \* \* Next Change \* \* \* \*

#### 5.6.2.3 Type SmPolicyContextData

Table 5.6.2.3-1: Definition of type SmPolicyContextData

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| accNetChId | AccNetChId | O | 0..1 | Indicates the access network charging identifier for the whole PDU session. For EPS interworking scenarios, it indicates the access network charging identifier for the default QoS flow / default EPS bearer or the whole PDU session. |  |
| chargEntityAddr | AccNetChargingAddress | O | 0..1 | Address of the network entity performing charging. |  |
| gpsi | Gpsi | O | 0..1 | Gpsi shall contain either an External Id or an MSISDN. |  |
| supi | Supi | M | 1 | Subscription Permanent Identifier.(NOTE 2) |  |
| invalidSupi | boolean | C | 0..1 | When this attribute is included and set to true, it indicates that the "supi" attribute contains an invalid value. This attribute shall be present if the SUPI is not available in the NF service consumer, or the SUPI is unauthenticated. When present it shall be set as follows:- true: invalid SUPI.- false (default): valid SUPI. |  |
| pduSessionId | PduSessionId | M | 1 | PDU session Id. |  |
| dnn | Dnn | M | 1 | The DNN of the PDU session, a full DNN with both the Network Identifier and Operator Identifier, or a DNN with the Network Identifier only.(NOTE 4) |  |
| dnnSelMode | DnnSelectionMode | O | 0..1 | Indicates whether the requested DNN corresponds to an explicitly subscribed DNN. | DNNSelectionMode |
| interGrpIds | array(GroupId) | O | 1..N | The internal Group Id(s). |  |
| notificationUri | Uri | M | 1 | Identifies the recipient of SM policies update notifications sent by the PCF. |  |
| pduSessionType | PduSessionType | M | 1 | Indicates the type of a PDU session. |  |
| accessType | AccessType | O | 0..1 | The Access Type where the served UE is camping. |  |
| ratType | RatType | O | 0..1 | The RAT Type where the served UE is camping. |  |
| addAccessInfo | AdditionalAccessInfo | O | 0..1 | Indicates the combination of additional Access Type and RAT Type for MA PDU session. | ATSSS |
| servingNetwork | PlmnIdNid | O | 0..1 | The serving network (a PLMN or an SNPN) where the served UE is camping. For the SNPN the NID together with the PLMN ID identifies the SNPN. |  |
| userLocationInfo | UserLocation | O | 0..1 | The location where the served UE is camping. (NOTE 3) |  |
| ueTimeZone | TimeZone | O | 0..1 | The time zone where the served UE is camping. |  |
| pei | Pei | O | 0..1 | The Permanent Equipment Identifier of the served UE. |  |
| ipv4Address | Ipv4Addr | O | 0..1 | The IPv4 Address of the served UE. |  |
| ipv6AddressPrefix | Ipv6Prefix | O | 0..1 | The Ipv6 Address Prefix of the served UE. |  |
| ipDomain | string | O | 0..1 | IPv4 address domain identifier.(NOTE 1) |  |
| subsSessAmbr | Ambr | O | 0..1 | UDM subscribed or DN-AAA authorized Session-AMBR. |  |
| authProfIndex | string | O | 0..1 | DN-AAA authorization profile index. | DN-Authorization |
| subsDefQos | SubscribedDefaultQos | O | 0..1 | Subscribed Default QoS Information. |  |
| vplmnQos | VplmnQos | O | 0..1 | QoS constraints in a VPLMN. | VPLMN-QoS-Control |
| numOfPackFilter | integer | O | 0..1 | Contains the number of supported packet filter for signalled QoS rules. |  |
| online | boolean | O | 0..1 | If it is included and set to true, the online charging is applied to the PDU session. |  |
| offline | boolean | O | 0..1 | If it is included and set to true, the offline charging is applied to the PDU session. |  |
| chargingCharacteristics | string | O | 0..1 | Contains the Charging Characteristics applied to the PDU session. Functional requirements for the Charging Characteristics are defined in 3GPP TS 32.255 [35] Annex A.The charging characteristics are encoded as specified in 3GPP TS 29.503 [34]. |  |
| 3gppPsDataOffStatus | boolean | O | 0..1 | If it is included and set to true, the 3GPP PS Data Off is activated by the UE. | 3GPP-PS-Data-Off |
| refQosIndication | boolean | O | 0..1 | If it is included and set to true, the reflective QoS is supported by the UE. |  |
| sliceInfo | Snssai | M | 1 | Identifies the S-NSSAI. |  |
| qosFlowUsage | QosFlowUsage | O | 0..1 | Indicates the required usage for default QoS flow. |  |
| servNfId | ServingNfIdentity | O | 0..1 | Contains the serving network function identity. |  |
| suppFeat | SupportedFeatures | C | 0..1 | Indicates the list of Supported features used as described in clause 5.8.This parameter shall be supplied by the NF service consumer in the POST request that requested the creation of an individual SM policy resource. |  |
| traceReq | TraceData | O | 0..1 | Trace control and configuration parameters information defined in 3GPP TS 32.422 [24]. |  |
| smfId | NfInstanceId | O | 0..1 | SMF instance identifier. |  |
| recoveryTime | DateTime | O | 0..1 | It includes the recovery time of the NF service consumer. |  |
| maPduInd | MaPduIndication | O | 0..1 | Contains the MA PDU session indication, i.e., MA PDU Request or MA PDU Network-Upgrade Allowed. | ATSSS |
| atsssCapab | AtsssCapability | O | 0..1 | Contains the ATSSS capability supported for the MA PDU Session. | ATSSS |
| ipv4FrameRouteList | array(Ipv4AddrMask) | O | 1..N | List of Framed Route information of IPv4. |  |
| ipv6FrameRouteList | array(Ipv6Prefix) | O | 1..N | List of Framed Route information of IPv6. |  |
| satBackhaulCategory | SatelliteBackhaulCategory | O | 0..1 | Satellite backhaul category or non-satellite backhaul used for the PDU session.When this attribute is not present, non-satellite backhaul applies. | SatBackhaulCategoryChg |
| pcfUeInfo | PcfUeCallbackInfo | O | 0..1 | PCF for the UE callback URI and SBA binding information. | AMInfluence |
| pvsInfo | array(ServerAddressingInfo) | O | 1..N | Provisioning Server(s) information that provision the UE with credentials and other data to enable SNPN access. | PvsSupport |
| onboardInd | boolean | O | 0..1 | If it is included and set to true, it indicates that the PDU session is used for UE Onboarding. | PvsSupport |
| nwdafDatas | array(NwdafData) | O | 1..N | List of NWDAF Instance IDs and their associated Analytics IDs consumed by the NF service consumer. | EneNA |
| uePolCont | UePolicyContainer | C | 0..1 | Indicates a UE policy container received from the UE. Only applicable to the 5GS and EPC interworking scenario as defined in Annex B. | EpsUrsp |
| NOTE 1: The value provided in this attribute is implementation specific. The only constraint is that the NF service consumer shall supply a different identifier for each overlapping address domain (e.g. the SMF NF instance identifier).NOTE 2: For an emergency session, when the SUPI is not available in the NF service consumer, or if available, the SUPI is unauthenticated, the value provided in the "supi" attribute is implementation specific.NOTE 3: The SMF may encode both 3GPP and non-3GPP access UE location in the "userLocationInfo" attribute.NOTE 4: The PCF uses the DNN as received from the NF service consumer without applying any transformation (e.g. in subsequent requests to the UDR). To successfully perform DNN matching, in a specific deployment a DNN shall always be encoded either with the full DNN (e.g., because there are multiple Operator Identifiers for a Network Identifier) or the DNN Network Identifier only. The NF service consumer may include the DNN Operator Identifier based on local configuration. |

\* \* \* Next Change \* \* \* \*

#### 5.6.2.4 Type SmPolicyDecision

Table 5.6.2.4-1: Definition of type SmPolicyDecision

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| sessRules | map(SessionRule) | O | 1..N | A map of Sessionrules with the content being the SessionRule as described in clause 5.6.2.7. The key used in this map for each entry is the sessRuleId attribute of the corresponding SessionRule. (NOTE 2) |  |
| pccRules | map(PccRule) | O | 1..N | A map of PCC rules with the content being the PCCRule as described in clause 5.6.2.6. The key used in this map for each entry is the pccRuleId attribute of the corresponding PccRule. |  |
| qosDecs | map(QosData) | O | 1..N | Map of QoS data policy decisions. The key used in this map for each entry is the qosId attribute of the corresponding QosData. (NOTE 2) |  |
| chgDecs | map(ChargingData) | O | 1..N | Map of Charging data policy decisions. The key used in this map for each entry is the chgId attribute of the corresponding ChargingData. |  |
| chargingInfo | ChargingInformation | C | 1 | Contains the CHF addresses, and if available, the associated CHF instance ID(s) and CHF set ID(s) of the PDU session. (NOTE 3) |  |
| traffContDecs | map(TrafficControlData) | O | 1..N | Map of Traffic Control data policy decisions. The key used in this map for each entry is the tcId attribute of the corresponding TrafficControlData. (NOTE 2) |  |
| umDecs | map(UsageMonitoringData) | O | 1..N | Map of Usage Monitoring data policy decisions. The key used in this map for each entry is the umId attribute of the corresponding UsageMonitoringData. | UMC |
| qosChars | map(QosCharacteristics) | O | 1..N | Map of QoS characteristics for non-standard 5QIs and non-preconfigured 5QIs. This map uses the 5QI values as keys. (NOTE 2) |  |
| qosMonDecs | map(QosMonitoringData) | O | 1..N | Map of QoS Monitoring data policy decision. The key used in this map for each entry is the qmId attribute of the corresponding QosMonitoringData. | QosMonitoring |
| reflectiveQoSTimer | DurationSec | O | 0..1 | Defines the lifetime of a UE derived QoS rule belonging to the PDU Session for reflective QoS. (NOTE 2) |  |
| offline | boolean | O | 0..1 | Indicates the offline charging is applicable to the PDU session when it is included and set to true. (NOTE 3) (NOTE 4) (NOTE 6) |  |
| online | boolean | O | 0..1 | Indicates the online charging is applicable to the PDU session when it is included and set to true. (NOTE 3) (NOTE 4) (NOTE 6) |  |
| offlineChOnly | boolean | O | 0..1 | Indicates that the online charging method shall never be used for any PCC rule activated during the lifetime of the PDU session, when this attribute is present and set to "true".The default value is "false", e.g. if this attribute is omitted.(NOTE 3) (NOTE 4) (NOTE 6) | OfflineChOnly |
| conds | map(ConditionData) | O | 1..N | A map of condition data with the content being as described in clause 5.6.2.9. The key used in this map for each entry is the condId attribute of the corresponding ConditionData. |  |
| revalidationTime | DateTime | O | 0..1 | Defines the time before which the NF service consumer shall have to re-request PCC rules. |  |
| pcscfRestIndication | boolean | O | 0..1 | If this attribute is included and set to true, it indicates that P-CSCF Restoration is requested. The default value "FALSE" applies if the attribute is not present and has not been supplied previously. | PCSCF-Restoration-Enhancement |
| policyCtrlReqTriggers | array(PolicyControlRequestTrigger) | O | 1..N | Defines the policy control request triggers subscribed by the PCF. |  |
| lastReqRuleData | array(RequestedRuleData) | O | 1..N | Defines the last list of rule control data requested by the PCF. |  |
| lastReqUsageData | RequestedUsageData | O | 0..1 | Indicates whether the last accumulated usage report is requested by the PCF or not, and includes references to the targeted usage monitoring data instances. | UMC |
| praInfos | map(PresenceInfoRm) | O | 1..N | Defines the PRA information provisioned by the PCF. The "praId" attribute within the PresenceInfo data type shall also be the key of the map. The "presenceState" attribute within the PresenceInfo data type shall not be supplied. | PRA |
| ipv4Index | IpIndex | C | 0..1 | Information that identifies the IP address allocation method for IPv4 address allocation. (NOTE 3) |  |
| ipv6Index | IpIndex | C | 0..1 | Information that identifies the IP address allocation method for IPv6 address allocation. (NOTE 3) |  |
| qosFlowUsage | QosFlowUsage | O | 0..1 | Indicates the required usage for default QoS flow. |  |
| relCause | SmPolicyAssociationReleaseCause | O | 0..1 | The cause for which the PCF requests the termination of the policy association. | RespBasedSessionRel |
| suppFeat | SupportedFeatures | C | 0..1 | Indicates the list of negotiated supported features.This parameter shall be supplied by the PCF in the response to the POST request that requested the creation of an individual SM policy resource. |  |
| tsnBridgeManCont | BridgeManagementContainer | O | 0..1 | Transports TSC user plane node management information | TimeSensitiveNetworking |
| tsnPortManContDstt | PortManagementContainer | O | 0..1 | Transports port management information for the DS-TT port. | TimeSensitiveNetworking |
| tsnPortManContNwtts | array(PortManagementContainer) | O | 1..N | Transports port management information for one or more NW-TT ports. | TimeSensitiveNetworking |
| redSessIndication | boolean | O | 0..1 | Indicates whether the PDU Session is a redundant PDU session:true: end to end redundant PDU session;false: Not end to end redundant PDU session;If this attribute is absent it means the PDU session is not an end to end redundant PDU session.(NOTE 2) (NOTE 3) | Dual-Connectivity-redundant-UP-paths |
| uePolCont | UePolicyContainer | O | 0..1 | Indicates a UE policy container for the UE. Only applicable to the 5GS and EPC interworking scenario as defined in Annex B. | EspUrsp |
| NOTE 1: For IPv4v6 PDU session, both the "ipv4Index" attribute and "ipv6Index" attribute may be provisioned by the PCF.NOTE 2: This attribute shall not be removed if it was provisioned.NOTE 3: This attribute may only be supplied by the PCF in the response to the initial POST request that requested the creation of an individual SM policy resource.NOTE 4: If both the "offline" attribute and the "online" attribute are omitted by the PCF, and when the "OfflineChOnly" feature is supported, if the "offlineChOnly" attribute is set to "false" or omitted by the PCF, the default charging method pre-configured at the SMF, if available, shall be applied to the PDU session. If both offline and online charging methods are pre-configured at the SMF, the SMF shall determine which one of them to be applied to the PDU session based on local policy. The "offline" attribute and the "online" attribute shall not be simultaneously present with the same value, i.e., both set to true or both set to false.NOTE 5: If the "chargingInfo" attribute is not supplied by the PCF, the charging information configured at the SMF shall be applied to the PDU session.NOTE 6: When the "OfflineChOnly" feature is supported and the "offlineChOnly" attribute is present and set to "true", the "online" attribute and the "offline" attribute shall not be present. |

\* \* \* Next Change \* \* \* \*

#### 5.6.2.19 Type SmPolicyUpdateContextData

Table 5.6.2.19-1: Definition of type SmPolicyUpdateContextData

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| repPolicyCtrlReqTriggers | array(PolicyControlRequestTrigger) | C | 1..N | The policy control request triggers which are met. It is omitted if no triggers are met such as in clauses 4.2.4.7 and 4.2.4.15. |  |
| accNetChIds | array(AccNetChId) | O | 1..N | Indicates the access network charging identifier for the whole PDU session. For EPS interworking scenarios, it indicates the access network charging identifier for the PCC rule(s) or the whole PDU session. |  |
| accessType | AccessType | O | 0..1 | The Access Type where the served UE is camping. |  |
| ratType | RatType | O | 0..1 | The RAT Type where the served UE is camping. |  |
| addAccessInfo | AdditionalAccessInfo | O | 0..1 | Indicates the combination of added Access Type and RAT Type for MA PDU session. | ATSSS |
| relAccessInfo | AdditionalAccessInfo | O | 0..1 | Indicates the combination of released Access Type and RAT Type for MA PDU session. | ATSSS |
| servingNetwork | PlmnIdNid | O | 0..1 | The serving network (a PLMN or an SNPN) where the served UE is camping. For the SNPN the NID together with the PLMN ID identifies the SNPN. |  |
| userLocationInfo | UserLocation | O | 0..1 | The location(s) where the served UE is camping. (NOTE 4) |  |
| ueTimeZone | TimeZone | O | 0..1 | The time zone where the served UE is camping. |  |
| ipv4Address | Ipv4Addr | O | 0..1 | The IPv4 Address of the served UE. |  |
| ipDomain | string | O | 0..1 | IPv4 address domain identifier.(NOTE 2) |  |
| relIpv4Address | Ipv4Addr | O | 0..1 | Indicates the released IPv4 Address of the served UE. |  |
| ipv6AddressPrefix | Ipv6Prefix | O | 0..1 | The Ipv6 Address Prefix of the served UE. |  |
| relIpv6AddressPrefix | Ipv6Prefix | O | 0..1 | Indicates the released IPv6 Address Prefix of the served UE in multi-homing case. |  |
| relUeMac | MacAddr48 | O | 0..1 | Indicates the released MAC Address of the served UE. |  |
| ueMac | MacAddr48 | O | 0..1 | The MAC Address of the served UE. |  |
| subsSessAmbr | Ambr | O | 0..1 | UDM subscribed or DN-AAA authorized Session-AMBR. |  |
| authProfIndex | string | O | 0..1 | DN-AAA authorization profile index. | DN-Authorization |
| subsDefQos | SubscribedDefaultQos | O | 0..1 | Subscribed Default QoS Information. |  |
| vplmnQos | VplmnQos | O | 0..1 | QoS constraints in a VPLMN (NOTE 5) | VPLMN-QoS-Control |
| vplmnQosNotApp | boolean | O | 0..1 | If it is included and set to true, indicates that the QoS constraints in the VPLMN are not applicable. (NOTE 5) | VPLMN-QoS-Control |
| numOfPackFilter | integer | O | 0..1 | Contains the number of supported packet filter for signalled QoS rules.(NOTE 1) |  |
| accuUsageReports | array(AccuUsageReport) | O | 1..N | Contains the accumulated usage report(s). | UMC |
| 3gppPsDataOffStatus | boolean | O | 0..1 | If it is included and set to true, the 3GPP PS Data Off is activated by the UE. | 3GPP-PS-Data-Off  |
| appDetectionInfos | array(AppDetectionInfo) | O | 1..N | Reports the start/stop of the application traffic and detected SDF descriptions if applicable. | ADC |
| ruleReports | array(RuleReport) | O | 1..N | Used to report the PCC rule failure. |  |
| sessRuleReports | array(SessionRuleReport) | O | 1..N | Used to report the session rule failure. | SessionRuleErrorHandling |
| qncReports | array(QosNotificationControlInfo) | O | 1..N | QoS Notification Control information. |  |
| qosMonReports | array(QosMonitoringReport) | O | 1..N | QoS Monitoring reporting information. | QosMonitoring |
| userLocationInfoTime | DateTime | O | 0..1 | Contains the NTP time at which the UE was last known to be in the location. (NOTE 3) |  |
| repPraInfos | map(PresenceInfo) | O | 1..N | Reports the changes of presence reporting area. The "praId" attribute within the PresenceInfo data type shall also be the key of the map. The "presenceState" attribute within the PresenceInfo data type shall be supplied. The "additionalPraId" attribute within the PresenceInfo data type shall not be supplied. | PRA |
| ueInitResReq | UeInitiatedResourceRequest | O | 0..1 | Indicates a UE requests specific QoS handling for selected SDF. |  |
| refQosIndication | boolean | O | 0..1 | If it is included and set to true, the reflective QoS is supported by the UE. If it is included and set to false, the reflective QoS is revoked by the UE. |  |
| qosFlowUsage | QosFlowUsage | O | 0..1 | Indicates the required usage for default QoS flow. |  |
| creditManageStatus | CreditManagementStatus | O | 0..1 | Indicates the reason of the credit management session failure. |  |
| servNfId | ServingNfIdentity | O | 0..1 | Contains the serving network function identity. |  |
| traceReq | TraceData | C | 0..1 | It shall be included if trace is required to be activated, modified or deactivated (see 3GPP TS 32.422 [24]). For trace modification, it shall contain a complete replacement of trace data.For trace deactivation, it shall contain the Null value. |  |
| addIpv6AddrPrefixes | array(Ipv6Prefix) | O | 1..N | The Ipv6 Address Prefixes of the served UE. (NOTE 6) | MultiIpv6AddrPrefix |
| addRelIpv6AddrPrefixes | array(Ipv6Prefix) | O | 1..N | Indicates the released IPv6 Address Prefixes of the served UE in multi-homing case. (NOTE 6) | MultiIpv6AddrPrefix |
| tsnBridgeInfo | TsnBridgeInfo | O | 0..1 | Transports TSN bridge information. | TimeSensitiveNetworking |
| tsnBridgeManCont | BridgeManagementContainer | O | 0..1 | Transports TSN bridge management information. | TimeSensitiveNetworking |
| tsnPortManContDstt | PortManagementContainer | O | 0..1 | Transports TSN port management information for the DS-TT port. | TimeSensitiveNetworking |
| tsnPortManContNwtts | array(PortManagementContainer) | O | 1..N | Transports TSN port management information for one or more NW-TT ports. | TimeSensitiveNetworking |
| maPduInd | MaPduIndication | O | 0..1 | Contains the MA PDU session indication, i.e., MA PDU Request or MA PDU Network-Upgrade Allowed. (NOTE 1) | ATSSS |
| atsssCapab | AtsssCapability | O | 0..1 | Contains the ATSSS capability supported for the MA PDU session. (NOTE 1) | ATSSS |
| mulAddrInfos | array(IpMulticastAddressInfo) | O | 1..N | Contains the IP multicast address information. | WWC |
| policyDecFailureReports | array(PolicyDecisionFailureCode) | O | 1..N | Indicates the type(s) of the failed policy decision and/or condition data. | PolicyDecisionErrorHandling |
| invalidPolicyDecs | array(InvalidParam) | O | 1..N | Indicates the invalid parameters for the reported type(s) of the failed policy decision and/or condition data. | ExtPolicyDecisionErrorHandling |
| trafficDescriptors | array(DddTrafficDescriptor) | O | 1..N | Contains the traffic descriptor(s) | DDNEventPolicyControl |
| typesOfNotif | array(DlDataDeliveryStatus) | O | 1..N | Contains the type of notification of DDD Status. | DDNEventPolicyControl |
| pccRuleId | string | O | 0..1 | Contains the identifier of the PCC rule which is used for traffic detection of event (e.g. DDN failure). | DDNEventPolicyControl2 |
| interGrpIds | array(GroupId) | O | 1..N | Internal Group Identifier(s) of the served UE. | GroupIdListChange |
| satBackhaulCategory | SatelliteBackhaulCategory | O | 0..1 | Satellite backhaul category or non-satellite backhaul used for the PDU session. | SatBackhaulCategoryChg |
| pcfUeInfo | PcfUeCallbackInfo | O | 0..1 | PCF for the UE callback URI and SBA binding information. | AMInfluence |
| nwdafDatas | array(NwdafData) | O | 1..N | List of NWDAF Instance IDs and their associated Analytics IDs consumed by the NF service consumer. | EneNA |
| anGwStatus | boolean | O | 1..N | When it is included and set to true, it indicates that the AN-Gateway has failed and that the PCF should refrain from sending policy decisions to the SMF until it is informed that the AN-Gateway has been recovered. (NOTE 1) | SGWRest |
| uePolCont | UePolicyContainer  | C | 0..1 | Indicates a UE policy container received from the UE. (NOTE 1) | EpsUrsp |
| NOTE 1: This attribute is only applicable to the 5GS and EPC/E-UTRAN interworking scenario as defined in Annex B.NOTE 2: The value provided in this attribute is implementation specific. The only constraint is that the NF service consumer shall supply a different identifier for each overlapping address domain (e.g. the SMF NF instance identifier).NOTE 3: The age of UE location included within the "userLocationInfoTime" attribute is the age of the 3GPP access UE location received from the AMF and shall be included only when the reported "userLocationInfo" attribute includes the UE location in the 3GPP access.NOTE 4: The SMF may encode both 3GPP and non-3GPP access UE location in the "userLocationInfo" attribute.NOTE 5: Only one of "vplmnQos" or "vplmnQosNotApp" attributes may be present.NOTE 6: When the "WWC" feature is supported, IPv6 prefix(es) shorter than /64 or full IPv6 address(es) with a /128 prefix may be encoded as the "addIpv6Prefixes" and the "addRelIpv6Prefixes" attributes, according to 3GPP TS 23.316 [42], clause 8.3.1 and 4.6.2. |

\* \* \* Next Change \* \* \* \*

#### 5.6.3.2 Simple data types

The simple data types defined in table 5.6.3.2-1 shall be supported. For additional simple data types see 3GPP TS 29.571 [11].

Table 5.6.3.2-1: Simple data types

|  |  |  |  |
| --- | --- | --- | --- |
| Type Name | Type Definition | Description | Applicability |
| 5GSmCause | Uinteger | Indicates the 5GSM cause code value as defined in clause 9.11.4.2 of 3GPP TS 24.501 [20]. | RAN-NAS-Cause |
| EpsRanNasRelCause | string | Indicates the RAN or NAS release cause code information in 3GPP-EPS access type or indicates the TWAN or untrusted WLAN release cause code information in Non-3GPP-EPS access type. It shall be coded as per the RAN/NAS Cause in clause 8.103 of 3GPP TS 29.274 [37], starting with Octet 5. | RAN-NAS-Cause |
| FlowDescription | string | Defines a packet filter for an IP flow.Refer to clause 5.4.2 of 3GPP TS 29.212 [23] for encoding. |  |
| PacketFilterContent | string | Defines a packet filter for an IP flow.Refer to clause 5.3.54 of 3GPP TS 29.212 [23] for encoding. |  |
| TsnPortNumber | Uinteger | Port number of a DS-TT or NW-TT port. | TimeSensitiveNetworking |
| ApplicationDescriptor | Bytes | Defines the OS Id and the OS application identifier for an ATSSS rule, where the OS Id is optional. It is a sequence of octets representing the traffic descriptor(s) of the ATSSS rule as Os Id, if applicable, and Os App Id as defined in table 6.1.3.2-1 of 3GPP TS 24.193 [43]. | ATSSS |
| UePolicyContainer | Bytes | Defines a UE policy delivery service message. Refer to Annex D.5 of 3GPP TS 24.501 [20] for encoding. | EpsUrsp |

\* \* \* Next Change \* \* \* \*

#### 5.6.3.6 Enumeration: PolicyControlRequestTrigger

Table 5.6.3.6-1: Enumeration PolicyControlRequestTrigger

|  |  |  |
| --- | --- | --- |
| Enumeration value | Description | Applicability |
| PLMN\_CH | PLMN Change. |  |
| RES\_MO\_RE | A request for resource modification has been received by the NF service consumer. (NOTE) |  |
| AC\_TY\_CH | Access Type Change. It also indicates the addition or removal of Access Type for MA PDU session. |  |
| UE\_IP\_CH | UE IP address change. (NOTE) |  |
| UE\_MAC\_CH | A new UE MAC address is detected or a used UE MAC address is inactive for a specific period. |  |
| AN\_CH\_COR | Access Network Charging Correlation Information. |  |
| US\_RE | The PDU Session or the Monitoring key specific resources consumed by a UE either reached the threshold or needs to be reported for other reasons. | UMC |
| APP\_STA | The start of application traffic has been detected. | ADC |
| APP\_STO | The stop of application traffic has been detected. | ADC |
| AN\_INFO | Access Network Information report. | NetLoc |
| CM\_SES\_FAIL | Credit management session failure. |  |
| PS\_DA\_OFF | The NF service consumer reports when the 3GPP PS Data Off status changes. (NOTE) | 3GPP-PS-Data-Off |
| DEF\_QOS\_CH | Default QoS Change. (NOTE) |  |
| SE\_AMBR\_CH | Session-AMBR Change. (NOTE) |  |
| QOS\_NOTIF | The NF service consumer notify the PCF when receiving notification from RAN that QoS targets of the QoS Flow cannot be guaranteed or can be guaranteed. |  |
| NO\_CREDIT | Out of credit. |  |
| REALLO\_OF\_CREDIT | Reallocation of credit | ReallocationOfCredit |
| PRA\_CH | Change of UE presence in Presence Reporting Area. | PRA |
| SAREA\_CH | Location Change with respect to the Serving Area. |  |
| SCNN\_CH | Location Change with respect to the Serving CN node. |  |
| RE\_TIMEOUT | Indicates the NF service consumer generated the request because there has been a PCC revalidation timeout (i.e. Enforced PCC rule request defined in table 6.1.3.5.-1 of 3GPP TS 23.503 [6]). |  |
| RES\_RELEASE | Indicates that the NF service consumer can inform the PCF of the outcome of the release of resources for those rules that require so. | RAN-NAS-Cause |
| SUCC\_RES\_ALLO | Indicates that the NF service consumer shall inform the PCF of the successful resource allocation for those rules that requires so. |  |
| RAT\_TY\_CH | RAT type change. |  |
| REF\_QOS\_IND\_CH | Reflective QoS indication Change. |  |
| NUM\_OF\_PACKET\_FILTER | Indicates that the NF service consumer shall report the number of supported packet filter for signalled QoS rules. (NOTE) Only applicable to the interworking scenario as defined in Annex B. |  |
| UE\_STATUS\_RESUME | Indicates that the UE's status is resumed. Only applicable to the interworking scenario as defined in Annex B. | PolicyUpdateWhenUESuspends |
| UE\_TZ\_CH | UE Time Zone Change. |  |
| AUTH\_PROF\_CH | Indicates that the DN-AAA authorization profile index has changed. (NOTE) | DN-Authorization |
| TSN\_BRIDGE\_INFO | Indicates the NF service consumer has detected information about new TSC user plane node port(s), and/or new/updated UMIC and/or PMIC(s). | TimeSensitiveNetworking |
| QOS\_MONITORING | Indicates that the NF service consumer notifies the PCF of the QoS Monitoring information. | QosMonitoring |
| SCELL\_CH | Location Change with respect to the Serving Cell. |  |
| USER\_LOCATION\_CH | Indicates that user location has changed, applicable to serving area change and serving cell change. | AggregatedUELocChanges |
| EPS\_FALLBACK | EPS Fallback report is enabled in the NF service consumer. Only applicable to the interworking scenario as defined is Annex B. | EPSFallbackReport |
| MA\_PDU | Indicates that the NF service consumer notifies the PCF of the MA PDU session request. Only applicable to the interworking scenario as defined in Annex B. (NOTE) | ATSSS |
| 5G\_RG\_JOIN | The 5G-RG has joined to an IP Multicast Group. | WWC |
| 5G\_RG\_LEAVE | The 5G-RG has left an IP Multicast Group. | WWC |
| DDN\_FAILURE | Indicates that the NF service consumer requests policies from PCF if it received an event subscription for DDN Failure event. | DDNEventPolicyControl |
| DDN\_DELIVERY\_STATUS | Indicates that the NF service consumer requests policies from PCF if it received an event subscription for DDN Delievery Status event. | DDNEventPolicyControl |
| GROUP\_ID\_LIST\_CHG | UE Internal Group Identifier(s) has changed: the NF service consumer reports that UDM provided list of group Ids has changed. (NOTE) | GroupIdListChange |
| DDN\_FAILURE\_CANCELLATION | Indicates that the event subscription for DDN Failure event is cancelled. | DDNEventPolicyControl2 |
| DDN\_DELIVERY\_STATUS\_CANCELLATION | Indicates that the event subscription for DDD STATUS is cancelled. | DDNEventPolicyControl2 |
| VPLMN\_QOS\_CH | Indicates that the NF service consumer has detected the change of the QoS supported in the VPLMN, the change from the case where the QoS constraints are applicable to the case where the QoS constraints are not applicable (e.g. the UE moves back from the home routed to the non-roaming scenario) or vice versa. (NOTE) | VPLMN-QoS-Control |
| SUCC\_QOS\_UPDATE | Indicates that the NF service consumer notifies the PCF of the successful update of the QoS for MPS.  | MPSforDTS |
| SAT\_CATEGORY\_CHG | Indicates that the SMF has detected a change between different satellite category, or non-satellite backhaul. | SatBackhaulCategoryChg |
| PCF\_UE\_NOTIF\_IND | Indicates the SMF has detected the AMF forwarded the PCF for the UE indication to receive/stop receiving notifications of SM Policy association established/terminated events.(NOTE) | AMInfluence |
| NWDAF\_DATA\_CHG | Indicates that the NWDAF instance IDs used for the PDU session and/or associated Analytics IDs have changed. (NOTE) | EneNA |
| UE\_POL\_CONT\_IND | Indicates that the NF service consumer has detected a new UE policy container. Only applicable to the interworking scenario as defined in Annex B. | EprsUrsp |
| NOTE: The NF service consumer always reports to the PCF. |

The PCF may provision the values of policy control request trigger which are not always reported by the NF service consumer as defined in clause 4.2.6.4.

When the NF service consumer detects the corresponding policy control request trigger(s), the NF service consumer shall report the detected trigger(s) to the PCF as defined in clause 4.2.4.1 with the additional information for different independent policy control request triggers as follows:

If the "PLMN\_CH" is provisioned, when the NF service consumer detects a change of the serving network (a PLMN or an SNPN), the NF service consumer shall include the "PLMN\_CH" within the "repPolicyCtrlReqTriggers" attribute and the current identifier of the serving network within the "servingNetwork" attribute.

NOTE 1: Handover between non-equivalent SNPNs, and between SNPN and PLMN is not supported. When the UE is operating in SNPN access mode, the trigger reports changes of equivalent SNPNs.

When the NF service consumer receives the resource modification request from the UE, the NF service consumer shall include the "RES\_MO\_RE" within the "repPolicyCtrlReqTriggers" attribute and the information for requesting the PCC rule as defined in clause 4.2.4.17.

If the "AC\_TY\_CH" is provisioned, when the NF service consumer detects a change of access type, the NF service consumer shall include the "AC\_TY\_CH" within the "repPolicyCtrlReqTriggers" attribute and the current access type within the "accessType" attribute. The RAT type encoded in the "ratType" attribute shall also be provided when applicable to the specific access type. Specific attributes for the EPC interworking case are described in Annex B. If the ATSSS feature is supported, when the NF service consumer detects an access is added or released for MA PDU session, the NF service consumer shall include the added Access Type or released Access type encoded as "accessType" attribute within the AdditionalAccessInfo data structure. The RAT type encoded in the "ratType" attribute shall also be provided within the AdditionalAccessInfo data structure when applicable to the added access type or released access type.

When the NF service consumer detects an IPv4 address and/or an IPv6 prefix is allocated or released, the NF service consumer shall include the "UE\_IP\_CH" within the "repPolicyCtrlReqTriggers" attribute and new allocated UE Ipv4 address within the "ipv4Address" attribute and/or the UE Ipv6 prefix within the "ipv6AddressPrefix" attribute or the released UE Ipv4 address within the "relIpv4Address" attribute and/or the UE Ipv6 prefix within the "relIpv6AddressPrefix" attribute. If the "MultiIpv6AddrPrefix" feature is supported ,and if multiple allocated or released IPv6 prefixes are detected, the NF service consumer shall include the new allocated UE Ipv6 prefixes within the "addIpv6AddrPrefixes" attribute and the released UE Ipv6 prefixes within the "addRelIpv6AddrPrefixes" attribute.

When the NF service consumer detects a new UE MAC address or a used UE MAC address is not used any more, the NF service consumer shall include the "UE\_MAC\_CH" within the "repPolicyCtrlReqTriggers" attribute and new detected UE MAC address within the "ueMac" attribute or the not used UE MAC address within the "relUeMac" attribute.

If the "AN\_CH\_COR" is provisioned, when the NF service consumer is provisioned with the PCC rule as defined in clause 4.2.6.5.1, the NF service consumer shall notify the PCF of access network charging identifier associated with the PCC rules as defined in clause 4.2.4.13.

If the "US\_RE" is provisioned, when the NF service consumer receives the usage report from the UPF, the NF service consumer shall notify the PCF of the accumulated usage as defined in clause 4.2.4.10. Applicable to functionality introduced with the UMC feature as described in clause 5.8.

If the "APP\_STA" is provisioned, when the NF service consumer receives the application start report from the UPF, the NF service consumer shall notify the PCF of the application start report as defined in clause 4.2.4.6. Applicable to functionality introduced with the ADC feature as described in clause 5.8.

If the "APP\_STO" is provisioned, when the NF service consumer receives the application stop report from the UPF, the NF service consumer shall notify the PCF of the application stop report as defined in clause 4.2.4.6. Applicable to functionality introduced with the ADC feature as described in clause 5.8.

If the "AN\_INFO" is provisioned, when the NF service consumer receives the reported access network information from the access network, the NF service consumer shall notify the PCF of the access network information as defined in clause 4.2.4.9. Applicable to functionality introduced with the NetLoc feature as described in clause 5.8.

If the "CM\_SES\_FAIL" is provisioned, when the NF service consumer receives a detected transient/permanent failure from the CHF, the NF service consumer shall include the "CM\_SES\_FAIL" within the "repPolicyCtrlReqTriggers" attribute. If the failure does not apply to all PCC Rules, the affected PCC Rules are indicated within the "ruleReports" attribute, with the "ruleStatus" attribute set to value ACTIVE and the "failureCode" attribute set to the corresponding value as reported by the CHF; otherwise if the failure applies to the session, the "creditManageStatus" shall be set to the corresponding value as reported by the CHF.

If the "PS\_DA\_OFF" is provisioned, when the NF service consumer receives a change of 3GPP PS Data Off status from the UE, the NF service consumer shall notify the PCF as defined in clause 4.2.4.8. Applicable to functionality introduced with the 3GPP-PS-Data-Off feature as described in clause 5.8.

When the NF service consumer detects a change of subscribed default QoS, the NF service consumer shall include the "DEF\_QOS\_CH" within the "repPolicyCtrlReqTriggers" attribute and the new subscribed default QoS within the "subsDefQos" attribute.

When the NF service consumer detects a change of Session-AMBR, the NF service consumer shall include the "SE\_AMBR\_CH" within the "repPolicyCtrlReqTriggers" attribute and the new Session-AMBR within the "subsSessAmbr" attribute.

If the "QOS\_NOTIF" is provisioned, when the NF service consumer receives a notification from access network that QoS targets of the QoS Flow cannot be guaranteed or can be guaranteed again, the NF service consumer shall send the notification as defined in clause 4.2.4.20.

If the "NO\_CREDIT" is provisioned, when the NF service consumer detects the credit for the PCC rule(s) is no longer available, the NF service consumer shall include the "NO\_CREDIT" within the "repPolicyCtrlReqTriggers" attribute, the termination action the NF service consumer applies to the PCC rules as instructed by the CHF within the "finUnitAct" attribute and the affected PCC rules within the "ruleReports" attribute.

When the "ReallocationOfCredit" feature is supported, if the "REALLO\_OF\_CREDIT" is provisioned, when the NF service consumer detects the credit for the PCC rule(s) is reallocated, the NF service consumer shall include the "REALLO\_OF\_CREDIT" within the "repPolicyCtrlReqTriggers" attribute and include the affected PCC rules for which credit has been reallocated after credit was no longer available and the "ruleStatus" attribute set to value ACTIVE within the "ruleReports" attribute.

If the "PRA\_CH" is provisioned, to detect when the UE enters/leaves certain presence reporting areas, the NF service consumer is provisioned the presence reporting area information as defined in clause 4.2.6.5.6. When the NF service consumer receives the presence reporting area information from the serving node, the NF service consumer shall notify the PCF of the reported presence area information as defined in clause 4.2.4.16. This report includes reporting the initial status at the time the request for reports is initiated. Applicable to the functionality introduced by the PRA or ePRA feature as described in clause 5.8.

If the "SAREA\_CH" is provisioned, when the NF service consumer detects a change of serving area (i.e. tracking area, or if the feature "2G3GIWK" is supported routing area), the NF service consumer shall include the "SAREA\_CH" within the "repPolicyCtrlReqTriggers" attribute and the current TAI within the "userLocationInfo" attribute in either the "eutraLocation" or "nrLocation", or the current Routing Area within the "userLocationInfo" attribute in the "utraLocation" attribute when UTRAN access, or in the "geraLocation" attribute when GERAN access, as applicable. Non-3GPP access user location is reported in the "n3gaLocation" attribute when applicable. The attributes used in case of EPC interworking are described in Annex B.

If the "SCNN\_CH" is provisioned, when the NF service consumer detects a change of serving Network Function (i.e. the AMF, ePDG, S-GW or if the feature "2G3GIWK" is supported SGSN), the NF service consumer shall include the "SCNN\_CH" within the "repPolicyCtrlReqTriggers" attribute and the current serving Network Function in the "servNfId" attribute if available. When the serving Network Function is an AMF, the NF service consumer shall include the AMF Network Function Instance Identifier within the "servNfInstId" attribute and the Globally Unique AMF Identifier within the "guami" attribute. The attributes included in case of EPC interworking are described in Annex B.

NOTE 1: In the home-routed roaming case, if the AMF change is unknown to the H-SMF, then the AMF change is not reported.

If the "RE\_TIMEOUT" is provisioned, when the NF service consumer is provisioned with the revalidation time by the PCF, the NF service consumer shall request the policy before the indicated revalidation time is reached as defined in clause 4.2.4.3.

If the "RES\_RELEASE" is provisioned, when the NF service consumer receives the request of PCC rule removal as defined in clause 4.2.6.5.2, the NF service consumer shall report the outcome of resource release as defined in clause 4.2.4.12. Applicable to functionality introduced with the RAN-NAS-Cause feature as described in clause 5.8.

When "SUCC\_RES\_ALLO" is provisioned and PCC rules are provisioned according to clause 4.2.6.5.5, the NF service consumer shall inform the PCF of the successful resource allocation as defined in clause 4.2.4.14.

If the feature "2G3GIWK" is supported, and if the "RAI\_CH" is provisioned, when the NF service consumer detects a change of routing area, the NF service consumer shall include the "RAI\_CH" within the "repPolicyCtrlReqTriggers" attribute and the current RAI within the "userLocationInfo" attribute as described in Annex B.

If the "RAT\_TY\_CH" is provisioned, when the NF service consumer detects a change of the RAT type, the NF service consumer shall include the "RAT\_TY\_CH" within the "repPolicyCtrlReqTriggers" attribute and the current RAT type within the "ratType" attribute. For MA PDU session, the NF service consumer shall include the current RAT type at the SmPolicyUpdateContextData data type level or AdditionalAccessInfo data type level. If the RAT type is provided at the SmPolicyUpdateContextData data type level, the NF service consumer shall also provide the associated access type within the SmPolicyUpdateContextData data structure.

If the "REF\_QOS\_IND\_CH" is provisioned, when the NF service consumer receives a change of reflective QoS indication from the UE, the NF service consumer shall include the "REF\_QOS\_IND\_CH" within the "repPolicyCtrlReqTriggers" attribute and the indication within the "refQosIndication" attribute.

When the NF service consumer receives the number of supported packet filter for signalled QoS rules for the PDU session from the UE during the PDU Session Modification procedure after the first inter-system change from EPS to 5GS for a PDU Session established in EPS and transferred from EPS with N26 interface, the NF service consumer shall include the "NUM\_OF\_PACKET\_FILTER" within the "repPolicyCtrlReqTriggers" attribute and the number of supported packet filter for signalled QoS rules within the "numOfPackFilter" attribute. Only applicable to the interworking scenario as defined in Annex B.

If the "UE\_STATUS\_RESUME" is provisioned, when the NF service consumer detected the UE's status is resumed from suspend state, the NF service consumer shall inform the PCF of the UE status including the "UE\_STATUS\_RESUME" within "repPolicyCtrlReqTriggers" attribute. The PCF shall after this update the NF service consumer with PCC Rules or session rules if necessary. Applicable to functionality introduced with the PolicyUpdateWhenUESuspends feature as described in clause 5.8.

If the "UE\_TZ\_CH" is provisioned, when the NF service consumer detects a change of the UE Time Zone, the NF service consumer shall include the "UE\_TZ\_CH" within the "repPolicyCtrlReqTriggers" attribute and the current UE Time Zone within the "ueTimeZone" attribute.

If the "DN-Authorization" feature is supported, when the NF service consumer detects a change of DN-AAA authorization profile index, the NF service consumer shall include the "AUTH\_PROF\_CH" within the "repPolicyCtrlReqTriggers" attribute and the new DN-AAA authorization profile index within the "authProfIndex" attribute.

If the "TimeSensitiveNetworking" or "TimeSensitiveCommunication" feature is supported and "TSN\_BRIDGE\_INFO" is provisioned, when the NF service consumer detects:

- there is information about new TSC user plane node port(s), e.g. a new manageable Ethernet port, the NF service consumer shall include the "TSN\_BRIDGE\_INFO" within the "repPolicyCtrlReqTriggers" attribute and the updated TSC user plane node information within the "tsnBridgeInfo" attribute; and/or

- the NF service consumer detects a UMIC or PMIC, the NF service consumer shall include the "TSN\_BRIDGE\_INFO" within the "repPolicyCtrlReqTriggers" attribute and the UMIC, if available, within the "tsnBridgeManCont" attribute, and/or the PMIC(s), if available, within the "tsnPortManContDstt" and the "tsnPortManContNwtts" attributes.

NOTE 2: When the NF service consumer detects updated Port Management Information of the NW-TT ports, the NF service consumer includes the PMIC within the "tsnPortManContNwtts" attribute of SmPolicyUpdateContextData data type.

If the "QoSMonitoring" feature is supported and if the "QOS\_MONITORING" is provisioned, upon receiving the QoS Monitoring report from the UPF, the NF service consumer shall send the QoS monitoring report for the concerned PC rules to the PCF as defined in clause 4.2.4.24.

If the "SCELL\_CH" is provisioned, when the NF service consumer detects a change of serving cell, the NF service consumer shall include the "SCELL\_CH" within the "repPolicyCtrlReqTriggers" attribute and the current cell Id within the "userLocationInfo" attribute either in the "eutraLocation" attribute when EPC/E-UTRAN access or "nrLocation" attribute when NR access or "geraLocation" attribute when GERAN access or "utraLocation" attribute when UTRAN access, as applicable.

NOTE 3: Location change of serving cell can increase signalling load on multiple interfaces. Hence, it is recommended that any such serving cell changes event trigger subscription is only applied for a limited number of subscribers.

If the "AggregatedUELocChanges" feature is supported and the "USER\_LOCATION\_CH" is provisioned, when the NF service consumer detects a change of serving cell and/or a change of serving area (i.e. tracking area), the NF service consumer shall include the "USER\_LOCATION\_CH" within the "repPolicyCtrlReqTriggers" attribute and the current serving area and/or cell Id within the "userLocationInfo" attribute in the "eutraLocation" attribute or "nrLocation" attribute or "geraLocation" attribute or "utraLocation" attribute, as applicable.

NOTE 4: The access network can be configured to report location changes only when transmission resources are established in the radio access network.

If the "EPSFallbackReport" feature is supported and the "EPS\_FALLBACK" is provisioned and there is a PCC rule installed that required the reporting, when the NF service consumer receives a PDU session modification response indicating the rejection of the establishment of the QoS flow with 5QI=1, the NF service consumer shall notify the PCF of EPS fallback as defined in clause B.3.4.6.

When the NF service consumer receives the MA PDU Request Indication or MA PDU Network-Upgrade Allowed Indication and ATSSS Capability from the UE during the PDU Session Modification procedure after the first inter-system change from EPS to 5GS for a PDU Session established in EPS and transferred from EPS with N26 interface, the NF service consumer shall include the "MA\_PDU" within the "repPolicyCtrlReqTriggers" attribute, the MA PDU session Indication in the "maPduInd" attribute, the ATSSS capability of the MA PDU session within the "atsssCapab" attribute. Only applicable to the interworking scenario as defined in Annex B.

If the "WWC" feature is supported and "5G\_RG\_JOIN" is provisioned and when the NF service consumer detects a 5G-RG has joined to an IP Multicast Group, the NF service consumer shall include the "5G\_RG\_JOIN" within the "repPolicyCtrlReqTriggers" attribute and the IP multicast addressing information within the "mulAddrInfos" attribute.

If the "WWC" feature is supported and "5G\_RG\_LEAVE" is provisioned and when the NF service consumer detects a 5G-RG has left an IP Multicast Group, the NF service consumer shall include the "5G\_RG\_LEAVE" within the "repPolicyCtrlReqTriggers" attribute and the IP multicast addressing information within the "mulAddrInfos" attribute.

If "DDNEventPolicyControl" feature is supported, and if "DDN\_FAILURE" is provisioned, when the NF service consumer receives an event subscription for DDN Failure event including the traffic descriptors, the NF service consumer shall include the "DDN\_FAILURE" within the "repPolicyCtrlReqTriggers" attribute and traffic descriptor(s) within the "trafficDescriptors" attribute.

If "DDNEventPolicyControl" feature is supported, and if "DDN\_DELIVERY\_STATUS" is provisioned, when the NF service consumer receives an event subscription for DDD Status event including the traffic descriptors, the NF service consumer shall include the "DDN\_DELIVERY\_STATUS" within the "repPolicyCtrlReqTriggers" attribute and traffic descriptor(s) within the "trafficDescriptors" attribute and the requested type(s) of notifications (notifications about downlink packets being buffered, and/or discarded).

If "GroupIdListChange" feature is supported, when the SMF receives the updated Internal Group Identifier(s) from the UDM, the SMF shall include the "GROUP\_ID\_LIST\_CHG" within the "repPolicyCtrlReqTriggers" attribute and the Internal Group Identifier(s) of the served UE within the "interGrpIds" attribute.

If "DDNEventPolicyControl2" feature is supported, and if "DDN\_FAILURE\_CANCELLATION" is provisioned, when the SMF receives a cancellation of event subscription for DDN Failure event, the SMF shall include the "DDN\_FAILURE\_CANCELLATION" within the "repPolicyCtrlReqTriggers" attribute and the PCC rule identifier of the PCC rule which is used for traffic detection of DDN failure event within the "pccRuleId" attribute.

If "DDNEventPolicyControl2" feature is supported, and if "DDN\_DELIVERY\_STATUS\_CANCELLATION" is provisioned, when the SMF receives a cancellation of event subscription for DDD Status event, the SMF shall include the "DDN\_DELIVERY\_STATUS\_CANCELLATION" within the "repPolicyCtrlReqTriggers" attribute and the PCC rule identifier of the PCC rule which is used for traffic detection of DDD status event within the "pccRuleId" attribute.

When the "VPLMN-QoS-Control" feature is supported and if the NF service consumer receives a new QoS value supported in the VPLMN, the NF service consumer shall include the "VPLMN\_QOS\_CH" within the "repPolicyCtrlReqTriggers" attribute and the received QoS constraints within the "vplmnQos" attribute; if the NF service consumer detects that the UE moves from a VPLMN with QoS constraints to the HPLMN or to a VPLMN without QoS constraints, the NF service consumer shall include the "VPLMN\_QOS\_CH" within the "repPolicyCtrlReqTriggers" attribute and the "vplmnQosNotApp" attribute set to true.

If the "MPSforDTS" feature is supported, and if "SUCC\_QOS\_UPDATE" is provisioned, when the resources for the MPS for DTS invocation/revocation are successfully allocated for MPS for DTS, the NF service consumer shall include the "SUCC\_QOS\_UPDATE" within the "repPolicyCtrlReqTriggers" attribute.

If "SatBackhaulCategoryChg" feature is supported, and if "SAT\_CATEGORY\_CHG" is provisioned, the NF service consumer notifies the PCF when there is a change of the backhaul which is used for the PDU session between different satellite backhaul categories (i.e., GEO, MEO, LEO, or other satellite) or between a satellite backhaul and a non-satellite backhaul. The NF service consumer shall include the satellite backhaul category or non-satellite backhaul within the "satBackhaulCategory" attribute together with the "SAT\_CATEGORY\_CHG" policy control request trigger within the "repPolicyCtrlReqTriggers" attribute.

NOTE 5: The type (i.e. GEO, MEO, LEO or other satellite) of the satellite involved in the backhaul is referred as the satellite backhaul category. Only a single backhaul category can be indicated.

If the "AMInfluence" feature is supported, the NF service consumer notifies the PCF about the PCF for the UE request to be notified of PDU session established/terminated events by forwarding within the "pcfUeInfo" attribute, the received PCF for the UE callback URI within the "callbackUri" attribute and, if received, SBA binding information within the "bindingInfo" attribute, together with the "PCF\_UE\_NOTIF\_IND" policy control request trigger within the "repPolicyCtrlReqTriggers" attribute. The NF service consumer notifies the PCF about the PCF for the UE request to stop being notified about the PDU session established/terminated events by sending the "pcfUeInfo" attribute set to NULL together with the "PCF\_UE\_NOTIF\_IND" policy control request trigger within the "repPolicyCtrlReqTriggers" attribute.

If "EneNA" feature is supported, the NF service consumer notifies the PCF when there is a change in the list of NWDAF Instance IDs used for the PDU Session and/or associated Analytics IDs. The NF service consumer shall include within the "nwdafDatas" attribute the list of NWDAF instance IDs used for the PDU Session within the "nwdafInstanceId" attribute and their associated Analytic ID(s) within the "nwdafEvents" attribute, and the "NWDAF\_DATA\_CHG" within the "repPolicyCtrlReqTriggers" attribute.

If the "EpsUrsp" feature is supported and "UE\_POL\_CONT\_IND" is provisioned, when the NF service consumer detects a new UE policy container, the the NF service consumer shall include the "UE\_POL\_CONT\_IND" within the "repPolicyCtrlReqTriggers" attribute and the UE policy container within the "uePolCont" attribute. Only applicable to the interworking scenario as defined in Annex B.

Editor's Note: It will be aligned with SA2 (once it is specified in 3GPP TS 23.503) the name of the Policy Control Request trigger to indicate the provisioning of a UE Policy Container and whether it needs to be provisioned or the NF service consumer always reports it to the PCF.

\* \* \* Next Change \* \* \* \*

## 5.8 Feature negotiation

The optional features in table 5.8-1 are defined for the Npcf\_SMPolicyControl API. They shall be negotiated using the extensibility mechanism defined in clause 6.6 of 3GPP TS 29.500 [4].

Table 5.8-1: Supported Features

|  |  |  |
| --- | --- | --- |
| Feature number | Feature Name | Description |
| 1 | TSC | This feature indicates support for traffic steering control in the (S)Gi-LAN, steering the 5G-LAN type of services or routing of the user traffic to a local Data Network identified by the DNAI per AF request. If the NF service consumer supports this feature, the PCF shall behave as described in clause 4.2.6.2.6. |
| 2 | ResShare | This feature indicates the support of service data flows that share resources. If the NF service consumer supports this feature, the PCF shall behave as described in clause 4.2.6.2.8. |
| 3 | 3GPP-PS-Data-Off | This feature indicates the support of 3GPP PS Data off status change reporting. |
| 4 | ADC | This feature indicates the support of application detection and control. |
| 5 | UMC | Indicates that the usage monitoring control is supported. |
| 6 | NetLoc | This feature indicates the support of the Access Network Information Reporting for 5GS. |
| 7 | RAN-NAS-Cause | This feature indicates the support for the detailed release cause code information from the access network.(NOTE) |
| 8 | ProvAFsignalFlow | This feature indicates support for the feature of IMS Restoration as described in clause 4.2.3.17. If NF service consumer supports this feature the PCF may provision AF signalling IP flow information. |
| 9 | PCSCF-Restoration-Enhancement | This feature indicates support of P-CSCF Restoration Enhancement. It is used for the NF service consumer to indicate if it supports P-CSCF Restoration Enhancement. |
| 10 | PRA | This feature indicates the support of presence reporting area change reporting. The support of the update of a UE Dedicated Presence Reporting Area is unspecified. |
| 11 | RuleVersioning | This feature indicates the support of PCC rule versioning as defined in clause 4.2.6.7. |
| 12 | SponsoredConnectivity | This feature indicates support for sponsored data connectivity feature. If the NF service consumer supports this feature, the PCF may authorize sponsored data connectivity to the subscriber. |
| 13 | RAN-Support-Info | This feature indicates the support of maximum packet loss rate value(s) for uplink and/or downlink voice service data flow(s). |
| 14 | PolicyUpdateWhenUESuspends | This feature indicates the support of report when the UE is suspended and then resumed from suspend state. Only applicable to the interworking scenario as defined in Annex B. |
| 15 | AccessTypeCondition | This feature indicates the support of access type conditioned authorized Session-AMBR as defined in clause 4.2.6.3.2.4. |
| 16 | MultiIpv6AddrPrefix | This feature indicates the support of multiple Ipv6 address prefixes reporting. |
| 17 | SessionRuleErrorHandling | This feature indicates the support of session rule error handling. |
| 18 | AF\_Charging\_Identifier | This feature indicates the support of long character strings as charging identifiers. |
| 19 | ATSSS | This feature indicates the support of the access traffic switching, steering and splitting functionality as defined in clauses 4.2.6.2.17 and 4.2.6.3.4. |
| 20 | PendingTransaction | This feature indicates support for the race condition handling as defined in 3GPP TS 29.513 [7]. |
| 21 | URLLC | This feature indicates support of Ultra-Reliable Low-Latency Communication (URLLC) requirements, i.e. AF application relocation acknowledgement requirement and UE address(es) preservation. The TSC feature shall be supported in order to support this feature. |
| 22 | MacAddressRange | Indicates the support of a set of MAC addresses with a specific range in the traffic filter. |
| 23 | WWC | Indicates support of wireless and wireline convergence access as defined in annex C. |
| 24 | QosMonitoring | Indicates support of QoS monitoring as defined in clause 4.2.3.25 and 4.2.4.24. |
| 25 | AuthorizationWithRequiredQoS | Indicates support of policy authorization for the AF session with required QoS as defined in clause 4.2.3.22. |
| 26 | EnhancedBackgroundDataTransfer | Indicates the support of applying the Background Data Transfer Policy to a future PDU session. |
| 27 | DN-Authorization | This feature indicates the support of DN-AAA authorization data for policy control. |
| 28 | PDUSessionRelCause | Indicates the support of "PS\_TO\_CS\_HO" PDU session release cause. |
| 29 | SamePcf | This feature indicates the support of same PCF selection for the parameter's combination. |
| 30 | ADCmultiRedirection | This feature indicates support for multiple redirection information in application detection and control. It requires the support of ADC feature. |
| 31 | RespBasedSessionRel | Indicates support of handling PDU session termination functionality as defined in clause 4.2.4.22. |
| 32 | TimeSensitiveNetworking | Indicates that the 5G System is integrated within the external network as a TSN bridge. |
| 33 | EMDBV | This feature indicates the support of the ExtMaxDataBurstVol data type defined in 3GPP TS 29.571 [11]. The use of this data type is specified in clause 4.2.2.1. |
| 34 | DNNSelectionMode | This feature indicates the support of DNN selection mode. |
| 35 | EPSFallbackReport | This feature indicates the support of the report of EPS Fallback as defined in clauses B.3.3.2 and B.3.4.6. |
| 36 | PolicyDecisionErrorHandling | This feature indicates the support of the error report of the policy decision and/or condition data which is not referred by any PCC rule or session rule as defined in clause 4.2.3.26 and 4.2.4.26. |
| 37 | DDNEventPolicyControl | This feature indicates the support for policy control in the case of DDN Failure and Delivery Status events as defined in clause 4.2.4.27. |
| 38 | ReallocationOfCredit | This feature indicates the support of notifications of reallocation of credit. |
| 39 | BDTPolicyRenegotiation | This feature indicates the support of the BDT policy re-negotiation. |
| 40 | ExtPolicyDecisionErrorHandling | This feature indicates the support of the error report of a faulty SM policy decision parameter as defined in clause 4.2.3.26 and 4.2.4.26. It requires the support of PolicyDecisionErrorHandling feature. |
| 41 | ImmediateTermination | This feature indicates the support of the termination the PDU session when the NF service consumer cannot ensure the UE, RAN, AMF, or UPF can revert to the status before the PDU session modification occurred, as defined in clause 4.2.4.21. |
| 42 | AggregatedUELocChanges | This feature indicates the support of notifications of serving area (i.e. tracking area) and/or serving cell changes. |
| 43 | ES3XX | Extended Support for 3xx redirections. This feature indicates the support of redirection for any service operation, according to Stateless NF procedures as specified in clauses 6.5.3.2 and 6.5.3.3 of 3GPP TS 29.500 [4] and according to HTTP redirection principles for indirect communication, as specified in clause 6.10.9 of 3GPP TS 29.500 [4].  |
| 44 | GroupIdListChange | This feature indicates the support for the notification of changes in the list of internal group identifiers. |
| 45 | DisableUENotification | Indicates the support of disabling QoS flow parameters signalling to the UE when the SMF is notified by the NG-RAN of changes in the fulfilled QoS situation. This feature requires that the AuthorizationWithRequiredQoS featute is also supported. |
| 46 | OfflineChOnly | This feature enables the PCF to signal the "PDU Session with offline charging only" indication as defined in clause 4.2.2.3.3. |
| 47 | Dual-Connectivity-redundant-UP-paths | Indicates the support of policy authorization of end to end redundant user plane path using dual connectivity as described in clause 4.2.2.20. |
| 48 | DDNEventPolicyControl2 | This feature indicates the support for the policy control removal in the case of DDN Failure and/or Delivery Status event(s) is cancelled as defined in clause 4.2.4.27. The DDNEventPolicyControl feature shall be supported in order to support this feature. |
| 49 | VPLMN-QoS-Control | Indicates the support of QoS constraints from the VPLMN for the derivation of the authorized Session-AMBR and authorized default QoS. |
| 50 | 2G3GIWK | This feature indicates the support of GERAN and UTRAN access over N7 interface. |
| 51 | TimeSensitiveCommunication | Indicates that the 5G System is integrated within the external network as a TSC user plane node to enable the Time Sensitive Communications and Time Synchronization. This feature requires that the TimeSensitiveNetworking feature is also supported. |
| 52 | AF\_latency | This feature indicates the support of Edge relocation considering user plane latency. This feature requires that the TSC feature is also supported. |
| 53 | SatBackhaulCategoryChg | This feature indicates the support of notification of a change between different satellite backhaul categories, or between satellite backhaul and non-satellite backhaul. |
| 54 | CHFsetSupport | Indicates the support of CHF redundancy and failover mechanisms based on CHF instance availability within a CHF Set, as described in clause 4.2.2.3.1. |
| 55 | EnATSSS | Indicates the support of ATSSS enhancement. It requires the support of ATSSS feature. |
| 56 | MPSforDTS | Indicates support of the MPSfor DTS feature as described in clause 4.2.6.2.12.4. |
| 57 | RoutingInfoRemoval | Indicates the support of the removal of the "routeToLocs" attribute from the TrafficControlData instance. |
| 58 | ePRA | This feature indicates the support of presence reporting area change reporting. It additionally supports the update of the elements of a UE Dedicated Presence Reporting Area by the full replacement of the previously provided one comparing with the PRA feature.  |
| 59 | AMInfluence | Indicates the support of the delivery of the PCF for the UE request to be notified by the PCF for the PDU session about PDU session established/terminated events. |
| 60 | PvsSupport | This feature indicates the support of SNPN UE Remote Provisioning via User Plane as described in clause 4.2.2.21. |
| 61 | EneNA | This feature indicates the support of NWDAF data reporting. |
| 62 | BIUMR | This feature bit indicates whether the NF Service Consumer (e.g. SMF) and PCF supports Binding Indication Update for multiple resource contexts specified in clauses 6.12.1 and 5.2.3.2.6 of 3GPP TS 29.500 [4]. |
| 63 | EASIPreplacement | This feature indicates the support of EAS IP replacement. This feature requires that the TSC feature is also supported. |
| 64 | ExposureToEAS | This feature indicates the support of exposure of QoS monitoring results to local AF. This feature requires that QosMonitoring feature is also supported. |
| 65 | SimultConnectivity | This feature indicates the support of temporary simultaneously connectivity at edge relocation. This feature requires that the TSC feature is also supported.  |
| 66 | SGWRest | This feature indicates the support of SGW Restoration procedures. Only applicable to the interworking scenario as defined in Annex B. |
| 67 | ReleaseToReactivate | This feature indicates that the PCF can request the SMF for reactivation of a PDU session based on an SM Policy Association release cause. |
| 68 | EASDiscovery | This feature indicates the support of EAS (re)discovery. |
| 69 | AccNetChargId\_String | This feature indicates the support of long character strings as access network charging identifier. |
| 70 | WLAN\_Location | This feature indicates the support of the report of the WLAN location information received from the ePDG/EPC, if available. It is only applicable to EPS interworking scenarios as specified in Annex B. |
| 71 | PackFiltAllocPrecedence | This feature indicates the support of the control of the maximum number of packet filters in the EPS network in the EPS interworking scenarios as described in Annex B. |
| 72 | SatBackhaulCategoryChg\_v2 | This feature indicates the support of the indication of satellite backhaul categories, or the indication of non-satellite backhaul during the response to the update notify request. |
| 73 | UEUnreachable | This feature indicates the support for the reporting of UE temporarily unavailable. |
| 74 | AltQoSProfilesSupportReport | This feature indicates the support of the report of whether Alternative QoS parameters are supported by NG-RAN. This feature requires that AuthorizationWithRequiredQoS feature is also supported. |
| 75 | Ext2PolicyDecisionErrorHandling | This feature indicates the support of the error report of the policy decision and/or condition data which is not referred by any PCC rule or session rule when no PCC rules and no session rules are provided and the handling of partial errors.It requires the support of ExtPolicyDecisionErrorHandling feature. |
| XX | EpsUrsp | This feature indicates the support of URSP provisioning in EPS. Only applicable to the interworking scenario as defined in Annex B. |
| NOTE: 5GS and EPS release cause code information is supported. The EPS release cause code information from the access network is only applicable to EPS interworking scenarios as specified in Annex B. |

\* \* \* Next Change \* \* \* \*

## B.3.2 Npcf\_SMPolicyControl\_Create Service Operation

### B.3.2.0 General

When the UE establishes the PDN connection through the EPC network and the SMF+PGW-C receives the Create Session Request message as defined in 3GPP TS 29.274 [37], the SMF+PGW-C shall behave as defined in clause 4.2.2.2 with the differences that the SMF+PGW-C shall include (if available) in SmPolicyContextData data structure:

- the IMSI of the user within the "supi" attribute;

- the MSISDN of the user within the "gpsi" attribute;

- APN within the "dnn" attribute;

- PDU Session Id determined by the SMF+PGW-C within "pduSessionId" attribute for a UE that has an EPS subscription that allows 5GC interworking but does not support 5GC NAS.

NOTE 1: For a PDN connection established via the MME or ePDG, the PDU Session ID value is assigned from a reserved range as specified in Table 5.4.2-1 of 3GPP TS 29.571 [11]. The PDU session ID value assigned at PDN connection establishment remains unchanged along the PDN connection, i.e., it does not change when the UE handovers between EPS and EPC/ePDG. In the scenarios where UE handover between EPS and EPC/ePDG is enabled, to ensure uniqueness of the assigned PDU Session ID value, the SMF+PGW-C can retrieve from UDM the already assigned PDU Session ID values, allocate a non-colliding PDU Session ID value, and register in UDM the allocated PDU session ID;

- PDN Type within the "pduSessionType" attribute;

- IMEI-SV within the "pei" attribute;

- IP-CAN type within the "accessType" attribute;

- RAT type within the "ratType" attribute;

NOTE 2: See Annex B.3.2.2 for further information.

- subscribed APN-AMBR within "subsSessAmbr" attribute;

- subscribed Default EPS bearer QoS within "subsDefQos" attribute;

NOTE 3: Subscribed APN-AMBR and the QCI within the subscribed default EPS bearer QoS are mapped to subscribed Session-AMBR and 5QI as defined in Annex B.3.6.1 respectively.

- user location information within the "userLocationInfo" attribute;

NOTE 4: See Annex B.3.2.1 for further information.

- the S-NSSAI determined by the SMF+PGW-C within the "sliceInfo" attribute;

- the bearer usage required of the default bearer within the "qosFlowUsage" attribute;

- the UE time zone information within "ueTimeZone" attribute, if available; and

NOTE 5: The UE time zone is not available in EPC untrusted WLAN.

- UE policy container within "uePolCont" attribute, if available.

When the UE establishes the PDN connection in an 5GS-EPC interworking deployment, the SMF+PGW-C shall behave as defined in clause 4.2.2.2 (access through 5GS network) or this clause (access through the EPC network) and additionally, if the feature "PackFiltAllocPrecedence" is supported and there is a possibility to run into a restriction regarding the number of TFT packet filters that can be allocated when interworking with EPS with N26 is supported (see clause 4.11.1 of TS 23.502 [3]), the PCF may provide, as part of the PccRule data type(s) for the PCC Rules to be installed, the "packFiltAllPrec" attribute to indicate the order of the PCC Rules in the allocation of TFT packet filter(s) by the SMF+PGW-C.

NOTE 6: PCF can know that interworking with EPS with N26 is supported based on the received DNN and S-NSSAI of the PDU Session.

\* \* \* Next Change \* \* \* \*

### B.3.2.X Detection of the SM Policy Association enabling URSP provisioning in EPS

When the feature "EpsUrsp" is supported and a UE policy container is received in the "uePolCon" attribute, the PCF detects that the Npcf\_SMPolicyControl\_Create request relates to SM Policy Association enabling URSP provisioning in EPS. The PCF establishes a UE Policy Association with PCF for the UE and transparently forwards the UE policy contatiner to the PCF for the UE as described in 3GPP TS 29.525 [55].

Editor's Note: It will be aligned with SA2 (once it is specified in 3GPP TS 23.503) the name of the Policy Control Request trigger to indicate the provisioning of a UE Policy Container and whether it needs to be provisioned or the NF service consumer always reports it to the PCF.

\* \* \* Next Change \* \* \* \*

## B.3.3 Npcf\_SMPolicyControl\_UpdateNotify Service Operation

### B.3.3.Y Forwarding of UE policy container for URSP provisioning in EPS

The PCF may receive a UE policy container and/or policy control triggers from the PCF for the UE during the lifetime of the PDU session and forward it to the SMF+PGW-C by invoking the procedure defined in clause 4.2.3.2.

If the feature "EpsUrsp" is supported the PCF initiates the Npcf\_SMPolicyControl\_UpdateNotify request and transparently forwards the the UE policy container to the SMF+PGW-C via the SmPolicyDecision structure, in which the UE policy container is encoded in the "uePolCont" attribute.

\* \* \* Next Change \* \* \* \*

## B.3.4 Npcf\_SMPolicyControl\_Update Service Operation

### B.3.4.0 General

When the established PDN connection through the EPC/E-UTRAN network is modified and SMF+PGW-C receives Modify Bearer Request, Modify Bearer or Delete Bearer Command message and if the SMF detects the policy control request trigger(s) is met or the error(s) needs to be reported or when the UE handed over from the 5GS to the EPS and the SMF detects the policy control request trigger(s) is met, the SMF+PGW-C shall behave as defined in clause 4.2.4.2 with the differences that the SMF+PGW-C shall include (if available) in the SmPolicyUpdateContextData data structure:

- IP-CAN type within the "accessType" attribute;

- RAT type within the "ratType" attribute;

NOTE 1: See Annex B.3.4.5 for further information.

- subscribed APN-AMBR within the "subsSessAmbr" attribute;

- subscribed Default EPS bearer QoS Information within the "subsDefQos" attribute;

NOTE 2: Subscribed APN-AMBR and the QCI within the subscribed default EPS bearer QoS are mapped to subscribed Session-AMBR and 5QI as defined in Annex B.3.6.1 respectively.

- the bearer usage required for the dedicated bearer within the "qosFlowUsage" attribute if the UE initiates a resource modification request procedure and the bearer usage request was present in the Bearer Resource Command;

- user location information of EPC within the "userLocationInfo" attribute; and

NOTE 3: See Annex B.3.4.3 for further information.

- UE policy container within "uePolCont" attribute, if available.

The policy control request trigger "RES\_MO\_RE" is not supported when the PDN connection is established through the EPC/E-UTRAN network. The SMF+PGW shall reject the PDU session modification that initiated the UE's resource modification.

During interworking from 5GS to EPS, if the feature "PackFiltAllocPrecedence" is supported, for QoS Flows without EPS bearer ID(s) assigned or for QoS Flows related to PCC Rules that do not have allocated TFT packet filters, the SMF+PGW-C shall delete those PCC Rules and inform the PCF. The SMF+PGW-C shall include the "ruleReports" attribute containing the RuleReport data instance which specifies the affected PCC rules within the "pccRuleIds" attribute, set to "INACTIVE" the value within the "ruleStatus" attribute and the "PACKET\_FILTER\_TFT\_ALLOCATION\_EXCEEDED" as the value of the "failureCode" attribute.

If the feature "PackFiltAllocPrecedence" is supported, the PCF may provide, as part of the PccRule data type for the new PCC Rules to be installed the "packFiltAllPrec" attribute to indicate the order of the PCC Rules in the allocation of TFT packet filter(s) by the SMF+PGW-C. The PCF may include this parameter if the feature "PackFiltAllocPrecedence" is supported and there is a possibility to run into a restriction regarding the number of TFT packet filters that can be allocated for the PDU Session and interworking with EPS with N26 deployment is supported as described in Annex B.3.2.0.

\* \* \* Next Change \* \* \* \*

### B.3.4.Z Reporting of UE Policy container for URSP provisioning in EPS

When a new UE policy container is received the SMF+PGW-C requests to update the SM Policy Association and provides to the PCF information on the conditions that have been met.

Editor's Note: It will be aligned with SA2 (once it is specified in 3GPP TS 23.503) the name of the Policy Control Request trigger to indicate the provisioning of a UE Policy Container and whether it needs to be provisioned or the NF service consumer always reports it to the PCF.

The Policy Control Request Trigger condition "UE\_POL\_CONT\_IND" is met when the SMF+PGW-C receives a UE policy container from the UE. The SMF+PGW-C shall transparently forward to the PCF the UE policy container encoded within the "uePolCont" attribute. The PCF shall transparently forward the UE policy container to the PCF for the UE in Npcf\_UEPolicyControl\_Update Request.

\* \* \* Next Change \* \* \* \*

# A.2 Npcf\_SMPolicyControl API

openapi: 3.0.0

info:

 title: Npcf\_SMPolicyControl API

 version: 1.3.0-alpha.1

 description: |

 Session Management Policy Control Service

 © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: 3GPP TS 29.512 V18.0.0; 5G System; Session Management Policy Control Service.

 url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.512/'

security:

 - {}

 - oAuth2ClientCredentials:

 - npcf-smpolicycontrol

servers:

 - url: '{apiRoot}/npcf-smpolicycontrol/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in clause 4.4 of 3GPP TS 29.501

paths:

 /sm-policies:

 post:

 summary: Create a new Individual SM Policy

 operationId: CreateSMPolicy

 tags:

 - SM Policies (Collection)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/SmPolicyContextData'

 responses:

 '201':

 description: Created

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/SmPolicyDecision'

 headers:

 Location:

 description: Contains the URI of the newly created resource

 required: true

 schema:

 type: string

 '308':

 description: Permanent Redirect

 headers:

 Location:

 description: >

 Contains the URI of the PCF within the existing PCF binding information stored in

 the BSF for the same UE ID, S-NSSAI and DNN combination

 required: true

 schema:

 type: string

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '502':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/502'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 callbacks:

 SmPolicyUpdateNotification:

 '{$request.body#/notificationUri}/update':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/SmPolicyNotification'

 responses:

 '200':

 description: >

 OK. The current applicable values corresponding to the policy control request

 trigger is reported

 content:

 application/json:

 schema:

 oneOf:

 - $ref: '#/components/schemas/UeCampingRep'

 - type: array

 items:

 $ref: '#/components/schemas/PartialSuccessReport'

 minItems: 1

 - type: array

 items:

 $ref: '#/components/schemas/PolicyDecisionFailureCode'

 minItems: 1

 '204':

 description: No Content, Notification was succesfull

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 description: Bad Request.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ErrorReport'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '502':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/502'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 SmPolicyControlTerminationRequestNotification:

 '{$request.body#/notificationUri}/terminate':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TerminationNotification'

 responses:

 '204':

 description: No Content, Notification was successful

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '502':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/502'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /sm-policies/{smPolicyId}:

 get:

 summary: Read an Individual SM Policy

 operationId: GetSMPolicy

 tags:

 - Individual SM Policy (Document)

 parameters:

 - name: smPolicyId

 in: path

 description: Identifier of a policy association

 required: true

 schema:

 type: string

 responses:

 '200':

 description: OK. Resource representation is returned

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/SmPolicyControl'

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/406'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '502':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/502'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /sm-policies/{smPolicyId}/update:

 post:

 summary: Update an existing Individual SM Policy

 operationId: UpdateSMPolicy

 tags:

 - Individual SM Policy (Document)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/SmPolicyUpdateContextData'

 parameters:

 - name: smPolicyId

 in: path

 description: Identifier of a policy association

 required: true

 schema:

 type: string

 responses:

 '200':

 description: OK. Updated policies are returned

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/SmPolicyDecision'

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '502':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/502'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /sm-policies/{smPolicyId}/delete:

 post:

 summary: Delete an existing Individual SM Policy

 operationId: DeleteSMPolicy

 tags:

 - Individual SM Policy (Document)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/SmPolicyDeleteData'

 parameters:

 - name: smPolicyId

 in: path

 description: Identifier of a policy association

 required: true

 schema:

 type: string

 responses:

 '204':

 description: No content

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '502':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/502'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{nrfApiRoot}/oauth2/token'

 scopes:

 npcf-smpolicycontrol: Access to the Npcf\_SMPolicyControl API

 schemas:

 SmPolicyControl:

 description: >

 Contains the parameters used to request the SM policies and the SM policies authorized by

 the PCF.

 type: object

 properties:

 context:

 $ref: '#/components/schemas/SmPolicyContextData'

 policy:

 $ref: '#/components/schemas/SmPolicyDecision'

 required:

 - context

 - policy

 SmPolicyContextData:

 description: Contains the parameters used to create an Individual SM policy resource.

 type: object

 properties:

 accNetChId:

 $ref: '#/components/schemas/AccNetChId'

 chargEntityAddr:

 $ref: '#/components/schemas/AccNetChargingAddress'

 gpsi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 supi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 invalidSupi:

 type: boolean

 description: >

 When this attribute is included and set to true, it indicates that the supi attribute

 contains an invalid value.This attribute shall be present if the SUPI is not available

 in the SMF or the SUPI is unauthenticated. When present it shall be set to true for an

 invalid SUPI and false (default) for a valid SUPI.

 interGrpIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 minItems: 1

 pduSessionId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionId'

 pduSessionType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionType'

 chargingcharacteristics:

 type: string

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 dnnSelMode:

 $ref: 'TS29502\_Nsmf\_PDUSession.yaml#/components/schemas/DnnSelectionMode'

 notificationUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 accessType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/AccessType'

 ratType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 addAccessInfo:

 $ref: '#/components/schemas/AdditionalAccessInfo'

 servingNetwork:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnIdNid'

 userLocationInfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 ueTimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 pei:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

 ipv4Address:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 ipv6AddressPrefix:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

 ipDomain:

 type: string

 description: Indicates the IPv4 address domain

 subsSessAmbr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ambr'

 authProfIndex:

 type: string

 description: Indicates the DN-AAA authorization profile index

 subsDefQos:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SubscribedDefaultQos'

 vplmnQos:

 $ref: 'TS29502\_Nsmf\_PDUSession.yaml#/components/schemas/VplmnQos'

 numOfPackFilter:

 type: integer

 description: Contains the number of supported packet filter for signalled QoS rules.

 online:

 type: boolean

 description: >

 If it is included and set to true, the online charging is applied to the PDU session.

 offline:

 type: boolean

 description: >

 If it is included and set to true, the offline charging is applied to the PDU session.

 3gppPsDataOffStatus:

 type: boolean

 description: >

 If it is included and set to true, the 3GPP PS Data Off is activated by the UE.

 refQosIndication:

 type: boolean

 description: If it is included and set to true, the reflective QoS is supported by the UE.

 traceReq:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TraceData'

 sliceInfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 qosFlowUsage:

 $ref: '#/components/schemas/QosFlowUsage'

 servNfId:

 $ref: '#/components/schemas/ServingNfIdentity'

 suppFeat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 smfId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 recoveryTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 maPduInd:

 $ref: '#/components/schemas/MaPduIndication'

 atsssCapab:

 $ref: '#/components/schemas/AtsssCapability'

 ipv4FrameRouteList:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4AddrMask'

 minItems: 1

 ipv6FrameRouteList:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

 minItems: 1

 satBackhaulCategory:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SatelliteBackhaulCategory'

 pcfUeInfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PcfUeCallbackInfo'

 pvsInfo:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ServerAddressingInfo'

 minItems: 1

 onboardInd:

 type: boolean

 description: >

 If it is included and set to true, it indicates that the PDU session is used for

 UE Onboarding.

 nwdafDatas:

 type: array

 items:

 $ref: '#/components/schemas/NwdafData'

 minItems: 1

 uePolCont:

 $ref: '#/components/schemas/UePolicyContainer'

 required:

 - supi

 - pduSessionId

 - pduSessionType

 - dnn

 - notificationUri

 - sliceInfo

 SmPolicyDecision:

 description: Contains the SM policies authorized by the PCF.

 type: object

 properties:

 sessRules:

 type: object

 additionalProperties:

 $ref: '#/components/schemas/SessionRule'

 minProperties: 1

 description: >

 A map of Sessionrules with the content being the SessionRule as described in

 clause 5.6.2.7. The key used in this map for each entry is the sessRuleId

 attribute of the corresponding SessionRule.

 pccRules:

 type: object

 additionalProperties:

 $ref: '#/components/schemas/PccRule'

 minProperties: 1

 description: >

 A map of PCC rules with the content being the PCCRule as described in

 clause 5.6.2.6. The key used in this map for each entry is the pccRuleId

 attribute of the corresponding PccRule.

 nullable: true

 pcscfRestIndication:

 type: boolean

 description: >

 If it is included and set to true, it indicates the P-CSCF Restoration is requested.

 qosDecs:

 type: object

 additionalProperties:

 $ref: '#/components/schemas/QosData'

 minProperties: 1

 description: >

 Map of QoS data policy decisions. The key used in this map for each entry is the qosId

 attribute of the corresponding QosData.

 chgDecs:

 type: object

 additionalProperties:

 $ref: '#/components/schemas/ChargingData'

 minProperties: 1

 description: >

 Map of Charging data policy decisions. The key used in this map for each entry

 is the chgId attribute of the corresponding ChargingData.

 nullable: true

 chargingInfo:

 $ref: '#/components/schemas/ChargingInformation'

 traffContDecs:

 type: object

 additionalProperties:

 $ref: '#/components/schemas/TrafficControlData'

 minProperties: 1

 description: >

 Map of Traffic Control data policy decisions. The key used in this map for each entry

 is the tcId attribute of the corresponding TrafficControlData.

 umDecs:

 type: object

 additionalProperties:

 $ref: '#/components/schemas/UsageMonitoringData'

 minProperties: 1

 description: >

 Map of Usage Monitoring data policy decisions. The key used in this map for each entry

 is the umId attribute of the corresponding UsageMonitoringData.

 nullable: true

 qosChars:

 type: object

 additionalProperties:

 $ref: '#/components/schemas/QosCharacteristics'

 minProperties: 1

 description: >

 Map of QoS characteristics for non standard 5QIs. This map uses the 5QI values as keys.

 qosMonDecs:

 type: object

 additionalProperties:

 $ref: '#/components/schemas/QosMonitoringData'

 minProperties: 1

 description: >

 Map of QoS Monitoring data policy decisions. The key used in this map for each entry

 is the qmId attribute of the corresponding QosMonitoringData.

 nullable: true

 reflectiveQoSTimer:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 conds:

 type: object

 additionalProperties:

 $ref: '#/components/schemas/ConditionData'

 minProperties: 1

 description: >

 A map of condition data with the content being as described in clause 5.6.2.9. The key

 used in this map for each entry is the condId attribute of the corresponding ConditionData.

 nullable: true

 revalidationTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 offline:

 type: boolean

 description: >

 Indicates the offline charging is applicable to the PDU session when it is included and

 set to true.

 online:

 type: boolean

 description: >

 Indicates the online charging is applicable to the PDU session when it is included and

 set to true.

 offlineChOnly:

 type: boolean

 default: false

 description: >

 Indicates that the online charging method shall never be used for any PCC rule activated

 during the lifetime of the PDU session.

 policyCtrlReqTriggers:

 type: array

 items:

 $ref: '#/components/schemas/PolicyControlRequestTrigger'

 minItems: 1

 description: Defines the policy control request triggers subscribed by the PCF.

 nullable: true

 lastReqRuleData:

 type: array

 items:

 $ref: '#/components/schemas/RequestedRuleData'

 minItems: 1

 description: Defines the last list of rule control data requested by the PCF.

 lastReqUsageData:

 $ref: '#/components/schemas/RequestedUsageData'

 praInfos:

 type: object

 additionalProperties:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfoRm'

 minProperties: 1

 description: >

 Map of PRA information. The praId attribute within the PresenceInfo data type is the key

 of the map.

 nullable: true

 ipv4Index:

 $ref: 'TS29519\_Policy\_Data.yaml#/components/schemas/IpIndex'

 ipv6Index:

 $ref: 'TS29519\_Policy\_Data.yaml#/components/schemas/IpIndex'

 qosFlowUsage:

 $ref: '#/components/schemas/QosFlowUsage'

 relCause:

 $ref: '#/components/schemas/SmPolicyAssociationReleaseCause'

 suppFeat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 tsnBridgeManCont:

 $ref: '#/components/schemas/BridgeManagementContainer'

 tsnPortManContDstt:

 $ref: '#/components/schemas/PortManagementContainer'

 tsnPortManContNwtts:

 type: array

 items:

 $ref: '#/components/schemas/PortManagementContainer'

 minItems: 1

 redSessIndication:

 type: boolean

 description: >

 Indicates whether the PDU session is a redundant PDU session. If absent it means the PDU

 session is not a redundant PDU session.

 uePolCont:

 $ref: '#/components/schemas/UePolicyContainer'

 SmPolicyNotification:

 description: Represents a notification on the update of the SM policies.

 type: object

 properties:

 resourceUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 smPolicyDecision:

 $ref: '#/components/schemas/SmPolicyDecision'

 PccRule:

 description: Contains a PCC rule information.

 type: object

 properties:

 flowInfos:

 type: array

 items:

 $ref: '#/components/schemas/FlowInformation'

 minItems: 1

 description: An array of IP flow packet filter information.

 appId:

 type: string

 description: A reference to the application detection filter configured at the UPF.

 appDescriptor:

 $ref: '#/components/schemas/ApplicationDescriptor'

 contVer:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/ContentVersion'

 pccRuleId:

 type: string

 description: Univocally identifies the PCC rule within a PDU session.

 precedence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 afSigProtocol:

 $ref: '#/components/schemas/AfSigProtocol'

 appReloc:

 type: boolean

 description: Indication of application relocation possibility.

 easRedisInd:

 type: boolean

 description: Indicates the EAS rediscovery is required.

 refQosData:

 type: array

 items:

 type: string

 minItems: 1

 maxItems: 1

 description: >

 A reference to the QosData policy decision type. It is the qosId described in

 clause 5.6.2.8.

 refAltQosParams:

 type: array

 items:

 type: string

 minItems: 1

 description: >

 A Reference to the QosData policy decision type for the Alternative QoS parameter sets

 of the service data flow.

 refTcData:

 type: array

 items:

 type: string

 minItems: 1

 maxItems: 1

 description: >

 A reference to the TrafficControlData policy decision type. It is the tcId described in

 clause 5.6.2.10.

 refChgData:

 type: array

 items:

 type: string

 minItems: 1

 maxItems: 1

 description: >

 A reference to the ChargingData policy decision type. It is the chgId described in

 clause 5.6.2.11.

 nullable: true

 refChgN3gData:

 type: array

 items:

 type: string

 minItems: 1

 maxItems: 1

 description: >

 A reference to the ChargingData policy decision type only applicable to Non-3GPP access

 if "ATSSS" feature is supported. It is the chgId described in clause 5.6.2.11.

 nullable: true

 refUmData:

 type: array

 items:

 type: string

 minItems: 1

 maxItems: 1

 description: >

 A reference to UsageMonitoringData policy decision type. It is the umId described in

 clause 5.6.2.12.

 nullable: true

 refUmN3gData:

 type: array

 items:

 type: string

 minItems: 1

 maxItems: 1

 description: >

 A reference to UsageMonitoringData policy decision type only applicable to Non-3GPP

 access if "ATSSS" feature is supported. It is the umId described in clause 5.6.2.12.

 nullable: true

 refCondData:

 type: string

 description: >

 A reference to the condition data. It is the condId described in clause 5.6.2.9.

 nullable: true

 refQosMon:

 type: array

 items:

 type: string

 minItems: 1

 maxItems: 1

 description: >

 A reference to the QosMonitoringData policy decision type. It is the qmId described in

 clause 5.6.2.40.

 nullable: true

 addrPreserInd:

 type: boolean

 nullable: true

 tscaiInputDl:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TscaiInputContainer'

 tscaiInputUl:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TscaiInputContainer'

 tscaiTimeDom:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 ddNotifCtrl:

 $ref: '#/components/schemas/DownlinkDataNotificationControl'

 ddNotifCtrl2:

 $ref: '#/components/schemas/DownlinkDataNotificationControlRm'

 disUeNotif:

 type: boolean

 nullable: true

 packFiltAllPrec:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 required:

 - pccRuleId

 nullable: true

 SessionRule:

 description: Contains session level policy information.

 type: object

 properties:

 authSessAmbr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ambr'

 authDefQos:

 $ref: '#/components/schemas/AuthorizedDefaultQos'

 sessRuleId:

 type: string

 description: Univocally identifies the session rule within a PDU session.

 refUmData:

 type: string

 description: >

 A reference to UsageMonitoringData policy decision type. It is the umId described in

 clause 5.6.2.12.

 nullable: true

 refUmN3gData:

 type: string

 description: >

 A reference to UsageMonitoringData policy decision type to apply for Non-3GPP access. It

 is the umId described in clause 5.6.2.12.

 nullable: true

 refCondData:

 type: string

 description: >

 A reference to the condition data. It is the condId described in clause 5.6.2.9.

 nullable: true

 required:

 - sessRuleId

 nullable: true

 QosData:

 description: Contains the QoS parameters.

 type: object

 properties:

 qosId:

 type: string

 description: Univocally identifies the QoS control policy data within a PDU session.

 5qi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/5Qi'

 maxbrUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

 maxbrDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

 gbrUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

 gbrDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

 arp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Arp'

 qnc:

 type: boolean

 description: >

 Indicates whether notifications are requested from 3GPP NG-RAN when the GFBR can no longer

 (or again) be guaranteed for a QoS Flow during the lifetime of the QoS Flow.

 priorityLevel:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/5QiPriorityLevelRm'

 averWindow:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/AverWindowRm'

 maxDataBurstVol:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/MaxDataBurstVolRm'

 reflectiveQos:

 type: boolean

 description: >

 Indicates whether the QoS information is reflective for the corresponding service data

 flow.

 sharingKeyDl:

 type: string

 description: >

 Indicates, by containing the same value, what PCC rules may share resource in downlink

 direction.

 sharingKeyUl:

 type: string

 description: >

 Indicates, by containing the same value, what PCC rules may share resource in uplink

 direction.

 maxPacketLossRateDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketLossRateRm'

 maxPacketLossRateUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketLossRateRm'

 defQosFlowIndication:

 type: boolean

 description: >

 Indicates that the dynamic PCC rule shall always have its binding with the QoS Flow

 associated with the default QoS rule

 extMaxDataBurstVol:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ExtMaxDataBurstVolRm'

 packetDelayBudget:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketDelBudget'

 packetErrorRate:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketErrRate'

 required:

 - qosId

 nullable: true

 ConditionData:

 description: Contains conditions of applicability for a rule.

 type: object

 properties:

 condId:

 type: string

 description: Uniquely identifies the condition data within a PDU session.

 activationTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTimeRm'

 deactivationTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTimeRm'

 accessType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/AccessType'

 ratType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 required:

 - condId

 nullable: true

 TrafficControlData:

 description: >

 Contains parameters determining how flows associated with a PCC Rule are treated (e.g.

 blocked, redirected, etc).

 type: object

 properties:

 tcId:

 type: string

 description: Univocally identifies the traffic control policy data within a PDU session.

 flowStatus:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/FlowStatus'

 redirectInfo:

 $ref: '#/components/schemas/RedirectInformation'

 addRedirectInfo:

 type: array

 items:

 $ref: '#/components/schemas/RedirectInformation'

 minItems: 1

 muteNotif:

 type: boolean

 description: Indicates whether applicat'on's start or stop notification is to be muted.

 trafficSteeringPolIdDl:

 type: string

 description: >

 Reference to a pre-configured traffic steering policy for downlink traffic at the SMF.

 nullable: true

 trafficSteeringPolIdUl:

 type: string

 description: >

 Reference to a pre-configured traffic steering policy for uplink traffic at the SMF.

 nullable: true

 routeToLocs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RouteToLocation'

 minItems: 1

 description: A list of location which the traffic shall be routed to for the AF request

 nullable: true

 maxAllowedUpLat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UintegerRm'

 easIpReplaceInfos:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/EasIpReplacementInfo'

 minItems: 1

 description: Contains EAS IP replacement information.

 nullable: true

 traffCorreInd:

 type: boolean

 simConnInd:

 type: boolean

 description: >

 Indicates whether simultaneous connectivity should be temporarily maintained for the

 source and target PSA.

 simConnTerm:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 upPathChgEvent:

 $ref: '#/components/schemas/UpPathChgEvent'

 steerFun:

 $ref: '#/components/schemas/SteeringFunctionality'

 steerModeDl:

 $ref: '#/components/schemas/SteeringMode'

 steerModeUl:

 $ref: '#/components/schemas/SteeringMode'

 mulAccCtrl:

 $ref: '#/components/schemas/MulticastAccessControl'

 required:

 - tcId

 nullable: true

 ChargingData:

 description: Contains charging related parameters.

 type: object

 properties:

 chgId:

 type: string

 description: Univocally identifies the charging control policy data within a PDU session.

 meteringMethod:

 $ref: '#/components/schemas/MeteringMethod'

 offline:

 type: boolean

 description: >

 Indicates the offline charging is applicable to the PCC rule when it is included and set

 to true.

 online:

 type: boolean

 description: >

 Indicates the online charging is applicable to the PCC rule when it is included and set

 to true.

 sdfHandl:

 type: boolean

 description: >

 Indicates whether the service data flow is allowed to start while the SMF is waiting for

 the response to the credit request.

 ratingGroup:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatingGroup'

 reportingLevel:

 $ref: '#/components/schemas/ReportingLevel'

 serviceId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ServiceId'

 sponsorId:

 type: string

 description: Indicates the sponsor identity.

 appSvcProvId:

 type: string

 description: Indicates the application service provider identity.

 afChargingIdentifier:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

 afChargId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationChargingId'

 required:

 - chgId

 nullable: true

 UsageMonitoringData:

 description: Contains usage monitoring related control information.

 type: object

 properties:

 umId:

 type: string

 description: Univocally identifies the usage monitoring policy data within a PDU session.

 volumeThreshold:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/VolumeRm'

 volumeThresholdUplink:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/VolumeRm'

 volumeThresholdDownlink:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/VolumeRm'

 timeThreshold:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSecRm'

 monitoringTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTimeRm'

 nextVolThreshold:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/VolumeRm'

 nextVolThresholdUplink:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/VolumeRm'

 nextVolThresholdDownlink:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/VolumeRm'

 nextTimeThreshold:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSecRm'

 inactivityTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSecRm'

 exUsagePccRuleIds:

 type: array

 items:

 type: string

 minItems: 1

 description: >

 Contains the PCC rule identifier(s) which corresponding service data flow(s) shall be

 excluded from PDU Session usage monitoring. It is only included in the

 UsageMonitoringData instance for session level usage monitoring.

 nullable: true

 required:

 - umId

 nullable: true

 RedirectInformation:

 description: Contains the redirect information.

 type: object

 properties:

 redirectEnabled:

 type: boolean

 description: Indicates the redirect is enable.

 redirectAddressType:

 $ref: '#/components/schemas/RedirectAddressType'

 redirectServerAddress:

 type: string

 description: >

 Indicates the address of the redirect server. If "redirectAddressType" attribute

 indicates the IPV4\_ADDR, the encoding is the same as the Ipv4Addr data type defined in

 3GPP TS 29.571.If "redirectAddressType" attribute indicates the IPV6\_ADDR, the encoding

 is the same as the Ipv6Addr data type defined in 3GPP TS 29.571.If "redirectAddressType"

 attribute indicates the URL or SIP\_URI, the encoding is the same as the Uri data type

 defined in 3GPP TS 29.571.

 FlowInformation:

 description: Contains the flow information.

 type: object

 properties:

 flowDescription:

 $ref: '#/components/schemas/FlowDescription'

 ethFlowDescription:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EthFlowDescription'

 packFiltId:

 type: string

 description: An identifier of packet filter.

 packetFilterUsage:

 type: boolean

 description: The packet shall be sent to the UE.

 tosTrafficClass:

 type: string

 description: >

 Contains the Ipv4 Type-of-Service and mask field or the Ipv6 Traffic-Class field and

 mask field.

 nullable: true

 spi:

 type: string

 description: the security parameter index of the IPSec packet.

 nullable: true

 flowLabel:

 type: string

 description: the Ipv6 flow label header field.

 nullable: true

 flowDirection:

 $ref: '#/components/schemas/FlowDirectionRm'

 SmPolicyDeleteData:

 description: >

 Contains the parameters to be sent to the PCF when an individual SM policy is deleted.

 type: object

 properties:

 userLocationInfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 ueTimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 servingNetwork:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnIdNid'

 userLocationInfoTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 ranNasRelCauses:

 type: array

 items:

 $ref: '#/components/schemas/RanNasRelCause'

 minItems: 1

 description: Contains the RAN and/or NAS release cause.

 accuUsageReports:

 type: array

 items:

 $ref: '#/components/schemas/AccuUsageReport'

 minItems: 1

 description: Contains the usage report

 pduSessRelCause:

 $ref: '#/components/schemas/PduSessionRelCause'

 qosMonReports:

 type: array

 items:

 $ref: '#/components/schemas/QosMonitoringReport'

 minItems: 1

 QosCharacteristics:

 description: Contains QoS characteristics for a non-standardized or a non-configured 5QI.

 type: object

 properties:

 5qi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/5Qi'

 resourceType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/QosResourceType'

 priorityLevel:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/5QiPriorityLevel'

 packetDelayBudget:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketDelBudget'

 packetErrorRate:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketErrRate'

 averagingWindow:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/AverWindow'

 maxDataBurstVol:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/MaxDataBurstVol'

 extMaxDataBurstVol:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ExtMaxDataBurstVol'

 required:

 - 5qi

 - resourceType

 - priorityLevel

 - packetDelayBudget

 - packetErrorRate

 ChargingInformation:

 description: Contains the addresses of the charging functions.

 type: object

 properties:

 primaryChfAddress:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 secondaryChfAddress:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 primaryChfSetId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfSetId'

 primaryChfInstanceId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 secondaryChfSetId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfSetId'

 secondaryChfInstanceId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 required:

 - primaryChfAddress

 AccuUsageReport:

 description: Contains the accumulated usage report information.

 type: object

 properties:

 refUmIds:

 type: string

 description: An id referencing UsageMonitoringData objects associated with this usage report.

 volUsage:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

 volUsageUplink:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

 volUsageDownlink:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

 timeUsage:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 nextVolUsage:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

 nextVolUsageUplink:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

 nextVolUsageDownlink:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

 nextTimeUsage:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 required:

 - refUmIds

 SmPolicyUpdateContextData:

 description: >

 Contains the policy control request trigger(s) that were met and the corresponding new

 value(s) or the error report of the policy enforcement.

 type: object

 properties:

 repPolicyCtrlReqTriggers:

 type: array

 items:

 $ref: '#/components/schemas/PolicyControlRequestTrigger'

 minItems: 1

 description: The policy control reqeust trigges which are met.

 accNetChIds:

 type: array

 items:

 $ref: '#/components/schemas/AccNetChId'

 minItems: 1

 description: >

 Indicates the access network charging identifier for the PCC rule(s) or whole PDU

 session.

 accessType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/AccessType'

 ratType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 addAccessInfo:

 $ref: '#/components/schemas/AdditionalAccessInfo'

 relAccessInfo:

 $ref: '#/components/schemas/AdditionalAccessInfo'

 servingNetwork:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnIdNid'

 userLocationInfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 ueTimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 relIpv4Address:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 ipv4Address:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 ipDomain:

 type: string

 description: Indicates the IPv4 address domain

 ipv6AddressPrefix:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

 relIpv6AddressPrefix:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

 addIpv6AddrPrefixes:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

 addRelIpv6AddrPrefixes:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

 relUeMac:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

 ueMac:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

 subsSessAmbr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ambr'

 authProfIndex:

 type: string

 description: Indicates the DN-AAA authorization profile index

 subsDefQos:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SubscribedDefaultQos'

 vplmnQos:

 $ref: 'TS29502\_Nsmf\_PDUSession.yaml#/components/schemas/VplmnQos'

 vplmnQosNotApp:

 type: boolean

 description: >

 If it is included and set to true, indicates that the QoS constraints in the VPLMN are

 not applicable.

 numOfPackFilter:

 type: integer

 description: Contains the number of supported packet filter for signalled QoS rules.

 accuUsageReports:

 type: array

 items:

 $ref: '#/components/schemas/AccuUsageReport'

 minItems: 1

 description: Contains the usage report

 3gppPsDataOffStatus:

 type: boolean

 description: If it is included and set to true, the 3GPP PS Data Off is activated by the UE.

 appDetectionInfos:

 type: array

 items:

 $ref: '#/components/schemas/AppDetectionInfo'

 minItems: 1

 description: >

 Report the start/stop of the application traffic and detected SDF descriptions

 if applicable.

 ruleReports:

 type: array

 items:

 $ref: '#/components/schemas/RuleReport'

 minItems: 1

 description: Used to report the PCC rule failure.

 sessRuleReports:

 type: array

 items:

 $ref: '#/components/schemas/SessionRuleReport'

 minItems: 1

 description: Used to report the session rule failure.

 qncReports:

 type: array

 items:

 $ref: '#/components/schemas/QosNotificationControlInfo'

 minItems: 1

 description: QoS Notification Control information.

 qosMonReports:

 type: array

 items:

 $ref: '#/components/schemas/QosMonitoringReport'

 minItems: 1

 userLocationInfoTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 repPraInfos:

 type: object

 additionalProperties:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

 minProperties: 1

 description: >

 Reports the changes of presence reporting area. The praId attribute within the

 PresenceInfo data type is the key of the map.

 ueInitResReq:

 $ref: '#/components/schemas/UeInitiatedResourceRequest'

 refQosIndication:

 type: boolean

 description: >

 If it is included and set to true, the reflective QoS is supported by the UE. If it is

 included and set to false, the reflective QoS is revoked by the UE.

 qosFlowUsage:

 $ref: '#/components/schemas/QosFlowUsage'

 creditManageStatus:

 $ref: '#/components/schemas/CreditManagementStatus'

 servNfId:

 $ref: '#/components/schemas/ServingNfIdentity'

 traceReq:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TraceData'

 maPduInd:

 $ref: '#/components/schemas/MaPduIndication'

 atsssCapab:

 $ref: '#/components/schemas/AtsssCapability'

 tsnBridgeInfo:

 $ref: '#/components/schemas/TsnBridgeInfo'

 tsnBridgeManCont:

 $ref: '#/components/schemas/BridgeManagementContainer'

 tsnPortManContDstt:

 $ref: '#/components/schemas/PortManagementContainer'

 tsnPortManContNwtts:

 type: array

 items:

 $ref: '#/components/schemas/PortManagementContainer'

 minItems: 1

 mulAddrInfos:

 type: array

 items:

 $ref: '#/components/schemas/IpMulticastAddressInfo'

 minItems: 1

 policyDecFailureReports:

 type: array

 items:

 $ref: '#/components/schemas/PolicyDecisionFailureCode'

 minItems: 1

 description: Contains the type(s) of failed policy decision and/or condition data.

 invalidPolicyDecs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/InvalidParam'

 minItems: 1

 description: >

 Indicates the invalid parameters for the reported type(s) of the failed policy decision

 and/or condition data.

 trafficDescriptors:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DddTrafficDescriptor'

 minItems: 1

 pccRuleId:

 type: string

 description: >

 Contains the identifier of the PCC rule which is used for traffic detection of event.

 typesOfNotif:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DlDataDeliveryStatus'

 minItems: 1

 interGrpIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 minItems: 1

 satBackhaulCategory:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SatelliteBackhaulCategory'

 pcfUeInfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PcfUeCallbackInfo'

 nwdafDatas:

 type: array

 items:

 $ref: '#/components/schemas/NwdafData'

 minItems: 1

 nullable: true

 anGwStatus:

 type: boolean

 description: >

 When it is included and set to true, it indicates that the AN-Gateway has failed and

 that the PCF should refrain from sending policy decisions to the SMF until it is

 informed that the AN-Gateway has been recovered.

 uePolCont:

 $ref: '#/components/schemas/UePolicyContainer'

 UpPathChgEvent:

 description: Contains the UP path change event subscription from the AF.

 type: object

 properties:

 notificationUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 notifCorreId:

 type: string

 description: >

 It is used to set the value of Notification Correlation ID in the notification sent by

 the SMF.

 dnaiChgType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DnaiChangeType'

 afAckInd:

 type: boolean

 required:

 - notificationUri

 - notifCorreId

 - dnaiChgType

 nullable: true

 TerminationNotification:

 description: Represents a Termination Notification.

 type: object

 properties:

 resourceUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 cause:

 $ref: '#/components/schemas/SmPolicyAssociationReleaseCause'

 required:

 - resourceUri

 - cause

 AppDetectionInfo:

 description: Contains the detected application's traffic information.

 type: object

 properties:

 appId:

 type: string

 description: A reference to the application detection filter configured at the UPF

 instanceId:

 type: string

 description: >

 Identifier sent by the SMF in order to allow correlation of application Start and Stop

 events to the specific service data flow description, if service data flow descriptions

 are deducible.

 sdfDescriptions:

 type: array

 items:

 $ref: '#/components/schemas/FlowInformation'

 minItems: 1

 description: Contains the detected service data flow descriptions if they are deducible.

 required:

 - appId

 AccNetChId:

 description: >

 Contains the access network charging identifier for the PCC rule(s) or for the whole

 PDU session.

 type: object

 properties:

 accNetChaIdValue:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

 accNetChargId:

 type: string

 description: A character string containing the access network charging id.

 refPccRuleIds:

 type: array

 items:

 type: string

 minItems: 1

 description: >

 Contains the identifier of the PCC rule(s) associated to the provided Access Network

 Charging Identifier.

 sessionChScope:

 type: boolean

 description: >

 When it is included and set to true, indicates the Access Network Charging Identifier

 applies to the whole PDU Session

 oneOf:

 - required: [accNetChaIdValue]

 - required: [accNetChargId]

 AccNetChargingAddress:

 description: Describes the network entity within the access network performing charging

 type: object

 anyOf:

 - required: [anChargIpv4Addr]

 - required: [anChargIpv6Addr]

 properties:

 anChargIpv4Addr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 anChargIpv6Addr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 RequestedRuleData:

 description: >

 Contains rule data requested by the PCF to receive information associated with PCC rule(s).

 type: object

 properties:

 refPccRuleIds:

 type: array

 items:

 type: string

 minItems: 1

 description: >

 An array of PCC rule id references to the PCC rules associated with the control data.

 reqData:

 type: array

 items:

 $ref: '#/components/schemas/RequestedRuleDataType'

 minItems: 1

 description: >

 Array of requested rule data type elements indicating what type of rule data is

 requested for the corresponding referenced PCC rules.

 required:

 - refPccRuleIds

 - reqData

 RequestedUsageData:

 description: >

 Contains usage data requested by the PCF requesting usage reports for the corresponding

 usage monitoring data instances.

 type: object

 properties:

 refUmIds:

 type: array

 items:

 type: string

 minItems: 1

 description: >

 An array of usage monitoring data id references to the usage monitoring data instances

 for which the PCF is requesting a usage report. This attribute shall only be provided

 when allUmIds is not set to true.

 allUmIds:

 type: boolean

 description: >

 This boolean indicates whether requested usage data applies to all usage monitoring data

 instances. When it's not included, it means requested usage data shall only apply to the

 usage monitoring data instances referenced by the refUmIds attribute.

 UeCampingRep:

 description: >

 Contains the current applicable values corresponding to the policy control request triggers.

 type: object

 properties:

 accessType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/AccessType'

 ratType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 servNfId:

 $ref: '#/components/schemas/ServingNfIdentity'

 servingNetwork:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnIdNid'

 userLocationInfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 ueTimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 netLocAccSupp:

 $ref: '#/components/schemas/NetLocAccessSupport'

 satBackhaulCategory:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SatelliteBackhaulCategory'

 RuleReport:

 description: Reports the status of PCC.

 type: object

 properties:

 pccRuleIds:

 type: array

 items:

 type: string

 minItems: 1

 description: Contains the identifier of the affected PCC rule(s).

 ruleStatus:

 $ref: '#/components/schemas/RuleStatus'

 contVers:

 type: array

 items:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/ContentVersion'

 minItems: 1

 description: Indicates the version of a PCC rule.

 failureCode:

 $ref: '#/components/schemas/FailureCode'

 retryAfter:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 finUnitAct:

 $ref: 'TS32291\_Nchf\_ConvergedCharging.yaml#/components/schemas/FinalUnitAction'

 ranNasRelCauses:

 type: array

 items:

 $ref: '#/components/schemas/RanNasRelCause'

 minItems: 1

 description: indicates the RAN or NAS release cause code information.

 altQosParamId:

 type: string

 description: >

 Indicates the alternative QoS parameter set that the NG-RAN can guarantee. It is

 included during the report of successfull resource allocation and indicates that NG-RAN

 used an alternative QoS profile because the requested QoS could not be allocated..

 altQosNotSuppInd:

 type: boolean

 description: >

 When present and set to true it indicates that the Alternative QoS profiles are not

 supported by NG-RAN.

 required:

 - pccRuleIds

 - ruleStatus

 RanNasRelCause:

 description: Contains the RAN/NAS release cause.

 type: object

 properties:

 ngApCause:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NgApCause'

 5gMmCause:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/5GMmCause'

 5gSmCause:

 $ref: '#/components/schemas/5GSmCause'

 epsCause:

 $ref: '#/components/schemas/EpsRanNasRelCause'

 UeInitiatedResourceRequest:

 description: Indicates that a UE requests specific QoS handling for the selected SDF.

 type: object

 properties:

 pccRuleId:

 type: string

 ruleOp:

 $ref: '#/components/schemas/RuleOperation'

 precedence:

 type: integer

 packFiltInfo:

 type: array

 items:

 $ref: '#/components/schemas/PacketFilterInfo'

 minItems: 1

 reqQos:

 $ref: '#/components/schemas/RequestedQos'

 required:

 - ruleOp

 - packFiltInfo

 PacketFilterInfo:

 description: Contains the information from a single packet filter sent from the SMF to the PCF.

 type: object

 properties:

 packFiltId:

 type: string

 description: An identifier of packet filter.

 packFiltCont:

 $ref: '#/components/schemas/PacketFilterContent'

 tosTrafficClass:

 type: string

 description: >

 Contains the Ipv4 Type-of-Service and mask field or the Ipv6 Traffic-Class field and

 mask field.

 spi:

 type: string

 description: The security parameter index of the IPSec packet.

 flowLabel:

 type: string

 description: The Ipv6 flow label header field.

 flowDirection:

 $ref: '#/components/schemas/FlowDirection'

 RequestedQos:

 description: Contains the QoS information requested by the UE.

 type: object

 properties:

 5qi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/5Qi'

 gbrUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 gbrDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 required:

 - 5qi

 QosNotificationControlInfo:

 description: Contains the QoS Notification Control Information.

 type: object

 properties:

 refPccRuleIds:

 type: array

 items:

 type: string

 minItems: 1

 description: >

 An array of PCC rule id references to the PCC rules associated with the QoS notification

 control info.

 notifType:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/QosNotifType'

 contVer:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/ContentVersion'

 altQosParamId:

 type: string

 description: >

 Indicates the alternative QoS parameter set the NG-RAN can guarantee. When it is omitted

 and the notifType attribute is set to NOT\_GUAARANTEED it indicates that the lowest

 priority alternative QoS profile could not be fulfilled.

 altQosNotSuppInd:

 type: boolean

 description: >

 When present and set to true it indicates that the Alternative QoS profiles are not

 supported by NG-RAN.

 required:

 - refPccRuleIds

 - notifType

 PartialSuccessReport:

 description: >

 Includes the information reported by the SMF when some of the PCC rules and/or session rules

 and/or policy decision and/or condition data are not successfully installed/activated or

 stored.

 type: object

 properties:

 failureCause:

 $ref: '#/components/schemas/FailureCause'

 ruleReports:

 type: array

 items:

 $ref: '#/components/schemas/RuleReport'

 minItems: 1

 description: Information about the PCC rules provisioned by the PCF not successfully installed/activated.

 sessRuleReports:

 type: array

 items:

 $ref: '#/components/schemas/SessionRuleReport'

 minItems: 1

 description: >

 Information about the session rules provisioned by the PCF not successfully installed.

 ueCampingRep:

 $ref: '#/components/schemas/UeCampingRep'

 policyDecFailureReports:

 type: array

 items:

 $ref: '#/components/schemas/PolicyDecisionFailureCode'

 minItems: 1

 description: Contains the type(s) of failed policy decision and/or condition data.

 invalidPolicyDecs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/InvalidParam'

 minItems: 1

 description: >

 Indicates the invalid parameters for the reported type(s) of the failed policy decision

 and/or condition data.

 required:

 - failureCause

 AuthorizedDefaultQos:

 description: Represents the Authorized Default QoS.

 type: object

 properties:

 5qi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/5Qi'

 arp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Arp'

 priorityLevel:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/5QiPriorityLevelRm'

 averWindow:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/AverWindowRm'

 maxDataBurstVol:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/MaxDataBurstVolRm'

 maxbrUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

 maxbrDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

 gbrUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

 gbrDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

 extMaxDataBurstVol:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ExtMaxDataBurstVolRm'

 ErrorReport:

 description: Contains the rule,policy decision and/or condition data error reports.

 type: object

 properties:

 error:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 ruleReports:

 type: array

 items:

 $ref: '#/components/schemas/RuleReport'

 minItems: 1

 description: Used to report the PCC rule failure.

 sessRuleReports:

 type: array

 items:

 $ref: '#/components/schemas/SessionRuleReport'

 minItems: 1

 description: Used to report the session rule failure.

 polDecFailureReports:

 type: array

 items:

 $ref: '#/components/schemas/PolicyDecisionFailureCode'

 minItems: 1

 description: Used to report failure of the policy decision and/or condition data.

 invalidPolicyDecs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/InvalidParam'

 minItems: 1

 description: >

 Indicates the invalid parameters for the reported type(s) of the failed policy decision

 and/or condition data.

 SessionRuleReport:

 description: Represents reporting of the status of a session rule.

 type: object

 properties:

 ruleIds:

 type: array

 items:

 type: string

 minItems: 1

 description: Contains the identifier of the affected session rule(s).

 ruleStatus:

 $ref: '#/components/schemas/RuleStatus'

 sessRuleFailureCode:

 $ref: '#/components/schemas/SessionRuleFailureCode'

 policyDecFailureReports:

 type: array

 items:

 $ref: '#/components/schemas/PolicyDecisionFailureCode'

 minItems: 1

 description: Contains the type(s) of failed policy decision and/or condition data.

 required:

 - ruleIds

 - ruleStatus

 ServingNfIdentity:

 description: Contains the serving Network Function identity.

 type: object

 properties:

 servNfInstId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 guami:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Guami'

 anGwAddr:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/AnGwAddress'

 sgsnAddr:

 $ref: '#/components/schemas/SgsnAddress'

 SteeringMode:

 description: Contains the steering mode value and parameters determined by the PCF.

 type: object

 properties:

 steerModeValue:

 $ref: '#/components/schemas/SteerModeValue'

 active:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/AccessType'

 standby:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/AccessTypeRm'

 3gLoad:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 prioAcc:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/AccessType'

 thresValue:

 $ref: '#/components/schemas/ThresholdValue'

 steerModeInd:

 $ref: '#/components/schemas/SteerModeIndicator'

 required:

 - steerModeValue

 AdditionalAccessInfo:

 description: >

 Indicates the combination of additional Access Type and RAT Type for a MA PDU session.

 type: object

 properties:

 accessType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/AccessType'

 ratType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 required:

 - accessType

 QosMonitoringData:

 description: Contains QoS monitoring related control information.

 type: object

 properties:

 qmId:

 type: string

 description: Univocally identifies the QoS monitoring policy data within a PDU session.

 reqQosMonParams:

 type: array

 items:

 $ref: '#/components/schemas/RequestedQosMonitoringParameter'

 minItems: 1

 description: >

 indicates the UL packet delay, DL packet delay and/or round trip packet delay between

 the UE and the UPF is to be monitored when the QoS Monitoring for URLLC is enabled for

 the service data flow.

 repFreqs:

 type: array

 items:

 $ref: '#/components/schemas/ReportingFrequency'

 minItems: 1

 repThreshDl:

 type: integer

 description: Indicates the period of time in units of miliiseconds for DL packet delay.

 nullable: true

 repThreshUl:

 type: integer

 description: Indicates the period of time in units of miliiseconds for UL packet delay.

 nullable: true

 repThreshRp:

 type: integer

 description: >

 Indicates the period of time in units of miliiseconds for round trip packet delay.

 nullable: true

 waitTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSecRm'

 repPeriod:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSecRm'

 notifyUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UriRm'

 notifyCorreId:

 type: string

 nullable: true

 directNotifInd:

 type: boolean

 description: >

 Indicates that the direct event notification sent by UPF to the Local NEF or AF is

 requested if it is included and set to true.

 required:

 - qmId

 - reqQosMonParams

 - repFreqs

 nullable: true

 QosMonitoringReport:

 description: Contains reporting information on QoS monitoring.

 type: object

 properties:

 refPccRuleIds:

 type: array

 items:

 type: string

 minItems: 1

 description: >

 An array of PCC rule id references to the PCC rules associated with the QoS monitoring

 report.

 ulDelays:

 type: array

 items:

 type: integer

 minItems: 1

 dlDelays:

 type: array

 items:

 type: integer

 minItems: 1

 rtDelays:

 type: array

 items:

 type: integer

 minItems: 1

 required:

 - refPccRuleIds

#

 TsnBridgeInfo:

 description: Contains parameters that describe and identify the TSC user plane node.

 type: object

 properties:

 bridgeId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 dsttAddr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

 dsttPortNum:

 $ref: '#/components/schemas/TsnPortNumber'

 dsttResidTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

#

 PortManagementContainer:

 description: Contains the port management information container for a port.

 type: object

 properties:

 portManCont:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Bytes'

 portNum:

 $ref: '#/components/schemas/TsnPortNumber'

 required:

 - portManCont

 - portNum

 BridgeManagementContainer:

 description: Contains the UMIC.

 type: object

 properties:

 bridgeManCont:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Bytes'

 required:

 - bridgeManCont

 IpMulticastAddressInfo:

 description: Contains the IP multicast addressing information.

 type: object

 properties:

 srcIpv4Addr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 ipv4MulAddr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 srcIpv6Addr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 ipv6MulAddr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 DownlinkDataNotificationControl:

 description: Contains the downlink data notification control information.

 type: object

 properties:

 notifCtrlInds:

 type: array

 items:

 $ref: '#/components/schemas/NotificationControlIndication'

 minItems: 1

 typesOfNotif:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DlDataDeliveryStatus'

 minItems: 1

 DownlinkDataNotificationControlRm:

 description: >

 This data type is defined in the same way as the DownlinkDataNotificationControl data type,

 but with the nullable:true property.

 type: object

 properties:

 notifCtrlInds:

 type: array

 items:

 $ref: '#/components/schemas/NotificationControlIndication'

 minItems: 1

 nullable: true

 typesOfNotif:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DlDataDeliveryStatus'

 minItems: 1

 nullable: true

 nullable: true

 ThresholdValue:

 description: Indicates the threshold value(s) for RTT and/or Packet Loss Rate.

 type: object

 properties:

 rttThres:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UintegerRm'

 plrThres:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketLossRateRm'

 nullable: true

 NwdafData:

 description: >

 Indicates the list of Analytic ID(s) per NWDAF instance ID used for the PDU Session consumed

 by the SMF.

 type: object

 properties:

 nwdafInstanceId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 nwdafEvents:

 type: array

 items:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/NwdafEvent'

 minItems: 1

 required:

 - nwdafInstanceId

 5GSmCause:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 EpsRanNasRelCause:

 type: string

 description: Defines the EPS RAN/NAS release cause.

 PacketFilterContent:

 type: string

 description: Defines a packet filter for an IP flow.

 FlowDescription:

 type: string

 description: Defines a packet filter for an IP flow.

 TsnPortNumber:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 ApplicationDescriptor:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Bytes'

 FlowDirection:

 anyOf:

 - type: string

 enum:

 - DOWNLINK

 - UPLINK

 - BIDIRECTIONAL

 - UNSPECIFIED

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration and is not used to encode

 content defined in the present version of this API.

 description: |

 Possible values are:

 - DOWNLINK: The corresponding filter applies for traffic to the UE.

 - UPLINK: The corresponding filter applies for traffic from the UE.

 - BIDIRECTIONAL: The corresponding filter applies for traffic both to and from the UE.

 - UNSPECIFIED: The corresponding filter applies for traffic to the UE (downlink), but has no

 specific direction declared. The service data flow detection shall apply the filter for

 uplink traffic as if the filter was bidirectional. The PCF shall not use the value

 UNSPECIFIED in filters created by the network in NW-initiated procedures. The PCF shall only

 include the value UNSPECIFIED in filters in UE-initiated procedures if the same value is

 received from the SMF.

 FlowDirectionRm:

 description: >

 This data type is defined in the same way as the "FlowDirection" data type, with the only

 difference that it allows null value.

 anyOf:

 - $ref: '#/components/schemas/FlowDirection'

 - $ref: 'TS29571\_CommonData.yaml#/components/schemas/NullValue'

 ReportingLevel:

 anyOf:

 - type: string

 enum:

 - SER\_ID\_LEVEL

 - RAT\_GR\_LEVEL

 - SPON\_CON\_LEVEL

 - $ref: 'TS29571\_CommonData.yaml#/components/schemas/NullValue'

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration and is not used to encode

 content defined in the present version of this API.

 description: |

 Possible values are:

 - SER\_ID\_LEVEL: Indicates that the usage shall be reported on service id and rating group

 combination level.

 - RAT\_GR\_LEVEL: Indicates that the usage shall be reported on rating group level.

 - SPON\_CON\_LEVEL: Indicates that the usage shall be reported on sponsor identity and rating

 group combination level.

 MeteringMethod:

 anyOf:

 - type: string

 enum:

 - DURATION

 - VOLUME

 - DURATION\_VOLUME

 - EVENT

 - $ref: 'TS29571\_CommonData.yaml#/components/schemas/NullValue'

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration and is not used to encode

 content defined in the present version of this API.

 description: |

 Possible values are:

 - DURATION: Indicates that the duration of the service data flow traffic shall be metered.

 - VOLUME: Indicates that volume of the service data flow traffic shall be metered.

 - DURATION\_VOLUME: Indicates that the duration and the volume of the service data flow

 traffic shall be metered.

 - EVENT: Indicates that events of the service data flow traffic shall be metered.

 PolicyControlRequestTrigger:

 anyOf:

 - type: string

 enum:

 - PLMN\_CH

 - RES\_MO\_RE

 - AC\_TY\_CH

 - UE\_IP\_CH

 - UE\_MAC\_CH

 - AN\_CH\_COR

 - US\_RE

 - APP\_STA

 - APP\_STO

 - AN\_INFO

 - CM\_SES\_FAIL

 - PS\_DA\_OFF

 - DEF\_QOS\_CH

 - SE\_AMBR\_CH

 - QOS\_NOTIF

 - NO\_CREDIT

 - REALLO\_OF\_CREDIT

 - PRA\_CH

 - SAREA\_CH

 - SCNN\_CH

 - RE\_TIMEOUT

 - RES\_RELEASE

 - SUCC\_RES\_ALLO

 - RAI\_CH

 - RAT\_TY\_CH

 - REF\_QOS\_IND\_CH

 - NUM\_OF\_PACKET\_FILTER

 - UE\_STATUS\_RESUME

 - UE\_TZ\_CH

 - AUTH\_PROF\_CH

 - QOS\_MONITORING

 - SCELL\_CH

 - USER\_LOCATION\_CH

 - EPS\_FALLBACK

 - MA\_PDU

 - TSN\_BRIDGE\_INFO

 - 5G\_RG\_JOIN

 - 5G\_RG\_LEAVE

 - DDN\_FAILURE

 - DDN\_DELIVERY\_STATUS

 - GROUP\_ID\_LIST\_CHG

 - DDN\_FAILURE\_CANCELLATION

 - DDN\_DELIVERY\_STATUS\_CANCELLATION

 - VPLMN\_QOS\_CH

 - SUCC\_QOS\_UPDATE

 - SAT\_CATEGORY\_CHG

 - PCF\_UE\_NOTIF\_IND

 - NWDAF\_DATA\_CHG

 - UE\_POL\_CONT\_IND

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration and is not used to encode

 content defined in the present version of this API.

 description: |

 Possible values are:

 - PLMN\_CH: PLMN Change

 - RES\_MO\_RE: A request for resource modification has been received by the SMF. The SMF

 always reports to the PCF.

 - AC\_TY\_CH: Access Type Change

 - UE\_IP\_CH: UE IP address change. The SMF always reports to the PCF.

 - UE\_MAC\_CH: A new UE MAC address is detected or a used UE MAC address is inactive for a

 specific period

 - AN\_CH\_COR: Access Network Charging Correlation Information

 - US\_RE: The PDU Session or the Monitoring key specific resources consumed by a UE either

 reached the threshold or needs to be reported for other reasons.

 - APP\_STA: The start of application traffic has been detected.

 - APP\_STO: The stop of application traffic has been detected.

 - AN\_INFO: Access Network Information report

 - CM\_SES\_FAIL: Credit management session failure

 - PS\_DA\_OFF: The SMF reports when the 3GPP PS Data Off status changes. The SMF always

 reports to the PCF.

 - DEF\_QOS\_CH: Default QoS Change. The SMF always reports to the PCF.

 - SE\_AMBR\_CH: Session-AMBR Change. The SMF always reports to the PCF.

 - QOS\_NOTIF: The SMF notify the PCF when receiving notification from RAN that QoS targets of

 the QoS Flow cannot be guranteed or gurateed again.

 - NO\_CREDIT: Out of credit

 - REALLO\_OF\_CREDIT: Reallocation of credit

 - PRA\_CH: Change of UE presence in Presence Reporting Area

 - SAREA\_CH: Location Change with respect to the Serving Area

 - SCNN\_CH: Location Change with respect to the Serving CN node

 - RE\_TIMEOUT: Indicates the SMF generated the request because there has been a PCC

 revalidation timeout

 - RES\_RELEASE: Indicate that the SMF can inform the PCF of the outcome of the release of

 resources for those rules that require so.

 - SUCC\_RES\_ALLO: Indicates that the requested rule data is the successful resource

 allocation.

 - RAI\_CH: Location Change with respect to the RAI of GERAN and UTRAN.

 - RAT\_TY\_CH: RAT Type Change.

 - REF\_QOS\_IND\_CH: Reflective QoS indication Change

 - NUM\_OF\_PACKET\_FILTER: Indicates that the SMF shall report the number of supported packet

 filter for signalled QoS rules

 - UE\_STATUS\_RESUME: Indicates that the UE's status is resumed.

 - UE\_TZ\_CH: UE Time Zone Change

 - AUTH\_PROF\_CH: The DN-AAA authorization profile index has changed

 - QOS\_MONITORING: Indicate that the SMF notifies the PCF of the QoS Monitoring information.

 - SCELL\_CH: Location Change with respect to the Serving Cell.

 - USER\_LOCATION\_CH: Indicate that user location has been changed, applicable to serving area

 change and serving cell change.

 - EPS\_FALLBACK: EPS Fallback report is enabled in the SMF.

 - MA\_PDU: UE Indicates that the SMF notifies the PCF of the MA PDU session request

 - TSN\_BRIDGE\_INFO: TSC user plane node information available

 - 5G\_RG\_JOIN: The 5G-RG has joined to an IP Multicast Group.

 - 5G\_RG\_LEAVE: The 5G-RG has left an IP Multicast Group.

 - DDN\_FAILURE: Event subscription for DDN Failure event received.

 - DDN\_DELIVERY\_STATUS: Event subscription for DDN Delivery Status received.

 - GROUP\_ID\_LIST\_CHG: UE Internal Group Identifier(s) has changed: the SMF reports that UDM

 provided list of group Ids has changed.

 - DDN\_FAILURE\_CANCELLATION: The event subscription for DDN Failure event is cancelled.

 - DDN\_DELIVERY\_STATUS\_CANCELLATION: The event subscription for DDD STATUS is cancelled.

 - VPLMN\_QOS\_CH: Change of the QoS supported in the VPLMN.

 - SUCC\_QOS\_UPDATE: Indicates that the requested MPS Action is successful.

 - SAT\_CATEGORY\_CHG: Indicates that the SMF has detected a change between different satellite

 backhaul categories, or between a satellite backhaul and a non-satellite backhaul.

 - PCF\_UE\_NOTIF\_IND: Indicates the SMF has detected the AMF forwarded the PCF for the UE

 indication to receive/stop receiving notifications of SM Policy association

 established/terminated events.

 - NWDAF\_DATA\_CHG: Indicates that the NWDAF instance IDs used for the PDU session and/or

 associated Analytics IDs used for the PDU session and available in the SMF have changed.

 - UE\_POL\_CONT\_IND: Indicates that a new UE policy container is available.

 RequestedRuleDataType:

 anyOf:

 - type: string

 enum:

 - CH\_ID

 - MS\_TIME\_ZONE

 - USER\_LOC\_INFO

 - RES\_RELEASE

 - SUCC\_RES\_ALLO

 - EPS\_FALLBACK

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration and is not used to encode

 content defined in the present version of this API.

 description: |

 Possible values are:

 - CH\_ID: Indicates that the requested rule data is the charging identifier.

 - MS\_TIME\_ZONE: Indicates that the requested access network info type is the UE's timezone.

 - USER\_LOC\_INFO: Indicates that the requested access network info type is the UE's location.

 - RES\_RELEASE: Indicates that the requested rule data is the result of the release of

 resource.

 - SUCC\_RES\_ALLO: Indicates that the requested rule data is the successful resource

 allocation.

 - EPS\_FALLBACK: Indicates that the requested rule data is the report of QoS flow rejection

 due to EPS fallback.

 RuleStatus:

 anyOf:

 - type: string

 enum:

 - ACTIVE

 - INACTIVE

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration and is not used to encode

 content defined in the present version of this API.

 description: |

 Possible values are

 - ACTIVE: Indicates that the PCC rule(s) are successfully installed (for those provisioned

 from PCF) or activated (for those pre-defined in SMF), or the session rule(s) are

 successfully installed

 - INACTIVE: Indicates that the PCC rule(s) are removed (for those provisioned from PCF) or

 inactive (for those pre-defined in SMF) or the session rule(s) are removed.

 FailureCode:

 anyOf:

 - type: string

 enum:

 - UNK\_RULE\_ID

 - RA\_GR\_ERR

 - SER\_ID\_ERR

 - NF\_MAL

 - RES\_LIM

 - MAX\_NR\_QoS\_FLOW

 - MISS\_FLOW\_INFO

 - RES\_ALLO\_FAIL

 - UNSUCC\_QOS\_VAL

 - INCOR\_FLOW\_INFO

 - PS\_TO\_CS\_HAN

 - APP\_ID\_ERR

 - NO\_QOS\_FLOW\_BOUND

 - FILTER\_RES

 - MISS\_REDI\_SER\_ADDR

 - CM\_END\_USER\_SER\_DENIED

 - CM\_CREDIT\_CON\_NOT\_APP

 - CM\_AUTH\_REJ

 - CM\_USER\_UNK

 - CM\_RAT\_FAILED

 - UE\_STA\_SUSP

 - UNKNOWN\_REF\_ID

 - INCORRECT\_COND\_DATA

 - REF\_ID\_COLLISION

 - TRAFFIC\_STEERING\_ERROR

 - DNAI\_STEERING\_ERROR

 - AN\_GW\_FAILE

 - MAX\_NR\_PACKET\_FILTERS\_EXCEEDED

 - PACKET\_FILTER\_TFT\_ALLOCATION\_EXCEEDED

 - MUTE\_CHG\_NOT\_ALLOWED

 - UE\_TEMPORARILY\_UNAVAILABLE

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration and is not used to encode

 content defined in the present version of this API.

 description: |

 Possible values are

 - UNK\_RULE\_ID: Indicates that the pre-provisioned PCC rule could not be successfully

 activated because the PCC rule identifier is unknown to the SMF.

 - RA\_GR\_ERR: Indicate that the PCC rule could not be successfully installed or enforced

 because the Rating Group specified within the Charging Data policy decision which the PCC

 rule refers to is unknown or, invalid.

 - SER\_ID\_ERR: Indicate that the PCC rule could not be successfully installed or enforced

 because the Service Identifier specified within the Charging Data policy decision which the

 PCC rule refers to is invalid, unknown, or not applicable to the service being charged.

 - NF\_MAL: Indicate that the PCC rule could not be successfully installed (for those

 provisioned from the PCF) or activated (for those pre-defined in SMF) or enforced (for those

 already successfully installed) due to SMF/UPF malfunction.

 - RES\_LIM: Indicate that the PCC rule could not be successfully installed (for those

 provisioned from PCF) or activated (for those pre-defined in SMF) or enforced (for those

 already successfully installed) due to a limitation of resources at the SMF/UPF.

 - MAX\_NR\_QoS\_FLOW: Indicate that the PCC rule could not be successfully installed (for those

 provisioned from PCF) or activated (for those pre-defined in SMF) or enforced (for those

 already successfully installed) due to the fact that the maximum number of QoS flows has

 been reached for the PDU session.

 - MISS\_FLOW\_INFO: Indicate that the PCC rule could not be successfully installed or enforced

 because neither the "flowInfos" attribute nor the "appId" attribute is specified within the

 PccRule data structure by the PCF during the first install request of the PCC rule.

 - RES\_ALLO\_FAIL: Indicate that the PCC rule could not be successfully installed or

 maintained since the QoS flow establishment/modification failed, or the QoS flow was

 released.

 - UNSUCC\_QOS\_VAL: indicate that the QoS validation has failed or when Guaranteed Bandwidth >

 Max-Requested-Bandwidth.

 - INCOR\_FLOW\_INFO: Indicate that the PCC rule could not be successfully installed or

 modified at the SMF because the provided flow information is not supported by the network

 (e.g. the provided IP address(es) or Ipv6 prefix(es) do not correspond to an IP version

 applicable for the PDU session).

 - PS\_TO\_CS\_HAN: Indicate that the PCC rule could not be maintained because of PS to CS

 handover.

 - APP\_ID\_ERR: Indicate that the rule could not be successfully installed or enforced because

 the Application Identifier is invalid, unknown, or not applicable to the application

 required for detection.

 - NO\_QOS\_FLOW\_BOUND: Indicate that there is no QoS flow which the SMF can bind the PCC

 rule(s) to.

 - FILTER\_RES: Indicate that the Flow Information within the "flowInfos" attribute cannot be

 handled by the SMF because any of the restrictions defined in clause 5.4.2 of 3GPP TS 29.212

 was not met.

 - MISS\_REDI\_SER\_ADDR: Indicate that the PCC rule could not be successfully installed or

 enforced at the SMF because there is no valid Redirect Server Address within the Traffic

 Control Data policy decision which the PCC rule refers to provided by the PCF and no

 preconfigured redirection address for this PCC rule at the SMF.

 - CM\_END\_USER\_SER\_DENIED: Indicate that the charging system denied the service request due

 to service restrictions (e.g. terminate rating group) or limitations related to the

 end-user, for example the end-user's account could not cover the requested service.

 - CM\_CREDIT\_CON\_NOT\_APP: Indicate that the charging system determined that the service can

 be granted to the end user but no further credit control is needed for the service (e.g.

 service is free of charge or is treated for offline charging).

 - CM\_AUTH\_REJ: Indicate that the charging system denied the service request in order to

 terminate the service for which credit is requested.

 - CM\_USER\_UNK: Indicate that the specified end user could not be found in the charging

 system.

 - CM\_RAT\_FAILED: Indicate that the charging system cannot rate the service request due to

 insufficient rating input, incorrect AVP combination or due to an attribute or an attribute

 value that is not recognized or supported in the rating.

 - UE\_STA\_SUSP: Indicates that the UE is in suspend state.

 - UNKNOWN\_REF\_ID: Indicates that the PCC rule could not be successfully installed/modified

 because the referenced identifier to a Policy Decision Data or to a Condition Data is

 unknown to the SMF.

 - INCORRECT\_COND\_DATA: Indicates that the PCC rule could not be successfully

 installed/modified because the referenced Condition data are incorrect.

 - REF\_ID\_COLLISION: Indicates that PCC rule could not be successfully installed/modified

 because the same Policy Decision is referenced by a session rule (e.g. the session rule and

 the PCC rule refer to the same Usage Monitoring decision data).

 - TRAFFIC\_STEERING\_ERROR: Indicates that enforcement of the steering of traffic to the

 N6-LAN or 5G-LAN failed; or the dynamic PCC rule could not be successfully installed or

 modified at the NF service consumer because there are invalid traffic steering policy identifier(s) within the provided Traffic Control Data policy decision to which the PCC

 rule refers.

 - DNAI\_STEERING\_ERROR: Indicates that the enforcement of the steering of traffic to the

 indicated DNAI failed; or the dynamic PCC rule could not be successfully installed or

 modified at the NF service consumer because there is invalid route information for a DNAI(s)

 (e.g. routing profile id is not configured) within the provided Traffic Control Data policy decision to which the PCC rule refers.

 - AN\_GW\_FAILED: This value is used to indicate that the AN-Gateway has failed and that the

 PCF should refrain from sending policy decisions to the SMF until it is informed that the

 S-GW has been recovered. This value shall not be used if the SM Policy association

 modification procedure is initiated for PCC rule removal only.

 - MAX\_NR\_PACKET\_FILTERS\_EXCEEDED: This value is used to indicate that the PCC rule could not

 be successfully installed, modified or enforced at the NF service consumer because the

 number of supported packet filters for signalled QoS rules for the PDU session has been

 reached.

 - PACKET\_FILTER\_TFT\_ALLOCATION\_EXCEEDED: This value is used to indicate that the PCC rule is

 removed at 5GS to EPS mobility because TFT allocation was not possible since the number of

 active packet filters in the EPC bearer is exceeded.

 - MUTE\_CHG\_NOT\_ALLOWED: Indicates that the PCC rule could not be successfully modified

 because the mute condition for application detection report cannot be changed. Applicable

 when the functionality introduced with the ADC feature applies.

 AfSigProtocol:

 anyOf:

 - type: string

 enum:

 - NO\_INFORMATION

 - SIP

 - $ref: 'TS29571\_CommonData.yaml#/components/schemas/NullValue'

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration and is not used to encode

 content defined in the present version of this API.

 description: |

 Possible values are

 - NO\_INFORMATION: Indicate that no information about the AF signalling protocol is being

 provided.

 - SIP: Indicate that the signalling protocol is Session Initiation Protocol.

 RuleOperation:

 anyOf:

 - type: string

 enum:

 - CREATE\_PCC\_RULE

 - DELETE\_PCC\_RULE

 - MODIFY\_PCC\_RULE\_AND\_ADD\_PACKET\_FILTERS

 - MODIFY\_ PCC\_RULE\_AND\_REPLACE\_PACKET\_FILTERS

 - MODIFY\_ PCC\_RULE\_AND\_DELETE\_PACKET\_FILTERS

 - MODIFY\_PCC\_RULE\_WITHOUT\_MODIFY\_PACKET\_FILTERS

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Possible values are

 - CREATE\_PCC\_RULE: Indicates to create a new PCC rule to reserve the resource requested by

 the UE.

 - DELETE\_PCC\_RULE: Indicates to delete a PCC rule corresponding to reserve the resource

 requested by the UE.

 - MODIFY\_PCC\_RULE\_AND\_ADD\_PACKET\_FILTERS: Indicates to modify the PCC rule by adding new

 packet filter(s).

 - MODIFY\_ PCC\_RULE\_AND\_REPLACE\_PACKET\_FILTERS: Indicates to modify the PCC rule by replacing

 the existing packet filter(s).

 - MODIFY\_ PCC\_RULE\_AND\_DELETE\_PACKET\_FILTERS: Indicates to modify the PCC rule by deleting

 the existing packet filter(s).

 - MODIFY\_PCC\_RULE\_WITHOUT\_MODIFY\_PACKET\_FILTERS: Indicates to modify the PCC rule by

 modifying the QoS of the PCC rule.

 RedirectAddressType:

 anyOf:

 - type: string

 enum:

 - IPV4\_ADDR

 - IPV6\_ADDR

 - URL

 - SIP\_URI

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration and is not used to encode

 content defined in the present version of this API.

 description: |

 Possible values are

 - IPV4\_ADDR: Indicates that the address type is in the form of "dotted-decimal" IPv4

 address.

 - IPV6\_ADDR: Indicates that the address type is in the form of IPv6 address.

 - URL: Indicates that the address type is in the form of Uniform Resource Locator.

 - SIP\_URI: Indicates that the address type is in the form of SIP Uniform Resource

 Identifier.

 QosFlowUsage:

 anyOf:

 - type: string

 enum:

 - GENERAL

 - IMS\_SIG

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration and is not used to encode

 content defined in the present version of this API.

 description: |

 Possible values are

 - GENERAL: Indicate no specific QoS flow usage information is available.

 - IMS\_SIG: Indicate that the QoS flow is used for IMS signalling only.

 FailureCause:

 description: Indicates the cause of the failure in a Partial Success Report.

 anyOf:

 - type: string

 enum:

 - PCC\_RULE\_EVENT

 - PCC\_QOS\_FLOW\_EVENT

 - RULE\_PERMANENT\_ERROR

 - RULE\_TEMPORARY\_ERROR

 - POL\_DEC\_ERROR

 - type: string

 description: >

 This string provides forward-compatibility with future extensions to the enumeration

 and is not used to encode content defined in the present version of this API.

 CreditManagementStatus:

 description: Indicates the reason of the credit management session failure.

 anyOf:

 - type: string

 enum:

 - END\_USER\_SER\_DENIED

 - CREDIT\_CTRL\_NOT\_APP

 - AUTH\_REJECTED

 - USER\_UNKNOWN

 - RATING\_FAILED

 - type: string

 description: >

 This string provides forward-compatibility with future extensions to the enumeration

 and is not used to encode content defined in the present version of this API.

 SessionRuleFailureCode:

 anyOf:

 - type: string

 enum:

 - NF\_MAL

 - RES\_LIM

 - SESSION\_RESOURCE\_ALLOCATION\_FAILURE

 - UNSUCC\_QOS\_VAL

 - INCORRECT\_UM

 - UE\_STA\_SUSP

 - UNKNOWN\_REF\_ID

 - INCORRECT\_COND\_DATA

 - REF\_ID\_COLLISION

 - AN\_GW\_FAILED

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration and is not used to encode

 content defined in the present version of this API.

 description: |

 Possible values are

 - NF\_MAL: Indicates that the PCC rule could not be successfully installed (for those

 provisioned from the PCF) or activated (for those pre-defined in SMF) or enforced (for those

 already successfully installed) due to SMF/UPF malfunction.

 - RES\_LIM: Indicates that the PCC rule could not be successfully installed (for those

 provisioned from PCF) or activated (for those pre-defined in SMF) or enforced (for those

 already successfully installed) due to a limitation of resources at the SMF/UPF.

 - SESSION\_RESOURCE\_ALLOCATION\_FAILURE: Indicates the session rule could not be successfully

 enforced due to failure during the allocation of resources for the PDU session in the UE,

 RAN or AMF.

 - UNSUCC\_QOS\_VAL: indicates that the QoS validation has failed.

 - INCORRECT\_UM: The usage monitoring data of the enforced session rule is not the same for

 all the provisioned session rule(s).

 - UE\_STA\_SUSP: Indicates that the UE is in suspend state.

 - UNKNOWN\_REF\_ID: Indicates that the session rule could not be successfully

 installed/modified because the referenced identifier to a Policy Decision Data or to a

 Condition Data is unknown to the SMF.

 - INCORRECT\_COND\_DATA: Indicates that the session rule could not be successfully

 installed/modified because the referenced Condition data are incorrect.

 - REF\_ID\_COLLISION: Indicates that the session rule could not be successfully

 installed/modified because the same Policy Decision is referenced by a PCC rule (e.g. the

 session rule and the PCC rule refer to the same Usage Monitoring decision data).

 - AN\_GW\_FAILED: Indicates that the AN-Gateway has failed and that the PCF should refrain

 from sending policy decisions to the SMF until it is informed that the S-GW has been

 recovered. This value shall not be used if the SM Policy association modification procedure

 is initiated for session rule removal only.

 SteeringFunctionality:

 anyOf:

 - type: string

 enum:

 - MPTCP

 - ATSSS\_LL

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration and is not used to encode

 content defined in the present version of this API.

 description: |

 Possible values are

 - MPTCP: Indicates that PCF authorizes the MPTCP functionality to support traffic

 steering, switching and splitting.

 - ATSSS\_LL: Indicates that PCF authorizes the ATSSS-LL functionality to support traffic

 steering, switching and splitting.

 SteerModeValue:

 description: Indicates the steering mode value determined by the PCF.

 anyOf:

 - type: string

 enum:

 - ACTIVE\_STANDBY

 - LOAD\_BALANCING

 - SMALLEST\_DELAY

 - PRIORITY\_BASED

 - type: string

 description: >

 This string provides forward-compatibility with future extensions to the enumeration

 and is not used to encode content defined in the present version of this API.

 MulticastAccessControl:

 description: >

 Indicates whether the service data flow, corresponding to the service data flow template, is

 allowed or not allowed.

 anyOf:

 - type: string

 enum:

 - ALLOWED

 - NOT\_ALLOWED

 - type: string

 description: >

 This string provides forward-compatibility with future extensions to the enumeration

 and is not used to encode content defined in the present version of this API.

 RequestedQosMonitoringParameter:

 description: Indicates the requested QoS monitoring parameters to be measured.

 anyOf:

 - type: string

 enum:

 - DOWNLINK

 - UPLINK

 - ROUND\_TRIP

 - type: string

 description: >

 This string provides forward-compatibility with future extensions to the enumeration

 and is not used to encode content defined in the present version of this API.

 ReportingFrequency:

 description: Indicates the frequency for the reporting.

 anyOf:

 - type: string

 enum:

 - EVENT\_TRIGGERED

 - PERIODIC

 - SESSION\_RELEASE

 - type: string

 description: >

 This string provides forward-compatibility with future extensions to the enumeration

 and is not used to encode content defined in the present version of this API.

 SgsnAddress:

 description: describes the address of the SGSN

 type: object

 anyOf:

 - required: [sgsnIpv4Addr]

 - required: [sgsnIpv6Addr]

 properties:

 sgsnIpv4Addr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 sgsnIpv6Addr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 SmPolicyAssociationReleaseCause:

 description: >

 Represents the cause due to which the PCF requests the termination of the SM policy

 association.

 anyOf:

 - type: string

 enum:

 - UNSPECIFIED

 - UE\_SUBSCRIPTION

 - INSUFFICIENT\_RES

 - VALIDATION\_CONDITION\_NOT\_MET

 - REACTIVATION\_REQUESTED

 - type: string

 description: >

 This string provides forward-compatibility with future extensions to the enumeration

 and is not used to encode content defined in the present version of this API.

 PduSessionRelCause:

 description: Contains the SMF PDU Session release cause.

 anyOf:

 - type: string

 enum:

 - PS\_TO\_CS\_HO

 - RULE\_ERROR

 - type: string

 description: >

 This string provides forward-compatibility with future extensions to the enumeration

 and is not used to encode content defined in the present version of this API.

 MaPduIndication:

 description: >

 Contains the MA PDU session indication, i.e., MA PDU Request or MA PDU Network-Upgrade

 Allowed.

 anyOf:

 - type: string

 enum:

 - MA\_PDU\_REQUEST

 - MA\_PDU\_NETWORK\_UPGRADE\_ALLOWED

 - type: string

 description: >

 This string provides forward-compatibility with future extensions to the enumeration

 and is not used to encode content defined in the present version of this API.

 AtsssCapability:

 description: Contains the ATSSS capability supported for the MA PDU Session.

 anyOf:

 - type: string

 enum:

 - MPTCP\_ATSSS\_LL\_WITH\_ASMODE\_UL

 - MPTCP\_ATSSS\_LL\_WITH\_EXSDMODE\_DL\_ASMODE\_UL

 - MPTCP\_ATSSS\_LL\_WITH\_ASMODE\_DLUL

 - ATSSS\_LL

 - MPTCP\_ATSSS\_LL

 - type: string

 description: >

 This string provides forward-compatibility with future extensions to the enumeration

 and is not used to encode content defined in the present version of this API.

#

 NetLocAccessSupport:

 anyOf:

 - type: string

 enum:

 - ANR\_NOT\_SUPPORTED

 - TZR\_NOT\_SUPPORTED

 - LOC\_NOT\_SUPPORTED

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration and is not used to encode

 content defined in the present version of this API.

 description: |

 Possible values are

 - ANR\_NOT\_SUPPORTED: Indicates that the access network does not support the report of access

 network information.

 - TZR\_NOT\_SUPPORTED: Indicates that the access network does not support the report of UE

 time zone.

 - LOC\_NOT\_SUPPORTED: Indicates that the access network does not support the report of UE

 Location (or PLMN Id).

 PolicyDecisionFailureCode:

 description: Indicates the type of the failed policy decision and/or condition data.

 anyOf:

 - type: string

 enum:

 - TRA\_CTRL\_DECS\_ERR

 - QOS\_DECS\_ERR

 - CHG\_DECS\_ERR

 - USA\_MON\_DECS\_ERR

 - QOS\_MON\_DECS\_ERR

 - CON\_DATA\_ERR

 - POLICY\_PARAM\_ERR

 - type: string

 description: >

 This string provides forward-compatibility with future extensions to the enumeration

 and is not used to encode content defined in the present version of this API.

#

 NotificationControlIndication:

 description: >

 Indicates that the notification of DDD Status is requested and/or that the notification of

 DDN Failure is requested.

 anyOf:

 - type: string

 enum:

 - DDN\_FAILURE

 - DDD\_STATUS

 - type: string

 description: >

 This string provides forward-compatibility with future extensions to the enumeration

 and is not used to encode content defined in the present version of this API.

#

 SteerModeIndicator:

 description: Contains Autonomous load-balance indicator or UE-assistance indicator.

 anyOf:

 - type: string

 enum:

 - AUTO\_LOAD\_BALANCE

 - UE\_ASSISTANCE

 - type: string

 description: >

 This string provides forward-compatibility with future extensions to the enumeration

 and is not used to encode content defined in the present version of this API.

#

\* \* \* Next Change \* \* \* \*

### C.2.1.5 Policy control request trigger

The Policy Control Request Triggers defined in clause 5.6.3.6 and related procedures are supported for a 5G-RG connecting to the 5GC via NG-RAN.

The Policy Control Request Triggers defined in clause 5.6.3.6 are supported for a 5G-RG or FN-RG connecting to the 5GC via W-5GAN with the following not supporting ones:

- PLMN\_CH

- SAREA\_CH

- SCNN\_CH

- PRA\_CH

- PS\_DA\_OFF

- QOS\_NOTIF

- RES\_RELEASE

- UE\_STATUS\_RESUME

- TSN\_BRIDGE\_INFO

- QOS\_MONITORING

- SCELL\_CH

- EPS\_FALLBACK

- DDN\_FAILURE

- DDN\_DELIVERY\_STATUS

- USER\_LOCATION\_CH

- UE\_POL\_CONT\_IND

Consequently, the procedures related to above policy control request triggers are not supported in the corresponding service operations.

The PS\_DA\_OFF Policy Control Request Trigger may apply for the 5G-RG connecting to the 5GC via W-5GAN (see clause 4.2.2.8 and 4.2.4.8) in an hybrid access scenario (see clause C.3.6.2).

The RES\_MO\_RE Policy Control Request trigger is not supported for a FN-RG as described in BBF TR-456 [47] and CableLabs WR-TR-5WWC-ARCH [48] specification.

\* \* \* End Change \* \* \* \*