**3GPP TSG-CT WG3 Meeting #128 *C3-232172***

**Bratislava, Slovakia, 22nd - 26th May, 2023 (revision of C3-232abc)**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.522** | **CR** | **0935** | **rev** | **-** | **Current version:** | **18.1.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | MemberUESelectionAssistance API, OpenAPI definition | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei, Ericsson | | | | | | | | | |
| ***Source to TSG:*** | CT3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | AIMLsys | | | | |  | ***Date:*** | | | 2023-05-05 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | In order to enable 5GC to assist the Application AI/ML AF to preform candidate member selection, a new NEF northbound serivce (i.e. Nnef\_MemberUESelectionAssistance service) is specifed in TS 23.502 to enable the AF request the NEF to provide a list of recommended UEs based on the member selection filtering criteria requested by the AF.  It is proposed to define a new API for the new service. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Define the OpenAPI file for the new service. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Misalignment between stage 2 and stage 3. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | A.29 (new) | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | | **X** |  | Other core specifications | | | | TS/TR 23.501 CR 4565  TS/TR 23.502 CR 4157 | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | The CR introduces a new OpenAPI file for MemberUESelectionAssistance API. | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

**Additional discussion(if needed):**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

A.29 MemberUESelectionAssistance API

openapi: 3.0.0

info:

title: 3gpp-musa

version: 1.0.0-alpha.1

description: |

API for Member UE Selectio nAssistance.

© 2023, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: >

3GPP TS 29.522 V18.1.0; 5G System; Network Exposure Function Northbound APIs.

url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.522/'

servers:

- url: '{apiRoot}/3gpp-musa/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 4.4 of 3GPP TS 29.501

security:

- {}

- oAuth2ClientCredentials: []

paths:

/{afId}/subscriptions:

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

get:

summary: read all of the active subscriptions for the AF

operationId: ReadAllSubscriptions

tags:

- Member UE Selection Assistance Subscription

responses:

'200':

description: OK.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/MemUeSelectAssistSubsc'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

post:

summary: Create a new subscription to Member UE Selection Assistance.

operationId: CreateMemberUESelectionAssistanceSubcription

tags:

- Member UE Selection Assistance Subscription

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/MemUeSelectAssistSubsc'

responses:

'201':

description: Create a new Individual Member UE Selection Assistance Subscription resource.

content:

application/json:

schema:

$ref: '#/components/schemas/MemUeSelectAssistSubsc'

headers:

Location:

description: >

Contains the URI of the newly created resource, according to the structure

{apiRoot}/3gpp-musa/v1/{afId}/subscriptions/{subscriptionId}.

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

callbacks:

notificationDestination:

'{$request.body#/notifUri}':

post:

requestBody:

required: true

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/MemUeSeletAssistNotif'

minItems: 1

responses:

'204':

description: No Content, Notification was succesfull

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{afId}/subscriptions/{subscriptionId}:

parameters:

- name: afId

in: path

description: Identifier of the AF.

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource.

required: true

schema:

type: string

get:

summary: Read an active subscription identified by the subscriptionId.

tags:

- Individual Member UE Selection Assistance Subscription

responses:

'200':

description: OK (Successful get the active subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/MemUeSelectAssistSubsc'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

put:

summary: Update/Replace an existing subscription resource.

tags:

- Individual Member UE Selection Assistance Subscription

requestBody:

description: Parameters to replace the existing subscription.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/MemUeSelectAssistSubsc'

responses:

'200':

description: OK (Successful update of the subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/MemUeSelectAssistSubsc'

'204':

description: No Content

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

summary: Delete an existing subscription.

tags:

- Individual Member UE Selection Assistance Subscription

responses:

'204':

description: No Content (Successful deletion of the existing subscription)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{nrfApiRoot}/oauth2/token'

scopes: {}

schemas:

MemUeSelectAssistSubsc:

description: Represents an Member UE Selection Assistance Subscription.

type: object

properties:

tgtUes:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

minItems: 1

description: Identifies the list of UEs for Member Selection Assistance Reporting.

notifUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

notifId:

type: string

filterCriters:

type: string

appId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

expTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

timeWins:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

required:

- tgtUes

- notifUri

- notifId

- filterCriters

MemUeSeletAssistNotif:

description: Represents a Member UE Selection Assistance notification.

type: object

properties:

notifId:

type: string

remdUes:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

minItems: 1

description: Identifies the list of UEs for Member Selection Assistance Reporting.

required:

- notifId

- remdUes

\*\*\* End of Changes \*\*\*