**3GPP TSG-CT WG3 Meeting #128 *C3-232612***

**Bratislava, Slovakia, 22nd - 26th May, 2023** (revision of C3-232369)

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.122** | **CR** | **0666** | **rev** | **2** | **Current version:** | **18.1.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **x** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | AsSessionWithQoS enhancements to support multi-modal services | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Ericsson | | | | | | | | | |
| ***Source to TSG:*** | CT3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | XRM | | | | |  | ***Date:*** | | | 2023-05-26 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | B |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | 3GPP TS 23.501, 23.502 and TS 23.503 version 18.1.0 include Policy control enhancements to support multi-modal services, as agreed in SA2#155 meeting.  As introduced in DP C3-232358, the AsSessionWithQoS can be extended to support in an AF request the QoS request for multiple single-modal data flows.  Impacts to AsSessionWithQoS API must be reflected in stage 3 | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | AsSessionWithQoS API is enhanced with additional parameters to allow the AF provides service requirements for each single-modal data flow that comprises the multi-modal service:   * A new IE multiModDatFlows, a map of AsSessMediaComponent data type, is added to encode the multiple single-modal data and flows. * The AsSessMediaComponent data type (defined in 5.14.2.1.13) is composed by the IEs of the MediaComponent data type (which represents the QoS requirements for the single-modal data flow), and flow information for the single-modal data flow. * A new referenced structured data type “MultiModalFlows” is added in a new clause 5.14.2.1.14, to represent a single-modal flow information within a media component * A new attribute "multiModFlows = array(MultiModalFlows)” is added to data type: UserPlaneEventReport | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | There is an inconsistency between SA2 and CT3 in terms of AsSessionWithQoS API to support multi-modal services | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.14.2.1.1, 5.14.2.1.2, 5.14.2.1.3, 5.14.2.1.5, 5.14.2.1.13 (new), 5.14.2.1.14 (new), 5.14.2.1.15 (new), 5.14.2.1.16 (new), A.14 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **x** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **x** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **x** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR impacts the AsSessionWithQoS OpenAPI file with a backwards compatible feature. | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

\* \* \* \* First change \* \* \* \*

##### 5.14.2.1.1 Introduction

This clause defines data structures to be used in resource representations, including subscription resources.

Table 5.14.2.1.1-1 specifies data types re-used by the AsSessionWithQoS API from other specifications, including a reference to their respective specifications and when needed, a short description of their use within the AsSessionWithQoS API.

Table 5.14.2.1.1-1: AsSessionWithQoS API re-used Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Reference | Comments | Applicability |
| AcceptableServiceInfo | 3GPP TS 29.514 [52] | Acceptable maximum requested bandwidth. |  |
| AlternativeServiceRequirementsData | 3GPP TS 29.514 [52] | Contains alternative QoS related parameters and a reference to them. |  |
| BitRate | 3GPP TS 29.571 [45] | String representing a bit rate that shall be formatted as follows:  Pattern: '^\d+(\.\d+)? (bps|Kbps|Mbps|Gbps|Tbps)$'  Examples:  "125 Mbps", "0.125 Gbps", "125000 Kbps" |  |
| BitRateRm | 3GPP TS 29.571 [45] | This data type is defined in the same way as the "BitRate" data type, but with the OpenAPI "nullable: true" property. |  |
| Dnn | 3GPP TS 29.571 [45] | Identifies a DNN. |  |
| EthFlowDescription | 3GPP TS 29.514 [52] | Defines a packet filter for an Ethernet flow.(NOTE 1) |  |
| ExtMaxDataBurstVol | 3GPP TS 29.571 [45] | Unsigned integer indicating Maximum Data Burst Volume (see clauses 5.7.3.7 and 5.7.4 of 3GPP TS 23.501 [8]), expressed in Bytes.  Minimum = 4096. Maximum = 2000000. |  |
| ExtMaxDataBurstVolRm | 3GPP TS 29.571 [45] | This data type is defined in the same way as the "ExtMaxDataBurstVol" data type, but with the OpenAPI "nullable: true" property. |  |
| IpAddr | 3GPP TS 29.571 [45] | UE IP Address. |  |
| MacAddr48 | 3GPP TS 29.571 [45] | MAC Address. |  |
| MediaType | 3GPP TS 29.514 [52] | Indicates the media type of a single-modal data flow of a multimodal service. | XRM\_5G |
| MultiModalId | 3GPP TS 29.514 [52] | Represents multi-modal service identifier. | XRM\_5G |
| PacketDelBudget | 3GPP TS 29.571 [45] | Unsigned integer indicating Packet Delay Budget (see clauses 5.7.3.4 and 5.7.4 of 3GPP TS 23.501 [8])), expressed in milliseconds.  Minimum = 1. |  |
| PacketDelBudgetRm | 3GPP TS 29.571 [45] | This data type is defined in the same way as the "PacketDelBudget" data type, but with the OpenAPI "nullable: true" property. |  |
| PacketErrRate | 3GPP TS 29.571 [45] | String representing Packet Error Rate (see clauses 5.7.3.5 and 5.7.4 of 3GPP TS 23.501 [8]), expressed as a "*scalar* x 10-k" where the scalar and the *exponent k are each encoded as one decimal digit*.  Pattern: '^([0-9]E-[0-9])$'  Examples:  Packer Error Rate 4x10-6 shall be encoded as "4E-6".  Packer Error Rate 10-2 shall be encoded as "1E-2". |  |
| PacketErrRateRm | 3GPP TS 29.571 [45] | This data type is defined in the same way as the "PacketErrRate" data type, but with the OpenAPI "nullable: true" property. |  |
| PlmnIdNid | 3GPP TS 29.571 [45] | Identifies the network: the PLMN Identifier (the mobile country code and the mobile network code) or the SNPN Identifier (the PLMN Identifier and the NID). |  |
| ProblemDetails | 5.2.1.2.12 | Problem Details when returning an error response. |  |
| RatType | 3GPP TS 29.571 [45] | Identifies the RAT Type. |  |
| ReportingFrequency | 3GPP TS 29.512 [8] | Indicates the frequency for the reporting, such as event triggered, periodic, when the PDU Session is released, and/or any combination. (NOTE 2) |  |
| RequestedQosMonitoringParameter | 3GPP TS 29.512 [8] | Indicates the QoS information to be measured, e.g.UL packet delay, DL packet delay or round trip packet delay between the UE and the UPF is to be monitored when the QoS Monitoring for packet delay is enabled for the service data flow. (NOTE 2) |  |
| Snssai | 3GPP TS 29.571 [45] | Identifies the S-NSSAI. |  |
| SupportedFeatures | 3GPP TS 29.571 [45] | Used to negotiate the applicability of the optional features defined in table 5.14.4-1. |  |
| TscaiInputContainer | 3GPP TS 29.514 [52] | TSCAI Input information container. | TSC\_5G, XRM\_5G |
| TscPriorityLevel | 3GPP TS 29.514 [52] | Represents priority of TSC Flows. | TSC\_5G, XRM\_5G |
| TscPriorityLevelRm | 3GPP TS 29.514 [52] | Represents the same as the TscPriorityLevel data type, but with the OpenAPI "nullable: true" property. | TSC\_5G, XRM\_5G |
| TsnQosContainer | 3GPP TS 29.514 [52] | Represents individual QoS parameters | XRM\_5G |
| TsnQosContainerRm | 3GPP TS 29.514 [52] | Represents the same as the TsnQosContainer data type, but with the OpenAPI "nullable: true" property. | XRM\_5G |
| Uinteger | 3GPP TS 29.571 [45] | Unsigned Integer, i.e. only value 0 and integers above 0 are permissible.  Minimum = 0. |  |
| UintegerRm | 3GPP TS 29.571 [45] | This data type is defined in the same way as the "Uinteger" data type, but with the OpenAPI "nullable: true" property. |  |
| NOTE 1: In order to support a set of MAC addresses with a specific range in the traffic filter, feature MacAddressRange\_5G as specified in clause 5.14.4 shall be supported.  NOTE 2: In order to support QoS Monitoring, feature QoSMonitoring\_5G as specified in clause 5.14.4 shall be supported. | | |  |

Table 5.14.2.1.1-2 specifies the data types defined for the AsSessionWithQoS API.

Table 5.14.2.1.1-2: AsSessionWithQoS API specific Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Clause defined | Description | Applicability |
| AdditionalInfoAsSessionWithQos | 5.14.2.1.10 | Describes additional error information specific for this API. |  |
| AsSessionWithQoSSubscription | 5.14.2.1.2 | Represents an individual AS session with required QoS subscription resource. |  |
| AsSessionWithQoSSubscriptionPatch | 5.14.2.1.3 | Represents parameters to modify an AS session with specific QoS subscription. |  |
| AsSessionMediaComponent | 5.14.2.1.13 | Represents media component data for a multimodal service. It contains service data flow information for a single modal data flow of a multimodal service. | XRM\_5G |
| AsSessionMediaComponentRm | 5.14.2.1.14 | Represents the same as the AsSessMediaComponent data type but with the "nullable: true" property. | XRM\_5G |
| MultiModalFlows | 5.14.2.1.15 | Represents flow information within a single-modal data flow for a multimodal service. | XRM\_5G |
| ProblemDetailsAsSessionWithQos | 5.14.2.1.11 | ProblemDetails as defined in clause 5.2.12.12 extended with specific error information for this API, as described in AdditionalInfoAsSessionWithQos. |  |
| QosMonitoringInformation | 5.14.2.1.6 | Represents QoS monitoring information. | QoSMonitoring\_5G |
| QosMonitoringInformationRm | 5.14.2.1.7 | Represents the same as the QosMonitoringInformation data type but with the "nullable: true" property. | QoSMonitoring\_5G |
| QosMonitoringReport | 5.14.2.1.8 | Represents a QoS monitoring report. | QoSMonitoring\_5G |
| TscQosRequirement | 5.14.2.1.9 | Represents QoS requirements for time sensitive communication. | TSC\_5G |
| TscQosRequirementRm | 5.14.2.1.10 | Represents the same as the TscQosRequirement data type but with the "nullable: true" property. | TSC\_5G |
| UserPlaneEvent | 5.14.2.2.3 | Represents the user plane event. | enNB |
| UserPlaneEventReport | 5.14.2.1.5 | Represents an event report for user plane. | enNB |
| UserPlaneNotificationData | 5.14.2.1.4 | Represents the parameters to be conveyed in a user plane event(s) notification. | enNB |

\*\*\* Next Change \*\*\*

##### 5.14.2.1.2 Type: AsSessionWithQoSSubscription

This type represents an AS session request with specific QoS for the service provided by the SCS/AS to the SCEF via T8 interface. The structure is used for subscription request and response.

Table 5.14.2.1.2-1: Definition of type AsSessionWithQoSSubscription

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | Cardinality | Description | Applicability (NOTE 1) |
| self | Link | 0..1 | Link to the resource "Individual AS Session with Required QoS Subscription".  This parameter shall be supplied by the SCEF in HTTP responses. |  |
| dnn | Dnn | 0..1 | Identifies a DNN, a full DNN with both the Network Identifier and Operator Identifier, or a DNN with the Network Identifier only. (NOTE 3) |  |
| snssai | Snssai | 0..1 | Identifies an S-NSSAI. (NOTE 3) |  |
| supportedFeatures | SupportedFeatures | 0..1 | Used to negotiate the supported optional features of the API as described in clause 5.2.7.  This attribute shall be provided in the POST request and in the response of successful resource creation. |  |
| notificationDestination | Link | 1 | Contains the URL to receive the notification bearer level event(s) from the SCEF. |  |
| exterAppId | string | 0..1 | Identifies the external Application Identifier. (NOTE 2) | AppId |
| flowInfo | array(FlowInfo) | 0..N | Describe the IP data flow which requires QoS.  (NOTE 2) |  |
| ethFlowInfo | array(EthFlowDescription) | 0..N | Identifies Ethernet packet flows.  (NOTE 2) (NOTE 6) | EthAsSessionQoS\_5G |
| enEthFlowInfo | array(EthFlowInfo) | 0..N | Identifies the Ethernet flows which require QoS. Each Ethernet flow consists of a flow identifier and the corresponding UL and/or DL flows.  (NOTE 2) (NOTE 6) | EnEthAsSessionQoS\_5G |
| qosReference | string | 0..1 | Identifies a pre-defined QoS information. (NOTE 5) |  |
| altQoSReferences | array(string) | 0..N | Identifies an ordered list of pre-defined QoS information. The lower the index of the array for a given entry, the higher the priority. (NOTE 4) | AlternativeQoS\_5G |
| altQosReqs | array(AlternativeServiceRequirementsData) | 0..N | Identifies an ordered list of alternative service requirements that include individual QoS parameter sets. The lower the index of the array for a given entry, the higher the priority. (NOTE 4) | AltQosWithIndParams\_5G |
| disUeNotif | boolean | 0..1 | Indicates whether to disable QoS flow parameters signalling to the UE when the SMF is notified by the NG-RAN of changes in the fulfilled QoS situation. The fulfilled situation is either the QoS profile or an Alternative QoS Profile.  - true: the QoS flow parameters signalling to the UE is disabled;  - false (default): the QoS flow parameters signalling to the UE is not disabled. | DisableUENotification\_5G |
| ueIpv4Addr | Ipv4Addr | 0..1 | The Ipv4 address of the UE.  (NOTE 2) |  |
| ipDomain | string | 0..1 | The IPv4 address domain identifier.  The attribute may only be provided if the ueIpv4Addr attribute is present. |  |
| ueIpv6Addr | Ipv6Addr | 0..1 | The Ipv6 address of the UE.  (NOTE 2) |  |
| macAddr | MacAddr48 | 0..1 | Identifies the MAC address.  (NOTE 2) | EthAsSessionQoS\_5G |
| usageThreshold | UsageThreshold | 0..1 | Time period and/or traffic volume in which the QoS is to be applied. |  |
| sponsorInfo | SponsorInformation | 0..1 | Indicates a sponsor information |  |
| qosMonInfo | QosMonitoringInformation | 0..1 | Qos Monitoring information. It can be present when the event "QOS\_MONITORING" is subscribed. | QoSMonitoring\_5G |
| directNotifInd | boolean | 0..1 | Indicates whether the direct event notification is requested.  - true: the direct event notification is requested;  - false (default): the direct event notification is not requested. | ExposureToEAS |
| tscQosReq | TscQosRequirement | 0..1 | Contains the QoS requirements for time sensitive communication. (NOTE 5) | TSC\_5G |
| requestTestNotification | boolean | 0..1 | Set to true by the SCS/AS to request the SCEF to send a test notification as defined in clause 5.2.5.3. Set to false or omitted otherwise. | Notification\_test\_event |
| websockNotifConfig | WebsockNotifConfig | 0..1 | Configuration parameters to set up notification delivery over Websocket protocol as defined in clause 5.2.5.4. | Notification\_websocket |
| events | array(UserPlaneEvent) | 0..N | Corresponds to the list of user plane event(s) to which the SCS/AS requests to subscribe to. | enNB |
| multiModalId | MultiModalId | 0..1 | Multi-modal Service Identifier, as defined in 3GPP TS 29.514 [52]. | XRM\_5G |
| multiModDatFlows | map(AsSessionMediaComponent) | 0..N | Each element of the map represents Media Component data for a single-modal data flow(s) of a multimodal service. The key of the map is the attribute "medCompN". (NOTE 7) | XRM\_5G |
| NOTE 1: Properties marked with a feature as defined in clause 5.14.4 are applicable as described in clause 5.2.7. If no features are indicated, the related property applies for all the features.  NOTE 2: One of "ueIpv4Addr", "ueIpv6Addr" or "macAddr" shall be included. If ipv4 or ipv6 address is provided, IP flow information shall be provided. If MAC address is provided and the AppId feature is not supported, Ethernet flow information (either "ethFlowInfo", or if the feature EnEthAsSessionQoS\_5G is supported, "enEthFlowInfo")shall be provided. If the AppId feature is supported, one of IP flow information, Ethernet flow information (if EthAsSessionQoS\_5G and/or EnEthAsSessionQoS\_5G is supported) or External Application Identifier shall be provided.  NOTE 3: The property is only applicable for the NEF.  NOTE 4: The attributes "altQoSReferences" and "altQosReqs" are mutually exclusive. The attributes "qosReference" and "altQosReqs" are also mutually exclusive.  NOTE 5: The attributes "reqGbrDl", "reqGbrUl", "reqMbrDl", "reqMbrUl", "maxTscBurstSize", "req5Gsdelay", "reqPer" (if the ExtQoS\_5G feature is supported), and "priority" within the "tscQosReq" attribute may be provided only if the "qosReference" attribute is not provided.  NOTE 6: When the Ethernet flow information is provided and, the EthAsSessionQoS\_5G and EnEthAsSessionQoS\_5G features are supported, either the "ethFlowInfo" or the "enEthFlowInfo" shall be provided, but not both simultenously.  NOTE 7: The attributes "exterAppId", "flowInfo", "ethFlowInfo", "enEthFlowInfo", "qosReference", "altQoSReferences", "altQosReqs", "tscQosReq", "qosMonInfo" may be provided only if the "multiModDatFlows" attribute is not provided. | | | | |

Editor’s Note: The support of multiple modal flows (multiModalFlows) in the same AF request needs to be revisited based on the SA2 progress in next meetings.

\*\*\* Next Change \*\*\*

##### 5.14.2.1.3 Type: AsSessionWithQoSSubscriptionPatch

This type represents an AS session request with specific QoS for the service provided by the SCS/AS to the SCEF via T8 interface. The structure is used for PATCH request.

Table 5.14.2.1.3-1: Definition of type AsSessionWithQoSSubscriptionPatch

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | Cardinality | Description | Applicability (NOTE 1) |
| exterAppId | string | 0..1 | Identifies the external Application Identifier. (NOTE 2) | AppId |
| flowInfo | array(FlowInfo) | 0..N | Describe the data flow which requires QoS. (NOTE 2) |  |
| ethFlowInfo | array(EthFlowDescription) | 0..N | Describes Ethernet packet flows. (NOTE 2) | EthAsSessionQoS\_5G |
| enEthFlowInfo | array(EthFlowInfo) | 0..N | Identifies the Ethernet flows which require QoS. Each Ethernet flow consists of a flow identifier and the corresponding UL and/or DL flows.  (NOTE 2) | EnEthAsSessionQoS\_5G |
| qosReference | string | 0..1 | Pre-defined QoS reference. (NOTE 3) (NOTE 4) |  |
| altQoSReferences | array(string) | 0..N | Identifiers an ordered list of pre-defined QoS information. The lower the index of the array for a given entry, the higher the priority. (NOTE 3) | AlternativeQoS\_5G |
| altQosReqs | array(AlternativeServiceRequirementsData) | 1..N | Identifies an ordered list of alternative service requirements that include individual QoS parameter sets. The lower the index of the array for a given entry, the higher the priority. (NOTE 3) | AltQosWithIndParams\_5G |
| disUeNotif | boolean | 0..1 | Indicates whether to disable QoS flow parameters signalling to the UE when the SMF is notified by the NG-RAN of changes in the fulfilled QoS situation. The fulfilled situation is either the QoS profile or an Alternative QoS Profile.  - true: the QoS flow parameters signalling to the UE is disabled;  - false: the QoS flow parameters signalling to the UE is not disabled. | DisableUENotification\_5G |
| usageThreshold | UsageThresholdRm | 0..1 | Time period and/or traffic volume in which the QoS is to be applied. |  |
| qosMonInfo | QosMonitoringInformationRm | 0..1 | Qos Monitoring information. It can be present when the event "QOS\_MONITORING" is subscribed. | QoSMonitoring\_5G |
| directNotifInd | boolean | 0..1 | Indicates whether the direct event notification is requested.  - true: the direct event notification is requested;  - false: the direct event notification is not requested. | ExposureToEAS |
| tscQosReq | TscQosRequirementRm | 0..1 | Contains the QoS requirements for time sensitive communication. (NOTE 4) | TSC\_5G |
| notificationDestination | Link | 0..1 | Contains the URL to receive the notification event(s) from the SCEF. |  |
| events | array(UserPlaneEvent) | 0..N | Corresponds to the list of user plane event(s) to which the SCS/AS requests to subscribe to. | enNB |
| multiModalId | MultiModalId | 0..1 | Multi-modal Service Identifier, as defined in 3GPP TS 29.514 [52]. | XRM\_5G |
| multiModDatFlows | map(AsSessionMediaComponentRm) | 0..N | Each element of the map represents Media Component data for a single-modal data flow(s) of a multimodal service. The key of the map is the attribute "medCompN". (NOTE 5) | XRM\_5G |
| NOTE 1: Properties marked with a feature as defined in clause 5.14.4 are applicable as described in clause 5.2.7. If no features are indicated, the related property applies for all the features.  NOTE 2: One of "exterAppId", "flowInfo" or either "ethFlowInfo" or "enEthFlowInfo" may be provided.  NOTE 3 The attributes "altQoSReferences" and "altQosReqs" are mutually exclusive. The attributes "qosReference" and "altQosReqs" are also mutually exclusive.  NOTE 4: The attributes "reqGbrDl", "reqGbrUl", "reqMbrDl", "reqMbrUl", "maxTscBurstSize", "req5Gsdelay", "reqPer" (if the ExtQoS\_5G feature is supported), and "priority" within the "tscQosReq" attribute may be provided only if the "qosReference" attribute is not provided.  NOTE 5: The attributes "exterAppId", "flowInfo", "ethFlowInfo", "enEthFlowInfo", "qosReference", "altQoSReferences", "altQosReqs", "tscQosReq", "qosMonInfo" may be provided only if the "multiModDatFlows" attribute is not provided. | | | | |

\*\*\* Next Change \*\*\*

##### 5.14.2.1.5 Type: UserPlaneEventReport

This type represents an event report for user plane. It shall comply with the provisions defined in table 5.14.2.1.5-1.

Table 5.14.2.1.5-1: Definition of the UserPlaneEventReport data type

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | Cardinality | Description | Applicability (NOTE 1) |
| event | UserPlaneEvent | 1 | Indicates the event reported by the SCEF. |  |
| accumulatedUsage | AccumulatedUsage | 0..1 | Contains the applicable information corresponding to the event. |  |
| flowIds | array(integer) | 0..N | Identifies the affected flows that were sent during event subscription. It may be omitted when the reported event applies to all the flows sent during the subscription.  (NOTE 2) |  |
| multiModFlows | array(MultiModalFlows) | 0..N | Each element of the array identifies the flow filters for the multimodal data flows that were sent during event subscription and that are affected by the reported event. It may be omitted when the reported event applies to all the multimodal data flows sent during the subscription. (NOTE 2) | XRM\_5G |
| appliedQosRef | string | 0..1 | The currently applied QoS reference (or applied individual QoS parameter set, if AltQosWithIndParams\_5G is supported). Applicable for event QOS\_NOT\_GUARANTEED or SUCCESSFUL\_RESOURCES\_ALLOCATION.  When it is omitted and the "event" attribute is QOS\_NOT\_GUARANTEED, the event report indicates that the lowest priority alternative QoS profile could not be fulfilled either. | AlternativeQoS\_5G, AltQosWithIndParams\_5G |
| altQosNotSuppInd | boolean | 0..1 | It may be set to true when the "event" attribute is QOS\_NOT\_GUARANTEED to indicate that alternative service requirements are not supported by the access network. The default value false shall apply if the attribute is not present. | AltQoSProfilesSupportReport |
| plmnId | PlmnIdNid | 0..1 | PLMN Identifier or the SNPN Identifier.  It may be present when the reported event is "PLMN\_CHG" and which is allowed to be exposured to the AF based on the local policy or local configuration. | enNB\_5G |
| qosMonReports | array(QosMonitoringReport) | 0..N | Contains the QoS Monitoring Reporting information. | QoSMonitoring\_5G |
| ratType | RatType | 0..1 | RAT type may be present if applicable, when the notified event is "ACCESS\_TYPE\_CHANGE" and which is allowed to be exposured to the AF based on the local policy or local configuration. | enNB\_5G |
| NOTE 1: Properties marked with a feature as defined in clause 5.14.4 are applicable as described in clause 5.2.7. If no features are indicated, the related property applies for all the features.  NOTE 2: The attributes "flowIds" and "multiModFlows" are mutually exclusive | | | | |

\*\*\* Next Change \*\*\*

#### 5.14.2.1.13 Type AsSessionMediaComponent

This type represents media component data for a single-modal data flow of a multimodal service. It shall comply with the provisions defined in table 5.14.2.1.13-1.

Table 5.14.2.1.13-1: Definition of type AsSessionMediaComponent

| Attribute name | Data type | Cardinality | Description | Applicability |
| --- | --- | --- | --- | --- |
| flowInfos | array(FlowInfo) | 0..N | Contains the IP data flow(s) description for a single-modal data flow. |  |
| qosReference | string | 0..1 | Identifies a pre-defined QoS information. |  |
| altSerReqs | array(string) | 0..N | Ordered list of alternative service requirements that include a set of QoS references. The lower the index of the array for a given entry, the higher the priority.(NOTE) |  |
| altSerReqsData | array(AlternativeServiceRequirementsData) | 0..N | Ordered list of alternative service requirements that include individual QoS parameter sets. The lower the index of the array for a given entry, the higher the priority. (NOTE) |  |
| disUeNotif | boolean | 0..1 | Indicates to disable QoS flow parameters signalling to the UE when the SMF is notified by the NG-RAN of changes in the fulfilled QoS situation when it is included and set to "true". The fulfilled situation is either the QoS profile or an Alternative QoS Profile. The default value "false" shall apply, if the attribute is not present and has not been supplied previously. |  |
| medCompN | integer | 1 | Identifies the media component number, and it contains the ordinal number of the media component. |  |
| medType | MediaType | 0..1 | Indicates the media type of the service. |  |
| marBwUl | BitRate | 0..1 | Maximum requested bandwidth for the Uplink. |  |
| marBwDl | BitRate | 0..1 | Maximum requested bandwidth for the Downlink. |  |
| mirBwUl | BitRate | 0..1 | Minimum requested bandwidth for the Uplink. |  |
| mirBwDl | BitRate | 0..1 | Minimum requested bandwidth for the Downlink. |  |
| tsnQos | TsnQoSContainer | 0..1 | Transports QoS parameters for TSC traffic. |  |
| tscaiInputUl | TscaiInputContainer | 0..1 | Transports TSCAI input parameters for TSC traffic at the ingress interface of the DS-TT/UE (uplink flow direction). |  |
| tscaiInputDl | TscaiInputContainer | 0..1 | Transports TSCAI input parameters for TSC traffic at the ingress of the NW-TT (downlink flow direction). |  |
| rTLatencyReq | boolean | 0..1 | Contains the Round-Trip (RT) latency requirement of the service data flow. |  |
| pduSetQos | PduSetQosPara | 0..1 | PDU Set QoS parameters for XRM traffic. |  |

Editor’s Note: the list of IEs of a AsSessionMediaComponent to complete the QoS parameters developed for the MediaComponent data defined in TS 29.514 and applicable to external AFs is FFS.

\*\*\* Next Change \*\*\*

#### 5.14.2.1.14 Type AsSessionMediaComponentRm

This type represents the AsSessionMediaComponent with the "nullable: true" property. It shall comply with the provisions defined in table 5.14.2.1.14-1

Table 5.14.2.1.14-1: Definition of type AsSessionMediaComponentRm

| Attribute name | Data type | Cardinality | Description | Applicability |
| --- | --- | --- | --- | --- |
| flowInfos | array(FlowInfo) | 0..N | Contains the IP data flow(s) description for a single-modal data flow. |  |
| qosReference | string | 0..1 | Identifies a pre-defined QoS information. |  |
| altSerReqs | array(string) | 0..N | Ordered list of alternative service requirements that include a set of QoS references. The lower the index of the array for a given entry, the higher the priority.(NOTE) |  |
| altSerReqsData | array(AlternativeServiceRequirementsData) | 0..N | Ordered list of alternative service requirements that include individual QoS parameter sets. The lower the index of the array for a given entry, the higher the priority. (NOTE) |  |
| disUeNotif | boolean | 0..1 | Indicates to disable QoS flow parameters signalling to the UE when the SMF is notified by the NG-RAN of changes in the fulfilled QoS situation when it is included and set to "true". The fulfilled situation is either the QoS profile or an Alternative QoS Profile. The default value "false" shall apply, if the attribute is not present and has not been supplied previously. |  |
| medCompN | integer | 1 | Identifies the media component number, and it contains the ordinal number of the media component. |  |
| medType | MediaType | 0..1 | Indicates the media type of the service. |  |
| marBwUl | BitRateRm | 0..1 | Maximum requested bandwidth for the Uplink. |  |
| marBwDl | BitRateRm | 0..1 | Maximum requested bandwidth for the Downlink. |  |
| mirBwUl | BitRateRm | 0..1 | Minimum requested bandwidth for the Uplink. |  |
| mirBwDl | BitRateRm | 0..1 | Minimum requested bandwidth for the Downlink. |  |
| tsnQos | TsnQoSContainerRm | 0..1 | Transports QoS parameters for TSC traffic. |  |
| tscaiInputUl | TscaiInputContainer | 0..1 | Transports TSCAI input parameters for TSC traffic at the ingress interface of the DS-TT/UE (uplink flow direction). |  |
| tscaiInputDl | TscaiInputContainer | 0..1 | Transports TSCAI input parameters for TSC traffic at the ingress of the NW-TT (downlink flow direction). |  |
| rTLatencyReq | boolean | 0..1 | Contains the Round-Trip (RT) latency requirement of the service data flow. |  |
| pduSetQos | PduSetQosPara | 0..1 | PDU Set QoS parameters for XRM traffic. |  |

\*\*\* Next Change \*\*\*

##### 5.14.2.1.15 Type: MultiModalFlows

This type represents a flow information within a single-modal data flow. It shall comply with the provisions defined in table 5.14.2.1.15-1.

Table 5.14.2.1.15-1: Definition of the type MultiModalFlows

|  |  |  |  |
| --- | --- | --- | --- |
| Attribute name | Data type | Cardinality | Description |
| medCompN | integer | 1 | It contains the ordinal number of the single-modal data flow. Identifies the single-modal data flow |
| flowIds | array(integer) | 0..N | Identifies the affected flows within the single-modal data flow (identified by the medCompN attribute). It may be omitted when all flows are affected. |

\*\*\* Next Change \*\*\*

# A.14 AsSessionWithQoS API

openapi: 3.0.0

info:

title: 3gpp-as-session-with-qos

version: 1.3.0-alpha.1

description: |

API for setting us an AS session with required QoS.

© 2023, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.122 V18.1.0 T8 reference point for Northbound APIs

url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.122/'

security:

- {}

- oAuth2ClientCredentials: []

servers:

- url: '{apiRoot}/3gpp-as-session-with-qos/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 5.2.4 of 3GPP TS 29.122.

paths:

/{scsAsId}/subscriptions:

get:

summary: Read all or queried active subscriptions for the SCS/AS.

operationId: FetchAllASSessionWithQoSSubscriptions

tags:

- AS Session with Required QoS Subscriptions

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

- name: ip-addrs

in: query

description: The IP address(es) of the requested UE(s).

required: false

content:

application/json:

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/IpAddr'

minItems: 1

- name: ip-domain

in: query

description: >

The IPv4 address domain identifier. The attribute may only be provided if IPv4 address

is included in the ip-addrs query parameter.

required: false

schema:

type: string

- name: mac-addrs

in: query

description: The MAC address(es) of the requested UE(s).

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

minItems: 1

responses:

'200':

description: OK.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/AsSessionWithQoSSubscription'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

post:

summary: Creates a new subscription resource.

operationId: CreateASSessionWithQoSSubscription

tags:

- AS Session with Required QoS Subscriptions

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

requestBody:

description: Request to create a new subscription resource

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/AsSessionWithQoSSubscription'

callbacks:

notificationDestination:

'{request.body#/notificationDestination}':

post:

requestBody: # contents of the callback message

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/UserPlaneNotificationData'

responses:

'204':

description: No Content (successful notification)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

responses:

'201':

description: Created (Successful creation of subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/AsSessionWithQoSSubscription'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

description: Forbidden

content:

application/problem+json:

schema:

$ref: '#/components/schemas/ProblemDetailsAsSessionWithQos'

headers:

Retry-After:

description: >

Indicates the time the AF has to wait before making a new request. It can be a

non-negative integer (decimal number) indicating the number of seconds the AF

has to wait before making a new request or an HTTP-date after which the AF can

retry a new request.

schema:

type: string

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{scsAsId}/subscriptions/{subscriptionId}:

get:

summary: Read an active subscriptions for the SCS/AS and the subscription Id.

operationId: FetchIndASSessionWithQoSSubscription

tags:

- Individual AS Session with Required QoS Subscription

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

responses:

'200':

description: OK (Successful get the active subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/AsSessionWithQoSSubscription'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

put:

summary: Updates/replaces an existing subscription resource.

operationId: UpdateIndASSessionWithQoSSubscription

tags:

- Individual AS Session with Required QoS Subscription

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

requestBody:

description: Parameters to update/replace the existing subscription

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/AsSessionWithQoSSubscription'

responses:

'200':

description: OK (Successful update of the subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/AsSessionWithQoSSubscription'

'204':

description: No Content (Successful update of the subscription)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

description: Forbidden

content:

application/problem+json:

schema:

$ref: '#/components/schemas/ProblemDetailsAsSessionWithQos'

headers:

Retry-After:

description: >

Indicates the time the AF has to wait before making a new request. It can be a

non-negative integer (decimal number) indicating the number of seconds the AF

has to wait before making a new request or an HTTP-date after which the AF can

retry a new request.

schema:

type: string

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

patch:

summary: Updates/replaces an existing subscription resource.

operationId: ModifyIndASSessionWithQoSSubscription

tags:

- Individual AS Session with Required QoS Subscription

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

requestBody:

required: true

content:

application/merge-patch+json:

schema:

$ref: '#/components/schemas/AsSessionWithQoSSubscriptionPatch'

responses:

'200':

description: OK. The subscription was modified successfully.

content:

application/json:

schema:

$ref: '#/components/schemas/AsSessionWithQoSSubscription'

'204':

description: No Content. The subscription was modified successfully.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

description: Forbidden

content:

application/problem+json:

schema:

$ref: '#/components/schemas/ProblemDetailsAsSessionWithQos'

headers:

Retry-After:

description: >

Indicates the time the AF has to wait before making a new request. It can be a

non-negative integer (decimal number) indicating the number of seconds the AF

has to wait before making a new request or an HTTP-date after which the AF can

retry a new request.

schema:

type: string

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

summary: Deletes an already existing subscription.

operationId: DeleteIndASSessionWithQoSSubscription

tags:

- Individual AS Session with Required QoS Subscription

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

responses:

'204':

description: No Content (Successful deletion of the existing subscription)

'200':

description: OK (Successful deletion of the existing subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/UserPlaneNotificationData'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{tokenUrl}'

scopes: {}

schemas:

AsSessionWithQoSSubscription:

description: Represents an individual AS session with required QoS subscription resource.

type: object

properties:

self:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

notificationDestination:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

exterAppId:

type: string

description: Identifies the external Application Identifier.

flowInfo:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/FlowInfo'

minItems: 1

description: Describe the data flow which requires QoS.

ethFlowInfo:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EthFlowDescription'

minItems: 1

description: Identifies Ethernet packet flows.

enEthFlowInfo:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/EthFlowInfo'

minItems: 1

description: >

Identifies the Ethernet flows which require QoS. Each Ethernet flow consists of a flow

idenifer and the corresponding UL and/or DL flows.

multiModalId:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/MultiModalId'

qosReference:

type: string

description: Identifies a pre-defined QoS information

altQoSReferences:

type: array

items:

type: string

minItems: 1

description: >

Identifies an ordered list of pre-defined QoS information. The lower the index of the

array for a given entry, the higher the priority.

altQosReqs:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/AlternativeServiceRequirementsData'

minItems: 1

description: >

Identifies an ordered list of alternative service requirements that include individual

QoS parameter sets. The lower the index of the array for a given entry, the higher the

priority.

disUeNotif:

description: >

Indicates whether the QoS flow parameters signalling to the UE when the SMF is notified

by the NG-RAN of changes in the fulfilled QoS situation is disabled (true) or

not (false). Default value is false. The fulfilled situation is either the QoS profile

or an Alternative QoS Profile.

type: boolean

ueIpv4Addr:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv4Addr'

ipDomain:

type: string

ueIpv6Addr:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv6Addr'

macAddr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

usageThreshold:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/UsageThreshold'

sponsorInfo:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/SponsorInformation'

qosMonInfo:

$ref: '#/components/schemas/QosMonitoringInformation'

directNotifInd:

type: boolean

description: >

Indicates whether the direct event notification is requested (true) or not (false).

Default value is false.

tscQosReq:

$ref: '#/components/schemas/TscQosRequirement'

requestTestNotification:

type: boolean

description: >

Set to true by the SCS/AS to request the SCEF to send a test notification as defined

in clause 5.2.5.3. Set to false or omitted otherwise.

websockNotifConfig:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/WebsockNotifConfig'

events:

description: >

Represents the list of user plane event(s) to which the SCS/AS requests to subscribe to.

type: array

items:

$ref: '#/components/schemas/UserPlaneEvent'

minItems: 1

multiModDatFlows:

type: object

additionalProperties:

$ref: '#/components/schemas/AsSessionMediaComponent'

minProperties: 1

description: >

Contains media component data for a single-modal data flow(s).

The key of the map is the medCompN attribute.

required:

- notificationDestination

AsSessionWithQoSSubscriptionPatch:

description: Represents parameters to modify an AS session with specific QoS subscription.

type: object

properties:

exterAppId:

type: string

description: Identifies the external Application Identifier.

flowInfo:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/FlowInfo'

minItems: 1

description: Describe the IP data flow which requires QoS.

ethFlowInfo:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EthFlowDescription'

minItems: 1

description: Identifies Ethernet packet flows.

enEthFlowInfo:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/EthFlowInfo'

minItems: 1

description: >

Identifies the Ethernet flows which require QoS. Each Ethernet flow consists of a flow

idenifer and the corresponding UL and/or DL flows.

multiModalId:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/MultiModalId'

qosReference:

type: string

description: Pre-defined QoS reference

altQoSReferences:

type: array

items:

type: string

minItems: 1

description: >

Identifies an ordered list of pre-defined QoS information. The lower the index of the

array for a given entry, the higher the priority.

altQosReqs:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/AlternativeServiceRequirementsData'

minItems: 1

description: >

Identifies an ordered list of alternative service requirements that include individual

QoS parameter sets. The lower the index of the array for a given entry, the higher the

priority.

disUeNotif:

type: boolean

description: >

Indicates whether the QoS flow parameters signalling to the UE when the SMF is notified

by the NG-RAN of changes in the fulfilled QoS situation is disabled (true) or

not (false). The fulfilled situation is either the QoS profile or an Alternative QoS

Profile.

usageThreshold:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/UsageThresholdRm'

qosMonInfo:

$ref: '#/components/schemas/QosMonitoringInformationRm'

directNotifInd:

type: boolean

description: >

Indicates whether the direct event notification is requested (true) or not (false).

notificationDestination:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

tscQosReq:

$ref: '#/components/schemas/TscQosRequirementRm'

events:

description: >

Represents the updated list of user plane event(s) to which the SCS/AS requests to

subscribe to.

type: array

items:

$ref: '#/components/schemas/UserPlaneEvent'

minItems: 1

multiModDatFlows:

type: object

additionalProperties:

$ref: '#/components/schemas/AsSessionMediaComponentRm'

minProperties: 1

description: >

Contains media component data for a single-modal data flow(s).

The key of the map is the medCompN attribute.

QosMonitoringInformation:

description: Represents QoS monitoring information.

type: object

properties:

reqQosMonParams:

type: array

items:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/RequestedQosMonitoringParameter'

minItems: 1

repFreqs:

type: array

items:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/ReportingFrequency'

minItems: 1

repThreshDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

repThreshUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

repThreshRp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

waitTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

repPeriod:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

required:

- reqQosMonParams

- repFreqs

QosMonitoringInformationRm:

description: >

Represents the same as the QosMonitoringInformation data type but with

the nullable:true property.

type: object

properties:

reqQosMonParams:

type: array

items:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/RequestedQosMonitoringParameter'

minItems: 1

repFreqs:

type: array

items:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/ReportingFrequency'

minItems: 1

repThreshDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UintegerRm'

repThreshUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UintegerRm'

repThreshRp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UintegerRm'

waitTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSecRm'

repPeriod:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSecRm'

QosMonitoringReport:

description: Represents a QoS monitoring report.

type: object

properties:

ulDelays:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

minItems: 1

dlDelays:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

minItems: 1

rtDelays:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

minItems: 1

pdmf:

type: boolean

description: Represents the packet delay measurement failure indicator.

UserPlaneNotificationData:

description: Represents the parameters to be conveyed in a user plane event(s) notification.

type: object

properties:

transaction:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

eventReports:

type: array

items:

$ref: '#/components/schemas/UserPlaneEventReport'

minItems: 1

description: Contains the reported event and applicable information

required:

- transaction

- eventReports

UserPlaneEventReport:

description: Represents an event report for user plane.

type: object

properties:

event:

$ref: '#/components/schemas/UserPlaneEvent'

accumulatedUsage:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/AccumulatedUsage'

flowIds:

type: array

items:

type: integer

minItems: 1

description: >

Identifies the affected flows that were sent during event subscription. It might be

omitted when the reported event applies to all the flows sent during the subscription.

multiModFlows:

type: array

items:

$ref: '#/components/schemas/MultiModalFlows'

minItems: 1

description: >

Identifies the the flow filters for the single-modal data flows thatwere sent

during event subscription.

It may be omitted when the reported event applies to all the

single-modal data flows sent during the subscription.

appliedQosRef:

type: string

description: >

The currently applied QoS reference. Applicable for event QOS\_NOT\_GUARANTEED or

SUCCESSFUL\_RESOURCES\_ALLOCATION.

altQosNotSuppInd:

type: boolean

description: >

When present and set to true it indicates that the Alternative QoS profiles are not

supported by the access network. Applicable for event QOS\_NOT\_GUARANTEED.

plmnId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnIdNid'

qosMonReports:

type: array

items:

$ref: '#/components/schemas/QosMonitoringReport'

minItems: 1

description: Contains the QoS Monitoring Reporting information

ratType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

required:

- event

TscQosRequirement:

description: Represents QoS requirements for time sensitive communication.

type: object

properties:

reqGbrDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

reqGbrUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

reqMbrDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

reqMbrUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

maxTscBurstSize:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ExtMaxDataBurstVol'

req5Gsdelay:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketDelBudget'

reqPer:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketErrRate'

priority:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TscPriorityLevel'

tscaiTimeDom:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

tscaiInputDl:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TscaiInputContainer'

tscaiInputUl:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TscaiInputContainer'

capBatAdaptation:

type: boolean

description: >

Indicates the capability for AF to adjust the burst sending time, when it is supported

and set to "true". The default value is "false" if omitted.

TscQosRequirementRm:

description: >

Represents the same as the TscQosRequirement data type but with the nullable:true property.

type: object

properties:

reqGbrDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

reqGbrUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

reqMbrDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

reqMbrUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

maxTscBurstSize:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ExtMaxDataBurstVolRm'

req5Gsdelay:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketDelBudgetRm'

reqPer:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketErrRateRm'

priority:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TscPriorityLevelRm'

tscaiTimeDom:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UintegerRm'

tscaiInputDl:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TscaiInputContainer'

tscaiInputUl:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TscaiInputContainer'

capBatAdaptation:

type: boolean

description: >

Indicates the capability for AF to adjust the burst sending time, when it is supported

and set to "true". The default value is "false" if omitted.

nullable: true

AdditionInfoAsSessionWithQos:

description: Describes additional error information specific for this API.

type: object

properties:

acceptableServInfo:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/AcceptableServiceInfo'

ProblemDetailsAsSessionWithQos:

description: Extends ProblemDetails to also include the acceptable service info.

allOf:

- $ref: 'TS29122\_CommonData.yaml#/components/schemas/ProblemDetails'

- $ref: '#/components/schemas/AdditionInfoAsSessionWithQos'

AsSessionMediaComponent:

description: >

Representmedia component data for a single-modal data flow of

a multimodal service.

type: object

required:

- medCompN

allOf:

- not:

required: [altSerReqs,altSerReqsData]

- not:

required: [qosReference,altSerReqsData]

properties:

flowInfos:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/FlowInfo'

minItems: 1

nullable: true

description: >

Contains the IP data flow(s) description for a single-modal data flow.

qosReference:

type: string

disUeNotif:

type: boolean

altSerReqs:

type: array

items:

type: string

minItems: 1

altSerReqsData:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/AlternativeServiceRequirementsData'

minItems: 1

description: >

Contains alternative service requirements that include individual QoS parameter sets.

marBwDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

marBwUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

medCompN:

type: integer

medType:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/MediaType'

mirBwDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

mirBwUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

tsnQos:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TsnQosContainer'

tscaiInputDl:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TscaiInputContainer'

tscaiInputUl:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TscaiInputContainer'

tscaiTimeDom:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

rTLatencyReq:

type: boolean

description: Round-Trip latency requirement of the service data flow.

pduSetQos:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSetQosPara'

AsSessionMediaComponentRm:

description: >

Represents the AsSessionMediaComponent data type with nullable information.

type: object

required:

- medCompN

not:

required: [altSerReqs,altSerReqsData]

properties:

flowInfos:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/FlowInfo'

minItems: 1

nullable: true

description: >

Contains the IP data flow(s) description for a single-modal data flow.

qosReference:

type: string

nullable: true

altSerReqs:

type: array

items:

type: string

minItems: 1

nullable: true

altSerReqsData:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/AlternativeServiceRequirementsData'

minItems: 1

description: >

Contains removable alternative service requirements that include individual QoS

parameter sets.

nullable: true

disUeNotif:

type: boolean

nullable: true

marBwDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

marBwUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

medCompN:

type: integer

medType:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/MediaType'

mirBwDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

mirBwUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

tsnQos:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TsnQosContainerRm'

tscaiInputDl:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TscaiInputContainer'

tscaiInputUl:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TscaiInputContainer'

rTLatencyReq:

type: boolean

description: Round-Trip latency requirement of the service data flow.

pduSetQos:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSetQosPara'

nullable: true

MultiModalFlows:

description: Represents a flow information within a single-modal data flow.

type: object

properties:

medCompN:

type: integer

description: >

It contains the ordinal number of the single-modal data flow. Identifies the

single-modal data flow.

flowIds:

type: array

items:

type: integer

minItems: 1

description: >

Identifies the affected flow(s) within the single-modal data flow

(identified by the medCompN attribute).

It may be omitted when all flows are affected.

required:

- medCompN

UserPlaneEvent:

anyOf:

- type: string

enum:

- SESSION\_TERMINATION

- LOSS\_OF\_BEARER

- RECOVERY\_OF\_BEARER

- RELEASE\_OF\_BEARER

- USAGE\_REPORT

- FAILED\_RESOURCES\_ALLOCATION

- QOS\_GUARANTEED

- QOS\_NOT\_GUARANTEED

- QOS\_MONITORING

- SUCCESSFUL\_RESOURCES\_ALLOCATION

- ACCESS\_TYPE\_CHANGE

- PLMN\_CHG

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: |

Represents the user plane event.

Possible values are:

- SESSION\_TERMINATION: Indicates that Rx session is terminated.

- LOSS\_OF\_BEARER : Indicates a loss of a bearer.

- RECOVERY\_OF\_BEARER: Indicates a recovery of a bearer.

- RELEASE\_OF\_BEARER: Indicates a release of a bearer.

- USAGE\_REPORT: Indicates the usage report event.

- FAILED\_RESOURCES\_ALLOCATION: Indicates the resource allocation is failed.

- QOS\_GUARANTEED: The QoS targets of one or more SDFs are guaranteed again.

- QOS\_NOT\_GUARANTEED: The QoS targets of one or more SDFs are not being guaranteed.

- QOS\_MONITORING: Indicates a QoS monitoring event.

- SUCCESSFUL\_RESOURCES\_ALLOCATION: Indicates the resource allocation is successful.

- ACCESS\_TYPE\_CHANGE: Indicates an Access type change.

- PLMN\_CHG: Indicates a PLMN change.

\* \* \* \* End of changes \* \* \* \*