**3GPP** **TSG CT WG3 Meeting 128 TDoc C3-232214**

**Bratislava, Slovakia, 22nd - 26th May, 2023**

**Title: LS on Issues on SMF event exposure and muting enhancements**

**Release: Rel-18**

**Work Item: eNA\_Ph3, AIMLsys**

**Source: CT3**

**To: SA2**

**Cc:**

**Contact person: Xuefei Zhang**

**summer.xuefei@huawei.com**

**Send any reply LS to: 3GPP Liaisons Coordinator,** [**mailto:3GPPLiaison@etsi.org**](mailto:3GPPLiaison@etsi.org)

**Attachments:** **N/A**

# Overall description

CT3 has the following question on collecting the data from SMF defined in table 6.9.2-2 and Table 6.18.2-2 of TS 23.288 via Nsmf\_EventExposure service.

**Question 1:** Which event ID of SMF will be used to collect the 5QI?

CT3 has the following question on the Muting Exception Instructions described in clause 4.15.1 of 23.502:

*Muting Exception Instructions specify actions to be taken by the Event provider NF if the Deactivation notification flag is set and an exception occurs at the Event Producer NF (e.g. the Event provider can no longer buffer notifications because storage space is no longer available). The actions are specified in clause 6.2.7 of TS 23.288 [50].*

CT3 has observed that there are APIs that are required to support the Event Reporting Information of 23.502 clause 4.15.1 (including the muting instructions), which are currently not specified to be used by the NWDAF for data collection.

**Question 2:** Do the Muting Exception Instructions (and the actions specified in clause 6.2.7 of TS 23.288) apply to such APIs (i.e. APIs that are currently not specified to be used by the NWDAF for data collection) or not?

# Actions

**To SA2:**

**ACTION:** CT3 kindly asks SA2 to answer above questions and amend the SA2 specifications accordingly.

# 3 Dates of next TSG CT WG 3 meetings

3GPP TSG CT3#129 21st – 25th August 2023 Goteborg, SE