**3GPP TSG-CT WG3 Meeting #130C3-234053**

**Xiamen, China, 9 - 13 October, 2023 (revision of C3-233abc)**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **29.520** | **CR** | **0780** | **rev** |  | **Current version:** | **18.3.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Support of End-to-end data volume transfer time for list of UEs |
|  |  |
| ***Source to WG:*** | Huawei, Samsung, Ericsson |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | AIMLsys |  | ***Date:*** | 2023-09-20 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | According to clause 6.18.1 of TS 23.288, the UEs might be classified into three classes (high-transfer time, medium-transfer time and low-transfer time) according to the threshold of the corresponding class, i.e. the consumer may provide the thresholds for each class respectively.The millisecond unit shasll be used for the data transmission time. |
|  |  |
| ***Summary of change:*** | Update E2eDataVolTransTimeReq data type to support the consumer providing the thresholds for each class respectively. |
|  |  |
| ***Consequences if not approved:*** | Open issue in the specification. |
|  |  |
| ***Clauses affected:*** | 3.2, 5.1.6.2.82, 5.1.6.2.87, 5.1.6.2.90, A.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ... |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR introduces backward compatible features to the OpenAPI of the Nnwdaf\_EventsSubscription API. |
|  |  |
| ***This CR's revision history:*** |  |

**Additional discussion(if needed):**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

## 3.2 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

5QI 5G QoS Identifier

ADRF Analytics Data Repository Function

AF Application Function

AI/ML Artificial Intelligence/Machine Learning

AMF Access and Mobility Management Function

AOI Area of Interest

API Application Programming Interface

CEF Charging Enablement Function

DCCF Data Collection Coordination Function

DNN Data Network Name

FL Federated Learning

GFBR Guaranteed Flow Bit Rate

GMLC Gateway Mobile Location Centre

HTTP Hypertext Transfer Protocol

JSON JavaScript Object Notation

LADN Local Area Data Network

LMF Location Management Function

MFAF Messaging Framework Adaptor Function

ML Machine Learning

MTLF Model Training Logical Function

NEF Network Exposure Function

NF Network Function

NLOS Non Line Of Sight

NRF Network Repository Function

NSSF Network Slice Selection Function

NWDAF Network Data Analytics Function

OAM Operation, Administration, and Maintenance

PCF Policy Control Function

PFD Packet Flow Description

PFDF Packet Flow Description Function

S-NSSAI Single Network Slice Selection Assistance Information

SMCC Session Management Congestion Control

SMCCE Session Management Congestion Control Experience

SMF Session Management Function

SSC Session and Service Continuity

SUPI Subscription Permanent Identifier

UDM Unified Data Management

UPF User Plane Function

URI Uniform Resource Identifier

URSP UE Route Selection Policy

UTC Universal Time Coordinated

\*\*\* Next Change \*\*\*

##### 5.1.6.2.82 Type E2eDataVolTransTimeReq

Table 5.1.6.2.82-1: Definition of type E2eDataVolTransTimeReq

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| criterion | E2eDataVolTransTimeCriterion | O | 0..1 | Indicates the ordering criterion for the list of E2E data volume transfer time. |  |
| order | MatchingDirection | O | 0..1 | Indicate the order: ascending or descending. May be present when the "criterion" attribute is included.(NOTE 1) |  |
|  |  |  |  |  |  |
| highTransTmThld | Uinteger | O | 0..1 | Indicates the threshold of high-transfer time in unit of millisecond. The reached or greater value is ranking as high-transfer time.(NOTE 2) |  |
|  |  |  |  |  |  |
| lowTransTmThld | Uinteger | O | 0..1 | Indicates the threshold of low-transfer time in unit of millisecond. The reached or smaller value is ranking as low-transfer time.(NOTE 2) |  |
| repeatDataTrans | Uinteger | C | 0..1 | Target number of repeating data transmissions within the Analytics target period.(NOTE 3) |  |
| tsIntervalDataTrans | DateTime | C | 0..1 | Target time interval between data transmissions within the Analytics target period.(NOTE 3) |  |
| dataVolume | DataVolume | O | 0..1 | Data Volume UL/DL: indicates a specific data volume transmitted once from UE to AF and/or from AF to UE when subscribed event is "E2E\_DATA\_VOL\_TRANS\_TIME". |  |
| maxNumberUes | Uinteger | O | 0..1 | maximum number of UEs |  |
| NOTE 1: "CROSSED" value in data type "MatchingDirection" is not applicable for the "order" attribute.NOTE 2: The value of "highTransTmThld" shall be not less than the value of "lowTransTmThld". If the value of "highTransTmThld" is greater than the value of "lowTransTmThld", then the value between "highTransTmThld" and "lowTransTmThld" is ranking as medium transfer time. If the value of "highTransTmThld" is equal to the value of "lowTransTmThld", then no medium-transfer time ranking. This property shall only be provided if the "notifMethod" in "evtReq" is set to "ON\_EVENT\_DETECTION" or "notificationMethod" in "eventSubscriptions" is set to "THRESHOLD" or omitted.NOTE 3: Only one of "repeatDataTrans" or "tsIntervalDataTrans" attribute may be present. |

\*\*\* Next Change \*\*\*

##### 5.2.6.2.87 Type E2eDataVolTransTimeUeList

Table 5.2.6.2.87-1: Definition of type E2eDataVolTransTimeUeList

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| highLevel | array(Supi) | C | 1..N | A list of UEs whose transfer time has reached or greater than the threshold of high level. This attribute may be present if the event subscription includes threshold for high level.(NOTE) |  |
| mediumLevel | array(Supi) | C | 1..N | A list of UEs whose transfer time is within the threshold range of medium level. This attribute may be present if If the value of "highTransTmThld" is greater than the value of "lowTransTmThld".(NOTE) |  |
| lowLevel | array(Supi) | C | 1..N | A list of UEs whose transfer time has reached or lower than the threshold of low level. This attribute may be present if the event subscription includes threshold for low level.(NOTE) |  |
| highRatio | SamplingRatio | C | 0..1 | This attribute contains ratio of UEs per E2E data volume transfer time for high level class.Shall be present if the analytics result applies for a group of UEs. |  |
| mediumRatio | SamplingRatio | C | 0..1 | This attribute contains ratio of UEs per E2E data volume transfer time for medium level class.Shall be present if the analytics result applies for a group of UEs. |  |
| lowRatio | SamplingRatio | C | 0..1 | This attribute contains ratio of UEs per E2E data volume transfer for low level time class.Shall be present if the analytics result applies for a group of UEs. |  |
| spatialValidity | NetworkAreaInfo | C | 0..1 | Represents the area where the Classified E2E data volume transfer times for a list of UEs analytics applies. Shall be present if "networkArea" attribute was provided in the request or subscription. |  |
| validityPeriod | TimeWindow | O | 0..1 | Represents the validity period for the Classified E2E data volume transfer times for a list of UEs statistics. |  |
| NOTE: At least one of "highLevel", "mediumLevel" or "lowLevel" shall be provided. |

\*\*\* Next Change \*\*\*

##### 5.1.6.2.90 Type DataVolumeTransferTime

Table 5.1.6.2.90-1: Definition of type DataVolumeTransferTime

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| uplinkVolume | Volume | O | 0..1 | Uplink traffic volume in unit of octet. |  |
| avgTransTimeUl | Uinteger | O | 0..1 | The average time of E2E uplink data volume transfer in unit of millisecond. |  |
| varTransTimeUl | Float | O | 0..1 | The E2E uplink data volume transfer time variance. |  |
| downlinkVolume | Volume | O | 0..1 | Downlink traffic volume in unit of octet. |  |
| avgTransTimeDl | Uinteger | O | 0..1 | The average time of E2E downlink data volume transfer in unit of millisecond. |  |
| varTransTimeDl | Float | O | 0..1 | The E2E downlink data volume transfer time variance. |  |

\*\*\* Next Change \*\*\*

# A.2 Nnwdaf\_EventsSubscription API

openapi: 3.0.0

info:

 version: 1.3.0-alpha.4

 title: Nnwdaf\_EventsSubscription

 description: |

 Nnwdaf\_EventsSubscription Service API.

 © 2023, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: 3GPP TS 29.520 V18.3.0; 5G System; Network Data Analytics Services.

 url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.520/'

security:

 - {}

 - oAuth2ClientCredentials:

 - nnwdaf-eventssubscription

servers:

 - url: '{apiRoot}/nnwdaf-eventssubscription/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in clause 4.4 of 3GPP TS 29.501.

paths:

 /subscriptions:

 post:

 summary: Create a new Individual NWDAF Events Subscription

 operationId: CreateNWDAFEventsSubscription

 tags:

 - NWDAF Events Subscriptions (Collection)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NnwdafEventsSubscription'

 responses:

 '201':

 description: Create a new Individual NWDAF Event Subscription resource.

 headers:

 Location:

 description: >

 Contains the URI of the newly created resource, according to the structure

 {apiRoot}/nnwdaf-eventssubscription/<apiVersion>/subscriptions/{subscriptionId}

 required: true

 schema:

 type: string

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NnwdafEventsSubscription'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '502':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/502'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 callbacks:

 myNotification:

 '{$request.body#/notificationURI}':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 type: array

 items:

 $ref: '#/components/schemas/NnwdafEventsSubscriptionNotification'

 minItems: 1

 responses:

 '204':

 description: The receipt of the Notification is acknowledged.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '502':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/502'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /subscriptions/{subscriptionId}:

 delete:

 summary: Delete an existing Individual NWDAF Events Subscription

 operationId: DeleteNWDAFEventsSubscription

 tags:

 - Individual NWDAF Events Subscription (Document)

 parameters:

 - name: subscriptionId

 in: path

 description: String identifying a subscription to the Nnwdaf\_EventsSubscription Service

 required: true

 schema:

 type: string

 responses:

 '204':

 description: >

 No Content. The Individual NWDAF Event Subscription resource matching the subscriptionId

 was deleted.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '501':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/501'

 '502':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/502'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 put:

 summary: Update an existing Individual NWDAF Events Subscription

 operationId: UpdateNWDAFEventsSubscription

 tags:

 - Individual NWDAF Events Subscription (Document)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NnwdafEventsSubscription'

 parameters:

 - name: subscriptionId

 in: path

 description: String identifying a subscription to the Nnwdaf\_EventsSubscription Service.

 required: true

 schema:

 type: string

 responses:

 '200':

 description: >

 The Individual NWDAF Event Subscription resource was modified successfully and a

 representation of that resource is returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NnwdafEventsSubscription'

 '204':

 description: The Individual NWDAF Event Subscription resource was modified successfully.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '501':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/501'

 '502':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/502'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /transfers:

 post:

 summary: Provide information about requested analytics subscriptions transfer and potentially create a new Individual NWDAF Event Subscription Transfer resource.

 operationId: CreateNWDAFEventSubscriptionTransfer

 tags:

 - NWDAF Event Subscription Transfers (Collection)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nnwdaf-eventssubscription

 - oAuth2ClientCredentials:

 - nnwdaf-eventssubscription

 - nnwdaf-eventssubscription:transfer

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/AnalyticsSubscriptionsTransfer'

 responses:

 '201':

 description: Create a new Individual NWDAF Event Subscription Transfer resource.

 headers:

 Location:

 description: >

 Contains the URI of the newly created resource, according to the structure

 {apiRoot}/nnwdaf-eventssubscription/<apiVersion>/transfers/{transferId}

 required: true

 schema:

 type: string

 '204':

 description: >

 No Content. The receipt of the information about analytics subscription(s) that are

 requested to be transferred and the ability to handle this information (e.g. execute the

 steps required to transfer an analytics subscription directly) is confirmed.

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '502':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/502'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /transfers/{transferId}:

 delete:

 summary: Delete an existing Individual NWDAF Event Subscription Transfer

 operationId: DeleteNWDAFEventSubscriptionTransfer

 tags:

 - Individual NWDAF Event Subscription Transfer (Document)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nnwdaf-eventssubscription

 - oAuth2ClientCredentials:

 - nnwdaf-eventssubscription

 - nnwdaf-eventssubscription:transfer

 parameters:

 - name: transferId

 in: path

 description: >

 String identifying a request for an analytics subscription transfer to the

 Nnwdaf\_EventsSubscription Service.

 required: true

 schema:

 type: string

 responses:

 '204':

 description: >

 No Content. The Individual NWDAF Event Subscription Transfer resource matching the

 transferId was deleted.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '501':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/501'

 '502':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/502'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 put:

 summary: Update an existing Individual NWDAF Event Subscription Transfer

 operationId: UpdateNWDAFEventSubscriptionTransfer

 tags:

 - Individual NWDAF Event Subscription Transfer (Document)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nnwdaf-eventssubscription

 - oAuth2ClientCredentials:

 - nnwdaf-eventssubscription

 - nnwdaf-eventssubscription:transfer

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/AnalyticsSubscriptionsTransfer'

 parameters:

 - name: transferId

 in: path

 description: >

 String identifying a request for an analytics subscription transfer to the

 Nnwdaf\_EventsSubscription Service

 required: true

 schema:

 type: string

 responses:

 '204':

 description: >

 The Individual NWDAF Event Subscription Transfer resource was modified successfully.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '501':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/501'

 '502':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/502'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{nrfApiRoot}/oauth2/token'

 scopes:

 nnwdaf-eventssubscription: Access to the Nnwdaf\_EventsSubscription API

 nnwdaf-eventssubscription:transfer: >

 Access to service operations applying to NWDAF event subscription transfer.

 schemas:

 NnwdafEventsSubscription:

 description: Represents an Individual NWDAF Event Subscription resource.

 type: object

 properties:

 eventSubscriptions:

 type: array

 items:

 $ref: '#/components/schemas/EventSubscription'

 minItems: 1

 description: Subscribed events

 evtReq:

 $ref: 'TS29523\_Npcf\_EventExposure.yaml#/components/schemas/ReportingInformation'

 notificationURI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 notifCorrId:

 type: string

 description: Notification correlation identifier.

 supportedFeatures:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 eventNotifications:

 type: array

 items:

 $ref: '#/components/schemas/EventNotification'

 minItems: 1

 failEventReports:

 type: array

 items:

 $ref: '#/components/schemas/FailureEventInfo'

 minItems: 1

 prevSub:

 $ref: '#/components/schemas/PrevSubInfo'

 consNfInfo:

 $ref: '#/components/schemas/ConsumerNfInformation'

 required:

 - eventSubscriptions

 EventSubscription:

 description: Represents a subscription to a single event.

 type: object

 properties:

 anySlice:

 $ref: '#/components/schemas/AnySlice'

 appIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 minItems: 1

 description: Identification(s) of application to which the subscription applies.

 deviations:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 minItems: 1

 dnns:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 minItems: 1

 description: Identification(s) of DNN to which the subscription applies.

 dnais:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnai'

 minItems: 1

 event:

 $ref: '#/components/schemas/NwdafEvent'

 extraReportReq:

 $ref: '#/components/schemas/EventReportingRequirement'

 ladnDnns:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 minItems: 1

 description: Identification(s) of LADN DNN to indicate the LADN service area as the AOI.

 loadLevelThreshold:

 type: integer

 description: >

 Indicates that the NWDAF shall report the corresponding network slice load level to the

 NF service consumer where the load level of the network slice identified by snssais is

 reached.

 notificationMethod:

 $ref: '#/components/schemas/NotificationMethod'

 matchingDir:

 $ref: '#/components/schemas/MatchingDirection'

 nfLoadLvlThds:

 type: array

 items:

 $ref: '#/components/schemas/ThresholdLevel'

 minItems: 1

 description: >

 Shall be supplied in order to start reporting when an average load level is reached.

 nfInstanceIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 minItems: 1

 nfSetIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfSetId'

 minItems: 1

 nfTypes:

 type: array

 items:

 $ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/NFType'

 minItems: 1

 networkArea:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 location:

 $ref: '#/components/schemas/GeoLocation'

 temporalGranSize:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 spatialGranSizeTa:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 spatialGranSizeCell:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 fineGranAreas:

 type: array

 items:

 $ref: 'TS29522\_AMPolicyAuthorization.yaml#/components/schemas/GeographicalArea'

 minItems: 1

 description: Indicates the fine granularity areas to which the subscription applies.

 visitedAreas:

 type: array

 items:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 minItems: 1

 maxTopAppUlNbr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 maxTopAppDlNbr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 nsiIdInfos:

 type: array

 items:

 $ref: '#/components/schemas/NsiIdInfo'

 minItems: 1

 nsiLevelThrds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 minItems: 1

 qosRequ:

 $ref: '#/components/schemas/QosRequirement'

 qosFlowRetThds:

 type: array

 items:

 $ref: '#/components/schemas/RetainabilityThreshold'

 minItems: 1

 ranUeThrouThds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 minItems: 1

 repetitionPeriod:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 snssaia:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 minItems: 1

 description: >

 Identification(s) of network slice to which the subscription applies. It corresponds to

 snssais in the data model definition of 3GPP TS 29.520.

 tgtUe:

 $ref: '#/components/schemas/TargetUeInformation'

 congThresholds:

 type: array

 items:

 $ref: '#/components/schemas/ThresholdLevel'

 minItems: 1

 nwPerfRequs:

 type: array

 items:

 $ref: '#/components/schemas/NetworkPerfRequirement'

 minItems: 1

 ueCommReqs:

 type: array

 items:

 $ref: '#/components/schemas/UeCommReq'

 minItems: 1

 ueMobilityReqs:

 type: array

 items:

 $ref: '#/components/schemas/UeMobilityReq'

 minItems: 1

 userDataConOrderCri:

 $ref: '#/components/schemas/UserDataConOrderCrit'

 bwRequs:

 type: array

 items:

 $ref: '#/components/schemas/BwRequirement'

 minItems: 1

 excepRequs:

 type: array

 items:

 $ref: '#/components/schemas/Exception'

 minItems: 1

 exptAnaType:

 $ref: '#/components/schemas/ExpectedAnalyticsType'

 exptUeBehav:

 $ref: 'TS29503\_Nudm\_SDM.yaml#/components/schemas/ExpectedUeBehaviourData'

 ratFreqs:

 type: array

 items:

 $ref: '#/components/schemas/RatFreqInformation'

 minItems: 1

 listOfAnaSubsets:

 type: array

 items:

 $ref: '#/components/schemas/AnalyticsSubset'

 minItems: 1

 disperReqs:

 type: array

 items:

 $ref: '#/components/schemas/DispersionRequirement'

 minItems: 1

 redTransReqs:

 type: array

 items:

 $ref: '#/components/schemas/RedundantTransmissionExpReq'

 minItems: 1

 wlanReqs:

 type: array

 items:

 $ref: '#/components/schemas/WlanPerformanceReq'

 minItems: 1

 upfInfo:

 $ref: 'TS29508\_Nsmf\_EventExposure.yaml#/components/schemas/UpfInformation'

 appServerAddrs:

 type: array

 items:

 $ref: 'TS29517\_Naf\_EventExposure.yaml#/components/schemas/AddrFqdn'

 minItems: 1

 dnPerfReqs:

 type: array

 items:

 $ref: '#/components/schemas/DnPerformanceReq'

 minItems: 1

 pduSesInfos:

 type: array

 items:

 $ref: '#/components/schemas/PduSessionInfo'

 minItems: 1

 useCaseCxt:

 type: string

 description: >

 Indicates the context of usage of the analytics. The value and format of this parameter

 are not standardized.

 pduSesTrafReqs:

 type: array

 items:

 $ref: '#/components/schemas/PduSesTrafficReq'

 minItems: 1

 locAccReqs:

 type: array

 items:

 $ref: '#/components/schemas/LocAccuracyReq'

 minItems: 1

 locGranularity:

 $ref: '#/components/schemas/LocInfoGranularity'

 locOrientation:

 $ref: '#/components/schemas/LocationOrientation'

 dataVlTrnsTmRqs:

 type: array

 items:

 $ref: '#/components/schemas/E2eDataVolTransTimeReq'

 minItems: 1

 accuReq:

 $ref: '#/components/schemas/AccuracyReq'

 pauseFlg:

 type: boolean

 description: >

 Pause analytics consumption flag. Set to "true" to indicate the NWDAF to stop sending

 the notifications of analytics. Default value is "false" if omitted.

 resumeFlg:

 type: boolean

 description: >

 Resume analytics consumption flag. Set to "true" to indicate the NWDAF to resume sending

 the notifications of analytics. Default value is "false" if omitted.

 movBehavReqs:

 type: array

 items:

 $ref: '#/components/schemas/MovBehavReq'

 minItems: 1

 required:

 - event

 not:

 required: [excepRequs, exptAnaType]

 NnwdafEventsSubscriptionNotification:

 description: Represents an Individual NWDAF Event Subscription Notification resource.

 type: object

 properties:

 eventNotifications:

 type: array

 items:

 $ref: '#/components/schemas/EventNotification'

 minItems: 1

 description: Notifications about Individual Events

 subscriptionId:

 type: string

 description: String identifying a subscription to the Nnwdaf\_EventsSubscription Service

 notifCorrId:

 type: string

 description: Notification correlation identifier.

 oldSubscriptionId:

 type: string

 description: >

 Subscription ID which was allocated by the source NWDAF. This parameter shall be present

 if the notification is for informing the assignment of a new Subscription Id by the

 target NWDAF.

 resourceUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 termCause:

 $ref: '#/components/schemas/TermCause'

 transEvents:

 type: array

 items:

 $ref: '#/components/schemas/NwdafEvent'

 minItems: 1

 required:

 - subscriptionId

 oneOf:

 - required: [eventNotifications]

 - allOf:

 - required: [resourceUri]

 - required: [oldSubscriptionId]

 EventNotification:

 description: Represents a notification on events that occurred.

 type: object

 properties:

 event:

 $ref: '#/components/schemas/NwdafEvent'

 start:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 expiry:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 timeStampGen:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 failNotifyCode:

 $ref: '#/components/schemas/NwdafFailureCode'

 rvWaitTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 anaMetaInfo:

 $ref: '#/components/schemas/AnalyticsMetadataInfo'

 nfLoadLevelInfos:

 type: array

 items:

 $ref: '#/components/schemas/NfLoadLevelInformation'

 minItems: 1

 nsiLoadLevelInfos:

 type: array

 items:

 $ref: '#/components/schemas/NsiLoadLevelInfo'

 minItems: 1

 pfdDetermInfos:

 type: array

 items:

 $ref: '#/components/schemas/PfdDeterminationInfo'

 minItems: 1

 sliceLoadLevelInfo:

 $ref: '#/components/schemas/SliceLoadLevelInformation'

 svcExps:

 type: array

 items:

 $ref: '#/components/schemas/ServiceExperienceInfo'

 minItems: 1

 qosSustainInfos:

 type: array

 items:

 $ref: '#/components/schemas/QosSustainabilityInfo'

 minItems: 1

 ueComms:

 type: array

 items:

 $ref: '#/components/schemas/UeCommunication'

 minItems: 1

 ueMobs:

 type: array

 items:

 $ref: '#/components/schemas/UeMobility'

 minItems: 1

 userDataCongInfos:

 type: array

 items:

 $ref: '#/components/schemas/UserDataCongestionInfo'

 minItems: 1

 abnorBehavrs:

 type: array

 items:

 $ref: '#/components/schemas/AbnormalBehaviour'

 minItems: 1

 nwPerfs:

 type: array

 items:

 $ref: '#/components/schemas/NetworkPerfInfo'

 minItems: 1

 dnPerfInfos:

 type: array

 items:

 $ref: '#/components/schemas/DnPerfInfo'

 minItems: 1

 disperInfos:

 type: array

 items:

 $ref: '#/components/schemas/DispersionInfo'

 minItems: 1

 redTransInfos:

 type: array

 items:

 $ref: '#/components/schemas/RedundantTransmissionExpInfo'

 minItems: 1

 wlanInfos:

 type: array

 items:

 $ref: '#/components/schemas/WlanPerformanceInfo'

 minItems: 1

 smccExps:

 type: array

 items:

 $ref: 'TS29520\_Nnwdaf\_AnalyticsInfo.yaml#/components/schemas/SmcceInfo'

 minItems: 1

 pduSesTrafInfos:

 type: array

 items:

 $ref: '#/components/schemas/PduSesTrafficInfo'

 minItems: 1

 dataVlTrnsTmInfos:

 type: array

 items:

 $ref: '#/components/schemas/E2eDataVolTransTimeInfo'

 minItems: 1

 accuInfo:

 $ref: '#/components/schemas/AccuracyInfo'

 cancelAccuInd:

 type: boolean

 description: >

 Indicates cancelled subscription of the analytics accuracy information.

 Set to "true" indicates the NWDAF cancelled subscription of analytics accuracy

 information as the NWDAF does not support the accuracy checking capability.

 Otherwise set to "false". Default value is "false" if omitted.

 pauseInd:

 type: boolean

 description: >

 Pause analytics consumption indication. Set to "true" to indicate the consumer to stop

 the consumption of the analytics. Default value is "false" if omitted.

 resumeInd:

 type: boolean

 description: >

 Resume analytics consumption indication. Set to "true" to indicate the consumer to

 resume the consumption of the analytics. Default value is "false" if omitted.

 movBehavInfos:

 type: array

 items:

 $ref: '#/components/schemas/MovBehavInfo'

 minItems: 1

 locAccInfos:

 type: array

 items:

 $ref: '#/components/schemas/LocAccuracyInfo'

 minItems: 1

 required:

 - event

 ServiceExperienceInfo:

 description: Represents service experience information.

 type: object

 properties:

 svcExprc:

 $ref: 'TS29517\_Naf\_EventExposure.yaml#/components/schemas/SvcExperience'

 svcExprcVariance:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 supis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 minItems: 1

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 appId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 srvExpcType:

 $ref: '#/components/schemas/ServiceExperienceType'

 ueLocs:

 type: array

 items:

 $ref: '#/components/schemas/LocationInfo'

 minItems: 1

 upfInfo:

 $ref: 'TS29508\_Nsmf\_EventExposure.yaml#/components/schemas/UpfInformation'

 dnai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnai'

 appServerInst:

 $ref: 'TS29517\_Naf\_EventExposure.yaml#/components/schemas/AddrFqdn'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 networkArea:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 nsiId:

 $ref: 'TS29531\_Nnssf\_NSSelection.yaml#/components/schemas/NsiId'

 ratio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 ratFreq:

 $ref: '#/components/schemas/RatFreqInformation'

 pduSesInfo:

 $ref: '#/components/schemas/PduSessionInfo'

 required:

 - svcExprc

 BwRequirement:

 description: Represents bandwidth requirements.

 type: object

 properties:

 appId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 marBwDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 marBwUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 mirBwDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 mirBwUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 required:

 - appId

 SliceLoadLevelInformation:

 description: Contains load level information applicable for one or several slices.

 type: object

 properties:

 loadLevelInformation:

 $ref: '#/components/schemas/LoadLevelInformation'

 snssais:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 minItems: 1

 description: Identification(s) of network slice to which the subscription applies.

 required:

 - loadLevelInformation

 - snssais

 NsiLoadLevelInfo:

 description: >

 Represents the network slice and optionally the associated network slice instance and the

 load level information.

 type: object

 properties:

 loadLevelInformation:

 $ref: '#/components/schemas/LoadLevelInformation'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 nsiId:

 $ref: 'TS29531\_Nnssf\_NSSelection.yaml#/components/schemas/NsiId'

 resUsage:

 $ref: '#/components/schemas/ResourceUsage'

 numOfExceedLoadLevelThr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 exceedLoadLevelThrInd:

 type: boolean

 description: >

 Indicates whether the Load Level Threshold is met or exceeded by the statistics value.

 Set to "true" if the Load Level Threshold is met or exceeded, otherwise set to "false".

 Shall be present if one of the element in the "listOfAnaSubsets" attribute was set to

 EXCEED\_LOAD\_LEVEL\_THR\_IND.

 networkArea:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 timePeriod:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

 resUsgThrCrossTimePeriod:

 type: array

 items:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

 minItems: 1

 description: >

 Each element indicates the time elapsed between times each threshold is met or exceeded

 or crossed. The start time and end time are the exact time stamps of the resource usage

 threshold is reached or exceeded. May be present if the "listOfAnaSubsets" attribute is

 provided and the maximum number of instances shall not exceed the value provided in the

 "numOfExceedLoadLevelThr" attribute.

 numOfUes:

 $ref: '#/components/schemas/NumberAverage'

 numOfPduSess:

 $ref: '#/components/schemas/NumberAverage'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 required:

 - loadLevelInformation

 - snssai

 NsiIdInfo:

 description: Represents the S-NSSAI and the optionally associated Network Slice Instance(s).

 type: object

 properties:

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 nsiIds:

 type: array

 items:

 $ref: 'TS29531\_Nnssf\_NSSelection.yaml#/components/schemas/NsiId'

 minItems: 1

 required:

 - snssai

 EventReportingRequirement:

 description: Represents the type of reporting that the subscription requires.

 type: object

 properties:

 accuracy:

 $ref: '#/components/schemas/Accuracy'

 accPerSubset:

 type: array

 items:

 $ref: '#/components/schemas/Accuracy'

 minItems: 1

 description: >

 Each element indicates the preferred accuracy level per analytics subset. It may be

 present if the "listOfAnaSubsets" attribute is present in the subscription request when

 the subscription event is NF\_LOAD, UE\_COMM, DISPERSION, NETWORK\_PERFORMANCE,

 WLAN\_PERFORMANCE, DN\_PERFORMANCE, SERVICE\_EXPERIENCE or E2E\_DATA\_VOL\_TRANS\_TIME,

 UE\_MOBILITY, PDU\_SESSION\_TRAFFIC or MOVEMENT\_BEHAVIOUR.

 startTs:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 endTs:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 offsetPeriod:

 type: integer

 description: >

 Offset period in units of seconds to the reporting time, if the value is negative means

 statistics in the past offset period, otherwise a positive value means prediction in the

 future offset period. May be present if the "repPeriod" attribute is included within the

 "evtReq" attribute or the "repetitionPeriod" attribute is included within the

 EventSubscription type.

 sampRatio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 maxObjectNbr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 maxSupiNbr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 timeAnaNeeded:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 anaMeta:

 type: array

 items:

 $ref: '#/components/schemas/AnalyticsMetadata'

 minItems: 1

 anaMetaInd:

 $ref: '#/components/schemas/AnalyticsMetadataIndication'

 histAnaTimePeriod:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

 TargetUeInformation:

 description: Identifies the target UE information.

 type: object

 properties:

 anyUe:

 type: boolean

 description: >

 Identifies any UE when setting to "true". Default value is "false" if omitted.

 supis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 minItems: 1

 gpsis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 minItems: 1

 intGroupIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 minItems: 1

 UeMobility:

 description: Represents UE mobility information.

 type: object

 properties:

 ts:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 recurringTime:

 $ref: 'TS29122\_CpProvisioning.yaml#/components/schemas/ScheduledCommunicationTime'

 duration:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 durationVariance:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 locInfos:

 type: array

 items:

 $ref: '#/components/schemas/LocationInfo'

 minItems: 1

 directionInfos:

 type: array

 items:

 $ref: '#/components/schemas/DirectionInfo'

 minItems: 1

 allOf:

 - required: [duration]

 - required: [locInfos]

 - oneOf:

 - required: [ts]

 - required: [recurringTime]

 LocationInfo:

 description: Represents UE location information.

 type: object

 properties:

 loc:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 geoLoc:

 $ref: 'TS29522\_AMPolicyAuthorization.yaml#/components/schemas/GeographicalArea'

 ratio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 geoDistrInfos:

 type: array

 items:

 $ref: '#/components/schemas/GeoDistributionInfo'

 minItems: 1

 required:

 - loc

 DirectionInfo:

 description: Represents the UE direction information.

 type: object

 properties:

 supi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 gpsi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 direction:

 type: string

 description: String identifying the moving direction of the UE.

 required:

 - direction

 oneOf:

 - required: [supi]

 - required: [gpsi]

 GeoDistributionInfo:

 description: Represents the geographical distribution of the UEs.

 type: object

 properties:

 loc:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 supis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 minItems: 1

 gpsis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 minItems: 1

 required:

 - loc

 oneOf:

 - required: [supis]

 - required: [gpsis]

 UeCommunication:

 description: Represents UE communication information.

 type: object

 properties:

 commDur:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 commDurVariance:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 perioTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 perioTimeVariance:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 ts:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 tsVariance:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 recurringTime:

 $ref: 'TS29122\_CpProvisioning.yaml#/components/schemas/ScheduledCommunicationTime'

 trafChar:

 $ref: '#/components/schemas/TrafficCharacterization'

 ratio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 perioCommInd:

 type: boolean

 description: >

 This attribute indicates whether the UE communicates periodically or not. Set to "true"

 to indicate the UE communicates periodically, otherwise set to "false" or omitted.

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 anaOfAppList:

 $ref: '#/components/schemas/AppListForUeComm'

 sessInactTimer:

 $ref: '#/components/schemas/SessInactTimerForUeComm'

 allOf:

 - required: [commDur]

 - required: [trafChar]

 - oneOf:

 - required: [ts]

 - required: [recurringTime]

 TrafficCharacterization:

 description: Identifies the detailed traffic characterization.

 type: object

 properties:

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 appId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 fDescs:

 type: array

 items:

 $ref: '#/components/schemas/IpEthFlowDescription'

 minItems: 1

 maxItems: 2

 ulVol:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

 ulVolVariance:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 dlVol:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

 dlVolVariance:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 anyOf:

 - required: [ulVol]

 - required: [dlVol]

 UserDataCongestionInfo:

 description: Represents the user data congestion information.

 type: object

 properties:

 networkArea:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 congestionInfo:

 $ref: '#/components/schemas/CongestionInfo'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 required:

 - networkArea

 - congestionInfo

 CongestionInfo:

 description: Represents the congestion information.

 type: object

 properties:

 congType:

 $ref: '#/components/schemas/CongestionType'

 timeIntev:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

 nsi:

 $ref: '#/components/schemas/ThresholdLevel'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 topAppListUl:

 type: array

 items:

 $ref: '#/components/schemas/TopApplication'

 minItems: 1

 topAppListDl:

 type: array

 items:

 $ref: '#/components/schemas/TopApplication'

 minItems: 1

 required:

 - congType

 - timeIntev

 - nsi

 TopApplication:

 description: Top application that contributes the most to the traffic.

 type: object

 properties:

 appId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 ipTrafficFilter:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/FlowInfo'

 ratio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 oneOf:

 - required: [appId]

 - required: [ipTrafficFilter]

 QosSustainabilityInfo:

 description: Represents the QoS Sustainability information.

 type: object

 properties:

 areaInfo:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 fineAreaInfos:

 type: array

 items:

 $ref: 'TS29522\_AMPolicyAuthorization.yaml#/components/schemas/GeographicalArea'

 minItems: 1

 description: >

 This attribute contains the geographical locations in a fine granularity. startTs:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 endTs:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 qosFlowRetThd:

 $ref: '#/components/schemas/RetainabilityThreshold'

 ranUeThrouThd:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 oneOf:

 - required: [qosFlowRetThd]

 - required: [ranUeThrouThd]

 QosRequirement:

 description: Represents the QoS requirements.

 type: object

 properties:

 5qi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/5Qi'

 gfbrUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 gfbrDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 resType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/QosResourceType'

 pdb:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketDelBudget'

 per:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketErrRate'

 deviceSpeed:

 $ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/VelocityEstimate'

 deviceType:

 $ref: '#/components/schemas/DeviceType'

 oneOf:

 - required: [5qi]

 - required: [resType]

 ThresholdLevel:

 description: Represents a threshold level.

 type: object

 properties:

 congLevel:

 type: integer

 nfLoadLevel:

 type: integer

 nfCpuUsage:

 type: integer

 nfMemoryUsage:

 type: integer

 nfStorageUsage:

 type: integer

 avgTrafficRate:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 maxTrafficRate:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 minTrafficRate:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 aggTrafficRate:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 varTrafficRate:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 avgPacketDelay:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketDelBudget'

 maxPacketDelay:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketDelBudget'

 varPacketDelay:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 avgPacketLossRate:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketLossRate'

 maxPacketLossRate:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketLossRate'

 varPacketLossRate:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 svcExpLevel:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 speed:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 NfLoadLevelInformation:

 description: Represents load level information of a given NF instance.

 type: object

 properties:

 nfType:

 $ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/NFType'

 nfInstanceId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 nfSetId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfSetId'

 nfStatus:

 $ref: '#/components/schemas/NfStatus'

 nfCpuUsage:

 type: integer

 nfMemoryUsage:

 type: integer

 nfStorageUsage:

 type: integer

 nfLoadLevelAverage:

 type: integer

 nfLoadLevelpeak:

 type: integer

 nfLoadAvgInAoi:

 type: integer

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 allOf:

 - required: [nfType]

 - required: [nfInstanceId]

 - anyOf:

 - required: [nfStatus]

 - required: [nfCpuUsage]

 - required: [nfMemoryUsage]

 - required: [nfStorageUsage]

 - required: [nfLoadLevelAverage]

 - required: [nfLoadLevelPeak]

 NfStatus:

 description: Contains the percentage of time spent on various NF states.

 type: object

 properties:

 statusRegistered:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 statusUnregistered:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 statusUndiscoverable:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 anyOf:

 - required: [statusRegistered]

 - required: [statusUnregistered]

 - required: [statusUndiscoverable]

 AnySlice:

 type: boolean

 description: >

 "false" represents not applicable for all slices. "true" represents applicable for all slices.

 LoadLevelInformation:

 type: integer

 description: >

 Load level information of the network slice and the optionally associated network slice

 instance.

 AbnormalBehaviour:

 description: Represents the abnormal behaviour information.

 type: object

 properties:

 supis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 minItems: 1

 excep:

 $ref: '#/components/schemas/Exception'

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 ratio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 addtMeasInfo:

 $ref: '#/components/schemas/AdditionalMeasurement'

 required:

 - excep

 Exception:

 description: Represents the Exception information.

 type: object

 properties:

 excepId:

 $ref: '#/components/schemas/ExceptionId'

 excepLevel:

 type: integer

 excepTrend:

 $ref: '#/components/schemas/ExceptionTrend'

 required:

 - excepId

 AdditionalMeasurement:

 description: Represents additional measurement information.

 type: object

 properties:

 unexpLoc:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 unexpFlowTeps:

 type: array

 items:

 $ref: '#/components/schemas/IpEthFlowDescription'

 minItems: 1

 unexpWakes:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 minItems: 1

 ddosAttack:

 $ref: '#/components/schemas/AddressList'

 wrgDest:

 $ref: '#/components/schemas/AddressList'

 circums:

 type: array

 items:

 $ref: '#/components/schemas/CircumstanceDescription'

 minItems: 1

 IpEthFlowDescription:

 description: Contains the description of an Uplink and/or Downlink Ethernet flow.

 type: object

 properties:

 ipTrafficFilter:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/FlowDescription'

 ethTrafficFilter:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EthFlowDescription'

 oneOf:

 - required: [ipTrafficFilter]

 - required: [ethTrafficFilter]

 AddressList:

 description: Represents a list of IPv4 and/or IPv6 addresses.

 type: object

 properties:

 ipv4Addrs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 minItems: 1

 ipv6Addrs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 minItems: 1

 CircumstanceDescription:

 description: Contains the description of a circumstance.

 type: object

 properties:

 freq:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 tm:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 locArea:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 vol:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

 RetainabilityThreshold:

 description: Represents a QoS flow retainability threshold.

 type: object

 properties:

 relFlowNum:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 relTimeUnit:

 $ref: '#/components/schemas/TimeUnit'

 relFlowRatio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 oneOf:

 - allOf:

 - required: [relFlowNum]

 - required: [relTimeUnit]

 - required: [relFlowRatio]

 NetworkPerfRequirement:

 description: Represents a network performance requirement.

 type: object

 properties:

 nwPerfType:

 $ref: '#/components/schemas/NetworkPerfType'

 relativeRatio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 absoluteNum:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 orderCriterion:

 $ref: '#/components/schemas/NetworkPerfOrderCriterion'

 rscUsgReq:

 $ref: '#/components/schemas/ResourceUsageRequirement'

 required:

 - nwPerfType

 not:

 required: [relativeRatio, absoluteNum]

 NetworkPerfInfo:

 description: Represents the network performance information.

 type: object

 properties:

 networkArea:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 nwPerfType:

 $ref: '#/components/schemas/NetworkPerfType'

 anaPeriod:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

 relativeRatio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 absoluteNum:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 rscUsgReq:

 $ref: '#/components/schemas/ResourceUsageRequirement'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 allOf:

 - required: [networkArea]

 - required: [nwPerfType]

 - oneOf:

 - required: [relativeRatio]

 - required: [absoluteNum]

 FailureEventInfo:

 description: Contains information on the event for which the subscription is not successful.

 type: object

 properties:

 event:

 $ref: '#/components/schemas/NwdafEvent'

 failureCode:

 $ref: '#/components/schemas/NwdafFailureCode'

 required:

 - event

 - failureCode

 AnalyticsMetadataIndication:

 description: >

 Contains analytics metadata information requested to be used during analytics generation.

 type: object

 properties:

 dataWindow:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

 dataStatProps:

 type: array

 items:

 $ref: '#/components/schemas/DatasetStatisticalProperty'

 minItems: 1

 strategy:

 $ref: '#/components/schemas/OutputStrategy'

 aggrNwdafIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 minItems: 1

 AnalyticsMetadataInfo:

 description: Contains analytics metadata information required for analytics aggregation.

 type: object

 properties:

 numSamples:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 dataWindow:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

 dataStatProps:

 type: array

 items:

 $ref: '#/components/schemas/DatasetStatisticalProperty'

 minItems: 1

 strategy:

 $ref: '#/components/schemas/OutputStrategy'

 accuracy:

 $ref: '#/components/schemas/Accuracy'

 NumberAverage:

 description: Represents average and variance information.

 type: object

 properties:

 number:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 variance:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 skewness:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 required:

 - number

 - variance

 AnalyticsSubscriptionsTransfer:

 description: Contains information about a request to transfer analytics subscriptions.

 type: object

 properties:

 subsTransInfos:

 type: array

 items:

 $ref: '#/components/schemas/SubscriptionTransferInfo'

 minItems: 1

 failTransEventReports:

 type: array

 items:

 $ref: '#/components/schemas/NwdafEvent'

 minItems: 1

 required:

 - subsTransInfos

 SubscriptionTransferInfo:

 description: Contains information about subscriptions that are requested to be transferred.

 type: object

 properties:

 transReqType:

 $ref: '#/components/schemas/TransferRequestType'

 nwdafEvSub:

 $ref: '#/components/schemas/NnwdafEventsSubscription'

 consumerId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 contextId:

 $ref: '#/components/schemas/AnalyticsContextIdentifier'

 sourceNfIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 minItems: 1

 sourceSetIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfSetId'

 minItems: 1

 modelInfo:

 type: array

 items:

 $ref: '#/components/schemas/ModelInfo'

 minItems: 1

 required:

 - transReqType

 - nwdafEvSub

 - consumerId

 ModelInfo:

 description: Contains information about an ML model.

 type: object

 properties:

 analyticsId:

 $ref: '#/components/schemas/NwdafEvent'

 mlModelInfos:

 type: array

 items:

 $ref: '#/components/schemas/MLModelInfo'

 minItems: 1

 required:

 - analyticsId

 - mlModelInfos

 MLModelInfo:

 description: Contains information about an ML models.

 type: object

 properties:

 mlFileAddrs:

 type: array

 items:

 $ref: 'TS29520\_Nnwdaf\_MLModelProvision.yaml#/components/schemas/MLModelAddr'

 minItems: 1

 modelProvId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 modelProvSetId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfSetId'

 oneOf:

 - required: [modelProvId]

 - required: [modelProvSetId]

 AnalyticsContextIdentifier:

 description: Contains information about available analytics contexts.

 type: object

 properties:

 subscriptionId:

 type: string

 description: The identifier of a subscription.

 nfAnaCtxts:

 type: array

 items:

 $ref: '#/components/schemas/NwdafEvent'

 minItems: 1

 description: >

 List of analytics types for which NF related analytics contexts can be retrieved.

 ueAnaCtxts:

 type: array

 items:

 $ref: '#/components/schemas/UeAnalyticsContextDescriptor'

 minItems: 1

 description: >

 List of objects that indicate for which SUPI and analytics types combinations analytics

 context can be retrieved.

 allOf:

 - anyOf:

 - required: [nfAnaCtxts]

 - required: [ueAnaCtxts]

 - required: [subscriptionId]

 UeAnalyticsContextDescriptor:

 description: Contains information about available UE related analytics contexts.

 type: object

 properties:

 supi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 anaTypes:

 type: array

 items:

 $ref: '#/components/schemas/NwdafEvent'

 minItems: 1

 description: >

 List of analytics types for which UE related analytics contexts can be retrieved.

 required:

 - supi

 - anaTypes

 DnPerfInfo:

 description: Represents DN performance information.

 type: object

 properties:

 appId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 dnPerf:

 type: array

 items:

 $ref: '#/components/schemas/DnPerf'

 minItems: 1

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 required:

 - dnPerf

 DnPerf:

 description: Represents DN performance for the application.

 type: object

 properties:

 appServerInsAddr:

 $ref: 'TS29517\_Naf\_EventExposure.yaml#/components/schemas/AddrFqdn'

 upfInfo:

 $ref: 'TS29508\_Nsmf\_EventExposure.yaml#/components/schemas/UpfInformation'

 dnai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnai'

 perfData:

 $ref: '#/components/schemas/PerfData'

 spatialValidCon:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 temporalValidCon:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

 required:

 - perfData

 PerfData:

 description: Represents DN performance data.

 type: object

 properties:

 avgTrafficRate:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 maxTrafficRate:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 minTrafficRate:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 aggTrafficRate:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 varTrafficRate:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 trafRateUeIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 minItems: 1

 avePacketDelay:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketDelBudget'

 maxPacketDelay:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketDelBudget'

 varPacketDelay:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 packDelayUeIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 minItems: 1

 avgPacketLossRate:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketLossRate'

 maxPacketLossRate:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketLossRate'

 varPacketLossRate:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 packLossUeIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 minItems: 1

 numOfUe:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 DispersionRequirement:

 description: Represents the dispersion analytics requirements.

 type: object

 properties:

 disperType:

 $ref: '#/components/schemas/DispersionType'

 classCriters:

 type: array

 items:

 $ref: '#/components/schemas/ClassCriterion'

 minItems: 1

 rankCriters:

 type: array

 items:

 $ref: '#/components/schemas/RankingCriterion'

 minItems: 1

 dispOrderCriter:

 $ref: '#/components/schemas/DispersionOrderingCriterion'

 order:

 $ref: '#/components/schemas/MatchingDirection'

 required:

 - disperType

 ClassCriterion:

 description: >

 Indicates the dispersion class criterion for fixed, camper and/or traveller UE, and/or the

 top-heavy UE dispersion class criterion.

 type: object

 properties:

 disperClass:

 $ref: '#/components/schemas/DispersionClass'

 classThreshold:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 thresMatch:

 $ref: '#/components/schemas/MatchingDirection'

 required:

 - disperClass

 - classThreshold

 - thresMatch

 RankingCriterion:

 description: Indicates the usage ranking criterion between the high, medium and low usage UE.

 type: object

 properties:

 highBase:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 lowBase:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 required:

 - highBase

 - lowBase

 DispersionInfo:

 description: >

 Represents the Dispersion information. When subscribed event is "DISPERSION", the

 "disperInfos" attribute shall be included.

 type: object

 properties:

 tsStart:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 tsDuration:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 disperCollects:

 type: array

 items:

 $ref: '#/components/schemas/DispersionCollection'

 minItems: 1

 disperType:

 $ref: '#/components/schemas/DispersionType'

 required:

 - tsStart

 - tsDuration

 - disperCollects

 - disperType

 DispersionCollection:

 description: Dispersion collection per UE location or per slice.

 type: object

 properties:

 ueLoc:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 supis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 minItems: 1

 gpsis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 minItems: 1

 appVolumes:

 type: array

 items:

 $ref: '#/components/schemas/ApplicationVolume'

 minItems: 1

 disperAmount:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 disperClass:

 $ref: '#/components/schemas/DispersionClass'

 usageRank:

 type: integer

 description: Integer where the allowed values correspond to 1, 2, 3 only.

 minimum: 1

 maximum: 3

 percentileRank:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 ueRatio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 allOf:

 - oneOf:

 - required: [ueLoc]

 - required: [snssai]

 - anyOf:

 - required: [disperAmount]

 - required: [disperClass]

 - required: [usageRank]

 - required: [percentileRank]

 ApplicationVolume:

 description: Application data volume per Application Id.

 type: object

 properties:

 appId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 appVolume:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

 required:

 - appId

 - appVolume

 RedundantTransmissionExpReq:

 description: Represents other redundant transmission experience analytics requirements.

 type: object

 properties:

 redTOrderCriter:

 $ref: '#/components/schemas/RedTransExpOrderingCriterion'

 order:

 $ref: '#/components/schemas/MatchingDirection'

 RedundantTransmissionExpInfo:

 description: >

 The redundant transmission experience related information. When subscribed event is

 "RED\_TRANS\_EXP", the "redTransInfos" attribute shall be included.

 type: object

 properties:

 spatialValidCon:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 redTransExps:

 type: array

 items:

 $ref: '#/components/schemas/RedundantTransmissionExpPerTS'

 minItems: 1

 required:

 - redTransExps

 RedundantTransmissionExpPerTS:

 description: The redundant transmission experience per Time Slot.

 type: object

 properties:

 tsStart:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 tsDuration:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 obsvRedTransExp:

 $ref: '#/components/schemas/ObservedRedundantTransExp'

 redTransStatus:

 type: boolean

 description: >

 Redundant Transmission Status. Set to "true" if redundant transmission was activated,

 otherwise set to "false". Default value is "false" if omitted.

 ueRatio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 required:

 - tsStart

 - tsDuration

 - obsvRedTransExp

 ObservedRedundantTransExp:

 description: Represents the observed redundant transmission experience related information.

 type: object

 properties:

 avgPktDropRateUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketLossRate'

 varPktDropRateUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 avgPktDropRateDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketLossRate'

 varPktDropRateDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 avgPktDelayUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketDelBudget'

 varPktDelayUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 avgPktDelayDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketDelBudget'

 varPktDelayDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 avgE2ePktDelayUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketDelBudget'

 varE2ePktDelayUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 avgE2ePktDelayDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketDelBudget'

 varE2ePktDelayDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 avgE2ePktLossRateUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketLossRate'

 varE2ePktLossRateUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 avgE2ePktLossRateDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketLossRate'

 varE2ePktLossRateDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 WlanPerformanceReq:

 description: Represents other WLAN performance analytics requirements.

 type: object

 properties:

 ssIds:

 type: array

 items:

 type: string

 minItems: 1

 bssIds:

 type: array

 items:

 type: string

 minItems: 1

 wlanOrderCriter:

 $ref: '#/components/schemas/WlanOrderingCriterion'

 order:

 $ref: '#/components/schemas/MatchingDirection'

 WlanPerformanceInfo:

 description: The WLAN performance related information.

 type: object

 properties:

 networkArea:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 wlanPerSsidInfos:

 type: array

 items:

 $ref: '#/components/schemas/WlanPerSsIdPerformanceInfo'

 minItems: 1

 wlanPerUeIdInfos:

 type: array

 items:

 $ref: '#/components/schemas/WlanPerUeIdPerformanceInfo'

 minItems: 1

 description: >

 WLAN performance information for UE Id(s) of WLAN access points deployed in the Area

 of Interest.

 required:

 - wlanPerSsidInfos

 WlanPerSsIdPerformanceInfo:

 description: The WLAN performance per SSID.

 type: object

 properties:

 ssId:

 type: string

 wlanPerTsInfos:

 type: array

 items:

 $ref: '#/components/schemas/WlanPerTsPerformanceInfo'

 minItems: 1

 required:

 - ssId

 - wlanPerTsInfos

 WlanPerUeIdPerformanceInfo:

 description: The WLAN performance per UE ID.

 type: object

 properties:

 supi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 wlanPerTsInfos:

 type: array

 items:

 $ref: '#/components/schemas/WlanPerTsPerformanceInfo'

 minItems: 1

 description: >

 WLAN performance information per Time Slot during the analytics target period.

 required:

 - supi

 - wlanPerTsInfos

 WlanPerTsPerformanceInfo:

 description: WLAN performance information per Time Slot during the analytics target period.

 type: object

 properties:

 tsStart:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 tsDuration:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 rssi:

 type: integer

 rtt:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 trafficInfo:

 $ref: '#/components/schemas/TrafficInformation'

 numberOfUes:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 required:

 - tsStart

 - tsDuration

 anyOf:

 - required: [rssi]

 - required: [rtt]

 - required: [trafficInfo]

 - required: [numberOfUes]

 TrafficInformation:

 description: Traffic information including UL/DL data rate and/or Traffic volume.

 type: object

 properties:

 uplinkRate:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 downlinkRate:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 uplinkVolume:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

 downlinkVolume:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

 totalVolume:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

 anyOf:

 - required: [uplinkRate]

 - required: [downlinkRate]

 - required: [uplinkVolume]

 - required: [downlinkVolume]

 - required: [totalVolume]

 AppListForUeComm:

 description: Represents the analytics of the application list used by UE.

 type: object

 properties:

 appId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 startTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 appDur:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 occurRatio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 spatialValidity:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 required:

 - appId

 SessInactTimerForUeComm:

 description: Represents the N4 Session inactivity timer.

 type: object

 properties:

 n4SessId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionId'

 sessInactiveTimer:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 required:

 - n4SessId

 - sessInactiveTimer

 DnPerformanceReq:

 description: Represents other DN performance analytics requirements.

 type: object

 properties:

 dnPerfOrderCriter:

 $ref: '#/components/schemas/DnPerfOrderingCriterion'

 order:

 $ref: '#/components/schemas/MatchingDirection'

 reportThresholds:

 type: array

 items:

 $ref: '#/components/schemas/ThresholdLevel'

 minItems: 1

 RatFreqInformation:

 description: Represents the RAT type and/or Frequency information.

 type: object

 properties:

 allFreq:

 type: boolean

 description: >

 Set to "true" to indicate to handle all the frequencies the NWDAF received, otherwise

 set to "false" or omit. The "allFreq" attribute and the "freq" attribute are mutually

 exclusive.

 allRat:

 type: boolean

 description: >

 Set to "true" to indicate to handle all the RAT Types the NWDAF received, otherwise

 set to "false" or omit. The "allRat" attribute and the "ratType" attribute are mutually

 exclusive.

 freq:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ArfcnValueNR'

 ratType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 svcExpThreshold:

 $ref: '#/components/schemas/ThresholdLevel'

 matchingDir:

 $ref: '#/components/schemas/MatchingDirection'

 PrevSubInfo:

 description: Information of the previous subscription.

 type: object

 properties:

 producerId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 producerSetId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfSetId'

 subscriptionId:

 type: string

 description: The identifier of a subscription.

 nfAnaEvents:

 type: array

 items:

 $ref: '#/components/schemas/NwdafEvent'

 minItems: 1

 ueAnaEvents:

 type: array

 items:

 $ref: '#/components/schemas/UeAnalyticsContextDescriptor'

 minItems: 1

 required:

 - subscriptionId

 oneOf:

 - required: [producerId]

 - required: [producerSetId]

 ResourceUsage:

 description: >

 The current usage of the virtual resources assigned to the NF instances belonging to a

 particular network slice instance.

 type: object

 properties:

 cpuUsage:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 memoryUsage:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 storageUsage:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 ConsumerNfInformation:

 description: Represents the analytics consumer NF Information.

 type: object

 properties:

 nfId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 nfSetId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfSetId'

 taiList:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Tai'

 minItems: 1

 oneOf:

 - oneOf:

 - required: [nfId]

 - required: [nfSetId]

 - required: [taiList]

 UeCommReq:

 description: UE communication analytics requirement.

 type: object

 properties:

 orderCriterion:

 $ref: '#/components/schemas/UeCommOrderCriterion'

 orderDirection:

 $ref: '#/components/schemas/MatchingDirection'

 UeMobilityReq:

 description: UE mobility analytics requirement.

 type: object

 properties:

 orderCriterion:

 $ref: '#/components/schemas/UeMobilityOrderCriterion'

 orderDirection:

 $ref: '#/components/schemas/MatchingDirection'

 ueLocOrderInd:

 type: boolean

 description: >

 UE Location order indication. Set to "true" to indicate the NWDAF to provide the UE

 Mobility analytics in a UE Location order, otherwise set to "false" or omit.

 PduSessionInfo:

 description: Represents combination of PDU Session parameter(s) information.

 type: object

 properties:

 pduSessType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionType'

 sscMode:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SscMode'

 accessType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/AccessType'

 PfdDeterminationInfo:

 description: Represents the PFD Determination information for a known application identifier.

 type: object

 properties:

 appId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 flowDescriptions:

 type: array

 items:

 type: string

 minItems: 1

 description: >

 Represents a 3-tuple with protocol, server ip and server port for UL/DL

 application traffic. The content of the string has the same encoding as the IPFilterRule

 AVP value as defined in IETF RFC 6733.

 urls:

 type: array

 items:

 type: string

 minItems: 1

 description: Represents the significant parts of the URL to be matched, e.g. host name.

 domainNames:

 type: array

 items:

 type: string

 minItems: 1

 description: Represents Domain name matching criteria.

 dnProtocol:

 $ref: 'TS29122\_PfdManagement.yaml#/components/schemas/DomainNameProtocol'

 required:

 - appId

 PduSesTrafficInfo:

 description: Represents the PDU Set traffic analytics information.

 type: object

 properties:

 supis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 minItems: 1

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 tdMatchTrafs:

 type: array

 items:

 $ref: '#/components/schemas/TdTraffic'

 minItems: 1

 tdUnmatchTrafs:

 type: array

 items:

 $ref: '#/components/schemas/TdTraffic'

 minItems: 1

 allOf:

 - anyOf:

 - required: [dnn]

 - required: [snssai]

 - anyOf:

 - required: [tdMatchTrafs]

 - required: [tdUnmatchTrafs]

 TdTraffic:

 description: Represents traffic that matches or unmatches Traffic Descriptor of URSP rule.

 type: object

 properties:

 pduSesTrafReqs:

 type: array

 items:

 $ref: '#/components/schemas/PduSesTrafficReq'

 minItems: 1

 ulVol:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

 dlVol:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

 allVol:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

 ulNumOfPkt:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 dlNumOfPkt:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 allNumOfPkt:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 PduSesTrafficReq:

 description: Represents the PDU Session traffic analytics requirements.

 type: object

 properties:

 flowDescs:

 type: array

 items:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/FlowDescription'

 minItems: 1

 description: >

 Indicates traffic flow filtering description(s) for IP flow(s).

 appId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 domainDescs:

 type: array

 items:

 type: string

 minItems: 1

 description: >

 FQDN(s) or a regular expression which are used as a domain name matching criteria.

 oneOf:

 - required: [flowDescs]

 - required: [appId]

 - required: [domainDescs]

 ResourceUsageRequirement:

 description: resource usage requirement.

 type: object

 properties:

 tfcDirc:

 $ref: '#/components/schemas/TrafficDirection'

 valExp:

 $ref: '#/components/schemas/ValueExpression'

 E2eDataVolTransTimeReq:

 description: Represents other E2E data volume transfer time analytics requirements.

 type: object

 properties:

 criterion:

 $ref: '#/components/schemas/E2eDataVolTransTimeCriterion'

 order:

 $ref: '#/components/schemas/MatchingDirection'

 highTransTmThld:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 lowTransTmThld:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 repeatDataTrans:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 tsIntervalDataTrans:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 dataVolume:

 $ref: '#/components/schemas/DataVolume'

 maxNumberUes:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 DataVolume:

 description: Data Volume including UL/DL.

 type: object

 properties:

 uplinkVolume:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

 downlinkVolume:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

 anyOf:

 - required: [uplinkVolume]

 - required: [downlinkVolume]

 E2eDataVolTransTimeInfo:

 description: >

 Represents the E2E data volume transfer time analytics information when subscribed event is

 "E2E\_DATA\_VOL\_TRANS\_TIME", the "dataVlTrnsTmInfos" attribute shall be included.

 type: object

 properties:

 e2eDataVolTransTimes:

 type: array

 items:

 $ref: '#/components/schemas/E2eDataVolTransTimePerTS'

 minItems: 1

 e2eDataVolTransTimeUeLists:

 type: array

 items:

 $ref: '#/components/schemas/E2eDataVolTransTimeUeList'

 minItems: 1

 geoDistrInfos:

 type: array

 items:

 $ref: '#/components/schemas/GeoDistributionInfo'

 minItems: 1

 required:

 - e2eDataVolTransTimes

 E2eDataVolTransTimePerTS:

 description: Represents the E2E data volume transfer time analytics per Time Slot.

 type: object

 properties:

 tsStart:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 tsDuration:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 e2eDataVolTransTimePerUe:

 type: array

 items:

 $ref: '#/components/schemas/E2eDataVolTransTimePerUe'

 minItems: 1

 repeatDataTrans:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 tsIntervalDataTrans:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 required:

 - tsStart

 - tsDuration

 - e2eDataVolTransTimePerUe

 E2eDataVolTransTimePerUe:

 description: Represents the E2E data volume transfer time per UE.

 type: object

 properties:

 supis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 minItems: 1

 gpsis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 appId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 ueLoc:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 dnai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnai'

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 spatialValidity:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 validityPeriod:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

 dataVolTransTime:

 $ref: '#/components/schemas/DataVolumeTransferTime'

 oneOf:

 - required: [ueLoc]

 - required: [snssai]

 E2eDataVolTransTimeUeList:

 description: >

 Contains the list of UEs classified based on experience level of E2E Data Volume Transfer

 Time

 properties:

 highLevel:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 minItems: 1

 mediumLevel:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 minItems: 1

 lowLevel:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 minItems: 1

 lowRatio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 mediumRatio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 highRatio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 spatialValidity:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 validityPeriod:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

 anyOf:

 - required: [highLevel]

 - required: [mediumLevel]

 - required: [lowLevel]

 DataVolumeTransferTime:

 description: >

 Indicates the E2E data volume transfer time and the data volume used to derive the transfer

 time.

 properties:

 uplinkVolume:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

 avgTransTimeUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 varTransTimeUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 downlinkVolume:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

 avgTransTimeDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 varTransTimeDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 GeoLocation:

 description: >

 Represents a horizontal and optionally vertical location using either geographic

 or local coordinates.

 type: object

 properties:

 point:

 $ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/Point'

 pointAlt:

 $ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/PointAltitude'

 refPoint:

 $ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/LocalOrigin'

 localCoords:

 $ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/RelativeCartesianLocation'

 anyOf:

 - required: [point]

 - required: [pointAlt]

 - allOf:

 - required: [refPoint]

 - required: [localCoords]

 LocAccuracyReq:

 description: >

 Contains location accuracy analytics requirements.

 type: object

 properties:

 accThres:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 accThresMatchDir:

 $ref: '#/components/schemas/MatchingDirection'

 inOutThres:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 inOutThresMatchDir:

 $ref: '#/components/schemas/MatchingDirection'

 posMethod:

 $ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/PositioningMethod'

 LocAccuracyInfo:

 description: >

 Contains location accuracy analytics.

 type: object

 properties:

 locAccPerMeths:

 type: array

 items:

 $ref: '#/components/schemas/LocAccuracyPerMethod'

 minItems: 1

 description: Location accuracy information per positioning method.

 inOutUePct:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 inOutInd:

 type: boolean

 description: Indicates if the target location is indoors or outdoors.

 required:

 - locAccPerMeths

 not:

 required: [inOutUePct, inOutInd]

 LocAccuracyPerMethod:

 description: >

 Contains location accuracy analytics per positioning method.

 type: object

 properties:

 posMethod:

 $ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/PositioningMethod'

 locAcc:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 losNlosPercent:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 required:

 - posMethod

 - locAcc

 AccuracyReq:

 description: Represents the analytics accuracy requirement information.

 type: object

 properties:

 accuTimeWin:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

 accuPeriod:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 accuDevThr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 minNum:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 updatedAnaFlg:

 type: boolean

 description: >

 Indicates the updated Analytics flag. Set to "true" indicates that the NWDAF can provide

 the updated analytics if the analytics can be generated within the analytics accuracy

 information time window, which is specified by "accuTimeWin" attribute.

 Otherwise set to “false”. Default value is “false” if omitted.

 correctionInterval:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 AccuracyInfo:

 description: The analytics accuracy information.

 type: object

 properties:

 accuracyVal:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 accuSampleNbr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 anaAccuInd:

 $ref: '#/components/schemas/AnalyticsAccuracyIndication'

 MovBehavReq:

 description: Represents the Movement Behaviour analytics requirements.

 properties:

 locationGranReq:

 $ref: '#/components/schemas/LocInfoGranularity'

 reportThresholds:

 $ref: '#/components/schemas/ThresholdLevel'

 MovBehavInfo:

 description: Represents the Movement Behaviour information.

 properties:

 geoLoc:

 $ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/GeographicalCoordinates'

 movBehavs:

 type: array

 items:

 $ref: '#/components/schemas/MovBehav'

 minItems: 1

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 MovBehav:

 description: Represents the Movement Behaviour information per time slot.

 properties:

 tsStart:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 tsDuration:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 numOfUe:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 ratio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 avrSpeed:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 speedThresdInfos:

 type: array

 items:

 $ref: '#/components/schemas/SpeedThresholdInfo'

 minItems: 1

 directionUeInfos:

 type: array

 items:

 $ref: '#/components/schemas/DirectionInfo'

 minItems: 1

 required:

 - tsStart

 - tsDuration

 SpeedThresholdInfo:

 description: UEs information whose speed is faster than the speed threshold.

 properties:

 numOfUe:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 ratio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 DirectionUeInfo:

 description: Heading directions information of the UE flow in the target area.

 properties:

 direction:

 $ref: '#/components/schemas/Direction'

 numOfUe:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 avrSpeed:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 ratio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 required:

 - direction

#

# ENUMERATIONS DATA TYPES

#

 NotificationMethod:

 anyOf:

 - type: string

 enum:

 - PERIODIC

 - THRESHOLD

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Represents the notification methods for the subscribed events.

 Possible values are:

 - PERIODIC: The notification of the subscribed NWDAF Event is periodical. The period

 between the notifications is identified by repetitionPeriod and represents time in

 seconds.

 - THRESHOLD: The subscribe of NWDAF Event is upon threshold exceeded.

 NwdafEvent:

 anyOf:

 - type: string

 enum:

 - SLICE\_LOAD\_LEVEL

 - NETWORK\_PERFORMANCE

 - NF\_LOAD

 - SERVICE\_EXPERIENCE

 - UE\_MOBILITY

 - UE\_COMMUNICATION

 - QOS\_SUSTAINABILITY

 - ABNORMAL\_BEHAVIOUR

 - USER\_DATA\_CONGESTION

 - NSI\_LOAD\_LEVEL

 - DN\_PERFORMANCE

 - DISPERSION

 - RED\_TRANS\_EXP

 - WLAN\_PERFORMANCE

 - SM\_CONGESTION

 - PFD\_DETERMINATION

 - PDU\_SESSION\_TRAFFIC

 - E2E\_DATA\_VOL\_TRANS\_TIME

 - MOVEMENT\_BEHAVIOUR

 - NUM\_OF\_UE

 - MOV\_UE\_RATIO

 - AVR\_SPEED

 - SPEED\_THRESHOLD

 - MOV\_UE\_DIRECTION

 - LOC\_ACCURACY

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Describes the NWDAF Events.

 Possible values are:

 - SLICE\_LOAD\_LEVEL: Indicates that the event subscribed is load level information of Network

 Slice.

 - NETWORK\_PERFORMANCE: Indicates that the event subscribed is network performance

 information.

 - NF\_LOAD: Indicates that the event subscribed is load level and status of one or several

 Network Functions.

 - SERVICE\_EXPERIENCE: Indicates that the event subscribed is service experience.

 - UE\_MOBILITY: Indicates that the event subscribed is UE mobility information.

 - UE\_COMMUNICATION: Indicates that the event subscribed is UE communication information.

 - QOS\_SUSTAINABILITY: Indicates that the event subscribed is QoS sustainability.

 - ABNORMAL\_BEHAVIOUR: Indicates that the event subscribed is abnormal behaviour.

 - USER\_DATA\_CONGESTION: Indicates that the event subscribed is user data congestion

 information.

 - NSI\_LOAD\_LEVEL: Indicates that the event subscribed is load level information of Network

 Slice and the optionally associated Network Slice Instance.

 - DN\_PERFORMANCE: Indicates that the event subscribed is DN performance information.

 - DISPERSION: Indicates that the event subscribed is dispersion information.

 - RED\_TRANS\_EXP: Indicates that the event subscribed is redundant transmission experience.

 - WLAN\_PERFORMANCE: Indicates that the event subscribed is WLAN performance.

 - SM\_CONGESTION: Indicates the Session Management Congestion Control Experience information

 for specific DNN and/or S-NSSAI.

 - PFD\_DETERMINATION: Indicates that the event subscribed is the PFD Determination nformation

 for known application identifier(s).

 - PDU\_SESSION\_TRAFFIC: Indicates that the event subscribed is the PDU Session traffic

 information.

 - E2E\_DATA\_VOL\_TRANS\_TIME: Indicates that the event subscribed is of E2E data volume

 transfer time.

 - MOVEMENT\_BEHAVIOUR: Indicates that the event subscribed is the Movement Behaviour

 information.

 - LOC\_ACCURACY: Indicates that the event subscribed is of location accuracy.

 Accuracy:

 anyOf:

 - type: string

 enum:

 - LOW

 - MEDIUM

 - HIGH

 - HIGHEST

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Represents the preferred level of accuracy of the analytics.

 Possible values are:

 - LOW: Low accuracy.

 - MEDIUM: Medium accuracy.

 - HIGH: High accuracy.

 - HIGHEST: Highest accuracy.

 CongestionType:

 anyOf:

 - type: string

 enum:

 - USER\_PLANE

 - CONTROL\_PLANE

 - USER\_AND\_CONTROL\_PLANE

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Indicates the congestion analytics type.

 Possible values are:

 - USER\_PLANE: The congestion analytics type is User Plane.

 - CONTROL\_PLANE: The congestion analytics type is Control Plane.

 - USER\_AND\_CONTROL\_PLANE: The congestion analytics type is User Plane and Control Plane.

 ExceptionId:

 anyOf:

 - type: string

 enum:

 - UNEXPECTED\_UE\_LOCATION

 - UNEXPECTED\_LONG\_LIVE\_FLOW

 - UNEXPECTED\_LARGE\_RATE\_FLOW

 - UNEXPECTED\_WAKEUP

 - SUSPICION\_OF\_DDOS\_ATTACK

 - WRONG\_DESTINATION\_ADDRESS

 - TOO\_FREQUENT\_SERVICE\_ACCESS

 - UNEXPECTED\_RADIO\_LINK\_FAILURES

 - PING\_PONG\_ACROSS\_CELLS

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Describes the Exception Id.

 Possible values are:

 - UNEXPECTED\_UE\_LOCATION: Unexpected UE location.

 - UNEXPECTED\_LONG\_LIVE\_FLOW: Unexpected long-live rate flows.

 - UNEXPECTED\_LARGE\_RATE\_FLOW: Unexpected large rate flows.

 - UNEXPECTED\_WAKEUP: Unexpected wakeup.

 - SUSPICION\_OF\_DDOS\_ATTACK: Suspicion of DDoS attack.

 - WRONG\_DESTINATION\_ADDRESS: Wrong destination address.

 - TOO\_FREQUENT\_SERVICE\_ACCESS: Too frequent Service Access.

 - UNEXPECTED\_RADIO\_LINK\_FAILURES: Unexpected radio link failures.

 - PING\_PONG\_ACROSS\_CELLS: Ping-ponging across neighbouring cells.

 ExceptionTrend:

 anyOf:

 - type: string

 enum:

 - UP

 - DOWN

 - UNKNOW

 - STABLE

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Represents the Exception Trend.

 Possible values are:

 - UP: Up trend of the exception level.

 - DOWN: Down trend of the exception level.

 - UNKNOW: Unknown trend of the exception level.

 - STABLE: Stable trend of the exception level.

 TimeUnit:

 anyOf:

 - type: string

 enum:

 - MINUTE

 - HOUR

 - DAY

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Represents the unit for the session active time.

 Possible values are:

 - MINUTE: Time unit is per minute.

 - HOUR: Time unit is per hour.

 - DAY: Time unit is per day.

 NetworkPerfType:

 anyOf:

 - type: string

 enum:

 - GNB\_ACTIVE\_RATIO

 - GNB\_COMPUTING\_USAGE

 - GNB\_MEMORY\_USAGE

 - GNB\_DISK\_USAGE

 - GNB\_RSC\_USAGE\_OVERALL\_TRAFFIC

 - GNB\_RSC\_USAGE\_GBR\_TRAFFIC

 - GNB\_RSC\_USAGE\_DELAY\_CRIT\_GBR\_TRAFFIC

 - NUM\_OF\_UE

 - SESS\_SUCC\_RATIO

 - HO\_SUCC\_RATIO

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Represents the network performance types.

 Possible values are:

 - GNB\_ACTIVE\_RATIO: Indicates that the network performance requirement is gNodeB active

 (i.e. up and running) rate. Indicates the ratio of gNB active (i.e. up and running) number

 to the total number of gNB.

 - GNB\_COMPUTING\_USAGE: Indicates gNodeB computing resource usage.

 - GNB\_MEMORY\_USAGE: Indicates gNodeB memory usage.

 - GNB\_DISK\_USAGE: Indicates gNodeB disk usage.

 - GNB\_RSC\_USAGE\_OVERALL\_TRAFFIC: The gNB resource usage.

 - GNB\_RSC\_USAGE\_GBR\_TRAFFIC: The gNB resource usage for GBR traffic.

 - GNB\_RSC\_USAGE\_DELAY\_CRIT\_GBR\_TRAFFIC: The gNB resource usage for Delay-critical GBR

 traffic.

 - NUM\_OF\_UE: Indicates number of UEs.

 - SESS\_SUCC\_RATIO: Indicates ratio of successful setup of PDU sessions to total PDU

 session setup attempts.

 - HO\_SUCC\_RATIO: Indicates Ratio of successful handovers to the total handover attempts.

 ExpectedAnalyticsType:

 anyOf:

 - type: string

 enum:

 - MOBILITY

 - COMMUN

 - MOBILITY\_AND\_COMMUN

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Represents the expected UE analytics type.

 Possible values are:

 - MOBILITY: Mobility related abnormal behaviour analytics is expected by the consumer.

 - COMMUN: Communication related abnormal behaviour analytics is expected by the consumer.

 - MOBILITY\_AND\_COMMUN: Both mobility and communication related abnormal behaviour analytics

 is expected by the consumer.

 MatchingDirection:

 anyOf:

 - type: string

 enum:

 - ASCENDING

 - DESCENDING

 - CROSSED

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Represents the matching direction when crossing a threshold.

 Possible values are:

 - ASCENDING: Threshold is crossed in ascending direction.

 - DESCENDING: Threshold is crossed in descending direction.

 - CROSSED: Threshold is crossed either in ascending or descending direction.

 NwdafFailureCode:

 anyOf:

 - type: string

 enum:

 - UNAVAILABLE\_DATA

 - BOTH\_STAT\_PRED\_NOT\_ALLOWED

 - UNSATISFIED\_REQUESTED\_ANALYTICS\_TIME

 - OTHER

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Represents the failure reason.

 Possible values are:

 - UNAVAILABLE\_DATA: Indicates the requested statistics information for the event is rejected

 since necessary data to perform the service is unavailable.

 - BOTH\_STAT\_PRED\_NOT\_ALLOWED: Indicates the requested analysis information for the event is

 rejected since the start time is in the past and the end time is in the future, which

 means the NF service consumer requested both statistics and prediction for the analytics.

 - UNSATISFIED\_REQUESTED\_ANALYTICS\_TIME: Indicates that the requested event is rejected since

 the analytics information is not ready when the time indicated by the "timeAnaNeeded"

 attribute (as provided during the creation or modification of subscription) is reached.

 - OTHER: Indicates the requested analysis information for the event is rejected due to other

 reasons.

 AnalyticsMetadata:

 anyOf:

 - type: string

 enum:

 - NUM\_OF\_SAMPLES

 - DATA\_WINDOW

 - DATA\_STAT\_PROPS

 - STRATEGY

 - ACCURACY

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Represents the types of analytics metadata information that can be requested.

 Possible values are:

 - NUM\_OF\_SAMPLES: Number of data samples used for the generation of the output analytics.

 - DATA\_WINDOW: Data time window of the data samples.

 - DATA\_STAT\_PROPS: Dataset statistical properties of the data used to generate the

 analytics.

 - STRATEGY: Output strategy used for the reporting of the analytics.

 - ACCURACY: Level of accuracy reached for the analytics.

 DatasetStatisticalProperty:

 anyOf:

 - type: string

 enum:

 - UNIFORM\_DIST\_DATA

 - NO\_OUTLIERS

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Represents the dataset statistical properties.

 Possible values are:

 - UNIFORM\_DIST\_DATA: Indicates the use of data samples that are uniformly distributed

 according to the different aspects of the requested analytics.

 - NO\_OUTLIERS: Indicates that the data samples shall disregard data samples that are at

 the extreme boundaries of the value range.

 OutputStrategy:

 anyOf:

 - type: string

 enum:

 - BINARY

 - GRADIENT

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Represents the output strategy used for the analytics reporting.

 Possible values are:

 - BINARY: Indicates that the analytics shall only be reported when the requested level

 of accuracy is reached within a cycle of periodic notification.

 - GRADIENT: Indicates that the analytics shall be reported according with the periodicity

 irrespective of whether the requested level of accuracy has been reached or not.

 TransferRequestType:

 anyOf:

 - type: string

 enum:

 - PREPARE

 - TRANSFER

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Represents the request type for the analytics subscription transfer.

 Possible values are:

 - PREPARE: Indicates that the request is for analytics subscription transfer preparation.

 - TRANSFER: Indicates that the request is for analytics subscription transfer execution.

 AnalyticsSubset:

 anyOf:

 - type: string

 enum:

 - NUM\_OF\_UE\_REG

 - NUM\_OF\_PDU\_SESS\_ESTBL

 - RES\_USAGE

 - NUM\_OF\_EXCEED\_RES\_USAGE\_LOAD\_LEVEL\_THR

 - PERIOD\_OF\_EXCEED\_RES\_USAGE\_LOAD\_LEVEL\_THR

 - EXCEED\_LOAD\_LEVEL\_THR\_IND

 - LIST\_OF\_TOP\_APP\_UL

 - LIST\_OF\_TOP\_APP\_DL

 - NF\_STATUS

 - NF\_RESOURCE\_USAGE

 - NF\_LOAD

 - NF\_PEAK\_LOAD

 - NF\_LOAD\_AVG\_IN\_AOI

 - DISPER\_AMOUNT

 - DISPER\_CLASS

 - RANKING

 - PERCENTILE\_RANKING

 - RSSI

 - RTT

 - TRAFFIC\_INFO

 - NUMBER\_OF\_UES

 - APP\_LIST\_FOR\_UE\_COMM

 - N4\_SESS\_INACT\_TIMER\_FOR\_UE\_COMM

 - AVG\_TRAFFIC\_RATE

 - MAX\_TRAFFIC\_RATE

 - AGG\_TRAFFIC\_RATE

 - VAR\_TRAFFIC\_RATE

 - AVG\_PACKET\_DELAY

 - MAX\_PACKET\_DELAY

 - VAR\_PACKET\_DELAY

 - AVG\_PACKET\_LOSS\_RATE

 - MAX\_PACKET\_LOSS\_RATE

 - VAR\_PACKET\_LOSS\_RATE

 - UE\_LOCATION

 - LIST\_OF\_HIGH\_EXP\_UE

 - LIST\_OF\_MEDIUM\_EXP\_UE

 - LIST\_OF\_LOW\_EXP\_UE

 - AVG\_UL\_PKT\_DROP\_RATE

 - VAR\_UL\_PKT\_DROP\_RATE

 - AVG\_DL\_PKT\_DROP\_RATE

 - VAR\_DL\_PKT\_DROP\_RATE

 - AVG\_UL\_PKT\_DELAY

 - VAR\_UL\_PKT\_DELAY

 - AVG\_DL\_PKT\_DELAY

 - VAR\_DL\_PKT\_DELAY

 - TRAFFIC\_MATCH\_TD

 - TRAFFIC\_UNMATCH\_TD

 - NUMBER\_OF\_UE

 - UE\_GEOG\_DIST

 - UE\_DIRECTION

 - USER\_LOCATION

 - AVG\_E2E\_UL\_PKT\_DELAY

 - VAR\_E2E\_UL\_PKT\_DELAY

 - AVG\_E2E\_DL\_PKT\_DELAY

 - VAR\_E2E\_DL\_PKT\_DELAY

 - AVG\_E2E\_UL\_PKT\_LOSS\_RATE

 - VAR\_E2E\_UL\_PKT\_LOSS\_RATE

 - AVG\_E2E\_DL\_PKT\_LOSS\_RATE

 - VAR\_E2E\_DL\_PKT\_LOSS\_RATE

 - E2E\_DATA\_VOL\_TRANS\_TIME\_FOR\_UE\_LIST

 - IN\_OUT\_PERCENT

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Represents the analytics subset.

 Possible values are:

 - NUM\_OF\_UE\_REG: The number of UE registered. This value is only applicable to

 NSI\_LOAD\_LEVEL event.

 - NUM\_OF\_PDU\_SESS\_ESTBL: The number of PDU sessions established. This value is only

 applicable to NSI\_LOAD\_LEVEL event.

 - RES\_USAGE: The current usage of the virtual resources assigned to the NF instances

 belonging to a particular network slice instance. This value is only applicable to

 NSI\_LOAD\_LEVEL event.

 - NUM\_OF\_EXCEED\_RES\_USAGE\_LOAD\_LEVEL\_THR: The number of times the resource usage threshold

 of the network slice instance is reached or exceeded if a threshold value is provided by

 the consumer. This value is only applicable to NSI\_LOAD\_LEVEL event.

 - PERIOD\_OF\_EXCEED\_RES\_USAGE\_LOAD\_LEVEL\_THR: The time interval between each time the

 threshold being met or exceeded on the network slice (instance). This value is only

 applicable to NSI\_LOAD\_LEVEL event.

 - EXCEED\_LOAD\_LEVEL\_THR\_IND: Whether the Load Level Threshold is met or exceeded by the

 statistics value. This value is only applicable to NSI\_LOAD\_LEVEL event.

 - LIST\_OF\_TOP\_APP\_UL: The list of applications that contribute the most to the traffic in

 the UL direction. This value is only applicable to USER\_DATA\_CONGESTION event.

 - LIST\_OF\_TOP\_APP\_DL: The list of applications that contribute the most to the traffic in

 the DL direction. This value is only applicable to USER\_DATA\_CONGESTION event.

 - NF\_STATUS: The availability status of the NF on the Analytics target period, expressed

 as a percentage of time per status value (registered, suspended, undiscoverable). This

 value is only applicable to NF\_LOAD event.

 - NF\_RESOURCE\_USAGE: The average usage of assigned resources (CPU, memory, storage). This

 value is only applicable to NF\_LOAD event.

 - NF\_LOAD: The average load of the NF instance over the Analytics target period. This value

 is only applicable to NF\_LOAD event.

 - NF\_PEAK\_LOAD: The maximum load of the NF instance over the Analytics target period. This

 value is only applicable to NF\_LOAD event.

 - NF\_LOAD\_AVG\_IN\_AOI: The average load of the NF instances over the area of interest. This

 value is only applicable to NF\_LOAD event.

 - DISPER\_AMOUNT: Indicates the dispersion amount of the reported data volume or transaction

 dispersion type. This value is only applicable to DISPERSION event.

 - DISPER\_CLASS: Indicates the dispersion mobility class: fixed, camper, traveller upon set

 its usage threshold, and/or the top-heavy class upon set its percentile rating threshold.

 This value is only applicable to DISPERSION event.

 - RANKING: Data/transaction usage ranking high (i.e.value 1), medium (2) or low (3). This

 value is only applicable to DISPERSION event.

 - PERCENTILE\_RANKING: Percentile ranking of the target UE in the Cumulative Distribution

 Function of data usage for the population of all UEs. This value is only applicable to

 DISPERSION event.

 - RSSI: Indicated the RSSI in the unit of dBm. This value is only applicable to

 WLAN\_PERFORMANCE event.

 - RTT: Indicates the RTT in the unit of millisecond. This value is only applicable to

 WLAN\_PERFORMANCE event.

 - TRAFFIC\_INFO: Traffic information including UL/DL data rate and/or Traffic volume. This

 value is only applicable to WLAN\_PERFORMANCE event.

 - NUMBER\_OF\_UES: Number of UEs observed for the SSID. This value is only applicable to

 WLAN\_PERFORMANCE event.

 - APP\_LIST\_FOR\_UE\_COMM: The analytics of the application list used by UE. This value is only

 applicable to UE\_COMM event.

 - N4\_SESS\_INACT\_TIMER\_FOR\_UE\_COMM: The N4 Session inactivity timer. This value is only

 applicable to UE\_COMM event.

 - AVG\_TRAFFIC\_RATE: Indicates average traffic rate. This value is only applicable to

 DN\_PERFORMANCE event.

 - MAX\_TRAFFIC\_RATE: Indicates maximum traffic rate. This value is only applicable to

 DN\_PERFORMANCE event.

 - AGG\_TRAFFIC\_RATE: Indicates aggregated traffic rate. This value is only applicable to

 DN\_PERFORMANCE event.

 - VAR\_TRAFFIC\_RATE: Indicates variance traffic rate. This value is only applicable to

 DN\_PERFORMANCE event.

 - AVG\_PACKET\_DELAY: Indicates average Packet Delay. This value is only applicable to

 DN\_PERFORMANCE event.

 - MAX\_PACKET\_DELAY: Indicates maximum Packet Delay. This value is only applicable to

 DN\_PERFORMANCE event.

 - VAR\_PACKET\_DELAY: Indicates variance Packet Delay. This value is only applicable to

 DN\_PERFORMANCE event.

 - AVG\_PACKET\_LOSS\_RATE: Indicates average Loss Rate. This value is only applicable to

 DN\_PERFORMANCE event.

 - MAX\_PACKET\_LOSS\_RATE: Indicates maximum Packet Loss Rate. This value is only applicable to

 DN\_PERFORMANCE event.

 - VAR\_PACKET\_LOSS\_RATE: Indicates variance Packet Loss Rate. This value is only applicable

 to DN\_PERFORMANCE event.

 - UE\_LOCATION: Indicates UE location information. This value is only applicable to

 SERVICE\_EXPERIENCE event.

 - LIST\_OF\_HIGH\_EXP\_UE: Indicates list of high experienced UE. This value is only applicable

 to SM\_CONGESTION event.

 - LIST\_OF\_MEDIUM\_EXP\_UE: Indicates list of medium experienced UE. This value is only

 applicable to SM\_CONGESTION event.

 - LIST\_OF\_LOW\_EXP\_UE: Indicates list of low experienced UE. This value is only applicable to

 SM\_CONGESTION event.

 - AVG\_UL\_PKT\_DROP\_RATE: Indicates average uplink packet drop rate on GTP-U path on N3. This

 value is only applicable to RED\_TRANS\_EXP event.

 - VAR\_UL\_PKT\_DROP\_RATE: Indicates variance of uplink packet drop rate on GTP-U path on N3.

 This value is only applicable to RED\_TRANS\_EXP event.

 - AVG\_DL\_PKT\_DROP\_RATE: Indicates average downlink packet drop rate on GTP-U path on N3.

 This value is only applicable to RED\_TRANS\_EXP event.

 - VAR\_DL\_PKT\_DROP\_RATE: Indicates variance of downlink packet drop rate on GTP-U path on N3.

 This value is only applicable to RED\_TRANS\_EXP event.

 - AVG\_UL\_PKT\_DELAY: Indicates average uplink packet delay round trip on GTP-U path on N3.

 This value is only applicable to RED\_TRANS\_EXP event.

 - VAR\_UL\_PKT\_DELAY: Indicates variance uplink packet delay round trip on GTP-U path on N3.

 This value is only applicable to RED\_TRANS\_EXP event.

 - AVG\_DL\_PKT\_DELAY: Indicates average downlink packet delay round trip on GTP-U path on N3.

 This value is only applicable to RED\_TRANS\_EXP event.

 - VAR\_DL\_PKT\_DELAY: Indicates variance downlink packet delay round trip on GTP-U path on N3.

 This value is only applicable to RED\_TRANS\_EXP event.

 - TRAFFIC\_MATCH\_TD: Identifies traffic that matches Traffic Descriptor provided by

 the consumer.

 - TRAFFIC\_UNMATCH\_TD: Identifies traffic that does not match Traffic Descriptor

 provided by the consumer.

 - NUMBER\_OF\_UE: Indicates the number of UEs. This value is only applicable to

 DN\_PERFORMANCE event.

 - UE\_GEOG\_DIST: Indicates the geographical distribution of the UEs that can be selected by

 the AF for application service. This value is only applicable to UE\_MOBILITY event.

 - UE\_DIRECTION: Indicates the direction of the UEs. This value is only applicable to

 UE\_MOBILITY event.

 - USER\_LOCATION: Indicates the user location. This value is only applicable to UE\_MOBILITY

 event.

 - AVG\_E2E\_UL\_PKT\_DELAY: Indicates average End-to-End (between UE and UPF) uplink packet

 delay. This value is only applicable to RED\_TRANS\_EXP event.

 - VAR\_E2E\_UL\_PKT\_DELAY: Indicates the variance of End-to-End (between UE and UPF) uplink

 packet delay. This value is only applicable to RED\_TRANS\_EXP event.

 - AVG\_E2E\_DL\_PKT\_DELAY: Indicates average End-to-End (between UE and UPF) downlink packet

 delay. This value is only applicable to RED\_TRANS\_EXP event.

 - VAR\_E2E\_DL\_PKT\_DELAY: Indicates the variance of End-to-End (between UE and UPF) downlink

 packet delay. This value is only applicable to RED\_TRANS\_EXP event.

 - AVG\_E2E\_UL\_PKT\_LOSS\_RATE: Indicates average End-to-End (between UE and UPF) uplink packet

 loss rate. This value is only applicable to RED\_TRANS\_EXP event.

 - VAR\_E2E\_UL\_PKT\_LOSS\_RATE: Indicates the variance of End-to-End (between UE and UPF) uplink

 packet loss rate. This value is only applicable to RED\_TRANS\_EXP event.

 - AVG\_E2E\_DL\_PKT\_LOSS\_RATE: Indicates average End-to-End (between UE and UPF) downlink

 packet loss rate. This value is only applicable to RED\_TRANS\_EXP event.

 - VAR\_E2E\_DL\_PKT\_LOSS\_RATE: Indicates the variance of End-to-End (between UE and UPF)

 downlink packet loss rate. This value is only applicable to RED\_TRANS\_EXP event.

 - E2E\_DATA\_VOL\_TRANS\_TIME\_FOR\_UE\_LIST: Indicates the classified E2E data volume transfer

 time statistics or predictions for multiple UEs with respect to one or more reporting

 thresholds.

 - NUM\_OF\_UE: Indicates the total number of users in the area of interest. This

 value is only applicable to MOVEMENT\_BEHAVIOUR event.

 - MOV\_UE\_RATIO: Indicates the Ratio of moving UEs in the area of interest. This value

 is only applicable to MOVEMENT\_BEHAVIOUR event.

 - AVR\_SPEED: Indicates the average speed of all UEs in the area of interest. This value

 is only applicable to MOVEMENT\_BEHAVIOUR event.

 - SPEED\_THRESHOLD: Indicates the information on UEs in the area of interest whose speed

 is faster than the speed threshold. This value is only applicable to MOVEMENT\_BEHAVIOUR

 event.

 - MOV\_UE\_DIRECTION: Indicates the heading directions of the UE flow in the target area.

 This value is only applicable to MOVEMENT\_BEHAVIOUR event.

 - IN\_OUT\_PERCENT: Indicates the percentage of indoor/outdoor UEs at a location.

 The value is only applicable to the LOC\_ACCURACY event.

 DispersionType:

 oneOf:

 - type: string

 enum:

 - DVDA

 - TDA

 - DVDA\_AND\_TDA

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Represents the dispersion type.

 Possible values are:

 - DVDA: Data Volume Dispersion Analytics.

 - TDA: Transactions Dispersion Analytics.

 - DVDA\_AND\_TDA: Data Volume Dispersion Analytics and Transactions Dispersion Analytics.

 DispersionClass:

 oneOf:

 - type: string

 enum:

 - FIXED

 - CAMPER

 - TRAVELLER

 - TOP\_HEAVY

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Represents the dispersion class.

 Possible values are:

 - FIXED: Dispersion class as fixed UE its data or transaction usage at a location or

 a slice, is higher than its class threshold set for its all data or transaction usage.

 - CAMPER: Dispersion class as camper UE, its data or transaction usage at a location or

 a slice, is higher than its class threshold and lower than the fixed class threshold set

 for its all data or transaction usage.

 - TRAVELLER: Dispersion class as traveller UE, its data or transaction usage at a location

 or a slice, is lower than the camper class threshold set for its all data or transaction

 usage.

 - TOP\_HEAVY: Dispersion class as Top\_Heavy UE, who's dispersion percentile rating at a

 location or a slice, is higher than its class threshold.

 DispersionOrderingCriterion:

 anyOf:

 - type: string

 enum:

 - TIME\_SLOT\_START

 - DISPERSION

 - CLASSIFICATION

 - RANKING

 - PERCENTILE\_RANKING

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Represents the order criterion for the list of dispersion.

 Possible values are:

 - TIME\_SLOT\_START: Indicates the order of time slot start.

 - DISPERSION: Indicates the order of data/transaction dispersion.

 - CLASSIFICATION: Indicates the order of data/transaction classification.

 - RANKING: Indicates the order of data/transaction ranking.

 - PERCENTILE\_RANKING: Indicates the order of data/transaction percentile ranking.

 DeviceType:

 anyOf:

 - type: string

 enum:

 - MOBILE\_PHONE

 - SMART\_PHONE

 - TABLET

 - DONGLE

 - MODEM

 - WLAN\_ROUTER

 - IOT\_DEVICE

 - WEARABLE

 - MOBILE\_TEST\_PLATFORM

 - UNDEFINED

 - type: string

 description: >

 This string provides forward-compatibility with future extensions to the enumeration but

 is not used to encode content defined in the present version of this API.

 description: |

 Represents the device type.

 Possible values are:

 - MOBILE\_PHONE: Mobile Phone.

 - SMART\_PHONE: Smartphone.

 - TABLET: Tablet.

 - DONGLE: Dongle.

 - MODEM: Modem.

 - WLAN\_ROUTER: WLAN Router.

 - IOT\_DEVICE: IoT Device.

 - WEARABLE: Wearable.

 - MOBILE\_TEST\_PLATFORM: Mobile Test Platform.

 - UNDEFINED: Undefined.

 RedTransExpOrderingCriterion:

 anyOf:

 - type: string

 enum:

 - TIME\_SLOT\_START

 - RED\_TRANS\_EXP

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Represents the order criterion for the list of Redundant Transmission Experience.

 Possible values are:

 - TIME\_SLOT\_START: Indicates the order of time slot start.

 - RED\_TRANS\_EXP: Indicates the order of Redundant Transmission Experience.

 WlanOrderingCriterion:

 anyOf:

 - type: string

 enum:

 - TIME\_SLOT\_START

 - NUMBER\_OF\_UES

 - RSSI

 - RTT

 - TRAFFIC\_INFO

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Represents the order criterion for the list of WLAN performance information.

 Possible values are:

 - TIME\_SLOT\_START: Indicates the order of time slot start.

 - NUMBER\_OF\_UES: Indicates the order of number of UEs.

 - RSSI: Indicates the order of RSSI.

 - RTT: Indicates the order of RTT.

 - TRAFFIC\_INFO: Indicates the order of Traffic information.

 ServiceExperienceType:

 anyOf:

 - type: string

 enum:

 - VOICE

 - VIDEO

 - OTHER

 - type: string

 description: >

 This string provides forward-compatibility with future extensions to the enumeration

 but is not used to encode content defined in the present version of this API.

 description: |

 Represents the type of the service experience analytics.

 Possible values are:

 - VOICE: Indicates that the service experience analytics is for voice service.

 - VIDEO: Indicates that the service experience analytics is for video service.

 - OTHER: Indicates that the service experience analytics is for other service.

 DnPerfOrderingCriterion:

 anyOf:

 - type: string

 enum:

 - AVERAGE\_TRAFFIC\_RATE

 - MAXIMUM\_TRAFFIC\_RATE

 - AVERAGE\_PACKET\_DELAY

 - MAXIMUM\_PACKET\_DELAY

 - AVERAGE\_PACKET\_LOSS\_RATE

 - type: string

 description: >

 This string provides forward-compatibility with future extensions to the enumeration but

 is not used to encode content defined in the present version of this API.

 description: |

 Represents the order criterion for the list of DN performance analytics.

 Possible values are:

 - AVERAGE\_TRAFFIC\_RATE: Indicates the average traffic rate.

 - MAXIMUM\_TRAFFIC\_RATE: Indicates the maximum traffic rate.

 - AVERAGE\_PACKET\_DELAY: Indicates the average packet delay.

 - MAXIMUM\_PACKET\_DELAY: Indicates the maximum packet delay.

 - AVERAGE\_PACKET\_LOSS\_RATE: Indicates the average packet loss rate.

 TermCause:

 anyOf:

 - type: string

 enum:

 - USER\_CONSENT\_REVOKED

 - NWDAF\_OVERLOAD

 - UE\_LEFT\_AREA

 - type: string

 description: >

 This string provides forward-compatibility with future extensions to the enumeration but

 is not used to encode content defined in the present version of this API.

 description: |

 Represents the cause for the analytics subscription termination request.

 Possible values are:

 - USER\_CONSENT\_REVOKED: The user consent has been revoked.

 - NWDAF\_OVERLOAD: The NWDAF is overloaded.

 - UE\_LEFT\_AREA: The UE has moved out of the NWDAF serving area.

 UserDataConOrderCrit:

 anyOf:

 - type: string

 enum:

 - APPLICABLE\_TIME\_WINDOW

 - NETWORK\_STATUS\_INDICATION

 - type: string

 description: >

 This string provides forward-compatibility with future extensions to the enumeration but

 is not used to encode content defined in the present version of this API.

 description: |

 Represents the cause for requesting to terminate an analytics subscription.

 Possible values are:

 - APPLICABLE\_TIME\_WINDOW: The ordering criterion is the Applicable Time Window.

 - NETWORK\_STATUS\_INDICATION: The ordering criterion is the network status indication.

 UeMobilityOrderCriterion:

 anyOf:

 - type: string

 enum:

 - TIME\_SLOT

 - type: string

 description: >

 This string provides forward-compatibility with future extensions to the enumeration but

 is not used to encode content defined in the present version of this API.

 description: |

 Represents the ordering criterion for the list of UE mobility analytics.

 Possible values are:

 - TIME\_SLOT: The ordering criterion is the time slot.

 UeCommOrderCriterion:

 anyOf:

 - type: string

 enum:

 - START\_TIME

 - DURATION

 - type: string

 description: >

 This string provides forward-compatibility with future extensions to the enumeration but

 is not used to encode content defined in the present version of this API.

 description: |

 Represents the ordering criterion for the list of UE communication analytics.

 Possible values are:

 - START\_TIME: The ordering criterion of the analytics is the start time.

 - DURATION: The ordering criterion of the analytics is the duration of the communication.

 NetworkPerfOrderCriterion:

 anyOf:

 - type: string

 enum:

 - NUMBER\_OF\_UES

 - COMMUNICATION\_PERF

 - MOBILITY\_PERF

 - type: string

 description: >

 This string provides forward-compatibility with future extensions to the enumeration but

 is not used to encode content defined in the present version of this API.

 description: |

 Represents the ordering criterion for the list of network performance analytics.

 Possible values are:

 - NUMBER\_OF\_UES: The ordering criterion of the analytics is the number of UEs.

 - COMMUNICATION\_PERF: The ordering criterion of the analytics is the communication performance.

 - MOBILITY\_PERF: The ordering criterion of the analytics is themobility performance.

 LocInfoGranularity:

 anyOf:

 - type: string

 enum:

 - TA\_LEVEL

 - CELL\_LEVEL

 - LON\_AND\_LAT\_LEVEL

 - type: string

 description: >

 This string provides forward-compatibility with future extensions to the enumeration but

 is not used to encode content defined in the present version of this API.

 description: |

 Represents the preferred granularity of location information.

 Possible values are:

 - TA\_LEVEL: Indicates location granularity of TA level.

 - CELL\_LEVEL: Indicates location granularity of Cell level.

 - LON\_AND\_LAT\_LEVEL: Indicates location granularity of longitude and latitude level.

 TrafficDirection:

 anyOf:

 - type: string

 enum:

 - UL\_AND\_DL

 - UL

 - DL

 - type: string

 description: >

 This string provides forward-compatibility with future extensions to the enumeration but

 is not used to encode content defined in the present version of this API.

 description: |

 Represents the traffic direction for the resource usage information.

 Possible values are:

 - UL\_AND\_DL: Uplink and downlink traffic.

 - UL: Uplink traffic.

 - DL: Downlink traffic.

 ValueExpression:

 anyOf:

 - type: string

 enum:

 - AVERAGE

 - PEAK

 - type: string

 description: >

 This string provides forward-compatibility with future extensions to the enumeration but

 is not used to encode content defined in the present version of this API.

 description: |

 Represents the average or peak value of the resource usage for the network performance type.

 Possible values are:

 - AVERAGE: Resource usage information in average value.

 - PEAK: Resource usage information in peak value.

 E2eDataVolTransTimeCriterion:

 anyOf:

 - type: string

 enum:

 - TIME\_SLOT\_START

 - E2E\_DATA\_VOL\_TRANS\_TIME

 - type: string

 description: >

 This string provides forward-compatibility with future extensions to the enumeration but

 is not used to encode content defined in the present version of this API.

 description: |

 Represents the ordering criterion for the list of E2E data volume transfer time.

 Possible values are:

 - TIME\_SLOT\_START: Indicates the order of time slot start.

 - E2E\_DATA\_VOL\_TRANS\_TIME: The ordering criterion is the E2E data volume transfer time.

 AnalyticsAccuracyIndication:

 anyOf:

 - type: string

 enum:

 - MEET

 - NOT\_MEET

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Represents the notification methods for the subscribed events.

 Possible values are:

 - MEET: Indicates meet the analytics accuracy requirement.

 - NOT\_MEET: Indicates not meet the analytics accuracy requirement.

 LocationOrientation:

 anyOf:

 - type: string

 enum:

 - HORIZONTAL

 - VERTICAL

 - HOR\_AND\_VER

 - type: string

 description: >

 This string provides forward-compatibility with future extensions to the enumeration but

 is not used to encode content defined in the present version of this API.

 description: |

 Possible values are:

 - HORIZONTAL: Indicates horizontal orientation.

 - VERTICAL: Indicates vertical orientation.

 - HOR\_AND\_VER: Indicates both horizontal and vertical orientation.

 Direction:

 anyOf:

 - type: string

 enum:

 - NORTH

 - SOUTH

 - EAST

 - WEST

 - type: string

 description: >

 This string provides forward-compatibility with future extensions to the enumeration but

 is not used to encode content defined in the present version of this API.

 description: |

 Possible values are:

 - NORTH: North direction.

 - SOUTH: South direction.

 - EAST: EAST direction.

 - WEST: WEST direction.

\*\*\* End of Changes \*\*\*