**3GPP TSG-CT WG3 Meeting #130 C3-234436**

**Xiamen, China, 9 - 13 October,2023 (Revision of C3-23xxxx)**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.522** | **CR** | **1097** | **rev** | **-** | **Current version:** | **18.3.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Updates to Member UE Selection procedures | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Ericsson | | | | | | | | | |
| ***Source to TSG:*** | CT3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | AIMLsys | | | | |  | ***Date:*** | | | 2023-09-15 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | The Member UE Selection Procedures needed to be updated, since the referred data type is not the procedures. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Updates the Member UE Selection procedures. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Member UE Selection procedures is not completely well described. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 4.4.36.2, 4.4.36.3 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR does not impact the OpenAPI file. | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

**Additional discussion(if needed):**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

#### 4.4.36.2 Procedure for Member UE Selection Assistance Subscription Creation

In order to subscribe to receive the Member UE selection assistance information, the AF shall send an HTTP POST request message to the NEF targeting the "Member UE Selection Assistance Subscriptions" collection resource, with the request message body including the MemUeSelectAssistSubsc data structure, as specified in clause 5.32.5.2.2.

The NEF shall then check whether the AF is authorized to perform this operation or not. If the AF is authorized and based on the Member UE filtering criteria provided by the AF, the NEF shall then interact with different 5GC NFs via the services offered by the 5GC NFs as specified.

Upon reception of a successful response from the 5GC NF, the NEF shall respond to the AF with a "201 Created" status code including a "Location" header field that shall contain the URI of the created resource, i.e. "{apiRoot}/3gpp-umsa/v1/{afId}/subscriptions/{subscriptionId}", and the response body containing a representation of the created "Individual Member UE Selection Assistance Subscription" resource within the MemUeSelectAssistSubsc data structure as specified in clause 5.32.2.2.2.

On failure or if the NEF receives an error response from the 5GC NF, the NEF shall take proper error handling actions, as specified in clause 5.32.7, and respond to the AF with an appropriate error status code. If the NEF received within an error response a "ProblemDetails" data structure with a "cause" attribute indicating an application error, the NEF shall relay this error response to the AF with a corresponding application error, when applicable.

\*\*\* 2nd Change \*\*\*

#### 4.4.36.3 Procedure for Member UE Selection Assistance Subscription Update

In order to update an existing Individual Member UE Selection Assistance Subscription, the AF shall send an HTTP PUT request message to the NEF targeting the "Individual Member UE Selection Assistance Subscription" resource, with the request message body including the MemUeSelectAssistSubsc data structure as specified in clause 5.32.5.2.2.

The NEF shall then check whether the AF is authorized to perform this operation or not. If the AF is authorized and based on the Member UE filtering criteria provided by the AF, the NEF shall then interact with different 5GC NFs via the services offered by the 5GC NFs as specified in.

Upon reception of a successful response from the 5GC NF, the NEF shall respond to the AF with a "200 OK" status code with the MemUeSelectAssistSubsc data structure or "204 No Content" status code, as specified in clause 5.32.2.3.3.

On failure or if the NEF receives an error response from the 5GC NF, the NEF shall take proper error handling actions, as specified in clause 5.32.7, and respond to the AF with an appropriate error status code. If the NEF received within an error response a "ProblemDetails" data structure with a "cause" attribute indicating an application error, the NEF shall relay this error response to the AF with a corresponding application error, when applicable.

\*\*\* End of Changes \*\*\*