**3GPP TSG-CT3 Meeting #130C3-234547**

**Xiamen, China, 9 - 13 October, 2023 (Revision of C3-234168)**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **29.558** | **CR** | **0128** | **rev** | **1** | **Current version:** | **17.4.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Corrections to boolean type definitions |
|  |  |
| ***Source to WG:*** | Ericsson |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | EDGEAPP |  | ***Date:*** | 2023-09-20 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** |  Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | The boolean type definitions in this TS missing several essential definitions. The false definition is missing in the easAckInd attribute within the AcrMgntEventSubsc data type. The default value definition is missing in the eecRegConf attribute of the EESProfile type. Some boolean type also missing the corresponding descriptions in the OpenAPI file.Hence needs to correct the boolean type definitions in this TS. |
|  |  |
| ***Summary of change:*** | Adding the missing default value definition for the eecRegConf attributes within the EESProfile which is also updated in the OpenAPI fileAdding the corresponding API |
|  |  |
| ***Consequences if not approved:*** | Missing the essential boolean type definitions in Eees\_ACRManagementEvent API and Eecs\_EESRegistration API will arouse wrong implemenation and wrong deployments. |
|  |  |
| ***Clauses affected:*** | 8.6.5.2.3, 9.1.5.2.3, A.7, A.11 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR introduces backwards compatible corrections in the OpenAPI files of the Eees\_ACRManagementEvent API and Eecs\_EESRegistration API. |
|  |  |
| ***This CR's revision history:*** |  |

**Additional discussion(if needed):**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

##### 8.6.5.2.3 Type: AcrMgntEventSubsc

Table 8.6.5.2.3-1: Definition of type AcrMgntEventSubsc

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| event | AcrMgntEvent | M | 1 | Indicates the subscribed ACR management event. |  |
| eventFilter | AcrMgntEventFilter | O | 0..1 | Represents the event filter for the subscribed ACR management event.This attribute may be provided only if the "event" attribute is set to "ACR\_MONITORING". |  |
| evtReq | ReportingInformation | O | 0..1 | Indicates the event reporting requirements (e.g. reporting periodicity, immediate reporting indication, etc).(NOTE) |  |
| tgtUeId | TargetUeIdentification | C | 0..1 | Contains the UE identification information.This attribute shall be provided only if the "event" attribute is set to either "UP\_PATH\_CHG", "ACR\_MONITORING" or "ACR\_FACILITATION". |  |
| dnaiChgType | DnaiChangeType | O | 0..1 | Identifies a type of notification regarding UP path management event.This attribute may be provided only if the "event" attribute is set to "UP\_PATH\_CHG". |  |
| easAckInd | boolean | O | 0..1 | Identifies whether EAS acknowledgement of UP path change event notifications is to be expected.Set to "true" if the EAS acknowledgement is expected. Set to "false" if the EAS acknowledgement is not expected.Default value is "false".This attribute may be provided only if the "event" attribute is set to "UP\_PATH\_CHG". |  |
| easChars | array(EasCharacteristics) | O | 1..N | Represents a list of EAS characteristics.This attribute may be provided only if the "event" attribute is set to either "ACR\_MONITORING" or "ACR\_FACILITATION". |  |
| NOTE: The "evtReq" takes precedence over the "evtReq" attribute of the AcrMgntEventsSubscription data structure when both are present. |

\*\*\* 2nd Change \*\*\*

##### 9.1.5.2.3 Type: EESProfile

Table 9.1.5.2.3-1: Definition of type EESProfile

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| eesId | string | M | 1 | The identifier of the EES |  |
| endPt | EndPoint | M | 1 | Endpoint information (e.g. URI, FQDN, IP address) used to communicate with the EES. This information is provided to the EEC to connect to the EES.  |  |
| easIds | array(string) | O | 1..N | The application identities of the Edge Application Servers, e.g. URI, FQDN, registered with the EES.  |  |
| provId | string | O | 0..1 | Identifier of the ECSP that provides the EES provider. |  |
| svcArea | ServiceArea | O | 0..1 | The list of geographical and topological areas that the EES serves. EECs in the UE that are outside the area shall not be served. |  |
| appLocs | array(Dnai) | O | 1..N | List of DNAI(s) associated with the EES. This is a list of potential locations of the applications.It is a subset of the DNAI(s) associated with the EDN, where the EES resides. |  |
| svcContSupp | array(ACRScenario) | O | 1..N | The ACR scenarios supported by the EES for service continuity. If this attribute is not present, then the EES does not support service continuity. |  |
| eecRegConf | boolean | M | 1 | Set to "true" if the EEC is required to register on the EES to use edge services. Set to "false" if EEC is not required to register on the EES to use edge services. Default value is "false". |  |

\*\*\* 3rd Change \*\*\*

# A.7 Eees\_ACRManagementEvent API

openapi: 3.0.0

info:

 title: EES ACR Management Event\_API

 description: |

 API for EES ACR Management Event.

 © 2023, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

 version: 1.0.4

externalDocs:

 description: >

 3GPP TS 29.558 V17.4.0 Enabling Edge Applications;

 Application Programming Interface (API) specification; Stage 3

 url: https://www.3gpp.org/ftp/Specs/archive/29\_series/29.558/

security:

 - {}

 - oAuth2ClientCredentials: []

servers:

 - url: '{apiRoot}/eees-acrmgntevent/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in clause 7.5 of 3GPP TS 29.558.

paths:

 /subscriptions:

 post:

 description: Create an Individual ACR Management Event Subscription resource.

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/AcrMgntEventsSubscription'

 callbacks:

 ACRManagementEventsNotification:

 '{request.body#/notificationDestination}':

 post:

 requestBody: # contents of the callback message

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/AcrMgntEventsNotification'

 responses:

 '204':

 description: No Content (successful notification)

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 UPPathChangeAvailabilityNotif:

 '{request.body#/notificationDestination}/report-availability':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/AvailabilityNotif'

 responses:

 '204':

 description: No Content. The notification is successful received.

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 responses:

 '201':

 description: Created (Successful creation)

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/AcrMgntEventsSubscription'

 headers:

 Location:

 description: 'Contains the URI of the newly created resource'

 required: true

 schema:

 type: string

 '204':

 description: >

 Successful case. The resource has been successfully created and no

 additional content is to be sent in the response message.

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 get:

 description: Retrieve all the ACR Management Events Subscriptions information.

 parameters:

 - name: supp-feat

 in: query

 description: Features supported by the EAS.

 required: false

 schema:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 responses:

 '200':

 description: OK (Successful get all of the active subscriptions)

 content:

 application/json:

 schema:

 type: array

 items:

 $ref: '#/components/schemas/AcrMgntEventsSubscription'

 minItems: 1

 description: All the active ACR management events subscriptions

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/406'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 /subscriptions/{subscriptionId}:

 get:

 description: Retrieve an Individual ACR Management Events Subscription.

 parameters:

 - name: subscriptionId

 in: path

 description: Subscription Id.

 required: true

 schema:

 type: string

 - name: supp-feat

 in: query

 description: Features supported by the EAS.

 required: false

 schema:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 responses:

 '200':

 description: OK (Successful get the active subscription).

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/AcrMgntEventsSubscription'

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/406'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 put:

 description: Fully replace an existing Individual ACR Management Events Subscription.

 parameters:

 - name: subscriptionId

 in: path

 description: Subscription Id.

 required: true

 schema:

 type: string

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/AcrMgntEventsSubscription'

 responses:

 '200':

 description: OK (Successful get the active subscription).

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/AcrMgntEventsSubscription'

 '204':

 description: No Content

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 patch:

 parameters:

 - name: subscriptionId

 in: path

 description: Subscription Id.

 required: true

 schema:

 type: string

 requestBody:

 description: Partial update an existing Individual ACR Management Events Subscription.

 required: true

 content:

 application/merge-patch+json:

 schema:

 $ref: '#/components/schemas/AcrMgntEventsSubscriptionPatch'

 responses:

 '200':

 description: >

 The Individual ACR Management Events Subscription is successfully modified

 and the updated subscription information is returned in the response.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/AcrMgntEventsSubscription'

 '204':

 description: No Content.

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 delete:

 description: Delete an existing Individual ACR Management Events Subscription.

 parameters:

 - name: subscriptionId

 in: path

 description: Subscription Id.

 required: true

 schema:

 type: string

 responses:

 '204':

 description: The individual subscription is deleted.

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

# Components

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{tokenUrl}'

 scopes: {}

 schemas:

 AcrMgntEventsSubscription:

 type: object

 description: Represents an Individual ACR Management Events Subscription.

 properties:

 self:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Uri'

 easId:

 type: string

 description: Identifier of an EAS.

 eventSubscs:

 type: array

 items:

 $ref: '#/components/schemas/AcrMgntEventSubsc'

 minItems: 1

 description: The subscribed ACR management events.

 evtReq:

 $ref: 'TS29523\_Npcf\_EventExposure.yaml#/components/schemas/ReportingInformation'

 notificationDestination:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Uri'

 eventReports:

 type: array

 items:

 $ref: '#/components/schemas/AcrMgntEventReport'

 minItems: 1

 description: The ACR management event report(s).

 availabilityInfo:

 $ref: '#/components/schemas/AvailabilityNotif'

 failEventReports:

 type: array

 items:

 $ref: '#/components/schemas/FailureAcrMgntEventInfo'

 minItems: 1

 description: Failure event reports.

 requestTestNotification:

 type: boolean

 description: >

 Set to true by the EAS to request the EES to send a test notification.

 Set to false or omitted otherwise.

 websockNotifConfig:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/WebsockNotifConfig'

 suppFeat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 required:

 - easId

 - eventSubscs

 - notificationDestination

 AcrMgntEventSubsc:

 type: object

 description: Represents an ACR Management Event Subscription.

 properties:

 event:

 $ref: '#/components/schemas/AcrMgntEvent'

 eventFilter:

 $ref: '#/components/schemas/AcrMgntEventFilter'

 evtReq:

 $ref: 'TS29523\_Npcf\_EventExposure.yaml#/components/schemas/ReportingInformation'

 tgtUeId:

 $ref: '#/components/schemas/TargetUeIdentification'

 dnaiChgType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DnaiChangeType'

 easAckInd:

 type: boolean

 description: >

 Identifies whether EAS acknowledgement of UP path change event notifications is to

 be expected. Set to "true" if the EAS acknowledgement is expected. Set to "false" if

 the EAS acknowledgement is not expected. Default value is "false" if ommited.

 easChars:

 type: array

 items:

 $ref: 'TS24558\_Eees\_EASDiscovery.yaml#/components/schemas/EasCharacteristics'

 minItems: 1

 description: A list of EAS characteristics.

 required:

 - event

 AcrMgntEventsSubscriptionPatch:

 type: object

 description: >

 Represents a modification request of Individual ACR Management Events Subscription.

 properties:

 eventSubscs:

 type: array

 items:

 $ref: '#/components/schemas/AcrMgntEventSubsc'

 minItems: 1

 description: The subscribed ACR management events.

 evtReq:

 $ref: 'TS29523\_Npcf\_EventExposure.yaml#/components/schemas/ReportingInformation'

 notificationDestination:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Uri'

 AcrMgntEventsNotification:

 type: object

 description: Represents the ACR management events notification.

 properties:

 subpId:

 type: string

 description: >

 String identifying the Individual ACR Management Events Subscription

 for which the notification is delivered.

 eventReports:

 type: array

 items:

 $ref: '#/components/schemas/AcrMgntEventReport'

 minItems: 1

 description: A list of ACR management event reports.

 required:

 - subpId

 - eventReports

 AcrMgntEventReport:

 type: object

 description: Represents an ACR management event report.

 properties:

 event:

 $ref: '#/components/schemas/AcrMgntEvent'

 timeStamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 upPathChgInfo:

 $ref: '#/components/schemas/UpPathChangeInfo'

 easEndPoint:

 $ref: 'TS29558\_Eees\_EASRegistration.yaml#/components/schemas/EndPoint'

 actStatus:

 $ref: '#/components/schemas/ActStatus'

 acId:

 type: string

 required:

 - event

 FailureAcrMgntEventInfo:

 type: object

 description: Represents a failure ACR management event.

 properties:

 event:

 $ref: '#/components/schemas/AcrMgntEvent'

 failureCode:

 $ref: '#/components/schemas/AcrMgntEventFailureCode'

 required:

 - event

 - failureCode

 TargetUeIdentification:

 description: Identifies the target UE information.

 type: object

 properties:

 gpsi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 intGrpId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 extGrpId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ExternalGroupId'

 ueIpAddr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/IpAddr'

 oneOf:

 - required: [gpsi]

 - required: [intGrpId]

 - required: [extGrpId]

 - required: [ueIpAddr]

 AvailabilityNotif:

 type: object

 description: >

 Represents the availability information of user plane path management events monitoring

 via the 3GPP 5GC network.

 properties:

 availabilityStatus:

 $ref: '#/components/schemas/AvailabilityStatus'

 required:

 - availabilityStatus

 UpPathChangeInfo:

 description: Represents user plane path change information.

 type: object

 properties:

 ueId:

 $ref: '#/components/schemas/IndUeIdentification'

 dnaiChgType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DnaiChangeType'

 sourceTrafficRoute:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RouteToLocation'

 targetTrafficRoute:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RouteToLocation'

 sourceDnai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnai'

 targetDnai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnai'

 srcUeIpv4Addr:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv4Addr'

 srcUeIpv6Prefix:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

 tgtUeIpv4Addr:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv4Addr'

 tgtUeIpv6Prefix:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

 required:

 - ueId

 - dnaiChgType

 IndUeIdentification:

 description: Represents identification information of a UE.

 type: object

 properties:

 gpsi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 externalId:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

 ueIpAddr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/IpAddr'

 oneOf:

 - required: [gpsi]

 - required: [externalId]

 - required: [ueIpAddr]

 AcrMgntEvent:

 anyOf:

 - type: string

 enum:

 - UP\_PATH\_CHG

 - ACR\_MONITORING

 - ACR\_FACILITATION

 - ACT\_START\_STOP

 - type: string

 description: >

 This string represents the ACR management.

 description: |

 Possible values are:

 - UP\_PATH\_CHG: User plane path change event.

 - ACR\_MONITORING: ACR monitoring event.

 - ACR\_FACILITATION: ACR facilitation event.

 - ACT\_START\_STOP: ACT start/stop event.

 AcrMgntEventFilter:

 anyOf:

 - type: string

 enum:

 - INTRA\_EDN\_MOBILITY

 - INTER\_EDN\_MOBILITY

 - type: string

 description: >

 This string represents the ACR Management Event filter.

 description: |

 Possible values are:

 - INTRA\_EDN\_MOBILITY: Indicates that the ACR Management Event filter is intra-EDN mobility.

 - INTER\_EDN\_MOBILITY: Indicates that the ACR Management Event filter is inter-EDN mobility.

 ActStatus:

 anyOf:

 - type: string

 enum:

 - ACT\_START

 - ACT\_STOP

 - type: string

 description: >

 This string represents the ACT status, i.e. ACT start or stop.

 description: |

 Possible values are:

 - ACT\_START: Indicates ACT start.

 - ACT\_STOP: Indicates ACT stop.

 AcrMgntEventFailureCode:

 anyOf:

 - type: string

 enum:

 - 3GPP\_UP\_PATH\_CHANGE\_MON\_NOT\_AVAILABLE

 - OTHER\_REASONS

 - type: string

 description: >

 This string represents the reason for ACR Management subscription failure for an event.

 description: |

 Possible values are:

 - 3GPP\_UP\_PATH\_CHANGE\_MON\_NOT\_AVAILABLE: Indicates that the ACR Management Event

 Subscription failed because user plane path management event notifications from the 3GPP

 network is NOT available. This value is only applicable for the "UP\_PATH\_CHG",

 "ACR\_MONITORING" and "ACR\_FACILITATION" events.

 - OTHER\_REASONS: Indicates that the ACR Management Event Subscription failed for other

 reasons. This value is applicable for all events.

 AvailabilityStatus:

 anyOf:

 - type: string

 enum:

 - AVAILABLE

 - NOT\_AVAILABLE

 - type: string

 description: >

 This string represents the availability status.

 description: |

 Possible values are:

 - AVAILABLE: Indicates availability.

 - NOT\_AVAILABLE: Indicates unavailability.

\*\*\* 4th Change \*\*\*

# A.11 Eecs\_EESRegistration API

openapi: 3.0.0

info:

 title: ECS EES Registration\_API

 description: |

 API for EES Registration.

 © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

 version: 1.0.1

externalDocs:

 description: >

 3GPP TS 29.558 V17.1.0 Enabling Edge Applications;

 Application Programming Interface (API) specification; Stage 3

 url: https://www.3gpp.org/ftp/Specs/archive/29\_series/29.558/

security:

 - {}

 - oAuth2ClientCredentials: []

servers:

 - url: '{apiRoot}/eecs-eesregistration/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in clause 7.5 of 3GPP TS 29.558.

paths:

 /registrations:

 post:

 description: Registers a new EES at the Edge Configuration Server.

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/EESRegistration'

 responses:

 '201':

 description: EES information is registered successfully at ECS.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/EESRegistration'

 headers:

 Location:

 description: 'Contains the URI of the newly created resource'

 required: true

 schema:

 type: string

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 /registrations/{registrationId}:

 get:

 description: Retrieve an Individual EES registration resource.

 parameters:

 - name: registrationId

 in: path

 description: Registration Id.

 required: true

 schema:

 type: string

 responses:

 '200':

 description: OK (The EES registration information at the Edge Configuration Server).

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/EESRegistration'

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/406'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 put:

 description: Fully replace an existing EES Registration resource.

 parameters:

 - name: registrationId

 in: path

 description: EES Registration Id.

 required: true

 schema:

 type: string

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/EESRegistration'

 responses:

 '200':

 description: OK (The EES registration information is updated successfully).

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/EESRegistration'

 '204':

 description: >

 No Content. The individual EES registration information is updated successfully.

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 patch:

 description: Partially update an existing EES Registration resource.

 parameters:

 - name: registrationId

 in: path

 description: EES registration Id.

 required: true

 schema:

 type: string

 requestBody:

 description: Partial update an existing EES registration resource.

 required: true

 content:

 application/merge-patch+json:

 schema:

 $ref: '#/components/schemas/EESRegistrationPatch'

 responses:

 '200':

 description: >

 The Individual EES registration is successfully modified and

 the updated registration information is returned in the response.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/EESRegistration'

 '204':

 description: >

 No Content. The individual EES registration information is updated successfully.

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 delete:

 description: Delete an existing EES registration at ECS.

 parameters:

 - name: registrationId

 in: path

 description: Registration Id.

 required: true

 schema:

 type: string

 responses:

 '204':

 description: The individual EES registration is deleted.

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{tokenUrl}'

 scopes: {}

 schemas:

 EESRegistration:

 type: object

 description: Represents an EES registration information.

 properties:

 eesProf:

 $ref: '#/components/schemas/EESProfile'

 expTime:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

 suppFeat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 required:

 - eesProf

 EESProfile:

 type: object

 description: Represents the EES profile information.

 properties:

 eesId:

 type: string

 description: Identifier of the EES.

 endPt:

 $ref: 'TS29558\_Eees\_EASRegistration.yaml#/components/schemas/EndPoint'

 easIds:

 type: array

 items:

 type: string

 minItems: 1

 description: Application identifiers of EASs that are registered with EES.

 provId:

 type: string

 description: Identifier of the ECSP that provides the EES provider.

 svcArea:

 $ref: '#/components/schemas/ServiceArea'

 appLocs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnai'

 minItems: 1

 description: List of DNAI(s) associated with the EES.

 svcContSupp:

 type: array

 items:

 $ref: '#/components/schemas/ACRScenario'

 minItems: 1

 description: The ACR scenarios supported by the EES for service continuity.

 eecRegConf:

 type: boolean

 description: >

 Set to true if the EEC is required to register to the EES to use edge service.

 Set to false if the EEC is not required to register to use edge services. Default

 value is false.

 required:

 - eesId

 - endPt

 - eecRegConf

 EESRegistrationPatch:

 type: object

 description: Represents partial update request of individual EES registration information.

 properties:

 eesProf:

 $ref: '#/components/schemas/EESProfile'

 expTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTimeRm'

 ServiceArea:

 type: object

 description: Represents a service area information of the EdgeApp entity.

 properties:

 topServAr:

 $ref: '#/components/schemas/TopologicalServiceArea'

 geoServAr:

 $ref: '#/components/schemas/GeographicalServiceArea'

 TopologicalServiceArea:

 type: object

 description: Represents topological service area information.

 properties:

 ecgis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ecgi'

 minItems: 1

 description: A list of E-UTRA cell identities.

 ncgis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ncgi'

 minItems: 1

 description: A list of NR cell identities.

 tais:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Tai'

 minItems: 1

 description: A list of tracking area identities.

 plmnIds:

 type: array

 items:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/PlmnId'

 minItems: 1

 description: A list of PLMN identities.

 GeographicalServiceArea:

 type: object

 description: Represents geographical service area information.

 properties:

 geoArs:

 type: array

 items:

 $ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/GeographicArea'

 minItems: 1

 description: A list of geographic area information.

 civicAddrs:

 type: array

 items:

 $ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/CivicAddress'

 minItems: 1

 description: A list of civic address information.

 ACRScenario:

 anyOf:

 - type: string

 enum:

 - EEC\_INITIATED

 - EEC\_EXECUTED\_VIA\_SOURCE\_EES

 - EEC\_EXECUTED\_VIA\_TARGET\_EES

 - SOURCE\_EAS\_DECIDED

 - SOURCE\_EES\_EXECUTED

 - EEL\_MANAGED\_ACR

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Possible values are:

 - EEC\_INITIATED: Represents the EEC initiated ACR scenario.

 - EEC\_EXECUTED\_VIA\_SOURCE\_EES: Represents the EEC ACR scenario executed via the S-EES.

 - EEC\_EXECUTED\_VIA\_TARGET\_EES: Represents the EEC ACR scenario executed via the T-EES.

 - SOURCE\_EAS\_DECIDED: Represents the EEC ACR scenario where the S-EAS decides to perform ACR.

 - SOURCE\_EES\_EXECUTED: Represents the EEC ACR scenario where S-EES executes the ACR.

 - EEL\_MANAGED\_ACR: Represents the EEC ACR scenario where the ACR is managed by the Edge Enabler Layer.

\*\*\* End of Changes \*\*\*