**3GPP TSG-CT3 Meeting #130C3-234xxx**

**Xiamen, China, 9th – 13th October 2023 was C3-234145**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.558** | **CR** | **0126** | **rev** | **1** | **Current version:** | **18.3.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | |
| ***Title:*** | Complete the definition of the ACR Selection event | | | | | | | | |
|  |  | | | | | | | | |
| ***Source to WG:*** | Huawei, Ericsson | | | | | | | | |
| ***Source to TSG:*** | CT3 | | | | | | | | |
|  |  | | | | | | | | |
| ***Work item code:*** | EDGEAPP\_Ph2 | | | | |  | ***Date:*** | | 2023-09-29 |
|  |  | | | |  | |  | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | |
| ***Reason for change:*** | | | There is one remaining Editor's Note in clauses 8.6.5.3.3 on the definition of the ACR facilitation event. As per the latest progress of the corresponding stage 2 requirements, there is no need to keep this Editor's Note.  Also, this new event is not yet added in the corresponding OpenAPI description. | | | | | | |
|  | | |  | | | | | | |
| ***Summary of change:*** | | | This CR proposes to:   * Remove this remaining Editor's Note in clauses 8.6.5.3.3. * Add the ACR selection event to the corresponding OpenAPI description. | | | | | | |
|  | | |  | | | | | | |
| ***Consequences if not approved:*** | | | * The definition of the the ACR Facilitation event is not completed in stage 3. | | | | | | |
|  | |  | | | | | | | |
| ***Clauses affected:*** | | 8.6.5.3.3, A.7 | | | | | | | |
|  | |  | | | | | | | |
|  | | **Y** | | **N** |  | | |  | |
| ***Other specs*** | |  | | **X** | Other core specifications | | | TS/TR ... CR ... | |
| ***affected:*** | |  | | **X** | Test specifications | | | TS/TR ... CR ... | |
| ***(show related CRs)*** | |  | | **X** | O&M Specifications | | | TS/TR ... CR ... | |
|  | |  | | | | | | | |
| ***Other comments:*** | | This CR introduces a backwards compatible new feature to the OpenAPI description of the Eees\_ACRManagementEvent API defined in this specification. | | | | | | | |
|  | |  | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | |

\* \* \* \* Start of changes \* \* \* \*

##### 8.6.5.3.3 Enumeration: AcrMgntEvent

Table 8.6.5.3.3-1: Enumeration AcrMgntEvent

|  |  |  |
| --- | --- | --- |
| Enumeration value | Description | Applicability |
| UP\_PATH\_CHG | Indicates that the ACR Management Event is user plane path change. |  |
| ACR\_MONITORING | Indicates that the ACR Management Event is ACR monitoring. |  |
| ACR\_FACILITATION | Indicates that the ACR Management Event is ACR facilitation. |  |
| ACT\_START\_STOP | Indicates that the ACR Management Event is ACT start/stop. |  |
| ACR\_SELECTION | Indicates that the ACR Management Event is ACR selection. | EdgeApp\_2 |

\* \* \* \* Next changes \* \* \* \*

# A.7 Eees\_ACRManagementEvent API

openapi: 3.0.0

info:

title: EES ACR Management Event\_API

description: |

API for EES ACR Management Event.

© 2023, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

version: 1.1.0-alpha.4

externalDocs:

description: >

3GPP TS 29.558 V18.3.0 Enabling Edge Applications;

Application Programming Interface (API) specification; Stage 3

url: https://www.3gpp.org/ftp/Specs/archive/29\_series/29.558/

security:

- {}

- oAuth2ClientCredentials: []

servers:

- url: '{apiRoot}/eees-acrmgntevent/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 7.5 of 3GPP TS 29.558.

paths:

/subscriptions:

post:

summary: Creates a new Individual ACR Management Events Subscription

operationId: CreateACRMngEventSubscr

tags:

- ACR Management Events Subscriptions (Collection)

description: Create an Individual ACR Management Event Subscription resource.

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/AcrMgntEventsSubscription'

callbacks:

ACRManagementEventsNotification:

'{request.body#/notificationDestination}':

post:

requestBody: # contents of the callback message

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/AcrMgntEventsNotification'

responses:

'204':

description: No Content (successful notification)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

UPPathChangeAvailabilityNotif:

'{request.body#/notificationDestination}/report-availability':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/AvailabilityNotif'

responses:

'204':

description: No Content. The notification is successful received.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

responses:

'201':

description: Created (Successful creation)

content:

application/json:

schema:

$ref: '#/components/schemas/AcrMgntEventsSubscription'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'204':

description: >

Successful case. The resource has been successfully created and no

additional content is to be sent in the response message.

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

get:

summary: Read all ACR Management Events Subscriptions

operationId: GetACRMngEventSubscrs

tags:

- ACR Management Events Subscriptions (Collection)

description: Retrieve all the ACR Management Events Subscriptions information.

parameters:

- name: supp-feat

in: query

description: Features supported by the EAS.

required: false

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

responses:

'200':

description: OK (Successful get all of the active subscriptions)

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/AcrMgntEventsSubscription'

minItems: 1

description: All the active ACR management events subscriptions

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/subscriptions/{subscriptionId}:

get:

summary: Read an Individual ACR Management Events Subscription

operationId: GetIndACRMngEventSubscr

tags:

- Individual ACR Management Events Subscription (Document)

description: Retrieve an Individual ACR Management Events Subscription.

parameters:

- name: subscriptionId

in: path

description: Subscription Id.

required: true

schema:

type: string

- name: supp-feat

in: query

description: Features supported by the EAS.

required: false

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

responses:

'200':

description: OK (Successful get the active subscription).

content:

application/json:

schema:

$ref: '#/components/schemas/AcrMgntEventsSubscription'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

put:

summary: Update an Individual ACR Management Events Subscription

operationId: UpdateIndACRMngEventSubscr

tags:

- Individual ACR Management Events Subscription (Document)

description: Fully replace an existing Individual ACR Management Events Subscription.

parameters:

- name: subscriptionId

in: path

description: Subscription Id.

required: true

schema:

type: string

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/AcrMgntEventsSubscription'

responses:

'200':

description: OK (Successful get the active subscription).

content:

application/json:

schema:

$ref: '#/components/schemas/AcrMgntEventsSubscription'

'204':

description: No Content

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

patch:

summary: Modify an Individual ACR Management Events Subscription

operationId: ModifyIndACRMngEventSubscr

tags:

- Individual ACR Management Events Subscription (Document)

parameters:

- name: subscriptionId

in: path

description: Subscription Id.

required: true

schema:

type: string

requestBody:

description: Partial update an existing Individual ACR Management Events Subscription.

required: true

content:

application/merge-patch+json:

schema:

$ref: '#/components/schemas/AcrMgntEventsSubscriptionPatch'

responses:

'200':

description: >

The Individual ACR Management Events Subscription is successfully modified

and the updated subscription information is returned in the response.

content:

application/json:

schema:

$ref: '#/components/schemas/AcrMgntEventsSubscription'

'204':

description: No Content.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

summary: Delete an Individual ACR Management Events Subscription

operationId: DeleteIndACRMngEventSubscr

tags:

- Individual ACR Management Events Subscription (Document)

description: Delete an existing Individual ACR Management Events Subscription.

parameters:

- name: subscriptionId

in: path

description: Subscription Id.

required: true

schema:

type: string

responses:

'204':

description: The individual subscription is deleted.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

# Components

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{tokenUrl}'

scopes: {}

schemas:

AcrMgntEventsSubscription:

type: object

description: Represents an Individual ACR Management Events Subscription.

properties:

self:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Uri'

easId:

type: string

description: Identifier of an EAS.

eventSubscs:

type: array

items:

$ref: '#/components/schemas/AcrMgntEventSubsc'

minItems: 1

description: The subscribed ACR management events.

evtReq:

$ref: 'TS29523\_Npcf\_EventExposure.yaml#/components/schemas/ReportingInformation'

notificationDestination:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Uri'

eventReports:

type: array

items:

$ref: '#/components/schemas/AcrMgntEventReport'

minItems: 1

description: The ACR management event report(s).

availabilityInfo:

$ref: '#/components/schemas/AvailabilityNotif'

failEventReports:

type: array

items:

$ref: '#/components/schemas/FailureAcrMgntEventInfo'

minItems: 1

description: Failure event reports.

requestTestNotification:

type: boolean

description: >

Set to true by the EAS to request the EES to send a test notification.

Set to false or omitted otherwise.

websockNotifConfig:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/WebsockNotifConfig'

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

required:

- easId

- eventSubscs

- notificationDestination

AcrMgntEventSubsc:

type: object

description: Represents an ACR Management Event Subscription.

properties:

event:

$ref: '#/components/schemas/AcrMgntEvent'

eventFilter:

$ref: '#/components/schemas/AcrMgntEventFilter'

evtReq:

$ref: 'TS29523\_Npcf\_EventExposure.yaml#/components/schemas/ReportingInformation'

tgtUeId:

$ref: '#/components/schemas/TargetUeIdentification'

dnaiChgType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DnaiChangeType'

easAckInd:

type: boolean

description: >

Identifies whether EAS acknowledgement of UP path change event notifications is to be

expected. Set to "true" if the EAS acknowledgement is expected. Default value is

"false". This attribute may be provided only if the "event" attribute is set to

"UP\_PATH\_CHG".

easChars:

type: array

items:

$ref: 'TS24558\_Eees\_EASDiscovery.yaml#/components/schemas/EasCharacteristics'

minItems: 1

description: A list of EAS characteristics.

trafFilterInfo:

$ref: '#/components/schemas/TrafficFilterInfo'

servContPlanInd:

type: boolean

description: >

Represents the service continuity planning indication (i.e., whether or not the EES

shall monitor whether the UE(s) enter the predicted location).

When set to true, it indicates that service continuity planning is required.

When set to false, it indicates that Service continuity planning is not required.

The default value when this attribute is omitted is false.

required:

- event

AcrMgntEventsSubscriptionPatch:

type: object

description: >

Represents a modification request of Individual ACR Management Events Subscription.

properties:

eventSubscs:

type: array

items:

$ref: '#/components/schemas/AcrMgntEventSubsc'

minItems: 1

description: The subscribed ACR management events.

evtReq:

$ref: 'TS29523\_Npcf\_EventExposure.yaml#/components/schemas/ReportingInformation'

notificationDestination:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Uri'

AcrMgntEventsNotification:

type: object

description: Represents the ACR management events notification.

properties:

subpId:

type: string

description: >

String identifying the Individual ACR Management Events Subscription

for which the notification is delivered.

eventReports:

type: array

items:

$ref: '#/components/schemas/AcrMgntEventReport'

minItems: 1

description: A list of ACR management event reports.

required:

- subpId

- eventReports

AcrMgntEventReport:

type: object

description: Represents an ACR management event report.

properties:

event:

$ref: '#/components/schemas/AcrMgntEvent'

timeStamp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

upPathChgInfo:

$ref: '#/components/schemas/UpPathChangeInfo'

easEndPoint:

$ref: 'TS29558\_Eees\_EASRegistration.yaml#/components/schemas/EndPoint'

actStatus:

$ref: '#/components/schemas/ActStatus'

acrParams:

$ref: '#/components/schemas/ACRParameters'

acId:

type: string

selACRScen:

type: array

items:

$ref: '#/components/schemas/SelectedACRScenarios'

minItems: 1

servContPlanInd:

type: boolean

description: >

Represents the service continuity planning indication (i.e., whether or not the EES will

monitor whether the UE(s) enter the predicted location).

When set to true, it indicates that service continuity planning will be performed.

When set to false, it indicates that Service continuity planning will not be performed.

The default value when this attribute is omitted is false.

required:

- event

ACRParameters:

type: object

description: Represents the ACR parameters.

properties:

predictExpTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

FailureAcrMgntEventInfo:

type: object

description: Represents a failure ACR management event.

properties:

event:

$ref: '#/components/schemas/AcrMgntEvent'

failureCode:

$ref: '#/components/schemas/AcrMgntEventFailureCode'

required:

- event

- failureCode

TargetUeIdentification:

description: Identifies the target UE information.

type: object

properties:

gpsi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

intGrpId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

extGrpId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ExternalGroupId'

ueIpAddr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/IpAddr'

oneOf:

- required: [gpsi]

- required: [intGrpId]

- required: [extGrpId]

- required: [ueIpAddr]

AvailabilityNotif:

type: object

description: >

Represents the availability information of user plane path management events monitoring

via the 3GPP 5GC network.

properties:

availabilityStatus:

$ref: '#/components/schemas/AvailabilityStatus'

required:

- availabilityStatus

UpPathChangeInfo:

description: Represents user plane path change information.

type: object

properties:

ueId:

$ref: '#/components/schemas/IndUeIdentification'

dnaiChgType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DnaiChangeType'

sourceTrafficRoute:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RouteToLocation'

targetTrafficRoute:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RouteToLocation'

sourceDnai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnai'

targetDnai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnai'

srcUeIpv4Addr:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv4Addr'

srcUeIpv6Prefix:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

tgtUeIpv4Addr:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv4Addr'

tgtUeIpv6Prefix:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

required:

- ueId

- dnaiChgType

IndUeIdentification:

description: Represents identification information of a UE.

type: object

properties:

gpsi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

externalId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

ueIpAddr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/IpAddr'

oneOf:

- required: [gpsi]

- required: [externalId]

- required: [ueIpAddr]

TrafficFilterInfo:

description: Represents the Traffic Filter Information.

type: object

properties:

ipFlows:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/FlowDescription'

minItems: 1

description: Contains the flow description for the Uplink and/or Downlink IP flows.

uris:

type: array

items:

type: string

minItems: 1

description: Indicates URI(s) matching criteria.

domainNames:

type: array

items:

type: string

minItems: 1

description: Indicates Domain Name matching criteria.

dnProtocol:

$ref: 'TS29122\_PfdManagement.yaml#/components/schemas/DomainNameProtocol'

anyOf:

- required: [ipFlows]

- required: [uris]

- required: [domainNames]

SelectedACRScenarios:

type: object

description: >

Represents the selected ACR scenario(s) applicable for a given combination of AC and UE.

properties:

acrList:

type: array

items:

$ref: 'TS29558\_Eecs\_EESRegistration.yaml#/components/schemas/ACRScenario'

minItems: 0

acId:

type: string

ueId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

required:

- acrList

- acId

- ueId

#

# ENUMERATIONS DATA TYPES

#

AcrMgntEvent:

anyOf:

- type: string

enum:

- UP\_PATH\_CHG

- ACR\_MONITORING

- ACR\_FACILITATION

- ACT\_START\_STOP

- ACR\_SELECTION

- type: string

description: >

This string provides forward-compatibility with future extensions to the enumeration

and is not used to encode content defined in the present version of this API.

description: |

Represents the ACR Management event.

Possible values are:

- UP\_PATH\_CHG: Indicates that ACR Management Event is the User plane path change event.

- ACR\_MONITORING: Indicates that ACR Management Event is the ACR monitoring event.

- ACR\_FACILITATION: Indicates that ACR Management Event is the ACR facilitation event.

- ACT\_START\_STOP: Indicates that ACR Management Event is the ACT start/stop event.

- ACR\_SELECTION: Indicates that ACR Management Event is the ACR selection event.

AcrMgntEventFilter:

anyOf:

- type: string

enum:

- INTRA\_EDN\_MOBILITY

- INTER\_EDN\_MOBILITY

- type: string

description: >

This string provides forward-compatibility with future extensions to the enumeration

and is not used to encode content defined in the present version of this API.

description: |

Represents the filtering criteria for the ACR Management event.

Possible values are:

- INTRA\_EDN\_MOBILITY: Indicates that the ACR Management Event filter is intra-EDN mobility.

- INTER\_EDN\_MOBILITY: Indicates that the ACR Management Event filter is inter-EDN mobility.

ActStatus:

anyOf:

- type: string

enum:

- ACT\_START

- ACT\_STOP

- type: string

description: >

This string provides forward-compatibility with future extensions to the enumeration

and is not used to encode content defined in the present version of this API.

description: |

Represents the ACT status.

Possible values are:

- ACT\_START: Indicates ACT start.

- ACT\_STOP: Indicates ACT stop.

AcrMgntEventFailureCode:

anyOf:

- type: string

enum:

- 3GPP\_UP\_PATH\_CHANGE\_MON\_NOT\_AVAILABLE

- OTHER\_REASONS

- type: string

description: >

This string provides forward-compatibility with future extensions to the enumeration

and is not used to encode content defined in the present version of this API.

description: |

Represents the failure reason for the ACR Management event.

Possible values are:

- 3GPP\_UP\_PATH\_CHANGE\_MON\_NOT\_AVAILABLE: Indicates that the ACR Management Event

Subscription failed because user plane path management event notifications from the 3GPP

network is NOT available. This value is only applicable for the "UP\_PATH\_CHG",

"ACR\_MONITORING" and "ACR\_FACILITATION" events.

- OTHER\_REASONS: Indicates that the ACR Management Event Subscription failed for other

reasons. This value is applicable for all events.

AvailabilityStatus:

anyOf:

- type: string

enum:

- AVAILABLE

- NOT\_AVAILABLE

- type: string

description: >

This string provides forward-compatibility with future extensions to the enumeration

and is not used to encode content defined in the present version of this API.

description: |

Represents the availability status.

Possible values are:

- AVAILABLE: Indicates availability.

- NOT\_AVAILABLE: Indicates unavailability.

\* \* \* \* End of changes \* \* \* \*