**3GPP TSG- WG3 Meeting #30 *4403\_r1***

**Xiamen, China, 9 - 13 October, 2023**  *(revision of C3-234403)*

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** | **134** | **rev** | **-** | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Eees\_EASRegistration - EAS sync and Bundle updates | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Samsung | | | | | | | | | |
| ***Source to TSG:*** | CT3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | EDGEAPP\_Ph2 | | | | |  | ***Date:*** | | | 2023-09-29 |
|  |  | | | |  | |  | | |  |
| ***Category:*** |  |  | | | | | ***Release:*** | | |  |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | As agreed in S6-232205, the EAS profile needs to be updated with the indication of EAS synchronization support. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Following updates to Eees\_EASRegistration service API   1. EAS profile update to indicate the support of EAS synchronization. 2. Remove EAS bundle requirements EN 3. Open API file update. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | EAS sync and bundle feature are not aligned to stage-2. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 8.1.5.2.3, A.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR proposes backward compatible change to Eees\_EASRegistration API. | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

\* \* \* First Change \* \* \* \*

##### 8.1.5.2.3 Type: EASProfile

Table 8.1.5.2.3-1: Definition of type EASProfile

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| easId | string | M | 1 | The application identifier of the EAS (e.g. URI, FQDN). |  |
| endPt | EndPoint | M | 1 | Endpoint information (URI, FQDN, IP address) used to communicate with the EAS. This information maybe discovered by EEC and exposed to ACs so that ACs can establish contact with the EAS. |  |
| easBdlInfos | array(EASBundleInfo) | O | 1..N | Represents a list of EAS bundles to which the EAS (identified by the "easId" attribute) belongs. | EdgeApp\_2 |
| acIds | array(string) | O | 1..N | Identities of the Application Clients that can be served by the EAS |  |
| provId | string | O | 0..1 | Identifier of the ASP that provides the EAS. |  |
| type | EASCategory | O | 0..1 | The EAS type with the 3GPP standardized value set.  (NOTE 1). |  |
| flexEasType | string | O | 0..1 | The EAS type with the flexible value set.  (NOTE 1) |  |
| scheds | array(ScheduledCommunicationTime) | O | 1..N | The availability schedule of the EAS. |  |
| svcArea | ServiceArea | O | 0..1 | The list of geographical and topological areas that the EAS serves. ACs in the UE that are outside the area shall not be served. |  |
| svcKpi | EASServiceKPI | O | 0..1 | Service characteristics provided by the EAS. |  |
| permLvl | array(PermissionLevel) | O | 1..N | Level of service permissions supported by the EAS. |  |
| easFeats | array(string) | O | 1..N | Service specific features supported by the EAS (e.g. single vs multi-player gaming service). |  |
| svcContSupp | array(ACRScenario) | O | 1..N | The ACR scenarios supported by the EAS for service continuity. If this attribute is not present, then the EAS does not support service continuity. |  |
| transContSupp | TransContSuppDetails | O | 0..1 | Represents the detailed information about the EAS (e.g. SEALDD Server) capability for seamless transport layer service continuity.  If this attribute is not present, then the EAS does not support the seamless transport layer service continuity capability. | SEALDD\_Support |
| appLocs | array(RouteToLocation) | O | 1..N | List of DNAI(s) and the corresponding N6 traffic routing information/routing profile ID, associated with the EAS.  It is a subset of the DNAI(s) associated with the EDN where the EAS resides. |  |
| avlRep | DurationSec | O | 0..1 | The period indicating to the EES, how often the EES needs to check the EAS's availability after a successful registration. |  |
| status | string | O | 0..1 | EAS status (e.g. Enabled, Disabled etc.) |  |
| genCtxDur | DurationSec | O | 0..1 | The general context holding time duration that the EAS holds the application context before the AC connects to EAS, after receiving an ACR notification from the EES following an ACR request form the EEC.  (NOTE 2) | EdgeApp\_2 |
| easSyncSupp | boolean | O | 0..1 | Indicates whether the EAS supports content synchronization between EASs.  - When set to "true", it indicates that content synchronization between EASs is supported by the EAS.  - When set to "false", it indicates that content synchronization between EASs is not supported by the EAS.  - The default value when this attribute is omitted is "false". | EdgeApp\_2 |
| NOTE 1: The "flexEasType" attribute and the "type" attribute are mutually exclusive. Either one of them may be provided. The same attribute should be used when this data type is conveyed over the EDGE-1 and EDGE-3 interfaces (i.e. for the Eees\_EASRegistration and the Eees\_EASDiscovery APIs).  NOTE 2: For determining the value of the "genCtxDur" attribute used to indicate the general context holding time duration, the EAS may rely on the value of the "easId" attribute (which identifies the type of the application). | | | | | |

\* \* \* Next Change \* \* \* \*

# A.2 Eees\_EASRegistration API

openapi: 3.0.0

info:

title: EES EAS Registration\_API

description: |

API for EAS Registration.

© 2023, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

version: 1.1.0-alpha.4

externalDocs:

description: >

3GPP TS 29.558 V18.3.0 Enabling Edge Applications;

Application Programming Interface (API) specification; Stage 3

url: https://www.3gpp.org/ftp/Specs/archive/29\_series/29.558/

servers:

- url: '{apiRoot}/eees-easregistration/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 7.5 of 3GPP TS 29.558.

security:

- {}

- oAuth2ClientCredentials: []

paths:

/registrations:

post:

summary: Creates a new Individual EAS Registration resource

operationId: CreateEASRegistration

tags:

- EAS Registrations (Collection)

description: Registers a new EAS at an EES.

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/EASRegistration'

responses:

'201':

description: EAS information is registered successfully at EES.

content:

application/json:

schema:

$ref: '#/components/schemas/EASRegistration'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/registrations/{registrationId}:

get:

summary: Read an Individual EAS Registration resource

operationId: ReadIndEASRegistration

tags:

- Individual EAS Registration (Document)

description: Retrieve an Individual EAS registration resource.

parameters:

- name: registrationId

in: path

description: Registration Id.

required: true

schema:

type: string

responses:

'200':

description: OK (The EAS registration information at the EES).

content:

application/json:

schema:

$ref: '#/components/schemas/EASRegistration'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

put:

summary: Update an Individual EAS Registration resource

operationId: UpdateIndEASRegistration

tags:

- Individual EAS Registration (Document)

description: Fully replace an existing EAS Registration resource.

parameters:

- name: registrationId

in: path

description: EAS registration Id.

required: true

schema:

type: string

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/EASRegistration'

responses:

'200':

description: OK (The EAS registration information is updated successfully).

content:

application/json:

schema:

$ref: '#/components/schemas/EASRegistration'

'204':

description: >

No Content. The individual EAS registration information is updated successfully.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

patch:

summary: Modify an Individual EAS Registration resource

operationId: ModifyIndEASRegistration

tags:

- Individual EAS Registration (Document)

description: Partially update an existing EAS Registration resource.

parameters:

- name: registrationId

in: path

description: EAS registration Id.

required: true

schema:

type: string

requestBody:

description: Partial update of an existing EAS registration resource.

required: true

content:

application/merge-patch+json:

schema:

$ref: '#/components/schemas/EASRegistrationPatch'

responses:

'200':

description: >

The Individual EAS registration is successfully modified and the updated

registration information is returned in the response.

content:

application/json:

schema:

$ref: '#/components/schemas/EASRegistration'

'204':

description: >

No Content. The individual EAS registration information is updated successfully.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

summary: Delete an Individual EAS Registration resource

operationId: DeleteIndEASRegistration

tags:

- Individual EAS Registration (Document)

description: Delete an existing EAS registration at EES.

parameters:

- name: registrationId

in: path

description: EAS registration Id.

required: true

schema:

type: string

responses:

'204':

description: The individual EAS registration is deleted.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{tokenUrl}'

scopes: {}

schemas:

EASRegistration:

type: object

description: Represents an EAS registration information.

properties:

easProf:

$ref: '#/components/schemas/EASProfile'

expTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

required:

- easProf

EASProfile:

type: object

description: Represents the EAS profile information.

properties:

easId:

type: string

description: Identifier of the EAS.

endPt:

$ref: '#/components/schemas/EndPoint'

easBdlInfos:

type: array

items:

$ref: '#/components/schemas/EASBundleInfo'

minItems: 1

acIds:

type: array

items:

type: string

minItems: 1

description: Identities of application clients that are served by the EAS.

provId:

type: string

description: Identifier of the ASP that provides the EAS.

type:

$ref: '#/components/schemas/EASCategory'

flexEasType:

type: string

description: The EAS type with flexible value set.

scheds:

type: array

items:

$ref: 'TS29122\_CpProvisioning.yaml#/components/schemas/ScheduledCommunicationTime'

minItems: 1

description: The availability schedule of the EAS.

svcArea:

$ref: 'TS29558\_Eecs\_EESRegistration.yaml#/components/schemas/ServiceArea'

svcKpi:

$ref: '#/components/schemas/EASServiceKPI'

permLvl:

type: array

items:

$ref: '#/components/schemas/PermissionLevel'

minItems: 1

description: level of service permissions supported by the EAS.

easFeats:

type: array

items:

type: string

minItems: 1

description: Service specific features supported by EAS.

appLocs:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RouteToLocation'

minItems: 1

description: List of DNAI(s) and the N6 traffic information associated with the EAS.

svcContSupp:

type: array

items:

$ref: 'TS29558\_Eecs\_EESRegistration.yaml#/components/schemas/ACRScenario'

minItems: 1

description: The ACR scenarios supported by the EAS for service continuity.

transContSupp:

$ref: '#/components/schemas/TransContSuppDetails'

avlRep:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

status:

type: string

description: EAS status information.

genCtxDur:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

easSyncSupp:

type: boolean

default: false

description: >

Set to true to indicate that content synchronization between EASs is supported.

Set to false to indicate that content synchronization between EASs is not supported.

The default value when this attribute is omitted is false.

required:

- easId

- endPt

not:

required: [ type, flexEasType ]

EASRegistrationPatch:

type: object

description: Represents partial update request of individual EAS registration information.

properties:

easProf:

$ref: '#/components/schemas/EASProfile'

expTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTimeRm'

EASServiceKPI:

type: object

description: Represents the EAS service KPI information.

properties:

maxReqRate:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

maxRespTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

avail:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

avlComp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

avlGraComp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

avlMem:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

avlStrg:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

connBand:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

EASBundleInfo:

type: object

description: Represents the EAS bundle information.

properties:

bdlId:

type: string

description: Indicates a bundle ID.

easIdsList:

type: array

items:

type: string

minItems: 1

bdlType:

$ref: '#/components/schemas/BdlType'

easBdlReqs:

$ref: '#/components/schemas/EASBdlReqs'

mainEasId:

type: string

required:

- bdlType

oneOf:

- required: [bdlId]

- required: [easIdsList]

EASBdlReqs:

type: object

description: Represents the EAS bundle requirements.

properties:

coordinatedEasDisc:

type: boolean

default: false

description: >

Set to true to indicate that coordianted EAS discovery is required.

Set to false to indicate that coordianted EAS discovery is not required.

The default value when this attribute is omitted is false.

coordinatedAcr:

$ref: '#/components/schemas/CoordinatedAcrReqs'

affinity:

$ref: '#/components/schemas/Affinity'

CoordinatedAcrReqs:

type: object

description: Represents the coordinated ACR related requirements for an EAS bundle.

properties:

coordinatedAcrInd:

type: boolean

default: false

description: >

Set to true to indicate that coordianted ACR is required.

Set to false to indicate that coordianted ACR is not required.

The default value when this attribute is omitted is false.

failureAction:

$ref: '#/components/schemas/FailureAction'

required:

- coordinatedAcrInd

EndPoint:

type: object

description: The end point information to reach EAS.

properties:

fqdn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Fqdn'

ipv4Addrs:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv4Addr'

minItems: 1

description: IPv4 addresses of the edge server.

ipv6Addrs:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv6Addr'

minItems: 1

description: IPv6 addresses of the edge server.

uri:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Uri'

oneOf:

- required: [uri]

- required: [fqdn]

- required: [ipv4Addrs]

- required: [ipv6Addrs]

PermissionLevel:

anyOf:

- type: string

enum:

- TRIAL

- GOLD

- SILVER

- OTHER

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: |

Indicates the level of service permissions supported by the EAS.

Possible values are:

- TRIAL: Level of service permission supported is TRIAL.

- GOLD: Level of service permission supported is GOLD.

- SILVER: Level of service permission supported is SILVER.

- OTHER: Any other level of service permissions supported.

EASCategory:

anyOf:

- type: string

enum:

- UAS

- V2X

- SEAL\_SEALDD\_SERVERS

- OTHER

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: |

Indicates the category or type of the EAS.

Possible values are:

- UAS: Indicates that the EAS category is for UAS services.

- V2X: Category of EAS is for V2X Services.

- SEALDD: Indicates that the EAS category is SEALDD Server for SEALDD services.

- OTHER: Any other type of EAS category.

TransContSuppDetails:

type: object

description: >

Represents the detailed information about the EAS (e.g. SEALDD Server) capability for

seamless transport layer service continuity.

properties:

transProtocs:

type: array

items:

$ref: '#/components/schemas/TransportProtocol'

minItems: 1

description: >

Indicates the transport layer protocols supported for EAS context transfer using

the seamless transport layer service continuity capability.

required:

- transProtocs

TransportProtocol:

anyOf:

- type: string

enum:

- QUIC

- TCP

- TCP\_TLS

- type: string

description: >

This string provides forward-compatibility with future extensions to the enumeration

and is not used to encode content defined in the present version of this API.

description: |

Indicates the transport layer protocol.

Possible values are:

- QUIC: Indicates the QUIC protocol.

- TCP: Indicates the Transmission Control (TCP) Protocol.

- TCP\_TLS: Indicates the Transmission Control Protocol (TCP) with Transport Layer Security

(TLS) protocol.

BdlType:

anyOf:

- type: string

enum:

- DIRECT

- PROXY

- type: string

description: >

This string provides forward-compatibility with future extensions to the enumeration and

is not used to encode content defined in the present version of this API.

description: |

Represents the EAS Bundle type.

Possible values are:

- DIRECT: Indicates that the EAS Bundle type is direct bundle.

- PROXY: Indicates that the EAS Bundle type is proxy bundle.

Affinity:

anyOf:

- type: string

enum:

- STRONG

- PREFERRED

- WEAK

- type: string

description: >

This string provides forward-compatibility with future extensions to the enumeration and

is not used to encode content defined in the present version of this API.

description: |

Represents the affinity requirements of an EAS bundle.

Possible values are:

- STRONG: Indicates that the affinity is strong, i.e., all the EASs of the bundle shall be

in the same EDN.

- PREFERRED: Indicates that the affinity is preferred, i.e., it is nice to have all the EASs

of the bundle in the same EDN, but it is not essential.

- WEAK: Indicates that the affinity is weak, i.e., it is not essential to have all the EASs

of the bundle in the same EDN.

FailureAction:

anyOf:

- type: string

enum:

- CANCEL

- PROCEED

- type: string

description: >

This string provides forward-compatibility with future extensions to the enumeration and

is not used to encode content defined in the present version of this API.

description: |

Represents the EAS bundle related failure action during ACR.

Possible values are:

- CANCEL: Indicates that ACR shall be cancelled for the other EAS(s) of the bundle for which

ACR is not failed.

- PROCEED: Indicates that ACR shall proceed for the other EAS(s) of the bundle for which

ACR is not failed.

\* \* \* End of Changes \* \* \* \*