**3GPP TSG-CT WG3 Meeting #130 *C3-234260r1***

**Xiamen, China, 9 - 13 October, 2023**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **29.522** | **CR** | **1076** | **rev** | **1** | **Current version:** | **18.3.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Incorrect description of error handling in subscription creation procedure |
|  |  |
| ***Source to WG:*** | ZTE, Nokia, Nokia Shanghai Bell |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | EDGE\_Ph2 |  | ***Date:*** | 2023-10-2 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** |  Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | There is a wrong description in 4.4.34.2: “*Upon receipt of the corresponding HTTP POST message, if the AF is authorized by the NEF to obtain the DNAI mapping information, the NEF shall interact with the UDR by invoking the Nudr\_DataRepository service as described in 3GPP TS 29.504 [20], if the NEF receives an error response from the UDR, the NEF shall not create, update or delete the resource and shall respond to the AF with a proper error status code.*”, as the NEF cannot update/delete the resource when receiving POST request for subscription creation. |
|  |  |
| ***Summary of change:*** | Update of 4.4.34.2 to remove “update or delete”. |
|  |  |
| ***Consequences if not approved:*** | Wrong description remains. |
|  |  |
| ***Clauses affected:*** | 4.4.34.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR does not have any impact in the OpenAPI specification. |
|  |  |
| ***This CR's revision history:*** |  |

**Additional discussion(if needed):**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

#### 4.4.34.2 Creation of a new subscription for DNAI Mapping

In order to create a new subscription for DNAI Mapping for a given AF, the AF shall initiate an HTTP POST request to the NEF for the "DNAI Mapping Subscriptions" resource. The HTTP POST request message body shall include the DnaiMapSub data structure that shall include either:

- FQDN of the EAS in the Local part of the DN as the "fqdn" attribute;

or

- EAS IP Address(es) in the Local part of the DN, "easIpAddrs" attribute;

and may include:

- an DNN as "dnn" attribute;

- an S-NSSAI as "snssai" attribute;

- an Event reporting requirements as "eventReq" attribute.

Upon receipt of the corresponding HTTP POST message, if the AF is authorized by the NEF to obtain the DNAI mapping information, the NEF shall interact with the UDR by invoking the Nudr\_DataRepository service as described in 3GPP TS 29.504 [20], if the NEF receives an error response from the UDR, the NEF shall not create the resource and shall respond to the AF with a proper error status code. If the NEF received within an error response a "ProblemDetails" data structure with a "cause" attribute indicating an application error, the NEF shall relay this error response to the AF with a corresponding application error, when applicable.

On successful DNAI Mapping subscription creation, the NEF shall return an HTTP POST response with an HTTP "201 Created" status code to the AF, including a "Location" header containing the URI of the created "Individual DNAI Mapping Subscription" resource and the response body containing a representation of the created resource within the DnaiMapSub data structure. If one-time reporting is not requested, an expiry time (if the subscription can be expired based on the operator’s policy) shall be included within the DnaiMapSub data structure.

On failure, the NEF shall take proper error handling actions, as specified in clause 5.30.7, and respond to the AF with an appropriate error status code.

\*\*\* End of Changes \*\*\*