**3GPP TSG-CT3 Meeting #130C3-234486**

**Xiamen, China, 9th – 13th October 2023 was C3-234431 was C3-234101**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.522** | **CR** | **1049** | **rev** | **2** | **Current version:** | **18.3.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | |
| ***Title:*** | Support the change of the PDU Session Type for a 5G VN group | | | | | | | | |
|  |  | | | | | | | | |
| ***Source to WG:*** | Huawei, SIA | | | | | | | | |
| ***Source to TSG:*** | CT3 | | | | | | | | |
|  |  | | | | | | | | |
| ***Work item code:*** | GMEC | | | | |  | ***Date:*** | | 2023-10-11 |
|  |  | | | |  | |  | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | |
| ***Reason for change:*** | | | As specified in clause 5.29.2 of TS 23.501 and clause 4.15.6.10 of TS 23.502, the AF may provision/update the requested PDU Session type for UEs belonging to a 5G VN group using the service parameters provisioning procedure under the scope of AF guidance of URSP determination. | | | | | | |
|  | | |  | | | | | | |
| ***Summary of change:*** | | | This CR proposes to:   * Update the ServiceParameter API to specify the support of the provisioning/update the requested PDU Session type for UEs belonging to a 5G VN group. | | | | | | |
|  | | |  | | | | | | |
| ***Consequences if not approved:*** | | | * The GMEC related stage 2 requirements on supporting provisioning/update the requested PDU Session type for UEs belonging to a 5G VN group are not specified in stage 3. | | | | | | |
|  | |  | | | | | | | |
| ***Clauses affected:*** | | 4.4.20, 5.11.2.2, 5.11.2.3.5, 5.11.3, A.27 | | | | | | | |
|  | |  | | | | | | | |
|  | | **Y** | | **N** |  | | |  | |
| ***Other specs*** | | **X** | |  | Other core specifications | | | TS 23.501 CR#4993 | |
| ***affected:*** | |  | | **X** | Test specifications | | | TS 23.502 CR#4496 | |
| ***(show related CRs)*** | |  | | **X** | O&M Specifications | | | TS/TR ... CR ... | |
|  | |  | | | | | | | |
| ***Other comments:*** | | This CR introduces a backwards compatibles new feature to the OpenAPI description of the NEF ServiceParameter API defined in this specification and the Nudr\_DataRepository API for Application Data defined in TS 29.519 and the Npcf\_UEPolicyControl API defined in TS 29.525. | | | | | | | |
|  | |  | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | |

\* \* \* \* Start of changes \* \* \* \*

### 4.4.20 Procedures for service specific parameter provisioning

These procedures are used by an AF to provide service specific parameters to the 5G system via the NEF.

In order to provision service specific parameters to the 5G system, the AF shall send an HTTP POST message to the NEF targetting the resource "Service Parameter Subscriptions", the HTTP POST request message body shall include the ServiceParameterData data structure that shall include:

- service description via one of the following:

a) a combination of DNN and S-NSSAI within the "dnn" attribute and the "snssai" attribute respectively;

b) an AF Service Identifier within the "afServiceId" attribute. In this case, the NEF may translate the received AF service identifier into a DNN and S-NSSAI combination; or

c) an application identifier within the "appId" attribute;

NOTE 1: When the feature "AfGuideURSP" is supported, the DNN, S-NSSAI and/or Application Identifier information can be provided in the "urspGuidance" attribute, hence only the "afServiceId" attribute needs to be included for providing guidance for URSP determination.

- indication of the UEs to which the subscription applies via one of the following:

a) identification of an individual UE within the "gpsi" attribute;

b) an IPv4 address of the UE within the "ueIpv4" attribute;

c) an IPv6 address of the UE within the "ueIpv6" attribute;

d) a MAC address of the UE within the "ueMac" attribute;

e) an identification of a group of UE(s) within the "externalGroupId" attribute;

NOTE 2: When the feature "PIN" is supported, AF can use "externalGroupId" attribute to indicate the external group identifier if more than one PEGC is present within the PIN. If external group identifier is not used for the PIN, then AF will indicate "gpsi" attribute in the individual request for each of the PEGC within the PIN.

f) an identification of any UE within the "anyUeInd" attribute; or

g) when the feature "VPLMNSpecificURSP" is supported, and the request is to influence the determination of own PLMN(s) specific URSP rules for any inbound roamer from one or more PLMN(s), an identification of the PLMN IDs of the roaming UEs within the "roamUeNetDescs" attribute; and

- service parameters for at least one of the following:

1) V2X service parameters via:

a) configuration parameters for V2X communications over PC5 within the "paramOverPc5" attribute; and

b) configuration parameters for V2X communications over Uu within the "paramOverUu" attribute;

2) if the "ProSe" and/or "ProSe\_Ph2" feature(s) is/are supported, 5G ProSe service parameters via:

a) configuration parameters for 5G ProSe direct discovery within the "paramForProSeDd" attribute;

b) configuration parameters for 5G ProSe direct communication within the "paramForProSeDc" attribute; and

c) configuration parameters for 5G ProSe UE-to-network relay, including configuration parameters for 5G ProSe UE-to-network relay UE within the "paramForProSeU2NRelUe" attribute and configuration parameters for 5G ProSe remote UE within the "ParamForProSeRemUe" attribute;

d) configuration parameters for 5G ProSe UE-to-UE relay, including configuration parameters for 5G ProSe UE-to-UE relay UE within the "paramForProSeU2URelUe" attribute and configuration parameters for 5G ProSe end UE within the "ParamForProSeEndUe" attribute, only if the "ProSe\_Ph2" feature is supported;

3) if the "AfGuideURSP" feature is supported, URSP service parameters via:

a) contents for the AF guidance on URSP within the "urspGuidance" attribute, which shall include one or more URSP rule requests. Each URSP rule request may include:

1. a traffic descriptor within the "trafficDesc" attribute;

2. a relative precedence within the "relatPrecedence" attribute;

3. when the feature "VPLMNSpecificURSP" is supported and the AF guidance is to influence the determination of VPLMN-specific URSP rules, the VPLMN description within the "visitedNetDescs" attribute; and/or

4. one or more route selection parameter sets within the "routeSelParamSets" attribute. Each route selection parameter set may include a precedence value within the "precedence" attribute, a DNN within the "dnn" attribute, an S-NSSAI within the "snssai" attribute, a spatial validity condition within the "spatialValidity" attribute, and if the "GMEC" feature is also supported, the requested PDU Session type within the "pduSessType" attribute. If the request contains only one route selection parameter set, each of the optional attributes "dnn", "snssai", "precedence", and "spatialValidity" that is missing from the request may be complemented by the NEF based on local configuration for the provided AF service identifier. It is up to the NEF to transform the information of the "spatialValidity" attribute into a list of TAIs;

Editor's Note: The requested PDU Session Type related functionality definition is FFS.

b) if the "PIN" feature is supported, traffic descriptor component within in the URSP rule via PIN Identifier within the "pinId" attribute applicable for the PEGC;

4) if the "A2X" feature is supported, A2X service parameters via:

a) configuration parameters for A2X communications over PC5 within the "a2xParamsPc5" attribute;

5) if the "AfGuideTNAPs" feature is supported, TNAP ID(s) service parameters via:

a) a list of the TNAP ID(s) collocated with the 5G-RG(s) of a specific user within the "tnaps" attribute;

and

6) if the "Ranging\_SL" feature is supported, ranging and sidelink positioning service parameters via configuration parameters for ranging and sidelink positioning within the "paramForRangingSlPos" attribute;

and may include:

- if the "AfNotifications" feature is supported:

a) subscription to event notification of the outcome related to invocation of service parameter provisioning within the "subNotifEvents" attribute; and

b) notification URI within the "notificationDestination" attribute.

In order to update an existing service parameter subscription, the AF shall send an HTTP PUT or HTTP PATCH message to the NEF targetting the resource "Individual Service Parameter Subscription" and requesting to change the subscription. When the HTTP PUT method is used, the NF service consumer should not update attributes that do not exist in the ServiceParameterDataPatch data type, i.e. such attributes should remain unchanged compared to the initial values provided in the HTTP POST request message.

In order to delete an existing service parameter subscription, the AF shall send an HTTP DELETE message to the NEF targetting the resource "Individual Service Parameter Subscription".

Upon receipt of the HTTP request from the AF, and if the AF is authorized, the NEF shall interact with the UDM by invoking the Nudm\_SubscriberDataManagement service as described in 3GPP TS 29.503 [17] to retrieve the SUPI or Internal Group Identifier. NEF may, based on local configuration, complement missing service parameters. Additionally, based on operator's local policy, NEF may support service specific authorization as described in clause 4.15.6.10 in 3GPP TS 23.502 [2]. Then the NEF shall interact with the UDR to create, update or delete the associated service parameters by using the Nudr\_DataRepository service as defined in 3GPP TS 29.519 [23]. If information related to AfNotifications feature are received from the AF, the NEF shall also include the required information (e.g. "policDelivNotifUri" and "policDelivNotifCorreId" attributes in 3GPP TS 29.519 [23]) in UDR data creation if the NEF supports the DeliveryOutcome feature (as described in 3GPP TS 29.504 [4]). If the NEF receives an error response from the UDR, the NEF shall not create, update or delete the resource and shall respond to the AF with a proper error status code. If the NEF received within an error response a "ProblemDetails" data structure with a "cause" attribute indicating an application error, the NEF shall relay this error response to the AF with a corresponding application error, when applicable.

After receiving a successful response from the UDR, the NEF shall:

- for an HTTP POST request, create an "Individual Service Parameter Subscription" resource which represents the Service Parameter provisioning request, addressed by a URI that contains the AF Identifier and a NEF-created configuration identifier, and shall respond to the AF with a 201 Created status code, including a Location header field containing the URI for the created resource. The AF shall use the URI received in the Location header in subsequent requests to the NEF to refer to this Service Parameter Subscription;

- for an HTTP PUT or HTTP PATCH request, update the "Individual Service Parameter Subscription" resource which represents the service parameter provisioning request, and respond to the AF with a 200 OK or 204 No Content status code; and

- for an HTTP DELETE request, remove all properties of the resource and delete the corresponding active "Individual Service Parameter Subscription" resource, then respond to the AF with a 204 No Content status code.

When the NEF receives the Service Specific Authorization Update information from the UDM by Nudm\_ServiceSpecificAuthorization\_UpdateNotify service operation defined in 3GPP TS 29.503 [17], if the authorization is revoked, the NEF shall provide a notification to AF by sending HTTP POST message that include the one or more AfNotification data structure(s). Upon receipt of the notification, the AF shall respond with a "204 No Content" status code to confirm the received notification.

When the NEF receives the notification of the outcome of invocation related to AF provisioned service parameters from the PCF by Npcf\_EventExposure\_Notify service operation defined in 3GPP TS 29.523 [22], the NEF shall determine the corresponding service parameter subscription and provide a notification to AF by sending HTTP POST message that include the AfNotification data structure. Upon receipt of the notification, the AF shall respond with a "204 No Content" status code to confirm the received notification.

\* \* \* \* Next changes \* \* \* \*

#### 5.11.2.2 Reused data types

The data types reused by the ServiceParameter API from other specifications are listed in table 5.9.2.2-1.

Table 5.11.2.2-1: Re-used Data Types

|  |  |  |
| --- | --- | --- |
| Data type | Reference | Comments |
| AppDescriptor | Clause 5.7.2.3.4 | Application descriptor describes the operation systems and the corresponding applications for each operation systems. |
| Dnn | 3GPP TS 29.571 [8] | Identifies a DNN. |
| EthFlowDescription | 3GPP TS 29.514 [7] | Defines a packet filter for an Ethernet flow. |
| ExternalGroupId | 3GPP TS 29.122 [4] | External Group Identifier for a user group. |
| Gpsi | 3GPP TS 29.571 [8] | Identifies a GPSI. |
| IpAddr | 3GPP TS 29.571 [8] | UE IP Address. |
| IPv4Addr | 3GPP TS 29.571 [8] | Identifies an IPv4 address. |
| IPv6Addr | 3GPP TS 29.571 [8] | Identifies an IPv6 address. |
| Link | 3GPP TS 29.122 [4] | Represents a referenced resource. |
| MacAddr48 | 3GPP TS 29.571 [8] | Identifies an MAC address. |
| Mcc | 3GPP TS 29.571 [8] | Mobile Country Code. |
| Mnc | 3GPP TS 29.571 [8] | Mobile Network Code. |
| PduSessionType | 3GPP TS 29.571 [8] | Represents the PDU session type. |
| PlmnId | 3GPP TS 29.571 [8] | Identifies a PLMN Identifier. |
| MtcProviderInformation | 3GPP TS 29.571 [8] | Indicates MTC provider information. |
| Snssai | 3GPP TS 29.571 [8] | Identifies the S-NSSAI. |
| SupportedFeatures | 3GPP TS 29.571 [8] | Used to negotiate the applicability of the optional features defined in table 5.11.3-1. |
| Tai | 3GPP TS 29.571 [8] | Tracking Area Identity information. |
| TnapId | 3GPP TS 29.571 [8] | Trusted Network Access Point identifier. |
| Uinteger | 3GPP TS 29.571 [8] | Unsigned integer. |

\* \* \* \* Next changes \* \* \* \*

##### 5.11.2.3.5 Type: RouteSelectionParameterSet

Table 5.11.2.3.5-1: Definition of type RouteSelectionParameterSet

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| dnn | Dnn | O | 0..1 | DNN to be matched with the DNN of the PDU Session. |  |
| snssai | Snssai | O | 0..1 | S-NSSAI to be matched with the S-NSSAI of the PDU Session. |  |
| precedence | Uinteger | O | 0..1 | Determines the order in which the Route Selection Descriptors are to be applied. |  |
| spatialValidityAreas | array(GeographicalArea) | O | 1..N | Indicates where the route selection parameters apply. It may correspond to a geographical area (e.g. a geographic shape that is known to the AF and is configured by the operator to correspond to a list of TAIs). |  |
| spatialValidityTais | array(Tai) | O | 1..N | Indicates the TAIs in which the route selection parameters apply. This attribute is applicable only within the 5GC and it shall not be included in the request messages of untrusted AFs for URSP guidance. |  |
| pduSessType | PduSessionType | O | 0..1 | Represents the requested PDU Session type. | GMEC |

\* \* \* \* Next changes \* \* \* \*

### 5.11.3 Used Features

The table below defines the features applicable to the ServiceParameter API. Those features are negotiated as described in clause 5.2.7 of 3GPP TS 29.122 [4].

Table 5.11.3-1: Features used by ServiceParameter API

|  |  |  |
| --- | --- | --- |
| Feature number | Feature Name | Description |
| 1 | ProSe | This feature indicates the support of UE policy and N2 information provisioning for 5G ProSe. |
| 2 | enNB | Indicates the support of enhancements to the northbound interfaces. |
| 3 | AfNotifications | This feature indicates the support of AF subscribed event(s) notifications. |
| 4 | Notification\_websocket | The delivery of notifications over Websocket is supported as described in 3GPP TS 29.122 [4]. This feature requires that the Notification\_test\_event feature is also supported. |
| 5 | Notification\_test\_event | The testing of notification connection is supported as described in 3GPP TS 29.122 [4]. |
| 6 | AfGuideURSP | This feature indicates the support of AF guidance for URSP determination. |
| 7 | A2X | This feature indicates the support of A2X communication. |
| 8 | ProSe\_Ph2 | This feature indicates the support of UE policy and N2 information provisioning for 5G ProSe UE-to-UE Relay function.  This feature requires that the ProSe feature is also supported. |
| 9 | PIN | This feature indicates the support of Personal IoT Network requirements. |
| 10 | VPLMNSpecificURSP | This feature indicates the support of AF guidance on VPLMN-specific URSP rules.  This feature requires that AfGuideURSP is also supported. |
| 11 | AfGuideTNAPs | This feature indicates the support of AF providing guidance to the HPLMN of the UE of the list of TNAP(s) collocated with the 5G-RG(s) of a specific user. |
| 12 | Ranging\_SL | This feature indicates the support of ranging and sidelink positioning requirements. |
| 13 | GMEC | This feature indicates the support of Generic Group Management, Exposure and Communication Enhancements.  The following functionalities are supported:  - Support the provisioning/update of the requested PDU Session type as part of the information provided by the AF for guiding URSP determination.  This feature requires the support of the "AfGuideURSP" feature. |

\* \* \* \* Next changes \* \* \* \*

# A.9 ServiceParameter API

openapi: 3.0.0

info:

title: 3gpp-service-parameter

version: 1.2.0-alpha.4

description: |

API for AF service paramter

© 2023, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: >

3GPP TS 29.522 V18.3.0; 5G System; Network Exposure Function Northbound APIs.

url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.522/'

security:

- {}

- oAuth2ClientCredentials: []

servers:

- url: '{apiRoot}/3gpp-service-parameter/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 5.2.4 of 3GPP TS 29.122.

paths:

/{afId}/subscriptions:

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

get:

summary: read all of the active subscriptions for the AF

operationId: ReadAllSubscriptions

tags:

- Service Parameter Subscriptions

parameters:

- name: gpsis

in: query

description: The GPSI of the requested UE(s).

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

minItems: 1

- name: ip-addrs

in: query

description: The IP address(es) of the requested UE(s).

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/IpAddr'

minItems: 1

- name: ip-domain

in: query

description: >

The IPv4 address domain identifier. The attribute may only be provided

if IPv4 address is included in the ip-addrs query parameter.

required: false

schema:

type: string

- name: mac-addrs

in: query

description: The MAC address(es) of the requested UE(s).

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

minItems: 1

responses:

'200':

description: OK.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/ServiceParameterData'

minItems: 0

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

post:

summary: Creates a new subscription resource

operationId: CreateAnSubscription

tags:

- Service Parameter Subscriptions

requestBody:

description: Request to create a new subscription resource

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/ServiceParameterData'

responses:

'201':

description: Created (Successful creation of subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/ServiceParameterData'

headers:

Location:

description: Contains the URI of the newly created resource.

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

callbacks:

notificationDestination:

'{$request.body#/notificationDestination}':

post:

requestBody:

description: >

Notifications upon AF Service Parameter Authorization Update,

and/or AF subscribed event notification of the outcome related

to the invocation of service parameters provisioning.

required: true

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/AfNotification'

minItems: 1

responses:

'204':

description: Expected response to a successful callback processing without a body

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{afId}/subscriptions/{subscriptionId}:

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

get:

summary: read an active subscriptions for the SCS/AS and the subscription Id

operationId: ReadAnSubscription

tags:

- Individual Service Parameter Subscription

responses:

'200':

description: OK (Successful get the active subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/ServiceParameterData'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

put:

summary: Fully updates/replaces an existing subscription resource

operationId: FullyUpdateAnSubscription

tags:

- Individual Service Parameter Subscription

requestBody:

description: Parameters to update/replace the existing subscription

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/ServiceParameterData'

responses:

'200':

description: OK (Successful update of the subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/ServiceParameterData'

'204':

description: OK (Successful update of the subscription)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

patch:

summary: Partial updates/replaces an existing subscription resource

operationId: PartialUpdateAnSubscription

tags:

- Individual Service Parameter Subscription

requestBody:

required: true

content:

application/merge-patch+json:

schema:

$ref: '#/components/schemas/ServiceParameterDataPatch'

responses:

'200':

description: OK. The subscription was modified successfully.

content:

application/json:

schema:

$ref: '#/components/schemas/ServiceParameterData'

'204':

description: OK. The subscription was modified successfully.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

summary: Deletes an already existing subscription

operationId: DeleteAnSubscription

tags:

- Individual Service Parameter Subscription

responses:

'204':

description: No Content (Successful deletion of the existing subscription)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{tokenUrl}'

scopes: {}

schemas:

ServiceParameterData:

description: Represents an individual Service Parameter subscription resource.

type: object

properties:

afServiceId:

type: string

description: Identifies a service on behalf of which the AF is issuing the request.

appId:

type: string

description: Identifies an application.

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

externalGroupId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalGroupId'

anyUeInd:

type: boolean

description: >

Identifies whether the AF request applies to any non-roaming UE. This attribute,

when provided, shall set to "true" if applicable for any UE, otherwise, set to "false".

roamUeNetDescs:

type: array

items:

$ref: '#/components/schemas/NetworkDescription'

minItems: 1

description: Each element identifies one or more PLMN IDs of inbound roamers.

gpsi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

ueIpv4:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

ueIpv6:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

ueMac:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

self:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

subNotifEvents:

type: array

items:

$ref: '#/components/schemas/Event'

minItems: 1

notificationDestination:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

requestTestNotification:

type: boolean

description: >

Set to true by the AF to request the NEF to send a test notification

as defined in clause 5.2.5.3 of 3GPP TS 29.122. Set to false or omitted otherwise.

websockNotifConfig:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/WebsockNotifConfig'

paramOverPc5:

$ref: '#/components/schemas/ParameterOverPc5'

paramOverUu:

$ref: '#/components/schemas/ParameterOverUu'

paramForProSeDd:

$ref: '#/components/schemas/ParamForProSeDd'

paramForProSeDc:

$ref: '#/components/schemas/ParamForProSeDc'

paramForProSeU2NRelUe:

$ref: '#/components/schemas/ParamForProSeU2NRelUe'

paramForProSeRemUe:

$ref: '#/components/schemas/ParamForProSeRemUe'

paramForProSeU2URelUe:

$ref: '#/components/schemas/ParamForProSeU2URelUe'

paramForProSeEndUe:

$ref: '#/components/schemas/ParamForProSeEndUe'

paramForRangingSlPos:

$ref: '#/components/schemas/ParamForRangingSlPos'

urspGuidance:

type: array

items:

$ref: '#/components/schemas/UrspRuleRequest'

minItems: 1

description: Contains the service parameter used to guide the URSP.

a2xParamsPc5:

$ref: '#/components/schemas/A2xParamsPc5'

tnaps:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TnapId'

minItems: 1

description: Contains the TNAP IDs collocated with the 5G-RG(s) of a specific user.

mtcProviderId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MtcProviderInformation'

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

ServiceParameterDataPatch:

description: >

Represents the parameters to request the modification of a service parameter

subscription resource.

type: object

properties:

paramOverPc5:

$ref: '#/components/schemas/ParameterOverPc5Rm'

paramOverUu:

$ref: '#/components/schemas/ParameterOverUuRm'

paramForProSeDd:

$ref: '#/components/schemas/ParamForProSeDdRm'

paramForProSeDc:

$ref: '#/components/schemas/ParamForProSeDcRm'

paramForProSeU2NRelUe:

$ref: '#/components/schemas/ParamForProSeU2NRelUeRm'

paramForProSeRemUe:

$ref: '#/components/schemas/ParamForProSeRemUeRm'

paramForProSeU2URelUe:

$ref: '#/components/schemas/ParamForProSeU2URelUeRm'

paramForProSeEndUe:

$ref: '#/components/schemas/ParamForProSeEndUeRm'

paramForRangingSlPos:

$ref: '#/components/schemas/ParamForRangingSlPosRm'

urspGuidance:

type: array

items:

$ref: '#/components/schemas/UrspRuleRequest'

minItems: 1

description: Contains the service parameter used to guide the URSP.

a2xParamsPc5:

$ref: '#/components/schemas/A2xParamsPc5Rm'

tnaps:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TnapId'

minItems: 1

description: Contains the TNAP IDs collocated with the 5G-RG(s) of a specific user.

nullable: true

subNotifEvents:

type: array

items:

$ref: '#/components/schemas/Event'

minItems: 1

nullable: true

notificationDestination:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

ParameterOverPc5:

description: >

Represents configuration parameters for V2X communications over PC5 reference point.

type: string

ParameterOverPc5Rm:

description: >

Represents the same as the ParameterOverPc5 data type but with the nullable:true property.

type: string

nullable: true

ParameterOverUu:

description: >

Represents configuration parameters for V2X communications over Uu reference point.

type: string

ParameterOverUuRm:

description: >

Represents the same as the ParameterOverUu data type but with the nullable:true property.

type: string

nullable: true

ParamForProSeDd:

description: Represents the service parameters for 5G ProSe direct discovery.

type: string

ParamForProSeDdRm:

description: >

This data type is defined in the same way as the ParamForProSeDd data type,

but with the OpenAPI nullable property set to true.

type: string

nullable: true

ParamForProSeDc:

description: Represents the service parameters for 5G ProSe direct communications.

type: string

ParamForProSeDcRm:

description: >

This data type is defined in the same way as the ParamForProSeDc data type,

but with the OpenAPI nullable property set to true.

type: string

nullable: true

ParamForProSeU2NRelUe:

description: Represents the service parameters for 5G ProSe UE-to-network relay UE.

type: string

ParamForProSeU2NRelUeRm:

description: >

This data type is defined in the same way as the ParamForProSeU2NRelay data type,

but with the OpenAPI nullable property set to true.

type: string

nullable: true

ParamForProSeRemUe:

description: Represents the service parameters for 5G ProSe Remote UE.

type: string

ParamForProSeRemUeRm:

description: >

This data type is defined in the same way as the ParamForProSeRemUe data type,

but with the OpenAPI nullable property set to true.

type: string

nullable: true

ParamForProSeU2URelUe:

description: Represents the service parameters for 5G ProSe UE-to-UE relay UE.

type: string

ParamForProSeU2URelUeRm:

description: >

This data type is defined in the same way as the ParamForProSeU2URelay data type,

but with the OpenAPI nullable property set to true.

type: string

nullable: true

ParamForProSeEndUe:

description: Represents the service parameters for 5G ProSe End UE.

type: string

ParamForProSeEndUeRm:

description: >

This data type is defined in the same way as the ParamForProSeEndUe data type,

but with the OpenAPI nullable property set to true.

type: string

nullable: true

ParamForRangingSlPos:

description: Represents the service parameters for ranging and sidelink positioning.

type: string

ParamForRangingSlPosRm:

description: >

This data type is defined in the same way as the ParamForRangingslpos data type,

but with the OpenAPI nullable property set to true.

type: string

nullable: true

A2xParamsPc5:

description: >

Represents configuration parameters for A2X communications over PC5 reference point.

type: string

A2xParamsPc5Rm:

description: >

Represents the same as the A2xParamsPc5 data type but with the nullable:true property.

type: string

nullable: true

UrspRuleRequest:

description: Contains parameters that can be used to guide the URSP.

type: object

properties:

trafficDesc:

$ref: '#/components/schemas/TrafficDescriptorComponents'

relatPrecedence:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

visitedNetDescs:

type: array

items:

$ref: '#/components/schemas/NetworkDescription'

minItems: 1

description: >

Each element identifies one or more PLMN IDs where AF guidance for VPLMN-specific

URSP rule applies.

routeSelParamSets:

type: array

items:

$ref: '#/components/schemas/RouteSelectionParameterSet'

minItems: 1

description: >

Sets of parameters that may be used to guide the Route Selection Descriptors of the

URSP.

RouteSelectionParameterSet:

description: >

Contains parameters that can be used to guide the Route Selection

Descriptors of the URSP.

type: object

properties:

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

precedence:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

spatialValidityAreas:

type: array

items:

$ref: 'TS29522\_AMPolicyAuthorization.yaml#/components/schemas/GeographicalArea'

minItems: 1

description: >

Indicates where the route selection parameters apply. It may correspond

to a geographical area, for example using a geographic shape that

is known to the AF and is configured by the operator to correspond to a list

of or TAIs.

spatialValidityTais:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Tai'

minItems: 1

description: >

Indicates the TAIs in which the route selection parameters apply. This attribute is

applicable only within the 5GC and it shall not be included in the request messages of

untrusted AFs for URSP guidance.

pduSessType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionType'

Event:

anyOf:

- type: string

enum:

- SUCCESS\_UE\_POL\_DEL\_SP

- UNSUCCESS\_UE\_POL\_DEL\_SP

- type: string

description: >

This string provides forward-compatibility with future extensions to the enumeration

and is not used to encode content defined in the present version of this API.

description: |

Represents the AF subscribe to event notification of the outcome related to the

invocation of AF provisioned service parameters.

Possible values are:

- SUCCESS\_UE\_POL\_DEL\_SP: Successful UE Policy Delivery related to

the invocation of AF provisioned Service Parameters.

- UNSUCCESS\_UE\_POL\_DEL\_SP: Unsuccessful UE Policy Delivery related to the invocation of AF

provisioned Service Parameters.

AfNotification:

description: >

Notifications upon AF Service Parameter Authorization Update e.g. to

revoke the authorization, and/or AF subscribed event notification of the

outcome related to the invocation of service parameter provisioning.

type: object

properties:

subscription:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

reportEvent:

$ref: '#/components/schemas/Event'

authResult:

$ref: '#/components/schemas/AuthorizationResult'

gpsis:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

minItems: 1

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

eventInfo:

$ref: '#/components/schemas/EventInfo'

required:

- subscription

anyOf:

- required: [reportEvent]

- required: [authResult]

TrafficDescriptorComponents:

description: Traffic descriptor components for the requested URSP.

type: object

properties:

appDescs:

type: object

additionalProperties:

$ref: 'TS29522\_5GLANParameterProvision.yaml#/components/schemas/AppDescriptor'

minProperties: 1

description: >

Describes the operation systems and the corresponding applications for each

operation systems. The key of map is osId.

flowDescs:

type: array

items:

type: string

minItems: 1

description: >

Represents a 3-tuple with protocol, server ip and server port for UL/DL

application traffic. The content of the string has the same encoding as the IPFilterRule

AVP value as defined in IETF RFC 6733.

domainDescs:

type: array

items:

type: string

minItems: 1

description: >

FQDN(s) or a regular expression which are used as a domain name matching

criteria.

ethFlowDescs:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EthFlowDescription'

minItems: 1

description: >

Descriptor(s) for destination information of non-IP traffic in which only

ethernet flow description is defined.

dnns:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

minItems: 1

description: This is matched against the DNN information provided by the application.

connCaps:

type: array

items:

$ref: '#/components/schemas/ConnectionCapabilities'

minItems: 1

description: >

This is matched against the information provided by a UE application when it

requests a network connection with certain capabilities.

anyOf:

- required: [appDescs]

- required: [flowDescs]

- required: [domainDescs]

- required: [ethFlowDescs]

- required: [dnns]

- required: [connCaps]

NetworkDescription:

description: >

Represents the description of a PLMN, by the definition of the PLMN ID, the MCC (and

applicable MNC(s)) or the indication of any PLMN.

type: object

properties:

plmnId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

mcc:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Mcc'

mncs:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Mnc'

minItems: 1

anyPlmnInd:

type: boolean

description: Indicates any PLMN.

oneOf:

- required: [plmnId]

- required: [mcc]

- required: [anyPlmnInd]

AuthorizationResult:

anyOf:

- type: string

enum:

- AUTH\_REVOKED

- type: string

description: >

This string provides forward-compatibility with future extensions to the enumeration

and is not used to encode content defined in the present version of this API.

description: |

Represents the NEF notify the AF about the service parameters authorization updates result,

e.g. to revoke an authorization.

Possible values are:

- AUTH\_REVOKED: Indicated the service parameters authorization is revoked.

EventInfo:

description: Indicates the event information.

type: object

properties:

failureCause:

$ref: '#/components/schemas/Failure'

Failure:

oneOf:

- type: string

enum:

- UNSPECIFIED

- UE\_NOT\_REACHABLE

- UNKNOWN

- UE\_TEMP\_UNREACHABLE

- type: string

description: >

This string provides forward-compatibility with future extensions to the enumeration

and is not used to encode content defined in the present version of this API.

description: |

Represents the failure reason for the unsuccessful result.

Possible values are:

- UNSPECIFIED: Indicates the PCF received the UE sent UE policy delivery service cause #111

(Protocol error, unspecified).

- UE\_NOT\_REACHABLE: Indicates the PCF received the notification from the AMF that the UE is

not reachable.

- UNKNOWN: Indicates unknown reasons upon no response from the UE, e.g. UPDS message type is

not defined or not implemented by the UE, or not compatible with the UPDS state, in which

the UE shall ignore the UPDS message.

- UE\_TEMP\_UNREACHABLE: Indicates the PCF received the notification from the AMF that the UE

is not reachable but the PCF will retry again.

ConnectionCapabilities:

anyOf:

- type: string

enum:

- IMS

- MMS

- SUPL

- INTERNET

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration and is not used to encode

content defined in the present version of this API.

description: |

Represents the information provided by a UE application when it requests a network

connection with certain capabilities.

Possible values are:

- IMS: Indicates the connection capability to support IMS service.

- MMS: Indicates the connection capability to support MMS service.

- SUPL: Indicates the connection capability to support SUPL service.

- INTERNET: Indicates the connection capability to support Internet service.

\* \* \* \* End of changes \* \* \* \*