**3GPP TSG-CT3 Meeting #130C3-234119**

**Xiamen, China, 9th – 13th October 2023**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** | **0754** | **rev** | **1** | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Corrections to the User Consent Revocation Notification definition |
|  |  |
| ***Source to WG:*** | Huawei, Nokia, Nokia Shanghai Bell |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | NBI18 |  | ***Date:*** | 2023-09-29 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | The following issues have been identified in the definition of the User Consent Revocation Notification:* In Table 5.3.3A.3.2-1, the description field wrongly refers to the TrafficInfluSub data type of the Nnef\_TrafficInfluence API defined in TS 29.522, whereas this notification is defined for the Nnef\_EventExposure API (reusing the SCEF MonitoringEvent API).
* The description field of the "revocationNotifUri" attribute indicates that this attribute is present when the "UserConsentRevocation" is supported by the AF. This may be confusing as the presence of this attribute is tied to the support of this feature by both the AF and NEF, not only the AF.
 |
|  |  |
| ***Summary of change:*** | This CR proposes to:* Correct the above mentioned issues.
 |
|  |  |
| ***Consequences if not approved:*** | * Wrong/confusing provisions related to the User Consent Revocation Notification remains in the specification.
 |
|  |  |
| ***Clauses affected:*** | 5.3.2.1.2, 5.3.3A.3.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR does not impact the OpenAPI descriptions defined in this specification. |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* \* Start of changes \* \* \* \*

##### 5.3.2.1.2 Type: MonitoringEventSubscription

This type represents a subscription to monitoring an event. The same structure is used in the subscription request and subscription response.

Table 5.3.2.1.2-1: Definition of type MonitoringEventSubscription

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | Cardinality | Description | Applicability (NOTE 3) |
| self | Link | 0..1 | Link to the resource "Individual Monitoring Event Subscription". This parameter shall be supplied by the SCEF in HTTP responses. |  |
| supportedFeatures | SupportedFeatures | 0..1 | Used to negotiate the supported optional features of the API as described in clause 5.2.7.This attribute shall be provided in the POST request and in the response of successful resource creation. |  |
| mtcProviderId | string | 0..1 | Identifies the MTC Service Provider and/or MTC Application. (NOTE 7) |  |
| appIds | array(string) | 0..N | Identifies the Application Identifier(s). (NOTE 16) | AppDetection\_5G |
| externalId | ExternalId | 0..1 | Identifies a user as defined in Clause 4.6.2 of 3GPP TS 23.682 [2].This attribute may also be present in a monitoring event subscription response message, if the "UEId\_retrieval" feature is supported and the corresponding request message includes the "ueIpAddr" attribute or the "ueMacAddr" attribute.(NOTE 1) (NOTE 5) |  |
| msisdn | Msisdn | 0..1 | Identifies the MS internal PSTN/ISDN number allocated for a UE.(NOTE 1) (NOTE 5) |  |
| addedExternalIds | array(ExternalId) | 0..N | Indicates addition of the external Identifier(s) within the active group. | Partial\_group\_modification |
| addedMsisdns | array(Msisdn) | 0..N | Indicates addition of the MSISDN(s) within the active group. | Partial\_group\_modification |
| excludedExternalIds | array(ExternalId) | 0..N | Indicates cancellation of the external Identifier(s) within the active group. | Partial\_group\_modification |
| excludedMsisdns | array(Msisdn) | 0..N | Indicates cancellation of the MSISDN(s) within the active group. | Partial\_group\_modification |
| externalGroupId | ExternalGroupId | 0..1 | Identifies a user group as defined in Clause 4.6.2 of 3GPP TS 23.682 [2].(NOTE 1) (NOTE 6) |  |
| addExtGroupIds | array(ExternalGroupId) | 0..N | Identifies user groups as defined in Clause 4.6.2 of 3GPP TS 23.682 [2].(NOTE 1) (NOTE 6) | Number\_of\_UEs\_in\_an\_area\_notification, Number\_of\_UEs\_in\_an\_area\_notification\_5G |
| ipv4Addr | Ipv4Addr | 0..1 | Identifies the Ipv4 address.(NOTE 1) | Location\_notification,Communication\_failure\_notification |
| ipv6Addr  | Ipv6Addr | 0..1 | Identifies the Ipv6 address.(NOTE 1) | Location\_notification,Communication\_failure\_notification |
| dnn | Dnn | 0..1 | Identifies a DNN, a full DNN with both the Network Identifier and Operator Identifier, or a DNN with the Network Identifier only. (NOTE 8) (NOTE 16) | Session\_Management\_Enhancement, UEId\_retrieval, AppDetection\_5G |
| notificationDestination | Link | 1 | An URI of a notification destination that T8 message shall be delivered to. |  |
| requestTestNotification | boolean | 0..1 | Set to "true" by the SCS/AS to request the SCEF to send a test notification as defined in clause 5.2.5.3. Set to "false" by the SCS/AS indicates not request SCEF to send a test notificationDefault "false" if omitted. | Notification\_test\_event |
| websockNotifConfig | WebsockNotifConfig | 0..1 | Configuration parameters to set up notification delivery over Websocket protocol as defined in clause 5.2.5.4. | Notification\_websocket |
| monitoringType | MonitoringType | 1 | Enumeration of monitoring type. Refer to clause 5.3.2.4.3. |  |
| maximumNumberOfReports | integer | 0..1 | Identifies the maximum number of event reports to be generated by the HSS, MME/SGSN as specified in clause 5.6.0 of 3GPP TS 23.682 [2].(NOTE 2, NOTE 9, NOTE 13)If "monitoringType" is "NUM\_OF\_REGD\_UES" or "NUM\_OF\_ESTD\_PDU\_SESSIONS", this attribute may also be provided with a value of 1 to indicate that one-time reporting of the network slice status information is requested by the AF. |  |
| monitorExpireTime | DateTime | 0..1 | Identifies the absolute time at which the related monitoring event request is considered to expire, as specified in clause 5.6.0 of 3GPP TS 23.682 [2].When the "monitoringType" is set to either "NUM\_OF\_REGD\_UES" or "NUM\_OF\_ESTD\_PDU\_SESSIONS", this attribute shall be absent in the response to a one-time reporting monitoring subscription request.(NOTE 2) |  |
| repPeriod | DurationSec | 0..1 | Identifies the periodic time for the event reports. (NOTE 8, NOTE 9, NOTE 13)If "monitoringType" is "NUM\_OF\_REGD\_UES" or "NUM\_OF\_ESTD\_PDU\_SESSIONS", this attribute may be provided. When provided, it also indicates that periodic reporting of the network slice status information is requested by the AF. |  |
| groupReportGuardTime | DurationSec | 0..1 | Identifies the time for which the SCEF can aggregate the monitoring event reports detected by the UEs in a group and report them together to the SCS/AS, as specified in clause 5.6.0 of 3GPP TS 23.682 [2]. |  |
| maximumDetectionTime | DurationSec | 0..1 | If "monitoringType" is "LOSS\_OF\_CONNECTIVITY", this parameter may be included to identify the maximum period of time after which the UE is considered to be unreachable. | Loss\_of\_connectivity\_notification |
| reachabilityType | ReachabilityType | 0..1 | If "monitoringType" is "UE\_REACHABILITY", this parameter shall be included to identify whether the request is for "Reachability for SMS" or "Reachability for Data". | Ue-reachability\_notification |
| maximumLatency | DurationSec | 0..1 | If "monitoringType" is "UE\_REACHABILITY", this parameter may be included to identify the maximum delay acceptable for downlink data transfers. | Ue-reachability\_notification |
| maximumResponseTime | DurationSec | 0..1 | If "monitoringType" is "UE\_REACHABILITY", this parameter may be included to identify the length of time for which the UE stays reachable to allow the SCS/AS to reliably deliver the required downlink data. | Ue-reachability\_notification |
| suggestedNumberOfDlPackets | integer | 0..1 | If "monitoringType" is "UE\_REACHABILITY", this parameter may be included to identify the number of packets that the serving gateway shall buffer in case that the UE is not reachable. | Ue-reachability-notification |
| idleStatusIndication | boolean | 0..1 | If "monitoringType" is set to "UE\_REACHABILITY" or "AVAILABILITY\_AFTER\_DDN\_FAILURE", this parameter may be included to indicate the notification of when a UE, for which PSM is enabled, transitions into idle mode.- "true": indicate enabling of notification- "false": indicate no need to notifyDefault: "false" if omitted. | Ue-reachability\_notification,Availability\_after\_DDN\_failure\_notification,Availability\_after\_DDN\_failure\_notification\_enhancement |
| locationType | LocationType | 0..1 | If "monitoringType" is "LOCATION\_REPORTING" or "NUMBER\_OF\_UES\_IN\_AN\_AREA", this parameter shall be included to identify whether the request is for Current Location, Initial Location or Last known Location. (NOTE 4) | Location\_notification, Number\_of\_UEs\_in\_an\_area\_notification, Number\_of\_UEs\_in\_an\_area\_notification\_5G,eLCS |
| accuracy | Accuracy | 0..1 | If "monitoringType" is "LOCATION\_REPORTING", this parameter may be included to identify the desired level of accuracy of the requested location information, as described in clause 4.9.2 of 3GPP TS 23.682 [2]. (NOTE 10, NOTE 11)For 5G, if the eLCS feature is not supported, the default value is "TA\_RA". | Location\_notification,eLCS |
| minimumReportInterval | DurationSec | 0..1 | If "monitoringType" is "LOCATION\_REPORTING", this parameter may be included to identify a minimum time interval between Location Reporting notifications. If the "ldrType" attribute is present and set to "ENTERING\_INTO\_AREA". "LEAVING\_FROM\_AREA", "BEING\_INSIDE\_AREA" or "MOTION", this attribute shall not be included if the maximumNumberOfReports attribute is present and set to one time event. | Location\_notification,eLCS |
| maxRptExpireIntvl | DurationSec | 0..1 | If "monitoringType" is "LOCATION\_REPORTING", this parameter may be included to identify a maximum time interval between Location Reporting notifications. If the "ldrType" attribute is present and set to "ENTERING\_INTO\_AREA". "LEAVING\_FROM\_AREA", "BEING\_INSIDE\_AREA" or "MOTION", this attribute shall not be included if the maximumNumberOfReports attribute is present and set to one time event. | eLCS |
| samplingInterval | DurationSec | 0..1 | If "monitoringType" is "LOCATION\_REPORTING", this parameter may be included to identify the maximum time interval between consecutive evaluations by a UE of a trigger event. | eLCS |
| reportingLocEstInd | boolean | 0..1 | If "monitoringType" is "LOCATION\_REPORTING", this parameter may be included to indicate whether event reporting requires the location information.Set to "true", indiates the location estimation information shall be included in event reporting.Set to "false", indicates the location estimation information shall not be included in event reporting.Default: "false" if omitted. | eLCS |
| linearDistance | LinearDistance | 0..1 | If "monitoringType" is "LOCATION\_REPORTING", this parameter may be included to indicate the linear(straight line) distance threshold for motion event reporting. | eLCS |
| locQoS | LocationQoS | 0..1 | If "monitoringType" is "LOCATION\_REPORTING", this parameter may be included to indicate the expected location QoS requirement for an immediate MT-LR or deferred MT-LR.The "Multiple QoS Class" (i.e. the "lcsQosClass" attribute within the LocationQoS data structure is set to "MULTIPLE\_QOS") shall only be used when the "MUTIQOS" feature is supported.(NOTE 10) | eLCS, MULTIQOS |
| svcId | ServiceIdentity | 0..1 | If "monitoringType" is "LOCATION\_REPORTING", this parameter may be included to indicate the service identity of AF. | eLCS |
| ldrType | LdrType | 0..1 | If "monitoringType" is "LOCATION\_REPORTING", this parameter may be included to indicate the event type for a deferred MT-LR. | eLCS |
| velocityRequested | VelocityRequested | 0..1 | If "monitoringType" is "LOCATION\_REPORTING", this parameter may be included to indicate if the velocity of the target UE is requested or not. | eLCS |
| maxAgeOfLocEst | AgeOfLocationEstimate | 0..1 | If "monitoringType" is "LOCATION\_REPORTING", this parameter may be included to indicate acceptable maximum age of location estimate. | eLCS |
| locTimeWindow | TimeWindow | 0..1 | If "monitoringType" is "LOCATION\_REPORTING", this parameter may be included to indicate the starting time and ending time for a deferred MT-LR. | eLCS |
| supportedGADShapes | array(SupportedGADShapes) | 0..N | Supported Geographical Area Description shapes. | eLCS |
| codeWord | CodeWord | 0..1 | Code word. | eLCS |
| associationType | AssociationType | 0..1 | If "monitoringType" is "CHANGE\_OF\_IMSI\_IMEI\_ASSOCIATION", this parameter shall be included to identify whether the change of IMSI-IMEI or IMSI-IMEISV association shall be detected. | Change\_of\_IMSI\_IMEI\_association\_notification |
| plmnIndication | boolean | 0..1 | If "monitoringType" is "ROAMING\_STATUS", this parameter may be included to indicate the notification of UE's Serving PLMN ID.- "true": The value shall be used to indicate enabling of notification;- "false": The value shall be used to indicate disabling of notification.Default: "false" if omitted. | Roaming\_status\_notification |
| locationArea | LocationArea | 0..1 | If "monitoringType" is "NUMBER\_OF\_UES\_IN\_AN\_AREA", this parameter may be included to indicate the area within which the SCS/AS requests the number of UEs.If "monitoringType" is "AREA\_OF\_INTEREST", this parameter shall be included to indicate the area within which the SCS/AS requests the presence status of a specific UAV. | Number\_of\_UEs\_in\_an\_area\_notification, UAV |
| locationArea5G | LocationArea5G | 0..1 | If "monitoringType" is "NUMBER\_OF\_UES\_IN\_AN\_AREA", this parameter may be included to indicate the area within which the AF requests the number of UEs. If "monitoringType" is "LOCATION\_REPORTING", this parameter may be included to indicate the area within which the AF requests the area event of the target UE. (NOTE 12)If "monitoringType" is "AREA\_OF\_INTEREST", this parameter shall be included to indicate the area within which the AF requests the presence status of a specific UAV. | Number\_of\_UEs\_in\_an\_area\_notification\_5G, eLCS, UAV |
| dddTraDescriptors | array(DddTrafficDescriptor) | 0..N | The traffic descriptor(s) of the downlink data source. May be included for event "DOWNLINK\_DATA\_DELIVERY\_STATUS" or "AVAILABILITY\_AFTER\_DDN\_FAILURE". | Downlink\_data\_delivery\_status\_5G,Availability\_after\_DDN\_failure\_notification\_enhancement |
| dddStati | array(DlDataDeliveryStatus) | 0..N | May be included for event "DOWNLINK\_DATA\_DELIVERY\_STATUS". The subscribed stati (delivered, transmitted, buffered) for the event. If omitted all stati are subscribed. | Downlink\_data\_delivery\_status\_5G |
| monitoringEventReport | MonitoringEventReport | 0..1 | Identifies a monitoring event report which is sent from the SCEF to the SCS/AS. |  |
| apiNames | array(string) | 0..N | If "monitoringType" is "API\_SUPPORT\_CAPABILITY", this parameter may be included. Each element identifies the name of an API.It shall set as {apiName} part of the URI structure for each T8 or N33 API as defined in the present specification or 3GPP TS 29.522 [62], respectively.This allows the SCS/AS to request the capability change for its interested APIs. If it is omitted, the SCS/AS requests to be notified for capability change for all APIs the SCEF+NEF supports.  | API\_support\_capability\_notification |
| tgtNsThreshold | SACInfo | 0..1 | Indicates the monitoring threshold value, for the network slice identified by the "snssai" attirbute, upon which event notification(s) are triggered.This attribute may be provided if the "monitoringType" attribute is set to "NUM\_OF\_REGD\_UES" or "NUM\_OF\_ESTD\_PDU\_SESSIONS". When provided, it also indicates that threshold based reporting of the network slice status information is requested by the AF.(NOTE 13) | NSAC |
| nsRepFormat | SACRepFormat | 0..1 | Indicates the requested NSAC reporting format, i.e. "PERCENTAGE" or "NUMERICAL".It shall be provided only if the "monitoringType" attribute is set to "NUM\_OF\_REGD\_UES" or "NUM\_OF\_ESTD\_PDU\_SESSIONS" and periodic reporting is requested (i.e. the "repPeriod" attribute is provided instead of the "tgtNsThreshold" attribute) or one-time reporting is requested (i.e. the "maximumNumberOfReports" attribute is provided with a value of 1). | NSAC |
| afServiceId | string | 0..1 | Contains the identifier of a service on behalf of which the AF is sending the request.It may be provided by an untrusted AF and only if the "monitoringType" attribute is set to either "NUM\_OF\_REGD\_UES" or "NUM\_OF\_ESTD\_PDU\_SESSIONS".(NOTE 15) | NSAC |
| snssai | Snssai | 0..1 | Indicates the S-NSSAI that the event monitoring subscription is targeting.This attribute may be provided if the "monitoringType" attribute is set to "NUM\_OF\_REGD\_UES" or "NUM\_OF\_ESTD\_PDU\_SESSIONS".This attribute may also be provided if the "monitoringType" attribute is set to "PDN\_CONNECTIVITY\_STATUS" or "DOWNLINK\_DATA\_DELIVERY\_STATUS".(NOTE 8) (NOTE 15) (NOTE 16) | NSAC, Session\_Management\_Enhancement, UEId\_retrieval, AppDetection\_5G |
| immediateRep | boolean | 0..1 | Indicates that immediate reporting is requested or not.- "true": indicate an immediate reporting is requested.- "false": indicate an immediate reporting is not requested.Default value: "false" if omitted.This attribute may be included if the "monitoringType" is set to either "NUM\_OF\_REGD\_UES" or "NUM\_OF\_ESTD\_PDU\_SESSIONS" when the "NSAC" feature is supported.(NOTE 13)This attribute may also be included if the SCS/AS requires immediate reporting of the subscribed event(s) when the "enNB1\_5G" feature is supported.(NOTE 4) | NSAC, enNB1\_5G |
| uavPolicy | UavPolicy | 0..1 | If "monitoringType" is "AREA\_OF\_INTEREST", this parameter may be included to indicate the 3GPP network to take corresponding action. | UAV |
| subType | SubType | 0..1 | If "monitoringType" is "NUMBER\_OF\_UES\_IN\_AN\_AREA", this parameter may be included to indicate the subscription type to be listed in the Event report.(NOTE 14) | UAV |
| sesEstInd | boolean | 0..1 | If "monitoringType" is "NUMBER\_OF\_UES\_IN\_AN\_AREA", this parameter may be included. If set to “true”, it indicates that only UE’s with “PDU session established for DNN(s) subject to aerial service” are to be listed in the Event report.If set to "false", it indicates that UE’s with "PDU session established for DNN(s) subject to aerial service" are not to be listed in the Event report.Default: "false" if omitted.(NOTE 14) | UAV |
| addnMonTypes | array(MonitoringType) | 0..N | Additional monitoring types. | enNB |
| addnMonEventReports | array(MonitoringEventReport) | 0..N | Additional monitoring event reports.May only be provided if the "addnMonTypes" attribute is provided in the same subscription creation/update request. | enNB |
| ueIpAddr | IpAddr | 0..1 | UE IP address. | UEId\_retrieval |
| ueMacAddr | MacAddr48 | 0..1 | UE MAC address. | UEId\_retrieval |
| revocationNotifUri | Uri | 0..1 | Contains the URI via which the AF desires to receive user consent revocation notifications. | UserConsentRevocation |
| NOTE 1: One of the properties "externalId", "msisdn", "ipv4Addr", "ipv6Addr" or "externalGroupId" shall be included for features "Location\_notification" and "Communication\_failure\_notification";. One of the properties "externalId", "msisdn" or "externalGroupId" shall be included for feature "eLCS". "ipv4Addr" or "ipv6Addr" is required for monitoring via the PCRF for an individual UE. One of the properties "externalId", "msisdn" or "externalGroupId" shall be included for features "Pdn\_connectivity\_status", "Loss\_of\_connectivity\_notification", "Ue-reachability\_notification", "Change\_of\_IMSI\_IMEI\_association\_notification", "Roaming\_status\_notification", "Availability\_after\_DDN\_failure\_notification" and "Availability\_after\_DDN\_failure\_notification\_enhancement".The property "externalGroupId" shall be included for the "GMEC" feature to subscribe to the group member list change event reporting.NOTE 2: Inclusion of either "maximumNumberOfReports" (with a value higher than 1) or "monitorExpireTime" makes the Monitoring Request a Continuous Monitoring Request, where the SCEF sends Notifications until either the maximum number of reports or the monitoring duration indicated by the property "monitorExpireTime" is exceeded. The "maximumNumberOfReports" with a value 1 makes the Monitoring Request a One-time Monitoring Request. At least one of "maximumNumberOfReports" or "monitorExpireTime" shall be provided.NOTE 3: Properties marked with a feature as defined in clause 5.3.4 are applicable as described in clause 5.2.7. If no features are indicated, the related property applies for all the features.NOTE 4: In this release, for features "Number\_of\_UEs\_in\_an\_area\_notification" and "Number\_of\_UEs\_in\_an\_area\_notification\_5G", locationType shall be set to "LAST\_KNOWN\_LOCATION". For 5G, if the "locationType" attribute sets to "LAST\_KNOWN\_LOCATION", the "maximumNumberOfReports" attribute shall set to 1 as a One-time Monitoring Request. For 5G, when the "enNB1\_5G" feature is supported and the "immediateRep" attribute is present set to "true" and outside the scope of the "NSAC" feature, then the "locationType" shall be set to "LAST\_KNOWN\_LOCATION"; when the "immediateRep" is present set to "false" and outside the scope of the "NSAC" feature, then the "locationType" shall be set to "CURRENT\_LOCATION".NOTE 5: The property does not apply for the features "Number\_of\_UEs\_in\_an\_area\_notification" and "Number\_of\_UEs\_in\_an\_area\_notification\_5G".NOTE 6: For the features "Number\_of\_UEs\_in\_an\_area\_notification" and "Number\_of\_UEs\_in\_an\_area\_notification\_5G", the property "externalGroupId" may be included for single group and "addExtGroupIds" may be included for multiple groups but not both.NOTE 7: The SCEF should check received MTC provider identifier and then the SCEF may: - override it with local configured value and send it to HSS;- send it directly to the HSS; or- reject the monitoring configuration request.NOTE 8: This property is only applicable for the NEF.NOTE 9: The value of the "maximumNumberOfReports" attribute sets to 1 and the "repPeriod" attribute are mutually exclusive.NOTE 10: If the "eLCS" feature is supported, the "accuracy" attribute and "locQoS" attribute are mutually exclusive, and only the "GEO\_AREA" value is applicable for the"accuracy" attribute.NOTE 11: The value of "TWAN\_ID" is only applicable when the monitoring subscription is via the PCRF as described in clause 4.4.2.2.4.NOTE 12: If the "eLCS" feature is supported, only the "geographicAreas" attribute within the "locationArea5G" attribute is applicable.NOTE 13: For the "NSAC" feature, if the "maximumNumberOfReports" attribute is provided with a value of 1, the "repPeriod" attribute and the "tgtNsThreshold" attribute shall not be provided and the "immediateRep" attribute shall be provided and set to true; otherwise, either the "repPeriod" attribute or the "tgtNsThreshold" attribute shall be provided, and if immediate reporting is requested, the "immediateRep" attribute shall be provided and set to true.NOTE 14: For the feature "UAV", the event "Number of UEs present in a geographical area" is used, where "subType" indication and/or "sesEstInd" may be used as event filters.NOTE 15: For the "NSAC" feature, the "snssai" and "afServiceId" attributes are mutually exclusive.NOTE 16: For the "AppDetection\_5G" feature, AF shall provide the "extAppIds" attribute along with "snssai" and "dnn" attributes for subscription of application traffic detection event notification. the subscription request applies to all the UEs associated with the "snssai" and the "dnn" provided in the request. |

\* \* \* \* Next changes \* \* \* \*

##### 5.3.3A.3.2 Target URI

The Callback URI **"{revocationNotifUri}"** shall be used with the the callback URI variables defined in table 5.3.3A.3.2-1.

Table 5.3.3A.3.2-1: Callback URI variables

|  |  |  |
| --- | --- | --- |
| Name | Data type | Definition |
| revocationNotifUri | Uri | Callback reference provided by the AF during the creation or update/modification of the subscription as defined in clauses 5.3.3.2.3.4 and 5.3.3.3.3.2 or 5.3.3.3.3.3. |

\* \* \* \* End of changes \* \* \* \*