**3GPP TSG- Meeting #130 *C3-234435\_R1***

**Xiamen, China, 09th – 13th October, 2023**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** | **0321** | **rev** | **-** | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Correction of the InterfaceDescription data structure | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** |  | | | | | | | | | |
| ***Source to TSG:*** | CT3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NBI18 | | | | |  | ***Date:*** | | |  |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | |  |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | The InterfaceDescription data structure has the "NOTE 2" that is defined but not used in the attribute descriptions. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | The description of the attributes are updated to include NOTE 2. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | * Incorrect specification of the InterfaceDescription data structure; * Low quality of the specification. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 8.2.4.2.3 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | * This CR does not affect any OpenAPI file. | | | | | | | | |
| ***()*** | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

**Additional discussion(if needed):**

**Proposed changes:**

\* \* \* First Change \* \* \* \*

##### 8.2.4.2.3 Type: InterfaceDescription

Table 8.2.4.2.3-1: Definition of type InterfaceDescription

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| ipv4Addr | Ipv4Addr | C | 0..1 | String identifying an IPv4 address (NOTE 1, NOTE 2) |  |
| ipv6Addr | Ipv6Addr | C | 0..1 | String identifying an IPv6 address (NOTE 1, NOTE 2) |  |
| fqdn | Fqdn | C | 0..1 | String containing a Fully Qualified Domain Name. (NOTE 1, NOTE 2) | ExtendedIntfDesc |
| port | Port | O | 0..1 | Port (NOTE 2) |  |
| apiPrefix | string | O | 0..1 | A string representing an optional deployment-specific string (API prefix) in the form of a sequence of path segments that starts with a "/" character. (NOTE 2) | ExtendedIntfDesc |
| securityMethods | array(SecurityMethod) | M | 1..N | Security methods supported by the interface. It takes precedence over the security methods provided in AefProfile, for this specific interface |  |
| NOTE 1: Exactly one of the attributes "ipv4Addr", "ipv6Addr" and "fqdn" shall be included.  NOTE 2: When the contents of this data type are used to construct the apiRoot of an API, they are used as described in clause 4.4.1 of 3GPP TS 29.501 [18]. | | | | | |

\* \* \* End of changes \* \* \* \*