**3GPP TSG-CT WG3 Meeting #130C3-234048**

**Xiamen, China, 9 - 13 October, 2023 (revision of C3-234abc)**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.519** | **CR** | **0447** | **rev** |  | **Current version:** | **17.11.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Corrections on attribute names of SM Policy Data | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei | | | | | | | | | |
| ***Source to TSG:*** | CT3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | 5GS\_Ph1-CT | | | | |  | ***Date:*** | | | 2023-09-20 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **A** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | The "refUmdLimitIds" attribute contained in SmPolicyDnnData data type misaligns with the OpenAPI file.  The "monKeys" attribute contained in LimitIdToMonitoringKey data type misaligns with the OpenAPI file.  The UsageMonitoringDataLimit and UsageMonitoringData data types in the description field and OpenAPI of "refUmdLimitIds" attribute are incorrect. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | This CR proposes to update the attribute names in the data model to align with the OpenAPI file. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Errors in the specification. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.4.2.15, 5.4.2.16, A.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR does not impact any OpenAPI file. | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

**Additional discussion(if needed):**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

#### 5.4.2.15 Type SmPolicyDnnData

Table 5.4.2.15-1: Definition of type SmPolicyDnnData

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| dnn | Dnn | M | 1 | DNN associated with the data |  |
| allowedServices | array(string) | O | 1..N | List of subscriber's allowed service identifiers |  |
| subscCats | array(string) | O | 1..N | List of categories associated with the subscriber |  |
| gbrUI | BitRate | O | 0..1 | Maximum aggregate UL bitrate that can be provided across all GBR QoS Flows in the DNN |  |
| gbrDl | BitRate | O | 0..1 | Maximum aggregate DL bitrate that can be provided across all GBR QoS Flows in the DNN |  |
| adcSupport | boolean | O | 0..1 | Indicates whether application detection and control is enabled for the PDU session.  True: Application detection and control is enabled for the PDU session;  False: Application detection and control is not enabled for the PDU session.  The absence of this attribute means that ADC support is not provisioned for the UE and PDU session. |  |
| subscSpendingLimits | boolean | O | 0..1 | Indicates whether the PCF must enforce policies based on subscriber spending limits.  True: Spending limit control is enabled;  False: Spending limit control is not enabled.  The absence of this attribute means that spending limit control is not provisioned for the UE and PDU session. |  |
| ipv4Index | IpIndex | O | 0..1 | Information that identifies which IP pool or external server is used to allocate the IPv4 address. |  |
| ipv6Index | IpIndex | O | 0..1 | Information that identifies which IP pool or external server is used to allocate the IPv6 address. |  |
| offline | boolean | O | 0..1 | Indicates whether the offline charging is applicable to the PDU session.  True: Offline charging is applicable to the PDU session;  False: Offline charging is not applicable to the PDU session.  The absence of this attribute means that the charging method is not provisioned for the UE and PDU session. |  |
| online | boolean | O | 0..1 | Indicates whether the online charging is applicable to the PDU session.  True: Online charging is applicable to the PDU session;  False: Online charging is not applicable to the PDU session.  The absence of this attribute means that the charging method is not provisioned for the UE and PDU session. |  |
| chfInfo | ChargingInformation | O | 0..1 | The address(es) and, if available, the CHF instance ID and the CHF set ID of the Charging Function. (NOTE) |  |
| refUmDataLimitIds | map(LimitIdToMonitoringKey) | O | 1..N | A reference to the "UsageMonDataLimit" or "UsageMonData" instances for this DNN and SNSSAI that may also include the related monitoring key(s). The key of the map is the limit identifier. |  |
| mpsPriority | boolean | O | 0..1 | True: Indicates subscription to the MPS priority service; priority applies to all traffic on the PDU Session.  False: MPS priority service is not subscribed.  The absence of this attribute means that MPS priority is not provisioned for the UE and PDU session. |  |
| mcsPriority | boolean | O | 0..1 | True: Indicates subscription to the MCS priority service; priority applies to all traffic on the PDU Session.  False: IMS signalling priority service is not subscribed.  The absence of this attribute means that IMS signalling priority is not provisioned for the UE and PDU session. |  |
| imsSignallingPrio | boolean | O | 0..1 | True: Indicates subscription to the IMS signalling priority service; priority only applies to IMS signalling traffic.  False: IMS signalling priority service is not subscribed.  The absence of this attribute means that IMS signalling priority is not provisioned for the UE and PDU session. |  |
| mpsPriorityLevel | integer | O | 0..1 | Relative priority level for the multimedia priority services |  |
| mcsPriorityLevel | integer | O | 0..1 | Relative priority level for the mission critical services |  |
| praInfos | map(PresenceInfo) | O | 1..N | Presence reporting area information. Each PresenceInfo element shall include the Presence Reporting Area Identifier within the "praId" attribute and, for a UE-dedicated presence reporting area, shall also include the list of elements composing the presence reporting area.  A "praId" may indicate a Presence Reporting Area Set.  The "praId" attribute within the PresenceInfo data type shall also be the key of the map.  The attribute "presenceState" shall not be present. |  |
| bdtRefIds | map(BdtReferenceIdRm) | O | 1..N | Identifies transfer policies of background data transfer.  Any string value can be used as a key of the map. | EnhancedBackgroundDataTransfer |
| locRoutNotAllowed | boolean | O | 0..1 | Identifies whether AF influence on traffic routing is allowed or not.  True: if no local routing is allowed;  False: local routing is allowed.  The absence of this attribute means that AF influence on traffic routing is not provisioned for the UE and PDU session. |  |
| NOTE: When the feature "CHFsetSupport" is supported, the "secondaryChfAddress" may be omitted (see 3GPP TS 29.512 [12], clause 4.2.2.3.1). | | | | | |

\*\*\* Next Change \*\*\*

#### 5.4.2.16 Type LimitIdToMonitoringKey

Table 5.4.2.16-1: Definition of type LimitIdToMonitoringKey

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| limitId | string | M | 1 | Limit Identifier. |  |
| monkey | array(string) | O | 1..N | Monitoring Keys. |  |
| NOTE: In this Release of the specification there is only one Monitoring Key per Limit Identifier | | | | | |

\*\*\* Next Change \*\*\*

# A.2 Nudr\_DataRepository API for Policy Data

For the purpose of referencing entities in the Open API file defined in this Annex, it shall be assumed that this Open API file is contained in a physical file named "TS29519\_Policy\_Data.yaml".

openapi: 3.0.0

info:

version: '-'

title: Unified Data Repository Service API file for policy data

description: |

The API version is defined in 3GPP TS 29.504

© 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: >

3GPP TS 29.519 V17.8.0; 5G System; Usage of the Unified Data Repository Service for Policy Data,

Application Data and Structured Data for Exposure.

url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.519/'

paths:

/policy-data/ues/{ueId}:

parameters:

- name: ueId

in: path

required: true

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/VarUeId'

get:

summary: Retrieve the policy data for a subscriber

operationId: ReadPolicyData

tags:

- PolicyDataForIndividualUe (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- nudr-dr:policy-data:ues:read

parameters:

- name: supp-feat

in: query

description: Supported Features

required: false

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

- name: data-subset-names

in: query

style: form

explode: false

description: List of policy data subset names

required: false

schema:

type: array

items:

$ref: '#/components/schemas/PolicyDataSubset'

minItems: 2

responses:

'200':

description: Upon success, a response body containing policy data shall be returned.

content:

application/json:

schema:

$ref: '#/components/schemas/PolicyDataForIndividualUe'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/policy-data/ues/{ueId}/am-data:

parameters:

- name: ueId

in: path

required: true

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/VarUeId'

get:

summary: Retrieves the access and mobility policy data for a subscriber

operationId: ReadAccessAndMobilityPolicyData

tags:

- AccessAndMobilityPolicyData (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- nudr-dr:policy-data:ues:am-data:read

responses:

'200':

description: >

Upon success, a response body containing access and mobility policies shall be returned.

content:

application/json:

schema:

$ref: '#/components/schemas/AmPolicyData'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/policy-data/ues/{ueId}/ue-policy-set:

parameters:

- name: ueId

in: path

required: true

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/VarUeId'

get:

summary: Retrieves the UE policy set data for a subscriber

operationId: ReadUEPolicySet

tags:

- UEPolicySet (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- nudr-dr:policy-data:ues:ue-policy-set:read

parameters:

- name: supp-feat

in: query

description: Supported Features

required: false

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

responses:

'200':

description: Upon success, a response body containing UE policies shall be returned.

content:

application/json:

schema:

$ref: '#/components/schemas/UePolicySet'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

put:

summary: Create or modify the UE policy set data for a subscriber

operationId: CreateOrReplaceUEPolicySet

tags:

- UEPolicySet (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- nudr-dr:policy-data:ues:ue-policy-set:create

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/UePolicySet'

responses:

'201':

description: >

Successful case. The resource has been successfully created and a response body

containing a representation of the created UEPolicySet resource shall be returned.

content:

application/json:

schema:

$ref: '#/components/schemas/UePolicySet'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'200':

description: >

Successful case. The resource has been successfully created and a response body

containing UE policies shall be returned.

content:

application/json:

schema:

$ref: '#/components/schemas/UePolicySet'

'204':

description: >

Successful case. The resource has been successfully updated and no additional content

is to be sent in the response message.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

patch:

summary: Modify the UE policy set data for a subscriber

operationId: UpdateUEPolicySet

tags:

- UEPolicySet (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- nudr-dr:policy-data:ues:ue-policy-set:modify

requestBody:

required: true

content:

application/merge-patch+json:

schema:

$ref: '#/components/schemas/UePolicySetPatch'

responses:

'204':

description: >

Successful case. The resource has been successfully updated and no additional content is

to be sent in the response message.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/policy-data/ues/{ueId}/sm-data:

get:

summary: Retrieves the session management policy data for a subscriber

operationId: ReadSessionManagementPolicyData

tags:

- SessionManagementPolicyData (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- nudr-dr:policy-data:ues:sm-data:read

parameters:

- name: ueId

in: path

required: true

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/VarUeId'

- name: snssai

in: query

required: false

content:

application/json:

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

- name: dnn

in: query

required: false

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

- name: fields

in: query

description: attributes to be retrieved

required: false

schema:

type: array

items:

type: string

minItems: 1

- name: supp-feat

in: query

description: Supported Features

required: false

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

responses:

'200':

description: Upon success, a response body containing SmPolicyData shall be returned.

content:

application/json:

schema:

$ref: '#/components/schemas/SmPolicyData'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

patch:

summary: Modify the session management policy data for a subscriber

operationId: UpdateSessionManagementPolicyData

tags:

- SessionManagementPolicyData (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- nudr-dr:policy-data:ues:sm-data:modify

parameters:

- name: ueId

in: path

required: true

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/VarUeId'

requestBody:

required: true

content:

application/merge-patch+json:

schema:

$ref: '#/components/schemas/SmPolicyDataPatch'

responses:

'204':

description: >

Successful case. The resource has been successfully updated and no

additional content is to be sent in the response message.

'200':

description: Expected response to a valid request

content:

application/json:

schema:

$ref: '#/components/schemas/SmPolicyData'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/policy-data/ues/{ueId}/sm-data/{usageMonId}:

get:

summary: Retrieve a usage monitoring resource

operationId: ReadUsageMonitoringInformation

tags:

- UsageMonitoringInformation (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- nudr-dr:policy-data:ues:sm-data:read

parameters:

- name: ueId

in: path

required: true

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/VarUeId'

- name: usageMonId

in: path

required: true

schema:

type: string

- name: supp-feat

in: query

description: Supported Features

required: false

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

responses:

'200':

description: Successful case. The usage monitoring data is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/UsageMonData'

'204':

description: The resource was found but no usage monitoring data is available.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

put:

summary: Create a usage monitoring resource

operationId: CreateUsageMonitoringResource

tags:

- UsageMonitoringInformation (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- nudr-dr:policy-data:ues:sm-data:create

parameters:

- name: ueId

in: path

required: true

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/VarUeId'

- name: usageMonId

in: path

required: true

schema:

type: string

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/UsageMonData'

responses:

'201':

description: >

Successful case. The resource has been successfully created and a response body is

returned containing a representation of the resource.

content:

application/json:

schema:

$ref: '#/components/schemas/UsageMonData'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

summary: Delete a usage monitoring resource

operationId: DeleteUsageMonitoringInformation

tags:

- UsageMonitoringInformation (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- nudr-dr:policy-data:ues:sm-data:modify

parameters:

- name: ueId

in: path

required: true

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/VarUeId'

- name: usageMonId

in: path

required: true

schema:

type: string

responses:

'204':

description: Successful case. The resource has been successfully deleted.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/policy-data/sponsor-connectivity-data/{sponsorId}:

parameters:

- name: sponsorId

in: path

required: true

schema:

type: string

get:

summary: Retrieves the sponsored connectivity information for a given sponsorId

operationId: ReadSponsorConnectivityData

tags:

- SponsorConnectivityData (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- nudr-dr:policy-data:sponsor-connectivity-data:read

responses:

'200':

description: >

Upon success, a response body containing Sponsor Connectivity Data shall be returned.

content:

application/json:

schema:

$ref: '#/components/schemas/SponsorConnectivityData'

'204':

description: The resource was found but no Sponsor Connectivity Data is available.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/policy-data/bdt-data:

get:

summary: Retrieves the BDT data collection

operationId: ReadBdtData

tags:

- BdtData (Store)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- nudr-dr:policy-data:bdt-data:read

parameters:

- name: bdt-ref-ids

in: query

description: List of the BDT reference identifiers.

required: false

schema:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/BdtReferenceId'

minItems: 1

style: form

explode: false

- name: supp-feat

in: query

description: Supported Features

required: false

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

responses:

'200':

description: Upon success, a response body containing the BDT data shall be returned.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/BdtData'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/policy-data/bdt-data/{bdtReferenceId}:

parameters:

- name: bdtReferenceId

in: path

required: true

schema:

type: string

get:

summary: Retrieves the BDT data information associated with a BDT reference Id

operationId: ReadIndividualBdtData

tags:

- IndividualBdtData (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- nudr-dr:policy-data:bdt-data:read

parameters:

- name: supp-feat

in: query

description: Supported Features

required: false

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

responses:

'200':

description: Upon success, a response body containing the BDT data shall be returned.

content:

application/json:

schema:

$ref: '#/components/schemas/BdtData'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

put:

summary: Creates an BDT data resource associated with an BDT reference Id

operationId: CreateIndividualBdtData

tags:

- IndividualBdtData (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- nudr-dr:policy-data:bdt-data:create

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/BdtData'

responses:

'201':

description: Successful case. The resource has been successfully created.

content:

application/json:

schema:

$ref: '#/components/schemas/BdtData'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

patch:

summary: Modifies an BDT data resource associated with an BDT reference Id

operationId: UpdateIndividualBdtData

tags:

- IndividualBdtData (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- nudr-dr:policy-data:bdt-data:modify

requestBody:

required: true

content:

application/merge-patch+json:

schema:

$ref: '#/components/schemas/BdtDataPatch'

responses:

'200':

description: Expected response to a valid request

content:

application/json:

schema:

$ref: '#/components/schemas/BdtData'

'204':

description: >

Successful case. The resource has been successfully updated and no additional content

is to be sent in the response message.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

summary: Deletes an BDT data resource associated with an BDT reference Id

operationId: DeleteIndividualBdtData

tags:

- IndividualBdtData (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- nudr-dr:policy-data:bdt-data:modify

responses:

'204':

description: Successful case. The resource has been successfully deleted.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/policy-data/subs-to-notify:

post:

summary: Create a subscription to receive notification of policy data changes

operationId: CreateIndividualPolicyDataSubscription

tags:

- PolicyDataSubscriptions (Collection)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data:subs-to-notify

- nudr-dr:policy-data:subs-to-notify:create

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/PolicyDataSubscription'

responses:

'201':

description: >

Upon success, a response body containing a representation of each Individual

subscription resource shall be returned.

content:

application/json:

schema:

$ref: '#/components/schemas/PolicyDataSubscription'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

callbacks:

policyDataChangeNotification:

'{$request.body#/notificationUri}':

post:

requestBody:

required: true

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/PolicyDataChangeNotification'

minItems: 1

responses:

'204':

description: No Content, Notification was successful

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/policy-data/subs-to-notify/{subsId}:

parameters:

- name: subsId

in: path

required: true

schema:

type: string

put:

summary: Modify a subscription to receive notification of policy data changes

operationId: ReplaceIndividualPolicyDataSubscription

tags:

- IndividualPolicyDataSubscription (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- nudr-dr:policy-data:subs-to-notify:modify

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/PolicyDataSubscription'

responses:

'200':

description: The individual subscription resource was updated successfully.

content:

application/json:

schema:

$ref: '#/components/schemas/PolicyDataSubscription'

'204':

description: >

The individual subscription resource was updated successfully and no

additional content is to be sent in the response message.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

summary: Delete the individual Policy Data subscription

operationId: DeleteIndividualPolicyDataSubscription

tags:

- IndividualPolicyDataSubscription (Document)

responses:

'204':

description: Upon success, an empty response body shall be returned.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/policy-data/ues/{ueId}/operator-specific-data:

get:

summary: Retrieve the operator specific policy data of an UE

operationId: ReadOperatorSpecificData

tags:

- OperatorSpecificData (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- nudr-dr:policy-data:ues:operator-specific-data:read

parameters:

- name: ueId

in: path

description: UE Id

required: true

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/VarUeId'

- name: fields

in: query

description: attributes to be retrieved

required: false

schema:

type: array

items:

type: string

minItems: 1

- name: supp-feat

in: query

description: Supported Features

required: false

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

responses:

'200':

description: Expected response to a valid request

content:

application/json:

schema:

type: object

additionalProperties:

$ref: 'TS29505\_Subscription\_Data.yaml#/components/schemas/OperatorSpecificDataContainer'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

patch:

summary: Modify the operator specific policy data of a UE

operationId: UpdateOperatorSpecificData

tags:

- OperatorSpecificData (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- nudr-dr:policy-data:ues:operator-specific-data:modify

parameters:

- name: ueId

in: path

description: UE Id

required: true

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/VarUeId'

requestBody:

content:

application/json-patch+json:

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PatchItem'

required: true

responses:

'204':

description: No content. Response to successful modification.

'200':

description: Expected response to a valid request

content:

application/json:

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PatchResult'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

put:

summary: Create or modify the operator specific policy data of a UE

operationId: ReplaceOperatorSpecificData

tags:

- OperatorSpecificData (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- nudr-dr:policy-data:ues:operator-specific-data:create

parameters:

- name: ueId

in: path

description: UE Id

required: true

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/VarUeId'

requestBody:

required: true

content:

application/json:

schema:

type: object

additionalProperties:

$ref: 'TS29505\_Subscription\_Data.yaml#/components/schemas/OperatorSpecificDataContainer'

responses:

'200':

description: OK

content:

application/json:

schema:

type: object

additionalProperties:

$ref: 'TS29505\_Subscription\_Data.yaml#/components/schemas/OperatorSpecificDataContainer'

'201':

description: >

Successful case. When the feature OSDResource\_Create\_Delete is supported

and the resource has been successfully created, a response body containing a

representation of the created OperatorSpecificData resource shall be returned.

content:

application/json:

schema:

type: object

additionalProperties:

$ref: 'TS29505\_Subscription\_Data.yaml#/components/schemas/OperatorSpecificDataContainer'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'204':

description: The resource has been successfully updated.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

summary: When the feature OSDResource\_Create\_Delete is supported, delete OperatorSpecificData resource

operationId: DeleteOperatorSpecificData

tags:

- OperatorSpecificData (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- nudr-dr:policy-data:ues:operator-specific-data:modify

parameters:

- name: ueId

in: path

required: true

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/VarUeId'

responses:

'204':

description: Successful case. The resource has been successfully deleted.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/policy-data/plmns/{plmnId}/ue-policy-set:

parameters:

- name: plmnId

in: path

required: true

schema:

$ref: 'TS29505\_Subscription\_Data.yaml#/components/schemas/VarPlmnId'

get:

summary: Retrieve the UE policy set data for an H-PLMN

operationId: ReadPlmnUePolicySet

tags:

- PlmnUePolicySet (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- nudr-dr:policy-data:plmns:ue-policy-set:read

responses:

'200':

description: Upon success, a response body containing UE policies shall be returned.

content:

application/json:

schema:

$ref: '#/components/schemas/UePolicySet'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'412':

$ref: 'TS29571\_CommonData.yaml#/components/responses/412'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/policy-data/slice-control-data/{snssai}:

parameters:

- name: snssai

in: path

required: true

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

get:

summary: Retrieves a network Slice specific policy control data resource

operationId: ReadSlicePolicyControlData

tags:

- SlicePolicyControlData (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- nudr-dr:policy-data:slice-control-data:read

parameters:

- name: supp-feat

in: query

description: Supported Features

required: false

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

responses:

'200':

description: >

Successful case. The network slice specific policy control data shall be returned.

content:

application/json:

schema:

$ref: '#/components/schemas/SlicePolicyData'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

patch:

summary: Modify a network Slice specific policy control data resource

operationId: UpdateSlicePolicyControlData

tags:

- SlicePolicyControlData (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- nudr-dr:policy-data:slice-control-data:modify

requestBody:

required: true

content:

application/merge-patch+json:

schema:

$ref: '#/components/schemas/SlicePolicyDataPatch'

responses:

'200':

description: >

The resource has been successfully updated and a response body containing network

slice specific policy control data shall be returned.

content:

application/json:

schema:

$ref: '#/components/schemas/SlicePolicyData'

'204':

description: >

The resource has been successfully updated and no additional content is

to be sent in the response message.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/policy-data/mbs-session-pol-data/{polSessionId}:

parameters:

- name: polSessionId

description: >

Represents the identifier of the MBS Session Policy Control Data.

in: path

required: true

schema:

$ref: '#/components/schemas/MbsSessPolDataId'

get:

summary: Retrieve MBS Session Policy Control Data for an MBS Session.

operationId: GetMBSSessPolCtrlData

tags:

- MBSSessionPolicyControlData (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:policy-data

- nudr-dr:policy-data:mbs-session-pol-data:read

responses:

'200':

description: >

OK. The requested MBS Session Policy Control Data is successfully returned.

content:

application/json:

schema:

$ref: '#/components/schemas/MbsSessPolCtrlData'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

schemas:

PolicyDataForIndividualUe:

description: Contains policy data for a given subscriber.

type: object

properties:

uePolicyDataSet:

$ref: '#/components/schemas/UePolicySet'

smPolicyDataSet:

$ref: '#/components/schemas/SmPolicyData'

amPolicyDataSet:

$ref: '#/components/schemas/AmPolicyData'

umData:

type: object

additionalProperties:

$ref: '#/components/schemas/UsageMonData'

minProperties: 1

description: >

Contains UM policies. The value of the limit identifier is used as the key of the map.

operatorSpecificDataSet:

type: object

additionalProperties:

$ref: 'TS29505\_Subscription\_Data.yaml#/components/schemas/OperatorSpecificDataContainer'

minProperties: 1

description: >

Contains Operator Specific Data resource data. The key of the map is operator

specific data element name and the value is the operator specific data of the UE.

AmPolicyData:

description: Contains the AM policy data for a given subscriber.

type: object

properties:

praInfos:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

minProperties: 1

description: >

Contains Presence reporting area information. The praId attribute within the

PresenceInfo data type is the key of the map.

subscCats:

type: array

items:

type: string

minItems: 1

UePolicySet:

description: Contains the UE policy data for a given subscriber.

type: object

properties:

praInfos:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

minProperties: 1

description: >

Contains Presence reporting area information. The praId attribute within the

PresenceInfo data type is the key of the map.

subscCats:

type: array

items:

type: string

minItems: 1

uePolicySections:

type: object

additionalProperties:

$ref: '#/components/schemas/UePolicySection'

minProperties: 1

description: >

Contains the UE Policy Sections. The UE Policy Section Identifier is used as

the key of the map.

upsis:

type: array

items:

type: string

minItems: 1

allowedRouteSelDescs:

type: object

additionalProperties:

$ref: '#/components/schemas/PlmnRouteSelectionDescriptor'

minProperties: 1

description: >

Contains allowed route selection descriptors per serving PLMN for a UE.

The serving PLMN identifier is the key of the map.

andspInd:

type: boolean

pei:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

osIds:

type: array

items:

$ref: '#/components/schemas/OsId'

minItems: 1

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

resetIds:

type: array

items:

type: string

minItems: 1

UePolicySetPatch:

description: Contains the UE policy set for a given subscriber.

type: object

properties:

uePolicySections:

type: object

additionalProperties:

$ref: '#/components/schemas/UePolicySection'

minProperties: 1

description: >

Contains the UE Policy Sections. The UE Policy Section Identifier is used

as the key of the map.

upsis:

type: array

items:

type: string

minItems: 1

andspInd:

type: boolean

pei:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

osIds:

type: array

items:

$ref: '#/components/schemas/OsId'

minItems: 1

UePolicySection:

description: Contains the UE policy section.

type: object

properties:

uePolicySectionInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Bytes'

upsi:

type: string

required:

- uePolicySectionInfo

- upsi

SmPolicyData:

description: Contains the SM policy data for a given subscriber.

type: object

properties:

smPolicySnssaiData:

type: object

additionalProperties:

$ref: '#/components/schemas/SmPolicySnssaiData'

minProperties: 1

description: >

Contains Session Management Policy data per S-NSSAI for all the SNSSAIs

of the subscriber. The key of the map is the S-NSSAI.

umDataLimits:

type: object

additionalProperties:

$ref: '#/components/schemas/UsageMonDataLimit'

minProperties: 1

description: >

Contains a list of usage monitoring profiles associated with the subscriber.

The limit identifier is used as the key of the map.

umData:

type: object

additionalProperties:

$ref: '#/components/schemas/UsageMonData'

minProperties: 1

description: >

Contains the remaining allowed usage data associated with the subscriber.

The limit identifier is used as the key of the map.

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

resetIds:

type: array

items:

type: string

minItems: 1

required:

- smPolicySnssaiData

SmPolicySnssaiData:

description: Contains the SM policy data for a given subscriber and S-NSSAI.

type: object

properties:

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

smPolicyDnnData:

type: object

additionalProperties:

$ref: '#/components/schemas/SmPolicyDnnData'

minProperties: 1

description: >

Session Management Policy data per DNN for all the DNNs of the indicated S-NSSAI.

The key of the map is the DNN.

ueSliceMbr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SliceMbr'

required:

- snssai

SmPolicyDnnData:

description: Contains the SM policy data for a given DNN (and S-NSSAI).

type: object

properties:

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

allowedServices:

type: array

items:

type: string

minItems: 1

subscCats:

type: array

items:

type: string

minItems: 1

gbrUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

gbrDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

adcSupport:

type: boolean

subscSpendingLimits:

type: boolean

ipv4Index:

$ref: '#/components/schemas/IpIndex'

ipv6Index:

$ref: '#/components/schemas/IpIndex'

offline:

type: boolean

online:

type: boolean

chfInfo:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/ChargingInformation'

refUmDataLimitIds:

type: object

additionalProperties:

$ref: '#/components/schemas/LimitIdToMonitoringKey'

minProperties: 1

description: >

A reference to the UsageMonDataLimit or UsageMonData instancesfor this DNN and SNSSAI

that may also include the related monitoring key(s).

The key of the map is the limit identifier.

mpsPriority:

type: boolean

mcsPriority:

type: boolean

imsSignallingPrio:

type: boolean

mpsPriorityLevel:

type: integer

mcsPriorityLevel:

type: integer

praInfos:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

minProperties: 1

description: >

Contains Presence reporting area information. The praId attribute within the

PresenceInfo data type is the key of the map.

bdtRefIds:

type: object

additionalProperties:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/BdtReferenceIdRm'

minProperties: 1

description: >

Identifies transfer policies of background data transfer. Any string value can

be used as a key of the map.

nullable: true

locRoutNotAllowed:

type: boolean

required:

- dnn

UsageMonDataLimit:

description: Contains usage monitoring control data for a subscriber.

type: object

properties:

limitId:

type: string

scopes:

type: object

additionalProperties:

$ref: '#/components/schemas/UsageMonDataScope'

minProperties: 1

description: >

Identifies the SNSSAI and DNN combinations to which the usage monitoring data

limit applies. The S-NSSAI is the key of the map.

umLevel:

$ref: '#/components/schemas/UsageMonLevel'

startDate:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

endDate:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

usageLimit:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/UsageThreshold'

resetPeriod:

$ref: '#/components/schemas/TimePeriod'

required:

- limitId

UsageMonData:

description: Contains remain allowed usage data for a subscriber.

type: object

properties:

limitId:

type: string

scopes:

type: object

additionalProperties:

$ref: '#/components/schemas/UsageMonDataScope'

minProperties: 1

description: >

Identifies the SNSSAI and DNN combinations for remain allowed usage data

for a subscriber. The S-NSSAI is the key of the map.

umLevel:

$ref: '#/components/schemas/UsageMonLevel'

allowedUsage:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/UsageThreshold'

resetTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

resetIds:

type: array

items:

type: string

minItems: 1

required:

- limitId

LimitIdToMonitoringKey:

description: >

Contains the limit identifier and the corresponding monitoring key for a given

S-NSSAI and DNN.

type: object

properties:

limitId:

type: string

monkey:

type: array

items:

type: string

minItems: 1

required:

- limitId

nullable: true

UsageMonDataScope:

description: >

Contains a SNSSAI and DNN combinations to which the UsageMonData instance belongs to.

type: object

properties:

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

dnn:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

minItems: 1

required:

- snssai

TimePeriod:

description: Contains the periodicity for the defined usage monitoring data limits.

type: object

properties:

period:

$ref: '#/components/schemas/Periodicity'

maxNumPeriod:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

required:

- period

SponsorConnectivityData:

description: >

Contains the sponsored data connectivity related information for a sponsor identifier.

type: object

properties:

aspIds:

type: array

items:

type: string

required:

- aspIds

BdtData:

description: Contains the background data transfer data.

type: object

properties:

aspId:

type: string

transPolicy:

$ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/TransferPolicy'

bdtRefId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/BdtReferenceId'

nwAreaInfo:

$ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

numOfUes:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

volPerUe:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/UsageThreshold'

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

trafficDes:

$ref: 'TS29122\_ResourceManagementOfBdt.yaml#/components/schemas/TrafficDescriptor'

bdtpStatus:

$ref: '#/components/schemas/BdtPolicyStatus'

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

resetIds:

type: array

items:

type: string

minItems: 1

required:

- aspId

- transPolicy

PolicyDataSubscription:

description: Identifies a subscription to policy data change notification.

type: object

properties:

notificationUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

notifId:

type: string

monitoredResourceUris:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

monResItems:

type: array

items:

$ref: '#/components/schemas/ResourceItem'

minItems: 1

excludedResItems:

type: array

items:

$ref: '#/components/schemas/ResourceItem'

minItems: 1

expiry:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

resetIds:

type: array

items:

type: string

minItems: 1

required:

- notificationUri

- monitoredResourceUris

PolicyDataChangeNotification:

description: Contains changed policy data for which notification was requested.

type: object

properties:

amPolicyData:

$ref: '#/components/schemas/AmPolicyData'

uePolicySet:

$ref: '#/components/schemas/UePolicySet'

plmnUePolicySet:

$ref: '#/components/schemas/UePolicySet'

smPolicyData:

$ref: '#/components/schemas/SmPolicyData'

usageMonData:

$ref: '#/components/schemas/UsageMonData'

SponsorConnectivityData:

$ref: '#/components/schemas/SponsorConnectivityData'

bdtData:

$ref: '#/components/schemas/BdtData'

opSpecData:

$ref: 'TS29505\_Subscription\_Data.yaml#/components/schemas/OperatorSpecificDataContainer'

opSpecDataMap:

type: object

additionalProperties:

$ref: 'TS29505\_Subscription\_Data.yaml#/components/schemas/OperatorSpecificDataContainer'

minProperties: 1

description: >

Operator Specific Data resource data, if changed and notification was requested.

The key of the map is operator specific data element name and the value is the

operator specific data of the UE.

ueId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/VarUeId'

sponsorId:

type: string

bdtRefId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/BdtReferenceId'

usageMonId:

type: string

plmnId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

delResources:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

minItems: 1

notifId:

type: string

reportedFragments:

type: array

items:

$ref: '#/components/schemas/NotificationItem'

minItems: 1

slicePolicyData:

$ref: '#/components/schemas/SlicePolicyData'

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

PlmnRouteSelectionDescriptor:

description: >

Contains the route selection descriptors (combinations of SNSSAI, DNNs, PDU session types,

SSC modes and ATSSS information) allowed by subscription to the UE for a serving PLMN

type: object

properties:

servingPlmn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

snssaiRouteSelDescs:

type: array

items:

$ref: '#/components/schemas/SnssaiRouteSelectionDescriptor'

minItems: 1

required:

- servingPlmn

SnssaiRouteSelectionDescriptor:

description: >

Contains the route selector parameters (DNNs, PDU session types, SSC modes and ATSSS

information) per SNSSAI

type: object

properties:

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

dnnRouteSelDescs:

type: array

items:

$ref: '#/components/schemas/DnnRouteSelectionDescriptor'

minItems: 1

required:

- snssai

DnnRouteSelectionDescriptor:

description: >

Contains the route selector parameters (PDU session types, SSC modes and ATSSS

information) per DNN

type: object

properties:

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

sscModes:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SscMode'

minItems: 1

pduSessTypes:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionType'

minItems: 1

atsssInfo:

description: >

Indicates whether MA PDU session establishment is allowed for this DNN.

When set to value true MA PDU session establishment is allowed for this DNN.

type: boolean

default: false

required:

- dnn

SmPolicyDataPatch:

description: Contains the SM policy data for a given subscriber.

type: object

properties:

umData:

type: object

additionalProperties:

$ref: '#/components/schemas/UsageMonData'

minProperties: 1

description: >

Contains the remaining allowed usage data associated with the subscriber.

The value of the limit identifier is used as the key of the map.

nullable: true

smPolicySnssaiData:

type: object

additionalProperties:

$ref: '#/components/schemas/SmPolicySnssaiDataPatch'

minProperties: 1

description: >

Modifiable Session Management Policy data per S-NSSAI for all the SNSSAIs

of the subscriber. The key of the map is the S-NSSAI.

SmPolicySnssaiDataPatch:

description: Contains the SM policy data for a given subscriber and S-NSSAI.

type: object

properties:

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

smPolicyDnnData:

type: object

additionalProperties:

$ref: '#/components/schemas/SmPolicyDnnDataPatch'

minProperties: 1

description: >

Modifiable Session Management Policy data per DNN for all the DNNs of the

indicated S-NSSAI. The key of the map is the DNN.

required:

- snssai

SmPolicyDnnDataPatch:

description: Contains the SM policy data for a given DNN (and S-NSSAI).

type: object

properties:

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

bdtRefIds:

type: object

additionalProperties:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/BdtReferenceIdRm'

minProperties: 1

description: >

Contains updated transfer policies of background data transfer.

Any string value can be used as a key of the map.

nullable: true

required:

- dnn

ResourceItem:

description: >

Identifies a subscription to policy data change notification when the change occurs

in a fragment (subset of resource data) of a given resource.

type: object

properties:

monResourceUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

items:

type: array

items:

$ref: '#/components/schemas/ItemPath'

minItems: 1

required:

- monResourceUri

- items

NotificationItem:

description: >

Identifies a data change notification when the change occurs in a fragment

(subset of resource data) of a given resource.

type: object

properties:

resourceId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

notifItems:

type: array

items:

$ref: '#/components/schemas/UpdatedItem'

minItems: 1

required:

- resourceId

- notifItems

UpdatedItem:

description: Identifies a fragment of a resource.

type: object

properties:

item:

$ref: '#/components/schemas/ItemPath'

value: {}

required:

- item

- value

BdtDataPatch:

description: Contains the modified background data transfer data.

type: object

properties:

transPolicy:

$ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/TransferPolicy'

bdtpStatus:

$ref: '#/components/schemas/BdtPolicyStatus'

SlicePolicyData:

description: Contains the network slice specific policy control information.

type: object

properties:

mbrUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

mbrDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

remainMbrUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

remainMbrDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

resetIds:

type: array

items:

type: string

minItems: 1

SlicePolicyDataPatch:

description: Contains the modified network slice specific policy control information.

type: object

properties:

remainMbrUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

remainMbrDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

oneOf:

- required: [remainMbrUl]

- required: [remainMbrDl]

MbsSessPolCtrlData:

description: Represents MBS Session Policy Control Data.

type: object

properties:

5qis:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/5Qi'

minItems: 1

maxMbsArpLevel:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ArpPriorityLevel'

maxMbsSessionAmbr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

maxGbr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

MbsSessPolDataId:

description: Represents the identifier used to access the MBS Session Policy Control Data.

type: object

properties:

mbsSessionId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MbsSessionId'

afAppId:

type: string

oneOf:

- required: [mbsSessionId]

- required: [afAppId]

# SIMPLE TYPES:

IpIndex:

description: >

Represents information that identifies which IP pool or external server

is used to allocate the IP address.

type: integer

OsId:

description: Represents the Operating System of the served UE.

type: string

format: uuid

ItemPath:

description: Identifies a fragment (subset of resource data) of a given resource.

type: string

# ENUMS:

UsageMonLevel:

description: Represents the usage monitoring level.

anyOf:

- type: string

enum:

- SESSION\_LEVEL

- SERVICE\_LEVEL

- type: string

Periodicity:

description: Represents the time period.

anyOf:

- type: string

enum:

- YEARLY

- MONTHLY

- WEEKLY

- DAILY

- HOURLY

- type: string

BdtPolicyStatus:

description: Indicates the validation status of a negotiated BDT policy.

anyOf:

- type: string

enum:

- INVALID

- VALID

- type: string

PolicyDataSubset:

description: Indicates a policy data subset.

anyOf:

- type: string

enum:

- AM\_POLICY\_DATA

- SM\_POLICY\_DATA

- UE\_POLICY\_DATA

- UM\_DATA

- OPERATOR\_SPECIFIC\_DATA

- type: string

\*\*\* End of Changes \*\*\*