**3GPP TSG-CT3 Meeting #130C3-234642**

**Xiamen, China, 9 - 13 October, 2023 (Revision of C3-234283)**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **29.552** | **CR** | **0075** | **rev** | **1** | **Current version:** | **18.2.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Procedures for Movement Behaviour Analytics |
|  |  |
| ***Source to WG:*** | Ericsson |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | eNA\_Ph3 |  | ***Date:*** | 2023-09-20 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** |  Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | Procedures for Movement Behaviour Analytics needs to be added to support this new analytics in the specification. |
|  |  |
| ***Summary of change:*** | Adding procedures for Movement Behaviour Analytics. |
|  |  |
| ***Consequences if not approved:*** | Missing procedures for Movement Behaviour Analytics. |
|  |  |
| ***Clauses affected:*** | 5.7.21(new) |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

**Additional discussion(if needed):**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

### 5.7.21 Movement Behaviour Analytics

This procedure is used by the NWDAF service consumer e.g. NEF or AF to obtain Movement Behaviour Analytics provided by NWDAF regarding the location, direction and velocity of UEs during an analytics target period in a target area.



Figure 5.7.21-1: Procedure for Movement Behaviour Analytics

1a. In order to obtain the Movement Behaviour Analytics, the NF may invoke Nnwdaf\_AnalyticsInfo\_Request service operation as described in clause 5.2.3.1.

1b-1c. In order to subscribe to the Movement Behaviour Analytics, the NF may invoke Nnwdaf\_EventsSubscription\_Subscribe service operation as described in clause 5.2.2.1.

2a-2b. If the event is set to "MOVEMENT\_BEHAVIOUR" and the subscription/request is authorized, the NWDAF may invoke Namf\_EventExposure\_Subscribe service operation as described in clause 5.3.2.2.2 of 3GPP TS 29.518 [18] to subscribe to the notification of UE ID and UE positions. The AMF responds to the NWDAF an HTTP "201 Created" response.

3a-3b. If step 2a and step 2b are performed, the AMF invokes Namf\_EventExposure\_Notify service operation as described in 3GPP TS 29.518 [18] clause 5.3.2.4. The NWDAF responds to the AMF an HTTP "204 No Content" response.

4a-4b. The NWDAF may invoke Ngmlc\_Location\_ProvideLocation service operation to retrieve UE Fine granularity locations by sending an HTTP POST request to the URI associated with the "provide-location" custom operation as described in 3GPP TS 29.515 [41] clause 5.2.2.2. The GMLC responds to the NWDAF an HTTP "201 Created" response.

5a-5b. If step 4a and step 4b are performed, the GMLC may invoke Ngmlc\_Location\_EventNotify service operation by sending an HTTP POST request to the NWDAF identified by the notification URI received in step 4a. The NWDAF responds to the GMLC an HTTP "204 No Content" response.

6. The NWDAF derives the Movement Behaviour Analytics based on the data collected from AMF and/or GMLC.

7a. If step 1a is performed, the NWDAF responds to the Nnwdaf\_AnalyticsInfo\_Request service operation as described in clause 5.2.3.1.

7b-7c. If step 1b and step 1c are performed, the NWDAF invokes Nnwdaf\_EventsSusbcription\_Notify service operation as described in clause 5.2.2.1.

NOTE: For details of Nnwdaf\_EventsSubscription\_Subscribe/Unsubscribe/Notify or Nnwdaf\_AnalyticsInfo\_Request service operations refer to 3GPP TS 29.520 [5].

\*\*\* End of Changes \*\*\*