**3GPP TSG-CT WG3 Meeting #130 *C3-234426r1***

**Xiamen, China, 9 - 13 October, 2023**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **29.575** | **CR** | **0069** | **rev** | **-** | **Current version:** | **18.3.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Updates to Nadrf\_MLModelManagement\_RetrievalRequest Service Operation |
|  |  |
| ***Source to WG:*** | Ericsson |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | eNA\_Ph3 |  | ***Date:*** | 2023-09-27 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** |  Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | Cardinality for the "nfInstanceId" and "nfSetId" attributes in the "NadrfMLModelStoreRecord" data type is incorrect. This CR proposes to correct the error in clause 5.2.6.2.2. |
|  |  |
| ***Summary of change:*** | The changes include:* Corrected the errors in clause 5.2.6.2.2.
 |
|  |  |
| ***Consequences if not approved:*** | Errors exist in the specification. |
|  |  |
| ***Clauses affected:*** | 5.2.6.2.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR has no impact to OpenAPI file. |
|  |  |
| ***This CR's revision history:*** |  |

**Additional discussion(if needed):**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

##### 5.2.6.2.2 Type: NadrfMLModelStoreRecord

Table 5.2.6.2.2-1: Definition of type NadrfMLModelStoreRecord

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| nfInstanceId | NfInstanceId | C | 0..1 | NF instanceIdentifier of the NWDAF containing MTLF.(NOTE) |  |
| nfSetId | NfSetId | C | 0..1 | NFset identifier of the NWDAF containing MTLF.(NOTE) |  |
| mlModelInfo | array(MLModelInfo) | M | 1..N | ML Model information. |  |
| suppFeat | SupportedFeatures | C | 0..1 | This IE represents a list of Supported features as described in clause 5.2.7.It shall be present if at least one feature defined in clause 5.2.7 is supported. |  |
| NOTE: One of "nfInstanceId" and "nfSetId" attributes shall be provided. |

\*\*\* End of Changes \*\*\*