**3GPP TSG-CT WG3 Meeting #130C3-234680**

**Xiamen, China, 9 - 13 October, 2023 (revision of C3-234150)**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **29.575** | **CR** | **0063** | **rev** | **1** | **Current version:** | **18.3.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Support of the storage of user consent |
|  |  |
| ***Source to WG:*** | Huawei |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | eNetAE |  | ***Date:*** | 2023-09-22 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | As per clause 6.2.2 in TS 23.288, the consumer needs to check the user consent of the data to be collected, which is defined for a specific purpose such as, e.g. analytics or model training. The consumer needs to take the user consent for the data collection purpose into account when collecting data.However, for the data stored on the ADRF, the current implementation allows the consumer to retrieve the data without checking the user consent. This will cause the consumer, whose purpose is to collect data for analytics, but retrieves the data of which only the user consent for model training is granted.The issue needs to be solved. |
|  |  |
| ***Summary of change:*** | Add an EN for how to ensure that the consumer to comply with the user consent when retrieving data from ADRF. |
|  |  |
| ***Consequences if not approved:*** | The implementation of user consent is incomplete, which may cause potential data security risk. |
|  |  |
| ***Clauses affected:*** | 4.2.2.6.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ... |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR does not impact the OpenAPI file. |
|  |  |
| ***This CR's revision history:*** |  |

**Additional discussion(if needed):**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

##### 4.2.2.6.2 Requesting retrieval and subscription of data or analytics

Figure 4.2.2.6.2-1 shows a scenario where the NF service consumer sends a request to the ADRF to retrieve and subscribe to data or analytics.



Figure 4.2.2.6.2-1: NF service consumer requesting to retrieve and subscribe to data or analytics

The NF service consumer shall invoke the Nadrf\_DataManagement\_RetrievalSubscribe service operation to retrieve and subscribe to data or analytics. The NF service consumer shall send an HTTP POST request with "{apiRoot}/nadrf-datamanagement/<apiVersion>/data-retrieval-subscriptions" as Resource URI representing the "ADRF Data Retrieval Subscriptions" resource, as shown in figure 4.2.2.6.2-1, step 1, to create an "Individual ADRF Data Retrieval Subscription" according to the information in the message body. The NadrfDataRetrievalSubscription data structure provided in the request body shall include:

- notification correlation identfier within the "notifCorrId" attribute;

- one of the following:

- analytics subscription information within the "anaSub" attribute;

- data subscription information within the "dataSub" attribute;

- data set identifier within the "dataSetId" attribute, if the "EnhDataMgmt" feature is supported;

- a notification target address within the "notificationURI" attribute;

- a time window for the data retrieval and subscription within the "timePeriod" attribute;

and may include:

- a Consumer triggered Notification indication within the "consTrigNotif" attribute.

Upon the reception of an HTTP POST request with "{apiRoot}/nadrf-datamanagement/<apiVersion>/data-retrieval-subscriptions" as Resource URI and NadrfDataRetrievalSubscription data structure as request body, the ADRF shall:

- create a new subscription;

- assign a subscriptionId;

- store the subscription.

If the ADRF created an "Individual ADRF Data Retrieval Subscription" resource, the ADRF shall respond with "201 Created" with the message body containing a representation of the created subscription, as shown in figure 4.2.2.6.2-1, step 2. The ADRF shall include a Location HTTP header field. The Location header field shall contain the URI of the created record i.e. "{apiRoot}/nadrf-datamanagement/<apiVersion>/data-retrieval-subscriptions/{subscriptionId}".

If an error occurs when processing the HTTP POST request, the ADRF shall send an HTTP error response as specified in clause 5.1.7.

Editor’s Note: How to ensure that the consumer to comply with the user consent when retrieving data from ADRF is FFS.

\*\*\* End of Changes \*\*\*