**3GPP TSG-CT WG3 Meeting #134 *C3-242453***

**Changsha, China, 15th – 19th April, 2024 (Revision of C3-24xxxx)**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.3* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.122** | **CR** | **0836** | **rev** | **-** | **Current version:** | **18.5.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | NEF monitoring events to assist application AIML operation | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Ericsson | | | | | | | | | |
| ***Source to TSG:*** | CT3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | AIMLsys | | | | |  | ***Date:*** | | | 2024-03-28 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19) Rel-20 (Release 20)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | TS 23.502 Table 4.15.3.1-1: List of events for monitoring capability added Session inactivity time, Traffic volume and UL/DL data rate events upon the early approved CR3786 in AIMLsys, while still not implemented in this TS in the MonitoringEvent API. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Adding Session inactivity time, Traffic volume and UL/DL data rate events in the MonitoringEvent API with new feature. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Not aligned with stage 2 requirement on NEF monitoring events assist application AIML operation. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 2, 5.3.2.1.1, 5.3.2.3.2, 5.3.2.4.3, 5.3.4, A.3 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR introduces backwards compatible feature in the OpenAPI file on MonitoringEvent API. | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

**Additional discussion(if needed):**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 23.682: "Architecture enhancements to facilitate communications with packet data networks and applications".

[3] 3GPP TS 23.032: "Universal Geographical Area Description (GAD)".

[4] Void.

[5] IETF RFC 8259: "The JavaScript Object Notation (JSON) Data Interchange Format".

[6] Hypertext Transfer Protocol (HTTP) Status Code Registry at IANA, <http://www.iana.org/assignments/http-status-codes>.

[7] IETF RFC 3986: "Uniform Resource Identifier (URI): Generic Syntax".

[8] IETF RFC 9457: "Problem Details for HTTP APIs".

[9] 3GPP TS 29.154: "Service capability exposure functionality over Nt reference point".

[10] 3GPP TS 29.214: "Policy and Charging Control over Rx reference point".

[11] 3GPP TS 29.336: "Home Subscriber Server (HSS) diameter interfaces for interworking with packet data networks and applications".

[12] 3GPP TS 29.128: "Mobility Management Entity (MME) and Serving GPRS Support Node (SGSN) interfaces for interworking with packet data networks and applications".

[13] 3GPP TS 29.201: "Representational State Transfer (REST) reference point between Application Function (AF) and Protocol Converter (PC)".

[14] 3GPP TS 23.003: "Numbering, addressing and identification".

[15] IETF RFC 3339: "Date and Time on the Internet: Timestamps".

[16] IETF RFC 9112: "HTTP/1.1".

[17] IETF RFC 9110: "HTTP Semantics".

[18] Void.

[19] Void.

[20] IETF RFC 9111: "HTTP Caching".

[21] Void.

[22] IETF RFC 9113: "HTTP/2".

[23] 3GPP TS 29.155: "Traffic steering control; Representational state transfer (REST) over St reference point".

[24] 3GPP TS 29.368: "Tsp interface protocol between the MTC Interworking Function (MTC-IWF) and Service Capability Server (SCS)".

[25] 3GPP TS 29.337: "Diameter-based T4 interface for communications with packet data networks and applications".

[26] 3GPP TS 29.250: "Nu reference point between SCEF and PFDF for sponsored data connectivity".

[27] Open API: "OpenAPI Specification Version 3.0.0", <https://spec.openapis.org/oas/v3.0.0>.

[28] IETF RFC 1166: "Internet Numbers".

[29] IETF RFC 5952: "A recommendation for Ipv6 address text representation".

[30] 3GPP TS 29.153: "Service capability exposure functionality over Ns reference point".

[31] 3GPP TS 24.250: "Protocol for Reliable Data Service; Stage 3".

[32] IETF RFC 6455: "The Websocket Protocol".

[33] 3GPP TS 29.272: "Mobility Management Entity (MME) and Serving GPRS Support Node (SGSN) related interfaces based on Diameter protocol".

[34] 3GPP TS 29.338: "Diameter based protocols to support Short Message Service (SMS) capable Mobile Management Entities (MMEs)".

[35] 3GPP TS 33.187: "Security aspects of Machine-Type Communications (MTC) and other mobile data applications communications enhancements".

[36] 3GPP TS 29.468: "Group Communication System Enablers for LTE (GCSE\_LTE);MB2 Reference Point;Stage 3".

[37] 3GPP TS 29.116: "Presentational state transfer over xMB reference point between Content Provider and BM-SC".

[38] IETF RFC 5789: "PATCH method for HTTP".

[39] IETF RFC 7396: "JSON Merge Patch".

[40] IETF RFC 8259: "The JavaScript Object Notation (JSON) Data Interchange Format".

[41] YAML (10/2009): "YAML Ain't Markup Language (YAML™) Version 1.2", <http://www.yaml.org/spec/1.2/spec.html>.

[42] 3GPP TS 29.572: "5G System; Location Management Services; Stage 3".

[43] 3GPP TS 23.040: "Technical realization of the Short Message Service (SMS)".

[44] 3GPP TS 29.500: "5G System; Technical Realization of Service Based Architecture; Stage 3".

[45] 3GPP TS 29.571: "5G System; Common Data Types for Service Based Interfaces Stage 3".

[46] IETF RFC 6733: "Diameter Base Protocol".

[47] 3GPP TS 23.222: "Common API Framework for 3GPP Northbound APIs; Stage 2".

[48] 3GPP TS 29.222: "Common API Framework for 3GPP Northbound APIs; Stage 3".

[49] 3GPP TS 29.501: "5G System; Principles and Guidelines for Services Definition; Stage 3".

[50] 3GPP TS 29.554: "5G System; Background Data Transfer Policy Control Service; Stage 3".

[51] IETF RFC 6749: "The OAuth 2.0 Authorization Framework".

[52] 3GPP TS 29.514: "5G System; Policy Authorization Service; Stage 3".

[53] 3GPP TS 33.122: "Security Aspects of Common API Framework for 3GPP Northbound APIs".

[54] 3GPP TS 38.413: "NG-RAN; NG Application Protocol (NGAP)".

[55] 3GPP TS 23.468: "Group Communication System Enablers for LTE (GCSE\_LTE); stage 2".

[56] 3GPP TS 26.348, "Northbound Application Programming Interface (API) for Multimedia Broadcast/Multicast Service (MBMS) at the xMB reference point".

[57] 3GPP TS 29.508: "5G System; Session Management Event Exposure Service; Stage 3".

[58] 3GPP TR 21.900: "Technical Specification Group working methods".

[59] 3GPP TS 36.331: "Evolved Universal Terrestrial Radio Access (E-UTRA) Radio Resource Control (RRC); Protocol Specification".

[60] 3GPP TS 38.331: "NR; Radio Resource Control (RRC) protocol specification".

[61] 3GPP TS 29.675: "User Equipment (UE) radio capability provisioning service; Stage 3".

[62] 3GPP TS 29.522: "5G System; Network Exposure Function Northbound APIs; Stage 3".

[63] 3GPP TS 29.503: "5G System; Unified Data Management Services; Stage 3".

[64] 3GPP TS 24.526: "User Equipment (UE) policies for 5G System (5GS); Stage 3".

[65] 3GPP TS 29.515: "5G System; Gateway Mobile Location Services; Stage 3".

[66] IETF RFC 5322: "Internet Message Format".

[67] IETF RFC 6902: "JavaScript Object Notation (JSON) Patch".

[68] 3GPP TS 33.558: "Security aspects of enhancement of support for enabling edge applications; Stage 2".

[69] IETF RFC 5234: "Augmented BNF for Syntax Specifications: ABNF".

[70] 3GPP TS 29.523: "5G System; Policy Control Event Exposure Service; Stage 3".

[71] IETF RFC 6901: "JavaScript Object Notation (JSON) Pointer".

[72] 3GPP TS 29.565: "5G System; Time Sensitive Communication and Time Synchronization Function Services; Stage 3".

[73] 3GPP TS 29.520: "5G System; Network Data Analytics Services; Stage 3".

\*\*\* 2nd Change \*\*\*

##### 5.3.2.1.1 Introduction

This clause defines data structures to be used in resource representations, including subscription resources.

Table 5.3.2.1.1-1 specifies data types re-used by the MonitoringEvent API from other specifications, including a reference to their respective specifications and when needed, a short description of their use within the MonitoringEvent API.

Table 5.3.2.1.1-1: MonitoringEvent API re-used Data Types

|  |  |  |
| --- | --- | --- |
| Data type | Reference | Comments |
| 2DRelativeLocation | 3GPP TS 29.572 [42] | Represents 2D local co-ordinates with origin corresponding to another known point. |
| 3DRelativeLocation | 3GPP TS 29.572 [42] | Represents 3D local co-ordinates with origin corresponding to another known point. |
| AccuracyFulfilmentIndicator | 3GPP TS 29.572 [42] | The indication whether the obtained location estimate satisfies the requested QoS or not. |
| AgeOfLocationEstimate | 3GPP TS 29.572 [42] | Age of the location estimate for change of location type or motion type of Location deferred report. |
| Angle | 3GPP TS 29.572 [42] | Indicates value of angle |
| ApplicationlayerId | 3GPP TS 29.571 [45] | Represents the Application Layer ID. |
| CivicAddress | 3GPP TS 29.572 [42] | Civic address. |
| CodeWord | 3GPP TS 29.515 [65] | Code word. |
| DddTrafficDescriptor | 3GPP TS 29.571 [45] | Traffic Descriptor of source of downlink data. |
| DlDataDeliveryStatus | 3GPP TS 29.571 [45] | Traffic Descriptor of source of downlink data notifications. |
| Dnn | 3GPP TS 29.571 [45] | Identifies a DNN. |
| Fqdn | 3GPP TS 29.571 [45] | Identifies a FQDN. |
| GeographicArea | 3GPP TS 29.572 [42] | Identifies the geographical information of the user(s). |
| Gpsi | 3GPP TS 29.571 [45] | Represents a GPSI. |
| IpAddr | 3GPP TS 29.571 [45] | UE IP Address. |
| LdrType | 3GPP TS 29.572 [42] | Location deferred requested event type. |
| LinearDistance | 3GPP TS 29.572 [42] | This IE shall be present and set to true if a location estimate is required for motion event report. |
| LocationQoS | 3GPP TS 29.572 [42] | Requested location QoS. |
| MacAddr48 | 3GPP TS 29.571 [45] | MAC Address. |
| MinorLocationQoS | 3GPP TS 29.572 [42] | Minor Location QoS. |
| NetworkAreaInfo | 3GPP TS 29.554 [50] | Identifies a network area information. |
| VelocityRequested | 3GPP TS 29.572 [42] | Velocity of the target UE requested. |
| PatchItem | 3GPP TS 29.571 [45] | Contains the list of changes to be made to a resource according to the JSON PATCH format specified in IETF RFC 6902 [67]. |
| PduSessionInformation | 3GPP TS 29.523 [70] | Represents PDU session identification information. |
| PositioningMethod | 3GPP TS 29.572 [42] | Identifies the positioning method used to obtain the location estimate of the UE. |
| RangeDirection | 3GPP TS 29.572 [42] | Represents the range and direction between two points. |
| RangingSlResult | 3GPP TS 29.572 [42] | Represents the requested result type for ranging and sidelink positioning |
| RelatedUE | 3GPP TS 29.572 [42] | Represents information on the related UE for ranging and sidelink positioning |
| SACEventStatus | 3GPP TS 29.571 [45] | Contains the network slice status information related to network slice admission control. |
| SACInfo | 3GPP TS 29.571 [45] | Represents network slice admission control information to control the triggering of notifications or convey network slice status information. |
| Snssai | 3GPP TS 29.571 [45] | Contains a S-NSSAI. |
| SupportedFeatures | 3GPP TS 29.571 [45] | Used to negotiate the applicability of the optional features defined in table 5.3.4-1. |
| ServiceIdentiy | 3GPP TS 29.515 [65] | Service identity. |
| SupportedGADShapes | 3GPP TS 29.572 [42] | Supported Geographical Area Description shapes. |
| TrafficInformation | 3GPP TS 29.520 [73] | Traffic information including UL/DL data rate and/or Traffic volume. |
| UcPurpose | 3GPP TS 29.503 [63] | Represents the purpose of a user consent. |
| Uinteger | 3GPP TS 29.571 [45] | Represents an unsigned Integer. |
| Uncertainty | 3GPP TS 29.572 [42] | Indicates value of uncertainty. |
| Uri | 5.2.1.3.2 | Represents a URI. |
| UserLocation | 3GPP TS 29.571 [6] | Represents a user location. |
| VelocityEstimate | 3GPP TS 29.572 [42] | UE velocity, if requested and available. |

Table 5.3.2.1.1-2 specifies the data types defined for the MonitoringEvent API.

Table 5.3.2.1.1-2: MonitoringEvent API specific Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Clause defined | Description | Applicability |
| Accuracy | 5.3.2.4.7 | Represents a desired granularity of accuracy for the requested location information. | Location\_notification,  eLCS, EDGEAPP |
| ApiCapabilityInfo | 5.3.2.3.9 | Represents the availability information of supported API. | API\_support\_capability\_notification |
| AppliedParameterConfiguration | 5.3.2.3.8 | Represents the parameter configuration applied in the network. | Enhanced\_param\_config |
| AssociationType | 5.3.2.4.6 | Represents an IMEI or IMEISV to IMSI association. | Change\_of\_IMSI\_IMEI\_association\_notification |
| ConsentRevocNotif | 5.3.2.3.12 | Represents the user consent revocation information conveyed in a user consent revocation notification. | UserConsentRevocation |
| ConsentRevoked | 5.3.2.3.13 | Represents the information related to revoked user consent(s). | UserConsentRevocation |
| FailureCause | 5.3.2.3.6 | Represents the reason of communication failure. | Communication\_failure\_notification |
| GroupMembListChanges | 5.3.2.3.13 | Represents information on the change(s) to a group's members list. | GMEC |
| IdleStatusInfo | 5.3.2.3.3 | Represents the information relevant to when the UE transitions into idle mode. | Ue-reachability\_notification,  Availability\_after\_DDN\_failure\_notification |
| InterfaceIndication | 5.3.2.4.10 | Represents the network entity used for data delivery towards the SCS/AS. | Pdn\_connectivity\_status |
| LocationFailureCause | 5.3.2.4.11 | Represents the cause of location/positioning failure. | eLCS |
| LocationInfo | 5.3.2.3.5 | Represents the user location information. | Location\_notification, eLCS |
| LocationType | 5.3.2.4.5 | Represents a location type. | Location\_notification, Number\_of\_UEs\_in\_an\_area\_notification, Number\_of\_UEs\_in\_an\_area\_notification\_5G,  eLCS |
| MonitoringEventReport | 5.3.2.3.2 | Represents an event monitoring report. |  |
| MonitoringEventReports | 5.3.2.3.10 | Represents one or multiple event monitoring report(s). | enNB |
| MonitoringEventSubscription | 5.3.2.1.2 | Represents a subscription to event(s) monitoring. |  |
| MonitoringNotification | 5.3.2.2.2 | Represents an event monitoring notification. |  |
| MonitoringType | 5.3.2.4.3 | Represents a monitoring event type. |  |
| PdnConnectionInformation | 5.3.2.3.7 | Represents the PDN connection information of the UE. | Pdn\_connectivity\_status |
| PdnConnectionStatus | 5.3.2.4.8 | Represents the PDN connection status. | Pdn\_connectivity\_status |
| PdnType | 5.3.2.4.9 | Represents a PDN connection type. |  |
| ReachabilityType | 5.3.2.4.4 | Represents a reachability type. | Ue-reachability\_notification |
| SACRepFormat | 5.3.2.4.13 | Represents the NSAC reporting format. | NSAC |
| SubType | 5.3.2.4.12 | Represents a subscription type. | UAV |
| UavPolicy | 5.3.2.3.11 | Represents the policy information included in the UAV presence monitoring request. | UAV |
| UePerLocationReport | 5.3.2.3.4 | Represents the number of UEs found at the indicated location. | Number\_of\_UEs\_in\_an\_area\_notification, Number\_of\_UEs\_in\_an\_area\_notification\_5G |
| UpCumEvtRep | 5.3.2.3.18 | Represents the cumulative event report for events reported via user plane. | eLCS\_en |
| UpLocRepAddrAfRm | 5.3.2.3.17 | Represents the user plane addressing information. | eLCS\_en |

\*\*\* 3rd Change \*\*\*

##### 5.3.2.3.2 Type: MonitoringEventReport

This data type represents a monitoring event notification which is sent from the SCEF to the SCS/AS.

Table 5.3.2.3.2-1: Definition of type MonitoringEventReport

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Attribute name | | Data type | | Cardinality | | Description | | Applicability (NOTE 1) | |
| imeiChange | | AssociationType | | 0..1 | | If "monitoringType" is "CHANGE\_OF\_IMSI\_IMEI\_ASSOCIATION", this parameter shall be included to identify the event of change of IMSI-IMEI or IMSI-IMEISV association is detected.  Refer to 3GPP TS 29.336 [11] Clause 8.4.22. | | Change\_of\_IMSI\_IMEI\_association\_notification | |
| externalId | | ExternalId | | 0..1 | | External identifier.  This attribute may also be present in the monitoring event subscription one-time response message, if the "UEId\_retrieval" feature is supported and the corresponding request message includes the "ueIpAddr" attribute or the "ueMacAddr" attribute.  (NOTE 2) | |  | |
| appId | | string | | 0..1 | | Represents the detected application. (NOTE 4) | | AppDetection\_5G | |
| pduSessInfo | | PduSessionInformation | | 0..1 | | Represents PDU session information related to the observed event.  If "monitoringType" is "APPLICATION\_START" and/or "APPLICATION\_STOP", this parameter shall be included to indicate the Application traffic detection details if available. | | AppDetection\_5G | |
| idleStatusInfo | | IdleStatusInfo | | 0..1 | | If "idleStatusIndication" in the "MonitoringEventSubscription"sets to "true", this parameter shall be included to indicate the information when the UE transitions into idle mode. | | Ue-reachability\_notification,  Availability\_after\_DDN\_failure\_notification | |
| locationInfo | | LocationInfo | | 0..1 | | If "monitoringType" is "LOCATION\_REPORTING", this parameter shall be included to indicate the user location related information. | | Location\_notification, eLCS | |
| locFailureCause | | LocationFailureCause | | 0..1 | | Indicates the location positioning failure cause. | | eLCS | |
| lossOfConnectReason | | integer | | 0..1 | | If "monitoringType" is "LOSS\_OF\_CONNECTIVITY", this parameter shall be included if available to identify the reason why loss of connectivity is reported.  Refer to 3GPP TS 29.336 [11] Clause 8.4.58. | | Loss\_of\_connectivity\_notification | |
| unavailPerDur | | DurationSec | | 0..1 | | If "monitoringType" is "LOSS\_OF\_CONNECTIVITY", then this parameter shall be included if available to identify the UE’s Unavailability Period Duration. | | Loss\_of\_connectivity\_notification\_5G | |
| maxUEAvailabilityTime | | DateTime | | 0..1 | | If "monitoringType" is "UE\_REACHABILITY", this parameter may be included to identify the timestamp until which a UE using a power saving mechanism is expected to be reachable for SM delivery.  Refer to Clause 5.3.3.22 of 3GPP TS 29.338 [34]. | | Ue-reachability\_notification | |
| msisdn | | Msisdn | | 0..1 | | Identifies the MS internal PSTN/ISDN number.  (NOTE 2) | |  | |
| monitoringType | | MonitoringType | | 1 | | Identifies the type of monitoring type as defined in clause 5.3.2.4.3. | |  | |
| uePerLocationReport | | UePerLocationReport | | 0..1 | | If "monitoringType" is "NUMBER\_OF\_UES\_IN\_AN\_AREA", this parameter shall be included to indicate the number of UEs found at the location.  If "subType" indicates "AERIAL\_UE" subscription type, this parameter shall be included to indicate the number of UAV’s found at the location. | | Number\_of\_UEs\_in\_an\_area\_notification, Number\_of\_UEs\_in\_an\_area\_notification\_5G | |
| plmnId | | PlmnId | | 0..1 | | If "monitoringType" is "ROAMING\_STATUS" and "plmnIIndication" in the "MonitoringEventSubscription" sets to "true", this parameter shall be included to indicate the UE's serving PLMN. | | Roaming\_status\_notification | |
| reachabilityType | | ReachabilityType | | 0..1 | | If "monitoringType" is "UE\_REACHABILITY", this parameter shall be included to identify the reachability of the UE.  Refer to 3GPP TS 29.336 [11] Clause 8.4.20. | | Ue-reachability\_notification | |
| roamingStatus | | boolean | | 0..1 | | If "monitoringType" is "ROAMING\_STATUS", this parameter shall be set to "true" if the new serving PLMN is different from the HPLMN. Set to false or omitted otherwise. | | Roaming\_status\_notification | |
| failureCause | | FailureCause | | 0..1 | | If "monitoringType" is "COMMUNICATION\_FAILURE", this parameter shall be included to indicate the reason of communication failure. | | Communication\_failure\_notification | |
| eventTime | | DateTime | | 0..1 | | Identifies when the event is detected or received.  Shall be included for each group of UEs. | |  | |
| pdnConnInfoList | | array(PdnConnectionInformation) | | 0..N | | If "monitoringType" is "PDN\_CONNECTIVITY\_STATUS", this parameter shall be included to indicate the PDN connection details. | | Pdn\_connectivity\_status | |
| dddStatus | | DlDataDeliveryStatus | | 0..1 | | If "monitoringType" is "DOWNLINK\_DATA\_DELIVERY\_STATUS", this parameter shall be included to identify the downlink data delivery status detected by the network. | | Downlink\_data\_delivery\_status\_5G | |
| dddTrafDescriptor | | DddTrafficDescriptor | | 0..1 | | If "monitoringType" is "DOWNLINK\_DATA\_DELIVERY\_STATUS", this parameter shall be included to identify the downlink data descriptor impacted by the downlink data delivery status change. | | Downlink\_data\_delivery\_status\_5G | |
| maxWaitTime | | DateTime | | 0..1 | | If "monitoringType" is "DOWNLINK\_DATA\_DELIVERY\_STATUS", this parameter may be included to identify the time before which the data will be buffered. | | Downlink\_data\_delivery\_status\_5G | |
| apiCaps | | array(ApiCapabilityInfo) | | 0..N | | If "monitoringType" is "API\_SUPPORT\_CAPABILITY", this parameter shall be included to indicate the availability of all APIs supported by the serving network or the availability of interested APIs, indicated by the "apiNames" attribute in "MonitoringEventSubscription", supported by the serving network.  If no API is supported by the serving network, an empty apiCaps shall be provided. | | API\_support\_capability\_notification | |
| nSStatusInfo | | SACEventStatus | | 0..1 | | If the "monitoringType" attribute is set to "NUM\_OF\_REGD\_UES" or "NUM\_OF\_ESTD\_PDU\_SESSIONS", this parameter shall be included to indicate the current network slice status information for the concerned network slice.  (NOTE 3) | | NSAC | |
| afServiceId | | string | | 0..1 | | Contains the identifier of the service to which the NSAC reporting is related.  It shall be provided only if it is present in the related NSAC subscription request and the "monitoringType" attribute is set to either "NUM\_OF\_REGD\_UES" or "NUM\_OF\_ESTD\_PDU\_SESSIONS". | | NSAC | |
| servLevelDevId | | string | | 0..1 | | If "monitoringType" is "AREA\_OF\_INTEREST" or "NUMBER\_OF\_UES\_IN\_AN\_AREA" and "subType" indicate "AERIAL\_UE", this parameter may be included to identify the UAV. | | UAV | |
| uavPresInd | | boolean | | 0..1 | | If "monitoringType" is "AREA\_OF\_INTEREST", this parameter shall be set to true if the specified UAV is in the monitoring area. Set to false or omitted otherwise. | | UAV | |
| groupMembListChanges | | GroupMembListChanges | | 0..1 | | Contains information on the change(s) to the group member list.  This attribute shall be present only if the "monitoringType" attribute is set to "GROUP\_MEMBER\_LIST\_CHANGE". | | GMEC | |
| sessInactiveTime | | DurationSec | | 0..1 | | The value of the session inactivity timer.  This attribute shall be present only if the "monitoringType" attribute is set to "SESSION\_INACTIVITY\_TIME". | | | AIMLsys | |
| trafficInfo | | TrafficInformation | | 0..1 | | The value of the UL/DL data rate and/or Traffic volume.  This attribute shall be present only if the "monitoringType" attribute is set to "TRAFFIC\_VOLUME” and/or "UL\_DL\_DATA\_RATE". | | | AIMLsys | |
| NOTE 1: Properties marked with a feature as defined in clause 5.3.4 are applicable as described in clause 5.2.7. If no features are indicated, the related property applies for all the features.  NOTE 2: Identifies the user for which the event occurred. At least one of the properties shall be included.  NOTE 3: If the "eNSAC" feature is supported, the "SACEventStatus" data type shall include an indication to report either the current number of registered UEs or the current number of UEs with at least one PDU session/PDN connection.  NOTE 4: When the "AppDetection\_5G" feature is supported and the "monitoringType" is "APPLICATION\_START" or "APPLICATION\_STOP", the "appId" attribute shall be provided if multiple instances were provided in the "appIds" attribute in the subscription request. | | | | | | | | | |

\*\*\* 4th Change \*\*\*

##### 5.3.2.4.3 Enumeration: MonitoringType

The enumeration MonitoringType represents a monitoring event type. It shall comply with the provisions defined in table 5.3.2.4.3-1.

Table 5.3.2.4.3-1: Enumeration MonitoringType

|  |  |  |
| --- | --- | --- |
| Enumeration value | Description | Applicability (NOTE 1) |
| LOSS\_OF\_CONNECTIVITY | The SCS/AS requests to be notified when the 3GPP network detects that the UE is no longer reachable for signalling or user plane communication | Loss\_of\_connectivity\_notification |
| UE\_REACHABILITY | The SCS/AS requests to be notified when the UE becomes reachable for sending either SMS or downlink data to the UE | Ue-reachability\_notification |
| LOCATION\_REPORTING | The SCS/AS requests to be notified of the current location or the last known location of the UE | Location\_notification, eLCS |
| CHANGE\_OF\_IMSI\_IMEI\_ASSOCIATION | The SCS/AS requests to be notified when the association of an ME (IMEI(SV)) that uses a specific subscription (IMSI) is changed | Change\_of\_IMSI\_IMEI\_association\_notification |
| ROAMING\_STATUS | The SCS/AS queries the UE's current roaming status and requests to get notified when the status changes | Roaming\_status\_notification |
| COMMUNICATION\_FAILURE | The SCS/AS requests to be notified of communication failure events | Communication\_failure\_notification |
| AVAILABILITY\_AFTER\_DDN\_FAILURE | The SCS/AS requests to be notified when the UE has become available after a DDN failure | Availability\_after\_DDN\_failure\_notification, Availability\_after\_DDN\_failure\_notification\_enhancement |
| NUMBER\_OF\_UES\_IN\_AN\_AREA | The SCS/AS requests to be notified the number of UEs in a given geographic area | Number\_of\_UEs\_in\_an\_area\_notification, Number\_of\_UEs\_in\_an\_area\_notification\_5G |
| PDN\_CONNECTIVITY\_STATUS | The SCS/AS requests to be notified when the 3GPP network detects that the UE’s PDN connection is set up or torn down. | Pdn\_connectivity\_status |
| DOWNLINK\_DATA\_DELIVERY\_STATUS | The AF requests to be notified when the 3GPP network detects that the downlink data delivery status is changed. | Downlink\_data\_delivery\_status\_5G |
| API\_SUPPORT\_CAPABILITY | The SCS/AS requests to be notified of the availability of support of service APIs. | API\_support\_capability\_notification |
| NUM\_OF\_REGD\_UES | The AF requests to be notified of the current number of registered UEs for a network slice. | NSAC |
| NUM\_OF\_ESTD\_PDU\_SESSIONS | The AF requests to be notified of the current number of established PDU Sessions for a network slice. | NSAC |
| AREA\_OF\_INTEREST | The SCS/AS requests to be notified when the UAV moves in or out of the geographic area. | UAV |
| GROUP\_MEMBER\_LIST\_CHANGE | The AF requests to be notified of the changes to a group members list. | GMEC |
| APPLICATION\_START | The AF requests to be notified about the start of application traffic has been detected. | AppDetection\_5G |
| APPLICATION\_STOP | The AF requests to be notified about the stop of application traffic has been detected. | AppDetection\_5G |
| SESSION\_INACTIVITY\_TIME | The AF requests to be notified of session inactivity time of the measured UE PDU Session. | AIMLsys |
| TRAFFIC\_VOLUME | The AF requests to be notified of traffic volume of the measured UE. | AIMLsys |
| UL\_DL\_DATA\_RATE | The AF requests to be notified of uplink and downlink data rate of the measured UE. | AIMLsys |
| NOTE 1: Properties marked with a feature as defined in clause 5.3.4 are applicable as described in clause 5.2.7. If no features are indicated, the related property applies for all the features.  NOTE 2: More monitoring types can be added in the future based on stage 2. | | |

\*\*\* 5th Change \*\*\*

### 5.3.4 Used Features

The table below defines the features applicable to the MonitoringEvent API. Those features are negotiated as described in clause 5.2.7.

Table 5.3.4-1: Features used by MonitoringEvent API

|  |  |  |
| --- | --- | --- |
| Feature Number | Feature | Description |
| 1 | Loss\_of\_connectivity\_notification | The SCS/AS is notified when the 3GPP network detects that the UE is no longer reachable for signalling or user plane communication |
| 2 | Ue-reachability\_notification | The SCS/AS is notified when the UE becomes reachable for sending either SMS or downlink data to the UE |
| 3 | Location\_notification | The SCS/AS is notified of the current location or the last known location of the UE |
| 4 | Change\_of\_IMSI\_IMEI\_association\_notification | The SCS/AS is notified when the association of an ME (IMEI(SV)) that uses a specific subscription (IMSI) is changed |
| 5 | Roaming\_status\_notification | The SCS/AS is notified when the UE's roaming status changes |
| 6 | Communication\_failure\_notification | The SCS/AS is notified of communication failure events |
| 7 | Availability\_after\_DDN\_failure\_notification | The SCS/AS is notified when the UE has become available after a DDN failure |
| 8 | Number\_of\_UEs\_in\_an\_area\_notification | The SCS/AS is notified the number of UEs present in a given geographic area  The feature supports pre-5G (e.g. 4G) requirement. |
| 9 | Notification\_websocket | The delivery of notifications over Websocket is supported according to clause 5.2.5.4. This feature requires that the Notification\_test\_event featute is also supported. |
| 10 | Notification\_test\_event | The testing of notification connection is supported according to clause 5.2.5.3. |
| 11 | Subscription\_modification | Modifications of an individual subscription resource. |
| 12 | Number\_of\_UEs\_in\_an\_area\_notification\_5G | The AF is notified the number of UEs present in a given geographic area.  The feature supports the 5G requirement. This feature may only be supported in 5G. |
| 13 | Pdn\_connectivity\_status | The SCS/AS requests to be notified when the 3GPP network detects that the UE’s PDN connection is set up or torn down. |
| 14 | Downlink\_data\_delivery\_status\_5G | The AF requests to be notified when the 3GPP network detects that the downlink data delivery status is changed. The feature is not applicable to pre-5G. |
| 15 | Availability\_after\_DDN\_failure\_notification\_enhancement | The AF is notified when the UE has become available after a DDN failure and the traffic matches the packet filter provided by the AF. The feature is not applicable to pre-5G. |
| 16 | Enhanced\_param\_config | This feature supports the co-existence of multiple event configurations for target UE(s) if there are parameters affecting periodic RAU/TAU timer and/or Active Time. Supporting this feature also requires the support of feature number 1 or 2. |
| 17 | API\_support\_capability\_notification | The SCS/AS is notified of the availability of support of service APIs. This feature is only applicable in interworking SCEF+NEF scenario. |
| 18 | eLCS | This feature supports the enhanced location exposure service (e.g. location information preciser than cell level).  The feature is not applicable to pre-5G (e.g. 4G). |
| 19 | NSAC | This feature controls the support of the Network Slice Admission Control (NSAC) functionalities.  The feature is not applicable to pre-5G (e.g. 4G). |
| 20 | Partial\_group\_modification | This feature supports the partial cancellation and/or partial addition to the group member(s) within the grouped event monitoring subscription. |
| 21 | UAV | The SCS/AS requests to be notified of the UAV presence status in a specific geographic area. This feature is only applicable in interworking SCEF+NEF scenario, or standalone 5G scenario.  This feature requires that Number\_of\_UEs\_in\_an\_area\_notification and Number\_of\_UEs\_in\_an\_area\_notification\_5G features are also supported. |
| 22 | MULTIQOS | This feature indicates the support for "Multiple QoS Class" which enables to support more than one Location QoS during LCS procedures.  This feature requires that the eLCS feature is also supported. |
| 23 | Session\_Management\_Enhancement | This feature supports Session Management enhancement with requested DNN and/or S-NSSAI. This feature requires that the Pdn\_connectivity\_status feature or Downlink\_data\_delivery\_status\_5G feature is also supported. |
| 24 | enNB | Indicates the support of enhancements to the northbound interfaces. |
| 25 | EDGEAPP | This feature controls the support of EDGE applications related functionalities (e.g. support the civic address as a possible location granularity).  The feature is not applicable to pre-5G (e.g. 4G). |
| 26 | UEId\_retrieval | This feature supports AF specific UE ID retrieval which is not applicable to pre-5G (e.g. 4G). |
| 27 | UserConsentRevocation | This feature indicates the support of user consent revocation management and enforcement (e.g. stop data processing) for EDGE applications. |
| 28 | Subscription\_Patch | This feature indicates the support of the PATCH method for partial modification of an existing event monitoring subscription. |
| 29 | GMEC | This feature indicates the support of Generic Group Management, Exposure and Communication Enhancements (e.g. Ggroup Member List Change event reporting).  This feature is not applicable to pre-5G (e.g. 4G). |
| 30 | Loss\_of\_connectivity\_notification\_5G | The AF is notified when the 3GPP network detects that the UE is no longer reachable for signalling or user plane communication.  This feature is not applicable to pre-5G (e.g. 4G). |
| 31 | enNB1 | Indicates the support of enhancements to this northbound API in Rel-18. |
| 32 | AppDetection\_5G | This feature indicates the support of Application traffic detection (start and stop) monitoring event.  This feature is not applicable to pre-5G (e.g. 4G). |
| 33 | enNB1\_5G | Indicates the support of enhancements to this northbound API for 5G in Rel-18.  This feature is not applicable to pre-5G (e.g. 4G). |
| 34 | eLCS\_en | This feature indicates the support of the enhancements to the eLCS feature.  The following functionalities are supported:  - Support the error handling related to the area event reporting for the case where the requested location area is not allowed.  - Support location reporting over user plane between UE and AF.  This feature is not applicable to pre-5G (e.g. 4G). |
| 35 | eNSAC | This feature indicates the support of the enhancements to the NSAC feature.  The following functionalities are supported:  - Support the status notification of the current number of UEs with at least one PDU session/PDN connection.This feature is not applicable to pre-5G (e.g. 4G). |
| 36 | Ranging\_SL | This feature indicates the support of the ranging and sidelink positioning functionality.  The following functionalities are supported:  - Support the ranging and sidelink input/output parameters.  This feature requires the support of eLCS feature.  This feature is not applicable to pre-5G (e.g. 4G). |
| 37 | AIMLsys | This feature indicates the support of AI/ML monitoring events, including Session inactivity time, Traffic volume and UL/DL data rate events.  This feature is not applicable to pre-5G (e.g. 4G). |
| Feature: A short name that can be used to refer to the bit and to the feature, e.g. "Notification".  Description: A clear textual description of the feature. | | |

\*\*\* 6th Change \*\*\*

# A.3 MonitoringEvent API

openapi: 3.0.0

info:

title: 3gpp-monitoring-event

version: 1.3.0-alpha.5

description: |

API for Monitoring Event.

© 2024, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.122 V18.5.0 T8 reference point for Northbound APIs

url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.122/'

security:

- {}

- oAuth2ClientCredentials: []

servers:

- url: '{apiRoot}/3gpp-monitoring-event/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 5.2.4 of 3GPP TS 29.122.

paths:

/{scsAsId}/subscriptions:

get:

summary: Read all or queried active subscriptions for the SCS/AS.

operationId: FetchAllMonitoringEventSubscriptions

tags:

- Monitoring Event Subscriptions

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

- name: ip-addrs

in: query

description: The IP address(es) of the requested UE(s).

required: false

content:

application/json:

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/IpAddr'

minItems: 1

- name: ip-domain

in: query

description: >

The IPv4 address domain identifier. The attribute may only be provided if IPv4 address

is included in the ip-addrs query parameter.

required: false

schema:

type: string

- name: mac-addrs

in: query

description: The MAC address(es) of the requested UE(s).

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

minItems: 1

responses:

'200':

description: OK (Successful get all or queried active subscriptions for the SCS/AS)

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/MonitoringEventSubscription'

minItems: 0

description: Monitoring event subscriptions

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

post:

summary: Creates a new subscription resource for monitoring event notification.

operationId: CreateMonitoringEventSubscription

tags:

- Monitoring Event Subscriptions

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

requestBody:

description: Subscription for notification about monitoring event

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/MonitoringEventSubscription'

callbacks:

notificationDestination:

'{request.body#/notificationDestination}':

post:

requestBody: # contents of the callback message

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/MonitoringNotification'

responses:

'204':

description: No Content (successful notification)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

UserConsentRevocationNotif:

'{request.body#/revocationNotifUri}':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/ConsentRevocNotif'

responses:

'204':

description: No Content (successful notification).

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

responses:

'201':

description: Created (Successful creation of subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/MonitoringEventSubscription'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'200':

description: The operation is successful and immediate report is included.

content:

application/json:

schema:

oneOf:

- $ref: '#/components/schemas/MonitoringEventReport'

- $ref: '#/components/schemas/MonitoringEventReports'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{scsAsId}/subscriptions/{subscriptionId}:

get:

summary: Read an active subscriptions for the SCS/AS and the subscription Id.

operationId: FetchIndMonitoringEventSubscription

tags:

- Individual Monitoring Event Subscription

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

responses:

'200':

description: OK (Successful get the active subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/MonitoringEventSubscription'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

put:

summary: Updates/replaces an existing subscription resource.

operationId: UpdateIndMonitoringEventSubscription

tags:

- Individual Monitoring Event Subscription

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

requestBody:

description: Parameters to update/replace the existing subscription

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/MonitoringEventSubscription'

responses:

'200':

description: OK (Successful update of the subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/MonitoringEventSubscription'

'204':

description: No Content (Successful update of the subscription)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

patch:

summary: Modifies an existing subscription of monitoring event.

operationId: ModifyIndMonitoringEventSubscription

tags:

- Individual Monitoring Event Subscription

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS.

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource.

required: true

schema:

type: string

requestBody:

description: >

This is used for PATCH request for partial cancellation and/or partial addition of certain

UE(s) within an active group.

required: true

content:

application/json-patch+json:

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PatchItem'

minItems: 1

responses:

'204':

description: The resource was modified successfully.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

summary: Deletes an already existing monitoring event subscription.

operationId: DeleteIndMonitoringEventSubscription

tags:

- Individual Monitoring Event Subscription

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

responses:

'204':

description: No Content (Successful deletion of the existing subscription)

'200':

description: OK (Successful deletion of the existing subscription)

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/MonitoringEventReport'

minItems: 1

description: >

The subscription was terminated successfully, the monitoring event report(s)

shall be included if received.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{tokenUrl}'

scopes: {}

schemas:

MonitoringEventSubscription:

description: Represents a subscription to event(s) monitoring.

type: object

properties:

self:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

mtcProviderId:

type: string

description: Identifies the MTC Service Provider and/or MTC Application.

appIds:

type: array

items:

type: string

description: Identifies the Application Identifier(s)

minItems: 1

externalId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

msisdn:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

addedExternalIds:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

minItems: 1

description: Indicates the added external Identifier(s) within the active group.

addedMsisdns:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

minItems: 1

description: Indicates the added MSISDN(s) within the active group.

excludedExternalIds:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

minItems: 1

description: Indicates cancellation of the external Identifier(s) within the active group.

excludedMsisdns:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

minItems: 1

description: Indicates cancellation of the MSISDN(s) within the active group.

externalGroupId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalGroupId'

addExtGroupId:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalGroupId'

minItems: 2

ipv4Addr:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv4Addr'

ipv6Addr:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv6Addr'

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

notificationDestination:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

requestTestNotification:

type: boolean

description: >

Set to true by the SCS/AS to request the SCEF to send a test notification

as defined in clause 5.2.5.3. Set to false by the SCS/AS indicates not request SCEF to

send a test notification, default false if omitted otherwise.

websockNotifConfig:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/WebsockNotifConfig'

monitoringType:

$ref: '#/components/schemas/MonitoringType'

maximumNumberOfReports:

type: integer

minimum: 1

description: >

Identifies the maximum number of event reports to be generated by the HSS, MME/SGSN

as specified in clause 5.6.0 of 3GPP TS 23.682.

monitorExpireTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

repPeriod:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

groupReportGuardTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

maximumDetectionTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

reachabilityType:

$ref: '#/components/schemas/ReachabilityType'

maximumLatency:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

maximumResponseTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

suggestedNumberOfDlPackets:

type: integer

minimum: 0

description: >

If "monitoringType" is "UE\_REACHABILITY", this parameter may be included to identify

the number of packets that the serving gateway shall buffer in case that

the UE is not reachable.

idleStatusIndication:

type: boolean

description: >

If "monitoringType" is set to "UE\_REACHABILITY" or "AVAILABILITY\_AFTER\_DDN\_FAILURE",

this parameter may be included to indicate the notification of when a UE, for which PSM

is enabled, transitions into idle mode. "true" indicates enabling of notification;

"false" indicate no need to notify. Default value is "false" if omitted.

locationType:

$ref: '#/components/schemas/LocationType'

accuracy:

$ref: '#/components/schemas/Accuracy'

minimumReportInterval:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

maxRptExpireIntvl:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

samplingInterval:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

reportingLocEstInd:

type: boolean

description: >

Indicates whether to request the location estimate for event reporting. If

"monitoringType" is "LOCATION\_REPORTING", this parameter may be included to indicate

whether event reporting requires the location information. If set to true, the location

estimation information shall be included in event reporting. If set to "false",

indicates the location estimation information shall not be included in event reporting.

Default "false" if omitted.

linearDistance:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/LinearDistance'

locQoS:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/LocationQoS'

svcId:

$ref: 'TS29515\_Ngmlc\_Location.yaml#/components/schemas/ServiceIdentity'

ldrType:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/LdrType'

velocityRequested:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/VelocityRequested'

maxAgeOfLocEst:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/AgeOfLocationEstimate'

locTimeWindow:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

supportedGADShapes:

type: array

items:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/SupportedGADShapes'

codeWord:

$ref: 'TS29515\_Ngmlc\_Location.yaml#/components/schemas/CodeWord'

upLocRepIndAf:

description: >

Indicates whether location reporting over user plane is requested or not.

"true" indicates the location reporting over user plane is requested.

"false" indicates the location reporting over user plane is not requested.

Default value is "false" if omitted.

type: boolean

default: false

upLocRepAddrAf:

$ref: '#/components/schemas/UpLocRepAddrAfRm'

associationType:

$ref: '#/components/schemas/AssociationType'

plmnIndication:

type: boolean

description: >

If "monitoringType" is "ROAMING\_STATUS", this parameter may be included to indicate the

notification of UE's Serving PLMN ID. Value "true" indicates enabling of notification;

"false" indicates disabling of notification. Default value is "false" if omitted.

locationArea:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/LocationArea'

locationArea5G:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/LocationArea5G'

dddTraDescriptors:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DddTrafficDescriptor'

minItems: 1

dddStati:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DlDataDeliveryStatus'

minItems: 1

apiNames:

type: array

items:

type: string

minItems: 1

monitoringEventReport:

$ref: '#/components/schemas/MonitoringEventReport'

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

tgtNsThreshold:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SACInfo'

nsRepFormat:

$ref: '#/components/schemas/SACRepFormat'

afServiceId:

type: string

immediateRep:

type: boolean

description: >

Indicates whether an immediate reporting is requested or not.

"true" indicate an immediate reporting is requested.

"false" indicate an immediate reporting is not requested.

Default value "false" if omitted.

uavPolicy:

$ref: '#/components/schemas/UavPolicy'

sesEstInd:

type: boolean

description: >

Set to true by the SCS/AS so that only UAV's with "PDU session established for DNN(s)

subject to aerial service" are to be listed in the Event report. Set to false or default

false if omitted otherwise.

subType:

$ref: '#/components/schemas/SubType'

addnMonTypes:

type: array

items:

$ref: '#/components/schemas/MonitoringType'

addnMonEventReports:

type: array

items:

$ref: '#/components/schemas/MonitoringEventReport'

ueIpAddr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/IpAddr'

ueMacAddr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

revocationNotifUri:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Uri'

reqRangSlRes:

type: array

items:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/RangingSlResult'

minItems: 1

relatedUEs:

type: object

additionalProperties:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/RelatedUE'

minProperties: 1

description: >

Contains a list of the related UE(s) for the ranging and sidelink positioning and the

corresponding information.

The key of the map shall be a any unique string set to the value.

required:

- notificationDestination

- monitoringType

anyOf:

- required: [maximumNumberOfReports]

- required: [monitorExpireTime]

MonitoringNotification:

description: Represents an event monitoring notification.

type: object

properties:

subscription:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

configResults:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ConfigResult'

minItems: 1

description: Each element identifies a notification of grouping configuration result.

monitoringEventReports:

type: array

items:

$ref: '#/components/schemas/MonitoringEventReport'

minItems: 1

description: Monitoring event reports.

addedExternalIds:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

minItems: 1

description: >

Identifies the added external Identifier(s) within the active group via

the "externalGroupId" attribute within the MonitoringEventSubscription data type.

addedMsisdns:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

minItems: 1

description: >

Identifies the added MSISDN(s) within the active group via the "externalGroupId"

attribute within the MonitoringEventSubscription data type.

cancelExternalIds:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

minItems: 1

description: >

Identifies the cancelled external Identifier(s) within the active group via

the "externalGroupId" attribute within the MonitoringEventSubscription data type.

cancelMsisdns:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

minItems: 1

description: >

Identifies the cancelled MSISDN(s) within the active group via the "externalGroupId"

attribute within the MonitoringEventSubscription data type.

cancelInd:

type: boolean

description: >

Indicates whether to request to cancel the corresponding monitoring subscription.

Set to false or omitted otherwise.

appliedParam:

$ref: '#/components/schemas/AppliedParameterConfiguration'

required:

- subscription

MonitoringEventReport:

description: Represents an event monitoring report.

type: object

properties:

imeiChange:

$ref: '#/components/schemas/AssociationType'

externalId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

appId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

pduSessInfo:

$ref: 'TS29523\_Npcf\_EventExposure.yaml#/components/schemas/PduSessionInformation'

idleStatusInfo:

$ref: '#/components/schemas/IdleStatusInfo'

locationInfo:

$ref: '#/components/schemas/LocationInfo'

locFailureCause:

$ref: '#/components/schemas/LocationFailureCause'

lossOfConnectReason:

type: integer

description: >

If "monitoringType" is "LOSS\_OF\_CONNECTIVITY", this parameter shall be included

if available to identify the reason why loss of connectivity is reported.

Refer to 3GPP TS 29.336 clause 8.4.58.

unavailPerDur:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

maxUEAvailabilityTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

msisdn:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

monitoringType:

$ref: '#/components/schemas/MonitoringType'

uePerLocationReport:

$ref: '#/components/schemas/UePerLocationReport'

plmnId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/PlmnId'

reachabilityType:

$ref: '#/components/schemas/ReachabilityType'

roamingStatus:

type: boolean

description: >

If "monitoringType" is "ROAMING\_STATUS", this parameter shall be set to "true"

if the new serving PLMN is different from the HPLMN. Set to false or

omitted otherwise.

failureCause:

$ref: '#/components/schemas/FailureCause'

eventTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

pdnConnInfoList:

type: array

items:

$ref: '#/components/schemas/PdnConnectionInformation'

minItems: 1

dddStatus:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DlDataDeliveryStatus'

dddTrafDescriptor:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DddTrafficDescriptor'

maxWaitTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

apiCaps:

type: array

items:

$ref: '#/components/schemas/ApiCapabilityInfo'

minItems: 0

nSStatusInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SACEventStatus'

afServiceId:

type: string

servLevelDevId:

type: string

description: >

If "monitoringType" is "AREA\_OF\_INTEREST", this parameter may be included

to identify the UAV.

uavPresInd:

type: boolean

description: >

If "monitoringType" is "AREA\_OF\_INTEREST", this parameter shall be set to true

if the specified UAV is in the monitoring area. Set to false or omitted otherwise.

groupMembListChanges:

$ref: '#/components/schemas/GroupMembListChanges'

sessInactiveTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

trafficInfo:

$ref: 'TS29520\_EventsSubscription.yaml#/components/schemas/TrafficInformation'

required:

- monitoringType

MonitoringEventReports:

description: Represents a set of event monitoring reports.

type: object

properties:

monitoringEventReports:

type: array

items:

$ref: '#/components/schemas/MonitoringEventReport'

minItems: 1

required:

- monitoringEventReports

IdleStatusInfo:

description: Represents the information relevant to when the UE transitions into idle mode.

type: object

properties:

activeTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

edrxCycleLength:

format: float

type: number

minimum: 0

suggestedNumberOfDlPackets:

type: integer

minimum: 0

description: >

Identifies the number of packets shall be buffered in the serving gateway.

It shall be present if the idle status indication is requested by the SCS/AS

with "idleStatusIndication" in the "monitoringEventSubscription" sets to "true".

idleStatusTimestamp:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

periodicAUTimer:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

UePerLocationReport:

description: Represents the number of UEs found at the indicated location.

type: object

properties:

ueCount:

type: integer

minimum: 0

description: Identifies the number of UEs.

externalIds:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

minItems: 1

description: Each element uniquely identifies a user.

msisdns:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

minItems: 1

description: Each element identifies the MS internal PSTN/ISDN number allocated for a UE.

servLevelDevIds:

type: array

items:

type: string

minItems: 1

description: Each element uniquely identifies a UAV.

required:

- ueCount

LocationInfo:

description: Represents the user location information.

type: object

properties:

ageOfLocationInfo:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationMin'

cellId:

type: string

description: >

Indicates the Cell Global Identification of the user which identifies the cell the UE

is registered.

enodeBId:

type: string

description: Indicates the eNodeB in which the UE is currently located.

routingAreaId:

type: string

description: Identifies the Routing Area Identity of the user where the UE is located.

trackingAreaId:

type: string

description: Identifies the Tracking Area Identity of the user where the UE is located.

plmnId:

type: string

description: Identifies the PLMN Identity of the user where the UE is located.

twanId:

type: string

description: Identifies the TWAN Identity of the user where the UE is located.

userLocation:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

geographicArea:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/GeographicArea'

civicAddress:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/CivicAddress'

positionMethod:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/PositioningMethod'

qosFulfilInd:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/AccuracyFulfilmentIndicator'

ueVelocity:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/VelocityEstimate'

ldrType:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/LdrType'

achievedQos:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/MinorLocationQoS'

relAppLayerId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationlayerId'

rangeDirection:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/RangeDirection'

twoDRelLoc:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/2DRelativeLocation'

threeDRelLoc:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/3DRelativeLocation'

relVelocity:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/VelocityEstimate'

upCumEvtRep:

$ref: '#/components/schemas/UpCumEvtRep'

FailureCause:

description: Represents the reason of communication failure.

type: object

properties:

bssgpCause:

type: integer

description: >

Identifies a non-transparent copy of the BSSGP cause code. Refer to 3GPP TS 29.128.

causeType:

type: integer

description: Identify the type of the S1AP-Cause. Refer to 3GPP TS 29.128.

gmmCause:

type: integer

description: >

Identifies a non-transparent copy of the GMM cause code. Refer to 3GPP TS 29.128.

ranapCause:

type: integer

description: >

Identifies a non-transparent copy of the RANAP cause code. Refer to 3GPP TS 29.128.

ranNasCause:

type: string

description: >

Indicates RAN and/or NAS release cause code information, TWAN release cause code

information or untrusted WLAN release cause code information. Refer to 3GPP TS 29.214.

s1ApCause:

type: integer

description: >

Identifies a non-transparent copy of the S1AP cause code. Refer to 3GPP TS 29.128.

smCause:

type: integer

description: >

Identifies a non-transparent copy of the SM cause code. Refer to 3GPP TS 29.128.

PdnConnectionInformation:

description: Represents the PDN connection information of the UE.

type: object

properties:

status:

$ref: '#/components/schemas/PdnConnectionStatus'

apn:

type: string

description: >

Identify the APN, it is depending on the SCEF local configuration whether or

not this attribute is sent to the SCS/AS.

pdnType:

$ref: '#/components/schemas/PdnType'

interfaceInd:

$ref: '#/components/schemas/InterfaceIndication'

ipv4Addr:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv4Addr'

ipv6Addrs:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv6Addr'

minItems: 1

macAddrs:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

minItems: 1

required:

- status

- pdnType

AppliedParameterConfiguration:

description: Represents the parameter configuration applied in the network.

type: object

properties:

externalIds:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

minItems: 1

description: Each element uniquely identifies a user.

msisdns:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

minItems: 1

description: Each element identifies the MS internal PSTN/ISDN number allocated for a UE.

maximumLatency:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

maximumResponseTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

maximumDetectionTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

ApiCapabilityInfo:

description: Represents the availability information of supported API.

type: object

properties:

apiName:

type: string

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

required:

- apiName

- suppFeat

UavPolicy:

description: >

Represents the policy information included in the UAV presence monitoring request.

type: object

properties:

uavMoveInd:

type: boolean

revokeInd:

type: boolean

required:

- uavMoveInd

- revokeInd

ConsentRevocNotif:

description: >

Represents the user consent revocation information conveyed in a user consent

revocation notification.

type: object

properties:

subscriptionId:

type: string

consentsRevoked:

type: array

items:

$ref: '#/components/schemas/ConsentRevoked'

minItems: 1

required:

- subscriptionId

- consentsRevoked

ConsentRevoked:

description: Represents the information related to a revoked user consent.

type: object

properties:

ucPurpose:

$ref: 'TS29503\_Nudm\_SDM.yaml#/components/schemas/UcPurpose'

externalId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

msisdn:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

required:

- ucPurpose

oneOf:

- required: [externalId]

- required: [msisdn]

GroupMembListChanges:

description: Represents information on the change(s) to a group's members list.

type: object

properties:

addedUEs:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

minItems: 1

removedUEs:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

minItems: 1

anyOf:

- required: [addedUEs]

- required: [removedUEs]

UpLocRepAddrAfRm:

description: Represents the user plane addressing information.

type: object

properties:

ipv4Addrs:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

minItems: 1

ipv6Addrs:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

minItems: 1

fqdn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Fqdn'

nullable: true

anyOf:

- required: [ipv4Addrs]

- required: [ipv6Addrs]

- required: [fqdn]

UpCumEvtRep:

description: Represents the cumulative event report.

type: object

properties:

upLocRepStat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

#

# ENUMS

#

MonitoringType:

anyOf:

- type: string

enum:

- LOSS\_OF\_CONNECTIVITY

- UE\_REACHABILITY

- LOCATION\_REPORTING

- CHANGE\_OF\_IMSI\_IMEI\_ASSOCIATION

- ROAMING\_STATUS

- COMMUNICATION\_FAILURE

- AVAILABILITY\_AFTER\_DDN\_FAILURE

- NUMBER\_OF\_UES\_IN\_AN\_AREA

- PDN\_CONNECTIVITY\_STATUS

- DOWNLINK\_DATA\_DELIVERY\_STATUS

- API\_SUPPORT\_CAPABILITY

- NUM\_OF\_REGD\_UES

- NUM\_OF\_ESTD\_PDU\_SESSIONS

- AREA\_OF\_INTEREST

- GROUP\_MEMBER\_LIST\_CHANGE

- APPLICATION\_START

- APPLICATION STOP

- SESSION\_INACTIVITY\_TIME

- TRAFFIC\_VOLUME

- UL\_DL\_DATA\_RATE

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: |

Represents a monitoring event type.

Possible values are

- LOSS\_OF\_CONNECTIVITY: The SCS/AS requests to be notified when the 3GPP network detects

that the UE is no longer reachable for signalling or user plane communication

- UE\_REACHABILITY: The SCS/AS requests to be notified when the UE becomes reachable for

sending either SMS or downlink data to the UE

- LOCATION\_REPORTING: The SCS/AS requests to be notified of the current location or

the last known location of the UE

- CHANGE\_OF\_IMSI\_IMEI\_ASSOCIATION: The SCS/AS requests to be notified when the association

of an ME (IMEI(SV)) that uses a specific subscription (IMSI) is changed

- ROAMING\_STATUS: The SCS/AS queries the UE's current roaming status and requests to get

notified when the status changes

- COMMUNICATION\_FAILURE: The SCS/AS requests to be notified of communication failure events

- AVAILABILITY\_AFTER\_DDN\_FAILURE: The SCS/AS requests to be notified when the UE has become

available after a DDN failure

- NUMBER\_OF\_UES\_IN\_AN\_AREA: The SCS/AS requests to be notified the number of UEs in a given

geographic area

- PDN\_CONNECTIVITY\_STATUS: The SCS/AS requests to be notified when the 3GPP network detects

that the UE’s PDN connection is set up or torn down

- DOWNLINK\_DATA\_DELIVERY\_STATUS: The AF requests to be notified when the 3GPP network

detects that the downlink data delivery status is changed.

- API\_SUPPORT\_CAPABILITY: The SCS/AS requests to be notified of the availability of support

of service APIs.

- NUM\_OF\_REGD\_UES: The AF requests to be notified of the current number of registered UEs

for a network slice.

- NUM\_OF\_ESTD\_PDU\_SESSIONS: The AF requests to be notified of the current number of

established PDU Sessions for a network slice.

- AREA\_OF\_INTEREST: The SCS/AS requests to be notified when the UAV moves in or

out of the geographic area.

- GROUP\_MEMBER\_LIST\_CHANGE: The AF requests to be notified of the changes to a group members

list.

- APPLICATION\_START: The AF requests to be notified about the start of application traffic

has been detected.

- APPLICATION\_STOP: The AF requests to be notified about the stop of application traffic

has been detected.

- SESSION\_INACTIVITY\_TIME: The AF requests to be notified of session inactivity time of the

measured UE PDU Session.

- TRAFFIC\_VOLUME: The AF requests to be notified of traffic volume of the measured UE.

- UL\_DL\_DATA\_RATE: The AF requests to be notified of uplink and downlink data rate of the

measured UE.

ReachabilityType:

anyOf:

- type: string

enum:

- SMS

- DATA

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: |

Represents a reachability type.

Possible values are

- SMS: The SCS/AS requests to be notified when the UE becomes reachable for sending SMS

to the UE

- DATA: The SCS/AS requests to be notified when the UE becomes reachable for sending

downlink data to the UE.

LocationType:

anyOf:

- type: string

enum:

- CURRENT\_LOCATION

- LAST\_KNOWN\_LOCATION

- CURRENT\_OR\_LAST\_KNOWN\_LOCATION

- INITIAL\_LOCATION

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: |

Represents a location type.

Possible values are

- CURRENT\_LOCATION: The SCS/AS requests to be notified for current location

- LAST\_KNOWN\_LOCATION: The SCS/AS requests to be notified for last known location

- CURRENT\_OR\_LAST\_KNOWN\_LOCATION: The AF requests the current or last known location

- INITIAL\_LOCATION: The AF requests the initial location

AssociationType:

anyOf:

- type: string

enum:

- IMEI

- IMEISV

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: |

Represents an IMEI or IMEISV to IMSI association.

Possible values are

- IMEI: The value shall be used when the change of IMSI-IMEI association shall be detected

- IMEISV: The value shall be used when the change of IMSI-IMEISV association shall be

detected

Accuracy:

anyOf:

- type: string

enum:

- CGI\_ECGI

- ENODEB

- TA\_RA

- PLMN

- TWAN\_ID

- GEO\_AREA

- CIVIC\_ADDR

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: |

Represents a desired granularity of accuracy of the requested location information.

Possible values are

- CGI\_ECGI: The SCS/AS requests to be notified using cell level location accuracy.

- ENODEB: The SCS/AS requests to be notified using eNodeB level location accuracy.

- TA\_RA: The SCS/AS requests to be notified using TA/RA level location accuracy.

- PLMN: The SCS/AS requests to be notified using PLMN level location accuracy.

- TWAN\_ID: The SCS/AS requests to be notified using TWAN identifier level location accuracy.

- GEO\_AREA: The SCS/AS requests to be notified using the geographical area accuracy.

- CIVIC\_ADDR: The SCS/AS requests to be notified using the civic address accuracy.

PdnConnectionStatus:

anyOf:

- type: string

enum:

- CREATED

- RELEASED

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: |

Represents the PDN connection status.

Possible values are

- CREATED: The PDN connection is created.

- RELEASED: The PDN connection is released.

PdnType:

anyOf:

- type: string

enum:

- IPV4

- IPV6

- IPV4V6

- NON\_IP

- ETHERNET

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: |

Represents the PDN connection type.

Possible values are

- IPV4: PDN connection of IPv4 type.

- IPV6: PDN connection of IPv6 type.

- IPV4V6: PDN connection of IPv4v6 type.

- NON\_IP: PDN connection of non-IP type.

- ETHERNET: PDN connection of Ethernet type.

InterfaceIndication:

anyOf:

- type: string

enum:

- EXPOSURE\_FUNCTION

- PDN\_GATEWAY

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: |

Represents the network entity used for data delivery towards the SCS/AS.

Possible values are

- EXPOSURE\_FUNCTION: SCEF is used for the PDN connection towards the SCS/AS.

- PDN\_GATEWAY: PDN gateway is used for the PDN connection towards the SCS/AS.

LocationFailureCause:

anyOf:

- type: string

enum:

- POSITIONING\_DENIED

- UNSUPPORTED\_BY\_UE

- NOT\_REGISTED\_UE

- UNSPECIFIED

- REQUESTED\_AREA\_NOT\_ALLOWED

- type: string

description: >

This string provides forward-compatibility with future extensions to the enumeration but

is not used to encode content defined in the present version of this API.

description: >

Represents the cause of location positioning failure.

Possible values are:

- POSITIONING\_DENIED: Positioning is denied.

- UNSUPPORTED\_BY\_UE: Positioning is not supported by UE.

- NOT\_REGISTED\_UE: UE is not registered.

- UNSPECIFIED: Unspecified.

- REQUESTED\_AREA\_NOT\_ALLOWED: The location request is rejected because the location area

requested by the AF for area event reporting is not allowed.

SubType:

anyOf:

- type: string

enum:

- AERIAL\_UE

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: |

Represents a subscription type.

Possible values are

- AERIAL\_UE: The UE has Aerial subscription.

SACRepFormat:

anyOf:

- type: string

enum:

- NUMERICAL

- PERCENTAGE

- type: string

description: >

This string provides forward-compatibility with future extensions to the enumeration but

is not used to encode content defined in the present version of this API.

description: Indicates the NSAC reporting format.

\*\*\* End of Changes \*\*\*