**3GPP TSG-CT WG3 Meeting #134 *C3-242396***

**Changsha, China, 15th – 19th April, 2024 (Revision of C3-24xxxx)**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.3* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.522** | **CR** | **1268** | **rev** | **-** | **Current version:** | **18.5.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Corrections to Websocket Notification in MSEventExposure API and DNAIMapping API | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Ericsson | | | | | | | | | |
| ***Source to TSG:*** | CT3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NBI18, EDGE\_Ph2 | | | | |  | ***Date:*** | | | 2024-04-03 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19) Rel-20 (Release 20)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Refer to the DP C3-242099, remove the not aligned Websocket Notification definition in MSEventExposure API and remove the Websocket Notification and test notification definition in DNAIMapping to keep alignment with Rel-18 introduced new northbound APIs needn’t specify Websocket notification. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Remove misaligned resource definition on Websocket notification, remove Websocket notification and test notification in DNAIMapping API. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Not aligned and not effective HTTP Notification defnition in this specification especially from Rel-18. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.28.4.2.3.2, 5.30.4.2.3.2, 5.30.5.2.2, 5.30.6, A.28 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR introduces backwards compatible corrections in the OpenAPI file of DNAIMapping API. | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

\* \* \* 1st Change \* \* \* \*

###### 5.28.4.2.3.2 Void

\* \* \* 2nd Change \* \* \* \*

###### 5.30.4.2.3.2 Void

\* \* \* 3rd Change \* \* \* \*

#### 5.30.5.1 General

This clause specifies the application data model supported by the DNAIMapping API. Table 5.30.5.1-1 specifies the data types defined for the DNAIMapping API.

Table 5.30.5.1-1: DNAIMapping specific Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Clause defined | Description | Applicability |
| DnaiMapSub | 5.30.5.2.2 | Represents DNAI Mapping subscription data. |  |
| DnaiMapUpdateNotif | 5.30.5.2.3 | Represents the notification data of they update of DNAI Mapping information. |  |

Table 5.30.5.1-2 specifies data types re-used by the DNAIMapping API from other specifications, including a reference to their respective specifications, and when needed, a short description of their use within the DNAIMapping API.

Table 5.30.5.1-2: Re-used Data Types

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Data type | | Reference | Comments | | Applicability |
| DateTime | | 3GPP TS 29.122 [4] | Represents a date and a time. | |  |
| Dnai | | 3GPP TS 29.571 [8] | Identifies a DNAI. | |  |
| DnaiEasInfo | | 3GPP TS 29.519 [23] | Contains EAS information for a DNAI. | |  |
| Dnn | | 3GPP TS 29.571 [8] | Identifies the DNN. | |  |
| Fqdn | | 3GPP TS 29.571 [8] | Identifies an FQDN. | |  |
| IpAddr | | 3GPP TS 29.571 [8] | Identifes an IP address. | |  |
| ReportingInformation | | 3GPP TS 29.523 [22] | Represents the event reporting requirements. | |  |
| Snssai | | 3GPP TS 29.571 [8] | Identifies an S-NSSAI. | |  |
| SupportedFeatures | | 3GPP TS 29.571 [8] | Represents the list of supported feature(s) and used to negotiate the applicability of the optional features. | |  |
| Uri | | 3GPP TS 29.122 [4] | Contains a URI. | |  |

\* \* \* 4th Change \* \* \* \*

##### 5.30.5.2.2 Type: DnaiMapSub

Table 5.30.5.2.2-1: Definition of type DnaiMapSub

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Attribute name | | Data type | | P | | Cardinality | | Description | | Applicability | |
| easIpAddrs | | array(IpAddr) | | C | | 1..N | | IP address(es) of the EASs in the Local part of the DN or the IP address ranges (IPv4 subnetwork(s) and/or IPv6 prefix(es) of the Local part of the DN where the EAS is deployed.  (NOTE) | |  | |
| fqdns | | array(Fqdn) | | C | | 1..N | | FQDN(s) of the EAS(s) in the Local part of the DN where the EAS(s) is/are deployed.  (NOTE) | |  | |
| dnn | | Dnn | | O | | 0..1 | | Identifies a DNN, a full DNN with both the Network Identifier and Operator Identifier, or a DNN with the Network Identifier only. | |  | |
| snssai | | Snssai | | O | | 0..1 | | Identifies an S-NSSAI. | |  | |
| immReports | | array(DnaiEasInfo) | | C | | 1..N | | DNAI EAS mapping information.  It shall be included in the subscription response if immediate reporting has been requested and the information is available. | |  | |
| eventReq | | ReportingInformation | | O | | 0..1 | | Indicates the event reporting requirements. | |  | |
| notifUri | | Uri | | M | | 1 | | Represents the notification URI to be used for DNAI Mapping information reporting. | |  | |
| notifCorrId | | string | | M | | 1 | | Notification correlation identifier | |  | |
| suppFeat | | SupportedFeatures | | C | | 0..1 | | Indicates the list of Supported features used as described in clause 5.30.4.  This attribute shall be provided in the POST request and in the response of successful resource creation. | |  | |
| NOTE: Either "easIpAddrs" or "fqdns" attribute shall be provided. | | | | | | | | | | | |

\* \* \* 5th Change \* \* \* \*

### 5.30.6 Used Features

The table below defines the features applicable to the DNAIMapping API. Those features are negotiated as described in clause 5.2.7 of 3GPP TS 29.122 [4].

Table 5.30.6-1: Features used by DNAIMapping API

|  |  |  |
| --- | --- | --- |
| Feature number | Feature Name | Description |
|  |  |  |

\* \* \* 6th Change \* \* \* \*

# A.28 DNAIMapping API

openapi: 3.0.0

info:

title: 3gpp-dnaimapping

version: 1.0.0-alpha.4

description: |

API for DNAI Mapping.

© 2024, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: >

3GPP TS 29.522 V18.5.0; 5G System; Network Exposure Function Northbound APIs.

url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.522/'

security:

- {}

- oAuth2ClientCredentials: []

servers:

- url: '{apiRoot}/3gpp-dnai-mapping/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 5.2.4 of 3GPP TS 29.122.

paths:

/{afId}/subscriptions:

get:

summary: read all of the active subscriptions for the AF

operationId: ReadAllSubscriptions

tags:

- DNAI Mapping Subscriptions

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

responses:

'200':

description: OK (Successful get all of the active subscriptions for the AF)

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/DnaiMapSub'

minItems: 0

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

post:

summary: Creates a new subscription resource

operationId: CreateNewSubscription

tags:

- DNAI Mapping Subscriptions

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

requestBody:

description: new subscription creation

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/DnaiMapSub'

callbacks:

notification:

'{request.body#/notifUri}':

post:

requestBody: # contents of the callback message

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/DnaiMapUpdateNotif'

responses:

'204':

description: No Content (successful notification)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

responses:

'201':

description: Created (Successful creation)

content:

application/json:

schema:

$ref: '#/components/schemas/DnaiMapSub'

headers:

Location:

description: Contains the URI of the newly created resource.

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{afId}/subscriptions/{subscriptionId}:

get:

summary: read an active subscription for the AF and the subscription Id

operationId: ReadAnSubscription

tags:

- Individual DNAI Mapping Subscription

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

responses:

'200':

description: OK (Successful get the active subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/DnaiMapSub'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

summary: Deletes an already existing subscription

operationId: DeleteAnSubscription

tags:

- Individual Dnai Mapping Subscription

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

responses:

'204':

description: No Content (Successful deletion of the existing subscription)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{tokenUrl}'

scopes: {}

schemas:

DnaiMapSub:

description: Represents a DNAI Mapping subscription.

type: object

properties:

easIpAddrs:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/IpAddr'

minItems: 1

description: >

IP address(es) of the EASs in the Local part of the DN or the IP address ranges(IPv4

subnetwork(s) and/or IPv6 prefix(es) of the Local part of the DN where the EAS is

deployed.

fqdns:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Fqdn'

minItems: 1

description: FQDN(s) where the EAS(s) is/are deployed.

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

eventReq:

$ref: 'TS29523\_Npcf\_EventExposure.yaml#/components/schemas/ReportingInformation'

immReport:

type: array

items:

$ref: 'TS29519\_Application\_Data.yaml#/components/schemas/DnaiEasInfo'

minItems: 1

description: DNAI EAS mapping information.

notifUri:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Uri'

notifCorrId:

type: string

description: Notification correlation identifier.

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

oneOf:

- required: [easIpAddrs]

- required: [fqdn]

required:

- notifUri

- notifCorrId

DnaiMapUpdateNotif:

description: Represents an updated DNAI Mapping notification.

type: object

properties:

dnaiEasAddrMap:

type: array

items:

$ref: 'TS29519\_Application\_Data.yaml#/components/schemas/DnaiEasInfo'

minItems: 1

description: >

Contains the mapping information between DNAI(s) and EAS address(es).

notifCorrId:

type: string

description: Notification correlation identifier.

required:

- dnaiEasAddrMap

- notifCorrId

\* \* \* End of Changes \* \* \* \*