**3GPP TSG CT WG3 Meeting #134 *C3-242119***

**Changsha, China, 15 - 19 April, 2024 (Revision of C3-242xyz)**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **29.517** | **CR** | **0130** | **rev** | **-** | **Current version:** | **18.5.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | ServiceExperienceInfoPerFlow data model update |
|  |  |
| ***Source to WG:*** | Nokia |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | SBIProtoc18 |  | ***Date:*** | 2024-04-08 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | As there is a condition exists for ipTrafficFilter and ethTrafficFilter, the corresponding presence has to be updated. |
|  |  |
| ***Summary of change:*** |  ServiceExperienceInfoPerFlow data model is updated. |
|  |  |
| ***Consequences if not approved:*** | The specification is missing the clarity for the implementors. The quality of the specification is not good. |
|  |  |
| ***Clauses affected:*** | 5.6.2.8 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR does not impact the OpenAPI descriptions defined in this specification. |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* \* First Change \* \* \* \*

#### 5.6.2.8 Type ServiceExperienceInfoPerFlow

Table 5.6.2.8-1: Definition of type ServiceExperienceInfoPerFlow

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| svcExprc | SvcExperience | M | 1 | Service experience. |  |
| timeIntev | TimeWindow | M | 1 | Represents a start and stop time of the measurement period for the AF service experience. |  |
| dnai | Dnai | O | 0..1 | Indicates the DN Access Identifiers representing location of the service flow. |  |
| ipTrafficFilter | FlowInfo | C | 0..1 | Identifies IP packet filter.(NOTE) |  |
| ethTrafficFilter | EthFlowDescription | C | 0..1 | Identifies Ethernet packet filter.(NOTE) |  |
| NOTE: Either "ipTrafficFilter" or "ethTrafficFilter" shall be provided. |

\* \* \* \* End of Changes \* \* \* \*