**3GPP TSG-CT WG3 Meeting #134 *C3-242289***

**Changsha, China, 15 - 19 April, 2024 *(Revision of C3-242xxx)***

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** | **302** | **rev** |  | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Corrections on the trigger description | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei | | | | | | | | | |
| ***Source to TSG:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | SBIProtoc18 | | | | |  | ***Date:*** | | |  |
|  |  | | | |  | |  | | |  |
| ***Category:*** |  |  | | | | | ***Release:*** | | |  |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | The "FEAT\_RENEG" trigger as described in clause 4.2.3.4 only applies during the AMF relocation (i.e. update service). Therefore, it is proposed to describe it separately with other triggers(e.g. in the create service). Nevertheless, some of the descriptions for triggers in the current specification are missing relevant indexes (in clause 4.2.3.1), or contain too many details that are not feasible for subsequent extensions (in clauses 5.6.2.2 and 5.6.2.5).  Hence, it is proposed to simply the description of "trigger" description to avoid misalignment. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | 1. Update the description of "tigger" attribute. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Unclear and incorrect specification. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.6.2.2, 5.6.2.5, 5.6.3.3, A.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR introduces backwards compatible corrections to the OpenAPI description of the Npcf\_AMPolicyControl API. | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

**Additional discussion(if needed):**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

#### 5.6.2.2 Type PolicyAssociation

Table 5.6.2.2-1: Definition of type PolicyAssociation

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| request | PolicyAssociationRequest | O | 0..1 | The information provided by the NF service consumer when requesting the creation of a policy association |  |
| triggers | array(RequestTrigger) | O | 1..N | Request Triggers that the PCF subscribes.  (NOTE 1) |  |
| servAreaRes | ServiceAreaRestriction | O | 0..1 | Service Area Restriction as part of the AMF Access and Mobility Policy as determined by the PCF |  |
| wlServAreaRes | WirelineServiceAreaRestriction | O | 0..1 | Wireline Service Area Restriction as part of the AMF Access and Mobility Policy as determined by the PCF | WirelineWirelessConvergence |
| rfsp | RfspIndex | O | 0..1 | RFSP Index as part of the AMF Access and Mobility Policy as determined by the PCF. |  |
| rfspValTime | DurationSec | O | 0..1 | Validity time of the RFSP Index value provided within the "rfsp" attribute.  It may be provided when the RFSP Index value within the "rfsp" attribute indicates the EPC/E-UTRAN access is prioritized over 5GS access. It shall be omitted for other RFSP Index values. | RFSPValidityTime |
| targetRfsp | RfspIndex | C | 0..1 | RFSP Index associated with the Target NSSAI. It shall be present if the Target NSSAI was received in the request and the trigger "TARGET\_NSSAI" is provided. | TargetNSSAI |
| pras | map(PresenceInfo) | C | 1..N | If the Trigger "PRA\_CH" is provided, the presence reporting area(s) for which reporting is requested shall be provided. The "praId" attribute within the PresenceInfo data type shall also be the key of the map. The "presenceState" and the "additionalPraId" attributes within the PresenceInfo data type shall not be supplied. The "praId" attribute within the PresenceInfo data type shall include the identifier of either a presence reporting area or a presence reporting area set. |  |
| smfSelInfo | SmfSelectionData | O | 0..1 | If the trigger "SMF\_SELECT\_CH" is provided, the conditions for SMF selection information replacement, as determined by the PCF shall be provided. | DNNReplacementControl |
| ueAmbr | Ambr | O | 0..1 | UE-AMBR as part of the AMF Access and Mobility Policy as determined by the PCF. | UE-AMBR\_Authorization |
| ueSliceMbrs | array(UeSliceMbr) | O | 1..N | One or more UE-Slice-MBR(s) for S-NSSAI(s) of serving PLMN as part of the AMF Access and Mobility Policy as determined by the PCF. | UE-Slice-MBR\_Authorization |
| pcfUeInfo | PcfUeCallbackInfo | O | 0..1 | Contains the PCF for the UE information necessary for the PCF for the PDU session to send established/terminated events notifications to the PCF for the UE. | AMInfluence |
| matchPdus | array(PduSessionInfo) | C | 1..N | Indicates the matched PDU session(s) for which the PCF for the UE information in the "pcfUeInfo" attribute shall be forwarded to the SMF. It shall be present when the "pcfUeInfo" attribute is present.  (NOTE 2) | AMInfluence |
| asTimeDisParam | AsTimeDistributionParam | O | 0..1 | Contains the 5G acess stratum time distribution parameters. | 5GAccessStratumTime |
| sliceUsgCtrlInfoSets | map(SliceUsgCtrlInfo) | O | 1..N | Represents the network slice usage control information.  The key of the map shall be set to the on-demand S-NSSAI (provided within the "snssai" attribute of the corresponding map entry encoded using the SliceUsgCtrlInfo data structure) to which the network slice usage control information is related. | NetSliceUsageCtrl |
| chfInfo | ChargingInformation | O | 0..1 | The address(es) and, if available, the CHF instance ID and the CHF set ID of the Charging Function.  (NOTE 3) | SLAMUP |
| suppFeat | SupportedFeatures | M | 1 | Indicates the negotiated supported features. |  |
| NOTE 1: The "triggers" attribute shall only contain the RequestTrigger values that required explicit subscription as described in clause 5.6.3.3.  NOTE 2: The DNN encoded within the PduSessionInfo element(s) of the "matchPdus" array contains a full DNN or only the DNN Network Identifier based on the DNN provided by the AF to the PCF in the AmInfluence API, as specified in 3GPP TS 29.522 [32]. When the DNN contains the Network Identifier only, the AMF shall match a PDU session for the received Network Identifier and for any value of the Operator Identifier.  NOTE 3: This attribute may only be supplied by the PCF in the response to the POST request that requested the creation of an individual AM policy resource. | | | | | |

\*\*\* Next Change \*\*\*

#### 5.6.2.5 Type PolicyUpdate

Table 5.6.2.5-1: Definition of type PolicyUpdate

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| resourceUri | Uri | M | 1 | The resource URI of the individual AM policy related to the notification.  (NOTE 3) |  |
| triggers | array(RequestTrigger) | O | 1..N | Request Triggers that the PCF subscribes.  (NOTE 1) (NOTE 2) |  |
| servAreaRes | ServiceAreaRestriction | O | 0..1 | Service Area Restriction as part of the AMF Access and Mobility Policy as determined by the PCF. |  |
| wlServAreaRes | WirelineServiceAreaRestriction | O | 0..1 | Wireline Service Area Restriction as part of the AMF Access and Mobility Policy as determined by the PCF | WirelineWirelessConvergence |
| rfsp | RfspIndex | O | 0..1 | RFSP Index as part of the AMF Access and Mobility Policy as determined by the PCF. |  |
| rfspValTime | DurationSec | O | 0..1 | Validity time of the RFSP Index value provided within the "rfsp" attribute.  It may be provided when the RFSP Index value within the "rfsp" attribute indicates the EPC/E-UTRAN access is prioritized over 5GS access. It shall be omitted for other RFSP Index values. | RFSPValidityTime |
| targetRfsp | RfspIndex | C | 0..1 | RFSP Index associated with the Target NSSAI. It shall be present when the Target NSSAI was received in the request. | TargetNSSAI |
| smfSelInfo | SmfSelectionData | C | 0..1 | It may include updated conditions for SMF Selection information replacement. It shall include the PCF decision of the selected DNN when the "smfSelInfo" attribute containing the UE requested S-NSSAI and DNN was sent in the request. | DNNReplacementControl |
| ueAmbr | Ambr | C | 0..1 | UE-AMBR as part of the AMF Access and Mobility Policy. | UE-AMBR\_Authorization |
| ueSliceMbrs | array(UeSliceMbr) | O | 1..N | One or more UE-Slice-MBR(s) for S-NSSAI(s) of serving PLMN as part of the AMF Access and Mobility Policy as determined by the PCF. | UE-Slice-MBR\_Authorization |
| pras | map(PresenceInfoRm) | C | 1..N | If the Trigger "PRA\_CH" is provided or if that trigger was already set but the requested presence reporting areas need to be changed, the presence reporting area(s) for which reporting is requested shall be provided. The "praId" attribute within the PresenceInfo data type shall also be the key of the map. The "presenceState" attribute within the PresenceInfo data type shall not be supplied. The "praId" attribute within the PresenceInfo data type shall include the identifier of either a presence reporting area or a presence reporting area set. |  |
| pcfUeInfo | PcfUeCallbackInfo | O | 0..1 | Contains the PCF for the UE information necessary for the PCF for the PDU session to send established/terminated event notifications to the PCF for the UE. | AMInfluence |
| matchPdus | array(PduSessionInfo) | C | 1..N | Indicates the matched PDU session(s) for which the PCF for the UE information in the "pcfUeInfo" attribute shall be forwarded to the SMF.  It shall be present when the "pcfUeInfo" attribute is present and was not previously provisioned by the PCF for the UE.  (NOTE 4) | AMInfluence |
| asTimeDisParam | AsTimeDistributionParam | O | 0..1 | Contains the 5G acess stratum time distribution parameters. | 5GAccessStratumTime |
| snssaiReplInfos | map(SnssaiReplaceInfo) | O | 1..N | Contains the network slice replacement related Information for one or more S-NSSAI(s) of the UE's Allowed NSSAI and/or Partially Allowed NSSAI.  The key of the map shall be set to the concerned unavailable S-NSSAI provided within the "snssai" attribute of the corresponding map entry (encoded using the SnssaiReplaceInfo data structure). | NetSliceRepl |
| sliceUsgCtrlInfoSets | map(SliceUsgCtrlInfo) | O | 1..N | Represents the updated network slice usage control information.  The key of the map shall be set to the on-demand S-NSSAI (provided within the "snssai" attribute of the corresponding map entry encoded using the SliceUsgCtrlInfo data structure) to which the network slice usage control information is related. | NetSliceUsageCtrl |
| suppFeat | SupportedFeatures | C | 0..1 | Indicates the negotiated supported features. It shall be included in the HTTP POST response when the NF service consumer provided the supported features in the HTTP POST request. | FeatureRenegotiation |
| NOTE 1: The "triggers" attribute shall only contain the RequestTrigger values that required explicit subscription as described in clause 5.6.3.3.  NOTE 2: The "SMF\_SELECT\_CH" trigger may be met only for new PDU sessions, i.e. it shall not apply to ongoing PDU sessions.  NOTE 3: When the PolicyUpdate data type is used in a policy update notify service operation, either the complete resource URI included in the "resourceUri" attribute or the "apiSpecificResourceUriPart" component (see clause 5.1) of the resource URI included in the "resourceUri" attribute may be used by the NF service consumer (e.g. AMF) for the identification of the Individual AM Policy Association resource related to the notification.  NOTE 4: The DNN encoded within the PduSessionInfo element(s) of the "matchPdus" array contains a full DNN or only the DNN Network Identifier based on the DNN provided by the AF to the PCF in the AmInfluence API, as specified in 3GPP TS 29.522 [32]. When the DNN contains the Network Identifier only, the AMF shall match a PDU session for the received Network Identifier and for any value of the Operator Identifier. | | | | | |

\*\*\* Next Change \*\*\*

#### 5.6.3.3 Enumeration: RequestTrigger

The enumeration RequestTrigger represents the possible Policy Control Request Triggers. It shall comply with the provisions defined in table 5.6.3.3-1.

Table 5.6.3.3-1: Enumeration RequestTrigger

|  |  |  |
| --- | --- | --- |
| Enumeration value | Description | Applicability |
| LOC\_CH | Location change (tracking area): the tracking area of the UE has changed.  (NOTE 1) |  |
| PRA\_CH | Change of UE presence in PRA: the NF service consumer reports the current presence status of the UE in a Presence Reporting Area, and notifies that the UE enters/leaves the Presence Reporting Area. |  |
| SERV\_AREA\_CH | Service Area Restriction change: the UDM notifies the NF service consumer that the subscribed service area restriction information has changed.  (NOTE 2) |  |
| RFSP\_CH | RFSP index change: the UDM notifies the NF service consumer that the subscribed RFSP index has changed.  (NOTE 2) |  |
| ALLOWED\_NSSAI\_CH | Allowed NSSAI change: the NF service consumer notifies that the set of UE allowed S-NSSAIs has changed.  (NOTE 1) | SliceSupport, DNNReplacementControl, NetSliceRepl |
| UE\_AMBR\_CH | UE-AMBR change: the UDM notifies the NF service consumer that the subscribed UE-AMBR has changed.  (NOTE 2) | UE-AMBR\_Authorization |
| SMF\_SELECT\_CH | SMF selection information change: UE request for an unsupported DNN or UE request for a DNN within the list of DNN candidates for replacement per S-NSSAI. | DNNReplacementControl |
| ACCESS\_TYPE\_CH | Access Type change: the NF service consumer notifies that the access type and the RAT type for a UE has changed.  (NOTE 1) | MultipleAccessTypes |
| UE\_SLICE\_MBR\_CH | UE-Slice-MBR change: the NF service consumer notifies any changes in the subscribed UE-Slice-MBR for each subscribed S-NSSAI of the home PLMN mapping to a S-NSSAI of the serving PLMN. | UE-Slice-MBR\_Authorization |
| NWDAF\_DATA\_CH | Indicates that the NWDAF instance IDs used for the UE and/or associated Analytics IDs have changed.  (NOTE 2) | EneNA |
| TARGET\_NSSAI | Generation of Target NSSAI: the NF service consumer notifies that the Target NSSAI was generated. | TargetNSSAI |
| SLICE\_REPLACE\_MGMT | Indicates that network slice replacement is needed for one or more S-NSSAI(s) of the UE's Allowed NSSAI and/or Partially Allowed NSSAI and the NF service consumer (i.e., AMF) cannot determine the Alternative S-NSSAI(s) for these S-NSSAI(s). | NetSliceRepl |
| FEAT\_RENEG | The NF service consumer notifies that the target AMF is requesting feature re-negotiation.  (NOTE 2) | FeatureRenegotation |
| PARTIALLY\_ALLOWED\_NSSAI\_CH | Change of the Partially Allowed NSSAI: the NF service consumer notifies that the set of Partially Allowed S-NSSAI(s) of the UE has changed.  (NOTE 1) | PartNetSliceSupport, NetSliceRepl |
| SNSSAIS\_PARTIALLY\_REJECTED\_CH | Change of the S-NSSAI(s) rejected partially in the RA: the NF service consumer notifies that the set of S-NSSAI(s) rejected partially in the RA for the UE has changed.  (NOTE 1) | PartNetSliceSupport |
| REJECTED\_SNSSAIS\_CH | Change of the Rejected S-NSSAI(s) in the RA: the NF service consumer notifies that the set of the Rejected S-NSSAI(s) in the RA for the UE has changed.  (NOTE 1) | PartNetSliceSupport |
| PENDING\_NSSAI\_CH | Change of the Pending NSSAI: the NF service consumer notifies that the set of Pending S-NSSAI(s) of the UE has changed.  (NOTE 1) | PartNetSliceSupport |
| NOTE 1: This includes reporting the current value at the time the trigger is provisioned during the update or update notification of the policy association.  NOTE 2: The NF service consumer always reports to the PCF. | | |

\*\*\* Next Change \*\*\*

# A.2 Npcf\_AMPolicyControl API

openapi: 3.0.0

info:

version: 1.3.0-alpha.5

title: Npcf\_AMPolicyControl

description: |

Access and Mobility Policy Control Service.

© 2024, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.507 V18.5.0; 5G System; Access and Mobility Policy Control Service.

url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.507/'

servers:

- url: '{apiRoot}/npcf-am-policy-control/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 4.4 of 3GPP TS 29.501

security:

- {}

- oAuth2ClientCredentials:

- npcf-am-policy-control

paths:

/policies:

post:

operationId: CreateIndividualAMPolicyAssociation

summary: Create individual AM policy association.

tags:

- AM Policy Associations (Collection)

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/PolicyAssociationRequest'

responses:

'201':

description: Created

content:

application/json:

schema:

$ref: '#/components/schemas/PolicyAssociation'

headers:

Location:

description: >

Contains the URI of the newly created resource, according to the structure

{apiRoot}/npcf-am-policy-control/v1/policies/{polAssoId}

required: true

schema:

type: string

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

callbacks:

policyUpdateNotification:

'{$request.body#/notificationUri}/update':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/PolicyUpdate'

responses:

'200':

description: >

OK. The current applicable values corresponding to the policy control request

trigger is reported

content:

application/json:

schema:

$ref: '#/components/schemas/AmRequestedValueRep'

'204':

description: No Content, Notification was successful.

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

policyAssocitionTerminationRequestNotification:

'{$request.body#/notificationUri}/terminate':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/TerminationNotification'

responses:

'204':

description: No Content, Notification was successful.

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/policies/{polAssoId}:

get:

operationId: ReadIndividualAMPolicyAssociation

summary: Read individual AM policy association.

tags:

- Individual AM Policy Association (Document)

parameters:

- name: polAssoId

in: path

description: Identifier of a policy association

required: true

schema:

type: string

responses:

'200':

description: OK. Resource representation is returned

content:

application/json:

schema:

$ref: '#/components/schemas/PolicyAssociation'

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

operationId: DeleteIndividualAMPolicyAssociation

summary: Delete individual AM policy association.

tags:

- Individual AM Policy Association (Document)

parameters:

- name: polAssoId

in: path

description: Identifier of a policy association

required: true

schema:

type: string

responses:

'204':

description: No Content. Resource was successfully deleted.

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/policies/{polAssoId}/update:

post:

operationId: ReportObservedEventTriggersForIndividualAMPolicyAssociation

summary: >

Report observed event triggers and obtain updated policies for an individual AM

policy association.

tags:

- Individual AM Policy Association (Document)

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/PolicyAssociationUpdateRequest'

parameters:

- name: polAssoId

in: path

description: Identifier of a policy association

required: true

schema:

type: string

responses:

'200':

description: OK. Updated policies are returned

content:

application/json:

schema:

$ref: '#/components/schemas/PolicyUpdate'

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{nrfApiRoot}/oauth2/token'

scopes:

npcf-am-policy-control: Access to the Npcf\_AMPolicyControl API

schemas:

PolicyAssociation:

description: Represents an individual AM Policy Association resource.

type: object

properties:

request:

$ref: '#/components/schemas/PolicyAssociationRequest'

triggers:

type: array

items:

$ref: '#/components/schemas/RequestTrigger'

minItems: 1

description: Request Triggers that the PCF subscribes.

servAreaRes:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ServiceAreaRestriction'

wlServAreaRes:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/WirelineServiceAreaRestriction'

rfsp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RfspIndex'

rfspValTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

targetRfsp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RfspIndex'

smfSelInfo:

$ref: '#/components/schemas/SmfSelectionData'

ueAmbr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ambr'

ueSliceMbrs:

type: array

items:

$ref: '#/components/schemas/UeSliceMbr'

minItems: 1

description: >

One or more UE-Slice-MBR(s) for S-NSSAI(s) of serving PLMN as part of the

AMF Access and Mobility Policy as determined by the PCF.

pras:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

minProperties: 1

description: >

Contains the presence reporting area(s) for which reporting was requested.

The praId attribute within the PresenceInfo data type is the key of the map.

pcfUeInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PcfUeCallbackInfo'

matchPdus:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionInfo'

description: >

Indicates the matched PDU session(s) for which the PCF for the UE information.

nullable: true

asTimeDisParam:

$ref: '#/components/schemas/AsTimeDistributionParam'

sliceUsgCtrlInfoSets:

type: object

additionalProperties:

$ref: '#/components/schemas/SliceUsgCtrlInfo'

minProperties: 1

description: >

Represents the network slice usage control information.

The key of the map shall be set to the on-demand S-NSSAI (within the "snssai" attribute

of the corresponding map entry encoded using the SliceUsgCtrlInfo data structure) to

which the network slice usage control information is related.

chfInfo:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/ChargingInformation'

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

required:

- suppFeat

PolicyAssociationRequest:

description: >

Information which the NF service consumer provides when requesting the creation of a policy

association. The serviveName property corresponds to the serviceName in the main body

of the specification.

type: object

properties:

notificationUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

altNotifIpv4Addrs:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

minItems: 1

description: Alternate or backup IPv4 Address(es) where to send Notifications.

altNotifIpv6Addrs:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

minItems: 1

description: Alternate or backup IPv6 Address(es) where to send Notifications.

altNotifFqdns:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Fqdn'

minItems: 1

description: Alternate or backup FQDN(s) where to send Notifications.

supi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

gpsi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

accessType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/AccessType'

accessTypes:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/AccessType'

minItems: 1

pei:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

userLoc:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

timeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

servingPlmn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnIdNid'

ratType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

ratTypes:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

minItems: 1

groupIds:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

minItems: 1

servAreaRes:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ServiceAreaRestriction'

wlServAreaRes:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/WirelineServiceAreaRestriction'

rfsp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RfspIndex'

ueAmbr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ambr'

ueSliceMbrs:

type: array

items:

$ref: '#/components/schemas/UeSliceMbr'

minItems: 1

description: >

The subscribed UE Slice-MBR for each subscribed S-NSSAI of the home PLMN mapping to

a S-NSSAI of the serving PLMN Shall be provided when available.

allowedSnssais:

description: array of allowed S-NSSAIs for the 3GPP access.

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 1

partAllowedNssai:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PartiallyAllowedSnssai'

minProperties: 1

description: >

Represents the Partially Allowed NSSAI.

The key of the map shall be set to the value of the "snssai" attribute of the

corresponding map entry (encoded using the PartiallyAllowedSnssai data

structure).

snssaisPartRejected:

type: object

additionalProperties:

$ref: '#/components/schemas/SnssaiPartRejected'

minProperties: 1

description: >

Represents the set of S-NSSAI(s) rejected partially in the RA.

The key of the map shall be set to the value of the "snssai" attribute of the

corresponding map entry (encoded using the SnssaiPartRejected data structure).

rejectedSnssais:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 1

pendingNssai:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 1

targetSnssais:

description: array of target S-NSSAIs.

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 1

mappingSnssais:

description: >

mapping of each S-NSSAI of the Allowed NSSAI to the corresponding S-NSSAI of the HPLMN.

type: array

items:

$ref: 'TS29531\_Nnssf\_NSSelection.yaml#/components/schemas/MappingOfSnssai'

minItems: 1

n3gAllowedSnssais:

description: array of allowed S-NSSAIs for the Non-3GPP access.

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 1

guami:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Guami'

serviveName:

$ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/ServiceName'

traceReq:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TraceData'

nwdafDatas:

type: array

items:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/NwdafData'

minItems: 1

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

required:

- notificationUri

- suppFeat

- supi

PolicyAssociationUpdateRequest:

description: >

Represents information that the NF service consumer provides when requesting the update of

a policy association.

type: object

properties:

notificationUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

altNotifIpv4Addrs:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

minItems: 1

description: Alternate or backup IPv4 Address(es) where to send Notifications.

altNotifIpv6Addrs:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

minItems: 1

description: Alternate or backup IPv6 Address(es) where to send Notifications.

altNotifFqdns:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Fqdn'

minItems: 1

description: Alternate or backup FQDN(s) where to send Notifications.

triggers:

type: array

items:

$ref: '#/components/schemas/RequestTrigger'

minItems: 1

description: Request Triggers that the NF service consumer observes.

servAreaRes:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ServiceAreaRestriction'

wlServAreaRes:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/WirelineServiceAreaRestriction'

rfsp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RfspIndex'

smfSelInfo:

$ref: '#/components/schemas/SmfSelectionData'

ueAmbr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ambr'

ueSliceMbrs:

type: array

items:

$ref: '#/components/schemas/UeSliceMbr'

minItems: 1

description: >

The subscribed UE-Slice-MBR for each subscribed S-NSSAI of the home PLMN mapping

to a S-NSSAI of the serving PLMN Shall be provided for the "UE\_SLICE\_MBR\_CH"

policy control request trigger.

praStatuses:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

minProperties: 1

description: >

Contains the UE presence status for tracking area for which changes of the UE presence

occurred. The praId attribute within the PresenceInfo data type is the key of the map.

userLoc:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

allowedSnssais:

description: array of allowed S-NSSAIs for the 3GPP access.

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 1

partAllowedNssai:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PartiallyAllowedSnssai'

minProperties: 1

description: >

Represents the Partially Allowed NSSAI.

The key of the map shall be set to the value of the "snssai" attribute of the

corresponding map entry (encoded using the PartiallyAllowedSnssai data

structure).

snssaisPartRejected:

type: object

additionalProperties:

$ref: '#/components/schemas/SnssaiPartRejected'

minProperties: 1

description: >

Represents the set of S-NSSAI(s) rejected partially in the RA.

The key of the map shall be set to the value of the "snssai" attribute of the

corresponding map entry (encoded using the SnssaiPartRejected data structure).

rejectedSnssais:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 1

pendingNssai:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 1

targetSnssais:

description: array of target S-NSSAIs.

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 1

mappingSnssais:

description: >

mapping of each S-NSSAI of the Allowed NSSAI to the corresponding S-NSSAI of the HPLMN.

type: array

items:

$ref: 'TS29531\_Nnssf\_NSSelection.yaml#/components/schemas/MappingOfSnssai'

minItems: 1

accessTypes:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/AccessType'

minItems: 1

ratTypes:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

minItems: 1

n3gAllowedSnssais:

description: array of allowed S-NSSAIs for the Non-3GPP access.

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 1

unavailSnssais:

description: >

Represents the unavailable S-NSSAI(s) from the UE's Allowed NSSAI and/or

Partially Allowed NSSAI that require network slice replacement.

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 1

traceReq:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TraceData'

guami:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Guami'

nwdafDatas:

type: array

items:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/NwdafData'

minItems: 1

nullable: true

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

PolicyUpdate:

description: >

Represents updated policies that the PCF provides in a notification or in a reply to an

Update Request.

type: object

properties:

resourceUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

triggers:

type: array

items:

$ref: '#/components/schemas/RequestTrigger'

minItems: 1

nullable: true

description: Request Triggers that the PCF subscribes.

servAreaRes:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ServiceAreaRestriction'

wlServAreaRes:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/WirelineServiceAreaRestriction'

rfsp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RfspIndex'

rfspValTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

targetRfsp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RfspIndex'

smfSelInfo:

$ref: '#/components/schemas/SmfSelectionData'

ueAmbr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ambr'

ueSliceMbrs:

type: array

items:

$ref: '#/components/schemas/UeSliceMbr'

minItems: 1

description: >

One or more UE-Slice-MBR(s) for S-NSSAI(s) of serving PLMN the allowed NSSAI as

part of the AMF Access and Mobility Policy as determined by the PCF.

pras:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfoRm'

description: >

Contains the presence reporting area(s) for which reporting was requested. The praId

attribute within the PresenceInfo data type is the key of the map.

minProperties: 1

nullable: true

pcfUeInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PcfUeCallbackInfo'

matchPdus:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionInfo'

description: >

Indicates the matched PDU session(s) for which the PCF for the UE information.

nullable: true

asTimeDisParam:

$ref: '#/components/schemas/AsTimeDistributionParam'

snssaiReplInfos:

nullable: true

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SnssaiReplaceInfo'

minProperties: 1

description: >

Contains the network slice replacement information.

The key of the map shall be set to the concerned unavailable S-NSSAI provided within the

"snssai" attribute of the corresponding map entry (encoded using the SnssaiReplaceInfo

data structure) to which the network slice replacement information is related.

sliceUsgCtrlInfoSets:

type: object

additionalProperties:

$ref: '#/components/schemas/SliceUsgCtrlInfo'

minProperties: 1

description: >

Represents the updated network slice usage control information.

The key of the map shall be set to the on-demand S-NSSAI (within the "snssai" attribute

of the corresponding map entry encoded using the SliceUsgCtrlInfo data structure) to

which the network slice usage control information is related.

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

required:

- resourceUri

TerminationNotification:

description: >

Represents a request to terminate a policy Association that the PCF provides in a

notification.

type: object

properties:

resourceUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

cause:

$ref: '#/components/schemas/PolicyAssociationReleaseCause'

required:

- resourceUri

- cause

SmfSelectionData:

description: Represents the SMF Selection information that may be replaced by the PCF.

type: object

properties:

unsuppDnn:

type: boolean

candidates:

type: object

additionalProperties:

$ref: '#/components/schemas/CandidateForReplacement'

minProperties: 1

description: >

Contains the list of DNNs per S-NSSAI that are candidates for replacement. The snssai

attribute within the CandidateForReplacement data type is the key of the map.

nullable: true

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

mappingSnssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

nullable: true

CandidateForReplacement:

description: Represents a list of candidate DNNs for replacement for an S-NSSAI.

type: object

properties:

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

dnns:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

minItems: 1

nullable: true

required:

- snssai

nullable: true

AmRequestedValueRep:

description: >

Represents the current applicable values corresponding to the policy control request

triggers.

type: object

properties:

userLoc:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

praStatuses:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

minProperties: 1

description: >

Contains the UE presence statuses for tracking areas. The praId attribute within the

PresenceInfo data type is the key of the map.

accessTypes:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/AccessType'

description: >

The Access Types where the served UE is camping.

minItems: 1

ratTypes:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

description: >

The 3GPP RAT Type and non-3GPP RAT Type where the served UE is camping.

allowedSnssais:

description: array of allowed S-NSSAIs for the 3GPP access.

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

n3gAllowedSnssais:

description: array of allowed S-NSSAIs for the Non-3GPP access.

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

partAllowedNssai:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PartiallyAllowedSnssai'

minProperties: 1

description: >

Represents the Partially Allowed NSSAI.

The key of the map shall be set to the value of the "snssai" attribute of the

corresponding map entry (encoded using the PartiallyAllowedSnssai data

structure).

snssaisPartRejected:

type: object

additionalProperties:

$ref: '#/components/schemas/SnssaiPartRejected'

minProperties: 1

description: >

Represents the set of S-NSSAI(s) rejected partially in the RA.

The key of the map shall be set to the value of the "snssai" attribute of the

corresponding map entry (encoded using the SnssaiPartRejected data structure).

rejectedSnssais:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 1

pendingNssai:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 1

AsTimeDistributionParam:

description: Contains the 5G acess stratum time distribution parameters.

type: object

properties:

asTimeDistInd:

type: boolean

description: >

Indicates the access stratum time distribution via Uu reference point is

Activated or not.

uuErrorBudget:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UintegerRm'

clkQltDetLvl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ClockQualityDetailLevel'

clkQltAcptCri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ClockQualityAcceptanceCriterion'

nullable: true

UeSliceMbr:

description: Contains a UE-Slice-MBR and the related information.

type: object

properties:

sliceMbr:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SliceMbr'

minProperties: 1

description: Contains the MBR for uplink and the MBR for downlink.

servingSnssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

mappedHomeSnssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

required:

- sliceMbr

- servingSnssai

nullable: true

SliceUsgCtrlInfo:

description: Represents network slice usage control information.

type: object

properties:

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

deregInactivTimer:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSecRm'

required:

- snssai

SnssaiPartRejected:

description: Represents the list of the S-NSSAI(s) rejected partially in the RA.

type: object

properties:

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

allowedTaiList:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Tai'

minItems: 1

rejectedTaiList:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Tai'

minItems: 1

required:

- snssai

oneOf:

- required: [ allowedTaiList ]

- required: [ rejectedTaiList ]

RequestTrigger:

anyOf:

- type: string

enum:

- LOC\_CH

- PRA\_CH

- SERV\_AREA\_CH

- RFSP\_CH

- ALLOWED\_NSSAI\_CH

- UE\_AMBR\_CH

- UE\_SLICE\_MBR\_CH

- SMF\_SELECT\_CH

- ACCESS\_TYPE\_CH

- NWDAF\_DATA\_CH

- TARGET\_NSSAI

- SLICE\_REPLACE\_MGMT

- FEAT\_RENEG

- PARTIALLY\_ALLOWED\_NSSAI\_CH

- SNSSAIS\_PARTIALLY\_REJECTED\_CH

- REJECTED\_SNSSAIS\_CH

- PENDING\_NSSAI\_CH

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: |

Represents the possible request triggers.

Possible values are:

- LOC\_CH: Location change (tracking area). The tracking area of the UE has changed.

- PRA\_CH: Change of UE presence in PRA. The AMF reports the current presence status

of the UE in a Presence Reporting Area, and notifies that the UE enters/leaves the

Presence Reporting Area.

- SERV\_AREA\_CH: Service Area Restriction change. The UDM notifies the AMF that the

subscribed service area restriction information has changed.

- RFSP\_CH: RFSP index change. The UDM notifies the AMF that the subscribed RFSP index has

changed.

- ALLOWED\_NSSAI\_CH: Allowed NSSAI change. The AMF notifies that the set of UE allowed

S-NSSAIs has changed.

- UE\_AMBR\_CH: UE-AMBR change. The UDM notifies the AMF that the subscribed UE-AMBR has

changed.

- SMF\_SELECT\_CH: SMF selection information change. The UE requested for an unsupported

DNN or UE requested for a DNN within the list of DNN candidates for replacement per

S-NSSAI.

- ACCESS\_TYPE\_CH: Access Type change. The AMF notifies that the access type and the RAT

type for a UE has changed.

- UE\_SLICE\_MBR\_CH: UE-Slice-MBR change. The NF service consumer notifies any changes

in the subscribed UE-Slice-MBR for each subscribed S-NSSAI of the home PLMN mapping

to a S-NSSAI of the serving PLMN.

- NWDAF\_DATA\_CH: NDWAF DATA CHANGE. The AMF notifies that the NWDAF instance IDs used

for the UE and/or associated Analytics IDs used for the UE and available in the AMF

have changed.

- TARGET\_NSSAI: Generation of Target NSSAI. The NF service consumer notifies that the

Target NSSAI was generated.

- SLICE\_REPLACE\_MGMT: Indicates that slice replacement is needed for one or more S-NSSAI(s)

of the UE's Allowed NSSAI and/or Partially Allowed NSSAI and the AMF cannot determine the

Alternative S-NSSAI(s) for these S-NSSAI(s).

- FEAT\_RENEG: The NF service consumer notifies that the target AMF is requesting feature

re-negotiation.

- PARTIALLY\_ALLOWED\_NSSAI\_CH: Partially Allowed NSSAI change. The NF service consumer

notifies that the set of Partially Allowed S-NSSAI(s) of the UE has changed.

- SNSSAIS\_PARTIALLY\_REJECTED\_CH: Change of the S-NSSAI(s) rejected partially in the RA. The

NF service consumer notifies that the set of S-NSSAI(s) rejected partially in the RA for

the UE has changed.

- REJECTED\_SNSSAIS\_CH: Change of the Rejected S-NSSAI(s) in the RA. The NF service consumer

notifies that the set of the Rejected S-NSSAI(s) in the RA for the UE has changed.

- PENDING\_NSSAI\_CH: Pending NSSAI change. The NF service consumer notifies that the set of

Pending S-NSSAI(s) of the UE has changed.

PolicyAssociationReleaseCause:

anyOf:

- type: string

enum:

- UNSPECIFIED

- UE\_SUBSCRIPTION

- INSUFFICIENT\_RES

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: |

Represents the cause why the PCF requests the termination of the policy association.

Possible values are:

- UNSPECIFIED: This value is used for unspecified reasons.

- UE\_SUBSCRIPTION: This value is used to indicate that the session needs to be

terminated because the subscription of UE has changed (e.g. was removed).

- INSUFFICIENT\_RES: This value is used to indicate that the server is overloaded and

needs to abort the session.

\*\*\* End of Changes \*\*\*