**3GPP TSG CT WG3 Meeting #134 *C3-242185r1***

**Changsha, China, 15-19 April 2024**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **29.122** | **CR** | **0825** | **rev** | **1** | **Current version:** | **18.5.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | missing applicable EnQoSMon feature for repPeriod and pdmf attributes |
|  |  |
| ***Source to WG:*** | ZTE |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | XRM |  | ***Date:*** | 2024-04-08 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** |  Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | According to the procedure description below from 29.522, EnQoSMon feature is applicable to "repPeriod" and "pdmf" attributes.- if the "EnQoSMon" feature is supported and QoS monitoring control is for packet delay and/or congestion and/or data rate and if the "MultiMedia" feature is supported, the request is not for multiple flows (i.e., the "multiModDatFlows" attribute is not included), the AF shall include:iii. within each of the provided QosMonitoringInformation data structure(s):3. when the "repFreqs" attribute includes the value "PERIODIC", the periodic time for reporting and the maximum period with no QoS measurement results reported within the "repPeriod" attribute; and4. when the "repFreqs" attribute includes the value "EVENT\_TRIGGERED":d. the maximum period with no QoS measurement results reported within the "repPeriod" attribute.Within the QosMonitoringReport data structure, the NEF shall include the received monitored QoS information.- if the feature "PacketDelayFailureReport" is supported or the "EnQoSMon" feature is supported, the packet delay measurement failure indicator within the "pdmf" attribute; |
|  |  |
| ***Summary of change:*** | Add EnQoSMon feature to the applicable feature column of "repPeriod" attribute and "pdmf" attribute to align with 29.522. |
|  | on |
| ***Consequences if not approved:*** | Misalignment with 29.522. |
|  |  |
| ***Clauses affected:*** | 5.14.4 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR does not have any impact in the OpenAPI specification. |
|  |  |
| ***This CR's revision history:*** |  |

**Additional discussion(if needed):**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

### 5.14.4 Used Features

The table below defines the features applicable to the AsSessionWithQoS API. Those features are negotiated as described in subclause 5.2.7.

**Table 5.14.4-1: Features used by AsSessionWithQoS API**

|  |  |  |
| --- | --- | --- |
| **Feature Number** | **Feature** | **Description** |
| 1 | Notification\_websocket | The delivery of notifications over Websocket is supported according to clause 5.2.5.4. This feature requires that the Notification\_test\_event featute is also supported. |
| 2 | Notification\_test\_event | The testing of notifications connections is supported according to clause 5.2.5.3. |
| 3 | EthAsSessionQoS\_5G | Setting up required QoS for Ethernet UE. This feature may only be supported in 5G. |
| 4 | MacAddressRange\_5G | Indicates the support of a set of MAC addresses with a specific range in the traffic filter. This feature may only be supported in 5G. |
| 5 | AlternativeQoS\_5G | Indicates the support of alternative QoS requirements and the QoS notification (i.e. whether the QoS targets for SDF(s) are not guaranteed or guaranteed again). This feature may only be supported in 5G. |
| 6 | QoSMonitoring\_5G | Indicates the support of QoS Monitoring functionality and the report for packet delay monitoring. This feature may only be supported in 5G. |
| 7 | DisableUENotification\_5G | Indicates the support of disabling QoS flow parameters signalling to the UE when the SMF is notified by the NG-RAN of changes in the fulfilled QoS situation. This feature may only be supported in 5G. This feature requires that the AlternativeQoS\_5G feature is also supported. |
| 8 | TSC\_5G | Indicates the support of Time Sensitive Communication. This feature may only be supported in 5G. |
| 9 | AppId | Indicates the support of dynamically providing the Application Identifier via the API. |
| 10 | ExposureToEAS | This feature indicates the support of direct notification in 5GC. This feature requires that the QoSMonitoring\_5G feature is also supported. |
| 11 | enNB | Indicates the support of enhancements to the northbound interfaces. |
| 12 | AltQosWithIndParams\_5G | This feature indicates the support of provisioning Alternative Service Requirements with individual QoS parameters. This feature requires that the AlternativeQoS\_5G feature is also supported. |
| 13 | EnEthAsSessionQoS\_5G | Indicates the support of required QoS for Ethernet UE, allowing to indicate separately different UL and/or DL Ethernet flows. This feature may only be supported in 5G. |
| 14 | enNB\_5G | Indicates the support of enhancements to the northbound interfaces and only applicable to 5G. |
| 15 | PacketDelayFailureReport | Indicates the support of packet delay failure report as part of QoS Monitoring procedures. This feature requires that QoSMonitoring\_5G is supported. This feature may only be supported in 5G. |
| 16 | ToSTC\_5G | Indicates the support of Type of Service or Traffic Class. This feature may only be supported in 5G. |
| 17 | EnTSCAC | Indicates the support of extensions to TSCAC and the RAN feedback for BAT offset and adjusted periodicity.This feature may only be supported in 5G, and requires that the TSC\_5G feature is also supported. |
| 18 | AltQoSProfilesSupportReport | This feature indicates the support of the report of whether Alternative QoS parameters are supported by the access network. This feature requires that AlternativeQoS\_5G and/or AltQosWithIndParams\_5G features are also supported. |
| 19 | ExtQoS\_5G | This feature indicates the support of extended QoS parameters. This feature may only be supported in 5G. |
| 20 | MultiMedia | Indicates the support for multi-modal or multimedia flows for single UE and multiple UE. This feature may only be supported in 5G. This feature may be used in eXtend Reality (XR) use cases. |
| 21 | ExtErrors | Indicates the support of additional application errors related to authorization or PDU Session availability. |
| 22 | QoSTiming\_5G | This feature indicates the support of QoS timing information for the transfer and support of data transmission (e.g., AI/ML transmission). This feature may only be supported in 5G. |
| 23 | ListUE\_5G | Indicates the support for the list of UEs This feature may only be supported in 5G. |
| 24 | GMEC\_5G | This feature indicates the support of Generic Group Management Exposure and Communication related enhancements.The following functionalities are supported:- Support AF requested QoS for a UE or group of UE(s) not identified by the UE address(es).This feature may only be supported in 5G.This feature requires the support of the "QoSMonitoring\_5G" and "AltQosWithIndParams\_5G" features. |
| 25 | PDUSetHandling | This feature indicates the support of PDU Set handling. This feature may be used for eXtended Reality (XR) and interactive media services.This feature may only be supported in 5G. |
| 26 | RTLatency | This feature indicates the support of Round-Trip latency. This feature may be used for eXtended Reality (XR) and interactive media services.This feature may only be supported in 5G. |
| 27 | EnQoSMon | This feature indicates the support of enhanced QoS monitoring functionality, i.e. the report of the congestion information, and/or, the RTT delay over two QoS flows, and/or, the data rate information, and/or, the Packet Delay Variation monitoring.This feature requires that QoSMonitoring\_5G is supported.In order to support the report of packet delay measurement failure, the PacketDelayFailureReport feature also requires to be supported.This feature may only be supported in 5G |
| 28 | PowerSaving | This feature indicates the support of the Power Saving for different traffic measurement**.**This feature may only be supported in 5G. |
| 29 | L4S | This feature indicates the support of the AF indication of ECN marking for L4S support.This feature may only be supported in 5G. |
| Feature: A short name that can be used to refer to the bit and to the feature, e.g. "Notification".Description: A clear textual description of the feature. |

Editor's Note: Whether and/how to indicate the support of end of burst indication, and provision the flow periodicity information within the Power Saving feature is FFS.

\*\*\* End of Changes \*\*\*