**3GPP TSG-CT WG3 Meeting #134 *C3-242179r1***

**Changsha, China, 15-19 April 2024**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.520** | **CR** | **0885** | **rev** | **1** | **Current version:** | **18.5.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | MLModel Training Notification correction | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | ZTE | | | | | | | | | |
| ***Source to TSG:*** | CT3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | eNA\_Ph3 | | | | |  | ***Date:*** | | | 2024-04-08 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | notifUri is contained not only in NwdafMLModelTrainSubsc data type, but also in NwdafMLModelTrainSubscPatch data type, however the latter one is not mentioned in the description of callback URI in the Table 5.5.5.2.2-1.  The Nnwdaf\_MLModelTraining\_Notify request includes an array of NwdafMLModelTrainNotif, and NwdafMLModelTrainNotif includes an array of  MLEventNotif. As the MLEventNotif data type contains the modle info for each analytics event, including a single NwdafMLModelTrainNotif in the notification is enough. Furthermore, it’s not indicated in the corresponding notification procedure that the POST request includes a list of NwdafMLModelTrainNotif data type. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Table 5.5.5.2.2-1 is updated to cover NwdafMLModelTrainSubscPatch data type.  Change array of NwdafMLModelTrainNotif to single in Nnwdaf\_MLModelTraining\_Notify.  Change array of NwdafMLModelTrainNotif to single in NwdafMLModelTrainSubsc for immediate reporting. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Incomplele description of notifUri. Not proper data type definition. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.5.5.2.2, 5.5.6.2.2, A.6 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR introduces a backwards compatible correction to the OpenAPI file of the Nnwdaf\_MLModelTraining API. | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

**Additional discussion(if needed):**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

##### 5.5.5.2.2 Operation Definition

Callback URI: **{notifUri}**

The operation shall support the callback URI variables defined in table 5.5.5.2.2-1, the request data structures specified in table 5.5.5.2.2-2 and the response data structure and response codes specified in table 5.5.5.2.2-3.

Table 5.5.5.2.2-1: Callback URI variables

|  |  |  |
| --- | --- | --- |
| Name | Data type | Definition |
| notifUri | Uri | The Notification Uri as assigned within the Individual NWDAF ML Model Training Subscription and described within the NwdafMLModelTrainSubsc/NwdafMLModelTrainSubscPatch data types (see tables 5.5.6.2.2-1 and 5.5.6.2.3-1). |

Table 5.5.5.2.2-2: Data structures supported by the POST Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| NwdafMLModelTrainNotif | M | 1 | Provides Information about observed events. |

**Table 5.5.5.2.2-3: Data structures supported by the POST Response Body on this resource**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Data type** | **P** | **Cardinality** | **Response codes** | **Description** |
| n/a |  |  | 204 No Content | The receipt of the Notification is acknowledged. |
| RedirectResponse | O | 0..1 | 307 Temporary Redirect | Temporary redirection, during the event notification. The response shall include a Location header field containing an alternative URI representing the end point of an alternative NF consumer (service) instance where the notification should be sent. |
| RedirectResponse | O | 0..1 | 308 Permanent Redirect | Permanent redirection, during the event notification. The response shall include a Location header field containing an alternative URI representing the end point of an alternative NF consumer (service) instance where the notification should be sent. |
| NOTE: The mandatory HTTP error status codes for the POST method listed in table 5.2.7.1-1 of 3GPP TS 29.500 [6] also apply. | | | | | |

Table 5.5.5.2.2-4: Headers supported by the 307 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | An alternative URI representing the end point of an alternative NF consumer (service) instance towards which the notification should be redirected. |
| 3gpp-Sbi-Target-Nf-Id | string | O | 0..1 | Identifier of the target NF (service) instance towards which the notification request is redirected. |

Table 5.5.5.2.2-5: Headers supported by the 308 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | An alternative URI representing the end point of an alternative NF consumer (service) instance towards which the notification should be redirected. |
| 3gpp-Sbi-Target-Nf-Id | string | O | 0..1 | Identifier of the target NF (service) instance towards which the notification request is redirected |

\*\*\* 2nd Change \*\*\*

##### 5.5.6.2.2 Type NwdafMLModelTrainSubsc

Table 5.5.6.2.2-1: Definition of type NwdafMLModelTrainSubsc

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  | |  | |  | |  | |  | |
| Attribute name | | Data type | | P | | Cardinality | | Description | | Applicability | |
| eventReq | | ReportingInformation | | O | | 0..1 | | Reporting requirement information of the subscription.  If omitted, the default values within the ReportingInformation data type apply. | |  | |
| failEventReports | | array(FailureEventInfoForMLModelTrain) | | O | | 1..N | | Supplied by the NWDAF containing MTLF when available, shall contain the event(s) that the subscription is not successful including the failure reason(s). | |  | |
| mlCorreId | | string | | C | | 0..1 | | Identifies the Machine Learning procedure for training the ML model.  It shall be present when the service is for Federated Learning. | |  | |
| mLEventSubscs | | array(MLEventSubscription) | | M | | 1..N | | Each element identifies the subscription for each event. The "modelInterInfo" attribute within the MLEventSubscription data type shall be provided. | |  | |
| mLModelInfos | | array(MLEventNotif) | | O | | 1..N | | Each element contains ML Model information for a specific analytics type. (NOTE) | |  | |
| immReports | | NwdafMLModelTrainNotif | | O | | 0..1 | | Immediately reported ML Model Training notifications. It may only be provided in the HTTP POST response of a subscription creation/update and only if the immediate reporting flag was set to "true" in the HTTP POST request. | |  | |
| mLModelTrainInfos | | array(MLModelTrainInfo) | | O | | 1..N | | Each element represents the ML Model training information for each event, include requirement on data availability and time availability. | |  | |
| mLPreFlag | | boolean | | C | | 0..1 | | Indicates whether the subscription is for preparation of ML Model training. Set to "true" if it is for ML training preparation, otherwise set to "false".  Default value is "false" if omitted.  It shall be present when the service is for preparation of Federated Learning. | |  | |
| mLAccChkFlg | | boolean | | O | | 0..1 | | Indicates whether request using the local training data as the testing dataset to calculate the Model Accuracy of the global ML model provided by the consumer. Set to "true" if it is requested, otherwise set to "false".  Default value is "false" if omitted. | |  | |
| mLTrainRepInfo | | MLTrainReportInfo | | O | | 0..1 | | Indicates the training reporting information.  This attribute can be provided when the "notifMethod" attribute within the ReportingInformation structure is set to "ON\_EVENT\_DETECTION" in the "eventReq" attribute. | |  | |
| notifCorreId | | string | | M | | 1 | | The value of Notification Correlation ID in the corresponding notification. | |  | |
| notifUri | | Uri | | M | | 1 | | URI at which the NF service consumer requests to receive notifications. | |  | |
| roundInd | | Uinteger | | O | | 0..1 | | Indicates the round number of the training in a multi-round training process. | |  | |
| suppFeats | | SupportedFeatures | | C | | 0..1 | | List of Supported features used as described in clause 5.5.8.  It shall be supplied by NF service consumer in the POST requests that request the creation of an NWDAF ML Model Training Subscriptions resource and shall be supplied by the NWDAF in the reply of corresponding request. | |  | |
| tgtRepUe | | TargetUeInformation | | O | | 0..1 | | Indicates the UE(s) information for which data for ML model training is requested. | |  | |
| uCaseCont | | string | | O | | 0..1 | | Indicates the use case context of the ML model. The value and format of this parameter are not standardized. | |  | |
| NOTE: It is up to implementation to determine whether to include the "mlFile" arttribute in the "MLEventNotif" data structure considering ML Model file size, etc. | | | | | | | | | | | |

\*\*\* 3rd Change \*\*\*

# A.6 Nnwdaf\_MLModelTraining API

openapi: 3.0.0

info:

title: Nnwdaf\_MLModelTraining

version: 1.0.0-alpha.3

description: |

Nnwdaf\_MLModelTraining API Service.

© 2023, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.520 V18.4.0; 5G System; Network Data Analytics Services.

url: https://www.3gpp.org/ftp/Specs/archive/29\_series/29.520/

servers:

- url: '{apiRoot}/nnwdaf-mlmodeltraining/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 4.4 of 3GPP TS 29.501

security:

- {}

- oAuth2ClientCredentials:

- nnwdaf-mlmodeltraining

paths:

/subscriptions:

post:

summary: Create a new Individual NWDAF ML Model Training Subscription resource.

operationId: CreateNWDAFMLModelTrainingSubcription

tags:

- Subscriptions (Collection)

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/NwdafMLModelTrainSubsc'

responses:

'201':

description: Create a new Individual NWDAF ML Model Training Subscription resource.

content:

application/json:

schema:

$ref: '#/components/schemas/NwdafMLModelTrainSubsc'

headers:

Location:

description: >

Contains the URI of the newly created resource, according to the structure

{apiRoot}/nnwdaf-mlmodeltraining/v1/subscriptions/{subscriptionId}.

required: true

schema:

type: string

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

callbacks:

myNotification:

'{$request.body#/notifUri}':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/NwdafMLModelTrainNotif'

responses:

'204':

description: No Content, Notification was succesfull

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/subscriptions/{subscriptionId}:

put:

summary: update an existing Individual NWDAF ML Model Training Subscription

operationId: UpdateNWDAFMLModelTrainingSubcription

tags:

- Individual NWDAF ML Model Training Subscription (Document)

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/NwdafMLModelTrainSubsc'

parameters:

- name: subscriptionId

in: path

description: String identifying a subscription to the Nnwdaf\_MLModelTraining Service.

required: true

schema:

type: string

responses:

'200':

description: >

The Individual NWDAF ML Model Training Subscription resource was modified successfully

and a representation of that resource is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/NwdafMLModelTrainSubsc'

'204':

description: >

The Individual NWDAF ML Model Training Subscription resource was modified successfully.

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

patch:

summary: partial update an existing Individual NWDAF ML Model Training Subscription

operationId: PartialUpdateNWDAFMLModelTrainingSubcription

tags:

- Individual NWDAF ML Model Training Subscription (Document)

requestBody:

required: true

content:

application/merge-patch+json:

schema:

$ref: '#/components/schemas/NwdafMLModelTrainSubscPatch'

parameters:

- name: subscriptionId

in: path

description: String identifying a subscription to the Nnwdaf\_MLModelTraining Service.

required: true

schema:

type: string

responses:

'200':

description: >

The Individual NWDAF ML Model Training Subscription resource was partial modified

successfully and a representation of that resource is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/NwdafMLModelTrainSubsc'

'204':

description: >

The Individual NWDAF ML Model Training Subscription resource was partial modified

successfully.

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

summary: Delete an existing Individual NWDAF ML Model Training Subscription.

operationId: DeleteNWDAFMLModelTrainingSubcription

tags:

- Individual NWDAF ML Model Training Subscription (Document)

parameters:

- name: subscriptionId

in: path

description: String identifying a subscription to the Nnwdaf\_MLModelTraining Service.

required: true

schema:

type: string

responses:

'204':

description: >

No Content. The Individual NWDAF ML Model Training Subscription matching the

subscriptionId was deleted.

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{nrfApiRoot}/oauth2/token'

scopes:

nnwdaf-mlmodeltraining: Access to the Nnwdaf\_MLModelTraining API

schemas:

NwdafMLModelTrainSubsc:

description: Represents a ML Model Training subscription.

type: object

properties:

mLEventSubscs:

type: array

items:

$ref: 'TS29520\_Nnwdaf\_MLModelProvision.yaml#/components/schemas/MLEventSubscription'

minItems: 1

description: Subscribed events

notifUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

suppFeats:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

eventReq:

$ref: 'TS29523\_Npcf\_EventExposure.yaml#/components/schemas/ReportingInformation'

failEventReports:

type: array

items:

$ref: '#/components/schemas/FailureEventInfoForMLModelTrain'

minItems: 1

description: >

Supplied by the NWDAF containing MTLF when available, shall contain the event(s) that

the subscription is not successful including the failure reason(s).

mlCorreId:

type: string

description: String identifying the subscription is for a Federated Learning procedure.

mLModelInfos:

type: array

items:

$ref: 'TS29520\_Nnwdaf\_MLModelProvision.yaml#/components/schemas/MLEventNotif'

minItems: 1

description: Represents the ML Model information.

immReports:

$ref: '#/components/schemas/NwdafMLModelTrainNotif'

description: Immediately reported ML Model Training notifications.

mLModelTrainInfos:

type: array

items:

$ref: '#/components/schemas/MLModelTrainInfo'

minItems: 1

description: Represents the ML Model training information.

mLPreFlag:

type: boolean

description: >

Indicates whether the subscription is for preparation of ML Model training. Set to

"true" if it is for ML training preparation, otherwise set to "false".

mLAccChkFlg:

type: boolean

description: >

Indicates whether request using the local training data as the testing dataset to

calculate the Model Accuracy of the global ML model provided by the consumer. Set to

"true" if it is requested, otherwise set to "false".

mLTrainRepInfo:

$ref: '#/components/schemas/MLTrainReportInfo'

notifCorreId:

type: string

description: >

String identifying the Notification Correlation ID in the corresponding notification.

roundInd:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

tgtRepUe:

$ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/TargetUeInformation'

uCaseCont:

type: string

description: >

String identifying the use case context of the ML model. The value and format of this

parameter is not standardized.

required:

- mLEventSubscs

- notifUri

- notifCorreId

NwdafMLModelTrainSubscPatch:

description: >

Represents parameters to request the modification of a ML Model Training subscription.

type: object

properties:

notifUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

eventReq:

$ref: 'TS29523\_Npcf\_EventExposure.yaml#/components/schemas/ReportingInformation'

mLModelInfos:

type: array

items:

$ref: 'TS29520\_Nnwdaf\_MLModelProvision.yaml#/components/schemas/MLEventNotif'

minItems: 1

description: Represents the ML Model information.

mLModelTrainInfos:

type: array

items:

$ref: '#/components/schemas/MLModelTrainInfo'

minItems: 1

description: Represents the ML Model training information.

mLPreFlag:

type: boolean

description: >

Indicates whether the subscription is for preparation of ML Model training. Set to

"true" if it is for ML training preparation, otherwise set to "false".

mLAccChkFlg:

type: boolean

description: >

Indicates whether request using the local training data as the testing dataset to

Calculate the Model Accuracy of the global ML model provided by the consumer. Set to

"true" if it is requested, otherwise set to "false".

mLTrainRepInfo:

$ref: '#/components/schemas/MLTrainReportInfo'

roundInd:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

tgtRepUe:

$ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/TargetUeInformation'

uCaseCont:

type: string

description: >

String identifying the use case context of the ML model. The value and format of this

parameter are not standardized.

NwdafMLModelTrainNotif:

description: Represents notifications on events that occurred.

type: object

properties:

delayEventNotif:

$ref: '#/components/schemas/DelayEventNotif'

mlCorreId:

type: string

description: String identifying the subscription is for a Federated Learning procedure.

mLModelInfos:

type: array

items:

$ref: 'TS29520\_Nnwdaf\_MLModelProvision.yaml#/components/schemas/MLEventNotif'

minItems: 1

description: Represents the ML Model information.

notifCorreId:

type: string

description: >

String identifying the Notification Correlation ID in the corresponding notification.

roundInd:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

statusReport:

$ref: '#/components/schemas/StatusReportInfo'

termTrainReq:

$ref: '#/components/schemas/TermTrainCause'

uCaseCont:

type: string

description: >

String identifying the context of use of ML model. The value and format of this

parameter are not standardized.

required:

- notifCorreId

oneOf:

- required: [delayEventNotif]

- required: [mLModelInfos]

- required: [termTrainReq]

- required: [mLModelInfos, termTrainReq]

MLModelTrainInfo:

description: >

Represents the ML Model training information, include requirement on data availability and

time availability, training filter information.

type: object

properties:

dataAvReq:

$ref: '#/components/schemas/DataAvReq'

timeAvReq:

type: string

description: >

String representing the requirement on available time for the ML model training.

MLTrainReportInfo:

description: Represents the ML Model training reporting information.

type: object

properties:

maxResTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

FailureEventInfoForMLModelTrain:

description: Represents the failure event information for a ML Model Training subscription.

type: object

properties:

mLTrainEvent:

$ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/NwdafEvent'

failureCodeTrain:

$ref: '#/components/schemas/FailureCodeTrain'

required:

- mLTrainEvent

- failureCodeTrain

DataAvReq:

description: Represents the requirement on available data for the ML model training.

type: object

properties:

dataStatProps:

type: array

items:

$ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/DatasetStatisticalProperty'

minItems: 1

inpEvents:

type: array

items:

$ref: 'TS29574\_Ndccf\_DataManagement.yaml#/components/schemas/DccfEvent'

minItems: 1

minNumSamples:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

timeWindows:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

minItems: 1

required:

- inpEvents

DelayEventNotif:

description: >

Indicating that the NWDAF containing MTLF is not able to complete the training of ML model

within the maximum response time, the cause code, and the expected time complete the

training.

type: object

properties:

delayEventInd:

type: boolean

description: >

Indicates that the NWDAF containing MTLF is not able to complete the training of ML

model within the maximum response time. Set to "true" if not able to complete the ML

model training on time, otherwise set to "false".

delayCause:

$ref: '#/components/schemas/DelayCause'

expCompTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

required:

- delayEventInd

StatusReportInfo:

description: >

Indicating status information generated by the NWDAF containing MTLF during ML model

training.

type: object

properties:

mlModelAcc:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

trainInDataInfo:

$ref: '#/components/schemas/TrainDataInfo'

TrainDataInfo:

description: Represents the training input data information.

type: object

properties:

areaDataSet:

type: string

description: Indicates the areas covered by the data set.

maxValues:

type: array

items:

type: string

minItems: 1

description: Represents the maximum value of one dimension of data.

minValues:

type: array

items:

type: string

minItems: 1

description: Represents the minimum value of one dimension of data.

samplRatio:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

#

# ENUMERATIONS DATA TYPES

#

FailureCodeTrain:

anyOf:

- type: string

enum:

- UNAVAILABLE\_ML\_MODEL\_TRAIN

- type: string

description: >

This string provides forward-compatibility with future extensions to the enumeration but

is not used to encode content defined in the present version of this API.

description: |

Represents the failure reason.

Possible values are:

- UNAVAILABLE\_ML\_MODEL\_TRAIN: The ML model training is unavailable.

TermTrainCause:

anyOf:

- type: string

enum:

- NWDAF\_OVERLOAD

- NOT\_AVAILABLE\_ML\_TRAIN

- OTHERS

- type: string

description: >

This string provides forward-compatibility with future extensions to the enumeration but

is not used to encode content defined in the present version of this API.

description: |

Represents the reasons that ML Model Training to be terminated.

Possible values are:

- NWDAF\_OVERLOAD: The NWDAF is overloaded for the ML model training.

- NOT\_AVAILABLE\_ML\_TRAIN: The ML model training process is not available.

- OTHERS: Other cause.

DelayCause:

anyOf:

- type: string

enum:

- ML\_MODEL\_TRAIN\_FAILURE

- NEED\_MORE\_TIME

- OTHERS

- type: string

description: >

This string provides forward-compatibility with future extensions to the enumeration but

is not used to encode content defined in the present version of this API.

description: |

Represents the reasons for ML Model training delay.

Possible values are:

- ML\_MODEL\_TRAIN\_FAILURE: The ML model training is failure.

- NEED\_MORE\_TIME: The ML model training needs more time.

- OTHERS: Other cause.

\*\*\* End of Changes \*\*\*