**3GPP TSG-CT WG4 Meeting #103-eC4-212xyz**

**E-Meeting, 14th – 23rd April 2021 (was C4-212125)**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **29.505** | **CR** | **0340** | **rev** | **1** | **Current version:** | **17.2.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Response for MWD resource creation |
|  |  |
| ***Source to WG:*** | Ericsson |
| ***Source to TSG:*** | CT4 |
|  |  |
| ***Work item code:*** | SBIProtoc17 |  | ***Date:*** | 2021-04-02 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | PUT method is defined for the creation of MessageWaitingData resource. But 201 Created reponse as the normal response for resource creation is missing. |
|  |  |
| ***Summary of change:*** | It is proposed to add 201 Created response for PUT operation on resource URI ‘{apiRoot}/nudr-dr/<apiVersion>/subscription-data/{ueId}/context-data/mwd’ when the resource is created and at the same time location header contained the URI of the created resource (used for GET/PATCH/DELETE operation) is returned. |
|  |  |
| ***Consequences if not approved:*** | Misaligned with other PUT method operation for response on resource creation, may cause interoperation problems on protocol implementations between the service consumer and service producer. |
|  |  |
| ***Clauses affected:*** | 5.2.12B.3.1, A.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR introduces backwards compatible corrections, with impacts to the following APIs:- TS29504\_Nudr\_DataRepository.yaml |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* First Change \* \* \* \*

##### 5.2.12B.3.1 PUT

This method shall support the URI query parameters specified in table 5.2.12B.3.1-1.

Table 5.2.12B.3.1-1: URI query parameters supported by the PUT method on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| n/a |  |  |  |  |

This method shall support the request data structures specified in table 5.2.12B.3.1-2 and the response data structures and response codes specified in table 5.2.12B.3.1-3.

Table 5.2.12B.3.1-2: Data structures supported by the PUT Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| MessageWaitingData | M | 1 | The Message Waiting Data list is created or updated with the received information. |

Table 5.2.12B.3.1-3: Data structures supported by the PUT Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Responsecodes | Description |
| n/a |  |  | 204 No Content | If the resource already existed, and it is successfully updated, an empty response body shall be returned  |
| MessageWaitingData | M | 1 | 201 Created | If the resource did not already exist, and it is successfully created, a response body containing a representation of the created Individual MessageWaitingData resource shall be returned. |
| NOTE: In addition, common data structures as listed in table 5.5-1 are supported. |

\* \* \* Next Change \* \* \* \*

## A.2 Nudr\_DataRepository API for Subscription Data

*(... text not shown for clarity ...)*

/subscription-data/{ueId}/context-data/mwd:

 put:

 summary: Create the Message Waiting Data of the UE

 operationId: CreateMessageWaitingData

 tags:

 - Message Waiting Data (Document)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nudr-dr

 - oAuth2ClientCredentials:

 - nudr-dr

 - nudr-dr:subscription-data

 parameters:

 - name: ueId

 in: path

 description: UE id

 required: true

 schema:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/VarUeId'

 requestBody:

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/MessageWaitingData'

 required: true

 responses:

 '201':

 description: Created

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/MessageWaitingData'

 headers:

 Location:

 description: 'Contains the URI of the newly created resource, according to the structure: {apiRoot}/nudr-dr/<apiVersion>/subscription-data/{ueId}/context-data/mwd'

 required: true

 schema:

 type: string

 '204':

 description: Upon success, an empty response body shall be returned

 default:

 description: Unexpected error

*(... text not shown for clarity ...)*

\* \* \* End of Changes \* \* \* \*