**3GPP TSG-CT WG4 Meeting #104-eC4-213xyz**

**E-Meeting, 19th – 28th May 2021 (was C4-213303)**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.503** | **CR** | **0654** | **rev** | **1** | **Current version:** | **17.2.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Identifier Translation | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Ericsson | | | | | | | | | |
| ***Source to TSG:*** | CT4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | SBIProtoc17 | | | | |  | ***Date:*** | | | 2021-05-08 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | 23.502 defines the following use cases for NEF as service consumer of Nudm id-translation-result service:   * UC1 4.13.2.2 step 4 stated that: The NEF invokes Nudm\_SDM\_Get (Identifier Translation, GPSI and AF Identifier) to resolve the GPSI to SUPI when the AF is authorized to trigger the UE.   NOTE 1: Optionally, mapping from GPSI (External Id) to GPSI (MSISDN) is also provided for legacy SMS infrastructure not supporting MSISDN-less SMS.   * UC2 4.13.7.2 step 3 stated that: The NEF invokes Nudm\_SDM\_Get (Identifier Translation, IMSI, Application Port ID, AF Identifier) to resolve the IMSI and Application Port ID to a GPSI (External Id). * UC3 4.15.6.8 step 3 stated that: The NEF invokes Nudm\_SDM\_Get (Identifier Translation, GPSI) to resolve the GPSI (External Identifier) to a SUPI.   Current Nudm id-transation service doesn’t include AF identifier (required in UC1 and UC2) as input query parameter for authorization.  It also does not include the requested GPSI type (additional GPSI type for UC1, requested GPSI type in UC2). | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | It is proposed to include:   * AF identifier as optional query parameter to indicate whether authorization based on AF identifier is additionally required * requested-GPSI-type as optional query parameter to indicate whether a specific GPSI type is additional required | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Stage 2 relevant use cases can’t be fulfilled | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 6.1.3.12.1, 6.1.3.12.3.1, 6.1.6.1, 6.1.6.3.X (new), A.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **x** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **x** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **x** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR introduces backwards compatible new features, with impacts to the following APIs:  - TS29503\_Nudm\_SDM.yaml | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

\* \* \* First Change \* \* \* \*

#### 6.1.3.12 Resource: IdTranslationResult (Document)

##### 6.1.3.12.1 Description

This resource represents the SUPI or GPSI. It is queried by the NEF for GPSI to SUPI translation or SUPI to GPSI translation. See 3GPP TS 23.502 [3] clauses 4.13.2.2, 4.13.7.2 and 4.15.6.8.

##### 6.1.3.12.2 Resource Definition

Resource URI: {apiRoot}/nudm-sdm/<apiVersion>/{ueId}/id-translation-result

This resource shall support the resource URI variables defined in table 6.1.3.12.2-1.

Table 6.1.3.12.2-1: Resource URI variables for this resource

|  |  |  |
| --- | --- | --- |
| Name | Data type | Definition |
| apiRoot | string | See clause 6.1.1 |
| ueId | VarUeId | Represents the Generic Public Subscription Identifier (see 3GPP TS 23.501 [2] clause 5.9.8) or Subscription Permanent Identifier (see 3GPP TS 23.501 [2] clause 5.9.2)  pattern: See pattern of type VarUeId in 3GPP TS 29.571 [7] |

##### 6.1.3.12.3 Resource Standard Methods

###### 6.1.3.12.3.1 GET

This method shall support the URI query parameters specified in table 6.1.3.12.3.1-1.

Table 6.1.3.12.3.1-1: URI query parameters supported by the GET method on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| supported-features | SupportedFeatures | O | 0..1 | see 3GPP TS 29.500 [4] clause 6.6 |
| af-id | string | O | 0..1 | AF Identifier, see 3GPP TS 23.502 [3] clause 4.13.2.2 and clause 4.13.7.2  If not present, additional authorization on AF indentifier is not required (see 3GPP TS 23.502 [3] clause 4.15.6.8) |
| app-port-id | AppPortId | C | 0..1 | If ueId is a SUPI in Resource URI variables, this shall be present and indicates Application port identity, see 3GPP TS 23.501 [2] clause 4.4.7 or 3GPP TS 23.502 [3] clause 4.13.7.2 |
| requested-gpsi-type | GpsiType | C | 0..1 | Indicates the requested GPSI type, and it may be included when the ueId variable in the resource URI is a SUPI.  If the ueId variable in the resource URI is a GPSI, this parameter should not be included (i.e., in that case, the UDM returns the GPSI type that was not used in ueId, if available). |

This method shall support the request data structures specified in table 6.1.3.12.3.1-2 and the response data structures and response codes specified in table 6.1.3.12.3.1-3.

Table 6.1.3.12.3.1-2: Data structures supported by the GET Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| n/a |  |  |  |

Table 6.1.3.12.3.1-3: Data structures supported by the GET Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response  codes | Description |
| IdTranslationResult | M | 1 | 200 OK | Upon success, a response body containing the SUPI and optionally the MSISDN shall be returned. |
| ProblemDetails | O | 0..1 | 404 Not Found | The "cause" attribute may be used to indicate one of the following application errors:  - USER\_NOT\_FOUND  - DATA\_NOT\_FOUND |
| NOTE: In addition common data structures as listed in table 5.2.7.1-1 of 3GPP TS 29.500 [4] are supported. | | | | |

Table 6.1.3.12.3.1-4: Headers supported by the GET method on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| If-None-Match | string | O | 0..1 | Validator for conditional requests, as described in IETF RFC 7232 [25], clause 3.2 |
| If-Modified-Since | string | O | 0..1 | Validator for conditional requests, as described in IETF RFC 7232 [25], clause 3.3 |

Table 6.1.3.12.3.1-5: Headers supported by the 200 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Cache-Control | string | O | 0..1 | Cache-Control containing max-age, as described in IETF RFC 7234 [26], clause 5.2 |
| ETag | string | O | 0..1 | Entity Tag, containing a strong validator, as described in IETF RFC 7232 [25], clause 2.3 |
| Last-Modified | string | O | 0..1 | Timestamp for last modification of the resource, as described in IETF RFC 7232 [25], clause 2.2 |

\* \* \* Next Change \* \* \* \*

#### 6.1.6.1 General

This clause specifies the application data model supported by the API.

Table 6.1.6.1-1 specifies the data types defined for the Nudm\_SDM service API.

Table 6.1.6.1-1: Nudm\_SDM specific Data Types

|  |  |  |
| --- | --- | --- |
| Data type | Clause defined | Description |
| Nssai | 6.1.6.2.2 | Network Slice Selection Assistance Information |
| SdmSubscription | 6.1.6.2.3 | A subscription to notifications |
| AccessAndMobilitySubscriptionData | 6.1.6.2.4 | Access and Mobility Subscription Data |
| SmfSelectionSubscriptionData | 6.1.6.2.5 | SMF Selection Subscription Data |
| DnnInfo | 6.1.6.2.6 | Data Network Name and associated information (LBO roaming allowed flag) |
| SnssaiInfo | 6.1.6.2.7 | S-NSSAI and associated information (DNN Info) |
| SessionManagementSubscriptionData | 6.1.6.2.8 | User subscribed session management data |
| DnnConfiguration | 6.1.6.2.9 | User subscribed data network configuration |
| PduSessionTypes | 6.1.6.2.11 | Default/allowed session types for a data network |
| SscModes | 6.1.6.2.12 | Default/allowed SSC modes for a data network |
| SmsSubscriptionData | 6.1.6.2.13 |  |
| SmsManagementSubscriptionData | 6.1.6.2.14 | SMS Management Subscription Data |
| SubscriptionDataSets | 6.1.6.2.15 |  |
| UeContextInSmfData | 6.1.6.2.16 | UE Context In SMF Data |
| PduSession | 6.1.6.2.17 |  |
| IdTranslationResult | 6.1.6.2.18 | SUPI that corresponds to a given GPSI |
| ModificationNotification | 6.1.6.2.21 |  |
| IpAddress | 6.1.6.2.22 | IP address (IPv4, or IPv6, or IPv6 prefix) |
| UeContextInSmsfData | 6.1.6.2.23 |  |
| SmsfInfo | 6.1.6.2.24 |  |
| AcknowledgeInfo | 6.1.6.2.25 |  |
| SorInfo | 6.1.6.2.26 | Steering Of Roaming Information |
| SharedData | 6.1.6.2.27 | Subscription Data shared by multiple UEs |
| PgwInfo | 6.1.6.2.28 | Information about the DNNs/APNs and PGW-C+SMF FQDNs used in interworking with EPS |
| TraceDataResponse | 6.1.6.2.29 | Contains Trace Data or a shared data Id identifying shared Trace Data |
| SteeringContainer | 6.1.6.2.30 |  |
| SdmSubsModification | 6.1.6.2.31 | Modification instruction for a subscription to notifications |
| EmergencyInfo | 6.1.6.2.32 | Information about emergency session |
| UpuInfo | 6.1.6.2.33 | UE Parameters Update Information |
| GroupIdentifiers | 6.1.6.2.34 |  |
| NiddInformation | 6.1.6.2.35 | Non-IP Data Delivery information |
| CagData | 6.1.6.2.36 |  |
| CagInfo | 6.1.6.2.37 |  |
| DataSetName | 6.1.6.3.3 |  |
| PduSessionContinuityInd | 6.1.6.3.7 |  |
| AdditionalSnssaiData | 6.1.6.2.38 | Additional information specific to a slice |
| VnGroupData | 6.1.6.2.39 |  |
| AppDescriptor | 6.1.6.2.40 |  |
| AppPortId | 6.1.6.2.41 | Application Port Id |
| LcsPrivacyData | 6.1.6.2.42 |  |
| Lpi | 6.1.6.2.43 |  |
| UnrelatedClass | 6.1.6.2.44 |  |
| PlmnOperatorClass | 6.1.6.2.45 |  |
| ValidTimePeriod | 6.1.6.2.46 |  |
| LcsMoData | 6.1.6.2.47 |  |
| EcRestrictionDataWb | 6.1.6.2.48 | Enhance Coverage Restriction Data |
| ExpectedUeBehaviourData | 6.1.6.2.49 | Expected UE Behaviour Data |
| SuggestedPacketNumDl | 6.1.6.2.52 | Suggested Number of Downlink Packets |
| SmfRegistrationInfo | 6.1.6.2.53 |  |
| FrameRouteInfo | 6.1.6.2.54 | Frame Route Information |
| SorUpdateInfo | 6.1.6.2.55 |  |
| EnhancedCoverageRestrictionData | 6.1.6.2.56 | Enhanced Coverage Restriction Data |
| EdrxParameters | 6.1.6.2.57 | eDRX Parameters |
| PtwParameters | 6.1.6.2.58 | Paging Time Window Parameters |
| OperationMode | 6.1.6.3.12 | Operation Mode |
| SorUpdateIndicator | 6.1.6.3.13 | SoR Update Indicator |
| ExternalUnrelatedClass | 6.1.6.2.62 |  |
| AfExternal | 6.1.6.2.63 |  |
| LcsClientExternal | 6.1.6.2.64 |  |
| LcsClientGroupExternal | 6.1.6.2.65 |  |
| ServiceTypeUnrelatedClass | 6.1.6.2.66 |  |
| UeId | 6.1.6.2.67 |  |
| DefaultUnrelatedClass | 6.1.6.2.68 |  |
| UeContextInAmfData | 6.1.6.2.70 |  |
| V2xSubscriptionData | 6.1.6.2.71 | V2X Subscription Data |
| LcsBroadcastAssistanceTypesData | 6.1.6.2.72 | LCS Broadcast Assistance Data Types |
| DatasetNames | 6.1.6.2.73 | Data Set Names |
| PlmnRestriction | 6.1.6.2.74 |  |
| DefaultDnnIndicator | 6.1.6.3.2 |  |
| LboRoamingAllowed | 6.1.6.3.2 |  |
| UeUsageType | 6.1.6.3.2 |  |
| MpsPriorityIndicator | 6.1.6.3.2 |  |
| McsPriorityIndicator | 6.1.6.3.2 |  |
| 3GppChargingCharacteristics | 6.1.6.3.2 | 3GPP Charging Characteristics |
| MicoAllowed | 6.1.6.3.2 |  |
| SmsSubscribed | 6.1.6.3.2 |  |
| SharedDataId | 6.1.6.3.2 |  |
| IwkEpsInd | 6.1.6.3.2 | Interworking with EPS Indication |
| SecuredPacket | 6.1.6.3.2 |  |
| UpuRegInd | 6.1.6.3.2 |  |
| ExtGroupId | 6.1.6.3.2 |  |
| NbIoTUePriority | 6.1.6.3.2 |  |
| CodeWord | 6.1.6.3.2 |  |
| AfId | 6.1.6.3.2 |  |
| LcsClientId | 6.1.6.3.2 |  |
| DataSetName | 6.1.6.3.3 |  |
| PduSessionContinuityInd | 6.1.6.3.7 |  |
| LocationPrivacyInd | 6.1.6.3.8 |  |
| PrivacyCheckRelatedAction | 6.1.6.3.9 |  |
| LcsClientClass | 6.1.6.3.10 |  |
| LcsMoServiceClass | 6.1.6.3.11 |  |
| OperationMode | 6.1.6.3.12 |  |
| CodeWordInd | 6.1.6.3.14 |  |
| MdtUserConsent | 6.1.6.3.15 | MDT User Consent |
| SharedDataTreatmentInstruction | 6.1.6.3.16 |  |
| GpsiType | 6.1.6.3.x | Type of GPSI (MSISDN or External-ID) |
| SorTransparentContainer | 6.1.6.3.2 |  |

Table 6.1.6.1-2 specifies data types re-used by the Nudm\_SDM service API from other specifications, including a reference to their respective specifications and when needed, a short description of their use within the Nudm\_SDM service API.

Table 6.1.6.1-2: Nudm\_SDM re-used Data Types

|  |  |  |
| --- | --- | --- |
| Data type | Reference | Comments |
| Dnn | 3GPP TS 29.571 [7] | Data Network Name with Network Identifier only; this type is used as key in a map of:  - DnnConfigurations; see clause 6.1.6.2.8;  - EpsIwkPgws; see clause 6.2.6.2.2;  - ExpectedUeBehaviourData; see clause 6.1.6.2.8; |
| DurationSec | 3GPP TS 29.571 [7] | Time value in seconds |
| ProblemDetails | 3GPP TS 29.571 [7] | Common data type used in response bodies |
| Snssai | 3GPP TS 29.571 [7] | Single NSSAI |
| Uri | 3GPP TS 29.571 [7] | Uniform Resource Identifier |
| Gpsi | 3GPP TS 29.571 [7] | Generic Public Subscription Identifier |
| RatType | 3GPP TS 29.571 [7] | Radio Access Technology Type |
| Area | 3GPP TS 29.571 [7] |  |
| ServiceAreaRestriction | 3GPP TS 29.571 [7] |  |
| CoreNetworkType | 3GPP TS 29.571 [7] |  |
| SupportedFeatures | 3GPP TS 29.571 [7] | see 3GPP TS 29.500 [4] clause 6.6 |
| PlmnId | 3GPP TS 29.571 [7] | PLMN Identity |
| PduSessionType | 3GPP TS 29.571 [7] |  |
| SubscribedDefaultQos | 3GPP TS 29.571 [7] | Subscribed Default QoS |
| Ambr | 3GPP TS 29.571 [7] |  |
| PduSessionId | 3GPP TS 29.571 [7] | PduSessionId is used as key in a map of PduSessions; see clause 6.1.6.2.16. |
| NfInstanceId | 3GPP TS 29.571 [7] |  |
| Supi | 3GPP TS 29.571 [7] |  |
| RfspIndex | 3GPP TS 29.571 [7] |  |
| SscMode | 3GPP TS 29.571 [7] |  |
| Ipv4Addr | 3GPP TS 29.571 [7] |  |
| Ipv6Addr | 3GPP TS 29.571 [7] |  |
| Ipv6Prefix | 3GPP TS 29.571 [7] |  |
| SorMac | 3GPP TS 29.509 [24] |  |
| SteeringInfo | 3GPP TS 29.509 [24] |  |
| AckInd | 3GPP TS 29.509 [24] |  |
| CounterSor | 3GPP TS 29.509 [24] |  |
| UpuMac | 3GPP TS 29.509 [24] |  |
| UpuData | 3GPP TS 29.509 [24] |  |
| UpuAckInd | 3GPP TS 29.509 [24] |  |
| CounterUpu | 3GPP TS 29.509 [24] |  |
| TraceData | 3GPP TS 29.571 [7] | Trace control and configuration parameters |
| NotifyItem | 3GPP TS 29.571 [7] |  |
| UpSecurity | 3GPP TS 29.571 [7] |  |
| ServiceName | 3GPP TS 29.510 [19] |  |
| OdbPacketServices | 3GPP TS 29.571 [7] |  |
| GroupId | 3GPP TS 29.571 [7] | This type is also used as key of a map in attributes:  - vnGroupInfo and sharedVnGroupDataIds; see clause 6.1.6.2.4, 6.1.6.2.8, 6.1.6.2.27; |
| DateTime | 3GPP TS 29.571 [7] |  |
| CagId | 3GPP TS 29.571 [7] |  |
| StnSr | 3GPP TS 29.571 [7] | Session Transfer Number for SRVCC |
| CMsisdn | 3GPP TS 29.571 [7] | Correlation MSISDN |
| OsId | 3GPP TS 29.519 [33] |  |
| Uint16 | 3GPP TS 29.571 [7] |  |
| RgWirelineCharacteristics | 3GPP TS 29.571 [7] |  |
| GeographicArea | 3GPP TS 29.572 [34] |  |
| LcsServiceType | 3GPP TS 29.572 [34] |  |
| ScheduledCommunicationTime | 3GPP TS 29.571 [7] | Scheduled Communication Time |
| LocationArea | 6.5.6.2.10 |  |
| StationaryIndication | 3GPP TS 29.571 [7] | Stationary Indication |
| TrafficProfile | 3GPP TS 29.571 [7] | Traffic Profile |
| ScheduledCommunicationType | 3GPP TS 29.571 [7] | Scheduled Communication Type |
| BatteryIndication | 3GPP TS 29.571 [7] | Battery Indication |
| AcsInfo | 3GPP TS 29.571 [7] | ACS Information |
| IPv4AddrMask | 3GPP TS 29.571 [7] |  |
| NefId | 3GPP TS 29.510 [19] |  |
| PatchResult | 3GPP TS 29.571 [7] |  |
| NrV2xAuth | 3GPP TS 29.571 [7] |  |
| LteV2xAuth | 3GPP TS 29.571 [7] |  |
| BitRate | 3GPP TS 29.571 [7] |  |
| MdtConfiguration | 3GPP TS 29.571 [7] |  |
| Uint64 | 3GPP TS 29.571 [7] |  |
| WirelineArea | 3GPP TS 29.571 [7] |  |
| WirelineServiceAreaRestriction | 3GPP TS 29.571 [7] |  |
| NfGroupId | 3GPP TS 29.571 [7] |  |

\* \* \* Next Change \* \* \* \*

##### 6.1.6.3.X Enumeration: GpsiType

Table 6.1.6.3.X-1: Enumeration GpsiType

|  |  |
| --- | --- |
| Enumeration value | Description |
| "MSISDN" | GPSI type of MSISDN |
| "EXT\_ID" | GPSI type of external identity |

\* \* \* Next Change \* \* \* \*

## A.2 Nudm\_SDM API

openapi: 3.0.0

info:

version: '2.2.0-alpha.2'

title: 'Nudm\_SDM'

description: |

Nudm Subscriber Data Management Service.

© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.503 Unified Data Management Services, version 17.1.0

url: 'http://www.3gpp.org/ftp/Specs/archive/29\_series/29.503/'

*(... text not shown for clarity ...)*

/{ueId}/id-translation-result:

get:

summary: retrieve a UE's SUPI or GPSI

operationId: GetSupiOrGpsi

tags:

- GPSI to SUPI Translation or SUPI to GPSI translation

parameters:

- name: ueId

in: path

description: Identifier of the UE

required: true

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/VarUeId'

- name: supported-features

in: query

description: Supported Features

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

- name: af-id

in: query

description: AF identifier

schema:

type: string

- name: app-port-id

in: query

description: Application port identifier

content:

application/json:

schema:

$ref: '#/components/schemas/AppPortId'

- name: requested-gpsi-type

in: query

description: Requested GPSI Type

schema:

$ref: '#/components/schemas/GpsiType'

- name: If-None-Match

in: header

description: Validator for conditional requests, as described in RFC 7232, 3.2

schema:

type: string

- name: If-Modified-Since

in: header

description: Validator for conditional requests, as described in RFC 7232, 3.3

schema:

type: string

responses:

'200':

description: Expected response to a valid request

content:

application/json:

schema:

$ref: '#/components/schemas/IdTranslationResult'

headers:

Cache-Control:

description: Cache-Control containing max-age, as described in RFC 7234, 5.2

schema:

type: string

ETag:

description: Entity Tag, containing a strong validator, as described in RFC 7232, 2.3

schema:

type: string

Last-Modified:

description: Timestamp for last modification of the resource, as described in RFC 7232, 2.2

schema:

type: string

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

description: Unexpected error

*(... text not shown for clarity ...)*

GpsiType:

description: Type of GPSI (MSISDN or External-ID)

anyOf:

- type: string

enum:

- MSISDN

- EXT\_ID

- type: string

\* \* \* End of Changes \* \* \* \*