**3GPP TSG-CT WG4 Meeting #106-eC4-215xyz**

**E-Meeting, 11th – 15th October 2021 (was C4-215171)**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **29.503** | **CR** | **0729** | **rev** | **1** | **Current version:** | **17.4.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Clarification of the response to modification of sdmSubscription |
|  |  |
| ***Source to WG:*** | Ericsson |
| ***Source to TSG:*** | CT4 |
|  |  |
| ***Work item code:*** | SBIProtoc17 |  | ***Date:*** | 2021-09-20 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | Table is not correct since both patchResult and sdmSubscription are mandatory and NOTE 2 is incorrect since it says that, when PatchReport is supported, UDM shall return either 204 or PatchReport; however PatchReport cannot be used to return "confirmed/accepted" values. |
|  |  |
| ***Summary of change:*** | Clarify in which cases patchResult or sdmSubscription is returned. |
|  |  |
| ***Consequences if not approved:*** | Ambiguos implementations of the modify operation. |
|  |  |
| ***Clauses affected:*** | 6.1.3.4.3.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR does not impact any OpenAPI specification files. |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* First Change \* \* \* \*

###### 6.1.3.4.3.2 PATCH

This method shall support the URI query parameters specified in table 6.1.3.4.3.2-1.

Table 6.1.3.4.3.2-1: URI query parameters supported by the PATCH method on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| supported-features | SupportedFeatures | O | 0..1 | see 3GPP TS 29.500 [4] clause 6.6 |

This method shall support the request data structures specified in table 6.1.3.4.3.2-2 and the response data structures and response codes specified in table 6.1.3.4.3.2-3.

Table 6.1.3.4.3.2-2: Data structures supported by the PATCH Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| SdmSubsModification | M | 1 | The modification Instruction |

Table 6.1.3.4.3.2-3: Data structures supported by the PATCH Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Responsecodes | Description |
| SdmSubscription | C | 0..1 | 200 OK | Upon partial success, if any of the requested modifications have not been accepted, but the server has set different values than those requested by the client, in any of the attributes of the resource, the modified SdmSubscription shall be returned including the accepted values, e.g. UDM shall return the list of monitored resource Uri successfully subscribed and/or the confirmed expiry time. Also, upon partial success, if the NF service consumer does not support the "PatchReport" feature, the UDM shall return an SdmSubscription object in the response.(NOTE 2) |
| PatchResult | C | 0..1 | 200 OK | Upon partial success, if the NF service consumer has included in the supported-feature query parameter the "PatchReport" feature, and in case some of the requested modifications are discarded while the rest of the modification instructions are fully accepted, UDM may return the execution report instead of the whole SdmSubscription. (NOTE 2) |
| n/a |  |  | 204 No Content | Upon success, an empty response body shall be returned indicating that all the modification instructions in the PATCH request have been implemented. |
|  |  |  |  |  |
| ProblemDetails | O | 0..1 | 404 Not Found | The "cause" attribute may be used to indicate one of the following application errors:- USER\_NOT\_FOUND- SUBSCRIPTION\_NOT\_FOUND, see 3GPP TS 29.500 [4] table 5.2.7.2-1. |
| ProblemDetails | O | 0..1 | 403 Forbidden | One or more attributes are not allowed to be modified.The "cause" attribute may be used to indicate one of the following application errors:- MODIFICATION\_NOT\_ALLOWED, see 3GPP TS 29.500 [4] table 5.2.7.2-1. |
| NOTE 1: In addition common data structures as listed in table 5.2.7.1-1 of 3GPP TS 29.500 [4] are supported.NOTE 2: One of SdmSubscription or PatchResult shall be returned. |

\* \* \* End of Changes \* \* \* \*