**3GPP TSG-CT WG4 Meeting #107-bis-eC4-220xyz**

**E-Meeting, 17th – 21st January 2022 (was C4-220216)**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **29.510** | **CR** | **0654** | **rev** | **1** | **Current version:** | **17.4.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Resource-based authorization on the NRF APIs |
|  |  |
| ***Source to WG:*** | Ericsson |
| ***Source to TSG:*** | CT4 |
|  |  |
| ***Work item code:*** | SBIProtoc17 |  | ***Date:*** | 2022-01-10 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | When Oauth2 -based authorization is used on an API, it is possible to indicate in the access token (via the "scope" claim) the specific access to resources and operations that are allowed for a given consumer.This mechanism has been introduced in 3GPP APIs since Rel-16 onwards, and has been added progressively to each API, as soon as relevant use cases are identified for it.For the NRF APIs, it is possible to have, among others, the following scenarios:- A given NRF consumer (e.g. an NF Service Producer) may be authorized to register its NF Profile in NRF (PUT request on the "/nf-instances/{nfInstanceId}" resource of the NFManagement API), but it is not authorized to retrieve the full catalog of registered NF Instances in the NRF (GET request on the "/nf-instances" resource of the NFManagement API).So, it is quite frequent to have authorization scenarios, where more granularity is desirable, than the existing usage of a "single scope per service", which basically means "allowed/not-allowed" for all the resources and operations of the entire API. |
|  |  |
| ***Summary of change:*** | Add scopes per resource/operation on the NFManagement and NFDiscovery APIs. |
|  |  |
| ***Consequences if not approved:*** | Authorization of the NRF APIs based on Oauth2 have a sub-optimal granularity and does not leverage well-established features (resource-based authorization) currently used in many other 3GPP APIs. |
|  |  |
| ***Clauses affected:*** | 6.1.8, 6.2.8, A.2, A.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR introduces backwards-compatible new features with impact on OpenAPI specification files:- TS29510\_Nnrf\_NFManagement.yaml- TS29510\_Nnrf\_NFDiscovery.yaml |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* First Change \* \* \* \*

### 6.1.8 Security

As indicated in 3GPP TS 33.501 [15], the access to the Nnrf\_NFManagement API may be authorized by means of the OAuth2 protocol (see IETF RFC 6749 [16]), using the "Client Credentials" authorization grant, where the NRF plays the role of the authorization server.

If Oauth2 authorization is used on the Nnrf\_NFManagement API, an NF Service Consumer, prior to consuming services offered by the Nnrf\_NFManagement API, shall obtain a "token" from the authorization server, by invoking the Access Token Request service, as described in clause 5.4.2.2.

NOTE: When multiple NRFs are deployed in a network, the NRF used as authorization server is the same NRF where the Nnrf\_NFManagement service is invoked by the NF Service Producer.

The Nnrf\_NFManagement API defines the following scopes for OAuth2 authorization:

Table 6.1.8-1: Oauth2 scopes defined in Nnrf\_NFManagement API

|  |  |
| --- | --- |
| Scope | Description |
| "nnrf-nfm" | Access to the Nnrf\_NFManagement API |
| "nnrf-nfm:nf-instances:read" | Acess to read the nf-instances resource |

\* \* \* Next Change \* \* \* \*

### 6.2.8 Security

As indicated in 3GPP TS 33.501 [15], the access to the Nnrf\_NFDiscovery API may be authorized by means of the OAuth2 protocol (see IETF RFC 6749 [16]), using the "Client Credentials" authorization grant, where the NRF plays the role of the authorization server.

If Oauth2 authorization is used, an NF Service Consumer, prior to consuming services offered by the Nnrf\_NFDiscovery API, shall obtain a "token" from the authorization server, by invoking the Access Token Request service, as described in clause 5.4.2.2.

NOTE: When multiple NRFs are deployed in a network, the NRF used as authorization server is the same NRF where the Nnrf\_NFDiscovery service is invoked by the NF Service Consumer.

The Nnrf\_NFDiscovery API defines the following scopes for OAuth2 authorization:

Table 6.2.8-1: Oauth2 scopes defined in Nnrf\_NFDiscovery API

|  |  |
| --- | --- |
| Scope | Description |
| "nnrf-disc" | Access to the Nnrf\_NFDiscovery API |
| "nnrf-disc:scp-domain:read" | Access to read the scp-domain-routing-info resource |
| "nnrf-disc:scp-domain-subs:write" | Access to create/delete a scp-domain subscription resource |

\* \* \* Next Change \* \* \* \*

## A.2 Nnrf\_NFManagement API

*(... text not shown for clarity ...)*

paths:

 /nf-instances:

 get:

 summary: Retrieves a collection of NF Instances

 operationId: GetNFInstances

 tags:

 - NF Instances (Store)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nnrf-nfm

 - oAuth2ClientCredentials:

 - nnrf-nfm

 - nnrf-nfm:nf-instances:read

 parameters:

 - name: nf-type

 in: query

 description: Type of NF

 required: false

 schema:

 $ref: '#/components/schemas/NFType'

*(... text not shown for clarity ...)*

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '/oauth2/token'

 scopes:

 nnrf-nfm: Access to the Nnrf\_NFManagement API

 nnrf-nfm:nf-instances:read: Acess to read the nf-instances resource

 schemas:

*(... text not shown for clarity ...)*

\* \* \* Next Change \* \* \* \*

## A.3 Nnrf\_NFDiscovery API

*(... text not shown for clarity ...)*

 /scp-domain-routing-info:

 get:

 operationId: SCPDomainRoutingInfoGet

 tags:

 - SCP Domain Routing Information (Document)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nnrf-disc

 - oAuth2ClientCredentials:

 - nnrf-disc

 - nnrf-disc:scp-domain:read

 parameters:

 - name: local

 in: query

 description: Indication of local SCP Domain Routing Information

 required: false

 schema:

 type: boolean

 default: false

*(... text not shown for clarity ...)*

 /scp-domain-routing-info-subs:

 post:

 summary: Create a new subscription

 operationId: ScpDomainRoutingInfoSubscribe

 tags:

 - SCP Domain Routing Information Subscriptions (Collection)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nnrf-disc

 - oAuth2ClientCredentials:

 - nnrf-disc

 - nnrf-disc:scp-domain-subs:write

 parameters:

 - name: Content-Encoding

 in: header

 description: Content-Encoding, described in IETF RFC 7231

 schema:

 type: string

*(... text not shown for clarity ...)*

 /scp-domain-routing-info-subs/{subscriptionID}:

 delete:

 summary: Deletes a subscription

 operationId: ScpDomainRoutingInfoUnsubscribe

 tags:

 - Individual SCP Domain Routing Information Subscription (Document)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nnrf-disc

 - oAuth2ClientCredentials:

 - nnrf-disc

 - nnrf-disc:scp-domain-subs-id:write

 parameters:

 - name: subscriptionID

 in: path

 required: true

 description: Unique ID of the subscription to remove

 schema:

 type: string

*(... text not shown for clarity ...)*

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '/oauth2/token'

 scopes:

 nnrf-disc: Access to the Nnrf\_NFDiscovery API

 nnrf-disc:scp-domain:read: Access to read the scp-domain-routing-info resource

 nnrf-disc:scp-domain-subs:write: Access to create/delete a scp-domain subscription resource

*(... text not shown for clarity ...)*

\* \* \* End of Changes \* \* \* \*