**3GPP TSG-CT WG4 Meeting #96C4-200591**

**E-Meeting, 24th – 28th February 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **29.503** | **CR** | **0328** | **rev** | **1** | **Current version:** | **16.2.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Availability after DDN Failure Event |
|  |  |
| ***Source to WG:*** | Huawei |
| ***Source to TSG:*** | CT4 |
|  |  |
| ***Work item code:*** | 5G\_CIoT |  | ***Date:*** | 2019-12-16 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | Alignment with stage 2, the traffic descriptor should be included when NEF subscribe to UDM for Availability after DDN Failure Event depending on S2-1910636 which was agreed in 3GPP TSG-SA2 Meeting #135. |
|  |  |
| ***Summary of change:*** | Indicates "AVAILABILITY\_AFTER\_DNN\_FAILURE" event type in description of datalinkReportCfg attribute |
|  |  |
| ***Consequences if not approved:*** | Stage 2 solution won't be implemented. |
|  |  |
| ***Clauses affected:*** | 6.4.6.2.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR will introduce no impacts in the OpenAPI specification file. |
|  |  |
| ***This CR's revision history:*** | Rev1:Correct "AVAILABILITY\_AFTER\_DNN\_FAILURE" to "AVAILABILITY\_AFTER\_DDN\_FAILURE" in Table 6.4.6.2.3-1 and Table 6.4.6.2.13-1. |

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*The start of changes\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

##### 6.4.6.2.3 Type: MonitoringConfiguration

Table 6.4.6.2.3-1: Definition of type MonitoringConfiguration

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| eventType | EventType | M | 1 | String; see clause 6.4.6.3.3 |
| immediateFlag | boolean | O | 0..1 | Indicates if an immediate event report in the subscription response indicating current value / status of the event is required or not. If the flag is not present then immediate reporting shall not be done. |
| locationReportingConfiguration | LocationReportingConfiguration | C | 0..1 | shall be present if eventType is "LOCATION\_REPORTING" |
| associationType | AssociationType | O | 0..1 | If the eventType indicates CHANGE\_OF\_SUPI\_PEI\_ASSOCIATION, this parameter may be included to identify whether the IMSI-IMEI or IMSI-IMEISV association shall be detected.If the flag is not present, then a value of IMEISV shall be used |
| datalinkReportCfg | DatalinkReportingConfiguration | C | 0..1 | shall be present if eventType is "DL\_DATA\_DELIVERY\_STATUS""AVAILABILITY\_AFTER\_DDN\_FAILURE".  |

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*Next change\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

##### 6.4.6.2.13 Type: DatalinkReportingConfiguration

Table 6.4.6.2.13-1: Definition of type DatalinkReportingConfiguration

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| dddTrafficDes | DddTrafficDescriptor | C | 0..1 | This IE shall be present for event type "DL\_DATA\_DELIVERY\_STATUS""AVAILABILITY\_AFTER\_DDN\_FAILURE".When present, this IE shall indicate the traffic descriptor of the downlink data. |
| dnn | Dnn | O | 0..1 | When present, this IE shall indicate the DNN of the PDU session serving the data link. |
| slice | Snssai | O | 0..1 | When present, this IE shall indicate the slice information of the PDU session serving the data link. |

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*The end of changes\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*