**3GPP TSG-CT WG4 Meeting #99eC4-204**

**E-Meeting, 18th – 28th August 2020 was C4-204126**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.0* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.503** | **CR** | **0472** | **rev** | **1** | **Current version:** | **16.4.0** |  |
|  | | | | | | | | |
| *For* [*HE**LP*](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Network Slices in AMF registrations | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Nokia, Nokia Shanghai Bell, Samsung | | | | | | | | | |
| ***Source to TSG:*** | CT4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | SBIProtoc16 | | | | |  | ***Date:*** | | | 2020-08-20 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12)* *Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | According to 28.554 (see clause 6.2.2) the UDM should be enabled to count the total number of subscribers registered to a given Network Slice Instance. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Add to AMF registration the list of S-NSSAIs identifying the Network Slices the subscriber is registered to. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Requirement from 28.554 cannot be met. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 6.2.6.1, 6.2.6.2.2, 6.2.6.2.3, 6.2.6.2.7, 6.2.6.2.8, A.3 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR introduces backwards compatible new features, with impacts on the following APIs:  - TS 29.503 Nudm\_UECM  - TS 29.504 Nudr\_DataRepository | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

\* \* \* \* Begin of Change \* \* \* \*

#### 6.2.6.1 General

This clause specifies the application data model supported by the API.

Table 6.2.6.1-1 specifies the data types defined for the Nudm\_UECM service API.

Table 6.2.6.1-1: Nudm\_UECM specific Data Types

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Data type | | Clause defined | | Description | |
| Amf3GppAccessRegistration | | 6.2.6.2.2 | | The complete set of information relevant to the AMF where the UE has registered via 3GPP access. | |
| AmfNon3GppAccessRegistration | | 6.2.6.2.3 | | The complete set of information relevant to the AMF where the UE has registered via non 3GPP access. | |
| SmfRegistration | | 6.2.6.2.4 | | The complete set of information relevant to an SMF serving the UE | |
| SmsfRegistration | | 6.2.6.2.6 | | The complete set of information relevant to the SMSF serving the UE. | |
| DeregistrationData | | 6.2.6.2.5 | | Data sent with the Deregistration Notification | |
| Amf3GppAccessRegistrationModification | | 6.2.6.2.7 | | Contains attributes of Amf3GppAccessRegistration that can be modified using PATCH | |
| AmfNon3GppAccessRegistrationModification | | 6.2.6.2.8 | | Contains attributes of AmfNon3GppAccessRegistration that can be modified using PATCH | |
| PcscfRestorationNotification | | 6.2.6.2.9 | | Information sent to the AMF or SMF when P-CSCF restoration is triggered. | |
| NetworkNodeDiameterAddress | | 6.2.6.2.10 | |  | |
| EpsIwkPgw | | 6.2.6.2.11 | |  | |
| TriggerRequest | | 6.2.6.2.12 | |  | |
| AmfDeregInfo | | 6.2.6.2.13 | |  | |
| EpsInterworkingInfo | | 6.2.6.2.14 | |  | |
| LocationInfo | | 6.2.6.2.15 | | Information used by (H)GMLC to send Location Service Request | |
| RegistrationLocationInfo | | 6.2.6.2.16 | | Serving AMF, optional VGMLC and access type related informations used by (H)GMLC to send Location Request | |
| VgmlcAddress | | 6.2.6.2.17 | | The address(es) of VGMLC | |
| PeiUpdateInfo | | 6.2.6.2.18 | |  | |
| RegistrationDataSets | | 6.2.6.2.19 | |  | |
| IpSmGwRegistration | | 6.2.6.2.20 | |  | |
| PurgeFlag | | 6.2.6.3.2 | | This flag indicates whether or not the NF has deregistered. | |
| E164Number | | 6.2.6.3.2 | |  | |
| DualRegistrationFlag | | 6.2.6.3.2 | | Dual Registration Flag | |
| DeregistrationReason | | 6.2.6.3.3 | |  | |
| ImsVoPs | | 6.2.6.3.4 | |  | |
| RegistrationReason | | 6.2.6.3.5 | |  | |
| RegistrationDataSetName | | 6.2.6.3.6 | |  | |

Table 6.2.6.1-2 specifies data types re-used by the Nudm\_uecm service API from other specifications, including a reference to their respective specifications and when needed, a short description of their use within the Nudm\_uecm service API.

Table 6.2.6.1-2: Nudm\_UECM re-used Data Types

|  |  |  |
| --- | --- | --- |
| Data type | Reference | Comments |
| Dnn | 3GPP TS 29.571 [7] | Data Network Name with Network Identifier only. |
| NfInstanceId | 3GPP TS 29.571 [7] | Network Function Instance Identifier |
| PduSessionId | 3GPP TS 29.571 [7] | PDU Session ID |
| Pei | 3GPP TS 29.571 [7] | Permanent Equipment Identifier |
| ProblemDetails | 3GPP TS 29.571 [7] | Common data type used in response bodies |
| Uri | 3GPP TS 29.571 [7] | Uniform Resource Identifier |
| SupportedFeatures | 3GPP TS 29.571 [7] | see 3GPP TS 29.500 [4] clause 6.6 |
| Supi | 3GPP TS 29.571 [7] | see 3GPP TS 23.501 [2] clause 5.9.2 |
| Guami | 3GPP TS 29.571 [7] | Globally Unique AMF Identifier |
| PlmnId | 3GPP TS 29.571 [7] | PLMN Identity |
| DiameterIdentity | 3GPP TS 29.571 [7] |  |
| AccessType | 3GPP TS 29.571 [7] | Access Type |
| BackupAmfInfo | 3GPP TS 29.571 [7] | Backup AMFs |
| ServiceName | 3GPP TS 29.510 [19] |  |
| PatchResult | 3GPP TS 29.571 [7] |  |
| Gpsi | 3GPP TS 29.571 [7] | Generic Public Subscription Identitfier |
| Ipv4Addr | 3GPP TS 29.571 [7] | IPv4 address |
| Ipv6Addr | 3GPP TS 29.571 [7] | IPv6 address |
| Fqdn | 3GPP TS 29.510 [19] | Fully Qualified Domain Name |
| Snssai | 3GPP TS 29.571 [7] | Single NSSAI |

\* \* \* \* Next of Change \* \* \* \*

##### 6.2.6.2.2 Type: Amf3GppAccessRegistration

Table 6.2.6.2.2-1: Definition of type Amf3GppAccessRegistration

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Attribute name | | | | Data type | | | | P | | | | Cardinality | | | | Description | | | |
| amfInstanceId | | | | NfInstanceId | | | | M | | | | 1 | | | | The identity the AMF uses to register in the NRF. | | | |
| deregCallbackUri | | | | Uri | | | | M | | | | 1 | | | | A URI provided by the AMF to receive (implicitly subscribed) notifications on deregistration.  The deregistration callback URI shall have unique information within AMF set to identify the UE to be deregistered. | | | |
| guami | | | | Guami | | | | M | | | | 1 | | | | This IE shall contain the serving AMF's GUAMI. | | | |
| ratType | | | | RatType | | | | M | | | | 1 | | | | This IE shall indicate the current RAT type of the UE. | | | |
| supportedFeatures | | | | SupportedFeatures | | | | O | | | | 0..1 | | | | See clause 6.2.8  These are the features supported by the AMF. | | | |
| purgeFlag | | | | PurgeFlag | | | | O | | | | 0..1 | | | | This flag indicates whether or not the AMF has deregistered. It shall not be included in the Registration service operation. | | | |
| pei | | | | Pei | | | | O | | | | 0..1 | | | | Permanent Equipment Identifier.  Absence of PEI indicates that the PEI is not available at the AMF. In this case the UDM/UDR shall not delete the PEI value stored from a previous registration. | | | |
| imsVoPs | | | | ImsVoPs | | | | O | | | | 0..1 | | | | Indicates per UE if "IMS Voice over PS Sessions" is homogeneously supported in all TAs in the serving AMF, or homogeneously not supported, or if support is non-homogeneous/unknown. Absence of this attribute shall be interpreted as "non homogenous or unknown" support. | | | |
| amfServiceNameDereg | | | | ServiceName | | | | O | | | | 0..1 | | | | When present, this IE shall contain the name of the AMF service to which the Deregistration Notification is to be sent (see clause 6.5.2.2 of 3GPP TS 29.500 [4]). | | | |
| pcscfRestorationCallbackUri | | | | Uri | | | | O | | | | 0..1 | | | | A URI provided by the AMF to receive (implicitly subscribed) notifications on the need for P-CSCF Restoration. | | | |
| amfServiceNamePcscfRest | | | | ServiceName | | | | O | | | | 0..1 | | | | When present, this IE shall contain the name of the AMF service to which P-CSCF Restoration Notifications are to be sent (see clause 6.5.2.2 of 3GPP TS 29.500 [4]). This IE may be included if pcscfRestorationCallbackUri is present. | | | |
| initialRegistrationInd | | | | boolean | | | | C | | | | 0..1 | | | | This IE shall be included by the AMF and set to true if the UE performs an Initial Registration. If the UE does not perform initial registration it shall be absent or set to false. When present and true, the UDM+HSS is requested to cancel previous registration in SGSN, if any.  Not applicable for Nudr and Nudm\_UECM GET operation.  (NOTE 2) | | | |
| backupAmfInfo | | | | array(BackupAmfInfo) | | | | C | | | | 1..N | | | | This IE shall be included if the NF service consumer is an AMF and the AMF supports the AMF management without UDSF for the first interaction with UDM.  The UDM uses this attribute to do an NRF query in order to invoke later services in a backup AMF, e.g. Namf\_EventExposure. | | | |
| drFlag | | | | DualRegistrationFlag | | | | O | | | | 0..1 | | | | Dual Registration flag. When present and true, this flag indicates that the UDM+HSS is requested not to send S6a-CLR to the registered MME/SGSN (if any). Otherwise, the registered MME (if any) shall be cancelled.  Not applicable for Nudr and Nudm\_UECM GET operation. | | | |
| urrpIndicator | | | | boolean | | | | O | | | | 0..1 | | | | This IE indicates whether "UE\_REACHABILITY\_FOR\_SMS" event for this user has been subscribed or not:  - true: the event has been subscribed  - false, or absence of this attribute: the event for this user is currently not subscribed  (NOTE 1) | | | |
| amfEeSubscriptionId | | | | string | | | | C | | | | 0..1 | | | | Shall be present if urrpIndicator is true and the UDM has subscribed to ReachabilityReport event for "UE Reachability for DL Traffic" at the AMF to receive One-Time UE Activity notification. It contains the subscription Id allocated by the AMF as received by the UDM as part of the HTTP "Location" header of the Namf\_EventExposure\_Subscribe response. The UDM shall make use of the Nudr\_DataRepository Update service operation (see 3GPP TS 29.504 [9]) to store the amfEeSubscription Id in the UDR. | | | |
| epsInterworkingInfo | | | | EpsInterworkingInfo | | | | C | | | | 0..1 | | | | This IE shall be included if the AMF has determined per APN/DNN which PGW-C+SMF is selected for EPS interworking with N26 and the AMF supports EPS interworking of non-3GPP access. For each APN/DNN, only one PGW-C+SMF shall be selected by the AMF for EPS interworking. | | | |
| ueSrvccCapability | | | | boolean | | | | O | | | | 0..1 | | | | This IE indicates whether the UE supports 5G SRVCC:  - true: 5G SRVCC is supported by the UE and AMF;  - false, or absence of this attribute: 5G SRVCC is not supported. | | | |
| registrationTime | | | | DateTime | | | | C | | | | 0..1 | | | | Time of Amf3GppAccessRegistration. Shall be present when used on Nudr. | | | |
| vgmlcAddress | | | | VgmlcAddress | | | | O | | | | 0..1 | | | | Address of the VGMLC | | | |
| contextInfo | | | | ContextInfo | | | | C | | | | 0..1 | | | | This IE if present may contain e.g. the headers received by the UDM along with the 3GppAccessRegistration.  Shall be absent on Nudm and may be present on Nudr | | | |
| singleNssais | | | | array(Snssai) | | | | O | | | | 1..N | | | | List of S-NSSAIs identifying the network slices the subscriber is registered to. | | | |
| NOTE 1: The urrpIndicator attribute shall only be exposed over the Nudr SBI, and it shall not be included by the AMF.  NOTE 2: Regardless of the Dual Registration Flag, the SGSN, if any, is required to be cancelled (see 3GPP TS 23.502 [3] clause 4.11.5.2) | | | | | | | | | | | | | | | | | | | |

\* \* \* \* Next of Change \* \* \* \*

##### 6.2.6.2.3 Type: AmfNon3GppAccessRegistration

Table 6.2.6.2.3-1: Definition of type AmfNon3GppAccessRegistration

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Attribute name | | Data type | | P | | Cardinality | | Description | |
| amfInstanceId | | NfInstanceId | | M | | 1 | | The identity the AMF uses to register in the NRF. | |
| deregCallbackUri | | Uri | | M | | 1 | | A URI provided by the AMF to receive (implicitly subscribed) notifications on deregistration.  The deregistration callback URI shall have unique information within AMF set to identify the UE to be deregistered. | | |
| guami | | Guami | | M | | 1 | | This IE shall contain the serving AMF's GUAMI. | | |
| ratType | | RatType | | M | | 1 | | This IE shall indicate the current RAT type of the UE. | | |
| supportedFeatures | | SupportedFeatures | | O | | 0..1 | | See clause 6.2.8  These are the features supported by the AMF. | |
| purgeFlag | | PurgeFlag | | O | | 0..1 | | This flag indicates whether or not the AMF has deregistered. It shall not be included in the Registration service operation. | |
| pei | | Pei | | O | | 0..1 | | Permanent Equipment Identifier  Absence of PEI indicates that the PEI is not available at the AMF. In this case the UDM/UDR shall not delete the PEI value stored from a previous registration. | |
| imsVoPs | | ImsVoPs | | M | | 1 | | Indicates per UE if "IMS Voice over PS Sessions" is supported, or not supported.  The value NON\_HOMOGENEOUS\_OR\_UNKNOWN is not applicable. | |
| amfServiceNameDereg | | ServiceName | | O | | 0..1 | | When present, this IE shall contain the name of the AMF service to which the Deregistration Notification is to be sent (see clause 6.5.2.2 of 3GPP TS 29.500 [4]). | |
| pcscfRestorationCallbackUri | | Uri | | O | | 0..1 | | A URI provided by the AMF to receive (implicitly subscribed) notifications on the need for P-CSCF Restoration. | |
| amfServiceNamePcscfRest | | ServiceName | | O | | 0..1 | | When present, this IE shall contain the name of the AMF service to which P-CSCF Restoration Notifications are to be sent (see clause 6.5.2.2 of 3GPP TS 29.500 [4]). This IE may be included if pcscfRestorationCallbackUri is present. | |
| backupAmfInfo | | array(BackupAmfInfo) | | C | | 1..N | | This IE shall be included if the NF service consumer is an AMF and the AMF supports the AMF management without UDSF for the first interaction with UDM.  The UDM uses this attribute to do an NRF query in order to invoke later services in a backup AMF, e.g. Namf\_EventExposure. | |
| urrpIndicator | | boolean | | O | | 0..1 | | This IE indicates whether "UE\_REACHABILITY\_FOR\_SMS" event for this user has been subscribed or not:  - true: the event has been subscribed  - false, or absence of this attribute: the event for this user is currently not subscribed | |
| amfEeSubscriptionId | | string | | C | | 0..1 | | Shall be present if urrpIndicator is true and the UDM has subscribed to Reachability-Report event for "UE Reachable for DL Traffic" at the AMFto receive One-Time UE Activity notification. It contains the subscription Id allocated by the AMF as received by the UDM as part of the HTTP "Location" header of the Namf\_EventExposure\_Subscribe response.  The UDM shall make use of the Nudr\_DataRepository Update service operation (see 3GPP TS 29.504 [9]) to store the amfEeSubscription Id in the UDR. | |
| registrationTime | | DateTime | | C | | 0..1 | | Time of AmfNon3GppAccessRegistration. Shall be present when used on Nudr. | |
| vgmlcAddress | | VgmlcAddress | | O | | 0..1 | | Address of the VGMLC | | |
| contextInfo | | ContextInfo | | C | | 0..1 | | This IE if present may contain e.g. the headers received by the UDM along with AmfNon3GppRegistration.  Shall be absent on Nudm and may be present on Nudr. | | |
| singleNssais | | array(Snssai) | | O | | 1..N | | List of S-NSSAIs identifying the network slices the subscriber is registered to. | | |
| NOTE: The urrpIndicator attribute shall only be exposed over the Nudr SBI, and it shall not be included by the AMF. | | | | | | | | | |

\* \* \* \* Next of Change \* \* \* \*

##### 6.2.6.2.7 Type: Amf3GppAccessRegistrationModification

This type is derived from the type Amf3GppAccessRegistration by deleting all attributes that are not subject to modification by means of the HTTP PATCH method.

Table 6.2.6.2.7-1: Definition of type Amf3GppAccessRegistrationModification

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Attribute name | | | Data type | | P | | Cardinality | | Description | |
| guami | | | Guami | | M | | 1 | | Guami of the AMF requesting the modification. If the MCC, MNC, AMF Region ID and AMF Set ID within the guami do not match the stored value, the modification request shall be rejected. | |
| purgeFlag | | | PurgeFlag | | O | | 0..1 | | This flag indicates whether or not the AMF has deregistered. It shall be included in the Deregistration service operation with a value of "TRUE". | |
| pei | | | Pei | | O | | 0..1 | | Permanent Equipment Identifier. | |
| imsVoPs | | | ImsVoPs | | O | | 0..1 | | Indicates per UE if "IMS Voice over PS Sessions" is homogeneously supported in all TAs in the serving AMF, or homogeneously not supported, or if support is non-homogeneous/unknown | |
| backupAmfInfo | | | array(BackupAmfInfo) | | C | | 0..N | | This IE shall be included if the NF service consumer is an AMF and the AMF supports the AMF management without UDSF for the Modification of the BackupAmfInfo.  The UDM uses this attribute to do an NRF query in order to invoke later services in a backup AMF, e.g. Namf\_EventExposure | |
| epsInterworkingInfo | | | EpsInterworkingInfo | | C | | 0..1 | | This IE shall be included if the AMF has determined per APN/DNN which PGW-C+SMF is selected for EPS interworking with N26 and the AMF supports EPS interworking of non-3GPP access. This IE shall also be included to update the PGW-C+SMF information if the AMF selects another PGW-C+SMF for EPS interworking with N26 for the same DNN. For each APN/DNN, only one PGW-C+SMF shall be selected by the AMF for EPS interworking. | |
| ueSrvccCapability | | boolean | | O | | 0..1 | | This IE indicates whether the UE supports 5G SRVCC:  - true: 5G SRVCC is supported by the UE and AMF;  - false: 5G SRVCC is not supported. | | |
| singleNssais | | array(Snssai) | | O | | 1..N | | List of S-NSSAIs identifying the network slices the subscriber is registered to. | | | |
| Note: Absence of optional attributes indicates: no modification. Attributes of this type are not marked "nullable: true" in the OpenAPI file as deletion of these attributes is not applicable. | | | | | | | | | | |

\* \* \* \* Next of Change \* \* \* \*

##### 6.2.6.2.8 Type: AmfNon3GppAccessRegistrationModification

This type is derived from the type AmfNon3GppAccessRegistration by deleting all attributes that are not subject to modification by means of the HTTP PATCH method.

Table 6.2.6.2.8-1: Definition of type AmfNon3GppAccessRegistrationModification

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| guami | Guami | M | 1 | Guami of the AMF requesting the modification. If the MCC, MNC, AMF Region ID and AMF Set ID within the guami do not match the stored value, the modification request shall be rejected. |
| purgeFlag | PurgeFlag | O | 0..1 | This flag indicates whether or not the AMF has deregistered. It shall be included in the Deregistration service operation with a value of "TRUE". |
| pei | Pei | O | 0..1 | Permanent Equipment Identifier |
| imsVoPs | ImsVoPs | O | 0..1 | If present indicates per UE that support of "IMS Voice over PS Sessions" has been modified to supported or not supported".  The value NON\_HOMOGENEOUS\_OR\_UNKNOWN is not applicable. |
| backupAmfInfo | array(BackupAmfInfo) | C | 0..N | This IE shall be included if the NF service consumer is an AMF and the AMF supports the AMF management without UDSF for the Modification of the BackupAmfInfo.  The UDM uses this attribute to do an NRF query in order to invoke later services in a backup AMF, e.g. Namf\_EventExposure |
| singleNssais | array(Snssai) | O | 1..N | List of S-NSSAIs identifying the network slices the subscriber is registered to. |
| Note: Absence of optional attributes indicates: no modification. Attributes of this type are not marked "nullable: true" in the OpenAPI file as deletion of these attributes is not applicable. | | | | |

\* \* \* \* Next of Change \* \* \* \*

## A.3 Nudm\_UECM API

openapi: 3.0.0

\*\*\*\*\*\*\*\*\*text not shown for clarity\*\*\*\*\*\*\*\*\*\*\*

Amf3GppAccessRegistration:

type: object

required:

- amfInstanceId

- deregCallbackUri

- guami

- ratType

properties:

amfInstanceId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

purgeFlag:

$ref: '#/components/schemas/PurgeFlag'

pei:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

imsVoPs:

$ref: '#/components/schemas/ImsVoPs'

deregCallbackUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

amfServiceNameDereg:

$ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/ServiceName'

pcscfRestorationCallbackUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

amfServiceNamePcscfRest:

$ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/ServiceName'

initialRegistrationInd:

type: boolean

guami:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Guami'

backupAmfInfo:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BackupAmfInfo'

minItems: 1

drFlag:

$ref: '#/components/schemas/DualRegistrationFlag'

ratType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

urrpIndicator:

type: boolean

amfEeSubscriptionId:

type: string

epsInterworkingInfo:

$ref: '#/components/schemas/EpsInterworkingInfo'

ueSrvccCapability:

type: boolean

registrationTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

vgmlcAddress:

$ref: '#/components/schemas/VgmlcAddress'

contextInfo:

$ref: 'TS29503\_Nudm\_SDM.yaml#/components/schemas/ContextInfo'

singleNssais:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 1

Amf3GppAccessRegistrationModification:

type: object

required:

- guami

properties:

guami:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Guami'

purgeFlag:

$ref: '#/components/schemas/PurgeFlag'

pei:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

imsVoPs:

$ref: '#/components/schemas/ImsVoPs'

backupAmfInfo:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BackupAmfInfo'

epsInterworkingInfo:

$ref: '#/components/schemas/EpsInterworkingInfo'

ueSrvccCapability:

type: boolean

nullable: true

singleNssais:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 1

\*\*\*\*\*\*\*\*\*text not shown for clarity\*\*\*\*\*\*\*\*\*\*\*

AmfNon3GppAccessRegistration:

type: object

required:

- amfInstanceId

- imsVoPs

- deregCallbackUri

- guami

- ratType

properties:

amfInstanceId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

purgeFlag:

$ref: '#/components/schemas/PurgeFlag'

pei:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

imsVoPs:

$ref: '#/components/schemas/ImsVoPs'

deregCallbackUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

amfServiceNameDereg:

$ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/ServiceName'

pcscfRestorationCallbackUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

amfServiceNamePcscfRest:

$ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/ServiceName'

guami:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Guami'

backupAmfInfo:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BackupAmfInfo'

minItems: 1

ratType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

urrpIndicator:

type: boolean

amfEeSubscriptionId:

type: string

registrationTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

vgmlcAddress:

$ref: '#/components/schemas/VgmlcAddress'

contextInfo:

$ref: 'TS29503\_Nudm\_SDM.yaml#/components/schemas/ContextInfo'

singleNssais:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 1

AmfNon3GppAccessRegistrationModification:

type: object

required:

- guami

properties:

guami:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Guami'

purgeFlag:

$ref: '#/components/schemas/PurgeFlag'

pei:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

imsVoPs:

$ref: '#/components/schemas/ImsVoPs'

backupAmfInfo:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BackupAmfInfo'

singleNssais:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 1

\*\*\*\*\*\*\*\*\*text not shown for clarity\*\*\*\*\*\*\*\*\*\*\*

\* \* \* \* End of Change \* \* \* \*