ETSI TS 102 230-1 V12.0.0 (2017-09)

Smart Cards;

UICC-Terminal interface;

Physical, electrical and logical test specification;

Part 1: Terminal features (Release 12)

**Technical Specification**

Reference

RTS/SCP-00102230Tvb00

Keywords

smart card, testing

***ETSI***

650 Route des Lucioles

F-06921 Sophia Antipolis Cedex - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Siret N° 348 623 562 00017 - NAF 742 C

Association à but non lucratif enregistrée à la

Sous-Préfecture de Grasse (06) N° 7803/88

***Important notice***

The present document can be downloaded from:  
<http://www.etsi.org/standards-search>

The present document may be made available in electronic versions and/or in print. The content of any electronic and/or print versions of the present document shall not be modified without the prior written authorization of ETSI. In case of any existing or perceived difference in contents between such versions and/or in print, the only prevailing document is the print of the Portable Document Format (PDF) version kept on a specific network drive within ETSI Secretariat.

Users of the present document should be aware that the document may be subject to revision or change of status. Information on the current status of this and other ETSI documents is available at <https://portal.etsi.org/TB/ETSIDeliverableStatus.aspx>

If you find errors in the present document, please send your comment to one of the following services:  
<https://portal.etsi.org/People/CommiteeSupportStaff.aspx>

***Copyright Notification***

No part may be reproduced or utilized in any form or by any means, electronic or mechanical, including photocopying and microfilm except as authorized by written permission of ETSI.  
The content of the PDF version shall not be modified without the written authorization of ETSI.  
The copyright and the foregoing restriction extend to reproduction in all media.

© European Telecommunications Standards Institute 2017.

All rights reserved.

**DECT**TM, **PLUGTESTS**TM, **UMTS**TM and the ETSI logo are Trade Marks of ETSI registered for the benefit of its Members.  
**3GPP**TM and **LTE**™ are Trade Marks of ETSI registered for the benefit of its Members and  
of the 3GPP Organizational Partners.  
**GSM**® and the GSM logo are Trade Marks registered and owned by the GSM Association.

Contents

Intellectual Property Rights 12

Foreword 12

Modal verbs terminology 12

Introduction 12

1 Scope 14

2 References 14

2.1 Normative references 14

2.2 Informative references 15

3 Definitions, symbols, abbreviations and coding conventions 15

3.1 Definitions 15

3.2 Symbols 15

3.3 Abbreviations 16

3.4 Coding conventions 17

3.5 Applicability 17

3.5.1 Applicability of the present document 17

3.5.2 Applicability of the individual test cases 17

3.5.3 Applicability to terminal equipment 17

3.6 Definitions 17

3.6.1 Format of table of the table of optional features 17

3.6.2 Format of the applicability table 18

3.6.3 Status and Notations 18

3.7 Table of optional features 19

3.8 Applicability table 20

4 Physical characteristic tests 24

4.1 Contact pressure 24

4.1.1 Definition and applicability 24

4.1.2 Conformance requirement 24

4.1.2.0 Description 24

4.1.2.1 Reference 24

4.1.3 Test purpose 24

4.1.4 Method of test 24

4.1.4.1 Initial conditions 24

4.1.4.2 Procedure 24

4.1.5 Acceptance criteria 24

4.2 Curvature of the contacting elements 24

4.2.1 Definition and applicability 24

4.2.2 Conformance requirement 25

4.2.2.0 Description 25

4.2.2.1 Reference 25

4.2.3 Test purpose 25

4.2.4 Method of test 25

4.2.4.1 Initial conditions 25

4.2.4.2 Procedure 25

4.2.5 Acceptance criteria 25

5 Electrical characteristic tests 25

5.1 Test of the power transition phases 25

5.1.1 Phase preceding Terminal power on 25

5.1.1.1 Definition and applicability 25

5.1.1.2 Conformance requirement 25

5.1.1.3 Reference 25

5.1.1.4 Test purpose 26

5.1.1.5 Method of test 26

5.1.1.5.1 Initial condition 26

5.1.1.5.2 Procedure 26

5.1.1.6 Acceptance criteria 26

5.1.2 Phase during UICC power on 26

5.1.2.1 Phase during UICC power on: 3 V - 5 V 26

5.1.2.1.1 Definition and applicability 26

5.1.2.1.2 Conformance requirement 26

5.1.2.1.3 Reference 26

5.1.2.1.4 Test purpose 27

5.1.2.1.5 Method of test 27

5.1.2.1.6 Acceptance criteria 27

5.1.2.2 Phase during UICC power on: 1,8 V - 3 V 27

5.1.2.2.1 Definition and applicability 27

5.1.2.2.2 Conformance requirement 27

5.1.2.2.3 Reference 27

5.1.2.2.4 Test purpose 27

5.1.2.2.5 Method of test 28

5.1.2.2.6 Acceptance criteria 28

5.1.3 Phase during Terminal power off 28

5.1.3.1 Phase during Terminal power off: 3 V - 5 V 28

5.1.3.1.1 Definition and applicability 28

5.1.3.1.2 Conformance requirement 28

5.1.3.1.3 Reference 28

5.1.3.1.4 Test purpose 29

5.1.3.1.5 Method of test 29

5.1.3.1.6 Acceptance criteria 29

5.1.3.2 Phase during Terminal power off: 1,8 V - 3 V 29

5.1.3.2.1 Definition and applicability 29

5.1.3.2.2 Conformance requirement 29

5.1.3.2.3 Reference 30

5.1.3.2.4 Test purpose 30

5.1.3.2.5 Method of test 30

5.1.3.2.6 Acceptance criteria 30

5.1.4 Warm reset timing 30

5.1.4.1 Definition and applicability 30

5.1.4.2 Conformance requirement 30

5.1.4.2.0 Description 30

5.1.4.2.1 Reference 31

5.1.4.3 Test purpose 31

5.1.4.4 Method of test 31

5.1.4.4.1 Initial conditions 31

5.1.4.4.2 Procedure 31

5.1.4.5 Acceptance criteria 31

5.1.5 UICC type recognition and voltage switching 31

5.1.5.1 Reaction of 3 V technology Terminals on type recognition of 3 V technology UICCs 31

5.1.5.1.1 Definition and applicability 31

5.1.5.1.2 Conformance requirement 31

5.1.5.1.3 Reference 31

5.1.5.1.4 Test purpose 32

5.1.5.1.5 Method of test 32

5.1.5.1.6 Acceptance criteria 32

5.1.5.2 Reaction of 3 V technology Terminals on type recognition of 1,8 V technology UICCs 32

5.1.5.2.1 Definition and applicability 32

5.1.5.2.2 Conformance requirement 32

5.1.5.2.3 Reference 32

5.1.5.2.4 Test purpose 33

5.1.5.2.5 Method of test 33

5.1.5.2.6 Acceptance criteria 33

5.1.5.3 Reaction of 1,8 V technology Terminals on type recognition of 1,8 V technology UICCs 33

5.1.5.3.1 Definition and applicability 33

5.1.5.3.2 Conformance requirement 33

5.1.5.3.3 Reference 33

5.1.5.3.4 Test purpose 33

5.1.5.3.5 Method of test 34

5.1.5.3.6 Acceptance criteria 34

5.1.5.4 Reaction of 1,8 V technology Terminals on type recognition of 3 V technology UICCs 34

5.1.5.4.1 Definition and applicability 34

5.1.5.4.2 Conformance requirement 34

5.1.5.4.3 Reference 34

5.1.5.4.4 Test purpose 34

5.1.5.4.5 Method of test 35

5.1.5.4.6 Acceptance criteria 35

5.1.5.5 Void 35

5.1.5.6 Reaction of Terminals receiving no ATR 35

5.1.5.6.1 Reaction of Terminals receiving no ATR, 3 V - 5 V 35

5.1.5.6.2 Reaction of Terminals receiving no ATR, 1,8 V - 3 V 36

5.2 Electrical tests on each Terminal contact 37

5.2.1 Nominal test conditions 37

5.2.2 Electrical tests on contact C1 (Card power supply - VCC) 37

5.2.2.1 Electrical tests on contact C1, Test 1: 3 V - 5 V 37

5.2.2.1.1 Definition and applicability 37

5.2.2.1.2 Conformance requirement 38

5.2.2.1.3 Reference 38

5.2.2.1.4 Test purpose 38

5.2.2.1.5 Method of test 38

5.2.2.1.6 Acceptance criteria 38

5.2.2.2 Electrical tests on contact C1, Test 2: 3 V - 5 V 38

5.2.2.2.1 Definition and applicability 38

5.2.2.2.2 Conformance requirement 38

5.2.2.2.3 Reference 38

5.2.2.2.4 Test purpose 39

5.2.2.2.5 Method of test 39

5.2.2.2.6 Acceptance criteria 41

5.2.2.3 Electrical tests on contact C1, Test 1: 1,8 V - 3 V 41

5.2.2.3.1 Definition and applicability 41

5.2.2.3.2 Conformance requirement 41

5.2.2.3.3 Reference 41

5.2.2.3.4 Test purpose 41

5.2.2.3.5 Method of test 41

5.2.2.3.6 Acceptance criteria 42

5.2.2.4 Electrical tests on contact C1, Test 2: 1,8 V - 3 V 42

5.2.2.4.1 Definition and applicability 42

5.2.2.4.2 Conformance requirement 42

5.2.2.4.3 Reference 42

5.2.2.4.4 Test purpose 42

5.2.2.4.5 Method of test 42

5.2.2.4.6 Acceptance criteria 43

5.2.3 Electrical tests on contact C2 (Reset - RST) 44

5.2.3.1 Electrical tests on contact C2: 3 V - 5 V 44

5.2.3.1.1 Definition and applicability 44

5.2.3.1.2 Conformance requirement 44

5.2.3.1.3 Reference 44

5.2.3.1.4 Test purpose 44

5.2.3.1.5 Method of test 44

5.2.3.1.6 Acceptance criteria 44

5.2.3.2 Electrical tests on contact C2: 1,8 V - 3 V 44

5.2.3.2.1 Definition and applicability 44

5.2.3.2.2 Conformance requirement 45

5.2.3.2.3 Reference 45

5.2.3.2.4 Test purpose 45

5.2.3.2.5 Method of test 45

5.2.3.2.6 Acceptance criteria 45

5.2.4 Electrical tests on contact C3 (Clock - CLK) 45

5.2.4.1 Electrical tests on contact C3: 3 V - 5 V 45

5.2.4.1.1 Definition and applicability 45

5.2.4.1.2 Conformance requirement 45

5.2.4.1.3 Reference 46

5.2.4.1.4 Test purpose 46

5.2.4.1.5 Method of test 46

5.2.4.1.6 Acceptance criteria 46

5.2.4.2 Electrical tests on contact C3: 1,8 V - 3 V 46

5.2.4.2.1 Definition and applicability 46

5.2.4.2.2 Conformance requirement 47

5.2.4.2.3 Reference 47

5.2.4.2.4 Test purpose 47

5.2.4.2.5 Method of test 47

5.2.4.2.6 Acceptance criteria 47

5.2.5 Electrical tests on contact C7 (Input/Output - I/O) 48

5.2.5.1 Electrical tests on contact C7, Test 1: 3 V - 5 V 48

5.2.5.1.1 Definition and applicability 48

5.2.5.1.2 Conformance requirement 48

5.2.5.1.3 Reference 48

5.2.5.1.4 Test purpose 48

5.2.5.1.5 Method of test 49

5.2.5.1.6 Acceptance criteria 49

5.2.5.2 Electrical tests on contact C7, Test 2: 3 V - 5 V 49

5.2.5.2.1 Definition and applicability 49

5.2.5.2.2 Conformance requirement 49

5.2.5.2.3 Reference 50

5.2.5.2.4 Test purpose 50

5.2.5.2.5 Method of test 50

5.2.5.2.6 Acceptance criteria 50

5.2.5.3 Electrical tests on contact C7, Test 1: 1,8 V - 3 V 50

5.2.5.3.1 Definition and applicability 50

5.2.5.3.2 Conformance requirement 50

5.2.5.3.3 Reference 51

5.2.5.3.4 Test purpose 51

5.2.5.3.5 Method of test 51

5.2.5.3.6 Acceptance criteria 51

5.2.5.4 Electrical tests on contact C7, Test 2: 1,8 V - 3 V 51

5.2.5.4.1 Definition and applicability 51

5.2.5.4.2 Conformance requirement 52

5.2.5.4.3 Reference 52

5.2.5.4.4 Test purpose 52

5.2.5.4.5 Method of test 52

5.2.5.4.6 Acceptance criteria 53

6 Initial communication tests 53

6.1 ATR 53

6.1.1 ATR characters 53

6.1.1.1 Definition and applicability 53

6.1.1.2 Conformance requirement 53

6.1.1.2.0 Description 53

6.1.1.2.1 Reference 53

6.1.1.3 Test purpose 53

6.1.1.4 Method of test 53

6.1.1.4.1 Initial conditions 53

6.1.1.4.2 Procedure 54

6.1.1.5 Acceptance criteria 56

6.2 Clock stop mode with 1,8 V technology UICC 57

6.2.1 Definition and applicability 57

6.2.2 Conformance requirement 57

6.2.2.0 Description 57

6.2.2.1 Reference 57

6.2.3 Test purpose 57

6.2.4 Method of test 57

6.2.4.1 Initial conditions 57

6.2.4.2 Procedure 57

6.2.5 Acceptance criteria 59

6.3 Clock stop mode with 3 V technology UICC 60

6.3.1 Definition and applicability 60

6.3.2 Conformance requirement 60

6.3.2.0 Description 60

6.3.2.1 Reference 60

6.3.3 Test purpose 60

6.3.4 Method of test 60

6.3.4.1 Initial conditions 60

6.3.4.2 Procedure 60

6.3.5 Acceptance criteria 62

6.4 Void 62

6.5 Speed enhancement 62

6.5.1 Definition and applicability 62

6.5.2 Conformance requirement 63

6.5.3 Test purpose 63

6.5.4 Method of test 63

6.5.4.1 Initial conditions 63

6.5.4.2 Procedure 63

6.5.5 Acceptance criteria 64

7 Transmission protocol tests 64

7.1 Character transmission 64

7.1.1 Bit/character duration during the transmission from the Terminal to the UICC 64

7.1.1.1 Definition and applicability 64

7.1.1.2 Conformance requirement 64

7.1.1.2.0 Description 64

7.1.1.2.1 Reference 64

7.1.1.3 Test purpose 65

7.1.1.4 Method of test 65

7.1.1.4.1 Initial conditions 65

7.1.1.4.2 Procedure 65

7.1.1.5 Acceptance criteria 65

7.1.2 Bit/character duration during the transmission from the UICC to the Terminal 65

7.1.2.1 Definition and applicability 65

7.1.2.2 Conformance requirement 65

7.1.2.2.0 Description 65

7.1.2.2.1 Reference 65

7.1.2.3 Test purpose 65

7.1.2.4 Method of test 65

7.1.2.4.1 Initial conditions 65

7.1.2.4.2 Procedure 66

7.1.2.5 Acceptance criteria 66

7.2 T=0 protocol 66

7.2.1 Timing 66

7.2.1.1 Definition and applicability 66

7.2.1.2 Conformance requirement 66

7.2.1.2.0 Description 66

7.2.1.2.1 Reference 66

7.2.1.3 Test purpose 66

7.2.1.4 Method of test 66

7.2.1.4.1 Initial conditions 66

7.2.1.4.2 Procedure 67

7.2.1.5 Acceptance criteria 67

7.2.2 Command processing, ACK, NACK, NULL procedure bytes 68

7.2.2.1 Definition and applicability 68

7.2.2.2 Conformance requirement 68

7.2.2.2.0 Description 68

7.2.2.2.1 Reference 68

7.2.2.3 Test purpose 68

7.2.2.4 Method of test 68

7.2.2.4.1 Initial conditions 68

7.2.2.4.2 Procedure 68

7.2.2.5 Acceptance criteria 69

7.2.3 Case 2 command, use of procedure bytes '61xx' and '6Cxx' 69

7.2.3.1 Definition and applicability 69

7.2.3.2 Conformance requirement 69

7.2.3.2.0 Description 69

7.2.3.2.1 Reference 69

7.2.3.3 Test purpose 69

7.2.3.4 Method of test 69

7.2.3.4.1 Initial conditions 69

7.2.3.4.2 Procedure 69

7.2.3.5 Acceptance criteria 69

7.2.4 Case 4 command, use of procedure bytes '61xx' 70

7.2.4.1 Definition and applicability 70

7.2.4.2 Conformance requirement 70

7.2.4.2.0 Description 70

7.2.4.2.1 Reference 70

7.2.4.3 Test purpose 70

7.2.4.4 Method of test 70

7.2.4.4.1 Initial conditions 70

7.2.4.4.2 Procedure 70

7.2.4.5 Acceptance criteria 70

7.2.5 Command processing, warning and error status bytes 71

7.2.5.1 Definition and applicability 71

7.2.5.2 Conformance requirement 71

7.2.5.2.0 Description 71

7.2.5.2.1 Reference 71

7.2.5.3 Test purpose 71

7.2.5.4 Method of test 71

7.2.5.4.1 Initial conditions 71

7.2.5.4.2 Procedure 71

7.2.5.5 Acceptance criteria 71

7.2.6 Error correction 71

7.2.6.1 Definition and applicability 71

7.2.6.2 Conformance requirement 72

7.2.6.2.0 Description 72

7.2.6.2.1 Reference 72

7.2.6.3 Test purpose 72

7.2.6.4 Method of test 72

7.2.6.4.1 Initial conditions 72

7.2.6.4.2 Procedure 72

7.2.6.5 Acceptance criteria 72

7.2.7 Error detection 72

7.2.7.1 Definition and applicability 72

7.2.7.2 Conformance requirement 72

7.2.7.2.0 Description 72

7.2.7.2.1 Reference 72

7.2.7.3 Test purpose 72

7.2.7.4 Method of test 73

7.2.7.4.1 Initial conditions 73

7.2.7.4.2 Procedure 73

7.2.7.5 Acceptance criteria 73

7.3 T=1 protocol 73

7.3.1 Character Waiting Time 73

7.3.1.1 Definition and applicability 73

7.3.1.2 Conformance requirement 73

7.3.1.2.0 Description 73

7.3.1.2.1 Reference 73

7.3.1.3 Test purpose 73

7.3.1.4 Method of test 73

7.3.1.4.1 Initial conditions 73

7.3.1.4.2 Procedure 74

7.3.1.5 Acceptance criteria 74

7.3.2 Block Timing 74

7.3.2.1 Definition and applicability 74

7.3.2.2 Conformance requirement 75

7.3.2.2.0 Description 75

7.3.2.2.1 Reference 75

7.3.2.3 Test purpose 75

7.3.2.4 Method of test 75

7.3.2.4.1 Initial conditions 75

7.3.2.4.2 Procedure 75

7.3.2.5 Acceptance criteria 76

7.3.3 Block Waiting Time extension 76

7.3.3.1 Definition and applicability 76

7.3.3.2 Conformance requirement 76

7.3.3.2.0 Description 76

7.3.3.2.1 Reference 76

7.3.3.3 Test purpose 76

7.3.3.4 Method of test 77

7.3.3.4.1 Initial conditions 77

7.3.3.4.2 Procedure 77

7.3.3.5 Acceptance criteria 78

7.3.4 Chaining - Respect of IFSC by Terminal 78

7.3.4.1 Definition and applicability 78

7.3.4.2 Conformance requirement 78

7.3.4.2.0 Description 78

7.3.4.2.1 Reference 78

7.3.4.3 Test purpose 78

7.3.4.4 Method of test 78

7.3.4.4.1 Initial conditions 78

7.3.4.4.2 Procedure 79

7.3.4.5 Acceptance criteria 80

7.3.5 Chaining - IFSD management 80

7.3.5.1 Definition and applicability 80

7.3.5.2 Conformance requirement 80

7.3.5.2.0 Description 80

7.3.5.2.1 Reference 80

7.3.5.3 Test purpose 80

7.3.5.4 Method of test 80

7.3.5.4.1 Initial conditions 80

7.3.5.4.2 Procedure 81

7.3.5.5 Acceptance criteria 81

7.3.6 I-Block error correction 81

7.3.6.1 Definition and applicability 81

7.3.6.2 Conformance requirement 81

7.3.6.2.0 Description 81

7.3.6.2.1 Reference 81

7.3.6.3 Test purpose 81

7.3.6.4 Method of test 81

7.3.6.4.1 Initial conditions 81

7.3.6.4.2 Procedure 82

7.3.6.5 Acceptance criteria 82

7.3.7 I-Block error detection 82

7.3.7.1 Definition and applicability 82

7.3.7.2 Conformance requirement 82

7.3.7.2.0 Description 82

7.3.7.2.1 Reference 82

7.3.7.3 Test purpose 82

7.3.7.4 Method of test 82

7.3.7.4.1 Initial conditions 82

7.3.7.4.2 Procedure 82

7.3.7.5 Acceptance criteria 83

7.3.8 R-Block error handling in non-chaining mode 83

7.3.8.1 Definition and applicability 83

7.3.8.2 Conformance requirement 83

7.3.8.2.0 Description 83

7.3.8.2.1 Reference 83

7.3.8.3 Test purpose 83

7.3.8.4 Method of test 83

7.3.8.4.1 Initial conditions 83

7.3.8.4.2 Procedure 84

7.3.8.5 Acceptance criteria 84

7.3.9 R-Block error handling in chaining mode 84

7.3.9.1 Definition and applicability 84

7.3.9.2 Conformance requirement 84

7.3.9.2.0 Description 84

7.3.9.2.1 Reference 84

7.3.9.3 Test purpose 84

7.3.9.4 Method of test 85

7.3.9.4.1 Initial conditions 85

7.3.9.4.2 Procedure 85

7.3.9.5 Acceptance criteria 85

7.3.10 Successive errors in both directions 85

7.3.10.1 Definition and applicability 85

7.3.10.2 Conformance requirement 85

7.3.10.2.0 Description 85

7.3.10.2.1 Reference 85

7.3.10.3 Test purpose 86

7.3.10.4 Method of test 86

7.3.10.4.1 Initial conditions 86

7.3.10.4.2 Procedure 86

7.3.10.5 Acceptance criteria 86

7.3.11 Chaining - Abortion 86

7.3.11.1 Definition and applicability 86

7.3.11.2 Conformance requirement 87

7.3.11.2.0 Description 87

7.3.11.2.1 Reference 87

7.3.11.3 Test purpose 87

7.3.11.4 Method of test 87

7.3.11.4.1 Initial conditions 87

7.3.11.4.2 Procedure 87

7.3.11.5 Acceptance criteria 87

7.3.12 Block repetition and resynchronization 88

7.3.12.1 Definition and applicability 88

7.3.12.2 Conformance requirement 88

7.3.12.2.0 Description 88

7.3.12.2.1 Reference 88

7.3.12.3 Test purpose 88

7.3.12.4 Method of test 88

7.3.12.4.1 Initial conditions 88

7.3.12.4.2 Procedure 88

7.3.12.5 Acceptance criteria 89

7.3.13 UICC is unresponsive 89

7.3.13.1 Definition and applicability 89

7.3.13.2 Conformance requirement 89

7.3.13.2.0 Description 89

7.3.13.2.1 Reference 90

7.3.13.3 Test purpose 90

7.3.13.4 Method of test 90

7.3.13.4.1 Initial conditions 90

7.3.13.4.2 Procedure 90

7.3.13.5 Acceptance criteria 90

8 Application dependent procedures 91

8.1 UICC presence detection 91

8.1.1 Definition and applicability 91

8.1.2 Conformance requirement 91

8.1.2.0 Description 91

8.1.2.1 Reference 91

8.1.3 Test purpose 91

8.1.4 Method of test 91

8.1.4.1 Initial conditions 91

8.1.4.2 Procedure 91

8.1.5 Acceptance criteria 92

9 Commands 92

9.1 TERMINAL CAPABILITY 92

9.1.1 Additional interfaces support 92

9.1.1.1 Definition and applicability 92

9.1.1.2 Conformance requirement 92

9.1.1.2.1 Description 92

9.1.1.2.2 Reference 92

9.1.1.3 Test purpose 92

9.1.1.4 Method of test 92

9.1.1.4.1 Initial conditions 92

9.1.1.4.2 Procedure 92

9.1.1.5 Acceptance criteria 93

Annex A (normative): UICC simulator functional requirement 94

A.1 General 94

A.2 Contacts C1, C3, C7 94

A.2.1 Default measurement/setting uncertainties 94

A.2.2 Contact C1 94

A.2.3 Contact C7 95

A.2.4 Contact C3 95

A.3 Definition of timing 95

Annex B (informative): Change history 96

History 97

# Intellectual Property Rights

IPRs essential or potentially essential to the present document may have been declared to ETSI. The information pertaining to these essential IPRs, if any, is publicly available for **ETSI members and non-members**, and can be found in ETSI SR 000 314: *"Intellectual Property Rights (IPRs); Essential, or potentially Essential, IPRs notified to ETSI in respect of ETSI standards"*, which is available from the ETSI Secretariat. Latest updates are available on the ETSI Web server (<https://ipr.etsi.org/>).

Pursuant to the ETSI IPR Policy, no investigation, including IPR searches, has been carried out by ETSI. No guarantee can be given as to the existence of other IPRs not referenced in ETSI SR 000 314 (or the updates on the ETSI Web server) which are, or may be, or may become, essential to the present document.

# Foreword

This Technical Specification (TS) has been produced by ETSI Technical Committee Smart Card Platform (SCP).

The contents of the present document are subject to continuing work within TC SCP and may change following formal TC SCP approval. If TC SCP modifies the contents of the present document, it will then be republished by ETSI with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TC SCP for information;

2 presented to TC SCP for approval;

3 or greater indicates TC SCP approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

The present document is part 2 of a multi-part deliverable covering the Test specification for the Terminal/Integrated Circuit Card (ICC) interface, as identified below:

**Part 1: "Terminal features";**

Part 2: "UICC features".

# Modal verbs terminology

In the present document "**shall**", "**shall not**", "**should**", "**should not**", "**may**", "**need not**", "**will**", "**will not**", "**can**" and "**cannot**" are to be interpreted as described in clause 3.2 of the [ETSI Drafting Rules](https://portal.etsi.org/Services/editHelp!/Howtostart/ETSIDraftingRules.aspx) (Verbal forms for the expression of provisions).

"**must**" and "**must not**" are **NOT** allowed in ETSI deliverables except when used in direct citation.

# Introduction

The present document defines the interface tests for the Terminal/UICC interface.

The aim of the present document is to ensure interoperability between an UICC and a Terminal independently of the respective manufacturer, card issuer or operator.

Application specific tests for applications residing on an UICC are specified in ETSI TS 131 121 [4].

# 1 Scope

The present document specifies the interface test for the Terminal/UICC.

The present document specifies the tests of:

* physical characteristics of the UICC;
* the electrical interface between the UICC and the Terminal;
* the initial communication establishment and the transport protocols;
* the application independent procedures.

# 2 References

## 2.1 Normative references

References are either specific (identified by date of publication and/or edition number or version number) or non‑specific. For specific references, only the cited version applies. For non-specific references, the latest version of the referenced document (including any amendments) applies.

* In the case of a reference to a TC SCP document, a non specific reference implicitly refers to the latest version of that document in the same Release as the present document.

Referenced documents which are not found to be publicly available in the expected location might be found at <http://docbox.etsi.org/Reference>.

NOTE: While any hyperlinks included in this clause were valid at the time of publication, ETSI cannot guarantee their long term validity.

The following referenced documents are necessary for the application of the present document.

[1] ETSI TS 102 221: "Smart Cards; UICC-Terminal interface; Physical and logical characteristics".

[2] ISO/IEC 7816-3: "Identification cards Integrated circuit cards - Part 3: Cards with contacts - Electrical interface and transmission protocols".

[3] ETSI TS 121 111: "Universal Mobile Telecommunications System (UMTS); LTE; USIM and IC card requirements (3GPP TS 21.111)".

[4] ETSI TS 131 121: "Universal Mobile Telecommunications System (UMTS); LTE; UICC-terminal interface; Universal Subscriber Identity Module (USIM) application test specification (3GPP TS 31.121)".

[5] ISO/IEC 9646-7: "Information technology - Open Systems Interconnection - Conformance testing methodology and framework - Part 7: Implementation Conformance Statements".

[6] ETSI TS 102 613: "Smart Cards; UICC - Contactless Front-end (CLF) Interface; Part 1: Physical and data link layer characteristics".

## 2.2 Informative references

References are either specific (identified by date of publication and/or edition number or version number) or non‑specific. For specific references, only the cited version applies. For non-specific references, the latest version of the referenced document (including any amendments) applies.

* In the case of a reference to a TC SCP document, a non specific reference implicitly refers to the latest version of that document in the same Release as the present document.

NOTE: While any hyperlinks included in this clause were valid at the time of publication, ETSI cannot guarantee their long term validity.

The following referenced documents are not necessary for the application of the present document but they assist the user with regard to a particular subject area.

Not applicable.

# 3 Definitions, symbols, abbreviations and coding conventions

## 3.1 Definitions

For the purposes of the present document, the following terms and definitions apply:

**3 V technology Smart Card:** Smart Card operating at 3 V ± 10 % and 5 V ± 10 %

**1,8 V technology Smart Card:** Smart Card operating at 1,8 V ± 10 % and 3 V ± 10 %

**3 V technology Terminal:** Terminal operating the Smart Card - Terminal interface at 3 V ± 10 % and 5 V ± 10 %

**1,8 V technology Terminal:** Terminal operating the Smart Card - Terminal interface at 1,8 V ± 10 % and 3 V ± 10 %

**access conditions:** set of security attributes associated with a file

**data object:** information coded as TLV objects, i.e. consisting of a Tag, a Length and a Value part

**Dedicated File (DF):** file containing access conditions and, optionally, Elementary Files (EFs) or other Dedicated Files (DFs)

**directory:** general term for MF, DF and ADF

**Elementary File (EF):** file containing access conditions and data and no other files

**file:** directory or an organized set of bytes or records in the UICC

**file identifier:** 2 bytes which address a file in the UICC

**Master File (MF):** unique mandatory file containing access conditions and optionally DFs and/or EFs

**plug-in UICC:** second format of UICC

**SWP interface**: the UICC-CLF interface according to ETSI TS 102 613 [6]

## 3.2 Symbols

For the purposes of the present document, the following symbols apply:

f frequency

Fi Clock rate conversion factor

I Current

Icc Current at VCC

Lc Length of Command data sent by the application layer in a case 3 or 4 Command

Le Maximum length of data Expected by the application layer in response to a case 2 or 4 Command

Luicc Exact Length of data available in the UICC to be returned in response to the case 2 or 4 Command received by the UICC

tF fall time

tR rise time

Vcc Voltage at VCC

## 3.3 Abbreviations

For the purposes of the present document, the following abbreviations apply:

ACK ACKnowledge

ADF Application Dedicated File

AID Application IDentifier

ATR Answer To Reset

BGT Block Guard Time

BWI Block Waiting Integer

BWT Block Waiting Time

CLF ContactLess Frontend

CLK CLocK

CWI Character Waiting Integer

CWT Character Waiting Time

DF Dedicated File

EDC Error Detection Code byte

EF Elementary File

etu elementary time unit

FCP File Control Parameters

GND GrouND

GSM Global System for Mobile communications

I/O Input/Output

I-Block Information-Block

ID IDentifier

IEC International Electrotechnical Commission

IFSC Information Field Size for the UICC

IFSD Information Field Size for the Terminal

INS INStruction

ISO International Organization for Standardization

LEN LENgth

LSB Least Significant Bit

MF Master File

MSB Most Significant Bit

N/A Not Applicable

NAD Node ADdress byte

PCB Protocol Control Byte

PIN Personal Identification Number

PPS Protocol and Parameter Selection

R-Block Receive-ready Block

RFU Reserved for Future Use

RST Reset

S-Block Supervisory-Block

SFI Short (elementary) File Identifier

SWP Single Wire Protocol

TBD To Be Defined

TE Terminal Equipment

TLV Tag Length Value

UE User Equipment

USIM Universal Subscriber Identity Module

VCC Power supply input

WI Waiting time Integer

WTX Waiting Time eXtension

WWT Work Waiting Time

## 3.4 Coding conventions

For the purposes of the present document, the following coding conventions apply.

All lengths are presented in bytes, unless otherwise stated. Each byte is represented by bits b8 to b1, where b8 is the Most Significant Bit (MSB) and b1 is the Least Significant Bit (LSB). In each representation, the leftmost bit is the MSB.

In the UICC, all bytes specified as RFU is to be set to '00' and all bits specified as RFU are to be set to 0. If the GSM and/or USIM application exists on a UICC or is built on a generic telecommunications card, then other values may apply for the non- GSM or non-USIM applications. The values will be defined in the appropriate specifications for such cards and applications. These bytes and bits are not to be interpreted by a Terminal in a GSM or 3G session.

The coding of all data objects in the present document is according to ETSI TS 102 221 [1]. All data objects are BER-TLV except if otherwise defined.

## 3.5 Applicability

### 3.5.1 Applicability of the present document

This present test specification applies to terminal equipment that supports UICC according to ETSI TS 102 221 [1].

### 3.5.2 Applicability of the individual test cases

Table A.1 lists the optional features for which the supplier of the implementation states the support.

### 3.5.3 Applicability to terminal equipment

The applicability to terminal equipment specified in table B.1 of the present document applies, unless otherwise specified.

## 3.6 Definitions

### 3.6.1 Format of table of the table of optional features

The columns in table A.1 have the following meaning:

|  |  |
| --- | --- |
| **Column** | **Meaning** |
| Option: | The optional feature supported or not by the implementation. |
| Status: | See chapter 3.6.2 'Status and Notations' |
| Support: | The support columns are to be filled in by the supplier of the implementation. The following common notations, defined in ISO/IEC 9646‑7 [], are used for the support column in table A.1.  Y or y supported by the implementation  N or n not supported by the implementation  N/A, n/a or - no answer required (allowed only if the status is N/A, directly or after evaluation of a conditional status) |
| Mnemonic: | The mnemonic column contains mnemonic identifiers for each item. |

### 3.6.2 Format of the applicability table

The applicability of every test in table B.1 is formally expressed by the use of Boolean expression defined in the following clause.

The columns in table B.1 have the following meaning:

|  |  |
| --- | --- |
| **Column** | **Meaning** |
| Test case: | The "Test case" column gives a reference to the test case number(s) detailed in the present document and required to validate the implementation of the corresponding item in the "Description" column |
| Description: | In the "Description" column a short non-exhaustive description of the requirement is found. |
| Release: | The "Release" column gives the Release applicable and onwards, for the item in the "Description" column |
| Rel x TE: | For a given Release, the corresponding "Rel X Terminal" column lists the tests required for a Terminal to be declared compliant to this Release. |
| Support: | The "Support" column is blank in the proforma, and is to be completed by the manufacturer in respect of each particular requirement to indicate the choices, which have been made in the implementation. |

### 3.6.3 Status and Notations

The "Release X Terminal" columns show the status of the entries as follows:

The following notations, defined in ISO/IEC 9646‑7 [5], are used for the status column:

M mandatory - the capability is required to be supported.

O optional - the capability may be supported or not.

N/A not applicable - in the given context, it is impossible to use the capability.

X prohibited (excluded) - there is a requirement not to use this capability in the given context.

O.i qualified optional - for mutually exclusive or selectable options from a set. "i" is an integer which identifies an unique group of related optional items and the logic of their selection which is defined immediately following the table.

Ci conditional - the requirement on the capability ("M", "O", "X" or "N/A") depends on the support of other optional or conditional items. "i" is an integer identifying an unique conditional status expression which is defined immediately following the table. For nested conditional expressions, the syntax "IF ... THEN (IF ... THEN ... ELSE...) ELSE ..." is to be used to avoid ambiguities.

References to items

For each possible item answer (answer in the support column) there exists a unique reference, used, for example, in the conditional expressions. It is defined as the table identifier, followed by a solidus character "/", followed by the item number in the table. If there is more than one support column in a table, the columns are to be discriminated by letters (a, b, etc.), respectively.

EXAMPLE: A.1/4 is the reference to the answer of item 4 in table A.1.

## 3.7 Table of optional features

Table A.1: Options

| Item | Option | Status | Support | Mnemonic |
| --- | --- | --- | --- | --- |
| 1 | Void | O |  | Void |
| 2 | Void | O |  | Void |
| 3 | Class A | O |  | O\_CLASS\_A |
| 4 | Class B | O |  | O\_CLASS\_B |
| 5 | Class C | O |  | O\_CLASS\_C |
| 6 | Compliant to ETSI TS 121 111 [3] | O |  | O\_COMP\_121\_111 |
| 7 | Low impedance buffer | O |  | O\_LIB |
| 8 | SWP interface | O |  | O\_SWP |

## 3.8 Applicability table

Table B.1a: Applicability of tests (Rel-99 to Rel-9)

| Test case | Description | Release | R99  TE | Rel-4 TE | Rel-5 TE | Rel-6  TE | Rel-7  TE | Rel-8  TE | Rel-9  TE | Support |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 4.1 | Contact pressure | R99 | M | M | M | M | M | M | M |  |
| 4.2 | Curvature of the contacting elements | R99 | M | M | M | M | M | M | M |  |
| 5.1.1 | Phase preceding Terminal power on | R99 | M | M | M | M | M | M | M |  |
| 5.1.2.1 | Phase during UICC power on: 3 V - 5 V | R99 | C001 | C001 | C001 | C001 | C001 | C001 | C001 |  |
| 5.1.2.2 | Phase during UICC power on: 1,8 V - 3 V | R99 | C002 | C002 | C002 | C002 | C002 | C002 | C002 |  |
| 5.1.3.1 | Phase during Terminal power off: 3 V - 5 V | R99 | C001 | C001 | C001 | C001 | C001 | C001 | C001 |  |
| 5.1.3.2 | Phase during Terminal power off: 1,8 V - 3 V | R99 | C002 | C002 | C002 | C002 | C002 | C002 | C002 |  |
| 5.1.4 | Warm reset timing | R99 | M | M | M | M | M | M | M |  |
| 5.1.5.1 | Reaction of 3 V technology Terminals on type recognition of 3 V technology UICCs | R99 | C001 | C001 | C001 | C001 | C001 | C001 | C001 |  |
| 5.1.5.2 | Reaction of 3 V technology Terminals on type recognition of 1,8 V technology UICCs | R99 | C001 | C001 | C001 | C001 | C001 | C001 | C001 |  |
| 5.1.5.3 | Reaction of 1,8 V technology Terminals on type recognition of 1,8 V technology UICCs | R99 | C002 | C002 | C002 | C002 | C002 | C002 | C002 |  |
| 5.1.5.4 | Reaction of 1,8 V technology Terminals on type recognition of 3 V technology UICCs | R99 | C002 | C002 | C002 | C002 | C002 | C002 | C002 |  |
| 5.1.5.6.1 | Reaction of Terminals receiving no ATR, 3 V - 5 V | R99 | C001 | C001 | C001 | C001 | C001 | C001 | C001 |  |
| 5.1.5.6.2 | Reaction of Terminals receiving no ATR, 1,8 V - 3 V | R99 | C002 | C002 | C002 | C002 | C002 | C002 | C002 |  |
| 5.2.2.1 | Electrical tests on contact C1, Test 1: 3 V - 5 V | R99 | C001 | C001 | C001 | C001 | C001 | C001 | C001 |  |
| 5.2.2.2 | Electrical tests on contact C1, Test 2: 3 V - 5 V | R99 | C001 | C001 | C001 | C001 | C001 | C001 | C001 |  |
| 5.2.2.3 | Electrical tests on contact C1, Test 1: 1,8 V - 3 V | R99 | C002 | C002 | C002 | C002 | C002 | C002 | C002 |  |
| 5.2.2.4 | Electrical tests on contact C1, Test 2: 1,8 V - 3 V | R99 | C002 | C002 | C002 | C002 | C002 | C002 | C002 |  |
| 5.2.3.1 | Electrical tests on contact C2: 3 V - 5 V | R99 | C001 | C001 | C001 | C001 | C001 | C001 | C001 |  |
| 5.2.3.2 | Electrical tests on contact C2: 1,8 V - 3 V | R99 | C002 | C002 | C002 | C002 | C002 | C002 | C002 |  |
| 5.2.4.1 | Electrical tests on contact C3: 3 V - 5 V | R99 | C001 | C001 | C001 | C001 | C001 | C001 | C001 |  |
| 5.2.4.2 | Electrical tests on contact C3: 1,8 V - 3 V | R99 | C002 | C002 | C002 | C002 | C002 | C002 | C002 |  |
| 5.2.5.1 | Electrical tests on contact C7, Test 1: 3 V - 5 V | R99 | C001 | C001 | C001 | C001 | C001 | C001 | C001 |  |
| 5.2.5.2 | Electrical tests on contact C7, Test 2: 3 V - 5 V | Rel-6 | N/A | N/A | N/A | C001 AND C007 | C001 AND C007 | C001 AND C007 | C001 AND C007 |  |
| 5.2.5.3 | Electrical tests on contact C7, Test 1: 1,8 V - 3 V | Rel-99 | C002 | C002 | C002 | C002 | C002 | C002 | C002 |  |
| 5.2.5.4 | Electrical tests on contact C7, Test 2: 1,8 V - 3 V | Rel-6 | N/A | N/A | N/A | C002 AND C007 | C002 AND C007 | C002 AND C007 | C002 AND C007 |  |
| 6.1 | ATR characters | R99 | M | M | M | M | M | M | M |  |
| 6.2 | Clock stop mode with 1,8 V technology UICC | R99 | C003 | C003 | C003 | C003 | C003 | C003 | C003 |  |
| 6.3 | Clock stop mode with 3 V technology UICC | R99 | C004 | C004 | C004 | C004 | C004 | C004 | C004 |  |
| 6.5 | Speed enhancement | R99 | M | M | M | M | M | M | M |  |
| 7.1.1 | Bit/character duration during the transmission from the Terminal to the UICC | R99 | M | M | M | M | M | M | M |  |
| 7.1.2 | Bit/character duration during the transmission from the UICC to the Terminal | R99 | M | M | M | M | M | M | M |  |
| 7.2.1 | Timing | R99 | M | M | M | M | M | M | M |  |
| 7.2.2 | Command processing, ACK, NACK, NULL procedure bytes | R99 | M | M | M | M | M | M | M |  |
| 7.2.3 | Case 2 command, use of procedure bytes '61xx' and '6Cxx' | R99 | M | M | M | M | M | M | M |  |
| 7.2.4 | Case 4 command, use of procedure bytes '61xx' | R99 | M | M | M | M | M | M | M |  |
| 7.2.5 | Command processing, warning and error status bytes | R99 | M | M | M | M | M | M | M |  |
| 7.2.6 | Error correction | R99 | M | M | M | M | M | M | M |  |
| 7.2.7 | Error detection | R99 | M | M | M | M | M | M | M |  |
| 7.3.1 | Character Waiting Time | R99 | M | M | M | M | M | M | M |  |
| 7.3.2 | Block Timing | R99 | M | M | M | M | M | M | M |  |
| 7.3.3 | Block Waiting Time extension | R99 | M | M | M | M | M | M | M |  |
| 7.3.4 | Chaining - Respect of IFSC by Terminal | R99 | M | M | M | M | M | M | M |  |
| 7.3.5 | Chaining - IFSD management | R99 | M | M | M | M | M | M | M |  |
| 7.3.6 | I-Block error correction | R99 | M | M | M | M | M | M | M |  |
| 7.3.7 | I-Block error detection | R99 | M | M | M | M | M | M | M |  |
| 7.3.8 | R-Block error handling in non‑chaining mode | R99 | M | M | M | M | M | M | M |  |
| 7.3.9 | R-Block error handling in chaining mode | R99 | M | M | M | M | M | M | M |  |
| 7.3.10 | Successive errors in both directions | R99 | M | M | M | M | M | M | M |  |
| 7.3.11 | Chaining - Abortion | R99 | M | M | M | M | M | M | M |  |
| 7.3.12 | Block repetition and resynchronization | R99 | M | M | M | M | M | M | M |  |
| 7.3.13 | UICC is unresponsive | R99 | M | M | M | M | M | M | M |  |
| 8.1 | UICC presence detection | R99 | M | M | N/A | N/A | N/A | N/A | N/A |  |
| 9.1.1 | TERMINAL CAPABILITY – Additional interfaces support | Rel-7 | N/A | N/A | N/A | N/A | N/A | N/A | C008 |  |

Table B.1b: Applicability of tests (from release 10)

| Test case | Description | Release | Rel-10  TE | Rel-11  TE | **Rel-12**  TE | Support |
| --- | --- | --- | --- | --- | --- | --- |
| 4.1 | Contact pressure | R99 | M | M | M |  |
| 4.2 | Curvature of the contacting elements | R99 | M | M | M |  |
| 5.1.1 | Phase preceding Terminal power on | R99 | M | M | M |  |
| 5.1.2.1 | Phase during UICC power on: 3 V - 5 V | R99 | C001 | C001 | C001 |  |
| 5.1.2.2 | Phase during UICC power on: 1,8 V - 3 V | R99 | C002 | C002 | C002 |  |
| 5.1.3.1 | Phase during Terminal power off: 3 V - 5 V | R99 | C001 | C001 | C001 |  |
| 5.1.3.2 | Phase during Terminal power off: 1,8 V - 3 V | R99 | C002 | C002 | C002 |  |
| 5.1.4 | Warm reset timing | R99 | M | M | M |  |
| 5.1.5.1 | Reaction of 3 V technology Terminals on type recognition of 3 V technology UICCs | R99 | C001 | C001 | C001 |  |
| 5.1.5.2 | Reaction of 3 V technology Terminals on type recognition of 1,8 V technology UICCs | R99 | C001 | C001 | C001 |  |
| 5.1.5.3 | Reaction of 1,8 V technology Terminals on type recognition of 1,8 V technology UICCs | R99 | C002 | C002 | C002 |  |
| 5.1.5.4 | Reaction of 1,8 V technology Terminals on type recognition of 3 V technology UICCs | R99 | C002 | C002 | C002 |  |
| 5.1.5.6.1 | Reaction of Terminals receiving no ATR, 3 V - 5 V | R99 | C001 | C001 | C001 |  |
| 5.1.5.6.2 | Reaction of Terminals receiving no ATR, 1,8 V - 3 V | R99 | C002 | C002 | C002 |  |
| 5.2.2.1 | Electrical tests on contact C1, Test 1: 3 V - 5 V | R99 | C001 | C001 | C001 |  |
| 5.2.2.2 | Electrical tests on contact C1, Test 2: 3 V - 5 V | R99 | C001 | C001 | C001 |  |
| 5.2.2.3 | Electrical tests on contact C1, Test 1: 1,8 V - 3 V | R99 | C002 | C002 | C002 |  |
| 5.2.2.4 | Electrical tests on contact C1, Test 2: 1,8 V - 3 V | R99 | C002 | C002 | C002 |  |
| 5.2.3.1 | Electrical tests on contact C2: 3 V - 5 V | R99 | C001 | C001 | C001 |  |
| 5.2.3.2 | Electrical tests on contact C2: 1,8 V - 3 V | R99 | C002 | C002 | C002 |  |
| 5.2.4.1 | Electrical tests on contact C3: 3 V - 5 V | R99 | C001 | C001 | C001 |  |
| 5.2.4.2 | Electrical tests on contact C3: 1,8 V - 3 V | R99 | C002 | C002 | C002 |  |
| 5.2.5.1 | Electrical tests on contact C7, Test 1: 3 V - 5 V | R99 | C001 | C001 | C001 |  |
| 5.2.5.2 | Electrical tests on contact C7, Test 2: 3 V - 5 V | Rel-6 | C001 AND C007 | C001 AND C007 | C001 AND C007 |  |
| 5.2.5.3 | Electrical tests on contact C7, Test 1: 1,8 V - 3 V | Rel-99 | C002 | C002 | C002 |  |
| 5.2.5.4 | Electrical tests on contact C7, Test 2: 1,8 V - 3 V | Rel-6 | C002 AND C007 | C002 AND C007 | C002 AND C007 |  |
| 6.1 | ATR characters | R99 | M | M | M |  |
| 6.2 | Clock stop mode with 1,8 V technology UICC | R99 | C003 | C003 | C003 |  |
| 6.3 | Clock stop mode with 3 V technology UICC | R99 | C004 | C004 | C004 |  |
| 6.5 | Speed enhancement | R99 | M | M | M |  |
| 7.1.1 | Bit/character duration during the transmission from the Terminal to the UICC | R99 | M | M | M |  |
| 7.1.2 | Bit/character duration during the transmission from the UICC to the Terminal | R99 | M | M | M |  |
| 7.2.1 | Timing | R99 | M | M | M |  |
| 7.2.2 | Command processing, ACK, NACK, NULL procedure bytes | R99 | M | M | M |  |
| 7.2.3 | Case 2 command, use of procedure bytes '61xx' and '6Cxx' | R99 | M | M | M |  |
| 7.2.4 | Case 4 command, use of procedure bytes '61xx' | R99 | M | M | M |  |
| 7.2.5 | Command processing, warning and error status bytes | R99 | M | M | M |  |
| 7.2.6 | Error correction | R99 | M | M | M |  |
| 7.2.7 | Error detection | R99 | M | M | M |  |
| 7.3.1 | Character Waiting Time | R99 | M | M | M |  |
| 7.3.2 | Block Timing | R99 | M | M | M |  |
| 7.3.3 | Block Waiting Time extension | R99 | M | M | M |  |
| 7.3.4 | Chaining - Respect of IFSC by Terminal | R99 | M | M | M |  |
| 7.3.5 | Chaining - IFSD management | R99 | M | M | M |  |
| 7.3.6 | I-Block error correction | R99 | M | M | M |  |
| 7.3.7 | I-Block error detection | R99 | M | M | M |  |
| 7.3.8 | R-Block error handling in non‑chaining mode | R99 | M | M | M |  |
| 7.3.9 | R-Block error handling in chaining mode | R99 | M | M | M |  |
| 7.3.10 | Successive errors in both directions | R99 | M | M | M |  |
| 7.3.11 | Chaining - Abortion | R99 | M | M | M |  |
| 7.3.12 | Block repetition and resynchronization | R99 | M | M | M |  |
| 7.3.13 | UICC is unresponsive | R99 | M | M | M |  |
| 8.1 | UICC presence detection | R99 | N/A | N/A | N/A |  |
| 9.1.1 | TERMINAL CAPABILITY – Additional interfaces support | Rel-7 | C008 | C008 | C008 |  |

Table B.1c: Applicability of tests (conditions and options list)

|  |  |
| --- | --- |
| C001 | IF (O\_CLASS\_A AND O\_CLASS\_B AND NOT O\_COMP\_121\_111) THEN M ELSE N/A. |
| C002 | IF (O\_CLASS\_B AND O\_CLASS\_C) THEN M ELSE N/A. |
| C003 | IF O\_CLASS\_C THEN M ELSE N/A. |
| C004 | IF O\_CLASS\_B THEN M ELSE N/A. |
| C005 | void |
| C006 | void |
| C007 | IF O\_LIB THEN M ELSE N/A. |
| C008 | IF\_O\_SWP THEN M ELSE N/A. |

# 4 Physical characteristic tests

## 4.1 Contact pressure

### 4.1.1 Definition and applicability

The contact pressure shall be large enough to ensure reliable and continuous contact (e.g. to overcome oxidization and to prevent interruption caused by vibration).

For applicability of this test case see clause 3.8.

### 4.1.2 Conformance requirement

#### 4.1.2.0 Description

Under no circumstances shall the contact force exceed 0,5 N per contact.

#### 4.1.2.1 Reference

ETSI TS 102 221 [1], clause 4.5.4.

### 4.1.3 Test purpose

To verify that the contact pressure of each contacting element is not greater than 0,5 N when each of the following types of card is used:

1) Unembossed.

2) Embossed on the contact side.

NOTE: Only type 1) applies to the plug-in UICC.

### 4.1.4 Method of test

#### 4.1.4.1 Initial conditions

The Terminal manufacturers shall provide, if possible, a separate card reader (mechanical components) to allow measurements.

#### 4.1.4.2 Procedure

The pressure of each contacting element is measured.

### 4.1.5 Acceptance criteria

The contact force shall not exceed 0,5 N per contact.

## 4.2 Curvature of the contacting elements

### 4.2.1 Definition and applicability

The contact pressure shall be large enough to ensure reliable and continuous contact (e.g. to overcome oxidization and to prevent interruption caused by vibration).

For applicability of this test case see clause 3.8.

### 4.2.2 Conformance requirement

#### 4.2.2.0 Description

The radius of any curvature of the contacting elements shall be greater than or equal to 0,8 mm over the contact area.

#### 4.2.2.1 Reference

ETSI TS 102 221 [1], clause 4.5.4.

### 4.2.3 Test purpose

To verify that the radius of curvature of the contacting elements is greater than or equal to 0,8 mm over the contact area.

### 4.2.4 Method of test

#### 4.2.4.1 Initial conditions

The Terminal manufacturers shall provide, if possible, a separate card reader (mechanical components) to allow measurements.

#### 4.2.4.2 Procedure

The radius of curvature of the contacting elements is measured on both axes.

### 4.2.5 Acceptance criteria

The radius of any curvature of the contacting elements shall be greater than or equal to 0,8 mm over the contact area.

# 5 Electrical characteristic tests

## 5.1 Test of the power transition phases

### 5.1.1 Phase preceding Terminal power on

#### 5.1.1.1 Definition and applicability

When the mobile equipment is switched off, the contacts of the UICC-Terminal interface remain in an inactive state in order to prevent any damage to the UICC.

For applicability of this test case see clause 3.8.

#### 5.1.1.2 Conformance requirement

The residual voltage across the contacts of the UICC-Terminal interface (C1, C2, C3, C7) shall not exceed ±0,4 V referenced to GND.

#### 5.1.1.3 Reference

ETSI TS 102 221 [1], clause 4.4.3.

#### 5.1.1.4 Test purpose

To verify that the residual voltage across the contacts of the UICC-Terminal interface (C1, C2, C3, C7) is not greater than ±0,4 V referenced to GND.

#### 5.1.1.5 Method of test

##### 5.1.1.5.1 Initial condition

The Terminal shall be connected to an UICC simulator.

The contact C1 (VCC) of the UICC-Terminal interface shall be loaded with an impedance of 10 kΩ.

The other contacts (C2, C3, C7) shall be loaded with an impedance of 50 kΩ.

##### 5.1.1.5.2 Procedure

The residual voltage on each contact shall be measured.

#### 5.1.1.6 Acceptance criteria

The residual voltage on each contact shall not exceed ±0,4 V referenced to GND.

### 5.1.2 Phase during UICC power on

#### 5.1.2.1 Phase during UICC power on: 3 V - 5 V

##### 5.1.2.1.1 Definition and applicability

When the user equipment is switched on or when the UICC-Terminal interface is being activated after supply voltage switching, the contacts shall be activated in a defined sequence in order to prevent any damage to the UICC.

A 3 V technology Terminal may switch from 3 V to 5 V after it has analysed the ATR and identified the UICC voltage class by deactivating the UICC and activating it at the new supply voltage.

For applicability of this test case see clause 3.8.

##### 5.1.2.1.2 Conformance requirement

1) When the UE is soft powered on, the contacts of the UICC-Terminal interface shall be activated to 3 V mode in the following order:

1 - VCC at state H and stable;

2 - CLK stable;

3 - RST at state L for at least 400 clock cycles after the clock signal is applied to CLK;

4 - I/O at state Z within 200 clock cycles after the clock signal is applied to CLK.

2) When the UICC - Terminal interface is being activated after the 3 V/5 V switching the contacts shall be activated to 5 V mode in the order given in 1).

##### 5.1.2.1.3 Reference

ETSI TS 102 221 [1], clause 4.4.2.

##### 5.1.2.1.4 Test purpose

To verify that the contacts of the UICC-Terminal interface are activated in the correct order, as described in the conformance requirement.

##### 5.1.2.1.5 Method of test

5.1.2.1.5.1 Initial condition

The Terminal shall be connected to an UICC-Terminal simulator.

5.1.2.1.5.2 Procedure

To test the requirements 1), the UE shall be soft powered on.

To test the requirement 2), the Terminal shall be caused to switch the voltage on the UICC-Terminal interface.

The verification of the activation procedure shall be started with the first contact leaving the inactive state. The UICC‑Terminal interface shall be monitored until it is fully activated.

##### 5.1.2.1.6 Acceptance criteria

The contacts of the UICC-Terminal interface shall be activated in the correct order, as described in the conformance requirement.

#### 5.1.2.2 Phase during UICC power on: 1,8 V - 3 V

##### 5.1.2.2.1 Definition and applicability

When the user equipment is switched on or when the UICC-Terminal interface is being activated after supply voltage switching, the contacts shall be activated in a defined sequence in order to prevent any damage to the UICC.

A 1,8 V technology Terminal may switch from 1,8 V to 3 V after it has analysed the ATR and identified the UICC voltage class by deactivating the UICC and activating it at the new supply voltage.

For applicability of this test case see clause 3.8.

##### 5.1.2.2.2 Conformance requirement

1) When the UE is soft powered on, the contacts of the UICC-Terminal interface shall be activated to 1,8 V mode in the following order:

1 - VCC at state H and stable;

2 - CLK stable;

3 - RST at state L for at least 400 clock cycles after the clock signal is applied to CLK;

4 - I/O at state Z within 200 clock cycles after the clock signal is applied to CLK.

2) When the UICC - Terminal interface is being activated after the 1,8 V/3 V switching the contacts shall be activated to 3 V mode in the order given in 1).

##### 5.1.2.2.3 Reference

ETSI TS 102 221 [1], clause 4.4.2.

##### 5.1.2.2.4 Test purpose

To verify that the contacts of the UICC-Terminal interface are activated in the correct order, as described in the conformance requirement.

##### 5.1.2.2.5 Method of test

5.1.2.2.5.1 Initial condition

The Terminal shall be connected to an UICC-Terminal simulator.

5.1.2.2.5.2 Procedure

To test the requirement 1), the UE shall be soft powered on.

To test the requirement 2), the Terminal shall be caused to switch the voltage on the UICC-Terminal interface.

The verification of the activation procedure shall be started with the first contact leaving the inactive state. The UICC‑Terminal interface shall be monitored until it is fully activated.

##### 5.1.2.2.6 Acceptance criteria

The contacts of the UICC-Terminal interface shall be activated in the correct order, as described in the conformance requirement.

### 5.1.3 Phase during Terminal power off

#### 5.1.3.1 Phase during Terminal power off: 3 V - 5 V

##### 5.1.3.1.1 Definition and applicability

When the user equipment is soft powered off or when the UICC-Terminal interface is being deactivated for 3 V/5 V switching, the contacts shall be deactivated in a defined sequence in order to prevent any damage to the UICC.

NOTE: If during UE operation the UICC is physically removed it is impractical to ensure correct sequencing of deactivation and the possible damage to the UICC cannot be safeguarded by a type approval test. Furthermore, in this situation the integrity of the UICC data is not guaranteed.

For applicability of this test case see clause 3.8.

##### 5.1.3.1.2 Conformance requirement

1) Depending on the state of the clock at the time of deactivation, the contacts of the UICC-Terminal shall be deactivated in one of two ways.

If the clock is running, the contacts of the UICC-Terminal interface shall be deactivated in the following order:

1 - RST at low level;

2 - Clock stopped at low level;

3 - I/O at status A;

4 - VCC inactive.

If the clock is stopped and is not restarted, the Terminal is allowed to deactivate all the contacts in any order, provided that all signals reach low level before Vcc leaves high level.

2) When the UICC - Terminal interface is deactivated for 3 V/5 V switching, the contacts shall be deactivated as given in 1).

##### 5.1.3.1.3 Reference

ETSI TS 102 221 [1], clause 4.4.2.

##### 5.1.3.1.4 Test purpose

To verify that, depending on the state of the clock (running or stopped), the contacts of the UICC-Terminal interface become deactivated in the correct order, as given in the conformance requirement.

##### 5.1.3.1.5 Method of test

5.1.3.1.5.1 Initial condition

The Terminal shall be connected to an UICC simulator.

The UICC characteristics of the directories (see ETSI TS 102 221 [1], clause 11.1.1.4.6.1) shall indicate that clock stop is allowed.

5.1.3.1.5.2 Procedure

To test the requirements 1), the UE shall be soft powered off.

To test the requirement 2), the Terminal shall be caused to switch the voltage on the UICC-Terminal interface.

The UICC-Terminal interface shall be monitored until it is fully deactivated.

##### 5.1.3.1.6 Acceptance criteria

The contacts of the UICC-Terminal interface shall be deactivated in the correct order, as given in the conformance requirements.

#### 5.1.3.2 Phase during Terminal power off: 1,8 V - 3 V

##### 5.1.3.2.1 Definition and applicability

When the user equipment is soft powered off or when the UICC-Terminal interface is being deactivated for 1,8 V/3 V switching, the contacts shall be deactivated in a defined sequence in order to prevent any damage to the UICC.

NOTE: If during UE operation the UICC is physically removed it is impractical to ensure correct sequencing of deactivation and the possible damage to the UICC cannot be safeguarded by a type approval test. Furthermore, in this situation the integrity of the UICC data is not guaranteed.

For applicability of this test case see clause 3.8.

##### 5.1.3.2.2 Conformance requirement

1) Depending on the state of the clock at the time of deactivation, the contacts of the UICC-Terminal shall be deactivated in one of two ways.

If the clock is running, the contacts of the UICC-Terminal interface shall be deactivated in the following order:

1 - RST at low level;

2 - Clock stopped at low level;

3 - I/O at status A;

4 - VCC inactive.

If the clock is stopped and is not restarted, the Terminal is allowed to deactivate all the contacts in any order, provided that all signals reach low level before Vcc leaves high level.

2) When the UICC-Terminal interface is deactivated for 1,8 V/3 V switching, the contacts shall be deactivated as given in 1).

##### 5.1.3.2.3 Reference

ETSI TS 102 221 [1], clause 4.4.2.

##### 5.1.3.2.4 Test purpose

To verify that, depending on the state of the clock (running or stopped), the contacts of the UICC-Terminal interface become deactivated in the correct order, as given in the conformance requirement.

##### 5.1.3.2.5 Method of test

5.1.3.2.5.1 Initial condition

The Terminal shall be connected to an UICC simulator.

The UICC characteristics of the directories (see ETSI TS 102 221 [1], clause 11.1.1.4.6.1) shall indicate that clock stop is allowed.

5.1.3.2.5.2 Procedure

To test the requirement 1), the UE shall be soft powered off.

To test the requirement 2), the Terminal shall be caused to switch the voltage on the UICC-Terminal interface.

The UICC-Terminal interface shall be monitored until it is fully deactivated.

##### 5.1.3.2.6 Acceptance criteria

The contacts of the UICC-Terminal interface shall be deactivated in the correct order, as given in the conformance requirements.

### 5.1.4 Warm reset timing

#### 5.1.4.1 Definition and applicability

The warm reset is performed according to clause 5.3.3 of ISO/IEC 7816‑3 [2] and the UICC shall enter either the negotiable or the specific mode.

For applicability of this test case see clause 3.8.

#### 5.1.4.2 Conformance requirement

##### 5.1.4.2.0 Description

1) VCC at state H and stable.

2) CLK stable.

3) RST at state H.

4) RST at state L for 400 clock cycles.

5) RST at state H for at least 400 clock cycles.

6) RST at state H for 40 000 clock cycles before deactivation if no answer is received.

##### 5.1.4.2.1 Reference

ETSI TS 102 221 [1], clause 6.6.

ISO/IEC 7816‑3 [2], clause 5.3.3.

#### 5.1.4.3 Test purpose

To verify that the contacts of the UICC-Terminal interface are activated in the correct order, as described in the conformance requirement.

#### 5.1.4.4 Method of test

##### 5.1.4.4.1 Initial conditions

The Terminal shall be connected to the UICC simulator.

##### 5.1.4.4.2 Procedure

a) The Terminal shall be made to initiate a warm reset (TBD).

b) The UICC simulator shall send a valid ATR:

b-1) 400 clock cycles after RST is set to state H.

b-2) 39 990 clock cycles after RST is set to state H. The contacts of the UICC-Terminal interface shall be monitored during the warm reset sequence.

#### 5.1.4.5 Acceptance criteria

The Terminal shall perform a warm reset as described in the conformance requirement.

In steps b-1) and b-2) the Terminal shall read the answer to the warm reset and work with the UICC.

### 5.1.5 UICC type recognition and voltage switching

#### 5.1.5.1 Reaction of 3 V technology Terminals on type recognition of 3 V technology UICCs

##### 5.1.5.1.1 Definition and applicability

When a 3 V technology Terminal detects a 3 V technology UICC during the ATR analysis the Terminal may either switch to 5 V operation or stay in 3 V operation.

For applicability of this test case see clause 3.8.

##### 5.1.5.1.2 Conformance requirement

1) A 3 V technology Terminal shall initially activate the UICC with 3 V (i.e. the first activation of a card session).

2) The Terminal shall analyse the ATR and identify the voltage class supported by the UICC.

3) If a 3 V technology Terminal identifies a 3 V technology UICC the Terminal may switch to 5 V operation. Switching from 3 V to 5 V shall only be performed by deactivating the UICC and activating it with 5 V supply voltage immediately after the analysis of the ATR without issuing any commands.

##### 5.1.5.1.3 Reference

ETSI TS 102 221 [1], clause 6.2.

##### 5.1.5.1.4 Test purpose

1) To verify that a 3 V technology Terminal initially activates the UICC with 3 V.

2) To verify that a 3 V technology Terminal correctly identifies the voltage class.

3) To verify that a 3 V technology Terminal deactivates the UICC-Terminal interface immediately after the analysis of the ATR without issuing any command and activates it with 5 V supply voltage or proceeds with the 3 V operation during the whole card session without switching to 5 V supply voltage.

##### 5.1.5.1.5 Method of test

5.1.5.1.5.1 Initial condition

The Terminal shall be connected to an UICC simulator simulating a 3 V technology UICC with nominal test conditions (see clause 5.2.1). All elementary files shall be coded as default.

The Terminal shall be powered on.

5.1.5.1.5.2 Procedure

The UICC simulator shall send an ATR indicating a 3 V technology UICC.

The UICC-Terminal interface shall be monitored for at least 1 minute until the UE is switched off.

##### 5.1.5.1.6 Acceptance criteria

1) The initial activation of the UICC-Terminal interface shall be performed with 3 V supply voltage.

2) The Terminal shall react in one of the following ways:

a) The Terminal deactivates the UICC-Terminal interface immediately after the receipt of the ATR from the UICC and activates it with 5 V supply voltage.

b) The Terminal proceeds with the card session without switching to another supply voltage.

#### 5.1.5.2 Reaction of 3 V technology Terminals on type recognition of 1,8 V technology UICCs

##### 5.1.5.2.1 Definition and applicability

When a 3 V technology Terminal detects a 1,8 V technology UICC during the ATR analysis the Terminal shall stay in 3 V operation.

For applicability of this test case see clause 3.8.

##### 5.1.5.2.2 Conformance requirement

1) A 3 V technology Terminal shall initially activate the UICC with 3 V (i.e. the first activation of a card session).

2) The Terminal shall analyse the ATR and identify the voltage class supported by the UICC.

3) If a 3 V technology Terminal identifies a 1,8 V technology UICC during the ATR analysis the Terminal shall stay in 3 V operation.

##### 5.1.5.2.3 Reference

ETSI TS 102 221 [1], clause 6.2.

##### 5.1.5.2.4 Test purpose

1) To verify that a 3 V technology Terminal initially activates the UICC with 3 V.

2) To verify that a 3 V technology Terminal correctly identifies the voltage class.

3) To verify that a 3 V technology Terminal stays in 3 V operation during the whole card session.

##### 5.1.5.2.5 Method of test

5.1.5.2.5.1 Initial condition

The Terminal shall be connected to an UICC simulator simulating a 1,8 V technology UICC with nominal test conditions (see clause 5.2.1). All elementary files shall be coded as default.

The Terminal shall be powered on.

5.1.5.2.5.2 Procedure

The UICC simulator shall send an ATR indicating a 1,8 V technology UICC.

The UICC-Terminal interface shall be monitored for at least 1 minute until the UE is switched off.

##### 5.1.5.2.6 Acceptance criteria

1) The initial activation of the UICC-Terminal interface shall be performed with 3 V supply voltage.

2) The Terminal shall react in the following way:

* The Terminal proceeds with the card session without switching to another supply voltage.

#### 5.1.5.3 Reaction of 1,8 V technology Terminals on type recognition of 1,8 V technology UICCs

##### 5.1.5.3.1 Definition and applicability

When a 1,8 V technology Terminal detects a 1,8 V technology UICC during the ATR analysis the Terminal may either switch to 3 V operation or stay in 1,8 V operation.

For applicability of this test case see clause 3.8.

##### 5.1.5.3.2 Conformance requirement

1) A 1,8 V technology Terminal shall initially activate the UICC with 1,8 V (i.e. the first activation of a card session).

2) The Terminal shall analyse the ATR and identify the voltage class supported by the UICC.

3) If a 1,8 V technology Terminal identifies a 1,8 V technology UICC the Terminal may switch to 3 V operation. Switching from 1,8 V to 3 V shall only be performed by deactivating the UICC and activating it with 3 V supply voltage immediately after the analysis of the ATR without issuing any commands.

##### 5.1.5.3.3 Reference

ETSI TS 102 221 [1], clause 6.2.

##### 5.1.5.3.4 Test purpose

1) To verify that a 1,8 V technology Terminal initially activates the UICC with 1,8 V.

2) To verify that a 1,8 V technology Terminal correctly identifies the voltage class.

3) To verify that a 1,8 V technology Terminal deactivates the UICC-Terminal interface immediately after the analysis of the ATR without issuing any command and activates it with 3 V supply voltage or proceeds with the 1,8 V operation during the whole card session without switching to 3 V supply voltage.

##### 5.1.5.3.5 Method of test

5.1.5.3.5.1 Initial condition

The Terminal shall be connected to an UICC simulator simulating a 1,8 V technology UICC with nominal test conditions (see clause 5.2.1). All elementary files are coded as default.

The Terminal shall be powered on.

5.1.5.3.5.2 Procedure

The UICC simulator shall send the ATR indicating a 3 V technology UICC.

The UICC-Terminal interface shall be monitored for at least 1 minute until the UE is switched off.

##### 5.1.5.3.6 Acceptance criteria

1) The initial activation of the UICC-Terminal interface shall be performed with 1,8 V supply voltage.

2) The Terminal shall react in one of the following ways:

a) The Terminal deactivates the UICC-Terminal interface immediately after the analysis of the ATR from the UICC and activates it with 3 V supply voltage.

b) The Terminal proceeds with the card session without switching to another supply voltage.

#### 5.1.5.4 Reaction of 1,8 V technology Terminals on type recognition of 3 V technology UICCs

##### 5.1.5.4.1 Definition and applicability

When a 1,8 V technology Terminal detects a 3 V technology UICC during the ATR analysis the Terminal shall switch to 3 V operation.

For applicability of this test case see clause 3.8.

##### 5.1.5.4.2 Conformance requirement

1) A 1,8 V technology Terminal shall initially activate the UICC with 1,8 V (i.e. the first activation of a card session).

2) The Terminal shall analyse the ATR and identify the voltage class supported by the UICC.

3) If a 1,8 V technology Terminal identifies a 3 V technology UICC the Terminal shall switch to 3 V operation. Switching from 1,8 V to 3 V shall only be performed by deactivating the UICC and activating it with 3 V supply voltage immediately after the analysis of the ATR without issuing any commands.

##### 5.1.5.4.3 Reference

ETSI TS 102 221 [1], clause 6.2.

##### 5.1.5.4.4 Test purpose

1) To verify that a 1,8 V technology Terminal initially activates the UICC with 1,8 V.

2) To verify that a 1,8 V technology Terminal correctly identifies the voltage class.

3) To verify that a 1,8 V technology Terminal deactivates the UICC-Terminal interface immediately after the recognition of a 3 V technology UICC (in order to switch the supply voltage).

4) To verify that a 1,8 V technology Terminal activates the UICC with 3 V.

##### 5.1.5.4.5 Method of test

5.1.5.4.5.1 Initial condition

The Terminal shall be connected to an UICC simulator simulating a 3 V technology UICC with nominal test conditions (see clause 5.2.1). All elementary files are coded as default.

The Terminal shall be powered on.

5.1.5.4.5.2 Procedure

The UICC simulator shall send the ATR indicating a 3 V technology UICC.

The UICC-Terminal interface shall be monitored for at least 1 minute until the UE is switched off.

##### 5.1.5.4.6 Acceptance criteria

1) The initial activation of the UICC-Terminal interface shall be performed with 1,8 V supply voltage.

2) The Terminal shall react in the following way:

- The Terminal deactivates the UICC-Terminal interface immediately after the analysis of the ATR from the UICC and activates it with 3 V supply voltage. The Terminal proceeds with the card session.

#### 5.1.5.5 Void

#### 5.1.5.6 Reaction of Terminals receiving no ATR

##### 5.1.5.6.1 Reaction of Terminals receiving no ATR, 3 V - 5 V

5.1.5.6.1.1 Definition and applicability

A Terminal supporting 3 V - 5 V shall initially activate the UICC with 3V. If no ATR is received, the UICC‑Terminal interface shall be deactivated and activated with 5V.

For applicability of this test case see clause 3.8.

5.1.5.6.1.2 Conformance requirement

If a Terminal does not receive an ATR, the Terminal shall deactivate the UICC-Terminal interface and repeat the activation with the next higher voltage class.

5.1.5.6.1.3 Reference

ETSI TS 102 221 [1], see clause 6.2.

5.1.5.6.1.4 Test purpose

To verify that a Terminal deactivates the UICC-Terminal interface and repeats the activation with the next higher voltage class in case that the Terminal cannot receive an ATR.

5.1.5.6.1.5 Method of test

5.1.5.6.1.5.1 Initial condition

The Terminal shall be connected to an UICC simulator. All elementary files shall be coded as default. The Terminal shall be powered on.

5.1.5.6.1.5.2 Procedure

The UICC simulator shall send no ATR.

5.1.5.6.1.6 Acceptance criteria

If no ATR is received by the Terminal, the Terminal shall wait at least 40 000 clock cycles before deactivating the UICC-Terminal interface. The Terminal shall then repeat the activation procedure with the next higher voltage class.

##### 5.1.5.6.2 Reaction of Terminals receiving no ATR, 1,8 V - 3 V

5.1.5.6.2.1 Definition and applicability

A Terminal supporting 1,8 V - 3 V shall initially activate the UICC with 1,8 V. If no ATR is received, the UICC‑Terminal interface shall be deactivated and activated with 3 V.

For applicability of this test case see clause 3.8.

5.1.5.6.2.2 Conformance requirement

If a Terminal does not receive an ATR, the Terminal shall deactivate the UICC-Terminal interface and repeat the activation with the next higher voltage class.

5.1.5.6.2.3 Reference

ETSI TS 102 221 [], see clause 6.2.

5.1.5.6.2.4 Test purpose

To verify that a Terminal deactivates the UICC-Terminal interface and repeats the activation with the next higher voltage class in case that the Terminal cannot receive an ATR.

5.1.5.6.2.5 Method of test

5.1.5.6.2.5.1 Initial condition

The Terminal shall be connected to an UICC simulator. All elementary files shall be coded as default. The Terminal shall be powered on.

5.1.5.6.2.5.2 Procedure

The UICC simulator shall send no ATR.

5.1.5.6.2.6 Acceptance criteria

If no ATR is received by the Terminal, the Terminal shall wait at least 40 000 clock cycles before deactivating the UICC-Terminal interface. The Terminal shall then repeat the activation procedure with the next higher voltage class.

## 5.2 Electrical tests on each Terminal contact

### 5.2.1 Nominal test conditions

Tables 5.1 to 5.3 give the electrical conditions that shall be applied by the UICC simulator to all contacts during a test if not stated otherwise.

Table 5.1: Nominal test conditions on 5V UICC - Terminal interface

|  |  |  |  |
| --- | --- | --- | --- |
| Contacts | Low level | High level | Max. capacitive load |
| C1 (VCC) | --- | I = 10 mA |  |
| C2 (RST) | I = ‑200 μA | I = +20 μA | 30 pF |
| C3 (CLK) | I = ‑200 μA | I = +20 μA | 30 pF |
| C5 (GND) | --- | --- |  |
| C7 (I/O)  Terminal input  Terminal output | I = +1 mA  I = ‑1 mA | I = +20 μA  I = +20 μA | 30 pF |

Table 5.2: Nominal test conditions on 3 V UICC-Terminal interface

|  |  |  |  |
| --- | --- | --- | --- |
| Contacts | Low level | High level | Max. capacitive load |
| C1 (VCC) | --- | I = 7.5 mA |  |
| C2 (RST) | I = ‑200 μA | I = +20 μA | 30 pF |
| C3 (CLK) | I = ‑20 μA | I = +20 μA | 30 pF |
| C5 (GND) | --- | --- |  |
| C7 (I/O)  Terminal input  Terminal output | I = +1 mA  I = ‑1 mA | I = +20 μA  I = +20 μA | 30 pF |

Table 5.3: Nominal test conditions on 1,8 V UICC-Terminal interface

| Contacts | Low level | High level | Max. capacitive load |
| --- | --- | --- | --- |
| C1 (VCC) | --- | I = 5 mA |  |
| C2 (RST) | I = ‑200 μA | I = +20 μA | 30 pF |
| C3 (CLK) | I = ‑20 μA | I = +20 μA | 30 pF |
| C5 (GND) | --- | --- |  |
| C7 (I/O)  Terminal input  Terminal output | I = +1 mA  I = ‑1 mA | I = +20 μA  I = +20 μA | 30 pF |

NOTE 1: Measurements of contacts voltage levels can be done at any time since the beginning of activation of the UICC and the end of deactivation of the UICC (ISO/IEC 7816-3 [2], clause 5.1).

NOTE 2: The reference point of all measurements is the contact C5 (Ground).

NOTE 3: Currents flowing into the UICC are considered positive.

### 5.2.2 Electrical tests on contact C1 (Card power supply - VCC)

#### 5.2.2.1 Electrical tests on contact C1, Test 1: 3 V - 5 V

##### 5.2.2.1.1 Definition and applicability

When the user equipment is activated, the supply voltage on the UICC -Terminal interface shall remain in the specified range in order to ensure correct operation and to prevent any damage to the UICC.

For applicability of this test case see clause 3.8.

##### 5.2.2.1.2 Conformance requirement

1) The voltage on contact C1 of the UICC-Terminal interface shall be 5 V ± 10 % for Icc up to 10 mA when the Terminal is in 5 V operation mode.

2) The voltage on contact C1 of the UICC-Terminal interface shall be 3 V ± 10 % for Icc up to 10 mA when the Terminal is in 3 V operation mode.

##### 5.2.2.1.3 Reference

1) ETSI TS 102 221 [1], clause 5.1.

2) ETSI TS 102 221 [1], clause 5.2.

##### 5.2.2.1.4 Test purpose

To verify that the Terminal keeps the voltage on contact C1 of the UICC-Terminal interface within the ranges specified in the conformance requirements.

##### 5.2.2.1.5 Method of test

5.2.2.1.5.1 Initial condition

The Terminal shall be connected to an UICC simulator.

The UE shall be activated.

The remaining contacts of the UICC-Terminal interface shall be in nominal test conditions (see clause 5.2.1).

5.2.2.1.5.2 Test Procedure

The voltage of contact C1 (VCC) of the UICC-Terminal interface shall be measured.

##### 5.2.2.1.6 Acceptance criteria

The voltage on contact C1 of the UICC-Terminal interface shall be within the ranges specified in the conformance requirements.

#### 5.2.2.2 Electrical tests on contact C1, Test 2: 3 V - 5 V

##### 5.2.2.2.1 Definition and applicability

When the user equipment is activated, the supply voltage on the UICC-Terminal interface shall be able to counteract spikes in the current consumption of the UICC up to the limits given in the conformance requirement, ensuring that the supply voltage stays in the specified range.

For applicability of this test case see clause 3.8.

##### 5.2.2.2.2 Conformance requirement

1) The voltage on contact C1 of the UICC-Terminal interface shall be 5 V ± 10 % for spikes in the current consumption with a maximum charge of 40 n. As with no more than 400 ns duration and an amplitude of at most 200 mA when the Terminal is in 5 V operation mode.

2) The voltage on contact C1 of the UICC-Terminal interface shall be 3 V ± 10 % for spikes in the current consumption with a maximum charge of 12 n. As with no more than 400 ns duration and an amplitude of at most 60 mA when the Terminal is in 3 V operation mode.

Note: For compatibility reasons a maximum spike duration of 400 ns is kept also for terminals implemented in accordance to ETSI TS 102 221 [1] - Release 12 and upwards.

##### 5.2.2.2.3 Reference

1) ETSI TS 102 221 [1], clause 5.1.

2) ETSI TS 102 221 [1], clause 5.2.

##### 5.2.2.2.4 Test purpose

To verify that the Terminal keeps the voltage on contact C1 of the UICC-Terminal interface within the specified range for the conditions given in the UICC-Terminal conformance requirement.

##### 5.2.2.2.5 Method of test

5.2.2.2.5.1 Initial condition

The Terminal shall be connected to an UICC simulator.

The UE shall be activated.

The remaining contacts of the interface shall held in nominal test condition (see clause 5.2.1).

5.2.2.2.5.2 Procedure

In order to test the requirements 1), the voltage on contact C1 of the UICC-Terminal interface shall be monitored and the following current spikes shall be applied:

1) continuous spikes:

* current amplitude 20 mA;
* current offset 0 mA;
* duration 100 ns;
* pause 100 ns.

2) continuous spikes:

* current 20 mA;
* current offset 0 mA;
* duration 400 ns;
* pause 400 ns.

3) continuous spikes:

* current amplitude 15 mA;
* current offset 5 mA;
* (i.e. maximum amplitude = 5 mA + 15 mA = 20 mA);
* duration 150 ns;
* pause 300 ns.

4) random spikes:

* current amplitude 200 mA;
* current offset 0 mA;
* duration 200 ns;
* pause between 0,1 ms and 500 ms, randomly varied.

5) random spikes:

* current amplitude 100 mA;
* current offset 0 mA;
* duration 400 ns;
* pause between 0,1 ms and 500 ms, randomly varied.

6) random spikes:

* current amplitude 195 mA;
* current offset 5mA;
* (i.e. maximum amplitude = 5 mA + 195 mA = 200 mA);
* Duration 200 ns;
* Pause between 0,1 ms and 500 ms, randomly varied.

In order to test the requirements 2), the voltage on contact C1 of the UICC-Terminal interface shall be monitored and the following current spikes shall be applied:

1) continuous spikes:

* current amplitude 12 mA;
* current offset 0 mA;
* duration 100 ns;
* pause 100 ns.

2) continuous spikes:

* current 12 mA;
* current offset 0 mA;
* duration 400 ns;
* pause 400 ns.

3) continuous spikes:

* current amplitude 9 mA;
* current offset 3 mA;
* (i.e. maximum amplitude = 3 mA + 9 mA = 12 mA);
* duration 150 ns;
* pause 300 ns.

4) random spikes:

* current amplitude 60 mA;
* current offset 0 mA;
* duration 200 ns;
* pause between 0,1 ms and 500 ms, randomly varied.

5) random spikes:

* current amplitude 30 mA;
* current offset 0 mA;
* duration 400 ns;
* pause between 0,1 ms and 500 ms, randomly varied.

6) random spikes:

* current amplitude 57 mA;
* current offset 3 mA;
* (i.e. maximum amplitude = 3 mA + 57 mA = 60 mA);
* duration 200 ns;
* pause between 0,1 ms and 500 ms, randomly varied.

The specified spike durations shall be measured at 50 % of the spike amplitude.

##### 5.2.2.2.6 Acceptance criteria

The voltage on contact C1 of the UICC-Terminal interface shall be within the ranges specified in the conformance requirements.

#### 5.2.2.3 Electrical tests on contact C1, Test 1: 1,8 V - 3 V

##### 5.2.2.3.1 Definition and applicability

When the user equipment is activated, the supply voltage on the UICC -Terminal interface shall remain in the specified range in order to ensure correct operation and to prevent any damage to the UICC.

For applicability of this test case see clause 3.8.

##### 5.2.2.3.2 Conformance requirement

1) The voltage on contact C1 of the UICC-Terminal interface shall be 3 V ± 10 % for Icc up to 10 mA when the Terminal is in 3 V operation mode.

2) The voltage on contact C1 of the UICC-Terminal interface shall be 1,8 V ± 10 % for Icc up to 10 mA when the Terminal is in 1,8 V operation mode.

##### 5.2.2.3.3 Reference

1) ETSI TS 102 221 [1], clause 5.2.

2) ETSI TS 102 221 [1], clause 5.3.

##### 5.2.2.3.4 Test purpose

To verify that the Terminal keeps the voltage on contact C1 of the UICC-Terminal interface within the ranges specified in the conformance requirements.

##### 5.2.2.3.5 Method of test

5.2.2.3.5.1 Initial condition

The Terminal shall be connected to an UICC simulator.

The UE shall be activated.

The remaining contacts of the UICC-Terminal interface shall be in nominal test conditions (see clause 5.2.1).

5.2.2.3.5.2 Test Procedure

The voltage of contact C1 (VCC) of the UICC-Terminal interface shall be measured.

##### 5.2.2.3.6 Acceptance criteria

The voltage on contact C1 of the UICC-Terminal interface shall be within the ranges specified in the conformance requirements.

#### 5.2.2.4 Electrical tests on contact C1, Test 2: 1,8 V - 3 V

##### 5.2.2.4.1 Definition and applicability

When the user equipment is activated, the supply voltage on the UICC-Terminal interface shall be able to counteract spikes in the current consumption of the UICC up to the limits given in the conformance requirement, ensuring that the supply voltage stays in the specified range.

For applicability of this test case see clause 3.8.

##### 5.2.2.4.2 Conformance requirement

1) The voltage on contact C1 of the UICC-Terminal interface shall be 3 V ± 10 % for spikes in the current consumption with a maximum charge of 12 n. As with no more than 400 ns duration and an amplitude of at most 60 mA when the Terminal is in 3 V operation mode.

2) The voltage on contact C1 of the UICC-Terminal interface shall be 1,8 V ± 10 % for spikes in the current consumption with a maximum charge of 12 n. As with no more than 400 ns duration and an amplitude of at most 60 mA when the Terminal is in 1,8 V operation mode.

Note: For compatibility reasons a maximum spike duration of 400 ns is kept also for terminals implemented in accordance to ETSI TS 102 221 [1] - Release 12 and upwards.

##### 5.2.2.4.3 Reference

1) ETSI TS 102 221 [1], clause 5.2.

2) ETSI TS 102 221 [1], clause 5.3.

##### 5.2.2.4.4 Test purpose

To verify that the Terminal keeps the voltage on contact C1 of the UICC-Terminal interface within the specified range for the conditions given in the UICC-Terminal conformance requirement.

##### 5.2.2.4.5 Method of test

5.2.2.4.5.1 Initial condition

The Terminal shall be connected to an UICC simulator.

The UE shall be activated.

The remaining contacts of the interface shall held in nominal test condition (see clause 5.2.1).

5.2.2.4.5.2 Procedure

In order to test the requirements 1) and 2), the voltage on contact C1 of the UICC-Terminal interface shall be monitored and the following current spikes shall be applied:

1) continuous spikes:

* current amplitude 12 mA;
* current offset 0 mA;
* duration 100 ns;
* pause 100 ns.

2) continuous spikes:

* current 12 mA;
* current offset 0 mA;
* duration 400 ns;
* pause 400 ns.

3) continuous spikes:

* current amplitude 9 mA;
* current offset 3 mA;
* (i.e. maximum amplitude = 3 mA + 9 mA = 12 mA);
* duration 150 ns;
* pause 300 ns.

4) random spikes:

* current amplitude 60 mA;
* current offset 0 mA;
* duration 200 ns;
* pause between 0,1 ms and 500 ms, randomly varied.

5) random spikes:

* current amplitude 30 mA;
* current offset 0 mA;
* duration 400 ns;
* pause between 0,1 ms and 500 ms, randomly varied.

6) random spikes:

* current amplitude 57 mA;
* current offset 3 mA;
* (i.e. maximum amplitude = 3 mA + 57 mA = 60 mA);
* duration 200 ns;
* pause between 0,1 ms and 500 ms, randomly varied.

The specified spike durations shall be measured at 50 % of the spike amplitude.

##### 5.2.2.4.6 Acceptance criteria

The voltage on contact C1 of the UICC-Terminal interface shall be within the ranges specified in the conformance requirements.

### 5.2.3 Electrical tests on contact C2 (Reset - RST)

#### 5.2.3.1 Electrical tests on contact C2: 3 V - 5 V

##### 5.2.3.1.1 Definition and applicability

When the user equipment is activated, the voltage on contact C2 of the UICC-Terminal interface shall remain in the specified range in order to ensure correct operation and to prevent any damage to the UICC.

For applicability of this test case see clause 3.8.

##### 5.2.3.1.2 Conformance requirement

1) The voltage on contact C2 (RST) of the UICC-Terminal interface shall be between ‑0,3 V and +0,6 V for a current of ‑200 A in low state and between Vcc -0,7 V and Vcc + 0,3 V for a current of +20 A in high state when the Terminal is in 5 V operation mode.

2) The voltage on contact C2 (RST) of the UICC-Terminal interface shall be between ‑0,3 V and 0,2 × Vcc for a current of ‑200 A in low state and between 0,8 × Vcc and Vcc + 0,3 V for a current of +20 A in high state when the Terminal is in 3 V operation mode.

##### 5.2.3.1.3 Reference

1) ETSI TS 102 221 [1], clause 5.1.

2) ETSI TS 102 221 [1], clause 5.2.

##### 5.2.3.1.4 Test purpose

To verify that the Terminal keeps the voltage on contact C2 (RST) of the UICC-Terminal interface within the specified range, as given in the conformance requirement.

##### 5.2.3.1.5 Method of test

5.2.3.1.5.1 Initial condition

The Terminal shall be connected to an UICC simulator.

The UE shall be activated.

The remaining contacts of the UICC-Terminal interface shall be held in nominal test conditions (see clause 5.2.1).

5.2.3.1.5.2 Procedure

The voltage on contact C2 (RST) of the UICC-Terminal interface shall be measured.

##### 5.2.3.1.6 Acceptance criteria

The voltage on contact C2 (RST) of the UICC-Terminal interface shall be within the range specified in the conformance requirement.

#### 5.2.3.2 Electrical tests on contact C2: 1,8 V - 3 V

##### 5.2.3.2.1 Definition and applicability

When the user equipment is activated, the voltage on contact C2 of the UICC-Terminal interface shall remain in the specified range in order to ensure correct operation and to prevent any damage to the UICC.

For applicability of this test case see clause 3.8.

##### 5.2.3.2.2 Conformance requirement

1) The voltage on contact C2 (RST) of the UICC-Terminal interface shall be between ‑0,3 V and 0,2 × Vcc for a current of ‑200 A in low state and between 0,8 × Vcc and Vcc + 0,3 V for a current of +20 A in high state when the Terminal is in 3 V operation mode.

2) The voltage on contact C2 (RST) of the UICC-Terminal interface shall be between ‑0,3 V and 0,2 × Vcc for a current of ‑200 A in low state and between 0,8 × Vcc and Vcc + 0,3 V for a current of +20 A in high state when the Terminal is in 1,8 V operation mode.

##### 5.2.3.2.3 Reference

1) ETSI TS 102 221 [], clause 5.2.

2) ETSI TS 102 221 [], clause 5.3.

##### 5.2.3.2.4 Test purpose

To verify that the Terminal keeps the voltage on contact C2 (RST) of the UICC-Terminal interface within the specified range, as given in the conformance requirement.

##### 5.2.3.2.5 Method of test

5.2.3.2.5.1 Initial condition

The Terminal shall be connected to an UICC simulator.

The UE shall be activated.

The remaining contacts of the UICC-Terminal interface shall be held in nominal test conditions (see clause 5.2.1).

5.2.3.2.5.2 Procedure

The voltage on contact C2 (RST) of the UICC-Terminal interface shall be measured.

##### 5.2.3.2.6 Acceptance criteria

The voltage on contact C2 (RST) of the UICC-Terminal interface shall be within the range specified in the conformance requirement.

### 5.2.4 Electrical tests on contact C3 (Clock - CLK)

#### 5.2.4.1 Electrical tests on contact C3: 3 V - 5 V

##### 5.2.4.1.1 Definition and applicability

When the user equipment is activated, the voltage, the rise/fall time of the signal, the clock cycle ratio and the frequency on contact C3 of the UICC - Terminal interface shall remain in the specified range in order to ensure correct operation and to prevent any damage to the UICC.

For applicability of this test case see clause 3.8.

##### 5.2.4.1.2 Conformance requirement

1) The voltage on contact C3 (CLK) of the UICC - Terminal interface shall be between ‑0,3 V and +0,5 V for a current of ‑200 A in low state and between 0,7 × Vcc and Vcc + 0,3 V for a current of +20 A in high state when the Terminal is in 5 V operation mode.

2) The rise and the fall time of the clock signal shall not exceed 9 % of the clock period with a maximum of 0,5 s when the Terminal is in 5 V operation mode.

3) The cycle ratio of the clock signal shall be between 40 % and 60 % of the period, in steady state when the Terminal is in 5 V operation mode.

4) The frequency of the clock signal shall be between 1 MHz and 5 MHz when the Terminal is in 5 V operation mode.

5) The voltage on contact C3 (CLK) of the UICC - Terminal interface shall be between ‑0,3 V and 0,2 × Vcc for a current of ‑20 A in low state and between 0,7 × Vcc and Vcc + 0,3 V for a current of +20 A in high state when the Terminal is in 3 V operation mode.

6) The rise and the fall time of the clock signal shall not exceed 50 ns when the Terminal is in 3 V operation mode.

7) The cycle ratio of the clock signal shall be between 40 % and 60 % of the period, in steady state when the Terminal is in 3 V operation mode.

8) The frequency of the clock signal shall be between 1 MHz and 5 MHz when the Terminal is in 3 V operation mode.

##### 5.2.4.1.3 Reference

1 - 4) ETSI TS 102 221 [1], clause 5.1.

5 - 8) ETSI TS 102 221 [1], clause 5.2.

##### 5.2.4.1.4 Test purpose

To verify that the Terminal keeps the voltage, the rise and fall time, the cycle ratio and the frequency on contact C3 (CLK) of the UICC - Terminal interface within the ranges specified in the conformance requirements.

##### 5.2.4.1.5 Method of test

5.2.4.1.5.1 Initial condition

The Terminal shall be connected to an UICC simulator.

The UE shall be activated.

The remaining contacts of the UICC-Terminal interface shall be held in nominal test conditions (see clause 5.2.1).

5.2.4.1.5.2 Procedure

The voltage, the rise/fall time, the clock cycle ratio and the frequency on contact C3 (CLK) of the UICC-Terminal interface shall be measured.

##### 5.2.4.1.6 Acceptance criteria

The voltage, the rise and fall time, the cycle ratio and the frequency on contact C3 (CLK) of the UICC-Terminal interface shall be within the ranges specified in the conformance requirements.

#### 5.2.4.2 Electrical tests on contact C3: 1,8 V - 3 V

##### 5.2.4.2.1 Definition and applicability

When the user equipment is activated, the voltage, the rise/fall time of the signal, the clock cycle ratio and the frequency on contact C3 of the UICC - Terminal interface shall remain in the specified range in order to ensure correct operation and to prevent any damage to the UICC.

For applicability of this test case see clause 3.8.

##### 5.2.4.2.2 Conformance requirement

1) The voltage on contact C3 (CLK) of the UICC - Terminal interface shall be between ‑0,3 V and 0,2 × Vcc for a current of ‑20 A in low state and between 0,7 × Vcc and Vcc + 0,3 V for a current of +20 A in high state when the Terminal is in 3 V operation mode.

2) The rise and the fall time of the clock signal shall not exceed 50 ns when the Terminal is in 3 V operation mode.

3) The cycle ratio of the clock signal shall be between 40 % and 60 % of the period, in steady state when the Terminal is in 3 V operation mode.

4) The frequency of the clock signal shall be between 1 MHz and 5 MHz when the Terminal is in 3 V operation mode.

5) The voltage on contact C3 (CLK) of the UICC-Terminal interface shall be between ‑0,3 V and 0,2 × Vcc for a current of ‑20 A in low state and between 0,7 × Vcc and Vcc + 0,3 V for a current of +20 A in high state when the Terminal is in 1,8 V operation mode.

6) The rise and the fall time of the clock signal shall not exceed 50 ns when the Terminal is in 1,8 V operation mode.

7) The cycle ratio of the clock signal shall be between 40 % and 60 % of the period, in steady state when the Terminal is in 1,8 V operation mode.

8) The frequency of the clock signal shall be between 1 MHz and 5 MHz when the Terminal is in 1,8 V operation mode.

##### 5.2.4.2.3 Reference

1 - 4) ETSI TS 102 221 [], clause 5.2.

5 - 8) ETSI TS 102 221 [], clause 5.3.

##### 5.2.4.2.4 Test purpose

To verify that the Terminal keeps the voltage, the rise and fall time, the cycle ratio and the frequency on contact C3 (CLK) of the UICC - Terminal interface within the ranges specified in the conformance requirements.

##### 5.2.4.2.5 Method of test

5.2.4.2.5.1 Initial condition

The Terminal shall be connected to an UICC simulator.

The UE shall be activated.

The remaining contacts of the UICC-Terminal interface shall be held in nominal test conditions (see clause 5.2.1).

5.2.4.2.5.2 Procedure

The voltage, the rise/fall time, the clock cycle ratio and the frequency on contact C3 (CLK) of the UICC-Terminal interface shall be measured.

##### 5.2.4.2.6 Acceptance criteria

The voltage, the rise and fall time, the cycle ratio and the frequency on contact C3 (CLK) of the UICC-Terminal interface shall be within the ranges specified in the conformance requirements.

### 5.2.5 Electrical tests on contact C7 (Input/Output - I/O)

#### 5.2.5.1 Electrical tests on contact C7, Test 1: 3 V - 5 V

##### 5.2.5.1.1 Definition and applicability

When the user equipment is activated, the Terminal shall keep the voltage, the current and the rise/fall time of the signal on contact C7 of the UICC-Terminal interface within the specified range in order to ensure correct operation and to prevent any damage to the UICC.

For applicability of this test case see clause 3.8.

##### 5.2.5.1.2 Conformance requirement

1) Terminal receiving state A (low state):

* With an imposed voltage of 0 V the current flowing out of the Terminal shall not exceed 1 mA when the Terminal is in 5 V operation mode.

2) Terminal transmitting state A (low state):

* The voltage shall be between -0,3 V and 0,15 × Vcc when a current of 1 mA flowing into the Terminal is applied when the Terminal is in 5 V operation mode.

3) Terminal transmitting or receiving state Z (high state):

* The voltage shall be between +3,8 V (VOH)/0,7 × Vcc (VIH) respectively and Vcc + 0,3 V when a current of 20 μA flowing out of the Terminal is applied when the Terminal is in 5 V operation mode.

4) The rise time and the fall time of the I/O signal shall not exceed 1 μs when the Terminal is in 5V operation mode.

5) Terminal receiving state A (low state):

* With an imposed voltage of 0 V the current flowing out of the Terminal shall not exceed 1 mA when the Terminal is in 3 V operation mode.

6) Terminal transmitting state A (low state):

* The voltage shall be between ‑0,3 V and 0,2 × Vcc when a current of 1 mA flowing into the Terminal is applied when the Terminal is in 3 V operation mode.

7) Terminal transmitting or receiving state Z (high state):

* The voltage shall be between 0,7 × Vcc and Vcc + 0,3 V when a current of 20 μA flowing out of the Terminal is applied when the Terminal is in 3 V operation mode.

8) The rise time and the fall time of the I/O signal shall not exceed 1 μs when the Terminal is in 3 V operation mode.

##### 5.2.5.1.3 Reference

1 - 4) ETSI TS 102 221 [1], clause 5.1.

5 - 8) ETSI TS 102 221 [1], clause 5.2.

##### 5.2.5.1.4 Test purpose

To verify that the Terminal keeps the voltage, the current and the rise and fall times of the signal on contact C7 (I/O) of the UICC-Terminal interface within the ranges specified in the conformance requirements.

##### 5.2.5.1.5 Method of test

5.2.5.1.5.1 Initial condition

The Terminal shall be connected to an UICC simulator.

The UE shall be activated.

The remaining contacts of the UICC-Terminal interface shall be held in nominal test conditions (see clause 5.2.1).

5.2.5.1.5.2 Procedure

The voltage, the current and the rise/fall time on contact C7 (I/O) of the UICC-Terminal interface shall be measured.

##### 5.2.5.1.6 Acceptance criteria

The voltage, the current and the rise and fall times of the signal on contact C7 (I/O) of the UICC-Terminal interface shall be within the ranges specified in the conformance requirements.

#### 5.2.5.2 Electrical tests on contact C7, Test 2: 3 V - 5 V

##### 5.2.5.2.1 Definition and applicability

When the user equipment is activated, the Terminal shall keep the voltage, the current and the rise/fall time of the signal on contact C7 of the UICC-Terminal interface within the specified range in order to ensure correct operation and to prevent any damage to the UICC.

For applicability of this test case see clause 3.8.

##### 5.2.5.2.2 Conformance requirement

1) Terminal receiving state A (low state):

* With an imposed voltage of 0 V the current flowing out of the Terminal shall not exceed 1 mA when the Terminal is in 5 V operation mode.

2) Terminal transmitting state A (low state):

* The voltage shall be between -0,3 V and 0,15 × Vcc when a current of 1 mA flowing into the Terminal is applied when the Terminal is in 5 V operation mode.

3) Terminal transmitting or receiving state Z (high state):

* The voltage shall be between +3,8 V (VOH)/0,7 × Vcc (VIH) respectively and Vcc + 0,3 V when a current of 20 μA flowing out of the Terminal is applied when the Terminal is in 5 V operation mode.

4) The rise time and the fall time of the I/O signal shall not exceed 100 ns when the Terminal is in 5V operation mode.

5) Terminal receiving state A (low state):

* With an imposed voltage of 0 V the current flowing out of the Terminal shall not exceed 1 mA when the Terminal is in 3 V operation mode.

6) Terminal transmitting state A (low state):

* The voltage shall be between ‑0,3 V and 0,2 × Vcc when a current of 1 mA flowing into the Terminal is applied when the Terminal is in 3 V operation mode.

7) Terminal transmitting or receiving state Z (high state):

* The voltage shall be between 0,7 × Vcc and Vcc + 0,3 V when a current of 20 μA flowing out of the Terminal is applied when the Terminal is in 3 V operation mode.

8) When the low impedance buffer is selected, the rise time and the fall time of the I/O signal shall not exceed 100 ns when the Terminal is in 3 V operation mode.

##### 5.2.5.2.3 Reference

1 - 4) ETSI TS 102 221 [], clause 5.1.

5 - 8) ETSI TS 102 221 [1], clause 5.2.

##### 5.2.5.2.4 Test purpose

To verify that the Terminal supporting low impedance buffer keeps the voltage, the current and the rise and fall times of the signal on contact C7 (I/O) of the UICC-Terminal interface within the ranges specified in the conformance requirements.

##### 5.2.5.2.5 Method of test

5.2.5.2.5.1 Initial condition

The Terminal shall be connected to a UICC simulator.

The UE shall be activated.

The remaining contacts of the UICC-Terminal interface shall be held in nominal test conditions (see clause 5.2.1).

An ATR indicating the support of the low impedance buffer shall have been received and the PPS procedure selecting the low impedance buffer shall have been successfully completed.

5.2.5.2.5.2 Procedure

The voltage, the current and the rise/fall time on contact C7 (I/O) of the UICC-Terminal interface shall be measured.

##### 5.2.5.2.6 Acceptance criteria

The voltage, the current and the rise and fall times of the signal on contact C7 (I/O) of the UICC-Terminal interface shall be within the ranges specified in the conformance requirements.

#### 5.2.5.3 Electrical tests on contact C7, Test 1: 1,8 V - 3 V

##### 5.2.5.3.1 Definition and applicability

When the user equipment is activated, the Terminal shall keep the voltage, the current and the rise/fall time of the signal on contact C7 of the UICC-Terminal interface within the specified range in order to ensure correct operation and to prevent any damage to the UICC.

For applicability of this test case see clause 3.8.

##### 5.2.5.3.2 Conformance requirement

1) Terminal receiving state A (low state):

* With an imposed voltage of 0 V the current flowing out of the Terminal shall not exceed 1 mA when the Terminal is in 3 V operation mode.

2) Terminal transmitting state A (low state):

* The voltage shall be between ‑0,3 V and 0,2 × Vcc when a current of 1 mA flowing into the Terminal is applied when the Terminal is in 3 V operation mode.

3) Terminal transmitting or receiving state Z (high state):

* The voltage shall be between 0,7 × Vcc and Vcc + 0,3 V when a current of 20 μA flowing out of the Terminal is applied when the Terminal is in 3 V operation mode.

4) The rise time and the fall time of the I/O signal shall not exceed 1 μs when the Terminal is in 3 V operation mode.

5) Terminal receiving state A (low state):

* With an imposed voltage of 0 V the current flowing out of the Terminal shall not exceed 1 mA when the Terminal is in 1,8 V operation mode.

6) Terminal transmitting state A (low state):

* The voltage shall be between ‑0,3 V and 0,2 × Vcc when a current of 1 mA flowing into the Terminal is applied when the Terminal is in 1,8 V operation mode.

7) Terminal transmitting or receiving state Z (high state):

* The voltage shall be between 0,7 × Vcc and Vcc + 0,3 V when a current of 20 μA flowing out of the Terminal is applied when the Terminal is in 1,8 V operation mode.

8) The rise time and the fall time of the I/O signal shall not exceed 1 μs when the Terminal is in 1,8 V operation mode.

##### 5.2.5.3.3 Reference

1 - 4) ETSI TS 102 221 [], clause 5.2.

4 - 8) ETSI TS 102 221 [], clause 5.3.

##### 5.2.5.3.4 Test purpose

To verify that the Terminal keeps the voltage, the current and the rise and fall times of the signal on contact C7 (I/O) of the UICC-Terminal interface within the ranges specified in the conformance requirements.

##### 5.2.5.3.5 Method of test

5.2.5.3.5.1 Initial condition

The Terminal shall be connected to an UICC simulator.

The UE shall be activated.

The remaining contacts of the UICC-Terminal interface shall be held in nominal test conditions (see clause 5.2.1).

5.2.5.3.5.2 Procedure

The voltage, the current and the rise/fall time on contact C7 (I/O) of the UICC-Terminal interface shall be measured.

##### 5.2.5.3.6 Acceptance criteria

The voltage, the current and the rise and fall times of the signal on contact C7 (I/O) of the UICC-Terminal interface shall be within the ranges specified in the conformance requirements.

#### 5.2.5.4 Electrical tests on contact C7, Test 2: 1,8 V - 3 V

##### 5.2.5.4.1 Definition and applicability

When the user equipment is activated, the Terminal shall keep the voltage, the current and the rise/fall time of the signal on contact C7 of the UICC-Terminal interface within the specified range in order to ensure correct operation and to prevent any damage to the UICC.

For applicability of this test case see clause 3.8.

##### 5.2.5.4.2 Conformance requirement

1) Terminal receiving state A (low state):

* With an imposed voltage of 0 V the current flowing out of the Terminal shall not exceed 1 mA when the Terminal is in 3 V operation mode.

2) Terminal transmitting state A (low state):

* The voltage shall be between ‑0,3 V and 0,2 × Vcc when a current of 1 mA flowing into the Terminal is applied when the Terminal is in 3 V operation mode.

3) Terminal transmitting or receiving state Z (high state):

* The voltage shall be between 0,7 × Vcc and Vcc + 0,3 V when a current of 20 μA flowing out of the Terminal is applied when the Terminal is in 3 V operation mode.

4) The rise time and the fall time of the I/O signal shall not exceed 100 ns when the Terminal is in 3 V operation mode.

5) Terminal receiving state A (low state):

* With an imposed voltage of 0 V the current flowing out of the Terminal shall not exceed 1 mA when the Terminal is in 1,8 V operation mode.

6) Terminal transmitting state A (low state):

* The voltage shall be between ‑0,3 V and 0,2 × Vcc when a current of 1 mA flowing into the Terminal is applied when the Terminal is in 1,8 V operation mode.

7) Terminal transmitting or receiving state Z (high state):

* The voltage shall be between 0,7 × Vcc and Vcc + 0,3 V when a current of 20 μA flowing out of the Terminal is applied when the Terminal is in 1,8 V operation mode.

8) When the low impedance buffer is selected, the rise time and the fall time of the I/O signal shall not exceed 100 ns when the Terminal is in 1,8 V operation mode.

##### 5.2.5.4.3 Reference

1 - 4) ETSI TS 102 221 [], clause 5.2.

4 - 8) ETSI TS 102 221 [], clause 5.3.

##### 5.2.5.4.4 Test purpose

To verify that the Terminal supporting low impedance buffer keeps the voltage, the current and the rise and fall times of the signal on contact C7 (I/O) of the UICC-Terminal interface within the ranges specified in the conformance requirements.

##### 5.2.5.4.5 Method of test

5.2.5.4.5.1 Initial condition

The Terminal shall be connected to a UICC simulator.

The UE shall be activated.

The remaining contacts of the UICC-Terminal interface shall be held in nominal test conditions (see clause 5.2.1).

An ATR indicating the support of the low impedance buffer shall have been received and the PPS procedure selecting the low impedance buffer shall have been successfully completed.

5.2.5.4.5.2 Procedure

The voltage, the current and the rise/fall time on contact C7 (I/O) of the UICC-Terminal interface shall be measured.

##### 5.2.5.4.6 Acceptance criteria

The voltage, the current and the rise and fall times of the signal on contact C7 (I/O) of the UICC-Terminal interface shall be within the ranges specified in the conformance requirements.

# 6 Initial communication tests

## 6.1 ATR

### 6.1.1 ATR characters

#### 6.1.1.1 Definition and applicability

The ATR is the first string of bytes sent from the UICC to the Terminal after a reset has been performed.

The historical bytes indicate to the external world how to use the card.

Both protocols T=0 and T=1 are mandatory for the Terminal. The protocol starts after either the answer to reset or a successful PPS exchange.

For applicability of this test case see clause 3.8.

#### 6.1.1.2 Conformance requirement

##### 6.1.1.2.0 Description

1) The Terminal shall adopt the data encoding convention and initial etu time defined in the initial character TS of the ATR.

2) The Terminal shall be able to receive interface characters for transmission protocols other than T=0 and T=1, historical bytes and a check byte, even if only T=0 and T=1 are used by the Terminal.

##### 6.1.1.2.1 Reference

ETSI TS 102 221 [1], clauses 6.3 and 7.

#### 6.1.1.3 Test purpose

1) To verify that the Terminal adopts the data encoding convention and initial etu time defined in the initial character TS of the ATR.

2) To verify that the Terminal accepts interface characters for transmission protocols (T=0 and T=1), historical bytes and a check byte.

#### 6.1.1.4 Method of test

##### 6.1.1.4.1 Initial conditions

The Terminal shall be connected to the UICC (or UICC simulator).

##### 6.1.1.4.2 Procedure

a) The Terminal shall be powered on.

b) The UICC (or UICC simulator) shall send an ATR as follows:

| Character | Value | Description |
| --- | --- | --- |
| TS | '3B' | Indicates direct convention |
| T0 | '97' | TA1 and TD1 are present  7 bytes of historical bytes |
| TA1 | '11' | Clock rate conversion factor FI=1 (F=372)  Baud rate adjustment factor DI=1 (D=1) |
| TD1 | '80' | TD2 only is present  Protocol T=0 supported by UICC |
| TD2 | '1F' | TA3 only is present  Global interface bytes following (T=15) |
| TA3 | '46' | Clock stop supported (low electrical state)  1,8 V technology UICC |
| T1 | '80' |  |
| T2 | '31' | Card data services |
| T3 | 'A0' | SELECT by AID supported  EFDIR present |
| T4 | '73' | Card capabilities |
| T5 | 'BE' | SFI supported |
| T6 | '21' | Data Coding Byte |
| T7 | '00' | No extended Lc and Le  No Logical channels supported |
| TCK | 'A2' | Check byte |

c) The Terminal shall be made to send further commands to the UICC (or UICC simulator) (e.g. by entering the PIN).

d) The Terminal is switched off and on.

e) The UICC (or UICC simulator) shall send an ATR as follows:

|  |  |  |
| --- | --- | --- |
| Character | Value | Description |
| TS | '3F' | Indicates inverse convention |
| T0 | '97' | TA1 and TD1 are present  7 bytes of historical bytes |
| TA1 | '11' | Clock rate conversion factor FI=1 (F=372)  Baud rate adjustment factor DI=1 (D=1) |
| TD1 | '80' | TD2 only is present  Protocol T=0 supported by UICC |
| TD2 | '1F' | TA3 only is present  Global interface bytes following (T=15) |
| TA3 | '46' | Clock stop supported (low electrical state)  1,8 V technology UICC |
| T1 | '80' |  |
| T2 | '31' | Card data services |
| T3 | 'A0' | SELECT by AID supported  EFDIR present |
| T4 | '73' | Card capabilities |
| T5 | 'BE' | SFI supported |
| T6 | '21' | Data Coding Byte |
| T7 | '00' | No extended Lc and Le  No Logical channels supported |
| TCK | 'A2' | Check byte |

f) The Terminal shall be made to send further commands to the UICC (or UICC simulator) (e.g. by entering the PIN).

g) The Terminal is switched off and on.

h) The UICC (or UICC simulator) shall send an ATR as follows:

| Character | Value | Description |
| --- | --- | --- |
| TS | '3F' | Indicates inverse convention |
| T0 | '97' | TA1, and TD1 are present  7 bytes of historical bytes |
| TA1 | '11' | Clock rate conversion factor FI=1 (F=372)  Baud rate adjustment factor DI=1 (D=1) |
| TD1 | '80' | Only TD2 is present  Protocol T=0 supported by UICC |
| TD2 | 'B1' | TA3, TB3 and TD3 are present  Protocol T=1 supported by UICC |
| TA3 | 'FE' | IFSC is 254 bytes long |
| TB3 | '00' | Block Waiting Integer=0  Character Waiting Integer=0 |
| TD3 | '1F' | Only TA4 is present  Global interface bytes following (T=15) |
| TA4 | '46' | Clock stop supported (low electrical state)  1,8 V technology UICC |
| T1 | '80' |  |
| T2 | '31' | Card data services |
| T3 | 'A0' | SELECT by AID supported  EFDIR present |
| T4 | '73' | Card capabilities |
| T5 | 'BE' | SFI supported |
| T6 | '21' | Data Coding Byte |
| T7 | '00' | No extended Lc and Le  No Logical channels supported |
| TCK | 'ED' | Check byte |

i) The Terminal shall be made to send further commands to the UICC (or UICC simulator) (e.g. by entering the PIN).

j) The Terminal is switched off and on.

k) The UICC (or UICC simulator) shall send an ATR as follows:

| Character | Value | Description |
| --- | --- | --- |
| TS | '3B' | Indicates direct convention |
| T0 | '97' | TA1, and TD1 are present  7 bytes of historical bytes |
| TA1 | '11' | Clock rate conversion factor FI=1 (F=372)  Baud rate adjustment factor DI=1 (D=1) |
| TD1 | '91' | TA2 and TD2 are present  Protocol T=1 supported by UICC |
| TA2 | '81' | Protocol T=1 used in specific mode  Parameters indicated by the interface bytes, and card is not able to change mode |
| TD2 | 'B1' | TA3, TB3 and TD3 are present  Protocol T=1 supported by UICC |
| TA3 | 'FE' | IFSC is 254 bytes long |
| TB3 | '00' | Block Waiting Integer=0  Character Waiting Integer=0 |
| TD3 | '0F' | Global interface bytes following (T=15) |
| TA4 | '46' | Clock stop supported (low electrical state)  1,8 V technology UICC |
| T1 | '80' |  |
| T2 | '31' | Card data services |
| T3 | 'A0' | SELECT by AID supported  EFDIR present |
| T4 | '73' | Card capabilities |
| T5 | 'BE' | SFI supported |
| T6 | '21' | Data Coding Byte |
| T7 | '00' | No extended Lc and Le  No Logical channels supported |
| TCK | '7D' | Check byte |

l) The Terminal shall be made to send further commands to the UICC (or UICC simulator) (e.g. by entering the PIN).

m) The Terminal is switched off and on.

n) The UICC (or UICC simulator) shall send an ATR as follows:

| Character | Value | Description |
| --- | --- | --- |
| TS | '3F' | Indicates inverse convention |
| T0 | '97' | TA1, and TD1 are present  7 bytes of historical bytes |
| TA1 | '11' | Clock rate conversion factor FI=1 (F=372)  Baud rate adjustment factor DI=1 (D=1) |
| TD1 | '91' | TA2 and TD2 are present  Protocol T=1 supported by UICC |
| TA2 | '81' | Protocol T=1 used in specific mode  Parameters indicated by the interface bytes, and card is not able to change mode |
| TD2 | 'B1' | TA3, TB3 and TD3 are present  Protocol T=1 supported by UICC |
| TA3 | 'FE' | IFSC is 254 bytes long |
| TB3 | '00' | Block Waiting Integer=0  Character Waiting Integer=0 |
| TD3 | '0F' | Global interface bytes following (T=15) |
| TA4 | '46' | Clock stop supported (low electrical state)  1,8 V technology UICC |
| T1 | '80' |  |
| T2 | '31' | Card data services |
| T3 | 'A0' | SELECT by AID supported  EFDIR present |
| T4 | '73' | Card capabilities |
| T5 | 'BE' | SFI supported |
| T6 | '21' | Data Coding Byte |
| T7 | '00' | No extended Lc and Le  No Logical channels supported |
| TCK | '7D' | Check byte |

o) The Terminal shall be made to send further commands to the UICC (or UICC simulator) (e.g. by entering the PIN).

#### 6.1.1.5 Acceptance criteria

In step c), the Terminal shall start a T=0 session in direct convention and work with the UICC (or UICC simulator).

In steps f) and i), the Terminal shall start a T=0 session in inverse convention and work with the UICC (or UICC simulator).

In step l), the Terminal shall start a T=1 session in direct convention and work with the UICC (or UICC simulator).

In step o), the Terminal shall start a T=1 session in inverse convention and work with the UICC (or UICC simulator).

## 6.2 Clock stop mode with 1,8 V technology UICC

### 6.2.1 Definition and applicability

The Terminal shall be able to receive interface characters, historical bytes and a check byte, even if only T=0 and T=1 are used by the Terminal.

T=15 global interface parameters shall be returned by the UICC.

The UICC shall support the clock stop procedure. The clock stop mode is indicated in TAi (i > 2) in T=15 in the ATR.

For applicability of this test case see clause 3.8.

### 6.2.2 Conformance requirement

#### 6.2.2.0 Description

If the UICC supports any other operating conditions even together with class A, clock stop mode shall be supported and the indication shall be set accordingly. The terminal shall follow this indication independently of operating conditions indicated by the card.

In case the UICC does not support any supply voltage indication, the UICC shall be treated as a 5 V only card by the Terminal.

The Terminal shall wait at least 1 860 clock cycles after having received the last character, including the guard time (2 etu), of the response before it switches off the clock. It shall wait at least 744 clock cycles before it sends the first command after having started the clock.

#### 6.2.2.1 Reference

ETSI TS 102 221 [1], clauses 6.7, 6.10 and 11.1.1.4.6.1.

ISO/IEC 7816‑3 [2], clauses 5.3.4 and 6.5.5.

### 6.2.3 Test purpose

1) To verify that the clock is only switched off as indicated in the ATR first global interface byte and file characteristics (byte 1 of the directory characteristics).

2) To verify that the timing of the clock switching is as specified.

### 6.2.4 Method of test

#### 6.2.4.1 Initial conditions

The Terminal shall be connected to the UICC simulator. PIN shall be enabled.

#### 6.2.4.2 Procedure

a) The Terminal shall be powered on and the UICC simulator shall send an ATR as follows:

| Character | Value | Description |
| --- | --- | --- |
| TS | '3B' | Indicates direct convention |
| T0 | '97' | TA1 and TD1 are present  7 bytes of historical bytes |
| TA1 | '11' | Clock rate conversion factor FI=1 (F=372)  Baud rate adjustment factor DI=1 (D=1) |
| TD1 | '80' | TD2 only is present  Protocol T=0 supported by UICC |
| TD2 | '1F' | TA3 only is present  Global interface bytes following (T=15) |
| TA3 | 'C6' | Clock stop supported (no preferred state)  1,8 V technology UICC |
| T1 | '80' |  |
| T2 | '31' | Card data services |
| T3 | 'A0' | SELECT by AID supported  EFDIR present |
| T4 | '73' | Card capabilities |
| T5 | 'BE' | SFI supported |
| T6 | '21' | Data Coding Byte |
| T7 | '00' | No extended Lc and Le  No Logical channels supported |
| TCK | '22' | Check byte |

and be used with bits set as follows:

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| b8 | b7 | b6 | b5 | B4 | b3 | b2 | b1 | Meaning |
| 0 | 1 | 1 | 0 | 0 | 0 | 0 | 1 | Voltage classes BC and clock stop mode supported. No preferred level. |

b) When the Terminal is in mode PIN check, 10 s shall elapse before the PIN shall be entered.

c) The Terminal shall be powered off and on. The UICC simulator shall send an ATR as follows:

| Character | Value | Description |
| --- | --- | --- |
| TS | '3B' | Indicates direct convention |
| T0 | '97' | TA1 and TD1 are present  7 bytes of historical bytes |
| TA1 | '11' | Clock rate conversion factor FI = 1 (F = 372)  Baud rate adjustment factor DI = 1 (D = 1) |
| TD1 | '80' | TD2 only is present  Protocol T=0 supported by UICC |
| TD2 | '1F' | TA3 only is present  Global interface bytes following (T=15) |
| TA3 | '86' | Clock stop supported (high electrical state)  1,8 V technology UICC |
| T1 | '80' |  |
| T2 | '31' | Card data services |
| T3 | 'A0' | SELECT by AID supported  EFDIR present |
| T4 | '73' | Card capabilities |
| T5 | 'BE' | SFI supported |
| T6 | '21' | Data Coding Byte |
| T7 | '00' | No extended Lc and Le  No Logical channels supported |
| TCK | '62' | Check byte |

and be used with bits set as follows:

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| b8 | b7 | b6 | b5 | b4 | b3 | b2 | b1 | Meaning |
| 0 | 1 | 1 | 0 | 0 | 1 | 0 | 1 | Voltage classes BC and clock stop mode supported. High level preferred |

d) When the Terminal is in mode PIN check, 10 s shall elapse before the PIN shall be entered.

e) The Terminal shall be powered off and on. The UICC simulator shall send an ATR as follows:

| Character | Value | Description |
| --- | --- | --- |
| TS | '3B' | Indicates direct convention |
| T0 | '97' | TA1 and TD1 are present  7 bytes of historical bytes |
| TA1 | '11' | Clock rate conversion factor FI=1 (F=372)  Baud rate adjustment factor DI=1 (D=1) |
| TD1 | '80' | TD2 only is present  Protocol T=0 supported by UICC |
| TD2 | '1F' | TA3 only is present  Global interface bytes following (T=15) |
| TA3 | '46' | Clock stop supported (low electrical state)  1,8 V technology UICC |
| T1 | '80' |  |
| T2 | '31' | Card data services |
| T3 | 'A0' | SELECT by AID supported  EFDIR present |
| T4 | '73' | Card capabilities |
| T5 | 'BE' | SFI supported |
| T6 | '21' | Data Coding Byte |
| T7 | '00' | No extended Lc and Le  No Logical channels supported |
| TCK | 'A2' | Check byte |

and be used with bits set as follows:

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| b8 | b7 | b6 | b5 | b4 | b3 | b2 | b1 | Meaning |
| 0 | 1 | 1 | 0 | 1 | 0 | 0 | 1 | Voltage classes BC and clock stop mode supported. Low level preferred |

f) When the Terminal is in mode PIN check, 10 s shall elapse before the PIN shall be entered.

### 6.2.5 Acceptance criteria

1) During step b), the Terminal shall switch off the clock at either high or low level.

2) During step d), the Terminal shall switch off the clock at high level.

3) During step f), the Terminal shall switch off the clock at low level.

4) During steps b), d) and f), the Terminal shall not switch off the clock until at least 1 860 clock cycles after having received the last character of the response including the minimum guard time (2 etu).

5) During steps b), d) and f), the Terminal shall wait at least 744 clock cycles before it sends the first command after having restarted the clock.

NOTE: The Terminal will operate at either 1,8 V or 3 V and use the supply voltage procedure if it does not support the first value.

## 6.3 Clock stop mode with 3 V technology UICC

### 6.3.1 Definition and applicability

The Terminal shall be able to receive interface characters, historical bytes and a check byte, even if only T=0 and T=1 are used by the Terminal.

T=15 global interface parameters shall be returned by the UICC.

The UICC shall support the clock stop procedure. The clock stop mode is indicated in TAi (i > 2) in T=15 in the ATR.

For applicability of this test case see clause 3.8.

### 6.3.2 Conformance requirement

#### 6.3.2.0 Description

If the UICC supports any other operating conditions even together with class A, clock stop mode shall be supported and the indication shall be set accordingly. The terminal shall follow this indication independently of operating conditions indicated by the card.

In case the UICC does not support any supply voltage indication, the UICC shall be treated as a 5 V only card by the Terminal.

The Terminal shall wait at least 1 860 clock cycles after having received the last character, including the guard time (2 etu), of the response before it switches off the clock. It shall wait at least 744 clock cycles before it sends the first command after having started the clock.

#### 6.3.2.1 Reference

ETSI TS 102 221 [1], clauses 6.7, 6.10 and 11.1.1.4.6.1.

ISO/IEC 7816‑3 [2], clauses 5.3.4 and 6.5.5.

### 6.3.3 Test purpose

1) To verify that the clock is only switched off as indicated in the ATR first global interface byte and file characteristics (byte 1 of the directory characteristics).

2) To verify that the timing of the clock switching is as specified.

### 6.3.4 Method of test

#### 6.3.4.1 Initial conditions

The Terminal shall be connected to the UICC simulator. PIN shall be enabled.

#### 6.3.4.2 Procedure

a) The Terminal shall be powered on and the UICC simulator shall send an ATR as follows:

| Character | Value | Description |
| --- | --- | --- |
| TS | '3B' | Indicates direct convention |
| T0 | '97' | TA1 and TD1 are present  7 bytes of historical bytes |
| TA1 | '11' | Clock rate conversion factor FI=1 (F=372)  Baud rate adjustment factor DI=1 (D=1) |
| TD1 | '80' | TD2 only is present  Protocol T=0 supported by UICC |
| TD2 | '1F' | TA3 only is present  Global interface bytes following (T=15) |
| TA3 | 'C3' | Clock stop supported (no preferred state)  3 V technology UICC |
| T1 | '80' |  |
| T2 | '31' | Card data services |
| T3 | 'A0' | SELECT by AID supported  EFDIR present |
| T4 | '73' | Card capabilities |
| T5 | 'BE' | SFI supported |
| T6 | '21' | Data Coding Byte |
| T7 | '00' | No extended Lc and Le  No Logical channels supported |
| TCK | '27' | Check byte |

and be used with bits set as follows:

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| b8 | b7 | b6 | b5 | B4 | b3 | b2 | b1 | Meaning |
| 0 | 0 | 1 | 1 | 0 | 0 | 0 | 1 | Voltage classes AB and clock stop mode supported. No preferred level |

b) When the Terminal is in mode PIN check, 10 s shall elapse before the PIN shall be entered.

c) The Terminal shall be powered off and on. The UICC simulator shall send an ATR as follows:

| Character | Value | Description |
| --- | --- | --- |
| TS | '3B' | Indicates direct convention |
| T0 | '97' | TA1 and TD1 are present  7 bytes of historical bytes |
| TA1 | '11' | Clock rate conversion factor FI=1 (F=372)  Baud rate adjustment factor DI=1 (D=1) |
| TD1 | '80' | TD2 only is present  Protocol T=0 supported by UICC |
| TD2 | '1F' | TA3 only is present  Global interface bytes following (T=15) |
| TA3 | '83' | Clock stop supported (high electrical state)  3 V technology UICC |
| T1 | '80' |  |
| T2 | '31' | Card data services |
| T3 | 'A0' | SELECT by AID supported  EFDIR present |
| T4 | '73' | Card capabilities |
| T5 | 'BE' | SFI supported |
| T6 | '21' | Data Coding Byte |
| T7 | '00' | No extended Lc and Le  No Logical channels supported |
| TCK | '67' | Check byte |

and be used with bits set as follows:

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| b8 | b7 | b6 | b5 | b4 | b3 | b2 | b1 | Meaning |
| 0 | 0 | 1 | 1 | 0 | 1 | 0 | 1 | Voltage classes AB and clock stop mode supported. High level preferred |

d) When the Terminal is in mode PIN check, 10 s shall elapse before the PIN shall be entered.

e) The Terminal shall be powered off and on. The UICC simulator shall send an ATR as follows:

|  |  |  |
| --- | --- | --- |
| Character | Value | Description |
| TS | '3B' | Indicates direct convention |
| T0 | '97' | TA1 and TD1 are present  7 bytes of historical bytes |
| TA1 | '11' | Clock rate conversion factor FI=1 (F=372)  Baud rate adjustment factor DI=1 (D=1) |
| TD1 | '80' | TD2 only is present  Protocol T=0 supported by UICC |
| TD2 | '1F' | TA3 only is present  Global interface bytes following (T=15) |
| TA3 | '43' | Clock stop supported (low electrical state)  3 V technology UICC |
| T1 | '80' |  |
| T2 | '31' | Card data services |
| T3 | 'A0' | SELECT by AID supported  EFDIR present |
| T4 | '73' | Card capabilities |
| T5 | 'BE' | SFI supported |
| T6 | '21' | Data Coding Byte |
| T7 | '00' | No extended Lc and Le  No Logical channels supported |
| TCK | 'A7' | Check byte |

and be used with bits set as follows:

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| b8 | b7 | b6 | b5 | b4 | b3 | b2 | b1 | Meaning |
| 0 | 0 | 1 | 1 | 1 | 0 | 0 | 1 | Voltage classes AB and clock stop mode supported. Low level preferred |

f) When the Terminal is in mode PIN check, 10 s shall elapse before the PIN shall be entered.

### 6.3.5 Acceptance criteria

1) During step b), the Terminal shall switch off the clock at either high or low level.

2) During step d), the Terminal shall switch off the clock at high level.

3) During step f), the Terminal shall switch off the clock at low level.

4) During steps b), d) and f), the Terminal shall operate at 3 V and not switch off the clock until at least 1 860 clock cycles after having received the last character of the response including the minimum guard time (2 etu).

5) During steps b), d) and f), the Terminal shall wait at least 744 clock cycles before it sends the first command after having restarted the clock.

## 6.4 Void

## 6.5 Speed enhancement

### 6.5.1 Definition and applicability

The Terminal shall at least support speed enhancement using (F,D) = (512,8) and (512,16) in addition to (372,1), the default.

For applicability of this test case see clause 3.8.

### 6.5.2 Conformance requirement

For the Terminal, it is mandatory to support F = 512 and D = 8 as well as F = 512 and D = 16 (in addition to the default values F = 372 and D = 1).

### 6.5.3 Test purpose

To verify that the Terminal supports the transmission parameters F = 512 and D = 8 as well as F = 512 and D = 16.

### 6.5.4 Method of test

#### 6.5.4.1 Initial conditions

The Terminal is connected to the UICC simulator.

#### 6.5.4.2 Procedure

a) The Terminal is powered on.

b) The UICC simulator sends an ATR as follows:

| Character | Value | Description |
| --- | --- | --- |
| TS | '3B' | Indicates direct convention |
| T0 | '97' | TA1, TD1 are present  7 bytes of historical bytes |
| TA1 | '94' | F=512, D=8 |
| TD1 | '80' | TD2 only is present  T=0 |
| TD2 | '1F' | TA3 only is present  Global interface bytes following |
| TA3 | '46' | Clock stop supported (low electrical state)  1,8 V technology UICC, supporting class B and class C |
| T1 | '80' |  |
| T2 | '31' | Card data services |
| T3 | 'A0' | SELECT by AID supported  EFDIR present |
| T4 | '73' | Card capabilities |
| T5 | 'BE' | SFI supported |
| T6 | '21' | Data Coding Byte |
| T7 | '00' | No extended Lc and Le  No Logical channels supported |
| TCK | '27' | Check byte |

c) After receipt of the PPS Request, the UICC simulator answers with the PPS Response "FF 10 94 7B" using a work waiting time of 9 600 etu (initial waiting time).

d) The UICC simulator transmits with enhanced speed (F = 512, D = 8).

e) The Terminal is switched off and on. The UICC simulator sends an ATR as follows:

| Character | Value | Description |
| --- | --- | --- |
| TS | '3B' | Indicates direct convention |
| T0 | '97' | TA1, TD1 are present  7 bytes of historical bytes |
| TA1 | '95' | F=512, D=16 |
| TD1 | '80' | TD2 only is present  T=0 |
| TD2 | '1F' | TA3 only is present  Global interface bytes following |
| TA3 | '46' | Clock stop supported (low electrical state)  1,8 V technology UICC, supporting class B and class C |
| T1 | '80' |  |
| T2 | '31' | Card data services |
| T3 | 'A0' | SELECT by AID supported  EFDIR present |
| T4 | '73' | Card capabilities |
| T5 | 'BE' | SFI supported |
| T6 | '21' | Data Coding Byte |
| T7 | '00' | No extended Lc and Le  No Logical channels supported |
| TCK | '26' | Check byte |

f) After receipt of the PPS Request, the UICC simulator answers with the PPS Response "FF 10 95 7B" using a work waiting time of 9 600 etu (initial waiting time).

g) The UICC simulator transmits with enhanced speed (F = 512, D = 16).

### 6.5.5 Acceptance criteria

After step b) the Terminal shall send to the UICC simulator the PPS Request "FF 10 94 7B".

After step c) the Terminal shall work with the UICC simulator.

After step e) the Terminal shall send to the UICC simulator the PPS Request "FF 10 95 7B".

After step f) the Terminal shall work with the UICC simulator.

# 7 Transmission protocol tests

## 7.1 Character transmission

### 7.1.1 Bit/character duration during the transmission from the Terminal to the UICC

#### 7.1.1.1 Definition and applicability

A character consists of 10 consecutive bits:

* 1 start bit in state L;
* 8 bits, which comprise the data byte;
* 1 even parity checking bit.

For applicability of this test case see clause 3.8.

#### 7.1.1.2 Conformance requirement

##### 7.1.1.2.0 Description

The bit/character duration and the delay between two consecutive characters (between start leading edges) sent by the Terminal shall be in the range specified.

##### 7.1.1.2.1 Reference

ETSI TS 102 221 [1], clause 7.2.1.

#### 7.1.1.3 Test purpose

To verify the timing during the transmission from the Terminal to the UICC.

#### 7.1.1.4 Method of test

##### 7.1.1.4.1 Initial conditions

The Terminal shall be connected to the UICC simulator, and powered on.

##### 7.1.1.4.2 Procedure

A number of characters are transmitted from the Terminal to the UICC simulator. The UICC simulator shall measure the bit/character duration and the delay between two consecutive characters for all characters transmitted by the Terminal.

#### 7.1.1.5 Acceptance criteria

The timing shall be in the specified range.

### 7.1.2 Bit/character duration during the transmission from the UICC to the Terminal

#### 7.1.2.1 Definition and applicability

A character consists of 10 consecutive bits:

* 1 start bit in state L;
* 8 bits, which comprise the data byte;
* 1 even parity checking bit.

For applicability of this test case see clause 3.8.

#### 7.1.2.2 Conformance requirement

##### 7.1.2.2.0 Description

The bit/character duration and the delay between two consecutive characters (between start leading edges) sent by the Terminal shall be in the range specified.

##### 7.1.2.2.1 Reference

ETSI TS 102 221 [1], clause 7.2.1.

#### 7.1.2.3 Test purpose

To verify the timing during the transmission from the UICC to the Terminal.

#### 7.1.2.4 Method of test

##### 7.1.2.4.1 Initial conditions

The Terminal shall be connected to the UICC simulator, and powered on.

##### 7.1.2.4.2 Procedure

The UICC simulator shall send responses with the maximum and minimum bit/character duration specified in ETSI TS 102 221 [1].

#### 7.1.2.5 Acceptance criteria

The Terminal shall accept the response and act accordingly.

## 7.2 T=0 protocol

### 7.2.1 Timing

#### 7.2.1.1 Definition and applicability

The minimum interval between the leading edge of the start bits of two consecutive characters shall be at least 12 etu. The Work Waiting Time (WWT) is the maximum interval between the start leading edge of any character sent by the UICC and the start leading edge of the previous character sent by either by the UICC or the terminal.

The value of the WWT shall not exceed 960 × WI × Fi/f. WI is an integer received in the specific interface byte TC2. The clock rate conversion factor, Fi, may be indicated in TA1.

For applicability of this test case see clause 3.8.

#### 7.2.1.2 Conformance requirement

##### 7.2.1.2.0 Description

1) If TA1 is absent the Terminal shall use the default value Fi = 372.

2) If no TC2 is available the Terminal shall use the default value of WI (10).

3) The Terminal shall accept characters sent by the UICC with the Work Waiting Time within the specified range.

##### 7.2.1.2.1 Reference

ETSI TS 102 221 [1], clause 7.2.2.1.

#### 7.2.1.3 Test purpose

1) To verify the correct evaluation of the characters TA1 and TC2 indicated in the ATR.

2) To verify that the Terminal accepts the minimum and maximum Work Waiting Time during the transmission from the UICC to the Terminal.

3) To verify that the Terminal deactivates the UICC if WWT is exceeded.

#### 7.2.1.4 Method of test

##### 7.2.1.4.1 Initial conditions

The Terminal shall be connected to the UICC simulator, and powered on.

##### 7.2.1.4.2 Procedure

a) Upon reception of a reset the UICC simulator shall transmit the ATR as follows:

| Character | Value | Description |
| --- | --- | --- |
| TS | '3B' | Indicates direct or inverse convention |
| T0 | '87' | TD1 only is present  7 bytes of historical bytes |
| TD1 | '80' | TD2 only is present |
| TD2 | '1F' | TA3 only is present  Global interface bytes following |
| TA3 | '46' | Clock stop supported (low electrical state)  1,8 V technology UICC |
| T1 | '80' |  |
| T2 | '31' | Card data services |
| T3 | 'A0' | SELECT by AID supported  EFDIR present |
| T4 | '73' | Card capabilities |
| T5 | 'BE' | SFI supported |
| T6 | '21' | Data Coding Byte |
| T7 | '00' | No extended Lc and Le  No Logical channels supported |
| TCK | 'A3' | Check byte |

b) Upon reception of a reset the UICC simulator shall transmit the ATR as follows:

| Character | Value | Description |
| --- | --- | --- |
| TS | '3B' | Indicates direct or inverse convention |
| T0 | '97' | TA1 and TD1 are present  7 bytes of historical bytes |
| TA1 | '11' | Clock rate conversion factor FI=1 (F=372)  Baud rate adjustment factor DI=1 (D=1) |
| TD1 | 'C0' | TC2 and TD2 are present |
| TC2 | '01' | WI=1 meaning WWT=960x(Fi/f)x1 |
| TD2 | '1F' | TA3 only is present  Global interface bytes following |
| TA3 | '46' | Clock stop supported (low electrical state)  1,8 V technology UICC |
| T1 | '80' |  |
| T2 | '31' | Card data services |
| T3 | 'A0' | SELECT by AID supported  EFDIR present |
| T4 | '73' | Card capabilities |
| T5 | 'BE' | SFI supported |
| T6 | '21' | Data Coding Byte |
| T7 | '00' | No extended Lc and Le  No Logical channels supported |
| TCK | 'E3' | Check byte |

c-1) The UICC simulator shall transmit with a WWT of 12 etu.

c-2) The UICC simulator shall transmit with the specified WWT (960 × (Fi/f) × WI).

c-3) The UICC simulator shall not transmit i.e. WWT exceeded.

#### 7.2.1.5 Acceptance criteria

In step a), the Terminal shall work with the UICC simulator using the default values of TA1 and TC2.

In steps c-1) and c-2) the Terminal shall work with the UICC simulator.

In step c-3) the Terminal shall initiate a deactivation of the UICC within 960 etu following the excess of WWT.

### 7.2.2 Command processing, ACK, NACK, NULL procedure bytes

#### 7.2.2.1 Definition and applicability

Procedure bytes are used to keep up the communication between the terminal and the UICC. They shall not be transmitted to the Application Layer.

The status bytes SW1 SW2 form an end sequence indicating the status of the UICC at the end of a command.

For applicability of this test case see clause 3.8.

#### 7.2.2.2 Conformance requirement

##### 7.2.2.2.0 Description

The Terminal shall correctly use the different modes of data transmission.

##### 7.2.2.2.1 Reference

ETSI TS 102 221 [1], clause 7.2.2.3.

ISO/IEC 7816‑3 [2], clause 8.3.

#### 7.2.2.3 Test purpose

To verify that the Terminal correctly uses the different modes of data transmission.

#### 7.2.2.4 Method of test

##### 7.2.2.4.1 Initial conditions

The Terminal shall be connected to the UICC simulator, and powered on.

T=0 ATR shall have been received and eventual PPS procedure successfully completed.

##### 7.2.2.4.2 Procedure

a) The Terminal shall be made to initiate a VERIFY PIN command with 8 bytes of data.

b) The UICC simulator shall answer the first 5 bytes with ACK=INS complemented.

c1) The UICC simulator shall answer the next data byte with NULL (NULL="60"). This byte is sent between 0.8 and 1.0 x Work Waiting Time after the previous procedure byte.

c2) The UICC simulator shall send a second NULL (NULL="60"). This byte is sent between 0.8 and 1.0 x Work Waiting Time after the previous procedure byte.

c3) The UICC simulator shall send a third NULL (NULL="60"). This byte is sent between 0.8 and 1.0 x Work Waiting Time after the previous procedure byte.

d) The UICC simulator shall then send ACK=INS. This byte is sent between 0.8 and 1.0 x Work Waiting Time after the previous procedure byte.

e) The UICC simulator shall answer the transmission of the rest of the data with NULL.

f) The UICC simulator shall then send SW1 and SW2, indicating correct execution of the command ("90" and "00" for SW1 and SW2 respectively). These bytes are sent when the elapsed time since step d) is greater than the Work Waiting Time.

#### 7.2.2.5 Acceptance criteria

The command shall be executed correctly.

### 7.2.3 Case 2 command, use of procedure bytes '61xx' and '6Cxx'

#### 7.2.3.1 Definition and applicability

Procedure bytes '61XX' and '6CXX' are returned by the UICC to control exchanges between the Transport Layer of the Terminal and the UICC, and should never be returned to the Application Layer of the Terminal. Command processing in the UICC is not complete if it has returned procedure bytes '61XX' or '6CXX'.

For applicability of this test case see clause 3.8.

#### 7.2.3.2 Conformance requirement

##### 7.2.3.2.0 Description

The UICC returns procedure bytes '61xx 'and '6Cxx' to the Transport Layer of the Terminal to indicate to it the manner in which it should retrieve the data requested by the command currently being processed. These procedure bytes are only used when processing case 2 and 4 commands using T=0.

##### 7.2.3.2.1 Reference

ETSI TS 102 221 [1], clause 7.3.1.1.5.

ISO/IEC 7816‑3 [2], clause 8.3.

#### 7.2.3.3 Test purpose

To verify that the Terminal correctly handles the procedure bytes '61XX' and '6CXX' when processing a case 2 command.

#### 7.2.3.4 Method of test

##### 7.2.3.4.1 Initial conditions

The Terminal shall be connected to the UICC simulator, and powered on.

T=0 ATR shall have been received and eventual PPS procedure successfully completed.

##### 7.2.3.4.2 Procedure

a) The Terminal shall be made to initiate a case 2 command with Le > Luicc (ex: READ RECORD command).

b) The UICC simulator shall send '6CLuicc' procedure bytes.

c) Following receipt of the command, the UICC simulator shall send '61xx' procedure bytes.

d) Following receipt of the command, the UICC simulator shall send corresponding data + '61yy' procedure bytes.

e) Following receipt of the command, the UICC simulator shall then send the rest of the data and SW1 and SW2, indicating correct execution of the command ("90" and "00" for SW1 and SW2 respectively).

#### 7.2.3.5 Acceptance criteria

After step b) the Terminal shall send the previous command with Le = 'Luicc'.

After step c) the Terminal shall send a GET RESPONSE command with Le = 'xx'.

After step f) the Terminal shall send a GET RESPONSE command with Le = 'yy'.

### 7.2.4 Case 4 command, use of procedure bytes '61xx'

#### 7.2.4.1 Definition and applicability

Procedure bytes '61XX' and '6CXX' are returned by the UICC to control exchanges between the Transport Layer of the Terminal and the UICC, and should never be returned to the Application Layer of the Terminal. Command processing in the UICC is not complete if it has returned procedure bytes '61XX' or '6CXX'.

For applicability of this test case see clause 3.8.

#### 7.2.4.2 Conformance requirement

##### 7.2.4.2.0 Description

The UICC returns procedure bytes '61xx' and '6Cxx' to the Transport Layer of the Terminal to indicate to it the manner in which it should retrieve the data requested by the command currently being processed. These procedure bytes are only used when processing case 2 and 4 commands using T=0.

##### 7.2.4.2.1 Reference

ETSI TS 102 221 [1], clause 7.3.1.1.5.

ISO/IEC 7816‑3 [2], clause 8.3.

#### 7.2.4.3 Test purpose

To verify that the Terminal correctly handles the procedure bytes '61XX' when processing a case 4 command.

#### 7.2.4.4 Method of test

##### 7.2.4.4.1 Initial conditions

The Terminal shall be connected to the UICC simulator, and powered on.

T=0 ATR shall have been received and eventual PPS procedure successfully completed.

##### 7.2.4.4.2 Procedure

a) The Terminal shall be made to initiate a case 4 command with Le > Luicc (ex: SELECT command).

b) The UICC simulator shall answer the command header with INS and send '61xx' procedure bytes following reception of data.

c) Following receipt of the command, the UICC simulator shall send corresponding data + '61yy' procedure bytes.

d) Following receipt of the command, the UICC simulator shall then send the rest of the data and SW1 and SW2, indicating correct execution of the command ("90" and "00" for SW1 and SW2 respectively).

#### 7.2.4.5 Acceptance criteria

After step b) the Terminal shall send a GET RESPONSE command with Le = 'xx'.

After step c) the Terminal shall send a GET RESPONSE command with Le = 'yy'.

### 7.2.5 Command processing, warning and error status bytes

#### 7.2.5.1 Definition and applicability

The status bytes SW1 SW2 form an end sequence indicating the status of the UICC at the end of a command.

For applicability of this test case see clause 3.8.

#### 7.2.5.2 Conformance requirement

##### 7.2.5.2.0 Description

In the case of an error, the UICC may return status indicating error or warning conditions instead of the '61xx' or '6Cxx' response.

##### 7.2.5.2.1 Reference

ETSI TS 102 221 [1], clauses 7.2.2.3 and 10.2.1.

#### 7.2.5.3 Test purpose

To verify that the Terminal correctly handles status bytes different than '9000'.

#### 7.2.5.4 Method of test

##### 7.2.5.4.1 Initial conditions

The Terminal shall be connected to the UICC simulator, and powered on.

T=0 ATR shall have been received and eventual PPS procedure successfully completed.

##### 7.2.5.4.2 Procedure

a) Warning:

a-1) The Terminal shall be made to initiate a case 4 command (ex: SELECT command).

a-2) The UICC simulator shall send warning status bytes ('62xx' '63xx' or '9xxx').

a-3) Following receipt of the command, the UICC simulator shall then send the rest of the data and SW1 and SW2, indicating correct execution of the command ("90" and "00" for SW1 and SW2 respectively).

b) Error:

b-1) The Terminal shall be made to initiate a case 4 command (ex: SELECT command).

b-2) The UICC simulator shall send error status bytes ('6xxx' except '6Cxx', '61xx', '62xx' and '63xx').

#### 7.2.5.5 Acceptance criteria

After step a-2) the Terminal shall send a GET RESPONSE command with Le = '00'.

After step b-2) the Terminal shall discontinue processing of the command.

### 7.2.6 Error correction

#### 7.2.6.1 Definition and applicability

If the UICC as receiver detects a parity error within 11 etu ± 0,2 etu starting from the leading edge of the start bit, in a character just received, it shall set I/O to state L to indicate the error to the Terminal.

For applicability of this test case see clause 3.8.

#### 7.2.6.2 Conformance requirement

##### 7.2.6.2.0 Description

The error detection and correction procedure is mandatory for T=0 protocol except for the Terminal during the ATR‑procedure.

##### 7.2.6.2.1 Reference

ETSI TS 102 221 [1], clause 7.2.2.4.

#### 7.2.6.3 Test purpose

To verify the error handling during the transmission from the Terminal to the UICC.

#### 7.2.6.4 Method of test

##### 7.2.6.4.1 Initial conditions

The Terminal shall be connected to the UICC simulator, and powered on.

##### 7.2.6.4.2 Procedure

The UICC simulator shall transmit an error signal in response to a received character by setting the I/O line to state L for a maximum of 2 etu and a minimum of 1 etu, 10,5 etu ± 0,2 etu after the leading edge of the start bit of the received character.

#### 7.2.6.5 Acceptance criteria

The Terminal shall repeat the disputed character after a minimum delay of 2 etu.

### 7.2.7 Error detection

#### 7.2.7.1 Definition and applicability

If the Terminal as receiver detects a parity error within 11 ± 0,2 etu starting from the leading edge of the start bit, in a character just received, it shall set I/O to state L to indicate the error to the UICC.

For applicability of this test case see clause 3.8.

#### 7.2.7.2 Conformance requirement

##### 7.2.7.2.0 Description

The error detection and correction procedure is mandatory for T=0 protocol except for the Terminal during the ATR‑procedure.

##### 7.2.7.2.1 Reference

ETSI TS 102 221 [1], clause 7.2.2.4.

#### 7.2.7.3 Test purpose

To verify the error handling during the transmission from the UICC to the Terminal.

#### 7.2.7.4 Method of test

##### 7.2.7.4.1 Initial conditions

The Terminal shall be connected to the UICC simulator, and powered on.

##### 7.2.7.4.2 Procedure

The UICC simulator shall send a response with a parity error and check that the terminals correctly handles it.

#### 7.2.7.5 Acceptance criteria

The Terminal shall detect the parity error by setting the I/O line to state L for a maximum of 2 etu and a minimum of 1 etu, 10,5 etu ± 0,2 etu after the leading edge of the start bit of the erroneous character and correctly evaluate the character when repeated by the UICC simulator.

## 7.3 T=1 protocol

### 7.3.1 Character Waiting Time

#### 7.3.1.1 Definition and applicability

CWT is defined as the maximum delay between the leading edges of two consecutive characters in the block.

For applicability of this test case see clause 3.8.

#### 7.3.1.2 Conformance requirement

##### 7.3.1.2.0 Description

CWI is used to calculate CWT and shall be in the range from 0 to 5. The value is set in bits b4 to b1 in TB3. The value of CWT may be calculated from the following equation: CWT = (11 + 2CWI) etu.

##### 7.3.1.2.1 Reference

ETSI TS 102 221 [], clause 7.2.3.1.

ISO/IEC 7816‑3 [2], clause 9.5.3.

#### 7.3.1.3 Test purpose

To verify that the Terminal respects the CWT indicated by the UICC.

#### 7.3.1.4 Method of test

##### 7.3.1.4.1 Initial conditions

The Terminal shall be connected to the UICC simulator, and powered on.

##### 7.3.1.4.2 Procedure

a) Upon reception of a reset the UICC simulator shall transmit the ATR as follows:

| Character | Value | Description |
| --- | --- | --- |
| TS | '3B' | Indicates direct convention |
| T0 | '97' | TA1, and TD1 are present  7 bytes of historical bytes |
| TA1 | '11' | Clock rate conversion factor FI=1 (F=372)  Baud rate adjustment factor DI=1 (D=1) |
| TD1 | '81' | Only TD2 is present  Protocol T=1 supported by UICC |
| TD2 | 'A1' | TB3 and TD3 are present  Protocol T=1 supported by UICC |
| TB3 | '05' | Block Waiting Integer=0  Character Waiting Integer=5 indicating CWT=43 etu |
| TD3 | '1F' | Only TA4 is present  Global interface bytes following (T=15) |
| TA4 | '46' | Clock stop supported (low electrical state)  1,8 V technology UICC |
| T1 | '80' |  |
| T2 | '31' | Card data services |
| T3 | 'A0' | SELECT by AID supported  EFDIR present |
| T4 | '73' | Card capabilities |
| T5 | 'BE' | SFI supported |
| T6 | '21' | Data Coding Byte |
| T7 | '00' | No extended Lc and Le  No Logical channels supported |
| TCK | '07' | Check byte |

b) Following receipt of the first block by the UICC simulator, the Terminal shall be made to initiate a command requiring reception of an I-Block.

b-1) The UICC simulator shall send the I-Block (data + '9000' indicating correct execution of the command) using CWT=11 etu.

b-2) The UICC simulator shall send the I-Block (data + '9000' indicating correct execution of the command) using CWT=43 etu.

#### 7.3.1.5 Acceptance criteria

In step b.1) and b.2) the Terminal shall acknowledge the error free I-Block.

### 7.3.2 Block Timing

#### 7.3.2.1 Definition and applicability

BWT is defined as the maximum delay between the leading edge of the last character of the block received by the card and the leading edge of the first character of the next block sent by the card.

BGT is defined as the minimum delay between the leading edge of two consecutive characters sent in opposite directions. The value of BGT shall be 22 etu.

For applicability of this test case see clause 3.8.

#### 7.3.2.2 Conformance requirement

##### 7.3.2.2.0 Description

BWI is used to calculate BWT and shall be in the range from 0 to 4. The value is set in bits b5 to b8 in TB3. The value of BWT may be calculated from the following equation: BWT = 11 + (2BWI × 960 × 372/f) etu.

The delay between the last character of a block received by the UICC and the first character of the next block sent from the UICC shall be in the interval: BGT < delay < BWT.

##### 7.3.2.2.1 Reference

ETSI TS 102 221 [1], clause 7.2.3.

ISO/IEC 7816‑3 [2], clause 9.5.3.

#### 7.3.2.3 Test purpose

To verify that the Terminal respects the BGT and BWT indicated by the UICC in the ATR and detects time-out.

#### 7.3.2.4 Method of test

##### 7.3.2.4.1 Initial conditions

The Terminal shall be connected to the UICC simulator, and powered on.

##### 7.3.2.4.2 Procedure

a) Upon reception of a reset the UICC simulator shall transmit the ATR as follows:

| Character | Value | Description |
| --- | --- | --- |
| TS | '3B' | Indicates direct convention |
| T0 | '97' | TA1, and TD1 are present  7 bytes of historical bytes |
| TA1 | '11' | Clock rate conversion factor FI=1 (F=372)  Baud rate adjustment factor DI=1 (D=1) |
| TD1 | '81' | Only TD2 is present  Protocol T=1 supported by UICC |
| TD2 | 'A1' | TB3 and TD3 are present  Protocol T=1 supported by UICC |
| TB3 | '31' | Block Waiting Integer=3 indicating BWT = 11 + (8 × 960 × 372 / f) etu  Character Waiting Integer=1 indicating CWT=13 etu |
| TD3 | '1F' | Only TA4 is present  Global interface bytes following |
| TA4 | '46' | Clock stop supported (low electrical state)  1,8 V technology UICC |
| T1 | '80' |  |
| T2 | '31' | Card data services |
| T3 | 'A0' | SELECT by AID supported  EFDIR present |
| T4 | '73' | Card capabilities |
| T5 | 'BE' | SFI supported |
| T6 | '21' | Data Coding Byte |
| T7 | '00' | No extended Lc and Le  No Logical channels supported |
| TCK | '33' | Check byte |

b) Following receipt of the first block by the UICC simulator, the Terminal shall be made to initiate a command requiring reception of chained I-Blocks.

c) The UICC simulator shall measure the delay between the last character of each block sent by the UICC and the first character of each following block sent by the Terminal.

d) BWT:

d-1) The UICC simulator shall send the I-Blocks using BGT = 22 etu.

d-2) The UICC simulator shall send each I-Block using BWT = 11 + (2BWI × 960 × 372/f) etu.

BWT excess:

d-3) The UICC simulator shall not send an I-Block.

#### 7.3.2.5 Acceptance criteria

In step c) the Terminal shall use a BGT of at least 22 etus.

In steps d-1) and d-2) the Terminal shall acknowledge reception of the I-Blocks without error.

In step d-3) the Terminal shall detect a time-out and send an R-Block requesting retransmission of the last block.

### 7.3.3 Block Waiting Time extension

#### 7.3.3.1 Definition and applicability

WTX is a parameter used to ask for more time to process a command.

Supervisory blocks, S-block, are used to send control information.

S-blocks are always used in pairs. A S(request) is always followed by a S(response) block.

* S(WTX request), a request for an extension of the waiting time;
* S(WTX response), an acknowledge of the extension of the waiting time.

For applicability of this test case see clause 3.8.

#### 7.3.3.2 Conformance requirement

##### 7.3.3.2.0 Description

The UICC might need more than BWT to process the previously received block, a S(WTX request) is sent by the UICC. The terminal shall acknowledge with a S(WTX response).

When an S(… request) has been sent and either a BWT time-out occurs (with the terminal) or the received response is not a S(… response), the S(… request) shall be resent.

##### 7.3.3.2.1 Reference

ETSI TS 102 221 [1], clause 7.2.3.1.

ISO/IEC 7816‑3 [2], clauses 9.5.3 and 9.7.3, scenarios 2, 14 and 15.

#### 7.3.3.3 Test purpose

1) To verify that the Terminal respects the WTX procedure and applies the extended BWT.

2) To verify that the Terminal handles the different types of errors in S(... request).

#### 7.3.3.4 Method of test

##### 7.3.3.4.1 Initial conditions

The Terminal shall be connected to the UICC simulator, and powered on.

##### 7.3.3.4.2 Procedure

a) Upon reception of a reset the UICC simulator shall transmit the ATR as follows:

| Character | Value | Description |
| --- | --- | --- |
| TS | '3B' | Indicates direct convention |
| T0 | '97' | TA1, and TD1 are present  7 bytes of historical bytes |
| TA1 | '11' | Clock rate conversion factor FI=1 (F=372)  Baud rate adjustment factor DI=1 (D=1) |
| TD1 | '81' | Only TD2 is present  Protocol T=1 supported by UICC |
| TD2 | 'A1' | TB3 and TD3 are present  Protocol T=1 supported by UICC |
| TB3 | '21' | Block Waiting Integer=2 indicating BWT = 11 + (4 × 960 × 372/f) etu  Character Waiting Integer=1 indicating CWT=13 etu |
| TD3 | '1F' | Only TA4 is present  Global interface bytes following |
| TA4 | '46' | Clock stop supported (low electrical state)  1,8 V technology UICC |
| T1 | '80' |  |
| T2 | '31' | Card data services |
| T3 | 'A0' | SELECT by AID supported  EFDIR present |
| T4 | '73' | Card capabilities |
| T5 | 'BE' | SFI supported |
| T6 | '21' | Data Coding Byte |
| T7 | '00' | No extended Lc and Le  No Logical channels supported |
| TCK | '23' | Check byte |

b) Following receipt of the first block by the UICC simulator, the Terminal shall be made to initiate a command requiring exchange of I-Blocks.

c-1) Error free S(WTX request):

c-1-1) Following receipt of the I-block, the UICC simulator shall send a S(WTX request) without error (BWT multiplied by 2).

c-1-2) The UICC simulator shall use the extended BWT when receiving the S(WTX response), then complete the command (data + '9000' indicating correct execution of the command).

c-2) Error in S(WTX request):

c-2-1) Following receipt of the I-block, the UICC simulator shall send a S(WTX request) and generate the following errors:

- Parity error.

- NAD ≠ '00'.

- S(WTX response) instead of S(WTX request).

- Other S(.... response) instead of S(WTX request).

- LEN error.

c-2-2) Following reception of the block sent by the Terminal (correct or with error assumed) the UICC simulator shall retransmit the S(WTX request) without error.

c-2-3) The UICC simulator shall use the extended BWT when receiving the S(WTX response), then complete the command (data + '9000' indicating correct execution of the command).

#### 7.3.3.5 Acceptance criteria

After steps c-1-1) and c-2-2) the Terminal shall send a S(WTX response).

After step c-2-1) the Terminal shall send an R-Block requesting retransmission of the last block.

### 7.3.4 Chaining - Respect of IFSC by Terminal

#### 7.3.4.1 Definition and applicability

Chaining allows the terminal or the UICC to transfer information, which is longer than IFSC or IFSD. If information longer than IFSC or IFSD is transferred, the information should be divided into pieces, each has a length ≤ IFSC or IFSD. Each piece should be sent in an I-block using the chaining function.

The IFSC defines the maximum length of the information field of blocks that can be received by the UICC.

For applicability of this test case see clause 3.8.

#### 7.3.4.2 Conformance requirement

##### 7.3.4.2.0 Description

The default value of the IFSC is 32 bytes. Another value may be indicated in TA3 of the ATR.

When the terminal is the sender, all I-blocks of a chain shall have LEN = IFSC bytes except for the last, which could have a value in the range of 0 to IFSC.

When a receiver receives a more-data I-block, a R(N(R)) shall be sent. N(R) = N(S) of the expected I-block. At least one chained block should follow.

##### 7.3.4.2.1 Reference

ETSI TS 102 221 [1], clauses 7.2.3.1.1 and 7.2.3.5.

ISO/IEC 7816‑3 [2], clause 9.7.3, scenarios 5 and 6.

#### 7.3.4.3 Test purpose

To verify that the Terminal respects the Information Field Size of the UICC in chaining mode.

#### 7.3.4.4 Method of test

##### 7.3.4.4.1 Initial conditions

The Terminal shall be connected to the UICC simulator, and powered on.

##### 7.3.4.4.2 Procedure

a) No TA3.

a-1) Upon reception of a reset the UICC simulator shall transmit the ATR as follows:

| Character | Value | Description |
| --- | --- | --- |
| TS | '3B' | Indicates direct convention |
| T0 | '97' | TA1, and TD1 are present  7 bytes of historical bytes |
| TA1 | '11' | Clock rate conversion factor FI=1 (F=372)  Baud rate adjustment factor DI=1 (D=1) |
| TD1 | '81' | Only TD2 is present  Protocol T=1 supported by UICC |
| TD2 | 'A1' | TB3 and TD3 are present  Protocol T=1 supported by UICC |
| TB3 | '00' | Block Waiting Integer=0  Character Waiting Integer=0 |
| TD3 | '1F' | Only TA4 is present  Global interface bytes following |
| TA4 | '46' | Clock stop supported (low electrical state)  1,8 V technology UICC |
| T1 | '80' |  |
| T2 | '31' | Card data services |
| T3 | 'A0' | SELECT by AID supported  EFDIR present |
| T4 | '73' | Card capabilities |
| T5 | 'BE' | SFI supported |
| T6 | '21' | Data Coding Byte |
| T7 | '00' | No extended Lc and Le  No Logical channels supported |
| TCK | '02' | Check byte |

a-2) Following receipt of the first block by the UICC simulator, the Terminal shall be made to initiate a command requiring sending of chained I-Blocks.

a-3) Following receipt of the command, the UICC simulator shall evaluate the length and acknowledge reception of the received I-Blocks without error.

b) TA3='FE'

b-1) Upon reception of a reset the UICC simulator shall transmit the ATR as follows:

| Character | Value | Description |
| --- | --- | --- |
| TS | '3B' | Indicates direct convention |
| T0 | '97' | TA1, and TD1 are present  7 bytes of historical bytes |
| TA1 | '11' | Clock rate conversion factor FI=1 (F=372)  Baud rate adjustment factor DI=1 (D=1) |
| TD1 | '81' | Only TD2 is present  Protocol T=1 supported by UICC |
| TD2 | 'B1' | TA3, TB3 and TD3 are present  Protocol T=1 supported by UICC |
| TA3 | 'FE' | IFSC is 254 bytes long |
| TB3 | '00' | Block Waiting Integer=0  Character Waiting Integer=0 |
| TD3 | '1F' | Only TA4 is present  Global interface bytes following |
| TA4 | '46' | Clock stop supported (low electrical state)  1,8 V technology UICC |
| T1 | '80' |  |
| T2 | '31' | Card data services |
| T3 | 'A0' | SELECT by AID supported  EFDIR present |
| T4 | '73' | Card capabilities |
| T5 | 'BE' | SFI supported |
| T6 | '21' | Data Coding Byte |
| T7 | '00' | No extended Lc and Le  No Logical channels supported |
| TCK | 'EC' | Check byte |

b-2) Following receipt of the first block by the UICC simulator, the Terminal shall be made to initiate a command requiring sending of chained I-Blocks.

b-3) Following receipt of the command, the UICC simulator shall evaluate the length and acknowledge reception of the received I-Blocks without error.

#### 7.3.4.5 Acceptance criteria

In step a-2) the Terminal shall send the chained I-Blocks, except the last one, using the default value of IFSC, i.e. 32 bytes long information field.

In step b-2) the Terminal shall send the chained I-Blocks, except the last one, using the specified value of IFSC, i.e. 254 bytes long information field.

### 7.3.5 Chaining - IFSD management

#### 7.3.5.1 Definition and applicability

Chaining allows the Terminal or the UICC to transfer information, which is longer than IFSC or IFSD. If information longer than IFSC or IFSD is transferred, the information should be divided into pieces, each has a length ≤ IFSC or IFSD. Each piece should be sent in an I-block using the chaining function.

When a receiver receives a more-data I-block, a R(N(R)) shall be sent. N(R) = N(S) of the expected I-block. At least one chained block should follow.

The IFSD defines the maximum length of the information field of blocks that the terminal can receive.

The default value of the IFSD is 32 bytes and may be adjusted during the card session. The maximum value of the IFSD is 254 bytes.

For applicability of this test case see clause 3.8.

#### 7.3.5.2 Conformance requirement

##### 7.3.5.2.0 Description

When the UICC is the sender, all I-blocks of a chain shall have LEN ≤ IFSD bytes per block.

##### 7.3.5.2.1 Reference

ETSI TS 102 221 [1], clause 7.2.3.

#### 7.3.5.3 Test purpose

To verify that the Terminal correctly handles the Information Field Size in chaining mode.

#### 7.3.5.4 Method of test

##### 7.3.5.4.1 Initial conditions

The Terminal shall be connected to the UICC simulator, and powered on.

ATR shall have been received and eventual PPS procedure successfully completed.

##### 7.3.5.4.2 Procedure

a) Following receipt of the first block by the UICC simulator, the Terminal shall be made to initiate a command requiring reception of chained I-Blocks.

b) The UICC simulator shall send an I-Block with LEN > IFSD.

c) Following correct receipt of the next block the UICC simulator shall send the rest of I-Blocks (data + '9000' indicating correct execution of the command).

#### 7.3.5.5 Acceptance criteria

In step b), the Terminal shall detect the incorrect LEN and send an R-Block requesting retransmission of the last block.

In step c) the Terminal shall acknowledge reception of the I-Blocks without error by sending R-Blocks with N(R)=sequence number of expected I-Block.

### 7.3.6 I-Block error correction

#### 7.3.6.1 Definition and applicability

Information blocks are used to transfer command and response APDUs.

The I-blocks are denoted as follows: I(N(S), M) where:

* N(S) is the send-sequence number of the block;
* M is the more-data bit used in the chaining function.

For applicability of this test case see clause 3.8.

#### 7.3.6.2 Conformance requirement

##### 7.3.6.2.0 Description

When an I-block has been sent and a BWT time-out occurs or an invalid block has been received (with the terminal), an R-block is sent, which requests with its N(R) for the expected I-block with N(S)=N(R).

##### 7.3.6.2.1 Reference

ETSI TS 102 221 [1], clause 7.2.3.4.

ISO/IEC 7816‑3 [2], clause 9.7.3, scenario 8.

#### 7.3.6.3 Test purpose

To verify that the Terminal sends an I-Block again when notified incorrect reception by the UICC (R-Block meaning error).

#### 7.3.6.4 Method of test

##### 7.3.6.4.1 Initial conditions

The Terminal shall be connected to the UICC simulator, and powered on.

ATR shall have been received and eventual PPS procedure successfully completed.

##### 7.3.6.4.2 Procedure

a) Following receipt of the first block by the UICC simulator, the Terminal shall be made to initiate a command requiring sending of chained I-Blocks.

b) The UICC simulator shall assume each transmitted I-Block, including the last non-chained one, is invalid by sending an R-Block requesting retransmission.

#### 7.3.6.5 Acceptance criteria

In step b), the Terminal shall resend each disputed I-Block.

### 7.3.7 I-Block error detection

#### 7.3.7.1 Definition and applicability

Information blocks are used to transfer command and response APDUs.

The I-blocks are denoted as follows: I(N(S), M) where:

* N(S) is the send-sequence number of the block;
* M is the more-data bit used in the chaining function.

For applicability of this test case see clause 3.8.

#### 7.3.7.2 Conformance requirement

##### 7.3.7.2.0 Description

When an I-block has been sent and a BWT time-out occurs or an invalid block has been received (with the terminal), an R-block is sent, which requests with its N(R) for the expected I-block with N(S)=N(R).

##### 7.3.7.2.1 Reference

ETSI TS 102 221 [1], clause 7.2.3.4.

ISO/IEC 7816‑3 [2], clause 9.7.3, scenario 9.

#### 7.3.7.3 Test purpose

To verify that the Terminal correctly handles the different types of invalid I-Blocks.

#### 7.3.7.4 Method of test

##### 7.3.7.4.1 Initial conditions

The Terminal shall be connected to the UICC simulator, and powered on.

ATR shall have been received and eventual PPS procedure successfully completed.

##### 7.3.7.4.2 Procedure

a) Following receipt of the first block by the UICC simulator, the Terminal shall be made to initiate a command requiring reception of I-Blocks.

b) The UICC simulator shall send I-Blocks and generate the following errors:

- Parity error.

- NAD ≠ '00'.

- PCB with wrong sequence number.

- PCB of an R-Block.

- PCB of an S-Block.

- LEN error (= 'FF').

- EDC error.

c) Following correct reception of the block sent by the Terminal, the UICC simulator shall retransmit the I-Block without error and complete the command (data + '9000' indicating correct execution of the command).

NOTE: Test can be achieved either by generating the errors in one session using chained blocks or through separate tests generating one error.

#### 7.3.7.5 Acceptance criteria

In step b), the Terminal shall detect the invalid block and send an R-Block requesting retransmission of the last block (N(R)=sequence number of last I-Block).

In step c) the Terminal shall acknowledge reception of the I-Block without error.

### 7.3.8 R-Block error handling in non-chaining mode

#### 7.3.8.1 Definition and applicability

Receive-ready blocks, R-blocks, are used to transfer acknowledgements.

The R-blocks are denoted as follows: R(N(R)), where:

- N(R) is the number of the expected I-block.

For applicability of this test case see clause 3.8.

#### 7.3.8.2 Conformance requirement

##### 7.3.8.2.0 Description

When an R-block was sent and an invalid block is received or BWT time-out, the R-block will be resent.

##### 7.3.8.2.1 Reference

ETSI TS 102 221 [1], clause 7.2.3.4.

ISO/IEC 7816‑3 [2], clause 9.7.3, scenario 10.

#### 7.3.8.3 Test purpose

To verify that the Terminal handles the different types of invalid R-Blocks and correctly recovers while sending non chained data.

#### 7.3.8.4 Method of test

##### 7.3.8.4.1 Initial conditions

The Terminal shall be connected to the UICC simulator, and powered on.

ATR shall have been received and eventual PPS procedure successfully completed.

##### 7.3.8.4.2 Procedure

a) Following receipt of the first block by the UICC simulator, the Terminal shall be made to initiate a command requiring sending of a non chained I-Block.

b) The UICC simulator shall assume the received block is invalid by sending an R-Block and generate the following errors:

- Parity error.

- NAD ≠ '00'.

- PCB with wrong sequence number.

- PCB with b6=1.

- PCB of an S-Block.

- LEN error.

- EDC error.

c) Following correct reception of the block sent by the Terminal, the UICC simulator shall retransmit the R‑Block without error.

#### 7.3.8.5 Acceptance criteria

In step b) the Terminal shall detect the invalid block and send an R-Block requesting retransmission of the last block (N(R)=sequence number of invalid R-Block).

After step c), the Terminal shall resend the first I-Block.

### 7.3.9 R-Block error handling in chaining mode

#### 7.3.9.1 Definition and applicability

Receive-ready blocks, R-blocks, are used to transfer acknowledgements.

The R-blocks are denoted as follows: R(N(R)), where:

- N(R) is the number of the expected I-block.

For applicability of this test case see clause 3.8.

#### 7.3.9.2 Conformance requirement

##### 7.3.9.2.0 Description

When an R-block was sent and an invalid block is received or BWT time-out, the R-block will be resent.

##### 7.3.9.2.1 Reference

ETSI TS 102 221 [1], clause 7.2.3.4.

ISO/IEC 7816‑3 [2], clause 9.7.3, scenario 21.

#### 7.3.9.3 Test purpose

To verify that the Terminal handles the different types of invalid R-Blocks and correctly recovers while sending chained data.

#### 7.3.9.4 Method of test

##### 7.3.9.4.1 Initial conditions

The Terminal shall be connected to the UICC simulator, and powered on.

ATR shall have been received and eventual PPS procedure successfully completed.

##### 7.3.9.4.2 Procedure

a) Following receipt of the first block by the UICC simulator, the Terminal shall be made to initiate a command requiring sending of chained I-Blocks.

b) The UICC simulator shall send an invalid R-Block and generate the following errors:

- Parity error.

- NAD ≠ '00'.

- PCB with b6=1.

- PCB of an S-Block.

- LEN error.

- EDC error.

c) Following correct reception of the block sent by the Terminal, the UICC simulator shall retransmit the R‑Block without error.

#### 7.3.9.5 Acceptance criteria

In step b) the Terminal shall detect the invalid block and send an R-Block requesting retransmission of the last block (N(R)=sequence number of invalid R-Block).

After step c), the Terminal shall send the rest of chained data (I-Block).

### 7.3.10 Successive errors in both directions

#### 7.3.10.1 Definition and applicability

Receive-ready blocks, R-blocks, are used to transfer acknowledgements.

The R-blocks are denoted as follows: R(N(R)), where:

* N(R) is the number of the expected I-block.

For applicability of this test case see clause 3.8.

#### 7.3.10.2 Conformance requirement

##### 7.3.10.2.0 Description

When an R-block was sent and an invalid block is received or BWT time-out, the R-block will be resent.

##### 7.3.10.2.1 Reference

ETSI TS 102 221 [1], clause 7.2.3.4.

ISO/IEC 7816‑3 [2], clause 9.7.3, scenarios 12 and 13.

#### 7.3.10.3 Test purpose

To verify that the Terminal properly recovers after receiving and being notified errors successively.

#### 7.3.10.4 Method of test

##### 7.3.10.4.1 Initial conditions

The Terminal shall be connected to the UICC simulator, and powered on.

ATR shall have been received and eventual PPS procedure successfully completed.

##### 7.3.10.4.2 Procedure

a) Following receipt of the first block by the UICC simulator, the Terminal shall be made to initiate a command requiring reception of I-Blocks.

b) The UICC simulator shall send an invalid I-Block.

c) Following correct reception of the block sent by the Terminal, the UICC simulator shall assume the received block is invalid by sending an R-Block, also invalid.

d) Following correct reception of the block sent by the Terminal:

d-1) No error:

d-1-1) The UICC simulator shall retransmit the I-Block without error and complete the command (data + '9000' indicating correct execution of the command).

d-2) Error assumed:

d-2-1) The UICC simulator shall assume the received block is invalid by sending an R-Block requesting retransmission (N(R)= correct sequence number of step c)).

d-2-2) Following correct reception of the block sent by the Terminal, the UICC simulator shall complete the command (data + '9000' indicating correct execution of the command).

#### 7.3.10.5 Acceptance criteria

After step b) and c), the Terminal shall detect the invalid block and send an R-Block requesting retransmission of the last block (N(R)=sequence number of invalid I-Block).

After step d-2-1), the Terminal shall resend the previous R-Block with N(R)=sequence number of invalid I-Block.

After step d-1) and d-2-2), the Terminal shall acknowledge the error free I-Block(s).

### 7.3.11 Chaining - Abortion

#### 7.3.11.1 Definition and applicability

Supervisory blocks, S-block, are used to send control information.

S-blocks are always used in pairs. A S(request) is always followed by a S(response) block.

* S(ABORT request), a request to abort the chain function;
* S(ABORT response), an acknowledge of the abortion of the chain function.

For applicability of this test case see clause 3.8.

#### 7.3.11.2 Conformance requirement

##### 7.3.11.2.0 Description

When an S(… request) has been sent and either a BWT time-out occurs (with the terminal) or the received response is not a S(… response), the S(… request) shall be resent. But if an S(… response) has been sent and either an invalid block is received or a BWT time-out occurs (with the terminal), an R-block shall be sent.

##### 7.3.11.2.1 Reference

ETSI TS 102 221 [1], clause 7.2.3.4.

ISO/IEC 7816‑3 [2], clause 9.7.3, scenarios 26 and 27.

#### 7.3.11.3 Test purpose

To verify that the Terminal correctly handles the abortion procedure in chaining mode.

#### 7.3.11.4 Method of test

##### 7.3.11.4.1 Initial conditions

The Terminal shall be connected to the UICC simulator, and powered on.

ATR shall have been received and eventual PPS procedure successfully completed.

##### 7.3.11.4.2 Procedure

a) Terminal sends chained data:

a-1) Following receipt of the first block by the UICC simulator, the Terminal shall be made to initiate a command requiring sending of chained I-Blocks.

a-2) The UICC simulator shall acknowledge receipt of the first chained I-Block by sending an R-Block without error.

a-3) Following receipt of the second I-Block, the UICC simulator shall send an S(ABORT request).

a-4) The UICC simulator shall acknowledge receipt of the response and give back the Terminal the right to send (R-Block without error) and complete the next command.

b) UICC sends chained data:

b-1) Following receipt of the first block by the UICC simulator, the Terminal shall be made to initiate a command requiring reception of chained I-Blocks.

b-2) The UICC simulator shall transmit the first chained I-Block without error.

b-3) Following correct reception of the block sent by the Terminal, the UICC simulator shall send an S(ABORT request).

b-4) The UICC simulator shall acknowledge receipt of the response without error.

b-5) The UICC simulator shall restart and complete the command (data + '9000' indicating correct execution of the command).

#### 7.3.11.5 Acceptance criteria

After steps a-3) and b-3), the Terminal shall send an S(ABORT response).

In step b-5) the Terminal shall acknowledge reception of the I-Blocks without error by sending R-Blocks with N(R)=sequence number of expected I-Block.

### 7.3.12 Block repetition and resynchronization

#### 7.3.12.1 Definition and applicability

Resynchronization of the protocol may be attempted at three consecutive levels. If one level is unsuccessful, then the next level is tried.

* For the terminal, the three levels are:
* Retransmission of blocks.
* Use of S(RESYNCH request).
* Card reset or deactivation.

Supervisory blocks, S-block, are used to send control information.

S-blocks are always used in pairs. A S(request) is always followed by a S(response) block.

* S(RESYNCH request), a request of a resynchronization;
* S(RESYNCH response), an acknowledge of the resynchronization.

For applicability of this test case see clause 3.8.

#### 7.3.12.2 Conformance requirement

##### 7.3.12.2.0 Description

When an S(… request) has been sent and either a BWT time-out occurs (with the terminal) or the received response is not a S(… response), the S(… request) shall be resent. But if an S(… response) has been sent and either an invalid block is received or a BWT time-out occurs (with the terminal), an R-block shall be sent.

If the terminal fails to receive an error-free block during a card-session, a maximum of two further attempts is allowed before a S(RESYNCH request) is sent.

##### 7.3.12.2.1 Reference

ETSI TS 102 221 [1], clause 7.2.3.4.

ISO/IEC 7816‑3 [2], clause 9.7.3, scenarios 29, 30, 31, 32 and 34.

#### 7.3.12.3 Test purpose

1) To verify that the Terminal resynchronizes the UICC if block repetition is unsuccessful.

2) To verify that the Terminal correctly handles an invalid response to an S(... request).

#### 7.3.12.4 Method of test

##### 7.3.12.4.1 Initial conditions

The Terminal shall be connected to the UICC simulator, and powered on.

ATR shall have been received and eventual PPS procedure successfully completed.

##### 7.3.12.4.2 Procedure

a) Following receipt of the first block by the UICC simulator, the Terminal shall be made to initiate a command requiring sending of an I-Block.

b) Following receipt of the first I-Block, the UICC simulator shall send an erroneous block or be unresponsive.

c) Following correct reception of the block sent by the Terminal, the UICC simulator shall send two more erroneous blocks or remain unresponsive two more times.

d-1) No error:

d-1-1) Following correct reception of the block (S(RESYNCH request)) sent by the Terminal, the UICC simulator shall send a S(RESYNCH response), then complete the next command without error.

d-2) Error assumed:

d-2-1) Following correct reception of the block (S(RESYNCH request)) sent by the Terminal, the UICC simulator shall send a S(RESYNCH response) and generate the following errors:

- Parity error.

- NAD ≠ '00'.

- LEN error (≠ '01').

- S(RESYNCH request) instead of S(RESYNCH response).

- Other S(... response).

- EDC error.

d-2-2) Following correct reception of the block (S(RESYNCH request)) sent by the Terminal, the UICC simulator shall send a S(RESYNCH response), then complete the next command without error.

#### 7.3.12.5 Acceptance criteria

After step b), the Terminal shall send an R-Block requesting retransmission.

In step c), the Terminal shall send the same R-Block as in b) two more times, then initiate an S(RESYNCH request).

After step d-2-1), the Terminal shall resend an S(RESYNCH request).

### 7.3.13 UICC is unresponsive

#### 7.3.13.1 Definition and applicability

Resynchronization of the protocol may be attempted at three consecutive levels. If one level is unsuccessful, then the next level is tried.

* For the terminal, the three levels are:
* Retransmission of blocks.
* Use of S(RESYNCH request).
* Card reset or deactivation.

For applicability of this test case see clause 3.8.

#### 7.3.13.2 Conformance requirement

##### 7.3.13.2.0 Description

After an ATR due to a Warm reset or successful PPS procedure, the communication between the terminal and the UICC can be initiated. But if the terminal fails to receive an error-free block, in the beginning of the protocol, a maximum of two more successive attempts to receive the block is allowed before resetting or a deactivation of the card takes place.

If the terminal fails to receive an error-free block during a card-session, a maximum of two further attempts is allowed before a S(RESYNCH request) is sent.

##### 7.3.13.2.1 Reference

ETSI TS 102 221 [1], clause 7.2.3.4.

ISO/IEC 7816‑3 [2], clause 9.7.3, scenarios 33 and 35.

#### 7.3.13.3 Test purpose

To verify that the Terminal correctly resets or deactivates the UICC at the start of the protocol and during the protocol if resynchronization is unsuccessful.

#### 7.3.13.4 Method of test

##### 7.3.13.4.1 Initial conditions

The Terminal shall be connected to the UICC simulator, and powered on.

ATR shall have been received and eventual PPS procedure successfully completed.

##### 7.3.13.4.2 Procedure

a) At the start of the protocol:

a-1) Following receipt of the first block, the UICC simulator shall be unresponsive.

a-2) Following correct reception of the block sent by the Terminal, the UICC simulator shall remain unresponsive two more times.

b) During the protocol:

b-1) Following receipt of the first block by the UICC simulator, the Terminal shall be made to initiate a command requiring sending of an I-Block.

b-2) Following receipt of the first I-Block, the UICC simulator shall be unresponsive.

b-3) Following correct reception of the block sent by the Terminal, the UICC simulator shall remain unresponsive two more times.

b-4) Following correct reception of the block (S(RESYNCH request)) sent by the Terminal, the UICC simulator shall remain unresponsive three more times.

#### 7.3.13.5 Acceptance criteria

After step a-1), the Terminal shall:

* send an R-Block if the first block it sent was an I-Block.
* repeat the S-Block if the first block it sent was an S-Block.

In step a-2), the Terminal shall send the same block as in a-1) two more times, then reset or deactivate the UICC.

After step b-2), the Terminal shall send an R-Block with N(R)=sequence number of previous I-Block.

In step b-3), the Terminal shall send the same R-Block as in b-2) two more times, then initiate an S(RESYNCH request).

In step b-4), the Terminal shall resend S(RESYNCH request) two more times, then reset or deactivate the UICC.

# 8 Application dependent procedures

## 8.1 UICC presence detection

### 8.1.1 Definition and applicability

To ensure that the UICC has not been removed during a card session, the Terminal sends, at frequent intervals, a STATUS command during each call.

This procedure shall be used in addition to a mechanical or other device used to detect the removal of a UICC.

### 8.1.2 Conformance requirement

#### 8.1.2.0 Description

A STATUS command shall be issued within all 30 second periods of inactivity on the UICC‑Terminal interface during a call. Inactivity in this case is defined as starting at the end of the last communication or the last issued STATUS command. If no response data is received to this STATUS command, then the call shall be terminated as soon as possible but at least within 5 s after the STATUS command has been sent. If the DF indicated in response to a STATUS command is not the same as that which was indicated in the previous response, or accessed by the previous command, then the call shall be terminated as soon as possible but at least within 5 seconds after the response data has been received.

#### 8.1.2.1 Reference

ETSI TS 102 221 [1], clause 14.5.2.

### 8.1.3 Test purpose

To verify that:

1) There are no periods of inactivity on the UICC‑Terminal interface greater than 30 seconds during a call.

2) The Terminal terminates a call within 5 seconds at the latest after having received an invalid response to the STATUS command.

### 8.1.4 Method of test

#### 8.1.4.1 Initial conditions

The Terminal shall be connected to the UICC simulator.

All elementary files shall be coded as default.

#### 8.1.4.2 Procedure

a) A call shall be set up using the generic call setup.

b) The UICC simulator shall monitor the time of periods of inactivity on the UICC-Terminal interface.

c) After 3 minutes, the call shall be cleared.

d) A call shall be set up using the generic call setup.

e) After one minute after the call was successfully set up, the UICC simulator shall respond to a STATUS command with the response data of the MF.

### 8.1.5 Acceptance criteria

1) During step b), the time of periods of inactivity on the UICC-Terminal interface shall not be longer than 30 s.

2) After step e), the Terminal shall terminate the call within 5 seconds at the latest after having received the wrong response to the STATUS command.

# 9 Commands

## 9.1 TERMINAL CAPABILITY

### 9.1.1 Additional interfaces support

#### 9.1.1.1 Definition and applicability

Terminals supporting an interface in addition to the interface defined in ETSI TS 102 221 [1] shall indicate it to the UICC by issuing the TERMINAL CAPABILITY command with an additional interface support TLV object during a new card session before the first application selection.

For applicability of this test case see clause 3.8.

#### 9.1.1.2 Conformance requirement

##### 9.1.1.2.1 Description

Terminals supporting an interface in addition to the interface defined in the present document and present in the list below (e.g. the UICC-CLF interface as defined in ETSI TS 102 613 [6]) shall indicate it to the UICC by issuing the TERMINAL CAPABILITY command with an additional interface support TLV object during a new card session before the first application selection. The terminal supporting the SWP interface shall send a TLV object with tag '82' to indicate the support of the SWP interface before the first application selection.

The TERMINAL CAPABILITY command shall not be issued by the terminal if the Terminal capability mechanism is not indicated inside the supported system command field.

##### 9.1.1.2.2 Reference

ETSI TS 102 221 [1], clauses 11.1.19.2.3 and 11.1.19.1.

#### 9.1.1.3 Test purpose

To verify that the terminal which supports the SWP interface sends a TERMINAL CAPABILITY command indicating the interface supported before the first application selection.

#### 9.1.1.4 Method of test

##### 9.1.1.4.1 Initial conditions

The UICC simulator shall support the SWP interface.

The Terminal shall be connected to the UICC simulator.

The UICC simulator shall indicate support of the TERMINAL CAPABILITY command in the FCP for the MF.

##### 9.1.1.4.2 Procedure

a) Power on the Terminal.

b) The UICC simulator shall send an ATR with a global interface byte tBi (i > 2) indicating the support of the SWP interface.

c) The terminal shall retrieve the FCP of the MF of the UICC using a SELECT command or a STATUS command.

d) The terminal sends a TERMINAL CAPABILITY command

#### 9.1.1.5 Acceptance criteria

In step d), the Terminal shall send TERMINAL CAPABILITY command indicating support of the SWP interface.

NOTE: Other commands may be sent by the terminal before the TERMINAL CAPABILITY command.

The terminal may send other TERMINAL CAPABILITY commands which do not include an Additional interfaces support TLV; such TERMINAL CAPABILITY commands shall be ignored for the purposes of this test case.

The terminal shall send the TERMINAL CAPABILITY command before the first application selection.

Annex A (normative):  
UICC simulator functional requirement

# A.1 General

The UICC simulator shall implement the functions of an UICC as described in ETSI TS 102 221 [1].

# A.2 Contacts C1, C3, C7

## A.2.1 Default measurement/setting uncertainties

Unless stated otherwise below, the following uncertainties apply:

Voltage measurement uncertainty: < ±50 mV

Time measurement uncertainty: < ±100 ns

## A.2.2 Contact C1

Continuous Spikes:

Voltage measurement uncertainty: < ±100 mV

Current Load Amplitude: 0 mA to 20 mA

Adjustable Step Size: 1 mA

Uncertainty: < ±1 mA

Additional Current Offset: 0 mA to 5 mA

Adjustable Step Size: 1 mA

Uncertainty: < ±1 mA

Pulse Width: 100 ns to 500 ns

Adjustable Step Size: 50 ns

Uncertainty: < ±25 ns

Rise and Fall Time: ≤ 50 ns

Pause Width: 100 ns to 500 ns

Adjustable Step Size: 50 ns

Uncertainty: < ±25 ns

Random Spikes:

Voltage measurement uncertainty: < ±100 mV

Current Load Amplitude: 50 mA to 200 mA

Adjustable Step Size: 1 mA

Uncertainty: < ±1 mA

Additional Current Offset: 0 mA to 5 mA

Adjustable Step Size: 1 mA

Uncertainty: < ±0,1 mA

Pulse Width: 100 ns to 500 ns

Adjustable Step Size: 50 ns

Uncertainty: < ±25 ns

Rise and Fall Time: ≤ 50 ns

Pause Width: 0,1 ms to 500 ms, randomly varied

Adjustable Step Size: 0,1 ms

Uncertainty: < ±0,1 ms

## A.2.3 Contact C7

The Elementary Time Unit (etu) used in the clauses below refer to the nominal bit duration on the I/O line, as defined in ISO/IEC 7816‑3 [2].

Voltage setting uncertainty: < ±25 mV

Rise and fall Time setting uncertainty: < ±100 ns

Jitter measurement uncertainty: < ±5 × 10E-3 etu

Jitter setting uncertainty: < ±5 × 10E-3 etu

## A.2.4 Contact C3

Frequency measurement uncertainty: < ±0,5 %

Voltage Measurement uncertainty: < ±50 mV

Rise and fall time measurement uncertainty: < ±5 ns

Duty cycle:

Measurement range: 35 % to 65 %

Measurement uncertainty: < ±2,5 %

# A.3 Definition of timing

It shall be possible to define all timings relative to the clock. The UICC simulator shall be able to calculate and to use the absolute values automatically, even if the Terminal changes the frequency during the communication.

Annex B (informative):  
Change history

The table below indicates all change requests that have been incorporated into the present document since it was created by TC SCP.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | | |
| Date | Meeting | Doc | CR | Rev | Cat | Subject/Comment | Old | New |
| 2001-06 | SCP-06 | SCP-010156 |  |  |  | TSG-T #11 agreed to transfer the contents of the test specification, 3GPP TS 31.120 to EP SCP. V1.0.0 is submitted to EP SCP for approval. It contains only editorial changes compared to 3GPP TS 31.120 V3.0.0 |  | 1.0.0 |
| 2001-06 | SCP-06 | SCP-010194 |  |  |  | Undoing a change regarding the coding conventions in clause 3.4 | 1.0.0 | 1.0.1 |
| 2001-06 | SCP-06 | - |  |  |  | EP SCP agreed that V1.0.1 was ready to be put under change control. As a result, V3.0.0 was created. | 1.0.1 | 3.0.0 |
| 2001-07 | SCP-06 | SCP-010193 | 001 |  | B | Alignment with Rel-4 version of core specification (UICC current consumption values for 3 V and 1,8V) | 3.0.0 | 4.0.0 |
|  |  | SCP-010200 | 002 |  | F | Correction of ATR examples regarding DCB and T4 |  |  |
| 2002-03 | SCP-09 | SCP-020052 | 003 |  | F | Correction of Errors in UICC type recognition | 4.0.0 | 4.1.0 |
| 2003-01 | SCP-12 | SCP-030013 | 005 |  | F | Correction of test on processing of ACK, NACK, NULL procedure bytes and correction of CHV | 4.1.0 | 4.2.0 |
|  |  | SCP-030062 | 006 |  | D | Remove UICC as an abbreviation to align with 3GPP TR 21.905 |  |  |
| 2003-09 | SCP-14 | SCP-030288 | 007 |  | F | Upgrade to Rel-5 version of the specification | 4.2.0 | 5.0.0 |
| 2004-05 | SCP-17 | SCP-040284 | 010 |  | A | Removal of test 6.4 and modification of the numbering order of electrical tests in clause 5.2 | 5.0.0 | 5.1.0 |
| 2004-09 | SCP#18 | SCP-040376 | 015 |  | A | Removal of transmit for WWT exceeded in test 7.2.1 Timing | 5.1.0 | 5.2.0 |
| 2004-11 | SCP#19 | SCP-040489 | 020 |  | A | Non-specific Referencing | 5.2.0 | 5.3.0 |
|  |  | SCP-040492 | 023 |  | A | Modification of test 7.3.2 Block Timing |  |  |
| 2005-06 | SCP#21 | SCP-050129 | 026 |  | F | Correction of test case 7.3.9 | 5.3.0 | 5.4.0 |
|  |  | SCP-050131 | 029 |  | F | Correction of test case 7.3.11 |  |  |
|  |  | SCP-050186 | 032 |  | F | Correction of references to ISO/IEC 7816 |  |  |
| 2005-09 | SCP#22 | SCP-050297 | 035 |  | A | Change of internal references | 5.4.0 | 5.5.0 |
| 2006-03 | SCP#25 | SCP-060160 | 038 |  | A | Removal of test case 5.1.5.5 | 5.5.0 | 5.6.0 |
| 2007-01 | SCP#29 | SCP-070062 | 041 |  | A | Essential correction of "Chaining - IFSD management" test case | 5.6.0 | 5.7.0 |
| 2007-10 | SCP#33 | SCP-070446 | 049 |  | F | CR to ETSI TS 102 230, Rel-5: Adding an applicability table to generate a base for a combined Rel-5 to Rel-7 test specification  Note: incorrect CR number renumbered from 42 to 49 | 5.7.0 | 5.8.0 |
| 2008-07 | SCP#38 | SCP-080337 | 047 |  | A | CR 102 230 Rel-5 Essential correction of ATR coding | 5.7.0 | 5.8.0 |
| 2008-10 | SCP#39 | SCP-080414 | 050 |  | F | Correction of cl. 5.2 chapter numbering | 5.8.0 | 5.9.0 |
| 2009-04 | SCP#41 | ------------------ | ---- |  | - | Upgrade of the specification to Rel-7 | 5.9.0 | 7.0.0 |
| 2009-04 | SCP#41 | SCP-090180 | 053 |  | B | Addition of a test case: analysing rise- and fall-time when a low impedance buffer is selected. | 7.0.0 | 7.1.0 |
| 2010-03 | SCP#44 | SCP(10)0065 | 055 |  | F | Creation of REL 8 of ETSI TS 102 230 | 7.1.0 | 8.0.0 |
| 2013-03 | SCP#45 | SCP(10)0116 | 059 |  | F | Correction of maximum allowed rise/fall time on contact C7 in test 5.2.5.2 | 8.0.0 | 8.1.0 |
| 2013-03 | SCP#58 | SCP(13)000016 | 061 |  | F | Enhancement of TC 7.2.2 with regards to NULL procedure byte | 8.0.0 | 8.1.0 |
| 2013-03 | SCP#57 | SCP(12)000229 | 060 |  | F | Creation of ETSI TS 102 230 REL-9 | 8.1.0 | 9.0.0 |
| 2013-04 | SCP#59 | SCP(13)000063 | 062 |  | F | Creation of ETSI TS 102 230 REL-10 | 9.0.0 | 10.0.0 |
| 2014-02 | SCP#62 | SCP(14)000009 | 063 |  | F | Modification of the electrical test cases | 10.0.0 | 10.1.0 |
| 2014-04 | - | - | - |  | - | Correction of clause numbering and related release information in applicability table | 10.1.0 | 10.1.1 |
| 2014-04 | SCP#63 | SCP(14)000106r1 | 064 | 1 | F | Modification of test case 5.1.5.6 | 10.1.1 | 10.2.0 |
| 2015-10 | SCP#70 | SCP(15)000212 | 067 |  | B | Creation of Rel-11 of the specification | 10.2.0 | 11.0.0 |
| 2015-10 | SCP#70 | SCP(15)000213 | 068 |  | B | Additional of TERMINAL CAPABILITY – Additional interfaces support test case | 10.2.0 | 11.0.0 |
|  |  |  |  |  |  | Addition/modification of section headers to remove hanging paragraphs (as required by updated ETSI drafting rules) | 10.2.0 | 11.0.0 |
| 2016-10 | SCP#75 | SCP(16)000168 | 069 | - | B | Creation of TS 102 230-1 REL-12 | 11.0.0. | 12.0.0 |
| 2016-10 | SCP#75 | SCP(16)000167r1 | 070 | - | C | Update the applicability of test case 9.1.1 | 11.0.0. | 12.0.0 |

# History

|  |  |  |
| --- | --- | --- |
| **Document history** | | |
| V11.0.0 | June 2016 | Publication |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |