**3GPP TSG-RAN Meeting #89-e *RP-201849***

**14 – 18 September 2020**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.0* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.455** | **CR** | **0008** | **rev** | **19** | **Current version:** | **16.0.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Completion of NRPPa positioning CR | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Ericsson, Intel, Huawei, Qualcomm, Nokia, Nokia Shanghai Bell | | | | | | | | | |
| ***Source to TSG:*** | R3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_POS-Core | | | | |  | ***Date:*** | | | 2020-09-14 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12)* *Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Add support of NR positioning in NRPPa | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | The following functions are added:   * Introduction of the Assistance Information Control and Assistance Information Feedback procedures (both Class 2) * Positioning information request/response/failure/update   + UL-SRS Activation (Class 1) and UL-SRS Deactivation (Class2) procedures to extend the Positioning Information Transfer function * TRP information request/response/failure * Measurement request/response/failure/report/update/abort/failure indication * Support of UL NR E-CID | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | No support for NR positioning over NRPPa | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 2, 3.3, 7, 8.1, 8.2.3.2, 8.x, 8.x.2, 8.2.x, 8.2.y, 8.2.z, 8.z, 9.1.1.a, 9.1.1.b, 9.1.1.c, 9.1.1.d, 9.1.1.e, 9.1.1.f, 9.1.1.g, 9.1.1.i, 9.1.1.j, 9.1.1.k, 9.1.1.l, 9.1.a, 9.1.x, 9.2.5, 9.2.a, 9.2.b, 9.2.c, 9.2.d, 9.2.9, 9.2.aa, 9.2.bb, 9.2.cc, 9.2.x, 9.2.y, 9.2.ya, 9.2.yb, 9.2.y1, 9.2.y2, 9.2.y3, 9.2.y5, 9.2.y6, 9.2.z, 9.2.z1, 9.2.z2, 9.2.z3, 9.2.z4, 9.2.z5, 9.2.z6, 9.2.z7, 9.2.z8, 9.2.z9, 9.2.z9a, 9.2.z9b, 9.2.z9c, 9.2.z9d, 9.2.z9e, 9.2.z10, 9.2.z11, 9.2.z12, 9.2.aa1, 9.2.bb1, 9.2.bb2, 9.2.xx1, 9.2.xx2, 9.3.3, 9.3.4, 9.3.5, 9.3.7 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | | **X** |  | Other core specifications | | | | TS 38.473 CR 0373  TS 38.305 CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | Rev6: added agreed TP in R3-197688  Rev9: added asn.1 with FFS related to editor’s notes  Rev10: allocated to R3-200784, withdrawn  Rev11: merged TP in R3-201290  Rev12: submitted to RAN3#107bis-e  Rev13: captured R3-202872, R3-201694, R3-202755 and R3-202776  Rev14: submitted to RAN3#108-e  Rev15: merged TPs R3-204208, R3-204216, R3-204207, R3-204211, R3-204212, R3-204331, R3-204299, R3-204213  Rev16: rapporteur editorial corrections and addition of co-sourcing companies  Rev17: incorporation of TP R3-205153  Rev18: merged TPs R3-205632, R3-205633, R3-205634, R3-205773, R3-205784, R3-205786, ASN.1 check and e-mail revision  Rev19: correction of missing extension with criticality for *ResultNR* IE and *ResultEUTRA* IEs and asn.1 alignment | | | | | | | | |

**START OF CHANGES**

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 38.413:"NG-RAN; NG Application Protocol (NGAP)".

[3] 3GPP TS 38.300: "NR; NR and NG-RAN Overall Description; Stage 2".

[4] 3GPP TS 38.413: "NG-RAN; NG Application Protocol (NGAP)".

[5] 3GPP TR 25.921 (version.7.0.0): "Guidelines and principles for protocol description and error handling".

[6] ITU-T Recommendation X.691 (2002-07): "Information technology - ASN.1 encoding rules - Specification of Packed Encoding Rules (PER) ".

[7] 3GPP TS 36.104: "Evolved Universal Terrestrial Radio Access Network (E-UTRAN); Base Station (BS) radio transmission and reception".

[8] 3GPP TS 23.032:"Technical Specification Group Services and System Aspects; Universal Geographical Area Description (GAD)".

[9] 3GPP TS 36.133: "Evolved Universal Terrestrial Radio Access (E-UTRA); Requirements for support of radio resource management".

[10] 3GPP TS 36.211:"Evolved Universal Terrestrial Radio Access Network (E-UTRAN); Physical Channels and Modulation".

[11] IEEE Std 802.11™-2012, IEEE Standard for Information technology - Telecommunications and information exchange between systems - Local and metropolitan area network.

[12] 3GPP TS 36.455: " Evolved Universal Terrestrial Radio Access (E-UTRA); LTE Positioning Protocol A (LPPa)".

[x] 3GPP TS 38.331: "NR; Radio Resource Control (RRC); Protocol specification".

[y] 3GPP TS 37.355: " Technical Specification Group Radio Access Network; LTE Positioning Protocol (LPP)".

[z] 3GPP TS 38.321: "NR; Medium Access Control (MAC) protocol specification".

[a] 3GPP TS 38.133: "NR; Requirements for support of radio resource management".

[b] 3GPP TS 36:214: "Evolved Universal Terrestrial Radio Access (E-UTRA); Physical layer (PHY); Measurements".

**NEXT CHANGE**

# 3 Definitions, symbols and abbreviations

## 3.1 Definitions

For the purposes of the present document, the terms and definitions given in 3GPP TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in 3GPP TR 21.905 [1].

**NG-RAN node:** as defined in TS 38.300 [3].

**ng-eNB:** as defined in TS 38.300 [3].

## 3.2 Symbols

For the purposes of the present document, the following symbols apply:

<symbol> <Explanation>

## 3.3 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

ARP Antenna Reference Point

BDS BeiDou Navigation Satellite System

CID Cell-ID (positioning method)

DL-PRS Downlink Positioning Reference Signal

E-CID Enhanced Cell-ID (positioning method)

EGNOS European Geostationary Navigation Overlay Service

GAGAN GPS Aided Geo Augmented Navigation

GLONASS GLObal'naya NAvigatsionnaya Sputnikovaya Sistema (Engl.: Global Navigation Satellite System

GNSS Global Navigation Satellite System

GPS Global Positioning System

LMF Location Management FunctionLPP LTE Positioning Protocol

MSAS Multi-functional Satellite Augmentation System

NavIC NAVigation with Indian Constellation

NRPPa NR Positioning Protocol A

OTDOA Observed Time Difference of Arrival

posSIB Positioning SIB

PRS Positioning Reference Signal (for E-UTRA)

QZSS Quasi-Zenith Satellite System

RSRP Reference Signal Received Power

RSSI Received Signal Strength Indicator

RSTD Reference Signal Time Difference

SBAS Space Based Augmentation System

SRS Sounding Reference Signal

TRP Transmission-Reception Point

UE User Equipment

UL-AoA Uplink Angle of Arrival

UL-RTOA Uplink Relative Time of Arrival

UL-SRS Uplink Sounding Reference Signal

WAAS Wide Area Augmentation System

Z-AoA Zenith Angles of Arrival

**NEXT CHANGE**

# 7 Functions of NRPPa

The NRPPa protocol provides the following functions:

- E-CID Location Information Transfer. This function allows the NG-RAN node to exchange location information with LMF for the purpose of E-CID positioning.

- OTDOA Information Transfer. This function allows the NG-RAN node to exchange information with the LMF for the purpose of OTDOA positioning.

- Reporting of General Error Situations. This function allows reporting of general error situations, for which function specific error messages have not been defined.

- Assistance Information Transfer. This function allows the LMF to exchange information with the NG-RAN node for the purpose of assistance information broadcasting.

- Positioning Information Transfer. This function allows the NG-RAN node to exchange positioning information with the LMF for the purpose of positioning.

- Measurement Information Transfer. This function allows the LMF to exchange measurement information with the NG-RAN node for the purpose of positioning.

- TRP Information Transfer. This function allows an LMF to obtain TRP related information from an NG-RAN node.

The mapping between the above functions and NRPPa EPs is shown in the table below.

Table 7-1: Mapping between NRPPa functions and NRPPa EPs

| Function | Elementary Procedure(s) |
| --- | --- |
| E-CID Location Information Transfer | a) E-CID Measurement Initiation  b) E-CID Measurement Failure Indication  c) E-CID Measurement Report  d) E-CID Measurement Termination |
| OTDOA Information Transfer | OTDOA Information Exchange |
| Assistance Information Transfer | a) Assistance Information Control  b) Assistance Information Feedback |
| Reporting of General Error Situations | Error Indication |
| Positioning Information Transfer | a) Positioning Information Exchange  b) Positioning Information Update  c) Positioning Activation  d) Positioning Deactivation |
| TRP Information Transfer | TRP Information Exchange |
| Measurement Information Transfer | a) Measurement  b) Measurement Update  c) Measurement Report  d) Measurement Abort  e) Measurement Failure Indication |

**NEXT CHANGE**

# 8 NRPPa procedures

## 8.1 Elementary procedures

In the following tables, all EPs are divided into Class 1 and Class 2 EPs.

Table 8.1-1: Class 1 Elementary Procedures

| Elementary Procedure | Initiating Message | Successful Outcome | Unsuccessful Outcome | |
| --- | --- | --- | --- | --- |
| Response message | Response message | |
| E-CID Measurement Initiation | E-CID MEASUREMENT INITIATION REQUEST | E-CID MEASUREMENT INITIATION RESPONSE | E-CID MEASUREMENT INITIATION FAILURE |
| OTDOA Information Exchange | OTDOA INFORMATION REQUEST | OTDOA INFORMATION RESPONSE | OTDOA INFORMATION FAILURE |
| Positioning Information Exchange | POSITIONING INFORMATION REQUEST | POSITIONING INFORMATION RESPONSE | POSITIONING INFORMATION FAILURE |
| TRP Information Exchange | TRP INFORMATION REQUEST | TRP INFORMATION RESPONSE | TRP INFORMATION FAILURE |
| Measurement | MEASUREMENT REQUEST | MEASUREMENT RESPONSE | MEASUREMENT FAILURE |
| Positioning Activation | POSITIONING ACTIVATION REQUEST | POSITIONING ACTIVATION RESPONSE | POSITIONING ACTIVATION  FAILURE |

Table 8.1-2: Class 2 Elementary Procedures

| Elementary Procedure | Initiating Message |
| --- | --- |
| E-CID Measurement Failure Indication | E-CID MEASUREMENT FAILURE INDICATION |
| E-CID Measurement Report | E-CID MEASUREMENT REPORT |
| E-CID Measurement Termination | E-CID MEASUREMENT TERMINATION COMMAND |
| Error Indication | ERROR INDICATION |
| Assistance Information Control | ASSISTANCE INFORMATION CONTROL |
| Assistance Information Feedback | ASSISTANCE INFORMATION FEEDBACK |
| Positioning Information Update | POSITIONING INFORMATION UPDATE |
| Measurement Report | MEASUREMENT REPORT |
| Measurement Update | MEASUREMENT UPDATE |
| Measurement Abort | MEASUREMENT ABORT |
| Measurement Failure Indication | MEASUREMENT FAILURE INDICATION |
| Positioning Deactivation | POSITIONING DEACTIVATION |

**NEXT CHANGE**

### 8.2.3 E-CID Measurement Report

#### 8.2.3.1 General

The purpose of E-CID Measurement Report procedure is for the NG-RAN node to provide the E-CID measurements for the UE to the LMF.

#### 8.2.3.2 Successful Operation



Figure 8.2.3.2-1: E-CID Measurement Report procedure, successful operation

The NG-RAN node initiates the procedure by sending an E-CID MEASUREMENT REPORT message. The E-CID MEASUREMENT REPORT message contains the E-CID measurement results according to the measurement configuration in the respective E-CID MEASUREMENT INITIATION REQUEST message.

The *Measured Results* IE shall be included in the *E-CID Measurement Result* IE of the E-CID MEASUREMENT REPORT message when measurement results other than the "Cell-ID" have been requested.

If available, the NG-RAN node shall include the *NG-RAN Access Point Position* IE or the *Geographical Coordinates* IE which is the configured estimated serving antenna position in the *E-CID Measurement Result* IE within the E-CID MEASUREMENT REPORT message. Upon reception of this *NG-RAN Access Point Position* IE, the LMF may use the value as the geographical position of the NG-RAN access point.

If available, the NG-RAN node shall include the *Cell Portion ID* IE in the E-CID MEASUREMENT REPORT message. Upon reception of the *Cell Portion ID* IE, the LMF may use the value as the cell portion for the measurement.

#### 8.2.3.3 Unsuccessful Operation

Not applicable.

**NEXT CHANGE**

## 8.x Assistance Information Transfer Procedures

### 8.x.1 Assistance Information Control

#### 8.x.1.1 General

The purpose of the Assistance Information Control procedure is to allow the LMF to signal positioning assistance information to the NG-RAN Node for assistance information broadcasting.

#### 8.x.1.2 Successful Operation



Figure 8.x.1.2-1: Assistance Information Control procedure

The LMF initiates the procedure by sending an ASSISTANCE INFORMATION CONTROL message.

If the *Assistance Information* IE is included in the ASSISTANCE INFORMATION CONTROL message, the NG-RAN Node shall replace any previously stored assistance information and use the received information to configure assistance information broadcasting.

If the *Broadcast Priority* IE is included in the *Assistance Information* IE, the NG-RAN Node may take it into account when configuring broadcasting for the relevant information. Assistance information having the same Broadcast Priority value should receive the same treatment (i.e. broadcast by the NG-RAN Node or not broadcast).

If the *Broadcast* IE is included in the ASSISTANCE INFORMATION CONTROL message and set to "start", the NG-RAN Node may start broadcasting the assistance information. If the *Broadcast* IE is included in the ASSISTANCE INFORMATION CONTROL message and set to "stop", the NG-RAN Node may stop broadcasting the assistance information.

If the *Positioning Broadcast Cells* IE is included in the ASSISTANCE INFORMATION CONTROL message, the NG-RAN shall, if supported, consider that the received assistance information is applicable to the cells in this IE.

#### 8.x.1.3 Abnormal Conditions

If the *Broadcast* IE is included in the ASSISTANCE INFORMATION CONTROL message and set to "start", and no assistance information is available, the NG-RAN Node shall consider the procedure as failed.

If neither the *Assistance Information* IE nor the *Broadcast* IE are included in the ASSISTANCE INFORMATION CONTROL message, the NG-RAN Node shall consider the procedure as failed.

### 8.x.2 Assistance Information Feedback

#### 8.x.2.1 General

The purpose of the Assistance Information Feedback procedure is to allow the NG-RAN Node to give feedback to the LMF on assistance information broadcasting.

#### 8.x.2.2 Successful Operation



Figure 8.x.2.2-1: Assistance Information Feedback procedure

If the *Assistance Information Failure List* IE is included in the ASSISTANCE INFORMATION FEEDBACK message, the LMF shall consider that assistance information broadcasting could not be configured for the relevant information.

If the *Positioning Broadcast Cells* IE is included in the ASSISTANCE INFORMATION FEEDBACK message, the LMF shall, if supported, consider that the feedback provided is applicable to the cells in this IE.

#### 8.x.2.3 Abnormal Conditions

Void.

**NEXT CHANGE**

### 8.2.x Positioning Information Exchange

#### 8.2.x.1 General

The Positioning Information Exchange procedure is initiated by the LMF to request to the NG-RAN node positioning information for the UE.

#### 8.2.x.2 Successful Operation



Figure 8.2.x.2-1: Positioning Information Exchange procedure, successful operation

The LMF initiates the procedure by sending a POSITIONING INFORMATION REQUEST message to the NG-RAN node.

If the *Requested SRS Transmission Characteristics* IE is included in the POSITIONING INFORMATION REQUEST message, the NG-RAN node may take this information into account when configuring SRS transmissions for the UE, and it shall include the *SRS Configuration* IE and the *SFN Initialisation Time* IE in the POSITIONING INFORMATION RESPONSE message.

#### 8.2.x.3 Unsuccessful Operation



Figure 8.2.6.3-1: Positioning Information Exchange procedure, unsuccessful operation

If the NG-RAN node is unable to configure any SRS transmissions for the UE, it shall respond with a POSITIONING INFORMATION FAILURE message. If a handover of the target UE has been triggered, the NG-RAN node shall send a POSITIONING INFORMATION FAILURE message with an appropriate cause value.

#### 8.2.x.4 Abnormal Conditions

Void.

### 8.2.y Positioning Information Update

#### 8.2.y.1 General

The Positioning Information Update procedure is initiated by the NG-RAN node to indicate to the LMF that a change has occurred in the SRS configuration.

#### 8.2.y.2 Successful Operation



Figure 8.2.y.2-1: Positioning Information Update procedure, successful operation

The NG-RAN node initiates the procedure by sending a POSITIONING INFORMATION UPDATE message to the LMF. This message shall include the SRS configuration information for all cells where the SRS configuration has changed.

#### 8.2.y.3 Unsuccessful Operation

Not Applicable.

#### 8.2.y.4 Abnormal Conditions

Void.

**NEXT CHANGE**

### 8.2.Z TRP Information Exchange

#### 8.2.Z.1 General

The purpose of the TRP Information Exchange procedure is to allow the LMF to request the NG-RAN node to provide detailed information for TRPs hosted by the NG-RAN node.

#### 8.2.Z.2 Successful Operation



Figure 8.2.Z.2-1: TRP Information Exchange procedure, successful operation

The LMF initiates the procedure by sending a TRP INFORMATION REQUEST message. The NG-RAN node responds with a TRP INFORMATION RESPONSE message that contains the requested TRP information.

If the LMF includes the *TRP List* IE in the TRP INFORMATION REQUEST message, the NG-RAN node should include in the TRP INFORMATION RESPONSE message, the requested information for all TRPs included in the *TRP List* IE.

If the LMF does not include the *TRP List* IE in the TRP INFORMATION REQUEST message, the NG-RAN node should include the requested information for all TRPs hosted by the NG-RAN node in the TRP INFORMATION RESPONSE message

#### 8.2.Z.3 Unsuccessful Operation



Figure 8.2.Z.3-1: TRP Information Exchange procedure, unsuccessful operation

If the NG-RAN node cannot provide any of the requested information for any TRP, the NG-RAN node shall respond with a TRP INFORMATION FAILURE message.

**NEXT CHANGE**

8.2.q Positioning Activation

8.2.q.1 General

The Positioning Activation procedure is initiated by the LMF to request the NG-RAN node to activate semi-persistent or trigger aperiodic UL SRS transmission by the UE.

8.2.q.2 Successful Operation

****

**Figure 8.2.q.2-1: Positioning Activation procedure, successful operation**

The LMF initiates the procedure by sending a POSITIONING ACTIVATION REQUEST message to the NG-RAN node.

The message includes an indication of the UL SRS resource set to be activated. For semi-persistent UL SRS, the message also indicates the spatial relation for the semi-persistent UL SRS resource to be activated.

Following successful activation of UL SRS transmission in the UE, the NG-RAN node shall respond with a POSITIONING ACTIVATION RESPONSE message.

8.2.q.3 Unsuccessful Operation

****

**Figure 8.2.q.3-1: Positioning Activation procedure, unsuccessful operation**

If the NG-RAN node is unable to activate UL SRS transmission in the UE, it shall respond with a POSITIONING ACTIVATION FAILURE message.

8.2.q.4 Abnormal Conditions

Void.

8.2.r Positioning Deactivation

8.2.r.1 General

The Positioning Deactivation procedure is initiated by the LMF to indicate to the NG-RAN node that UL SRS transmission should be deactivated in the UE.

8.2.r.2 Successful Operation

****

**Figure 8.2.y.2-1: Positioning Deactivation procedure, successful operation**

The LMF initiates the procedure by sending a POSITIONING DEACTIVATION message to the NG-RAN node. This message shall include an indication of the UL SRS resource set to be deactivated or release all the related resources.

8.2.y.3 Unsuccessful Operation

Not Applicable.

8.2.y.4 Abnormal Conditions

Void.

**NEXT CHANGE**

## 8.z Measurement Information Transfer

### 8.z.1 Measurement

#### 8.z.1.1 General

The Measurement procedure allows the LMF to request one or more TRPs in the NG-RAN node to perform and report positioning measurements.

#### 8.z.1.2 Successful Operation



Figure 8.z.1.2.1: Measurement procedure. Successful operation.

The LMF initiates the procedure by sending a MEASUREMENT REQUEST message to the NG-RAN node, indicating in the *TRP Measurement Request List*  IE the TRP(s) from which measurements are requested. The NG-RAN node shall use the included information to configure positioning measurements by the indicated TRP(s). If at least one of the requested measurements has been successful for at least one of the TRPs, the NG-RAN node shall reply with a MEASUREMENT RESPONSE message.

If the *Report Characteristics* IE is set to "OnDemand", the NG-RAN node shall return the corresponding measurement results in the MEASUREMENT RESPONSE message, and the LMF shall consider that this reporting has been terminated by the NG-RAN node. If the *Report Characteristics* IE is set to "Periodic", the NG-RAN node shall initiate the corresponding measurements, and it shall reply with the MEASUREMENT RESPONSE message without including any measurement results in the message. The NG-RAN node shall then periodically initiate the Measurement Report procedure for the corresponding measurements, with the requested reporting periodicity.

If the *Measurement Beam Information Request* IE is included in the MEASUREMENT REQUEST message, the NG-RAN node shall include the *Measurement Beam Information* IE in the *Measurement Result* IE of the MEASUREMENT RESPONSE message.

#### 8.z.1.3 Unsuccessful Operation



Figure 8.z.1.3.1: Measurement procedure. Unsuccessful operation.

If the NG-RAN node cannot configure any of the requested measurements for any of the TRPs in the *TRP Measurement Request List* IE of the MEASUREMENT REQUEST message, it shall respond with a MEASUREMENT FAILURE message with an appropriate cause value.

#### 8.z.1.4 Abnormal Conditions

Not applicable.

### 8.z.2 Measurement Report

#### 8.z.2.1 General

The Measurement Report procedure allows the NG-RAN node to report positioning measurements to the LMF.

#### 8.z.2.2 Successful Operation



Figure 8.z.2.2.1: Measurement Report procedure. Successful operation.

The NG-RAN node initiates the procedure by sending a MEASUREMENT REPORT message to the LMF. The MEASUREMENT REPORT message contains the measurement results according to the associated measurement configuration.

### 8.z.3 Measurement Update

#### 8.z.3.1 General

The Measurement Update Procedure allows the LMF to notify the NG-RAN node of a change in a previously configured measurement.

#### 8.z.3.2 Successful Operation



Figure 8.z.3.2.1: Measurement Update: Successful Operation.

The LMF initiates the procedure by sending a MEASUREMENT UPDATE message. Upon receiving the message, the NG-RAN node shall overwrite the previously received measurement configuration.

#### 8.z.3.3 Unsuccessful Operation

Not applicable.

#### 8.z.3.4 Abnormal Conditions

If the NG-RAN node cannot identify the previously requested measurement to be modified, it shall consider the procedure as failed and initiate local error handling.

### 8.z.4 Measurement Abort

#### 8.z.4.1 General

The purpose of the Measurement Abort Procedure is to enable the LMF to abort an on-going measurement.

#### 8.z.4.2 Successful Operation



Figure 8.z.4.2.1: Measurement Abort Procedure: Successful Operation.

The LMF initiates the procedure by sending a MEASUREMENT ABORT message.

Upon receiving this message, the NG-RAN node shall terminate the on-going measurement identified by the *LMF Measurement ID* IE and may release any resources previously allocated for the same measurement.

#### 8.z.4.3 Unsuccessful Operation

Not applicable.

#### 8.z.4.4 Abnormal Conditions

If the NG-RAN node cannot identify the previously requested measurement to be aborted, it shall ignore the MEASUREMENT ABORT message.

### 8.z.5 Measurement Failure Indication

#### 8.z.2.1 General

The Measurement Failure Indication procedure allows the NG-RAN node to notify the LMF that the measurements previously requested with the Measurement procedure can no longer be reported.

#### 8.z.2.2 Successful Operation



Figure 8.z.2.2.1: Measurement Report procedure. Successful operation.

Upon reception of the MEASUREMENT FAILURE INDICATION message, the LMF shall consider that the indicated measurements have been terminated by the NG-RAN node.

**NEXT CHANGE**

## 9.1 Message Functional Definition and Content

### 9.1.1 Messages for Location Information Transfer Procedures

#### 9.1.1.1 E-CID MEASUREMENT INITIATION REQUEST

This message is sent by LMF to initiate E-CID measurements.

Direction: LMF → NG-RAN node.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.3 |  | YES | reject |
| NRPPa Transaction ID | M |  | 9.2.4 |  | - |  |
| LMF UE Measurement ID | M |  | INTEGER (1..15,…, 256) |  | YES | reject |
| Report Characteristics | M |  | ENUMERATED (OnDemand, Periodic,…) |  | YES | reject |
| Measurement Periodicity | C-ifReportCharacteristicsPeriodic |  | ENUMERATED (120ms, 240ms, 480ms, 640ms, 1024ms, 2048ms, 5120ms, 10240ms, 1min, 6min, 12min, 30min, 60min,…) |  | YES | reject |
| **Measurement Quantities** |  | *1 .. <maxnoMeas>* |  |  | EACH | reject |
| >Measurement Quantities Item | M |  | ENUMERATED (Cell-ID, Angle of Arrival, Timing Advance Type 1, Timing Advance Type 2, RSRP, RSRQ,…, SS-RSRP, SS-RSRQ, CSI-RSRP, CSI-RSRQ, NR Angle of Arrival) |  | - | - |
| Other-RAT Measurement Quantities |  | *0 .. <maxnoMeas>* |  |  | EACH | ignore |
| >Other-RAT Measurement Quantities Item | M |  | ENUMERATED (GERAN, UTRAN ,…, NR, EUTRA) |  |  |  |
| WLAN Measurement Quantities |  | *0 .. <maxnoMeas>* |  |  | EACH | ignore |
| >WLAN Measurement Quantities Item | M |  | ENUMERATED (WLAN, ...) |  | - |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoMeas | Maximum no. of measured quantities that can be configured and reported with one message. Value is 64. |

|  |  |
| --- | --- |
| Condition | Explanation |
| ifReportCharacteristicsPeriodic | This IE shall be present if the *Report Characteristics* IE is set to the value "Periodic". |

#### 9.1.1.2 E-CID MEASUREMENT INITIATION RESPONSE

This message is sent by NG-RAN node to indicate that the requested E-CID measurement is successfully initiated.

Direction: NG-RAN node → LMF.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.3 |  | YES | reject |
| NRPPa Transaction ID | M |  | 9.2.4 |  | - |  |
| LMF UE Measurement ID | M |  | INTEGER (1..15,…, 256) |  | YES | reject |
| RAN UE Measurement ID | M |  | INTEGER (1..15,…, 256) |  | YES | reject |
| E-CID Measurement Result | O |  | 9.2.5 |  | YES | ignore |
| Criticality Diagnostics | O |  | 9.2.2 |  | YES | ignore |
| Cell Portion ID | O |  | 9.2.12 |  | YES | ignore |
| Other-RAT Measurement Result | O |  | 9.2.13 |  | YES | ignore |
| WLAN Measurement Result | O |  | 9.2.14 |  | YES | ignore |

#### 9.1.1.3 E-CID MEASUREMENT INITIATION FAILURE

This message is sent by NG-RAN node to indicate that the requested E-CID measurement cannot be initiated.

Direction: NG-RAN node → LMF.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.3 |  | YES | reject |
| NRPPa Transaction ID | M |  | 9.2.4 |  | - |  |
| LMF UE Measurement ID | M |  | INTEGER (1..15,…, 256) |  | YES | reject |
| Cause | M |  | 9.2.1 |  | YES | ignore |
| Criticality Diagnostics | O |  | 9.2.2 |  | YES | ignore |

#### 9.1.1.4 E-CID MEASUREMENT FAILURE INDICATION

This message is sent by NG-RAN node to indicate that the previously requested E-CID measurement can no longer be reported.

Direction: NG-RAN node → LMF.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.3 |  | YES | ignore |
| NRPPa Transaction ID | M |  | 9.2.4 |  | - |  |
| LMF UE Measurement ID | M |  | INTEGER (1..15,…, 256) |  | YES | reject |
| RAN UE Measurement ID | M |  | INTEGER (1..15,…, 256) |  | YES | reject |
| Cause | M |  | 9.2.1 |  | YES | ignore |

#### 9.1.1.5 E-CID MEASUREMENT REPORT

This message is sent by NG-RAN node to report the results of the requested E-CID measurement.

Direction: NG-RAN node → LMF.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.3 |  | YES | ignore |
| NRPPa Transaction ID | M |  | 9.2.4 |  | - |  |
| LMF UE Measurement ID | M |  | INTEGER (1..15,…, 256) |  | YES | reject |
| RAN UE Measurement ID | M |  | INTEGER (1..15,…, 256) |  | YES | reject |
| E-CID Measurement Result | M |  | 9.2.5 |  | YES | ignore |
| Cell Portion ID | O |  | 9.2.12 |  | YES | ignore |

#### 9.1.1.6 E-CID MEASUREMENT TERMINATION COMMAND

This message is sent by the LMF to terminate the requested E-CID measurement.

Direction: LMF → NG-RAN node.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.3 |  | YES | ignore |
| NRPPa Transaction ID | M |  | 9.2.4 |  | - |  |
| LMF UE Measurement ID | M |  | INTEGER (1..15,…, 256) |  | YES | reject |
| RAN UE Measurement ID | M |  | INTEGER (1..15,…, 256) |  | YES | reject |

**NEXT CHANGE**

#### 9.1.1.a POSITIONING INFORMATION REQUEST

This message is sent by LMF to request positioning information.

Direction: LMF → NG-RAN node.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.3 |  | YES | reject |
| NRPPa Transaction ID | M |  | 9.2.4 |  | - |  |
| Requested SRS Transmission Characteristics | O |  | 9.2.x |  | YES | ignore |

#### 9.1.1.b POSITIONING INFORMATION RESPONSE

This message is sent by NG-RAN node to provide positioning information.

Direction: NG-RAN node → LMF.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.3 |  | YES | reject |
| NRPPa Transaction ID | M |  | 9.2.4 |  | - |  |
| SRS Configuration | O |  | 9.2.y |  | YES | ignore |
| SFN Initialisation Time | O |  | 9.2.y5 |  | YES | ignore |
| Criticality Diagnostics | O |  | 9.2.2 |  | YES | ignore |

#### 9.1.1.c POSITIONING INFORMATION FAILURE

This message is sent by NG-RAN node to indicate that the positioning information cannot be provided.

Direction: NG-RAN node → LMF.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.3 |  | YES | reject |
| NRPPa Transaction ID | M |  | 9.2.4 |  | - |  |
| Cause | M |  | 9.2.1 |  | YES | ignore |
| Criticality Diagnostics | O |  | 9.2.2 |  | YES | ignore |

#### 9.1.1.d POSITIONING INFORMATION UPDATE

This message is sent by NG-RAN node to indicate that a change in the SRS configuration has occurred.

Direction: NG-RAN node → LMF.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.3 |  | YES | ignore |
| NRPPa Transaction ID | M |  | 9.2.4 |  | - |  |
| SRS Configuration | O |  | 9.2.y |  | YES | ignore |
| SFN Initialisation Time | O |  | 9.2.y5 |  | YES | ignore |

**NEXT CHANGE**

#### 9.1.1.e TRP INFORMATION REQUEST

This message is sent by an LMF to request information for TRPs hosted by an NG-RAN node.

Direction: LMF → NG-RAN node.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.3 |  | YES | reject |
| NRPPa Transaction ID | M |  | 9.2.4 |  | - |  |
| **TRP List** |  | *0 ..1* |  |  |  |  |
| **>TRP List Item** |  | *1 .. <maxnoTRPs>* |  |  | EACH | ignore |
| >>TRP ID | M |  | 9.2.aa |  |  |  |
| **TRP Information Type List** |  | *1* |  |  |  |  |
| **>TRP Information Type Item** |  | *1 .. <maxnoTRPInfoTypes>* |  |  | EACH | reject |
| >>TRP Information Type Item | M |  | ENUMERATED (nr pci, ng-ran cgi, nr arfcn, prs config, ssb config, sfn init time, spatial direction info, geo-coordinates, …) |  |  |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoTRPs | Maximum no. of TRPs in a NG-RAN node. Value is 65535 |
| maxnoTRPInfoTypes | Maximum no of TRP information types that can be requested and reported with one message. Value is 64. |

#### 9.1.1.f TRP INFORMATION RESPONSE

This message is sent by an NG-RAN node to convey TRP information to an LMF. This message only applies when the NG-RAN node is a gNB.

Direction: NG-RAN node → LMF.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.3 |  | YES | reject |
| NRPPa Transaction ID | M |  | 9.2.4 |  | - |  |
| **TRP Information List** |  | *1* |  |  | YES | ignore |
| **>TRP Information Item** | M | *1 .. <maxnoTRPs>* |  |  | EACH | ignore |
| >>TRP Information | M |  | 9.2.bb |  |  |  |
| Criticality Diagnostics | O |  | 9.2.2 |  | YES | ignore |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoTRPs | Maximum no. of TRPs in a NG-RAN node. Value is 65535. |

#### 9.1.1.g TRP INFORMATION FAILURE

This message is sent by an NG-RAN node to indicate that the requested TRP information cannot be provided to an LMF.

Direction: NG-RAN node → LMF.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.3 |  | YES | reject |
| NRPPa Transaction ID | M |  | 9.2.4 |  | - |  |
| Cause | M |  | 9.2.1 |  | YES | ignore |
| Criticality Diagnostics | O |  | 9.2.2 |  | YES | ignore |

**NEXT CHANGE**

#### 9.1.1.i POSITIONING ACTIVATION REQUEST

This message is sent by the LMF to cause the NG RAN node to activate/trigger UL SRS transmission by the UE.

Direction: LMF → NG-RAN node.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.3 |  | YES | reject |
| NRPPa Transaction ID | M |  | 9.2.4 |  | YES | reject |
| CHOICE *SRS type* | M |  |  |  | YES | reject |
| **>Semi-persistent** |  |  |  |  |  |  |
| >>SRS Resource Set ID | M |  | 9.2.y1 |  | - | - |
| >>SRS Spatial Relation | O |  | Spatial Relation Information  9.2.y2 |  | - | - |
| **>Aperiodic** |  |  |  |  |  |  |
| >>Aperiodic | M |  | ENUMERATED(true,…) |  | - | - |
| >>SRS Resource Trigger | O |  | 9.2.y3 |  | - | - |
| Activation Time | O |  | SFN Initialisation Time  9.2.y5 | indicates the start time when the SRS activation is requested | YES | ignore |

#### 9.1.1.j POSITIONING ACTIVATION RESPONSE

This message is sent by NG-RAN node to confirm successful UL SRS activation in the UE.

Direction: NG-RAN node → LMF.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.3 |  | YES | reject |
| NRPPa Transaction ID | M |  | 9.2.4 |  | YES | reject |
| Criticality Diagnostics | O |  | 9.2.2 |  | YES | ignore |
| System Frame Number | O |  | INTEGER(0..1023) |  | YES | ignore |
| Slot Number | O |  | INTEGER(0..79) |  | YES | ignore |

#### 9.1.1.k POSITIONING ACTIVATION FAILURE

This message is sent by NG-RAN node to indicate that activation of UL SRS transmission in the UE was unsuccessful.

Direction: NG-RAN node → LMF.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.3 |  | YES | reject |
| NRPPa Transaction ID | M |  | 9.2.4 |  | YES | reject |
| Cause | M |  | 9.2.1 |  | YES | ignore |
| Criticality Diagnostics | O |  | 9.2.2 |  | YES | ignore |

#### 9.1.1.l POSITIONING DEACTIVATION

This message is sent by the LMF to cause the NG RAN node to deactivate UL SRS transmission or release all the transmission by the UE.

Direction: LMF → NG-RAN node.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.3 |  | YES | ignore |
| NRPPa Transaction ID | M |  | 9.2.4 |  | YES | reject |
| CHOICE *Abort Transmission* | M |  |  |  | YES | Ignore |
| >SRS Resource Set ID deactivation | M |  | 9.2.y1 |  | YES | Ignore |
| >Release ALL |  | NULL |  | the NG-RAN node configures UE to stop transmitting SRS for the positioning purpose | YES | Ignore |

**NEXT CHANGE**

### 9.1.a Messages for Assistance Information Transfer Procedures

#### 9.1.a.1 ASSISTANCE INFORMATION CONTROL

This message is sent by the LMF to transfer assistance information.

Direction: LMF → NG-RAN Node.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.3 |  | YES | reject |
| NRPPa Transaction ID | M |  | 9.2.4 |  | - |  |
| Assistance Information | O |  | 9.2.a |  | YES | reject |
| Broadcast | O |  | ENUMERATED (start, stop, …) |  | YES | reject |
| Positioning Broadcast Cells | O |  | 9.2.xx2 | The cell(s) that are requested to broadcast posSIB(s) according to the *Assistance Information* IE. | YES | reject |

#### 9.1.a.2 ASSISTANCE INFORMATION FEEDBACK

This message is sent by the NG-RAN Node to give feedback on assistance information broadcasting.

Direction: NG-RAN Node → LMF.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.3 |  | YES | reject |
| NRPPa Transaction ID | M |  | 9.2.4 |  | - |  |
| Assistance Information Failure List | O |  | 9.2.e |  | YES | reject |
| Positioning Broadcast Cells | O |  | 9.2.xx2 | The cells associated to the feedback provided in the *Assistance Information Failure List* IE. | YES | reject |
| Criticality Diagnostics | O |  | 9.2.2 |  | YES | ignore |

**NEXT CHANGE**

### 9.1.x Messages for Measurement Information Transfer Procedures

#### 9.1.x.1 MEASUREMENT REQUEST

This message is sent by the LMF to request the NG-RAN node to configure a positioning measurement.

Direction: LMF → NG-RAN node.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.3 |  | YES | reject |
| NRPPa Transaction ID | M |  | 9.2.4 |  | - |  |
| LMF Measurement ID | M |  | INTEGER (1..65536) |  | YES | reject |
| **TRP Measurement Request List** |  | *1* |  |  | YES | reject |
| >TRP Measurement Request Item |  | *1..<maxnoofMeasTRPs>* |  |  |  |  |
| >>TRP ID | M |  | 9.2.aa |  |  |  |
| >>Search Window Information | O |  | 9.2.cc |  |  |  |
|  |  |  |  |  |  |  |
| Report Characteristics | M |  | ENUMERATED (OnDemand, Periodic, ...) |  | YES | reject |
| Measurement Periodicity | C-ifReportCharacteristicsPeriodic |  | ENUMERATED (120ms, 240ms, 480ms, 640ms, 1024ms, 2048ms, 5120ms, 10240ms, 1min, 6min, 12min, 30min, 60min,…) |  | YES | reject |
| **TRP Measurement Quantities** |  | 1 |  |  | YES |  |
| **>TRP Measurement Quantities Item** |  | *1 .. <maxnoPosMeas>* |  |  | EACH | reject |
| >TRP Measurement Type | M |  | ENUMERATED (gNB-RxTxTimeDiff, UL-SRS-RSRP, UL-AoA, UL-RTOA,…) |  | - |  |
| >Timing Reporting Granularity Factor | O |  | INTEGER (0..5) | TS 38.133 [a] |  |  |
| SFN initialisation Time | O |  | 9.2.y5 | If this IE is not present, the TRP may assume that the value is same as its own SFN initialisation time. | YES | ignore |
| SRS Configuration | O |  | 9.2.y |  | YES | ignore |
| Measurement Beam Information Request | O |  | ENUMERATED (true,...) |  | YES | ignore |
| System Frame Number | O |  | INTEGER(0..1023) |  | YES | ignore |
| Slot Number | O |  | INTEGER(0..79) |  | YES | ignore |

|  |  |
| --- | --- |
| Condition | Explanation |
| ifReportCharacteristicsPeriodic | This IE shall be present if the *Report Characteristics* IE is set to the value "Periodic". |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoPosMeas | Maximum no. of measured quantities that can be configured and reported with one positioning measurement message. Value is 16384. |
| maxnoofMeasTRPs | Maxmum no. of TRPs that can be included within one message. Value is 64. |

#### 9.1.x.2 MEASUREMENT RESPONSE

This message is sent by the NG-RAN node to report positioning measurements for the target UE.

Direction: NG-RAN node → LMF.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.3 |  | YES | reject |
| NRPPa Transaction ID | M |  | 9.2.4 |  | - |  |
| LMF Measurement ID | M |  | INTEGER (1..65536) |  | YES | reject |
| RAN Measurement ID | M |  | INTEGER (1..65536) |  | YES | reject |
| **TRP Measurement Response List** |  | *0..1* |  |  | YES | reject |
| **>TRP Measurement Response Item** |  | *1..<maxnoofMeasTRPs>* |  |  |  |  |
| >>TRP ID | M |  | 9.2.aa |  |  |  |
| >>Measurement Result | M |  | 9.2.z1 |  |  |  |
| Criticality Diagnostics | O |  | 9.2.11 |  | YES | ignore |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofMeasTRPs | Maxmum no. of TRPs that can be included within one message. Value is 64. |

#### 9.1.x.3 MEASUREMENT FAILURE

This message is sent by the NG-RAN node to report measurement failure.

Direction: NG-RAN node → LMF.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.3 |  | YES | reject |
| NRPPa Transaction ID | M |  | 9.2.4 |  | - |  |
| LMF Measurement ID | M |  | INTEGER (1..65536) |  | YES | reject |
| Cause | M |  | 9.2.1 |  | YES | ignore |
| Criticality Diagnostics | O |  | 9.2.11 |  | YES | ignore |

#### 9.1.x.4 MEASUREMENT REPORT

This message is sent by the NG-RAN node to report positioning measurements for the target UE.

Direction: NG-RAN node → LMF.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.3 |  | YES | reject |
| NRPPa Transaction ID | M |  | 9.2.4 |  | - |  |
| LMF Measurement ID | M |  | INTEGER (1..65536) |  | YES | reject |
| RAN Measurement ID | M |  | INTEGER (1..65536) |  | YES | reject |
| **TRP Measurement Report List** |  | *1* |  |  | YES | reject |
| **>TRP Measurement Report Item** |  | *1..<maxnoofMeasTRPs>* |  |  | EACH |  |
| >>TRP ID | M |  | 9.2.aa |  | - | - |
| >>Measurement Result | M |  | 9.2.z1 |  | - | - |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofMeasTRPs | Maxmum no. of TRPs that can be included within one message. Value is 64. |

#### 9.1.x.5 MEASUREMENT UPDATE

This message is sent by the LMF to update a previously configured measurement.

Direction: LMF → NG-RAN node.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.3 |  | YES | ignore |
| NRPPa Transaction ID | M |  | 9.2.4 |  | - |  |
| LMF Measurement ID | M |  | INTEGER (1..65536) |  | YES | reject |
| RAN Measurement ID | M |  | INTEGER (1..65536) |  | YES | reject |
| SRS Configuration | O |  | 9.2.y |  | YES | ignore |

#### 9.1.x.6 MEASUREMENT ABORT

This message is sent by the LMF to request the NG-RAN node to abort a measurement.

Direction: LMF → NG-RAN node.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.3 |  | YES | reject |
| NRPPa Transaction ID | M |  | 9.2.4 |  | - |  |
| LMF Measurement ID | M |  | INTEGER (1..65536) |  | YES | reject |
| RAN Measurement ID | M |  | INTEGER (1..65536) |  | YES | reject |

#### 9.1.x.7 MEASUREMENT FAILURE INDICATION

This message is sent by the NG-RAN node to indicate that the previously requested measurements can no longer be reported.

Direction: NG-RAN node → LMF.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.3 |  | YES | reject |
| NRPPa Transaction ID | M |  | 9.2.4 |  | - |  |
| LMF Measurement ID | M |  | INTEGER (1..65536) |  | YES | reject |
| RAN Measurement ID | M |  | INTEGER (1..65536) |  | YES | reject |
| Cause | M |  | 9.2.1 |  | YES | ignore |

**NEXT CHANGE**

### 9.2.5 E-CID Measurement Result

The purpose of the E-CID Measurement Result information element is to provide the E-CID measurement result.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE Type and Reference | Semantics Description | Criticality | Assigned Criticality |
| Serving Cell ID | M |  | NG-RAN CGI  9.2.6 | NG-RAN Cell Identifier of the serving cell | - |  |
| Serving Cell TAC | M |  | TAC  9.2.11 | Tracking Area Code of the serving cell | - |  |
| NG-RAN Access Point Position | O |  | 9.2.10 | The configured estimated geographical position of the antenna of the cell.  If the *Geographical Coordinates* IE is used, the *NG-RAN Access Point Position* IE shall be ignored. | - |  |
| **Measured Results** |  | *0 .. <maxnoMeas>* |  |  | - |  |
| >CHOICE *Measured Results Value* | M |  |  |  | - |  |
| >>Value Angle of Arrival EUTRA | M |  | INTEGER (0..719) | According to mapping in TS 36.133 [9] | - |  |
| >>Value Timing Advance Type 1 EUTRA | M |  | INTEGER (0..7690) | According to mapping in TS 36.214 [b] | - |  |
| >>Value Timing Advance Type 2 EUTRA | M |  | INTEGER (0..7690) | According to mapping in TS 36.214 [b] | - |  |
| >>**Result RSRP EUTRA** |  | *1 .. <maxCellReport>* |  |  | - |  |
| >>> PCI EUTRA | M |  | INTEGER (0..503) | Physical Cell Identifier of the reported E-UTRA cell | - |  |
| >>>EARFCN | M |  | INTEGER (0.. 262143, …) | Corresponds to NDL for FDD and NDL/UL for TDD in ref. TS 36.104 [7] | - |  |
| >>> CGI EUTRA | O |  | 9.2.6 | Cell Global Identifier of the reported E-UTRA cell | - |  |
| >>>Value RSRP EUTRA | M |  | INTEGER (0..97, …) |  | - |  |
| >>**Result RSRQ EUTRA** |  | *1 . <maxCellReport>* |  |  | - |  |
| >>> PCI EUTRA | M |  | 9.2.7 | Physical Cell Identifier of the reported E-UTRA cell | - |  |
| >>>EARFCN | M |  | INTEGER (0..262143, …) | Corresponds to NDL for FDD and NDL/UL for TDD in ref. TS 36.104 [7] | - |  |
| >>> CGI EUTRA | O |  | 9.2.7 | Cell Global Identifier of the reported E-UTRA cell | - |  |
| >>>Value RSRQ EUTRA | M |  | INTEGER (0..34, …) |  | - |  |
| **>>Result SS-RSRP** |  | *1 .. <maxCellReportNR>* |  |  | YES | ignore |
| >>>NR PCI | M |  | INTEGER (0..1007) |  | - |  |
| >>>NR ARFCN | M |  | INTEGER (0..3279165) |  | - |  |
| >>>NG-RAN CGI | O |  | 9.2.6 |  | - |  |
| >>>Value SS-RSRP Cell | O |  | INTEGER (0..127) | SS-RSRP measurement aggregated at cell level | - |  |
| **>>>SS-RSRP per SSB Resource** |  | *0 .. <maxIndexesReport>* |  |  | - |  |
| >>>>SSB Index | M |  | INTEGER (0..63) |  | - |  |
| >>>>Value SS-RSRP | M |  | INTEGER (0..127) | SS-RSRP measurement per SSB resource | - |  |
| **>>Result SS-RSRQ** |  | *1 .. <maxCellReportNR>* |  |  | YES | ignore |
| >>>NR PCI | M |  | INTEGER (0..1007) |  | - |  |
| >>>NR ARFCN | M |  | INTEGER (0..3279165) |  | - |  |
| >>>NG-RAN CGI | O |  | 9.2.6 |  | - |  |
| >>>Value SS-RSRQ Cell | O |  | INTEGER (0..127) | SS-RSRQ measurement aggregated at cell level | - |  |
| **>>>SS-RSRQ per SSB Resource** |  | *0 .. <maxIndexesReport>* |  |  | - |  |
| >>>>SSB Index | M |  | INTEGER (0..63) |  | - |  |
| >>>>Value SS-RSRQ | M |  | INTEGER (0..127) | SS-RSRQ measurement per SSB resource | - |  |
| **>>Result CSI-RSRP** |  | *1 .. <maxCellReportNR>* |  |  | YES | ignore |
| >>>NR PCI | M |  | INTEGER (0..1007) |  | - |  |
| >>>NR ARFCN | M |  | INTEGER (0..3279165) |  | - |  |
| >>>NG-RAN CGI | O |  | 9.2.6 |  | - |  |
| >>>Value CSI-RSRP Cell | O |  | INTEGER (0..127) | CSI-RSRP measurement aggregated at cell level | - |  |
| **>>>CSI-RSRP per CSI-RS Resource** |  | *0 .. <maxIndexesReport>* |  |  | - |  |
| >>>>CSI-RS Index | M |  | INTEGER (0..95) |  | - |  |
| >>>>Value CSI-RSRP | M |  | INTEGER (0..127) | CSI-RSRP measurement per CSI-RS resource | - |  |
| **>>Result CSI-RSRQ** |  | *1 .. <maxCellReportNR>* |  |  | YES | ignore |
| >>>NR PCI | M |  | INTEGER (0..1007) |  | - |  |
| >>>NR ARFCN | M |  | INTEGER (0..3279165) |  | - |  |
| >>>NG-RAN CGI | O |  | 9.2.6 |  | - |  |
| >>>Value CSI-RSRQ Cell | O |  | INTEGER (0..127) | CSI-RSRQ measurement aggregated at cell level | - |  |
| **>>>CSI-RSRQ per CSI-RS Resource** |  | *0 .. <maxIndexesReport>* |  |  | - |  |
| >>>>CSI-RS Index | M |  | INTEGER (0..95) |  | - |  |
| >>>>Value CSI-RSRQ | M |  | INTEGER (0..127) | CSI-RSRQ measurement per CSI-RS resource | - |  |
| >>Angle of Arrival NR | M |  | UL Angle of Arrival  9.2.z2 |  | YES | ignore |
| Geographical Coordinates | O |  | 9.2.z9 |  | YES | ignore |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoMeas | Maximum no. of measured quantities that can be configured and reported with one message. Value is 64. |
| maxCellReport | Maximum no. of cells that can be reported with one message. Value is 9. |
| maxCellReportNR | Maximum no. of NR cells that can be reported with one message. Value is 9. |
| maxIndexesReport | Maximum no. of beam level measurement results that can be reported with one message. Value is 64. |

**NEXT CHANGE**

### 9.2.13 Other-RAT Measurement Result

The purpose of the Inter-RAT Measurement Result information element is to provide the Inter-RAT measurement results.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE Type and Reference | Semantics Description | Criticality | Assigned Criticality |
| **Other-RAT Measured Results** |  | *1.. <maxnoMeas>* |  |  |  |  |
| >CHOICE *Other-RAT Measured Results Value* | M |  |  |  |  |  |
| >>**Result GERAN** | M | *1..<maxGERANMeas>* |  |  |  |  |
| >>>ARFCN of BCCH | M |  | INTEGER (0..1023, ...) |  |  |  |
| >>>Physical CellId GERAN | M |  | INTEGER (0..63, ...) |  |  |  |
| >>>RSSI | M |  | INTEGER (0..63, ...) |  |  |  |
| >>**Result UTRAN** |  | *1..<maxUTRANMeas>* |  |  |  |  |
| >>>UARFCN | M |  | INTEGER (0..16383, ...) |  |  |  |
| >>>CHOICE *Physical CellId UTRA* | M |  |  |  |  |  |
| >>>>Physical CellId UTRA FDD | M |  | INTEGER (0..511, ...) |  |  |  |
| >>>>Physical CellId UTRA TDD | M |  | INTEGER (0..127, ...) |  |  |  |
| >>>UTRA RSCP | O |  | INTEGER (-5..91, ...) |  |  |  |
| >>>UTRA EcNo | O |  | INTEGER (0..49, ...) | This IE applies to FDD only. |  |  |
| **>>Result NR** |  | *1..<maxNRMeas>* |  |  | YES | ignore |
| >>>NR PCI | M |  | INTEGER (0..3279165) |  | - |  |
| >>>NR ARFCN | M |  | INTEGER (0..1007) |  | - |  |
| >>>SS-RSRP Cell | O |  | INTEGER (0..127) | SS-RSRP measurement aggregated at cell level | - |  |
| >>>SS-RSRQ Cell | O |  | INTEGER (0..127) | SS-RSRQ measurement aggregated at cell level | - |  |
| >>>**SS-RSRP per SSB Resource** |  | *0 .. <maxnoIndexesToReport>* |  |  | - |  |
| >>>>SSB Index | M |  | INTEGER (0..63) |  | - |  |
| >>>>Value SS-RSRP | M |  | INTEGER (0..127) | SS-RSRP measurement per SSB resource | - |  |
| >>>**SS-RSRQ per SSB Resource** |  | *0 .. <maxnoIndexesToReport>* |  |  | - |  |
| >>>>SSB Index | M |  | INTEGER (0..63) |  | - |  |
| >>>>Value SS-RSRQ | M |  | INTEGER (0..127) | SS-RSRQ measurement per SSB resource | - |  |
| >>>CGI NR | O | 9.2.cc |  | Cell Global Identifier of the reported NR cell | - |  |
| **>>Result EUTRA** |  | *1..<maxEUTRAMeas>* |  |  | YES | ignore |
| >>>PCI EUTRA | M |  | 9.2.7 |  | - |  |
| >>>EARFCN | M |  | INTEGER (0..262143). |  | - |  |
| >>>RSRP EUTRA | O |  | INTEGER (0..97) |  | - |  |
| >>>RSRQ EUTRA | O |  | INTEGER (0..34) |  | - |  |
| >>>CGI EUTRA | O | 9.2.7 |  | Cell Global Identifier of the reported E-UTRA cell | - |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoMeas | Maximum no. of measured quantities that can be configured and reported with one message. Value is 64. |
| maxGERANMeas | Maximum no. of GERAN cells that can be reported with one message. Value is 8. |
| maxUTRANMeas | Maximum no. of UTRAN cells that can be reported with one message. Value is 8. |
| maxNRMeas | Maximum no. of NR cells that can be reported with one message. Value is 8. |
| maxEUTRAMeas | Maximum no. of EUTRA cells that can be reported with one message. Value is 8. |
| maxIndexesReport | Maximum no. of beam level measurement results that can be reported with one message. Value is 64. |

**NEXT CHANGE**

### 9.2.a Assistance Information

This IE contains the assistance information.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| **Assistance Information** | M |  |  |  |
| >**System Information** |  | *1..<maxNrOfPosSImessage>* |  | Corresponds to the number of SI messages with posSIBs to be scheduled |
| >>Broadcast Periodicity | M |  | ENUMERATED (ms80, ms160, ms320, ms640, ms1280, ms2560, ms5120, ...) | Broadcast Periodicity for the Pos SIBs, see TS 38.331 [x] |
| >>**Pos SIBs** |  | *1..<maxNrOfPosSIBs>* |  | Number of posSIBs in the System Information. |
| >>>PosSIB-Type | M |  | 9.2.d |  |
| >>>PosSIB Segments | M |  | 9.2.b |  |
| >>>Assistance Information Meta Data | O |  | 9.2.c |  |
| >>>Broadcast Priority | O |  | INTEGER (1..16, ...) | The priority of the assistance Information where 1 represents the highest priority and 16 the lowest priority |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxNrOfPosSImessage | Maximum number of positioning system information messages. Value is 32. |
| maxNrOfPosSIBs | Maximum number of positioning system information blocks included in the message. Value is 32. |

**NEXT CHANGE**

### 9.2.b PosSIB Segments

This IE provides one posSIB or two or more posSIB segments which must be scheduled in series in consecutive transmissions of the same SI message.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| **PosSIB Segments** |  | *1..<maxNrOfSegments>* |  |  |
| >Assistance Data SIB Element | M |  | OCTET STRING | TS 37.355 [y] |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxNrOfSegments | Maximum number of positioning SIB segments (in case of *Assistance Information Element* contains segmented data according to TS 37.355 [y]). Value is 64. |

**NEXT CHANGE**

### 9.2.c Assistance Information Meta Data

This parameter contains meta data for an assistance information element.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Encrypted | O |  | ENUMERATED (true, …) |  |
| GNSS ID | O |  | ENUMERATED (gps, sbas, qzss, galileo, glonass, bds, navic ...) |  |
| SBAS ID | O |  | ENUMERATED (waas, egnos, msas, gagan, ...) |  |

**NEXT CHANGE**

### 9.2.d Positioning SIB Type

This parameter defines a specific positioning SIB, as defined in TS 37.355 [y].

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Positioning SIB Type | M |  | ENUMERATED ( posSibType1-1,  posSibType1-2,  posSibType1-3,  posSibType1-4,  posSibType1-5,  posSibType1-6,  posSibType1-7,  posSibType1-8,  posSibType2-1,  posSibType2-2,  posSibType2-3,  posSibType2-4,  posSibType2-5,  posSibType2-6,  posSibType2-7,  posSibType2-8,  posSibType2-9,  posSibType2-10,  posSibType2-11,  posSibType2-12,  posSibType2-13,  posSibType2-14,  posSibType2-15,  posSibType2-16,  posSibType2-17,  posSibType2-18,  posSibType2-19,  posSibType2-20,  posSibType2-21,  posSibType2-22,  posSibType2-23,  posSibType2-24,  posSibType2-25,  posSibType3-1,  posSibType4-1,  posSibType5-1,  posSibType6-1,  posSibType6-2,  posSibType6-3,  ... ) |  |

**NEXT CHANGE**

### 9.2.e Assistance Information Failure List

This parameter identifies the assistance information for which the NG-RAN Node failed to configure broadcasting.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| **Assistance Information Failure List** |  | *1..<maxnoAssistInfoFailureListItems>* |  |  |
| >PosSIB-Type | M |  | 9.2.d |  |
| >Outcome | M |  | ENUMERATED (failed, ...) |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoAssistInfoFailureListItems | Maximum no. of assistance information failure list items that can be signaled with one message. Value is 32. |

**NEXT CHANGE**

### 9.2.aa TRP ID

The *TRP ID* IE is used to identify a TRP uniquely within an NG-RAN node.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE Type and Reference | Semantics Description |
| TRP Identifier | M |  | INTEGER (1..65535,…) | Identifies a TRP within an NG-RAN node |

### 9.2.bb TRP Information

The *TRP Information* IE contains information for one TRP within an NG-RAN node.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE Type and Reference | Semantics Description |
| TRP ID | M |  | 9.2.aa |  |
| **TRP Information Type** |  | *1 .. <maxnoTRPInfoTypes>* |  |  |
| >CHOICE *TRP Information Item* | M |  |  |  |
| >>NR PCI | M |  | INTEGER (0..1007) | NR Physical Cell ID |
| >>NG-RAN CGI | M |  | 9.2.6 |  |
| >>NR ARFCN | M |  | INTEGER (0..3279165) |  |
| >>PRS Configuration | M |  | 9.2.z6 |  |
| >>SSB Information | M |  | 9.2.z7 |  |
| >>SFN Initialisation Time | M |  | 9.2.y5 |  |
| >>Spatial Direction Information | M |  | 9.2.z8 |  |
| >>Geographical Coordinates | M |  | 9.2.z9 |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoTRPInfoTypes | Maximum no of TRP information types that can be requested and reported with one message. Value is 64. |

9.2.9 NR CGI

The Cell Global Identifier NR is used to globally identify an NR cell.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| PLMN Identity | M |  | 9.2.8 |  |
| NR Cell Identity | M |  | BIT STRING (SIZE(36)) |  |

9.2.cc Search Window Information

This information element contains search window information for the TRP.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE Type and Reference** | **Semantics Description** |
| Expected Propagation Delay | M |  | INTEGER  (-3841..3841,…) | Indicates when the SRS is expected to arrive in time at the TRP relative to the UL RTOA Reference Time.  The UL RTOA Reference Time for a target SRS is defined as , where  -     is the SFN Initialisation Time  -     , where and are the system frame number and the subframe number of the SRS, respectively.  Granularity 4Ts, where Ts=1/(15⋅103 ⋅2048) seconds.  Centre of the search window. |
| Delay Uncertainty | M |  | INTEGER  (1..246,…) | Indicates the uncertainty of the expected SRS arrival time at the TRP  Granularity 4Ts, where Ts=1/(15⋅103⋅2048) seconds.  Single-sided search window. |

### 9.2.x Requested SRS Transmission Characteristics

This IE contains the requested SRS configuration for the UE.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE Type and Reference | Semantics Description |
| Number Of Periodic Transmissions | O |  | INTEGER (0..500,…) | The number of periodic SRS transmissions requested. The value of ‘0’ represents an infinite number of periodic SRS transmissions.  This IE is applicable only if the *Resource Type* IE is set to “periodic”, otherwise, it is ignored. |
| Resource Type | M |  | ENUMERATED (periodic, semi-persistent, aperiodic, …) |  |
| CHOICE *Bandwidth* | M |  |  |  |
| >FR1 |  |  | ENUMERATED (5kHz, 10kHz, 20kHz, 40kHz, 50kHz, 80kHz, 100kHz, ...) |  |
| >FR2 |  |  | ENUMERATED (50kHz, 100kHz, 200kHz, 400kHz,…) |  |
| **SRS Resource Set List** |  | *0.. 1* |  |  |
| **>SRS Resource Set Item** |  | *1..<* *maxnoSRS-ResourceSets>* |  |  |
| >>Number of SRS Resources Per Set | O |  | INTEGER (1..16,...) | The number of SRS Resources per resource set for SRS transmission. |
| **>>Periodicity List** |  | *0.. 1* |  |  |
| **>>>Periodicity List Item** |  | 1..<*maxnoSRS-ResourcePerSet*> |  |  |
| >>>>PeriodicitySRS | M |  | ENUMERATED (0.125, 0.25, 0.5, 0.625, 1, 1.25, 2, 2.5, 4, 5, 8, 10, 16, 20, 32, 40, 64, 80, 160, 320, 640, 1280, 2560, 5120, 10240, …) | Milli-seconds |
| >>Spatial Relation Information | O |  | 9.2.y2 |  |
| >>Pathloss Reference Information | O |  | 9.2.y6 |  |
| SSB Information | O |  | 9.2.z7 |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoSRS-ResourceSets | Maximum no of requested SRS Resource Sets for SRS transmission. Value is 16. |
| maxnoSRS-ResourcePerSet | Maximum no of SRS Resources per set. Value is 16. |

### 9.2.y SRS Configuration

This information element contains the SRS configuration configured by the NG-RAN node for the UE.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE Type and Reference** | **Semantics Description** |
| **SRS Carrier List** |  | *1..<maxnoSRS-Carriers>* |  |  |
| >Point A | M |  | INTEGER (0..3279165,…)  NR ARFCN |  |
| >**Uplink Channel BW-PerSCS-List** |  | *1..<maxnoSCSs>* |  | SCS-SpecificCarrier TS 38.331 [x] |
| >>Offset To Carrier | M |  | INTEGER(0..2199,…) | First usable RB to Point A in the number of PRBs |
| >>Subcarrier Spacing | M |  | ENUMERATED(kHz15, kHz30, kHz60, kHz120,…) |  |
| >>Carrier Bandwidth | M |  | INTEGER(0..275,…) |  |
| >**Active UL BWP** | M |  |  | Only the configuration in the active UL BWP is needed. |
| >>Location And Bandwidth | M |  | INTEGER(0..37949,…) | BWP TS 38.331 [x] |
| >>Subcarrier Spacing | M |  | ENUMERATED(kHz15, kHz30, kHz60, kHz120,…) |  |
| >>Cyclic Prefix | M |  | ENUMERATED(Normal, Extended) |  |
| >>Tx Direct Current Location | M |  | INTEGER(0..3301,…) |  |
| >>Shift7dot5kHz | O |  | ENUMERATED(true,…) |  |
| >>SRS Config | M |  |  |  |
| >>>SRS Resource List |  | *0..1* |  |  |
| >>>>SRS Resource |  | *1..<maxnoSRS-Resources>* | 9.2.ya |  |
| >>>Positioning SRS Resource List |  | *0..1* |  |  |
| >>>>Positioning SRS Resource |  | *1..<maxnoSRS-PosResources>* | 9.2.yb |  |
| >>>SRS Resource Set List |  | *0..1* |  |  |
| >>>>SRS Resource Set |  | *1..<maxnoSRS-ResourceSets>* | 9.2.yc |  |
| >>>Positioning SRS Resource Set List |  | *0..1* |  |  |
| >>>>Positioning SRS Resource Set |  | *1..<maxnoSRS-PosResourceSets>* | 9.2.yd |  |
| >PCI | O |  | INTEGER (0..1007) | Physical Cell ID of the cell that contains the SRS carrier |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoSRS-Carriers | Maximum no of carriers for SRS. Value is 32. |
| maxnoSCSs | Maximum no of SCS spacings for a carrier. Value is 5. |
| maxnoSRS-Resources | Maximum no of SRS resources per UL BWP. Value is 64. |
| maxnoSRS-PosResources | Maximum no of positioning SRS resources per UL BWP. Value is 64. |
| maxnoSRS-ResourceSets | Maximum no of SRS resource sets. Value is 16. |
| maxnoSRS-PosResourceSets | Maximum no of positioning SRS resource sets per UL BWP. Value is 16. |

### 9.2.ya SRS Resource

This information element contains the SRS resource.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE Type and Reference | Semantics Description |
| SRS Resource ID | M |  | INTEGER(0..63) |  |
| Number of Ports | M |  | ENUMERATED(port1, ports2, ports4) |  |
| CHOICE *Transmission Comb* | M |  |  |  |
| >Comb Two |  |  |  |  |
| >>Comb Offset | M |  | INTEGER(0..1) |  |
| >>Cyclic Shift | M |  | INTEGER(0..7) |  |
| >Comb Four |  |  |  |  |
| >>Comb Offset | M |  | INTEGER(0..3) |  |
| >>Cyclic Shift | M |  | INTEGER(0..11) |  |
| Start Position | M |  | INTEGER(0..13) |  |
| Number of Symbols | M |  | ENUMERATED(n1,n2,n4) |  |
| Repetition Factor | M |  | ENUMERATED(r1,r2,r4) |  |
| Frequency Domain Position | M |  | INTEGER(0..67) |  |
| Frequency Domain Shift | M |  | INTEGER(0..268) |  |
| C-SRS | M |  | INTEGER(0..63) |  |
| B-SRS | M |  | INTEGER(0..3) |  |
| B-Hop | M |  | INTEGER(0..3) |  |
| Group or Sequence Hopping | M |  | ENUMERATED(neither, groupHopping, sequenceHopping) |  |
| CHOICE *Resource Type* | M |  |  |  |
| >Periodic |  |  |  |  |
| >>Periodicity | M |  | ENUMERATED(slot1, slot2, slot4, slot5, slot8, slot10, slot16, slot20, slot32, slot40, slot64, slot80, slot160, slot320, slot640, slot1280, slot2560, …) |  |
| >>Offset | M |  | INTEGER(0..2559, …) |  |
| >Semi-persistent |  |  |  |  |
| >>Periodicity | M |  | ENUMERATED(slot1, slot2, slot4, slot5, slot8, slot10, slot16, slot20, slot32, slot40, slot64, slot80, slot160, slot320, slot640, slot1280, slot2560, …) |  |
| >>Offset | M |  | INTEGER(0..2559, …) |  |
| >Aperiodic |  |  |  |  |
| >>Aperiodic Resource Type | M |  | EMUNERATED(true,…) |  |
| Slot Offset | M |  | INTEGER(0..2559) |  |
| Sequence ID | M |  | INTEGER(0..1023) |  |

### 9.2.yb Positioning SRS Resource

This information element contains the SRS resource for positioning.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE Type and Reference | Semantics Description |
| SRS Resource ID | M |  | INTEGER(0..63) |  |
| CHOICE *Transmission Comb* | M |  |  |  |
| >Comb Two |  |  |  |  |
| >>Comb Offset | M |  | INTEGER(0..1) |  |
| >>Cyclic Shift | M |  | INTEGER(0..7) |  |
| >Comb Four |  |  |  |  |
| >>Comb Offset | M |  | INTEGER(0..3) |  |
| >>Cyclic Shift | M |  | INTEGER(0..11) |  |
| >Comb Eight |  |  |  |  |
| >>Comb Offset | M |  | INTEGER(0..7) |  |
| >>Cyclic Shift | M |  | INTEGER(0..5) |  |
| Start Position | M |  | INTEGER(0..13) |  |
| Number of Symbols | M |  | ENUMERATED(n1,n2,n4, n8, n12} |  |
| Frequency Domain Shift | M |  | INTEGER(0..268) |  |
| C-SRS | M |  | INTEGER(0..63) |  |
| Group or Sequence Hopping | M |  | ENUMERATED(Neither, groupHopping, sequenceHopping) |  |
| CHOICE *Resource Type Positioning* | M |  |  |  |
| >periodic |  |  |  |  |
| >>Periodicity |  |  | ENUMERATED(slot, slot2, slot4, slot5, slot8, slot10, slot16, slot20, slot32, slot40, slot64, slot80, slot160, slot320, slot640, slot1280, slot2560, slot5120, slot10240, slot20480, slot40960, slot81920,…) |  |
| >>Offset |  |  | INTEGER(0..81919,…) |  |
| >semi-persistent |  |  |  |  |
| >>Periodicity |  |  | ENUMERATED(1,2,4,5,8,10,16,20,32,40,64,80,160,320,640,1280,2560,5120,10240,20480,40960,81920,…) |  |
| >>Offset |  |  | INTEGER(0..81919,…) |  |
| >aperiodic |  |  |  |  |
| >>slot offset |  |  | INTEGER(1..32) |  |
| Sequence ID | M |  | INTEGER(0..65535) |  |
| CHOICE *Spatial Relation Positioning* | O |  |  |  |
| >SSB | M |  |  |  |
| >>PCI | O |  | INTEGER (0..1007) |  |
| >>SSB index | M |  | INTEGER(0..63) |  |
| >PRS | M |  |  |  |
| >>PRS ID | O |  | INTEGER(0..255) | This IE is absent if the *SRS Configuration* IE is included in the MEASUREMENT REQUEST.  It is optionally present if the *SRS Configuration* IE is included in the POSITIONING INFORMATION RESPONSE/UPDATE messages |
| >>PRS Resource Set ID | M |  | INTEGER(0..7) |  |
| >>PRS Resource ID | M |  | INTEGER(0..63) |  |

9.2.yc SRS Resource Set

This information element indicates an SRS resource set in the UE for UL SRS transmission.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE Type and Reference** | **Semantics Description** |
| SRS Resource Set ID | M |  | INTEGER(0..15) |  |
| SRS Resource ID List |  | 1..<*maxnoSRS-ResourcePerSet*> |  |  |
| >SRS Resource ID | M |  | INTEGER(0..63) |  |
| CHOICE Resource Set Type | M |  |  |  |
| >periodic |  |  |  |  |
| >>periodicSet | M |  | ENUMERATED(true,…) |  |
| >semi-persistent |  |  |  |  |
| >>semi-persistentSet | M |  | ENUMERATED(true,…) |  |
| >aperiodic |  |  |  |  |
| >>SRS Resource Trigger | M |  | INTEGER(1..3) |  |
| >>Slot offset | M |  | INTEGER(1..32) |  |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoSRS-ResourcePerSet | Maximum no of SRS resources per SRS resource set. Value is 16. |

9.2.yd Positioning SRS Resource Set

This information element indicates a positioning SRS resource set in the UE for UL SRS transmission.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE Type and Reference** | **Semantics Description** |
| Positioning SRS Resource Set ID | M |  | INTEGER(0..15) |  |
| Positioning SRS Resource ID List |  | 1..<*maxnoSRS-PosResourcePerSet*> |  |  |
| >Positioning SRS Resource ID | M |  | INTEGER(0..63) |  |
| CHOICE *Resource Type* | M |  |  |  |
| >periodic |  |  |  |  |
| >>PosperiodicSet | M |  | ENUMERATED(true,…) |  |
| >semi-persistent |  |  |  |  |
| >>Possemi-persistentSet | M |  | ENUMERATED(true,…) |  |
| >aperiodic |  |  |  |  |
| >>SRS Resource Trigger | M |  | INTEGER(1..3) |  |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoSRS-PosResourcePerSet | Maximum no of positioning SRS resources per positioning SRS resource set. Value is 16. |

9.2.y1 SRS Resource Set ID

This information element indicates a resource set in the UE for UL SRS transmission.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE Type and Reference** | **Semantics Description** |
| Positioning SRS Resource Set ID | M |  | INTEGER (0..15) | According to TS 38.331 [x] |

9.2.y2 Spatial Relation Information

This information element indicates a spatial relation for transmission of UL SRS by a UE.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE Type and Reference** | **Semantics Description** |
| **Spatial Relation for Resource ID** |  | *1..<maxnoSpatialRelations>* |  | According to TS 38.321 [z] and TS 38.331 [x] |
| CHOICE *Reference Signal* | M |  |  |  |
| >NZP CSI-RS |  |  |  |  |
| >>NZP CSI-RS Resource ID | M |  | INTEGER (0..191) |  |
| >SSB |  |  |  |  |
| >>PCI | M |  | INTEGER (0..1007) |  |
| >>SSB Index | O |  | INTEGER (0..63) |  |
| >SRS |  |  |  |  |
| >>SRS Resource ID | M |  | INTEGER (0..63) |  |
| >Positioning SRS |  |  |  |  |
| >>SRS Pos Resource ID | M |  | INTEGER (0..63) |  |
| >DL-PRS |  |  |  |  |
| >>DL-PRS ID | M |  | INTEGER (0..255) |  |
| >>DL-PRS Resource Set ID | M |  | INTEGER (0..7) |  |
| >>DL PRS Resource ID | O |  | INTEGER (0..63) |  |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoSpatialRelations | Maximum no. of Spatial Relations that can be configured. Value is 64. |

9.2.y3 SRS Resource Trigger

This information element indicates a DCI code point according to a SRS resource set configuration.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE Type and Reference** | **Semantics Description** |
| **Aperiodic SRS Resource Trigger List** |  | *1..<maxnoSRS-TriggerStates>* |  | According to TS 38.331 [x] |
| >Aperiodic SRS Resource Trigger |  |  | INTEGER (1..3) |  |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoSRSTriggerStates | Maximum no. of SRS trigger states. Value is 3. |

9.2.y5 SFN Initialisation Time

This information element indicates the SFN initialisation time.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE Type and Reference** | **Semantics Description** |
| SFN initialisation time | M |  | BIT STRING (SIZE(64)) | Time in seconds relative to 00:00:00 on 1 January 1900 (calculated as continuous time without leap seconds and traceable to a common time reference) where binary encoding of the integer part is in the first 32 bits and binary encoding of the fraction part in the last 32 bits. The fraction part is expressed with a granularity of 1 /2\*\*32 second |

### 9.2.z1 Measurement Result

This information element contains the measurement result.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE Type and Reference | Semantics Description |
| **Measured Result Item** |  | *1 .. <maxnoPosMeas>* |  |  |
| >CHOICE *Measured Results Value* | M |  |  |  |
| >>UL Angle of Arrival | M |  | 9.2.z2 |  |
| >>UL SRS-RSRP | M |  | INTEGER (0..127) |  |
| >>UL RTOA | M |  | 9.2.z |  |
| >>gNB Rx-Tx Time Difference | M |  | 9.2.z10 |  |
| >Time Stamp | M |  | 9.2.z3 |  |
| >Measurement Quality | O |  | 9.2.z4 |  |
| >Measurement Beam Information | O |  | 9.2.aa1 |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoPosMeas | Maximum no. of measured quantities that can be configured and reported with one positioning measurement message. Value is 16384. |

### 9.2.z2 UL Angle of Arrival

This information element contains the uplink Angle of Arrival measurement.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE Type and Reference | Semantics Description |
| Azimuth Angle of Arrival | M |  | INTEGER(0..3599) | TS 38.133 [a] |
| Zenith Angle of Arrival | O |  | INTEGER(0..1799) | TS 38.133 [a] |
| Angle Coordinate System | O |  | ENUMERATED(LCS, GCS) |  |

### 9.2.z UL RTOA Measurement

This information element contains the uplink RTOA measurement.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE Type and Reference | Semantics Description |
| CHOICE *UL RTOA Measurement* | M |  |  |  |
| >k0 | M |  | INTEGER (0.. 1970049) | TS 38.133 [a] |
| >k1 | M |  | INTEGER (0.. 985025) | TS 38.133 [a] |
| >k2 | M |  | INTEGER (0.. 492513) | TS 38.133 [a] |
| >k3 | M |  | INTEGER (0.. 246257) | TS 38.133 [a] |
| >k4 | M |  | INTEGER (0.. 123129) | TS 38.133 [a] |
| >k5 | M |  | INTEGER (0.. 61565) | TS 38.133 [a] |
| Additional Path List | O |  | 9.2.z11 |  |

### 9.2.z10 gNB Rx-Tx Time Difference

This information element contains the gNB Rx-Tx Time Difference measurement.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE Type and Reference | Semantics Description |
| CHOICE *gNB Rx-Tx Time Difference Measurement* | M |  |  |  |
| >k0 | M |  | INTEGER (0.. 1970049) | TS 38.133 [a] |
| >k1 | M |  | INTEGER (0.. 985025) | TS 38.133 [a] |
| >k2 | M |  | INTEGER (0.. 492513) | TS 38.133 [a] |
| >k3 | M |  | INTEGER (0.. 246257) | TS 38.133 [a] |
| >k4 | M |  | INTEGER (0.. 123129) | TS 38.133 [a] |
| >k5 | M |  | INTEGER (0.. 61565) | TS 38.133 [a] |
| Additional Path List | O |  | 9.2.z11 |  |

### 9.2.z11 Additional Path List

This information element contains the additional path results of time measurement.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE Type and Reference | Semantics Description |
| **Additional Path Item** |  | *1..<maxnopath>* |  |  |
| >CHOICE *Relative Path Delay* | M |  |  |  |
| >>k0 | M |  | INTEGER(0..16351,…) |  |
| >>k1 | M |  | INTEGER(0..8176,…) |  |
| >>k2 | M |  | INTEGER(0..4088,…) |  |
| >>k3 | M |  | INTEGER(0..2044,…) |  |
| >>k4 | M |  | INTEGER(0..1022,…) |  |
| >>k5 | M |  | INTEGER(0..511,…) |  |
| >Path Quality | O |  | Measurement Quality  9.2.z4 |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnopath | Maximum no. of additional path measurement. Value is 2. |

### 9.2.z3 Time Stamp

This information element contains the time stamp associated with the measurement.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE Type and Reference | Semantics Description |
| System Frame Number | M |  | INTEGER(0..1023) |  |
| CHOICE *Slot Index* | M |  |  |  |
| >SCS-15 | M |  | INTEGER(0..9) |  |
| >SCS-30 | M |  | INTEGER(0..19) |  |
| >SCS-60 | M |  | INTEGER(0..39) |  |
| >SCS-120 | M |  | INTEGER(0..79) |  |
| Measurement time | O |  | SFN Initialisation Time  9.2.y5 |  |

### 9.2.z4 Measurement Quality

This information element contains the TRP’s best estimate of the quality of the measurement.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE Type and Reference | Semantics Description |
| CHOICE *Measurement Quality* | M |  |  |  |
| >Timing Measurement Quality |  |  |  |  |
| >>Measurement Quality | M |  | INTEGER(0..31) | TS 37.355 [y] |
| >>Resolution | M |  | ENUMERATED(0.1m, 1m, 10m, 30m, …) | TS 37.355 [y] |
| >Angle Measurement Quality |  |  |  |  |
| >>Azimuth Quality | M |  | INTEGER(0..255) |  |
| >>Zenith Quality | O |  | INTEGER(0..255) |  |
| >>Resolution | M |  | ENUMERATED (0.1deg, …) |  |

### 9.2.z6 PRS Configuration

This information element contains the DL PRS configuration for the TRP.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE Type and Reference | Semantics Description |
| **PRS Resource Set List** |  | 1..<maxnoofPRSresourceSet> |  |  |
| >PRS Resource Set ID | M |  | INTEGER(0..7) |  |
| >Subcarrier Spacing | M |  | ENUMERATED(kHz15, kHz30, kHz60, kHz120, …) |  |
| >PRS bandwidth | M |  | INTEGER(1..63) | 24,28,…,272 PRBs |
| >Start PRB | M |  | INTEGER(0..2176) | Starting PRB to Point A |
| >Point A | M |  | INTEGER (0..3279165) | NR ARFCN |
| >Comb Size | M |  | ENUMERATED(2, 4, 6, 12, …) |  |
| >CP Type | M |  | ENUMERATED(normal, extended, …) |  |
| >Resource Set Periodicity | M |  | ENUMERATED(4,5,8,10,16,20,32,40,64,80,160,320,640,1280,2560,5120,10240,20480,40960,81920,…) |  |
| >Resource Set Slot Offset | M |  | INTEGER(0..81919,…) |  |
| >Resource Repetition Factor | M |  | ENUMERATED(rf1,rf2,rf4,rf6,rf8,rf16,rf32,…) |  |
| >Resource Time Gap | M |  | ENUMERATED(tg1,tg2,tg4,tg8,tg16,tg32,…) |  |
| >Resource Number of Symbols | M |  | ENUMERATED(n2,n4,n6,n12,…) |  |
| >PRS Muting | O |  |  |  |
| >>Option1 | O |  |  |  |
| >>>Muting Pattern | M |  | 9.2.z15 |  |
| >>>Muting Bit Repetition Factor | M |  | ENUMERATED(1,2,4,8,…) |  |
| >>Option2 | O |  |  |  |
| >>>Muting Pattern | M |  | DL-PRS Muting Pattern  9.2.z15 |  |
| >PRS Resource Transmit Power | M |  | INTEGER(-60..50) |  |
| >**PRS Resource List** | M | 1..<maxnoofPRSresources> |  |  |
| >>PRS Resource ID | M |  | INTEGER(0..63) |  |
| >>Sequence ID | M |  | INTEGER(0..4095,…) |  |
| >>RE Offset | M |  | INTEGER(0..11) |  |
| >>Resource Slot Offset | M |  | INTEGER(0..511,…) |  |
| >>Resource Symbol Offset | M |  | INTEGER(0..12,…) |  |
| >>QCL Info | O |  |  |  |
| >>>QCL Source SSB Index | O |  | INTEGER(0..63) |  |
| >>>QCL Source PRS Info | O |  |  |  |
| >>>>QCL Source PRS Resource Set ID | M |  | INTEGER(0..7) |  |
| >>>>QCL Source PRS Resource ID | O |  | INTEGER(0..63) | If it is absent, the QCL source PRS resource ID is the same as the PRS resource ID |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofPRSresourceSet | Maximum no of PRS resources set. Value is 8. |
| maxnoofPRSresource | Maximum no of PRS resources per PRS resource set. Value is 64. |

### 9.2.z8 Spatial Direction Information

This information element contains the spatial direction information of the DL PRS resources for the TRP.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE Type and Reference | Semantics Description |
| NR-PRS Beam Information | M |  | 9.2.xx1 | The spatial directions of DL-PRS Resources for TRP |

### 9.2.z9 Geographical Coordinates

This information element contains the geographical coordinates for the TRP.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE Type and Reference** | **Semantics Description** |
| CHOICE *TRP Position Definition Type* | M |  |  |  |
| >*Direct* |  |  |  |  |
| >>CHOICE *Accuracy* | M |  |  |  |
| >>>*normal accuracy* |  |  |  |  |
| >>>>TRP Position | M |  | NG-RAN Access Point Position  9.2.10 | The configured estimated geographical position of the antenna of the cell/TRP. |
| >>>*high accuracy* |  |  |  |  |
| >>>>TRP High Accuracy Access Position | M |  | NG-RAN High Accuracy Access Point Position  9.2.bb1 | The configured estimated geographical high accuracy position of the antenna of the cell/TRP. |
| >*Referenced* |  |  |  |  |
| >>Reference Point | M |  | 9.2.z9d | The reference point is used to derive the TRP position |
| >>CHOICE *Type* | M |  |  |  |
| *>>>Geodetic* |  |  |  |  |
| >>>>TRP Position Relative Geodetic | M |  | Relative Geodetic Location  9.2.z9b | The configured estimated relative geodetic coordinate of the antenna of the cell/TRP |
| *>>>Cartesian* |  |  |  |  |
| >>>>TRP Position Relative Cartesian | M |  | Relative Cartesian Location  9.2.z9c | The configured estimated relative Cartesian coordinate of the antenna of the cell/TRP |
| DL-PRS Resource Coordinates | O |  | 9.2.z9a | DL-PRS Resource Coordinates relative to the TRP coordinate |

### 9.2.z9a DL-PRS Resource Coordinates

This information element contains the geographical coordinates of the antenna reference points (ARP) for the DL-PRS Resources of a TRP.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE Type and Reference** | **Semantics Description** |
| **DL-PRS Resource Set ARP List** | M | *1..<maxPRS-ResourceSets>* |  |  |
| >DL-PRS Resource Set ID | M |  | INTEGER (0..7) |  |
| >CHOICE *DL-PRS Resource Set ARP Location* | M |  |  | Relative to the geographical coordinates for the TRP. If this IE is absent, the Relative Location is zero for the indicated DL-PRS Resource Set ID. |
| *>>Geodetic* |  |  |  |  |
| >>>TRP Position Relative Geodetic | M |  | Relative Geodetic Location 9.2.z9b |  |
| *>>Cartesian* |  |  |  |  |
| >>>TRP Position Relative Cartesian | M |  | Relative Cartesian Location 9.2.z9c |  |
| >**DL-PRS Resource ARP List** | M | *1..<maxPRS-ResourcesPerSet>* |  |  |
| >>DL-PRS Resource ID | M |  | INTEGER (0..63) |  |
| >>CHOICE *DL-PRS Resource ARP Location* | M |  |  | Relative to the DL-PRS Resource Set ARP Location.  If this IE is absent, the Relative Location is zero for the indicated DL-PRS Resource ID. |
| >>>*Geodetic* |  |  |  |  |
| >>>TRP Position Relative Geodetic | M |  | Relative Geodetic Location 9.2.z9b |  |
| *>>>Cartesian* |  |  |  |  |
| >>>TRP Position Relative Cartesian | M |  | Relative Cartesian Location 9.2.z9c |  |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxPRS-ResourceSets | Maximum no of DL-PRS resource sets per TRP. Value is 2. |
| maxPRS-ResourcesPerSet | Maximum no of DL-PRS resources of the DL-PRS resource set of the TRP. Value is 64. |

### 9.2.z9b Relative Geodetic Location

This information element provides a location relative to some known reference location in a relative geodetic coordinate system.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE Type and Reference** | **Semantics Description** |
| Milli-Arc-Second Units | M |  | ENUMERATED (0.03, 0.3, 3, ...) | Units and scale factor for the delta-latitude and delta-longitude fields. 0.03, 0.3, 3, milliarcseconds. TS 37.355 [y]. |
| Height Units | M |  | ENUMERATED (mm, cm, m, ...) | Units and scale factor for the delta-height field.  10-3 metre, 10-2 metre, TS 37.355 [y]. |
| Delta Latitude | M |  | INTEGER (-1024..1023) | Delta value in latitude in the unit provided in Milli-Arc-Second Units. TS 37.355 [y]. |
| Delta Longitude | M |  | INTEGER (-1024..1023) | Delta value in longitude in the unit provided in Milli-Arc-Second Units. TS 37.355 [y]. |
| Delta Height | M |  | INTEGER (-1024..1023) | Delta value in ellipsoidal height in the unit provided in Height Units. TS 37.355 [y]. |
| Location uncertainty | M |  | 9.2.z9e |  |

### 9.2.bb1 NG-RAN High Accuracy Access Point Position

The *NG-RAN High Accuracy Access Point Position* IE is used to identify the geographical position of an NG-RAN Access Point. It is expressed as High Accuracy Ellipsoid point with altitude and uncertainty ellipsoid according to TS 23.032 [8].

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE Type and Reference | Semantics Description |
| Degrees of Latitude | M |  | INTEGER(-2147483648..2147483647) |  |
| Degrees of Longitude | M |  | INTEGER(-2147483648..2147483647) |  |
| Altitude | M |  | INTEGER(-64000..1280000) |  |
| Uncertainty Semi Major | M |  | INTEGER (0..255) |  |
| Uncertainty Semi Minor | M |  | INTEGER (0..255) |  |
| Orientation Major Axis | M |  | INTEGER (0..179) |  |
| Horizontal Confidence | M |  | INTEGER (0..100) |  |
| Uncertainty Altitude | M |  | INTEGER (0..255) |  |
| Vertical Confidence | M |  | INTEGER (0..100) |  |

### 9.2.z9c Relative Cartesian Location

This information element provides a location relative to some known reference location in a relative Cartesian coordinate system.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE Type and Reference** | **Semantics Description** |
| XYZ unit | M |  | ENUMERATED (mm, cm, dm,..) |  |
| X value | M |  | INTEGER  (-216.. 216-1) | Positive value represents northing from reference point, in units of *XYZ Unit* IE. |
| Y value | M |  | INTEGER  (-216.. 216-1) | Positive value represents easting from reference point in units of *XYZ Unit* IE. |
| Z value | M |  | INTEGER  (-215.. 215-1) | Positive value represents height above reference point in units of *XYZ Unit* IE. |
| Location uncertainty | M |  | 9.2.z9e |  |

9.2.z9d Reference Point

This information element provides a reference point information.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE Type and Reference** | **Semantics Description** |
| CHOICE *ReferencePoint* | M |  |  | Reference point to which relative location information is related to |
| >Coordinate ID |  |  |  |  |
| >>Coordinate ID | M |  | INTEGER(0.. 29-1,..) | Referential ID mapped via OAM |
| >Reference Point Coordinates |  |  |  |  |
| >>Reference Point Position | M |  | NG-RAN Access Point Position  9.2.10 |  |
| >Reference Point Coordinates High Accuracy |  |  |  |  |
| >>Reference Point High Accuracy Access Position | M |  | NG-RAN High Accuracy Access Point Position  9.2.bb1 |  |

9.2.z9e Location Uncertainty

This information element provides the location uncertainty information.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE Type and Reference** | **Semantics Description** |
| >Horizontal Uncertainty | M |  | INTEGER (0..255) | Horizontal uncertainty of the ARP latitude/longitude. Corresponds to the encoded high accuracy uncertainty as defined in TS 23.032 [8] |
| >Horizontal Confidence | M |  | INTEGER (0..100) | Corresponds to confidence as defined in TS 23.032 [8]. |
| >Vertical Uncertainty | M |  | INTEGER (0..255) | Vertical uncertainty of the ARP altitude. Corresponds to the encoded high accuracy uncertainty as defined in TS 23.032 [8] |
| >Vertical Confidence | M |  | INTEGER (0..100) | Corresponds to confidence as defined in TS 23.032 [8]. |

9.2.y6 Pathloss Reference Information

This information element indicates a pathloss reference for transmission of UL SRS by a UE.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE Type and Reference** | **Semantics Description** |
| CHOICE *Pathloss Reference Signal* | M |  |  |  |
| >*SSB* |  |  |  |  |
| >>PCI | M |  | INTEGER (0..1007) |  |
| >>SSB Index | O |  | INTEGER (0..63) |  |
| >*DL-PRS* |  |  |  |  |
| >>DL-PRS ID | M |  | INTEGER (0..255) |  |
| >>DL-PRS Resource Set ID | M |  | INTEGER (0..7) |  |
| >>DL PRS Resource ID | O |  | INTEGER (0..63) |  |

### 9.2.z7 SSB Information

This information element contains the SSB time/frequency information for the TRPs.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE Type and Reference | Semantics Description |
| **SSB Info List** |  | *1…<maxNoSSBs>* |  |  |
| >SSB Configuration | M |  | SSB Time/Frequency Configuration  9.2.z12 |  |
| >PCI | M |  | INTEGER (0..1007) |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxNoSSBs | Maximum no of SSBs for which the configuration can be provided. Value is 255. |

9.2.z12 SSB Time/Frequency Configuration

This information element contains the time and frequency configuration of an SSB.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE Type and Reference** | **Semantics Description** |
| SSB frequency | M |  | INTEGER (0..3279165) | ARFCN |
| SSB subcarrier spacing | M |  | ENUMERATED(15kHz, 30kHz, 60kHz, 120kHz, 240kHz,...) |  |
| SSB Transmit power | M |  | INTEGER (-60..50) | EPRE of SSS |
| SSB periodicity | M |  | ENUMERATED(5ms, 10ms, 20ms, 40ms, 80ms, 160ms, …) |  |
| SSB half frame index | M |  | INTEGER(0..1) |  |
| SSB SFN offset | M |  | INTEGER(0..15) |  |
| CHOICE SSB Position in Burst | O |  |  |  |
| >Short Bitmap |  |  | BIT STRING (SIZE(4)) |  |
| >Medium Bitmap |  |  | BIT STRING (SIZE(8)) |  |
| >Long Bitmap |  |  | BIT STRING (SIZE(64)) |  |
| SFN initialisation time | O |  | 9.2.y5 |  |

9.2.z15 DL-PRS Muting Pattern

This information element contains the DL-PRS muting pattern.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE Type and Reference** | **Semantics Description** |
| CHOICE DL-*PRS Muting Pattern* | M |  |  |  |
| >Two | M |  | BIT STRING (SIZE(2)) |  |
| >Four | M |  | BIT STRING (SIZE(4)) |  |
| >Six | M |  | BIT STRING (SIZE(6)) |  |
| >Eight | M |  | BIT STRING (SIZE(8)) |  |
| >Sixteen | M |  | BIT STRING (SIZE(16)) |  |
| >Thirty-two | M |  | BIT STRING (SIZE(32)) |  |

### 9.2.aa1 Measurement Beam Information

This information element contains the receiving beam information when measuring UL signals.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE Type and Reference | Semantics Description |
| PRS Resource ID | O |  | INTEGER(0..63) |  |
| PRS Resource Set ID | O |  | INTEGER(0..7) |  |
| SSB Index | O |  | INTEGER(0..63) |  |

9.2.xx1 NR-PRS Beam Information

This IE contains spatial direction information of the DL-PRS Resources.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| **NR-PRS Beam Information** |  | *1 .. <* *maxPRS-ResourceSets >* |  |  |
| >PRS Resource Set ID | M |  | INTEGER (0..7) | The resource set in which the resources are associated with the angle. |
| **>PRS Angle Item** |  | *1..<* *maxPRS-ResourcesPerSet >* |  |  |
| >>NR PRS Azimuth | M |  | INTEGER (0..359) |  |
| >>NR PRS Azimuth fine | O |  | INTEGER (0..9) | Fine angles |
| >>NR PRS Elevation | O |  | INTEGER (0..180) |  |
| >>NR PRS Elevation fine | O |  | INTEGER (0..9) | Fine angles |
| **LCS to GCS Translation** |  | *1 .. <maxnolcs-gcs-translation>* |  | Only the single value, 1, shall be used in this version of the specifications |
| >Alpha | M |  | INTEGER (0..359) |  |
| >Alpha-fine | O |  | INTEGER (0..9) | Fine angles |
| >Beta | M |  | INTEGER (0..359) |  |
| >Beta-fine | O |  | INTEGER (0..9) | Fine angles |
| >Gamma | M |  | INTEGER (0..359) |  |
| >Gamma-fine | O |  | INTEGER (0..9) | Fine angles |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxPRS-ResourceSets | Maximum no of DL-PRS resource sets per TRP. Value is 2. |
| maxPRS-ResourcesPerSet | Maximum no of DL-PRS resources of the DL-PRS resource set of the TRP. Value is 64. |
| maxnolcs-gcs-translation | Maximum no. of LCS-GS-Translation-Parameters that can reported with one message. Value is 3. |

9.2.xx2 Positioning Broadcast Cells

This IE is used to indicate the cells that are requested to broadcast, or failed to broadcast, the associated posSIB(s).

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| **Positioning Broadcast Cells** |  | *1 .. <maxnoBcastCell>* |  |  |
| >NG-RAN-CGI | M |  | 9.2.6 |  |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoBcastCells | Maximum no. of cells broadcasting a posSIB in a NG-RAN node. Value is 16384. |

**NEXT CHANGE**

### 9.3.3 Elementary Procedure Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Elementary Procedure definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

NRPPA-PDU-Descriptions {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-access (22) modules (3) nrppa (4) version1 (1) nrppa-PDU-Descriptions (0) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IE parameter types from other modules.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

IMPORTS

Criticality,

ProcedureCode,

NRPPATransactionID

FROM NRPPA-CommonDataTypes

ErrorIndication,

PrivateMessage,

E-CIDMeasurementInitiationRequest,

E-CIDMeasurementInitiationResponse,

E-CIDMeasurementInitiationFailure,

E-CIDMeasurementFailureIndication,

E-CIDMeasurementReport,

E-CIDMeasurementTerminationCommand,

OTDOAInformationRequest,

OTDOAInformationResponse,

OTDOAInformationFailure,

AssistanceInformationControl,

AssistanceInformationFeedback,

PositioningInformationRequest,

PositioningInformationResponse,

PositioningInformationFailure,

PositioningInformationUpdate,

MeasurementRequest,

MeasurementResponse,

MeasurementFailure,

MeasurementReport,

MeasurementUpdate,

MeasurementAbort,

MeasurementFailureIndication,

TRPInformationRequest,

TRPInformationResponse,

TRPInformationFailure,

PositioningActivationRequest,

PositioningActivationResponse,

PositioningActivationFailure,

PositioningDeactivation

FROM NRPPA-PDU-Contents

id-errorIndication,

id-privateMessage,

id-e-CIDMeasurementInitiation,

id-e-CIDMeasurementFailureIndication,

id-e-CIDMeasurementReport,

id-e-CIDMeasurementTermination,

id-oTDOAInformationExchange,

id-assistanceInformationControl,

id-assistanceInformationFeedback,

id-positioningInformationExchange,

id-positioningInformationUpdate,

id-Measurement,

id-MeasurementReport,

id-MeasurementUpdate,

id-MeasurementAbort,

id-MeasurementFailureIndication,

id-tRPInformationExchange,

id-positioningActivation,

id-positioningDeactivation

FROM NRPPA-Constants;

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Interface Elementary Procedure Class

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

NRPPA-ELEMENTARY-PROCEDURE ::= CLASS {

&InitiatingMessage ,

&SuccessfulOutcome OPTIONAL,

&UnsuccessfulOutcome OPTIONAL,

&procedureCode ProcedureCode UNIQUE,

&criticality Criticality DEFAULT ignore

}

WITH SYNTAX {

INITIATING MESSAGE &InitiatingMessage

[SUCCESSFUL OUTCOME &SuccessfulOutcome]

[UNSUCCESSFUL OUTCOME &UnsuccessfulOutcome]

PROCEDURE CODE &procedureCode

[CRITICALITY &criticality]

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Interface PDU Definition

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

NRPPA-PDU ::= CHOICE {

initiatingMessage InitiatingMessage,

successfulOutcome SuccessfulOutcome,

unsuccessfulOutcome UnsuccessfulOutcome,

...

}

InitiatingMessage ::= SEQUENCE {

procedureCode NRPPA-ELEMENTARY-PROCEDURE.&procedureCode ({NRPPA-ELEMENTARY-PROCEDURES}),

criticality NRPPA-ELEMENTARY-PROCEDURE.&criticality ({NRPPA-ELEMENTARY-PROCEDURES}{@procedureCode}),

nrppatransactionID NRPPATransactionID,

value NRPPA-ELEMENTARY-PROCEDURE.&InitiatingMessage ({NRPPA-ELEMENTARY-PROCEDURES}{@procedureCode})

}

SuccessfulOutcome ::= SEQUENCE {

procedureCode NRPPA-ELEMENTARY-PROCEDURE.&procedureCode ({NRPPA-ELEMENTARY-PROCEDURES}),

criticality NRPPA-ELEMENTARY-PROCEDURE.&criticality ({NRPPA-ELEMENTARY-PROCEDURES}{@procedureCode}),

nrppatransactionID NRPPATransactionID,

value NRPPA-ELEMENTARY-PROCEDURE.&SuccessfulOutcome ({NRPPA-ELEMENTARY-PROCEDURES}{@procedureCode})

}

UnsuccessfulOutcome ::= SEQUENCE {

procedureCode NRPPA-ELEMENTARY-PROCEDURE.&procedureCode ({NRPPA-ELEMENTARY-PROCEDURES}),

criticality NRPPA-ELEMENTARY-PROCEDURE.&criticality ({NRPPA-ELEMENTARY-PROCEDURES}{@procedureCode}),

nrppatransactionID NRPPATransactionID,

value NRPPA-ELEMENTARY-PROCEDURE.&UnsuccessfulOutcome ({NRPPA-ELEMENTARY-PROCEDURES}{@procedureCode})

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Interface Elementary Procedure List

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

NRPPA-ELEMENTARY-PROCEDURES NRPPA-ELEMENTARY-PROCEDURE ::= {

NRPPA-ELEMENTARY-PROCEDURES-CLASS-1 |

NRPPA-ELEMENTARY-PROCEDURES-CLASS-2 ,

...

}

NRPPA-ELEMENTARY-PROCEDURES-CLASS-1 NRPPA-ELEMENTARY-PROCEDURE ::= {

e-CIDMeasurementInitiation |

oTDOAInformationExchange |

positioningInformationExchange |

measurement |

tRPInformationExchange |

positioningActivation,

...

}

NRPPA-ELEMENTARY-PROCEDURES-CLASS-2 NRPPA-ELEMENTARY-PROCEDURE ::= {

e-CIDMeasurementFailureIndication |

e-CIDMeasurementReport |

e-CIDMeasurementTermination |

errorIndication |

privateMessage  |

assistanceInformationControl |

assistanceInformationFeedback |

positioningInformationUpdate |

measurementReport |

measurementUpdate |

measurementAbort |

measurementFailureIndication |

positioningDeactivation,

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Interface Elementary Procedures

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

e-CIDMeasurementInitiation NRPPA-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE E-CIDMeasurementInitiationRequest

SUCCESSFUL OUTCOME E-CIDMeasurementInitiationResponse

UNSUCCESSFUL OUTCOME E-CIDMeasurementInitiationFailure

PROCEDURE CODE id-e-CIDMeasurementInitiation

CRITICALITY reject

}

e-CIDMeasurementFailureIndication NRPPA-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE E-CIDMeasurementFailureIndication

PROCEDURE CODE id-e-CIDMeasurementFailureIndication

CRITICALITY ignore

}

e-CIDMeasurementReport NRPPA-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE E-CIDMeasurementReport

PROCEDURE CODE id-e-CIDMeasurementReport

CRITICALITY ignore

}

e-CIDMeasurementTermination NRPPA-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE E-CIDMeasurementTerminationCommand

PROCEDURE CODE id-e-CIDMeasurementTermination

CRITICALITY reject

}

oTDOAInformationExchange NRPPA-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE OTDOAInformationRequest

SUCCESSFUL OUTCOME OTDOAInformationResponse

UNSUCCESSFUL OUTCOME OTDOAInformationFailure

PROCEDURE CODE id-oTDOAInformationExchange

CRITICALITY reject

}

assistanceInformationControl NRPPA-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE AssistanceInformationControl

PROCEDURE CODE id-assistanceInformationControl

CRITICALITY reject

}

assistanceInformationFeedback NRPPA-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE AssistanceInformationFeedback

PROCEDURE CODE id-assistanceInformationFeedback

CRITICALITY reject

}

errorIndication NRPPA-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE ErrorIndication

PROCEDURE CODE id-errorIndication

CRITICALITY ignore

}

privateMessage NRPPA-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE PrivateMessage

PROCEDURE CODE id-privateMessage

CRITICALITY ignore

}

positioningInformationExchange NRPPA-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE PositioningInformationRequest

SUCCESSFUL OUTCOME PositioningInformationResponse

UNSUCCESSFUL OUTCOME PositioningInformationFailure

PROCEDURE CODE id-positioningInformationExchange

CRITICALITY reject

}

positioningInformationUpdate NRPPA-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE PositioningInformationUpdate

PROCEDURE CODE id-positioningInformationUpdate

CRITICALITY ignore

}

measurement NRPPA-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE MeasurementRequest

SUCCESSFUL OUTCOME MeasurementResponse

UNSUCCESSFUL OUTCOME MeasurementFailure

PROCEDURE CODE id-Measurement

CRITICALITY reject

}

measurementReport NRPPA-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE MeasurementReport

PROCEDURE CODE id-MeasurementReport

CRITICALITY ignore

}

measurementUpdate NRPPA-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE MeasurementUpdate

PROCEDURE CODE id-MeasurementUpdate

CRITICALITY ignore

}

measurementAbort NRPPA-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE MeasurementAbort

PROCEDURE CODE id-MeasurementAbort

CRITICALITY ignore

}

measurementFailureIndication NRPPA-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE MeasurementFailureIndication

PROCEDURE CODE id-MeasurementFailureIndication

CRITICALITY ignore

}

tRPInformationExchange NRPPA-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE TRPInformationRequest

SUCCESSFUL OUTCOME TRPInformationResponse

UNSUCCESSFUL OUTCOME TRPInformationFailure

PROCEDURE CODE id-tRPInformationExchange

CRITICALITY reject

}

positioningActivation NRPPA-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE PositioningActivationRequest

SUCCESSFUL OUTCOME PositioningActivationResponse

UNSUCCESSFUL OUTCOME PositioningActivationFailure

PROCEDURE CODE id-positioningActivation

CRITICALITY reject

}

positioningDeactivation NRPPA-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE PositioningDeactivation

PROCEDURE CODE id-positioningDeactivation

CRITICALITY ignore

}

END

-- ASN1STOP

### 9.3.4 PDU Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU definitions for NRPPa.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

NRPPA-PDU-Contents {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-access (22) modules (3) nrppa (4) version1 (1) nrppa-PDU-Contents (1) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IE parameter types from other modules.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

IMPORTS

Cause,

CriticalityDiagnostics,

E-CID-MeasurementResult,

OTDOACells,

OTDOA-Information-Item,

Measurement-ID,

UE-Measurement-ID,

MeasurementPeriodicity,

MeasurementQuantities,

ReportCharacteristics,

RequestedSRSTransmissionCharacteristics,

Cell-Portion-ID,

OtherRATMeasurementQuantities,

OtherRATMeasurementResult,

WLANMeasurementQuantities,

WLANMeasurementResult,

Assistance-Information,

Broadcast,

AssistanceInformationFailureList,

SRSConfiguration,

TRPMeasurementQuantities,

TrpMeasurementResult,

TRP-ID,

TRPInformationTypeList,

TRPInformationList,

TRP-MeasurementRequestList,

TRP-MeasurementResponseList,

MeasurementBeamInfoRequest,

PositioningBroadcastCells,

ActivationTime,

SRSResourceSetID,

SRSSpatialRelation,

SRSResourceTrigger,

TRPList,

AbortTransmission,

SystemFrameNumber,

SlotNumber,

SFNInitialisationTime

FROM NRPPA-IEs

PrivateIE-Container{},

ProtocolExtensionContainer{},

ProtocolIE-Container{},

ProtocolIE-ContainerList{},

ProtocolIE-Single-Container{},

NRPPA-PRIVATE-IES,

NRPPA-PROTOCOL-EXTENSION,

NRPPA-PROTOCOL-IES

FROM NRPPA-Containers

maxnoOTDOAtypes,

id-Cause,

id-CriticalityDiagnostics,

id-LMF-Measurement-ID,

id-LMF-UE-Measurement-ID,

id-OTDOACells,

id-OTDOA-Information-Type-Group,

id-OTDOA-Information-Type-Item,

id-ReportCharacteristics,

id-MeasurementPeriodicity,

id-MeasurementQuantities,

id-RAN-Measurement-ID,

id-RAN-UE-Measurement-ID,

id-E-CID-MeasurementResult,

id-RequestedSRSTransmissionCharacteristics,

id-Cell-Portion-ID,

id-OtherRATMeasurementQuantities,

id-OtherRATMeasurementResult,

id-WLANMeasurementQuantities,

id-WLANMeasurementResult,

id-Assistance-Information,

id-Broadcast,

id-AssistanceInformationFailureList,

id-SRSConfiguration,

id-TRPMeasurementQuantities,

id-MeasurementResult,

id-TRP-ID,

id-TRPInformationTypeList,

id-TRPInformationList,

id-TRP-MeasurementRequestList,

id-TRP-MeasurementResponseList,

id-TRP-MeasurementReportList,

id-MeasurementBeamInfoRequest,

id-PositioningBroadcastCells,

id-SRSType,

id-ActivationTime,

id-SRSResourceSetID,

id-TRPList,

id-SRSSpatialRelation,

id-AbortTransmission,

id-SystemFrameNumber,

id-SlotNumber,

id-SRSResourceTrigger,

id-SFNInitialisationTime

FROM NRPPA-Constants;

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- E-CID MEASUREMENT INITIATION REQUEST

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E-CIDMeasurementInitiationRequest ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{E-CIDMeasurementInitiationRequest-IEs}},

...

}

E-CIDMeasurementInitiationRequest-IEs NRPPA-PROTOCOL-IES ::= {

{ ID id-LMF-UE-Measurement-ID CRITICALITY reject TYPE UE-Measurement-ID PRESENCE mandatory}|

{ ID id-ReportCharacteristics CRITICALITY reject TYPE ReportCharacteristics PRESENCE mandatory}|

{ ID id-MeasurementPeriodicity CRITICALITY reject TYPE MeasurementPeriodicity PRESENCE conditional}|

-- The IE shall be present if the Report Characteritics IE is set to “periodic” --

{ ID id-MeasurementQuantities CRITICALITY reject TYPE MeasurementQuantities PRESENCE mandatory}|

{ ID id-OtherRATMeasurementQuantities CRITICALITY ignore TYPE OtherRATMeasurementQuantities PRESENCE optional}|

{ ID id-WLANMeasurementQuantities CRITICALITY ignore TYPE WLANMeasurementQuantities PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- E-CID MEASUREMENT INITIATION RESPONSE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E-CIDMeasurementInitiationResponse ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{E-CIDMeasurementInitiationResponse-IEs}},

...

}

E-CIDMeasurementInitiationResponse-IEs NRPPA-PROTOCOL-IES ::= {

{ ID id-LMF-UE-Measurement-ID CRITICALITY reject TYPE UE-Measurement-ID PRESENCE mandatory}|

{ ID id-RAN-UE-Measurement-ID CRITICALITY reject TYPE UE-Measurement-ID PRESENCE mandatory}|

{ ID id-E-CID-MeasurementResult CRITICALITY ignore TYPE E-CID-MeasurementResult PRESENCE optional}|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional}|

{ ID id-Cell-Portion-ID CRITICALITY ignore TYPE Cell-Portion-ID PRESENCE optional}|

{ ID id-OtherRATMeasurementResult CRITICALITY ignore TYPE OtherRATMeasurementResult PRESENCE optional}|

{ ID id-WLANMeasurementResult CRITICALITY ignore TYPE WLANMeasurementResult PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- E-CID MEASUREMENT INITIATION FAILURE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E-CIDMeasurementInitiationFailure ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{E-CIDMeasurementInitiationFailure-IEs}},

...

}

E-CIDMeasurementInitiationFailure-IEs NRPPA-PROTOCOL-IES ::= {

{ ID id-LMF-UE-Measurement-ID CRITICALITY reject TYPE UE-Measurement-ID PRESENCE mandatory}|

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory}|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- E-CID MEASUREMENT FAILURE INDICATION

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E-CIDMeasurementFailureIndication ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{E-CIDMeasurementFailureIndication-IEs}},

...

}

E-CIDMeasurementFailureIndication-IEs NRPPA-PROTOCOL-IES ::= {

{ ID id-LMF-UE-Measurement-ID CRITICALITY reject TYPE UE-Measurement-ID PRESENCE mandatory}|

{ ID id-RAN-UE-Measurement-ID CRITICALITY reject TYPE UE-Measurement-ID PRESENCE mandatory}|

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- E-CID MEASUREMENT REPORT

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E-CIDMeasurementReport ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{E-CIDMeasurementReport-IEs}},

...

}

E-CIDMeasurementReport-IEs NRPPA-PROTOCOL-IES ::= {

{ ID id-LMF-UE-Measurement-ID CRITICALITY reject TYPE UE-Measurement-ID PRESENCE mandatory}|

{ ID id-RAN-UE-Measurement-ID CRITICALITY reject TYPE UE-Measurement-ID PRESENCE mandatory}|

{ ID id-E-CID-MeasurementResult CRITICALITY ignore TYPE E-CID-MeasurementResult PRESENCE mandatory}|

{ ID id-Cell-Portion-ID CRITICALITY ignore TYPE Cell-Portion-ID PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- E-CID MEASUREMENT TERMINATION

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E-CIDMeasurementTerminationCommand ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{E-CIDMeasurementTerminationCommand-IEs}},

...

}

E-CIDMeasurementTerminationCommand-IEs NRPPA-PROTOCOL-IES ::= {

{ ID id-LMF-UE-Measurement-ID CRITICALITY reject TYPE UE-Measurement-ID PRESENCE mandatory}|

{ ID id-RAN-UE-Measurement-ID CRITICALITY reject TYPE UE-Measurement-ID PRESENCE mandatory},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- OTDOA INFORMATION REQUEST

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

OTDOAInformationRequest ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{OTDOAInformationRequest-IEs}},

...

}

OTDOAInformationRequest-IEs NRPPA-PROTOCOL-IES ::= {

{ ID id-OTDOA-Information-Type-Group CRITICALITY reject TYPE OTDOA-Information-Type PRESENCE mandatory},

...

}

OTDOA-Information-Type ::= SEQUENCE (SIZE(1..maxnoOTDOAtypes)) OF ProtocolIE-Single-Container { { OTDOA-Information-TypeIEs} }

OTDOA-Information-TypeIEs NRPPA-PROTOCOL-IES ::= {

{ ID id-OTDOA-Information-Type-Item CRITICALITY reject TYPE OTDOA-Information-Type-Item PRESENCE mandatory},

...

}

OTDOA-Information-Type-Item ::= SEQUENCE {

oTDOA-Information-Type-Item OTDOA-Information-Item,

iE-Extensions ProtocolExtensionContainer { { OTDOA-Information-Type-ItemExtIEs} } OPTIONAL,

...

}

OTDOA-Information-Type-ItemExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- OTDOA INFORMATION RESPONSE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

OTDOAInformationResponse ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{OTDOAInformationResponse-IEs}},

...

}

OTDOAInformationResponse-IEs NRPPA-PROTOCOL-IES ::= {

{ ID id-OTDOACells CRITICALITY ignore TYPE OTDOACells PRESENCE mandatory}|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- OTDOA INFORMATION FAILURE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

OTDOAInformationFailure ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{OTDOAInformationFailure-IEs}},

...

}

OTDOAInformationFailure-IEs NRPPA-PROTOCOL-IES ::= {

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory}|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- ASSISTANCE INFORMATION CONTROL

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

AssistanceInformationControl ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{AssistanceInformationControl-IEs}},

...

}

AssistanceInformationControl-IEs NRPPA-PROTOCOL-IES ::= {

{ ID id-Assistance-Information CRITICALITY reject TYPE Assistance-Information PRESENCE optional}|

{ ID id-Broadcast CRITICALITY reject TYPE Broadcast PRESENCE optional}|

{ ID id-PositioningBroadcastCells CRITICALITY reject TYPE PositioningBroadcastCells PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- ASSISTANCE INFORMATION FEEDBACK

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

AssistanceInformationFeedback ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{AssistanceInformationFeedback-IEs}},

...

}

AssistanceInformationFeedback-IEs NRPPA-PROTOCOL-IES ::= {

{ ID id-AssistanceInformationFailureList CRITICALITY reject TYPE AssistanceInformationFailureList PRESENCE optional}|

{ ID id-PositioningBroadcastCells CRITICALITY reject TYPE PositioningBroadcastCells PRESENCE optional}|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- ERROR INDICATION

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ErrorIndication ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ErrorIndication-IEs}},

...

}

ErrorIndication-IEs NRPPA-PROTOCOL-IES ::= {

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE optional}|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PRIVATE MESSAGE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PrivateMessage ::= SEQUENCE {

privateIEs PrivateIE-Container {{PrivateMessage-IEs}},

...

}

PrivateMessage-IEs NRPPA-PRIVATE-IES ::= {

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- POSITIONING INFORMATION REQUEST

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PositioningInformationRequest ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{PositioningInformationRequest-IEs}},

...

}

PositioningInformationRequest-IEs NRPPA-PROTOCOL-IES ::= {

{ ID id-RequestedSRSTransmissionCharacteristics CRITICALITY ignore TYPE RequestedSRSTransmissionCharacteristics PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- POSITIONING INFORMATION RESPONSE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PositioningInformationResponse ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{PositioningInformationResponse-IEs}},

...

}

PositioningInformationResponse-IEs NRPPA-PROTOCOL-IES ::= {

{ ID id-SRSConfiguration CRITICALITY ignore TYPE SRSConfiguration PRESENCE optional}|

{ ID id-SFNInitialisationTime CRITICALITY ignore TYPE SFNInitialisationTime PRESENCE optional}|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- POSITIONING INFORMATION FAILURE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PositioningInformationFailure ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{PositioningInformationFailure-IEs}},

...

}

PositioningInformationFailure-IEs NRPPA-PROTOCOL-IES ::= {

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory}|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- POSITIONING INFORMATION UPDATE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PositioningInformationUpdate ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{PositioningInformationUpdate-IEs}},

...

}

PositioningInformationUpdate-IEs NRPPA-PROTOCOL-IES ::= {

{ ID id-SRSConfiguration CRITICALITY ignore TYPE SRSConfiguration PRESENCE optional}|

{ ID id-SFNInitialisationTime CRITICALITY ignore TYPE SFNInitialisationTime PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- MEASUREMENT REQUEST

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

MeasurementRequest ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{MeasurementRequest-IEs}},

...

}

MeasurementRequest-IEs NRPPA-PROTOCOL-IES ::= {

{ ID id-LMF-Measurement-ID CRITICALITY reject TYPE Measurement-ID PRESENCE mandatory}|

{ ID id-TRP-MeasurementRequestList CRITICALITY reject TYPE TRP-MeasurementRequestList PRESENCE mandatory}|

{ ID id-ReportCharacteristics CRITICALITY reject TYPE ReportCharacteristics PRESENCE mandatory}|

{ ID id-MeasurementPeriodicity CRITICALITY reject TYPE MeasurementPeriodicity PRESENCE conditional}|

-- The IE shall be present if the Report Characteritics IE is set to “periodic” –

{ ID id-TRPMeasurementQuantities CRITICALITY reject TYPE TRPMeasurementQuantities PRESENCE mandatory}|

{ ID id-SRSConfiguration CRITICALITY ignore TYPE SRSConfiguration PRESENCE optional}|

{ ID id-SFNInitialisationTime CRITICALITY ignore TYPE SFNInitialisationTime PRESENCE optional}|

{ ID id-MeasurementBeamInfoRequest CRITICALITY ignore TYPE MeasurementBeamInfoRequest PRESENCE optional}|

{ ID id-SystemFrameNumber CRITICALITY ignore TYPE SystemFrameNumber PRESENCE optional}|

{ ID id-SlotNumber CRITICALITY ignore TYPE SlotNumber PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- MEASUREMENT RESPONSE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

MeasurementResponse ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{MeasurementResponse-IEs}},

...

}

MeasurementResponse-IEs NRPPA-PROTOCOL-IES ::= {

{ ID id-LMF-Measurement-ID CRITICALITY reject TYPE Measurement-ID PRESENCE mandatory}|

{ ID id-RAN-Measurement-ID CRITICALITY reject TYPE Measurement-ID PRESENCE mandatory}|

{ ID id-TRP-MeasurementResponseList CRITICALITY reject TYPE TRP-MeasurementResponseList PRESENCE mandatory}|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- MEASUREMENT FAILURE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

MeasurementFailure ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{MeasurementFailure-IEs}},

...

}

MeasurementFailure-IEs NRPPA-PROTOCOL-IES ::= {

{ ID id-LMF-Measurement-ID CRITICALITY reject TYPE Measurement-ID PRESENCE mandatory}|

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory}|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- MEASUREMENT REPORT

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

MeasurementReport ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{MeasurementReport-IEs}},

...

}

MeasurementReport-IEs NRPPA-PROTOCOL-IES ::= {

{ ID id-LMF-Measurement-ID CRITICALITY reject TYPE Measurement-ID PRESENCE mandatory}|

{ ID id-RAN-Measurement-ID CRITICALITY reject TYPE Measurement-ID PRESENCE mandatory}|

{ ID id-TRP-MeasurementReportList CRITICALITY reject TYPE TRP-MeasurementResponseList PRESENCE mandatory},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- MEASUREMENT UPDATE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

MeasurementUpdate ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{MeasurementUpdate-IEs}},

...

}

MeasurementUpdate-IEs NRPPA-PROTOCOL-IES ::= {

{ ID id-LMF-Measurement-ID CRITICALITY reject TYPE Measurement-ID PRESENCE mandatory}|

{ ID id-RAN-Measurement-ID CRITICALITY reject TYPE Measurement-ID PRESENCE mandatory}|

{ ID id-SRSConfiguration CRITICALITY ignore TYPE SRSConfiguration PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- MEASUREMENT ABORT

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

MeasurementAbort ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{MeasurementAbort-IEs}},

...

}

MeasurementAbort-IEs NRPPA-PROTOCOL-IES ::= {

{ ID id-LMF-Measurement-ID CRITICALITY reject TYPE Measurement-ID PRESENCE mandatory}|

{ ID id-RAN-Measurement-ID CRITICALITY reject TYPE Measurement-ID PRESENCE mandatory},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- MEASUREMENT FAILURE INDICATION

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

MeasurementFailureIndication ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{MeasurementFailureIndication-IEs}},

...

}

MeasurementFailureIndication-IEs NRPPA-PROTOCOL-IES ::= {

{ ID id-LMF-Measurement-ID CRITICALITY reject TYPE Measurement-ID PRESENCE mandatory}|

{ ID id-RAN-Measurement-ID CRITICALITY reject TYPE Measurement-ID PRESENCE mandatory}|

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- TRP INFORMATION REQUEST

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

TRPInformationRequest ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{TRPInformationRequest-IEs}},

...

}

TRPInformationRequest-IEs NRPPA-PROTOCOL-IES ::= {

{ ID id-TRPList CRITICALITY reject TYPE TRPList PRESENCE mandatory}|

{ ID id-TRPInformationTypeList CRITICALITY reject TYPE TRPInformationTypeList PRESENCE mandatory}, ...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- TRP INFORMATION RESPONSE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

TRPInformationResponse ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{TRPInformationResponse-IEs}},

...

}

TRPInformationResponse-IEs NRPPA-PROTOCOL-IES ::= {

{ ID id-TRPInformationList CRITICALITY ignore TYPE TRPInformationList PRESENCE mandatory}|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- TRP INFORMATION FAILURE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

TRPInformationFailure ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{TRPInformationFailure-IEs}},

...

}

TRPInformationFailure-IEs NRPPA-PROTOCOL-IES ::= {

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory}|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- POSITIONING ACTIVATION PROCEDURE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Positioning Activation Request

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PositioningActivationRequest ::= SEQUENCE {

protocolIEs ProtocolIE-Container { { PositioningActivationRequestIEs} },

...

}

PositioningActivationRequestIEs NRPPA-PROTOCOL-IES ::= {

{ ID id-SRSType CRITICALITY reject TYPE SRSType PRESENCE mandatory } |

{ ID id-ActivationTime CRITICALITY ignore TYPE ActivationTime PRESENCE optional },

...

}

SRSType ::= CHOICE {

semipersistentSRS SemipersistentSRS,

aperiodicSRS AperiodicSRS,

sRSType-extension ProtocolIE-Single-Container { { SRSType-ExtIEs} }

}

SRSType-ExtIEs NRPPA-PROTOCOL-IES ::= {

...

}

SemipersistentSRS ::= SEQUENCE {

sRSResourceSetID SRSResourceSetID,

iE-Extensions ProtocolExtensionContainer { {SemipersistentSRS-ExtIEs} } OPTIONAL,

...

}

SemipersistentSRS-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

{ ID id-SRSSpatialRelation CRITICALITY ignore EXTENSION SRSSpatialRelation PRESENCE optional},

...

}

AperiodicSRS ::= SEQUENCE {

aperiodic ENUMERATED{true,...},

sRSResourceTrigger SRSResourceTrigger OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {AperiodicSRS-ExtIEs} } OPTIONAL,

...

}

AperiodicSRS-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Positioning Activation Response

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PositioningActivationResponse ::= SEQUENCE {

protocolIEs ProtocolIE-Container { { PositioningActivationResponseIEs} },

...

}

PositioningActivationResponseIEs NRPPA-PROTOCOL-IES ::= {

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional }|

{ ID id-SystemFrameNumber CRITICALITY ignore TYPE SystemFrameNumber PRESENCE optional }|

{ ID id-SlotNumber CRITICALITY ignore TYPE SlotNumber PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Positioning Activation Failure

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PositioningActivationFailure ::= SEQUENCE {

protocolIEs ProtocolIE-Container { { PositioningActivationFailureIEs} },

...

}

PositioningActivationFailureIEs NRPPA-PROTOCOL-IES ::= {

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory }|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- POSITIONING DEACTIVATION PROCEDURE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Positioning Deactivation

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PositioningDeactivation ::= SEQUENCE {

protocolIEs ProtocolIE-Container { { PositioningDeactivationIEs} },

...

}

PositioningDeactivationIEs NRPPA-PROTOCOL-IES ::= {

{ ID id-AbortTransmission CRITICALITY ignore TYPE AbortTransmission PRESENCE mandatory } ,

...

}

END

-- ASN1STOP

### 9.3.5 Information Element definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Information Element Definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

NRPPA-IEs {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-access (22) modules (3) nrppa (4) version1 (1) nrppa-IEs (2) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

IMPORTS

id-MeasurementQuantities-Item,

id-GeographicalCoordinates,

id-ResultSS-RSRP,

id-ResultSS-RSRQ,

id-ResultCSI-RSRP,

id-ResultCSI-RSRQ,

id-AngleOfArrivalNR,

id-SRSSpatialRelation,

id-ResultNR,

id-ResultEUTRA,

maxCellinRANnode,

maxCellReport,

maxNrOfErrors,

maxNoMeas,

maxnoOTDOAtypes,

maxServCell,

id-OtherRATMeasurementQuantities-Item,

id-WLANMeasurementQuantities-Item,

maxGERANMeas,

maxUTRANMeas,

maxWLANchannels,

maxnoFreqHoppingBandsMinusOne,

id-TDD-Config-EUTRA-Item,

maxNrOfPosSImessage,

maxnoAssistInfoFailureListItems,

maxNrOfSegments,

maxNrOfPosSIBs,

maxnoPosMeas,

maxnoTRPs,

maxnoTRPInfoTypes,

maxNoOfMeasTRPs,

maxNoPath,

maxnoofAngleInfo,

maxnolcs-gcs-translation,

maxnoBcastCell,

maxnoSRSTriggerStates,

maxnoSpatialRelations,

maxNRMeas,

maxEUTRAMeas,

maxIndexesReport,

maxCellReportNR,

maxnoSRS-Carriers,

maxnoSCSs,

maxnoSRS-Resources,

maxnoSRS-PosResources,

maxnoSRS-ResourceSets,

maxnoSRS-ResourcePerSet,

maxnoSRS-PosResourceSets,

maxnoSRS-PosResourcePerSet,

maxPRS-ResourceSets,

maxPRS-ResourcesPerSet,

maxNoSSBs,

maxnoofPRSresourceSet,

maxnoofPRSresource

FROM NRPPA-Constants

Criticality,

NRPPATransactionID,

ProcedureCode,

ProtocolIE-ID,

TriggeringMessage

FROM NRPPA-CommonDataTypes

ProtocolExtensionContainer{},

ProtocolIE-Single-Container{},

NRPPA-PROTOCOL-EXTENSION,

NRPPA-PROTOCOL-IES

FROM NRPPA-Containers;

-- A

AbortTransmission ::= CHOICE {

sRSResourceSetID SRSResourceSetID,

releaseALL NULL,

choice-extension ProtocolIE-Single-Container { { AbortTransmission-ExtIEs } }

}

AbortTransmission-ExtIEs NRPPA-PROTOCOL-IES ::= {

...

}

ActiveULBWP ::= SEQUENCE {

locationAndBandwidth INTEGER (0..37949,...),

subcarrierSpacing ENUMERATED {kHz15, kHz30, kHz60, kHz120,...},

cyclicPrefix ENUMERATED {normal, extended},

txDirectCurrentLocation INTEGER (0..3301,...),

shift7dot5kHz ENUMERATED {true, ...} OPTIONAL,

sRSConfig SRSConfig,

iE-Extensions ProtocolExtensionContainer { { ActiveULBWP-ExtIEs} } OPTIONAL,

...

}

ActiveULBWP-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

ActivationTime ::= SFNInitialisationTime

AdditionalPathList ::= SEQUENCE (SIZE (1.. maxNoPath)) OF AdditionalPathListItem

AdditionalPathListItem ::= SEQUENCE {

relativeTimeOfPath RelativePathDelay,

pathQuality TrpMeasurementQuality OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { AdditionalPathListItem-ExtIEs} } OPTIONAL,

...

}

AdditionalPathListItem-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

AperiodicSRSResourceTriggerList ::= SEQUENCE (SIZE(1..maxnoSRSTriggerStates)) OF AperiodicSRSResourceTrigger

AperiodicSRSResourceTrigger ::= INTEGER (0..3, ...)

Assistance-Information ::= SEQUENCE {

systemInformation SystemInformation,

iE-Extensions ProtocolExtensionContainer { { Assistance-Information-ExtIEs} } OPTIONAL,

...

}

Assistance-Information-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

AssistanceInformationFailureList ::= SEQUENCE (SIZE (1..maxnoAssistInfoFailureListItems)) OF SEQUENCE {

posSIB-Type PosSIB-Type,

outcome Outcome,

iE-Extensions ProtocolExtensionContainer { {AssistanceInformationFailureList-ExtIEs} } OPTIONAL,

...

}

AssistanceInformationFailureList-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

AssistanceInformationMetaData ::= SEQUENCE {

encrypted ENUMERATED {true, ...} OPTIONAL,

gNSSID ENUMERATED {gps, sbas, qzss, galileo, glonass, bds, navic, ...} OPTIONAL,

sBASID ENUMERATED {waas, egnos, msas, gagan, ...} OPTIONAL, iE-Extensions ProtocolExtensionContainer { { AssistanceInformationMetaData-ExtIEs} } OPTIONAL,

...

}

AssistanceInformationMetaData-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

-- B

BandwidthSRS ::= CHOICE {

fR1 ENUMERATED {kHz5, kHz10, kHz20, kHz40, kHz50, kHz80, kHz100, ...},

fR2 ENUMERATED {kHz50, kHz100, kHz200, kHz400, ...},

...

}

BCCH ::= INTEGER (0..1023, ...)

Broadcast ::= ENUMERATED {

start,

stop,

...

}

BroadcastPeriodicity ::= ENUMERATED {

ms80,

ms160,

ms320,

ms640,

ms1280,

ms2560,

ms5120,

...

}

PositioningBroadcastCells ::= SEQUENCE (SIZE (1..maxnoBcastCell)) OF NG-RAN-CGI

BSSID ::= OCTET STRING (SIZE(6))

-- C

Cause ::= CHOICE {

radioNetwork CauseRadioNetwork,

protocol CauseProtocol,

misc CauseMisc,

cause-Extension ProtocolIE-Single-Container {{ Cause-ExtensionIE }}

}

Cause-ExtensionIE NRPPA-PROTOCOL-IES ::= {

...

}

CauseMisc ::= ENUMERATED {

unspecified,

...

}

CauseProtocol ::= ENUMERATED {

transfer-syntax-error,

abstract-syntax-error-reject,

abstract-syntax-error-ignore-and-notify,

message-not-compatible-with-receiver-state,

semantic-error,

unspecified,

abstract-syntax-error-falsely-constructed-message,

...

}

CauseRadioNetwork ::= ENUMERATED {

unspecified,

requested-item-not-supported,

requested-item-temporarily-not-available,

...

}

Cell-Portion-ID ::= INTEGER (0..4095,...)

CGI-EUTRA ::= SEQUENCE {

pLMN-Identity PLMN-Identity,

eUTRAcellIdentifier EUTRACellIdentifier,

iE-Extensions ProtocolExtensionContainer { {CGI-EUTRA-ExtIEs} } OPTIONAL,

...

}

CGI-EUTRA-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

CGI-NR ::= SEQUENCE {

pLMN-Identity PLMN-Identity,

nRcellIdentifier NRCellIdentifier,

iE-Extensions ProtocolExtensionContainer { {CGI-NR-ExtIEs} } OPTIONAL,

...

}

CGI-NR-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

CPLength-EUTRA ::= ENUMERATED {

normal,

extended,

...

}

CriticalityDiagnostics ::= SEQUENCE {

procedureCode ProcedureCode OPTIONAL,

triggeringMessage TriggeringMessage OPTIONAL,

procedureCriticality Criticality OPTIONAL,

nrppatransactionID NRPPATransactionID OPTIONAL,

iEsCriticalityDiagnostics CriticalityDiagnostics-IE-List OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {CriticalityDiagnostics-ExtIEs} } OPTIONAL,

...

}

CriticalityDiagnostics-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

CriticalityDiagnostics-IE-List ::= SEQUENCE (SIZE (1..maxNrOfErrors)) OF

SEQUENCE {

iECriticality Criticality,

iE-ID ProtocolIE-ID,

typeOfError TypeOfError,

iE-Extensions ProtocolExtensionContainer { {CriticalityDiagnostics-IE-List-ExtIEs} } OPTIONAL,

...

}

CriticalityDiagnostics-IE-List-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

-- D

DL-Bandwidth-EUTRA ::= ENUMERATED {

bw6,

bw15,

bw25,

bw50,

bw75,

bw100,

...

}

DL-PRS ::= SEQUENCE {

prsid INTEGER (0..255),

dl-PRSResourceSetID INTEGER (0..7),

dl-PRSResourceID INTEGER (0..63) OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {DL-PRS-ExtIEs} } OPTIONAL,

...

}

DL-PRS-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

DL-PRSMutingPattern ::= CHOICE {

two BIT STRING (SIZE(2)),

four BIT STRING (SIZE(4)),

six BIT STRING (SIZE(6)),

eight BIT STRING (SIZE(8)),

sixteen BIT STRING (SIZE(16)),

thirty-two BIT STRING (SIZE(32)),

choice-extension ProtocolIE-Single-Container { { DL-PRSMutingPattern-ExtIEs } }

}

DL-PRSMutingPattern-ExtIEs NRPPA-PROTOCOL-IES ::= {

...

}

DLPRSResourceCoordinates ::= SEQUENCE {

listofDL-PRSResourceSetARP SEQUENCE (SIZE(1.. maxPRS-ResourceSets)) OF DLPRSResourceSetARP,

iE-Extensions ProtocolExtensionContainer { { DLPRSResourceCoordinates-ExtIEs } } OPTIONAL,

...

}

DLPRSResourceCoordinates-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

DLPRSResourceSetARP ::= SEQUENCE {

dl-PRSResourceSetID INTEGER (0..7),

dL-PRSResourceSetARPLocation DL-PRSResourceSetARPLocation,

listofDL-PRSResourceARP SEQUENCE (SIZE(1.. maxPRS-ResourcesPerSet)) OF DLPRSResourceARP,

iE-Extensions ProtocolExtensionContainer { { DLPRSResourceSetARP-ExtIEs } } OPTIONAL,

...

}

DLPRSResourceSetARP-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

DL-PRSResourceSetARPLocation ::= CHOICE {

relativeGeodeticLocation RelativeGeodeticLocation,

relativeCartesianLocation RelativeCartesianLocation,

choice-Extension ProtocolIE-Single-Container { { DL-PRSResourceSetARPLocation-ExtIEs } }

}

DL-PRSResourceSetARPLocation-ExtIEs NRPPA-PROTOCOL-IES ::= {

...

}

DLPRSResourceARP ::= SEQUENCE {

dl-PRSResourceID INTEGER (0..63),

dL-PRSResourceARPLocation DL-PRSResourceARPLocation,

iE-Extensions ProtocolExtensionContainer { { DLPRSResourceARP-ExtIEs } } OPTIONAL,

...

}

DLPRSResourceARP-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

DL-PRSResourceARPLocation ::= CHOICE {

relativeGeodeticLocation RelativeGeodeticLocation,

relativeCartesianLocation RelativeCartesianLocation,

choice-Extension ProtocolIE-Single-Container { { DL-PRSResourceARPLocation-ExtIEs } }

}

DL-PRSResourceARPLocation-ExtIEs NRPPA-PROTOCOL-IES ::= {

...

}

-- E

E-CID-MeasurementResult ::= SEQUENCE {

servingCell-ID NG-RAN-CGI,

servingCellTAC TAC,

nG-RANAccessPointPosition NG-RANAccessPointPosition OPTIONAL,

measuredResults MeasuredResults OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { E-CID-MeasurementResult-ExtIEs} } OPTIONAL,

...

}

E-CID-MeasurementResult-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

{ ID id-GeographicalCoordinates CRITICALITY ignore EXTENSION GeographicalCoordinates PRESENCE optional},

...

}

EUTRACellIdentifier ::= BIT STRING (SIZE (28))

EARFCN ::= INTEGER (0..262143, ...)

-- F

-- G

GeographicalCoordinates ::= SEQUENCE {

tRPPositionDefinitionType TRPPositionDefinitionType,

dLPRSResourceCoordinates DLPRSResourceCoordinates OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { GeographicalCoordinates-ExtIEs } } OPTIONAL,

...

}

GeographicalCoordinates-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

GNB-RxTxTimeDiff ::= SEQUENCE {

rxTxTimeDiff GNBRxTxTimeDiffMeas,

additionalPathList AdditionalPathList OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { GNB-RxTxTimeDiff-ExtIEs} } OPTIONAL,

...

}

GNB-RxTxTimeDiff-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

GNBRxTxTimeDiffMeas ::= CHOICE {

k0 INTEGER (0.. 1970049),

k1 INTEGER (0.. 985025),

k2 INTEGER (0.. 492513),

k3 INTEGER (0.. 246257),

k4 INTEGER (0.. 123129),

k5 INTEGER (0.. 61565),

choice-extension ProtocolIE-Single-Container { { GNBRxTxTimeDiffMeas-ExtIEs } }

}

GNBRxTxTimeDiffMeas-ExtIEs NRPPA-PROTOCOL-IES ::= {

...

}

-- H

HESSID ::= OCTET STRING (SIZE(6))

-- I

-- J

-- K

-- L

LCG-to-GCS-TranslationItem::= SEQUENCE {

alpha INTEGER (0..359) OPTIONAL,

alphaFine INTEGER (0..9) OPTIONAL,

beta INTEGER (0..359) OPTIONAL,

betaFine INTEGER (0..9) OPTIONAL,

gamma INTEGER (0..359) OPTIONAL,

gammaFine INTEGER (0..9) OPTIONAL,

...

}

LocationUncertainty ::= SEQUENCE {

horizontalUncertainty INTEGER (0..255),

horizontalConfidence INTEGER (0..100),

verticalUncertainty INTEGER (0..255),

verticalConfidence INTEGER (0..100),

iE-Extensions ProtocolExtensionContainer { { LocationUncertainty-ExtIEs} } OPTIONAL,

...

}

LocationUncertainty-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

-- M

Measurement-ID ::= INTEGER (1.. 65536)

MeasurementBeamInfoRequest ::= ENUMERATED {true, ...}

MeasurementBeamInfo ::= SEQUENCE {

pRS-Resource-ID PRS-Resource-ID OPTIONAL,

pRS-Resource-Set-ID PRS-Resource-Set-ID OPTIONAL,

sSB-Index SSB-Index OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { MeasurementBeamInfo-ExtIEs} } OPTIONAL,

...

}

MeasurementBeamInfo-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

MeasurementPeriodicity ::= ENUMERATED {

ms120,

ms240,

ms480,

ms640,

ms1024,

ms2048,

ms5120,

ms10240,

min1,

min6,

min12,

min30,

min60,

...

}

MeasurementQuantities ::= SEQUENCE (SIZE (1.. maxNoMeas)) OF ProtocolIE-Single-Container { {MeasurementQuantities-ItemIEs} }

MeasurementQuantities-ItemIEs NRPPA-PROTOCOL-IES ::= {

{ ID id-MeasurementQuantities-Item CRITICALITY reject TYPE MeasurementQuantities-Item PRESENCE mandatory}

}

MeasurementQuantities-Item ::= SEQUENCE {

measurementQuantitiesValue MeasurementQuantitiesValue,

iE-Extensions ProtocolExtensionContainer { { MeasurementQuantitiesValue-ExtIEs} } OPTIONAL,

...

}

MeasurementQuantitiesValue-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

MeasurementQuantitiesValue ::= ENUMERATED {

cell-ID,

angleOfArrival,

timingAdvanceType1,

timingAdvanceType2,

rSRP,

rSRQ,

... ,

sS-RSRP,

sS-RSRQ,

cSI-RSRP,

cSI-RSRQ,

angleOfArrivalNR

}

MeasuredResults ::= SEQUENCE (SIZE (1.. maxNoMeas)) OF MeasuredResultsValue

MeasuredResultsValue ::= CHOICE {

valueAngleOfArrival-EUTRA INTEGER (0..719),

valueTimingAdvanceType1-EUTRA INTEGER (0..7690),

valueTimingAdvanceType2-EUTRA INTEGER (0..7690),

resultRSRP-EUTRA ResultRSRP-EUTRA,

resultRSRQ-EUTRA ResultRSRQ-EUTRA,

measuredResultsValue-Extension ProtocolIE-Single-Container {{ MeasuredResultsValue-ExtensionIE }}

}

MeasuredResultsValue-ExtensionIE NRPPA-PROTOCOL-IES ::= {

{ ID id-ResultSS-RSRP CRITICALITY ignore TYPE ResultSS-RSRP PRESENCE mandatory }|

{ ID id-ResultSS-RSRQ CRITICALITY ignore TYPE ResultSS-RSRQ PRESENCE mandatory }|

{ ID id-ResultCSI-RSRP CRITICALITY ignore TYPE ResultCSI-RSRP PRESENCE mandatory }|

{ ID id-ResultCSI-RSRQ CRITICALITY ignore TYPE ResultCSI-RSRQ PRESENCE mandatory }|

{ ID id-AngleOfArrivalNR CRITICALITY ignore TYPE UL-AoA PRESENCE mandatory },

...

}

-- N

NarrowBandIndex ::= INTEGER (0..15,...)

NG-RANAccessPointPosition ::= SEQUENCE {

latitudeSign ENUMERATED {north, south},

latitude INTEGER (0..8388607),

longitude INTEGER (-8388608..8388607),

directionOfAltitude ENUMERATED {height, depth},

altitude INTEGER (0..32767),

uncertaintySemi-major INTEGER (0..127),

uncertaintySemi-minor INTEGER (0..127),

orientationOfMajorAxis INTEGER (0..179),

uncertaintyAltitude INTEGER (0..127),

confidence INTEGER (0..100),

iE-Extensions ProtocolExtensionContainer { { NG-RANAccessPointPosition-ExtIEs} } OPTIONAL,

...

}

NG-RANAccessPointPosition-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

NGRANHighAccuracyAccessPointPosition ::= SEQUENCE {

latitude INTEGER (-2147483648.. 2147483647),

longitude INTEGER (-2147483648.. 2147483647),

altitude INTEGER (-64000..1280000),

uncertaintySemi-major INTEGER (0..255),

uncertaintySemi-minor INTEGER (0..255),

orientationOfMajorAxis INTEGER (0..179),

horizontalConfidence INTEGER (0..100),

uncertaintyAltitude INTEGER (0..255),

verticalConfidence INTEGER (0..100),

iE-Extensions ProtocolExtensionContainer { { NGRANHighAccuracyAccessPointPosition-ExtIEs} } OPTIONAL,

...

}

NGRANHighAccuracyAccessPointPosition-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

NG-RAN-CGI ::= SEQUENCE {

pLMN-Identity PLMN-Identity,

nG-RANcell NG-RANCell,

iE-Extensions ProtocolExtensionContainer { {NG-RAN-CGI-ExtIEs} } OPTIONAL,

...

}

NG-RAN-CGI-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

NG-RANCell ::= CHOICE {

eUTRA-CellID EUTRACellIdentifier,

nR-CellID NRCellIdentifier,

nG-RANCell-Extension ProtocolIE-Single-Container {{ NG-RANCell-ExtensionIE }}

}

NG-RANCell-ExtensionIE NRPPA-PROTOCOL-IES ::= {

...

}

NR-ARFCN ::= INTEGER (0..3279165)

NRCellIdentifier ::= BIT STRING (SIZE (36))

NR-PCI ::= INTEGER (0..1007)

NR-PRS-Beam-Information ::= SEQUENCE {

nR-PRS-Beam-InformationList SEQUENCE (SIZE(1.. maxPRS-ResourceSets)) OF NR-PRS-Beam-InformationItem,

lCG-to-GCS-TranslationList SEQUENCE (SIZE(1..maxnolcs-gcs-translation)) OF LCG-to-GCS-TranslationItem,

iE-Extensions ProtocolExtensionContainer { { NR-PRS-Beam-Information-IEs} } OPTIONAL,

...

}

NR-PRS-Beam-Information-IEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

NR-PRS-Beam-InformationItem ::= SEQUENCE {

pRSresourceSetID INTEGER (0..7),

pRSAngleItem SEQUENCE (SIZE(1..maxPRS-ResourcesPerSet)) OF PRSAngleItem,

...

}

NumberOfAntennaPorts-EUTRA ::= ENUMERATED {

n1-or-n2,

n4,

...

}

NumberOfDlFrames-EUTRA ::= ENUMERATED {

sf1,

sf2,

sf4,

sf6,

...

}

NumberOfDlFrames-Extended-EUTRA ::= INTEGER (1..160,...)

NumberOfFrequencyHoppingBands ::= ENUMERATED {

twobands,

fourbands,

...

}

NZP-CSI-RS-ResourceID::= INTEGER (0..191, ...)

-- O

OTDOACells ::= SEQUENCE (SIZE (1.. maxCellinRANnode)) OF SEQUENCE {

oTDOACellInfo OTDOACell-Information,

iE-Extensions ProtocolExtensionContainer { {OTDOACells-ExtIEs} } OPTIONAL,

...

}

OTDOACells-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

OTDOACell-Information ::= SEQUENCE (SIZE (1..maxnoOTDOAtypes)) OF OTDOACell-Information-Item

OTDOACell-Information-Item ::= CHOICE {

pCI-EUTRA PCI-EUTRA,

cGI-EUTRA CGI-EUTRA,

tAC TAC,

eARFCN EARFCN,

pRS-Bandwidth-EUTRA PRS-Bandwidth-EUTRA,

pRS-ConfigurationIndex-EUTRA PRS-ConfigurationIndex-EUTRA,

cPLength-EUTRA CPLength-EUTRA,

numberOfDlFrames-EUTRA NumberOfDlFrames-EUTRA,

numberOfAntennaPorts-EUTRA NumberOfAntennaPorts-EUTRA,

sFNInitialisationTime-EUTRA SFNInitialisationTime-EUTRA,

nG-RANAccessPointPosition NG-RANAccessPointPosition,

pRSMutingConfiguration-EUTRA PRSMutingConfiguration-EUTRA,

prsid-EUTRA PRS-ID-EUTRA,

tpid-EUTRA TP-ID-EUTRA,

tpType-EUTRA TP-Type-EUTRA,

numberOfDlFrames-Extended-EUTRA NumberOfDlFrames-Extended-EUTRA,

crsCPlength-EUTRA CPLength-EUTRA,

dL-Bandwidth-EUTRA DL-Bandwidth-EUTRA,

pRSOccasionGroup-EUTRA PRSOccasionGroup-EUTRA,

pRSFrequencyHoppingConfiguration-EUTRA PRSFrequencyHoppingConfiguration-EUTRA,

oTDOACell-Information-Item-Extension ProtocolIE-Single-Container {{ OTDOACell-Information-Item-ExtensionIE }}

}

OTDOACell-Information-Item-ExtensionIE NRPPA-PROTOCOL-IES ::= {

{ ID id-TDD-Config-EUTRA-Item CRITICALITY ignore TYPE TDD-Config-EUTRA-Item PRESENCE optional },

...

}

OTDOA-Information-Item ::= ENUMERATED {

pci,

cGI,

tac,

earfcn,

prsBandwidth,

prsConfigIndex,

cpLength,

noDlFrames,

noAntennaPorts,

sFNInitTime,

nG-RANAccessPointPosition,

prsmutingconfiguration,

prsid,

tpid,

tpType,

crsCPlength,

dlBandwidth,

multipleprsConfigurationsperCell,

prsOccasionGroup,

prsFrequencyHoppingConfiguration,

...,

tddConfig

}

OtherRATMeasurementQuantities ::= SEQUENCE (SIZE (0.. maxNoMeas)) OF ProtocolIE-Single-Container { {OtherRATMeasurementQuantities-ItemIEs} }

OtherRATMeasurementQuantities-ItemIEs NRPPA-PROTOCOL-IES ::= {

{ ID id-OtherRATMeasurementQuantities-Item CRITICALITY reject TYPE OtherRATMeasurementQuantities-Item PRESENCE mandatory}}

OtherRATMeasurementQuantities-Item ::= SEQUENCE {

otherRATMeasurementQuantitiesValue OtherRATMeasurementQuantitiesValue,

iE-Extensions ProtocolExtensionContainer { { OtherRATMeasurementQuantitiesValue-ExtIEs} } OPTIONAL,

...

}

OtherRATMeasurementQuantitiesValue-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

OtherRATMeasurementQuantitiesValue ::= ENUMERATED {

geran,

utran,

... ,

nR,

eUTRA

}

OtherRATMeasurementResult ::= SEQUENCE (SIZE (1.. maxNoMeas)) OF OtherRATMeasuredResultsValue

OtherRATMeasuredResultsValue ::= CHOICE {

resultGERAN ResultGERAN,

resultUTRAN ResultUTRAN,

otherRATMeasuredResultsValue-Extension ProtocolIE-Single-Container {{ OtherRATMeasuredResultsValue-ExtensionIE }}

}

OtherRATMeasuredResultsValue-ExtensionIE NRPPA-PROTOCOL-IES ::= {

{ ID id-ResultNR CRITICALITY ignore TYPE ResultNR PRESENCE mandatory }|

{ ID id-ResultEUTRA CRITICALITY ignore TYPE ResultEUTRA PRESENCE mandatory },

...

}

Outcome ::= ENUMERATED {

failed,

...

}

-- P

PathlossReferenceInformation ::= SEQUENCE {

pathlossReferenceSignal PathlossReferenceSignal,

iE-Extensions ProtocolExtensionContainer { { PathlossReferenceInformation-ExtIEs } } OPTIONAL,

...

}

PathlossReferenceInformation-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

PathlossReferenceSignal ::= CHOICE {

sSB-Reference SSB,

dL-PRS-Reference DL-PRS,

choice-Extension ProtocolIE-Single-Container {{ PathlossReferenceSignal-ExtensionIE }}

}

PathlossReferenceSignal-ExtensionIE NRPPA-PROTOCOL-IES ::= {

...

}

PCI-EUTRA ::= INTEGER (0..503, ...)

PhysCellIDGERAN ::= INTEGER (0..63, ...)

PhysCellIDUTRA-FDD ::= INTEGER (0..511, ...)

PhysCellIDUTRA-TDD ::= INTEGER (0..127, ...)

PLMN-Identity ::= OCTET STRING (SIZE(3))

PeriodicityList ::= SEQUENCE (SIZE (1.. maxnoSRS-ResourcePerSet)) OF PeriodicityItem

PeriodicityItem ::= ENUMERATED {ms0dot125, ms0dot25, ms0dot5, ms0dot625, ms1, ms1dot25, ms2, ms2dot5, ms4dot, ms5, ms8, ms10, ms16, ms20, ms32, ms40, ms64, ms80m, ms160, ms320, ms640m, ms1280, ms2560, ms5120, ms10240, ...}

PosSIBs ::= SEQUENCE (SIZE (1.. maxNrOfPosSIBs)) OF SEQUENCE {

posSIB-Type PosSIB-Type,

posSIB-Segments PosSIB-Segments,

assistanceInformationMetaData AssistanceInformationMetaData OPTIONAL,

broadcastPriority INTEGER (1..16,...) OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { PosSIBs-ExtIEs} } OPTIONAL,

...

}

PosSIBs-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

PosSIB-Segments ::= SEQUENCE (SIZE (1.. maxNrOfSegments)) OF SEQUENCE {

assistanceDataSIBelement OCTET STRING,

iE-Extensions ProtocolExtensionContainer { { PosSIB-Segments-ExtIEs} } OPTIONAL,

...

}

PosSIB-Segments-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

PosSIB-Type ::= ENUMERATED {

posSibType1-1,

posSibType1-2,

posSibType1-3,

posSibType1-4,

posSibType1-5,

posSibType1-6,

posSibType1-7,

posSibType1-8,

posSibType2-1,

posSibType2-2,

posSibType2-3,

posSibType2-4,

posSibType2-5,

posSibType2-6,

posSibType2-7,

posSibType2-8,

posSibType2-9,

posSibType2-10,

posSibType2-11,

posSibType2-12,

posSibType2-13,

posSibType2-14,

posSibType2-15,

posSibType2-16,

posSibType2-17,

posSibType2-18,

posSibType2-19,

posSibType2-20,

posSibType2-21,

posSibType2-22,

posSibType2-23,

posSibType2-24,

posSibType2-25,

posSibType3-1,

posSibType4-1,

posSibType5-1,

posSibType6-1,

posSibType6-2,

posSibType6-3,

...

}

PosSRSResource-List ::= SEQUENCE (SIZE (1..maxnoSRS-PosResources)) OF PosSRSResource-Item

PosSRSResource-Item ::= SEQUENCE {

srs-PosResourceId SRSPosResourceID,

transmissionCombPos TransmissionCombPos,

startPosition INTEGER (0..13),

nrofSymbols ENUMERATED {n1, n2, n4, n8, n12},

freqDomainShift INTEGER (0..268),

c-SRS INTEGER (0..63),

groupOrSequenceHopping ENUMERATED { neither, groupHopping, sequenceHopping },

resourceTypePos ResourceTypePos,

sequenceId INTEGER (0.. 65535),

spatialRelationPos SpatialRelationPos OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { PosSRSResource-Item-ExtIEs} } OPTIONAL,

...

}

PosSRSResource-Item-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

PosSRSResourceSet-List ::= SEQUENCE (SIZE (1..maxnoSRS-PosResourceSets)) OF PosSRSResourceSet-Item

PosSRSResourceID-List ::= SEQUENCE (SIZE (1..maxnoSRS-PosResourcePerSet)) OF SRSPosResourceID

PosSRSResourceSet-Item ::= SEQUENCE {

possrsResourceSetID INTEGER(0..15),

possRSResourceID-List PosSRSResourceID-List,

posresourceSetType PosResourceSetType,

iE-Extensions ProtocolExtensionContainer { { PosSRSResourceSet-Item-ExtIEs} } OPTIONAL,

...

}

PosSRSResourceSet-Item-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

PosResourceSetType ::= CHOICE {

periodic PosResourceSetTypePeriodic,

semi-persistent PosResourceSetTypeSemi-persistent,

aperiodic PosResourceSetTypeAperiodic,

choice-extension ProtocolIE-Single-Container {{ PosResourceSetType-ExtIEs }}

}

PosResourceSetType-ExtIEs NRPPA-PROTOCOL-IES ::= {

...

}

PosResourceSetTypePeriodic ::= SEQUENCE {

posperiodicSet ENUMERATED{true, ...},

iE-Extensions ProtocolExtensionContainer { { PosResourceSetTypePeriodic-ExtIEs} } OPTIONAL,

...

}

PosResourceSetTypePeriodic-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

PosResourceSetTypeSemi-persistent ::= SEQUENCE {

possemi-persistentSet ENUMERATED{true, ...},

iE-Extensions ProtocolExtensionContainer { { PosResourceSetTypeSemi-persistent-ExtIEs} } OPTIONAL,

...

}

PosResourceSetTypeSemi-persistent-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

PosResourceSetTypeAperiodic ::= SEQUENCE {

sRSResourceTrigger INTEGER(1..3),

iE-Extensions ProtocolExtensionContainer { { PosResourceSetTypeAperiodic-ExtIEs} } OPTIONAL,

...

}

PosResourceSetTypeAperiodic-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

PRS-Bandwidth-EUTRA ::= ENUMERATED {

bw6,

bw15,

bw25,

bw50,

bw75,

bw100,

...

}

PRSAngleItem ::= SEQUENCE {

pRSresourceAngleID INTEGER (0..63),

nRPRSAzimuth INTEGER (0..359),

nRPRSAzimuthFine INTEGER (0..9) OPTIONAL,

nRPRSElevation INTEGER (0..180) OPTIONAL,

nRPRSElevationFine INTEGER (0..9) OPTIONAL,

...

}

PRSInformationPos ::= SEQUENCE {

pRS-IDPos INTEGER(0..255) OPTIONAL,

pRS-Resource-Set-IDPos INTEGER(0..7),

pRS-Resource-IDPos INTEGER(0..63),

iE-Extensions ProtocolExtensionContainer { { PRSInformationPos-ExtIEs} } OPTIONAL,

...

}

PRSInformationPos-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

PRSConfiguration ::= SEQUENCE {

pRSResourceSet-List PRSResourceSet-List,

iE-Extensions ProtocolExtensionContainer { { PRSConfiguration-ExtIEs} } OPTIONAL,

...

}

PRSConfiguration-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

PRS-ConfigurationIndex-EUTRA ::= INTEGER (0..4095, ...)

PRS-ID-EUTRA ::= INTEGER (0..4095, ...)

PRSMutingConfiguration-EUTRA ::= CHOICE {

two BIT STRING (SIZE (2)),

four BIT STRING (SIZE (4)),

eight BIT STRING (SIZE (8)),

sixteen BIT STRING (SIZE (16)),

thirty-two BIT STRING (SIZE (32)),

sixty-four BIT STRING (SIZE (64)),

one-hundred-and-twenty-eight BIT STRING (SIZE (128)),

two-hundred-and-fifty-six BIT STRING (SIZE (256)),

five-hundred-and-twelve BIT STRING (SIZE (512)),

one-thousand-and-twenty-four BIT STRING (SIZE (1024)),

pRSMutingConfiguration-EUTRA-Extension ProtocolIE-Single-Container {{ PRSMutingConfiguration-EUTRA-ExtensionIE }}

}

PRSMutingConfiguration-EUTRA-ExtensionIE NRPPA-PROTOCOL-IES ::= {

...

}

PRSOccasionGroup-EUTRA ::= ENUMERATED {

og2,

og4,

og8,

og16,

og32,

og64,

og128,

...

}

PRSFrequencyHoppingConfiguration-EUTRA ::= SEQUENCE {

noOfFreqHoppingBands NumberOfFrequencyHoppingBands,

bandPositions SEQUENCE(SIZE (1..maxnoFreqHoppingBandsMinusOne)) OF NarrowBandIndex,

iE-Extensions ProtocolExtensionContainer { { PRSFrequencyHoppingConfiguration-EUTRA-Item-IEs} } OPTIONAL,

...

}

PRSFrequencyHoppingConfiguration-EUTRA-Item-IEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

PRSMuting::= SEQUENCE {

pRSMutingOption1 PRSMutingOption1,

pRSMutingOption2 PRSMutingOption2,

iE-Extensions ProtocolExtensionContainer { { PRSMuting-ExtIEs} } OPTIONAL,

...

}

PRSMuting-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

PRSMutingOption1 ::= SEQUENCE {

mutingPattern DL-PRSMutingPattern,

mutingBitRepetitionFactor ENUMERATED{n1,n2,n4,n8,...},

iE-Extensions ProtocolExtensionContainer { { PRSMutingOption1-ExtIEs} } OPTIONAL,

...

}

PRSMutingOption1-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

PRSMutingOption2 ::= SEQUENCE {

mutingPattern DL-PRSMutingPattern,

iE-Extensions ProtocolExtensionContainer { { PRSMutingOption2-ExtIEs} } OPTIONAL,

...

}

PRSMutingOption2-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

PRSResource-List::= SEQUENCE (SIZE (1..maxnoofPRSresource)) OF PRSResource-Item

PRSResource-Item ::= SEQUENCE {

pRSResourceID INTEGER(0..63),

sequenceID INTEGER(0..4095,...),

rEOffset INTEGER(0..11),

resourceSlotOffset INTEGER(0..511,...),

resourceSymbolOffset INTEGER(0..12,...),

qCLInfo PRSResource-QCLInfo OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { PRSResource-Item-ExtIEs} } OPTIONAL,

...

}

PRSResource-Item-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

PRSResource-QCLInfo ::= SEQUENCE {

qCLSourceSSBIndex INTEGER(0..63) OPTIONAL,

qCLSourcePRSInfo PRSResource-QCLSourcePRSInfo OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { PRSResource-QCLInfo-ExtIEs} } OPTIONAL,

...

}

PRSResource-QCLInfo-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

PRSResource-QCLSourcePRSInfo ::= SEQUENCE {

qCLSourcePRSResourceSetID INTEGER(0..7),

qCLSourcePRSResourceID INTEGER(0..63) OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { PRSResource-QCLSourcePRSInfo-ExtIEs} } OPTIONAL,

...

}

PRSResource-QCLSourcePRSInfo-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

PRSResourceSet-List ::= SEQUENCE (SIZE (1..maxnoofPRSresourceSet)) OF PRSResourceSet-Item

PRSResourceSet-Item ::= SEQUENCE {

pRSResourceSetID INTEGER(0..7),

subcarrierSpacing ENUMERATED{kHz15, kHz30, kHz60, kHz120, ...},

pRSbandwidth INTEGER(1..63),

startPRB INTEGER(0..2176),

pointA INTEGER (0..3279165),

combSize ENUMERATED{n2, n4, n6, n12, ...},

cPType ENUMERATED{normal, extended, ...},

resourceSetPeriodicity ENUMERATED{n4,n5,n8,n10,n16,n20,n32,n40,n64,n80,n160,n320,n640,n1280,n2560,n5120,n10240,n20480,n40960, n81920,...},

resourceSetSlotOffset INTEGER(0..81919,...),

resourceRepetitionFactor ENUMERATED{rf1,rf2,rf4,rf6,rf8,rf16,rf32,...},

resourceTimeGap ENUMERATED{tg1,tg2,tg4,tg8,tg16,tg32,...},

resourceNumberofSymbols ENUMERATED{n2,n4,n6,n12,...},

pRSMuting PRSMuting OPTIONAL,

pRSResourceTransmitPower INTEGER(-60..50),

pRSResource-List PRSResource-List,

iE-Extensions ProtocolExtensionContainer { { PRSResourceSet-Item-ExtIEs} } OPTIONAL,

...

}

PRSResourceSet-Item-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

PRS-Resource-ID ::= INTEGER (0..63)

PRS-Resource-Set-ID ::= INTEGER(0..7)

-- Q

-- R

ReferenceSignal ::= CHOICE {

nZP-CSI-RS NZP-CSI-RS-ResourceID,

sSB SSB,

sRS SRSResourceID,

positioningSRS SRSPosResourceID,

dL-PRS DL-PRS,

choice-Extension ProtocolIE-Single-Container {{ReferenceSignal-ExtensionIE }}

}

ReferenceSignal-ExtensionIE NRPPA-PROTOCOL-IES ::= {

...

}

ReferencePoint ::= CHOICE {

relativeCoordinateID CoordinateID,

referencePointCoordinate NG-RANAccessPointPosition,

referencePointCoordinateHA NGRANHighAccuracyAccessPointPosition,

choice-Extension ProtocolIE-Single-Container { { ReferencePoint-ExtIEs} }

}

ReferencePoint-ExtIEs NRPPA-PROTOCOL-IES ::= {

...

}

CoordinateID ::= INTEGER (0..511, ...)

RelativeGeodeticLocation ::= SEQUENCE {

milli-Arc-SecondUnits ENUMERATED {zerodot03, zerodot3, three, ...}, heightUnits ENUMERATED {mm, cm, m, ...},

deltaLatitude INTEGER (-1024.. 1023),

deltaLongitude INTEGER (-1024.. 1023),

deltaHeight INTEGER (-1024.. 1023),

locationUncertainty LocationUncertainty,

iE-extensions ProtocolExtensionContainer {{RelativeGeodeticLocation-ExtIEs }} OPTIONAL,

...

}

RelativeGeodeticLocation-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

RelativeCartesianLocation ::= SEQUENCE {

xYZunit ENUMERATED {mm, cm, dm, ...},

xvalue INTEGER (-65536..65535),

yvalue INTEGER (-65536..65535),

zvalue INTEGER (-32768..32767),

locationUncertainty LocationUncertainty,

iE-Extensions ProtocolExtensionContainer { { RelativeCartesianLocation-ExtIEs} } OPTIONAL,

...

}

RelativeCartesianLocation-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

RelativePathDelay ::= CHOICE {

k0 INTEGER(0..16351,...),

k1 INTEGER(0..8176,...),

k2 INTEGER(0..4088,...),

k3 INTEGER(0..2044,...),

k4 INTEGER(0..1022,...),

k5 INTEGER(0..511,...),

...

}

ReportCharacteristics ::= ENUMERATED {

onDemand,

periodic,

...

}

RequestedSRSTransmissionCharacteristics ::= SEQUENCE {

numberOfTransmissions INTEGER (0..500, ...) OPTIONAL,

resourceType ENUMERATED {periodic, semi-persistent, aperiodic, ...},

bandwidth BandwidthSRS,

listOfSRSResourceSet SEQUENCE (SIZE (1.. maxnoSRS-ResourceSets)) OF SRSResourceSet-Item OPTIONAL,

sSBInformation SSBInfo OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { RequestedSRSTransmissionCharacteristics-ExtIEs} } OPTIONAL,

...

}

RequestedSRSTransmissionCharacteristics-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

SRSResourceSet-Item ::= SEQUENCE {

numberOfSRSResourcePerSet INTEGER (1..16, ...) OPTIONAL,

periodicityList PeriodicityList OPTIONAL,

spatialRelationInformation SpatialRelationInfo OPTIONAL,

pathlossReferenceInformation PathlossReferenceInformation OPTIONAL,

...

}

ResourceSetType ::= CHOICE {

periodic ResourceSetTypePeriodic,

semi-persistent ResourceSetTypeSemi-persistent,

aperiodic ResourceSetTypeAperiodic,

choice-extension ProtocolIE-Single-Container {{ ResourceSetType-ExtIEs }}

}

ResourceSetType-ExtIEs NRPPA-PROTOCOL-IES ::= {

...

}

ResourceSetTypePeriodic ::= SEQUENCE {

periodicSet ENUMERATED{true, ...},

iE-Extensions ProtocolExtensionContainer { { ResourceSetTypePeriodic-ExtIEs} } OPTIONAL,

...

}

ResourceSetTypePeriodic-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

ResourceSetTypeSemi-persistent ::= SEQUENCE {

semi-persistentSet ENUMERATED{true, ...},

iE-Extensions ProtocolExtensionContainer { { ResourceSetTypeSemi-persistent-ExtIEs} } OPTIONAL,

...

}

ResourceSetTypeSemi-persistent-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

ResourceSetTypeAperiodic ::= SEQUENCE {

sRSResourceTrigger INTEGER(1..3),

slotoffset INTEGER(1..32),

iE-Extensions ProtocolExtensionContainer { { ResourceSetTypeAperiodic-ExtIEs} } OPTIONAL,

...

}

ResourceSetTypeAperiodic-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

ResourceType ::= CHOICE {

periodic ResourceTypePeriodic,

semi-persistent ResourceTypeSemi-persistent,

aperiodic ResourceTypeAperiodic,

choice-extension ProtocolIE-Single-Container {{ ResourceType-ExtIEs }}

}

ResourceType-ExtIEs NRPPA-PROTOCOL-IES ::= {

...

}

ResourceTypePeriodic ::= SEQUENCE {

periodicity ENUMERATED{slot1, slot2, slot4, slot5, slot8, slot10, slot16, slot20, slot32, slot40, slot64, slot80, slot160, slot320, slot640, slot1280, slot2560, ...},

offset INTEGER(0..2559, ...),

iE-Extensions ProtocolExtensionContainer { { ResourceTypePeriodic-ExtIEs} } OPTIONAL,

...

}

ResourceTypePeriodic-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

ResourceTypeSemi-persistent ::= SEQUENCE {

periodicity ENUMERATED{slot1, slot2, slot4, slot5, slot8, slot10, slot16, slot20, slot32, slot40, slot64, slot80, slot160, slot320, slot640, slot1280, slot2560, ...},

offset INTEGER(0..2559, ...),

iE-Extensions ProtocolExtensionContainer { { ResourceTypeSemi-persistent-ExtIEs} } OPTIONAL,

...

}

ResourceTypeSemi-persistent-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

ResourceTypeAperiodic ::= SEQUENCE {

aperiodicResourceType ENUMERATED{true, ...},

iE-Extensions ProtocolExtensionContainer { { ResourceTypeAperiodic-ExtIEs} } OPTIONAL,

...

}

ResourceTypeAperiodic-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

ResourceTypePos ::= CHOICE {

periodic ResourceTypePeriodicPos,

semi-persistent ResourceTypeSemi-persistentPos,

aperiodic ResourceTypeAperiodicPos,

choice-extension ProtocolIE-Single-Container {{ ResourceTypePos-ExtIEs }}

}

ResourceTypePos-ExtIEs NRPPA-PROTOCOL-IES ::= {

...

}

ResourceTypePeriodicPos ::= SEQUENCE {

periodicity ENUMERATED{slot1, slot2, slot4, slot5, slot8, slot10, slot16, slot20, slot32, slot40, slot64, slot80, slot160, slot320, slot640, slot1280, slot2560, slot5120, slot10240, slot20480, slot40960, slot81920, ...},

offset INTEGER(0..81919, ...),

iE-Extensions ProtocolExtensionContainer { { ResourceTypePeriodicPos-ExtIEs} } OPTIONAL,

...

}

ResourceTypePeriodicPos-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

ResourceTypeSemi-persistentPos ::= SEQUENCE {

periodicity ENUMERATED{slot1, slot2, slot4, slot5, slot8, slot10, slot16, slot20, slot32, slot40, slot64, slot80, slot160, slot320, slot640, slot1280, slot2560, slot5120, slot10240, slot20480, slot40960, slot81920, ...},

offset INTEGER(0..81919, ...),

iE-Extensions ProtocolExtensionContainer { { ResourceTypeSemi-persistentPos-ExtIEs} } OPTIONAL,

...

}

ResourceTypeSemi-persistentPos-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

ResourceTypeAperiodicPos ::= SEQUENCE {

slotOffset INTEGER (1..32),

iE-Extensions ProtocolExtensionContainer { { ResourceTypeAperiodicPos-ExtIEs} } OPTIONAL,

...

}

ResourceTypeAperiodicPos-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

ResultCSI-RSRP ::= SEQUENCE (SIZE (1.. maxCellReportNR)) OF ResultCSI-RSRP-Item

ResultCSI-RSRP-Item ::= SEQUENCE {

nR-PCI NR-PCI,

nR-ARFCN NR-ARFCN,

nG-RAN-CGI NG-RAN-CGI OPTIONAL,

valueCSI-RSRP-Cell ValueRSRP-NR OPTIONAL,

cSI-RSRP-PerCSI-RS ResultCSI-RSRP-PerCSI-RS OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { ResultCSI-RSRP-Item-ExtIEs} } OPTIONAL,

...

}

ResultCSI-RSRP-Item-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

ResultCSI-RSRP-PerCSI-RS ::= SEQUENCE (SIZE (1.. maxIndexesReport)) OF ResultCSI-RSRP-PerCSI-RS-Item

ResultCSI-RSRP-PerCSI-RS-Item ::= SEQUENCE {

cSI-RS-Index INTEGER (0..95),

valueCSI-RSRP ValueRSRP-NR,

iE-Extensions ProtocolExtensionContainer { { ResultCSI-RSRP-PerCSI-RS-Item-ExtIEs} } OPTIONAL,

...

}

ResultCSI-RSRP-PerCSI-RS-Item-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

ResultCSI-RSRQ ::= SEQUENCE (SIZE (1.. maxCellReportNR)) OF ResultCSI-RSRQ-Item

ResultCSI-RSRQ-Item ::= SEQUENCE {

nR-PCI NR-PCI,

nR-ARFCN NR-ARFCN,

nG-RAN-CGI NG-RAN-CGI OPTIONAL,

valueCSI-RSRQ-Cell ValueRSRQ-NR OPTIONAL,

cSI-RSRQ-PerCSI-RS ResultCSI-RSRQ-PerCSI-RS OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { ResultCSI-RSRQ-Item-ExtIEs} } OPTIONAL,

...

}

ResultCSI-RSRQ-Item-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

ResultCSI-RSRQ-PerCSI-RS ::= SEQUENCE (SIZE (1.. maxIndexesReport)) OF ResultCSI-RSRQ-PerCSI-RS-Item

ResultCSI-RSRQ-PerCSI-RS-Item ::= SEQUENCE {

cSI-RS-Index INTEGER (0..95),

valueCSI-RSRQ ValueRSRQ-NR,

iE-Extensions ProtocolExtensionContainer { { ResultCSI-RSRQ-PerCSI-RS-Item-ExtIEs} } OPTIONAL,

...

}

ResultCSI-RSRQ-PerCSI-RS-Item-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

ResultEUTRA ::= SEQUENCE (SIZE (1.. maxEUTRAMeas)) OF ResultEUTRA-Item

ResultEUTRA-Item ::= SEQUENCE {

pCI-EUTRA PCI-EUTRA,

eARFCN EARFCN,

valueRSRP-EUTRA ValueRSRP-EUTRA OPTIONAL,

valueRSRQ-EUTRA ValueRSRQ-EUTRA OPTIONAL,

cGI-EUTRA CGI-EUTRA OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { ResultEUTRA-Item-ExtIEs} } OPTIONAL,

...

}

ResultEUTRA-Item-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

ResultRSRP-EUTRA ::= SEQUENCE (SIZE (1.. maxCellReport)) OF ResultRSRP-EUTRA-Item

ResultRSRP-EUTRA-Item ::= SEQUENCE {

pCI-EUTRA PCI-EUTRA,

eARFCN EARFCN,

cGI-EUTRA CGI-EUTRA OPTIONAL,

valueRSRP-EUTRA ValueRSRP-EUTRA,

iE-Extensions ProtocolExtensionContainer { { ResultRSRP-EUTRA-Item-ExtIEs} } OPTIONAL,

...

}

ResultRSRP-EUTRA-Item-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

ResultRSRQ-EUTRA ::= SEQUENCE (SIZE (1.. maxCellReport)) OF ResultRSRQ-EUTRA-Item

ResultRSRQ-EUTRA-Item ::= SEQUENCE {

pCI-EUTRA PCI-EUTRA,

eARFCN EARFCN,

cGI-UTRA CGI-EUTRA OPTIONAL,

valueRSRQ-EUTRA ValueRSRQ-EUTRA,

iE-Extensions ProtocolExtensionContainer { { ResultRSRQ-EUTRA-Item-ExtIEs} } OPTIONAL,

...

}

ResultRSRQ-EUTRA-Item-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

ResultSS-RSRP ::= SEQUENCE (SIZE (1.. maxCellReportNR)) OF ResultSS-RSRP-Item

ResultSS-RSRP-Item ::= SEQUENCE {

nR-PCI NR-PCI,

nR-ARFCN NR-ARFCN,

nG-RAN-CGI NG-RAN-CGI OPTIONAL,

valueSS-RSRP-Cell ValueRSRP-NR OPTIONAL,

sS-RSRP-PerSSB ResultSS-RSRP-PerSSB OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { ResultSS-RSRP-Item-ExtIEs} } OPTIONAL,

...

}

ResultSS-RSRP-Item-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

ResultSS-RSRP-PerSSB ::= SEQUENCE (SIZE (1.. maxIndexesReport)) OF ResultSS-RSRP-PerSSB-Item

ResultSS-RSRP-PerSSB-Item ::= SEQUENCE {

sSB-Index INTEGER (0..63),

valueSS-RSRP ValueRSRP-NR,

iE-Extensions ProtocolExtensionContainer { { ResultSS-RSRP-PerSSB-Item-ExtIEs} } OPTIONAL,

...

}

ResultSS-RSRP-PerSSB-Item-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

ResultSS-RSRQ ::= SEQUENCE (SIZE (1.. maxCellReportNR)) OF ResultSS-RSRQ-Item

ResultSS-RSRQ-Item ::= SEQUENCE {

nR-PCI NR-PCI,

nR-ARFCN NR-ARFCN,

nG-RAN-CGI NG-RAN-CGI OPTIONAL,

valueSS-RSRQ-Cell ValueRSRQ-NR OPTIONAL,

sS-RSRQ-PerSSB ResultSS-RSRQ-PerSSB OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { ResultSS-RSRQ-Item-ExtIEs} } OPTIONAL,

...

}

ResultSS-RSRQ-Item-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

ResultSS-RSRQ-PerSSB ::= SEQUENCE (SIZE (1.. maxIndexesReport)) OF ResultSS-RSRQ-PerSSB-Item

ResultSS-RSRQ-PerSSB-Item ::= SEQUENCE {

sSB-Index INTEGER (0..63),

valueSS-RSRQ ValueRSRQ-NR,

iE-Extensions ProtocolExtensionContainer { { ResultSS-RSRQ-PerSSB-Item-ExtIEs} } OPTIONAL,

...

}

ResultSS-RSRQ-PerSSB-Item-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

ResultGERAN ::= SEQUENCE (SIZE (1.. maxGERANMeas)) OF ResultGERAN-Item

ResultGERAN-Item ::= SEQUENCE {

bCCH BCCH,

physCellIDGERAN PhysCellIDGERAN,

rSSI RSSI,

iE-Extensions ProtocolExtensionContainer { { ResultGERAN-Item-ExtIEs} } OPTIONAL,

...

}

ResultGERAN-Item-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

ResultNR ::= SEQUENCE (SIZE (1.. maxNRMeas)) OF ResultNR-Item

ResultNR-Item ::= SEQUENCE {

nR-PCI NR-PCI,

nR-ARFCN NR-ARFCN,

valueSS-RSRP-Cell ValueRSRP-NR OPTIONAL,

valueSS-RSRQ-Cell ValueRSRQ-NR OPTIONAL,

sS-RSRP-PerSSB ResultSS-RSRP-PerSSB OPTIONAL,

sS-RSRQ-PerSSB ResultSS-RSRQ-PerSSB OPTIONAL,

cGI-NR CGI-NR OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { ResultNR-Item-ExtIEs} } OPTIONAL,

...

}

ResultNR-Item-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

ResultUTRAN ::= SEQUENCE (SIZE (1.. maxUTRANMeas)) OF ResultUTRAN-Item

ResultUTRAN-Item ::= SEQUENCE {

uARFCN UARFCN,

physCellIDUTRAN CHOICE {

physCellIDUTRA-FDD PhysCellIDUTRA-FDD,

physCellIDUTRA-TDD PhysCellIDUTRA-TDD

},

uTRA-RSCP UTRA-RSCP OPTIONAL,

uTRA-EcN0 UTRA-EcN0 OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { ResultUTRAN-Item-ExtIEs} } OPTIONAL,

...

}

ResultUTRAN-Item-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

RSSI ::= INTEGER (0..63, ...)

-- S

SCS-SpecificCarrier ::= SEQUENCE {

offsetToCarrier INTEGER (0..2199,...),

subcarrierSpacing ENUMERATED {kHz15, kHz30, kHz60, kHz120,...},

carrierBandwidth INTEGER (0..275,...),

iE-Extensions ProtocolExtensionContainer { { SCS-SpecificCarrier-ExtIEs } } OPTIONAL,

...

}

SCS-SpecificCarrier-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

Search-window-information ::= SEQUENCE {

expectedPropagationDelay INTEGER (-3841..3841,...),

delayUncertainty INTEGER (1..246,...),

iE-Extensions ProtocolExtensionContainer { { Search-window-information-ExtIEs } } OPTIONAL,

...

}

Search-window-information-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

SFNInitialisationTime ::= BIT STRING (SIZE (64))

SFNInitialisationTime-EUTRA ::= BIT STRING (SIZE (64))

SlotNumber ::= INTEGER (0..79)

SpatialDirectionInformation ::= SEQUENCE {

nR-PRS-Beam-Information NR-PRS-Beam-Information,

iE-Extensions ProtocolExtensionContainer { { SpatialDirectionInformation-ExtIEs } } OPTIONAL,

...

}

SpatialDirectionInformation-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

SpatialRelationInfo ::= SEQUENCE {

spatialRelationforResourceID SpatialRelationforResourceID,

iE-Extensions ProtocolExtensionContainer { {SpatialRelationInfo-ExtIEs} } OPTIONAL,

...

}

SpatialRelationInfo-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

SpatialRelationforResourceID ::= SEQUENCE (SIZE(1..maxnoSpatialRelations)) OF SpatialRelationforResourceIDItem

SpatialRelationforResourceIDItem ::= SEQUENCE {

referenceSignal ReferenceSignal,

iE-Extensions ProtocolExtensionContainer { {SpatialRelationforResourceIDItem-ExtIEs} } OPTIONAL,

...

}

SpatialRelationforResourceIDItem-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

SpatialRelationPos ::= CHOICE {

sSBPos SSBPos,

pRSInformationPos PRSInformationPos,

choice-extension ProtocolIE-Single-Container {{ SpatialInformationPos-ExtIEs }}

}

SpatialInformationPos-ExtIEs NRPPA-PROTOCOL-IES ::= {

...

}

SRSConfig ::= SEQUENCE {

sRSResource-List SRSResource-List OPTIONAL,

posSRSResource-List PosSRSResource-List OPTIONAL,

sRSResourceSet-List SRSResourceSet-List OPTIONAL,

posSRSResourceSet-List PosSRSResourceSet-List OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { SRSConfig-ExtIEs } } OPTIONAL,

...

}

SRSConfig-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

SRSCarrier-List ::= SEQUENCE (SIZE(1.. maxnoSRS-Carriers)) OF SRSCarrier-List-Item

SRSCarrier-List-Item ::= SEQUENCE {

pointA INTEGER (0..3279165,...),

uplinkChannelBW-PerSCS-List UplinkChannelBW-PerSCS-List,

activeULBWP ActiveULBWP,

pCI INTEGER (0..1007) OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { SRSCarrier-List-Item-ExtIEs } } OPTIONAL,

...

}

SRSCarrier-List-Item-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

SRSConfiguration ::= SEQUENCE {

sRSCarrier-List SRSCarrier-List, iE-Extensions ProtocolExtensionContainer { { SRSConfiguration-ExtIEs } } OPTIONAL,

...

}

SRSConfiguration-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

SRSPosResourceID ::= INTEGER (0..63, ...)

SRSResource::= SEQUENCE {

sRSResourceID SRSResourceID,

nrofSRS-Ports ENUMERATED {port1, ports2, ports4},

transmissionComb TransmissionComb,

startPosition INTEGER (0..13),

nrofSymbols ENUMERATED {n1, n2, n4},

repetitionFactor ENUMERATED {n1, n2, n4},

freqDomainPosition INTEGER (0..67),

freqDomainShift INTEGER (0..268),

c-SRS INTEGER (0..63),

b-SRS INTEGER (0..3),

b-hop INTEGER (0..3),

groupOrSequenceHopping ENUMERATED { neither, groupHopping, sequenceHopping },

resourceType ResourceType,

slotOffset INTEGER (0..2559),

sequenceId INTEGER (0..1023),

iE-Extensions ProtocolExtensionContainer { { SRSResource-ExtIEs } } OPTIONAL,

...

}

SRSResource-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

SRSResourceID ::= INTEGER (0..63, ...)

SRSResource-List ::= SEQUENCE (SIZE (1..maxnoSRS-Resources)) OF SRSResource

SRSResourceSet-List ::= SEQUENCE (SIZE (1..maxnoSRS-ResourceSets)) OF SRSResourceSet

SRSResourceID-List::= SEQUENCE (SIZE (1..maxnoSRS-ResourcePerSet)) OF SRSResourceID

SRSResourceSet::= SEQUENCE {

sRSResourceSetID INTEGER(0..15),

sRSResourceID-List SRSResourceID-List,

resourceSetType ResourceSetType,

iE-Extensions ProtocolExtensionContainer { { SRSResourceSet-ExtIEs } } OPTIONAL,

...

}

SRSResourceSet-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

SRSResourceSetID ::= INTEGER (0..15, ...)

SRSResourceTrigger ::= SEQUENCE {

aperiodicSRSResourceTriggerList AperiodicSRSResourceTriggerList,

iE-Extensions ProtocolExtensionContainer { {SRSResourceTrigger-ExtIEs} } OPTIONAL,

...

}

SRSResourceTrigger-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

SRSSpatialRelation ::= SEQUENCE {

spatialRelationforResourceID SpatialRelationforResourceID,

iE-Extensions ProtocolExtensionContainer { {SRSSpatialRelation-ExtIEs} } OPTIONAL,

...

}

SRSSpatialRelation-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

SSBInfo ::= SEQUENCE {

listOfSSBInfo SEQUENCE (SIZE (1..maxNoSSBs)) OF SSBInfoList,

iE-Extensions ProtocolExtensionContainer { {SSBInfo-ExtIEs} } OPTIONAL,

...

}

SSBInfo-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

SSBInfoList ::= SEQUENCE {

pCI-NR INTEGER (0..1007),

sSB-Configuration TF-Configuration,

iE-Extensions ProtocolExtensionContainer { { SSBInfoList-ExtIEs} } OPTIONAL,

...

}

SSBInfoList-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

SSB ::= SEQUENCE {

pCI-NR INTEGER (0..1007),

ssb-index INTEGER (0..63) OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {SSB-ExtIEs} } OPTIONAL,

...

}

SSB-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

SSBPos ::= SEQUENCE {

pCI-NR INTEGER (0..1007) OPTIONAL,

ssb-index INTEGER (0..63),

iE-Extensions ProtocolExtensionContainer { {SSBPos-ExtIEs} } OPTIONAL,

...

}

SSBPos-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

SSBBurstPosition ::= CHOICE {

shortBitmap BIT STRING (SIZE(4)),

mediumBitmap BIT STRING (SIZE(8)),

longBitmap BIT STRING (SIZE(64)),

...

}

SSB-Index ::= INTEGER(0..63)

SSID ::= OCTET STRING (SIZE(1..32))

SystemFrameNumber ::= INTEGER (0..1023)

SystemInformation ::= SEQUENCE (SIZE (1.. maxNrOfPosSImessage)) OF SEQUENCE {

broadcastPeriodicity BroadcastPeriodicity,

posSIBs PosSIBs,

iE-Extensions ProtocolExtensionContainer { { SystemInformation-ExtIEs} } OPTIONAL,

...

}

SystemInformation-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

-- T

TAC ::= OCTET STRING (SIZE(3))

TDD-Config-EUTRA-Item ::= SEQUENCE {

subframeAssignment ENUMERATED { sa0, sa1, sa2, sa3, sa4, sa5, sa6, ... },

iE-Extensions ProtocolExtensionContainer { { TDD-Config-EUTRA-Item-Item-ExtIEs } } OPTIONAL,

...

}

TDD-Config-EUTRA-Item-Item-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

TF-Configuration ::= SEQUENCE {

sSB-frequency INTEGER (0..3279165),

sSB-subcarrier-spacing ENUMERATED {kHz15, kHz30, kHz120, kHz240, ...},

sSB-Transmit-power INTEGER (-60..50),

sSB-periodicity ENUMERATED {ms5, ms10, ms20, ms40, ms80, ms160, ...},

sSB-half-frame-offset INTEGER(0..1),

sSB-SFN-offset INTEGER(0..15),

sSB-BurstPosition SSBBurstPosition OPTIONAL,

sFN-initialisation-time SFNInitialisationTime OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { TF-Configuration-ExtIEs} } OPTIONAL,

...

}

TF-Configuration-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

TimeStamp ::= SEQUENCE {

systemFrameNumber SystemFrameNumber,

slotIndex TimeStampSlotIndex,

measurementTime SFNInitialisationTime OPTIONAL,

iE-Extension ProtocolExtensionContainer { { TimeStamp-ExtIEs} } OPTIONAL,

...

}

TimeStamp-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

TimeStampSlotIndex ::= CHOICE {

sCS-15 INTEGER(0..9),

sCS-30 INTEGER(0..19),

sCS-60 INTEGER(0..39),

sCS-120 INTEGER(0..79),

choice-extension ProtocolIE-Single-Container { { TimeStampSlotIndex-ExtIEs} }

}

TimeStampSlotIndex-ExtIEs NRPPA-PROTOCOL-IES ::= {

...

}

TP-ID-EUTRA ::= INTEGER (0..4095, ...)

TP-Type-EUTRA ::= ENUMERATED { prs-only-tp, ... }

TransmissionComb ::= CHOICE {

n2 SEQUENCE {

combOffset-n2 INTEGER (0..1),

cyclicShift-n2 INTEGER (0..7)

},

n4 SEQUENCE {

combOffset-n4 INTEGER (0..3),

cyclicShift-n4 INTEGER (0..11)

},

choice-extension ProtocolIE-Single-Container { { TransmissionComb-ExtIEs} }

}

TransmissionComb-ExtIEs NRPPA-PROTOCOL-IES ::= {

...

}

TransmissionCombPos ::= CHOICE {

n2 SEQUENCE {

combOffset-n2 INTEGER (0..1),

cyclicShift-n2 INTEGER (0..7)

},

n4 SEQUENCE {

combOffset-n4 INTEGER (0..3),

cyclicShift-n4 INTEGER (0..11)

},

n8 SEQUENCE {

combOffset-n8 INTEGER (0..7),

cyclicShift-n8 INTEGER (0..5)

},

choice-extension ProtocolIE-Single-Container { { TransmissionCombPos-ExtIEs} }

}

TransmissionCombPos-ExtIEs NRPPA-PROTOCOL-IES ::= {

...

}

TRPMeasurementQuantities ::= SEQUENCE (SIZE (1..maxnoPosMeas)) OF TRPMeasurementQuantitiesList-Item

TRPMeasurementQuantitiesList-Item ::= SEQUENCE {

tRPMeasurementQuantities-Item TRPMeasurementQuantities-Item,

timingReportingGranularityFactor INTEGER (0..5) OPTIONAL,

iE-Extensions ProtocolExtensionContainer {{ TRPMeasurementQuantitiesList-Item-ExtIEs}} OPTIONAL,

...

}

TRPMeasurementQuantitiesList-Item-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

TRPMeasurementQuantities-Item ::= ENUMERATED {

gNB-RxTxTimeDiff,

uL-SRS-RSRP,

uL-AoA,

uL-RTOA,

...

}

TrpMeasurementResult ::= SEQUENCE (SIZE (1.. maxnoPosMeas)) OF TrpMeasurementResultItem

TrpMeasurementResultItem ::= SEQUENCE {

measuredResultsValue TrpMeasuredResultsValue,

timeStamp TimeStamp,

measurementQuality TrpMeasurementQuality OPTIONAL,

measurementBeamInfo MeasurementBeamInfo OPTIONAL,

iE-Extensions ProtocolExtensionContainer {{TrpMeasurementResultItem-ExtIEs}} OPTIONAL,

...

}

TrpMeasurementResultItem-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

TrpMeasuredResultsValue ::= CHOICE {

uL-AngleOfArrival UL-AoA,

uL-SRS-RSRP UL-SRS-RSRP,

uL-RTOA UL-RTOAMeasurement,

gNB-RxTxTimeDiff GNB-RxTxTimeDiff,

choice-extension ProtocolIE-Single-Container { { TrpMeasuredResultsValue-ExtIEs } }

}

TrpMeasuredResultsValue-ExtIEs NRPPA-PROTOCOL-IES ::= {

...

}

TrpMeasurementQuality ::= CHOICE {

timingMeasQuality TrpMeasurementTimingQuality,

angleMeasQuality TrpMeasurementAngleQuality,

choice-Extension ProtocolIE-Single-Container {{ TrpMeasurementQuality-ExtIEs}}

}

TrpMeasurementQuality-ExtIEs NRPPA-PROTOCOL-IES ::= {

...

}

TrpMeasurementTimingQuality ::= SEQUENCE {

measurementQuality INTEGER (0..31),

resolution ENUMERATED {m0dot1, m1, m10, m30, ...},

...

}

TrpMeasurementAngleQuality ::= SEQUENCE {

azimuthQuality INTEGER (0..255),

zenithQuality INTEGER (0..255) OPTIONAL,

resolution ENUMERATED {deg0dot1, ...},

...

}

TRP-MeasurementRequestList ::= SEQUENCE (SIZE (1..maxNoOfMeasTRPs)) OF TRP-MeasurementRequestItem

TRP-MeasurementRequestItem ::= SEQUENCE {

tRP-ID TRP-ID,

search-window-information Search-window-information OPTIONAL,

iE-extensions ProtocolExtensionContainer { { TRP-MeasurementRequestItem-ExtIEs } } OPTIONAL,

...

}

TRP-MeasurementRequestItem-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

TRP-MeasurementResponseList ::= SEQUENCE (SIZE (1..maxNoOfMeasTRPs)) OF TRP-MeasurementResponseItem

TRP-MeasurementResponseItem ::= SEQUENCE {

tRP-ID TRP-ID,

measurementResult TrpMeasurementResult,

iE-extensions ProtocolExtensionContainer { { TRP-MeasurementResponseItem-ExtIEs } } OPTIONAL,

...

}

TRP-MeasurementResponseItem-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

TRPInformationList ::= SEQUENCE (SIZE (1.. maxnoTRPs)) OF SEQUENCE {

tRP-ID TRP-ID,

tRPInformation TRPInformation,

iE-Extensions ProtocolExtensionContainer { {TRPInformation-ExtIEs} } OPTIONAL,

...

}

TRPInformation-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

TRPInformation ::= SEQUENCE (SIZE (1..maxnoTRPInfoTypes)) OF TRPInformationItem

TRPInformationItem ::= CHOICE {

pCI-NR INTEGER (0..1007),

nG-RAN-CGI NG-RAN-CGI,

aRFCN INTEGER (0..3279165),

pRSConfiguration PRSConfiguration,

sSBinformation SSBInfo,

sFNInitialisationTime SFNInitialisationTime,

spatialDirectionInformation SpatialDirectionInformation,

geographicalCoordinates GeographicalCoordinates,

choice-extension ProtocolIE-Single-Container { { TRPInformationItem-ExtIEs } }

}

TRPInformationItem-ExtIEs NRPPA-PROTOCOL-IES ::= {

...

}

TRPInformationTypeList ::= SEQUENCE (SIZE(1.. maxnoTRPInfoTypes)) OF TRPInformationTypeItem

TRPInformationTypeItem ::= ENUMERATED {

nrPCI,

nG-RAN-CGI,

arfcn,

pRSConfig,

sSBInfo,

sFNInitTime,

spatialDirectInfo,

geoCoord,

...

}

TRPList ::= SEQUENCE (SIZE(1.. maxnoTRPs)) OF TRPItem

TRPItem ::= SEQUENCE {

tRP-ID TRP-ID,

...

}

TRP-ID ::= INTEGER (1.. maxnoTRPs, ...)

TRPPositionDefinitionType ::= CHOICE {

direct TRPPositionDirect,

referenced TRPPositionReferenced,

choice-extension ProtocolIE-Single-Container { { TRPPositionDefinitionType-ExtIEs } }

}

TRPPositionDefinitionType-ExtIEs NRPPA-PROTOCOL-IES ::= {

...

}

TRPPositionDirect ::= SEQUENCE {

accuracy TRPPositionDirectAccuracy,

iE-extensions ProtocolExtensionContainer { { TRPPositionDirect-ExtIEs } } OPTIONAL,

...

}

TRPPositionDirect-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

TRPPositionDirectAccuracy ::= CHOICE {

tRPPosition NG-RANAccessPointPosition ,

tRPHAposition NGRANHighAccuracyAccessPointPosition ,

choice-extension ProtocolIE-Single-Container { { TRPPositionDirectAccuracy-ExtIEs } }

}

TRPPositionDirectAccuracy-ExtIEs NRPPA-PROTOCOL-IES ::= {

...

}

TRPPositionReferenced ::= SEQUENCE {

referencePoint ReferencePoint,

referencePointType TRPReferencePointType,

iE-extensions ProtocolExtensionContainer { { TRPPositionReferenced-ExtIEs } } OPTIONAL,

...

}

TRPPositionReferenced-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

TRPReferencePointType ::= CHOICE {

tRPPositionRelativeGeodetic RelativeGeodeticLocation,

tRPPositionRelativeCartesian RelativeCartesianLocation,

choice-extension ProtocolIE-Single-Container { { TRPReferencePointType-ExtIEs } }

}

TRPReferencePointType-ExtIEs NRPPA-PROTOCOL-IES ::= {

...

}

TypeOfError ::= ENUMERATED {

not-understood,

missing,

...

}

-- U

UARFCN ::= INTEGER (0..16383, ...)

UE-Measurement-ID ::= INTEGER (1..15, ..., 256)

UTRA-EcN0 ::= INTEGER (0..49, ...)

UTRA-RSCP ::= INTEGER (-5..91, ...)

UL-AoA ::= SEQUENCE {

azimuthAoA INTEGER (0..3599),

zenithAoA INTEGER (0..1799) OPTIONAL,

angleCoordinateSystem ENUMERATED {lCS, gCS} OPTIONAL,

iE-extensions ProtocolExtensionContainer { { UL-AoA-ExtIEs } } OPTIONAL,

...

}

UL-AoA-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

UL-RTOAMeasurement ::= SEQUENCE {

uLRTOAmeas ULRTOAMeas,

additionalPathList AdditionalPathList OPTIONAL,

...

}

ULRTOAMeas::= CHOICE {

k0 INTEGER (0.. 1970049),

k1 INTEGER (0.. 985025),

k2 INTEGER (0.. 492513),

k3 INTEGER (0.. 246257),

k4 INTEGER (0.. 123129),

k5 INTEGER (0.. 61565),

...

}

UL-SRS-RSRP ::= INTEGER (0..127)

UplinkChannelBW-PerSCS-List ::= SEQUENCE (SIZE (1..maxnoSCSs)) OF SCS-SpecificCarrier

-- V

ValueRSRP-EUTRA ::= INTEGER (0..97, ...)

ValueRSRQ-EUTRA ::= INTEGER (0..34, ...)

ValueRSRP-NR ::= INTEGER (0..127)

ValueRSRQ-NR ::= INTEGER (0..127)

-- W

WLANMeasurementQuantities ::= SEQUENCE (SIZE (0.. maxNoMeas)) OF ProtocolIE-Single-Container { {WLANMeasurementQuantities-ItemIEs} }

WLANMeasurementQuantities-ItemIEs NRPPA-PROTOCOL-IES ::= {

{ ID id-WLANMeasurementQuantities-Item CRITICALITY reject TYPE WLANMeasurementQuantities-Item PRESENCE mandatory}}

WLANMeasurementQuantities-Item ::= SEQUENCE {

wLANMeasurementQuantitiesValue WLANMeasurementQuantitiesValue,

iE-Extensions ProtocolExtensionContainer { { WLANMeasurementQuantitiesValue-ExtIEs} } OPTIONAL,

...

}

WLANMeasurementQuantitiesValue-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

WLANMeasurementQuantitiesValue ::= ENUMERATED {

wlan,

...

}

WLANMeasurementResult ::= SEQUENCE (SIZE (1..maxNoMeas)) OF WLANMeasurementResult-Item

WLANMeasurementResult-Item ::= SEQUENCE {

wLAN-RSSI WLAN-RSSI,

sSID SSID OPTIONAL,

bSSID BSSID OPTIONAL,

hESSID HESSID OPTIONAL,

operatingClass WLANOperatingClass OPTIONAL,

countryCode WLANCountryCode OPTIONAL,

wLANChannelList WLANChannelList OPTIONAL,

wLANBand WLANBand OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { WLANMeasurementResult-Item-ExtIEs } } OPTIONAL,

...

}

WLANMeasurementResult-Item-ExtIEs NRPPA-PROTOCOL-EXTENSION ::= {

...

}

WLAN-RSSI ::= INTEGER (0..141, ...)

WLANBand ::= ENUMERATED {band2dot4, band5, ...}

WLANChannelList ::= SEQUENCE (SIZE (1..maxWLANchannels)) OF WLANChannel

WLANChannel ::= INTEGER (0..255)

WLANCountryCode ::= ENUMERATED {

unitedStates,

europe,

japan,

global,

...

}

WLANOperatingClass ::= INTEGER (0..255)

-- X

-- Y

-- Z

END

-- ASN1STOP

### 9.3.6 Common definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Common definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

NRPPA-CommonDataTypes {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-access (22) modules (3) nrppa (4) version1 (1) nrppa-CommonDataTypes (3)}

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Extension constants

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

maxPrivateIEs INTEGER ::= 65535

maxProtocolExtensions INTEGER ::= 65535

maxProtocolIEs INTEGER ::= 65535

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Common Data Types

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

Criticality ::= ENUMERATED { reject, ignore, notify }

NRPPATransactionID ::= INTEGER (0..32767)

Presence ::= ENUMERATED { optional, conditional, mandatory }

PrivateIE-ID ::= CHOICE {

local INTEGER (0.. maxPrivateIEs),

global OBJECT IDENTIFIER

}

ProcedureCode ::= INTEGER (0..255)

ProtocolIE-ID ::= INTEGER (0..maxProtocolIEs)

TriggeringMessage ::= ENUMERATED { initiating-message, successful-outcome, unsuccessful-outcome}

END

-- ASN1STOP

### 9.3.7 Constant definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Constant definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

NRPPA-Constants {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-access (22) modules (3) nrppa (4) version1 (1) nrppa-Constants (4) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

IMPORTS

ProcedureCode,

ProtocolIE-ID

FROM NRPPA-CommonDataTypes;

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Elementary Procedures

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

id-errorIndication ProcedureCode ::= 0

id-privateMessage ProcedureCode ::= 1

id-e-CIDMeasurementInitiation ProcedureCode ::= 2

id-e-CIDMeasurementFailureIndication ProcedureCode ::= 3

id-e-CIDMeasurementReport ProcedureCode ::= 4

id-e-CIDMeasurementTermination ProcedureCode ::= 5

id-oTDOAInformationExchange ProcedureCode ::= 6

id-assistanceInformationControl ProcedureCode ::= 7

id-assistanceInformationFeedback ProcedureCode ::= 8

id-positioningInformationExchange ProcedureCode ::= 9

id-positioningInformationUpdate ProcedureCode ::= 10

id-Measurement ProcedureCode ::= 11

id-MeasurementReport ProcedureCode ::= 12

id-MeasurementUpdate ProcedureCode ::= 13

id-MeasurementAbort ProcedureCode ::= 14

id-MeasurementFailureIndication ProcedureCode ::= 15

id-tRPInformationExchange ProcedureCode ::= 16

id-positioningActivation ProcedureCode ::= 17

id-positioningDeactivation ProcedureCode ::= 18

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Lists

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

maxNrOfErrors INTEGER ::= 256

maxCellinRANnode INTEGER ::= 3840

maxIndexesReport INTEGER ::= 64

maxNoMeas INTEGER ::= 64

maxCellReport INTEGER ::= 9

maxCellReportNR INTEGER ::= 9

maxnoOTDOAtypes INTEGER ::= 63

maxServCell INTEGER ::= 5

maxEUTRAMeas INTEGER ::= 8

maxGERANMeas INTEGER ::= 8

maxNRMeas INTEGER ::= 8

maxUTRANMeas INTEGER ::= 8

maxWLANchannels INTEGER ::= 16

maxnoFreqHoppingBandsMinusOne INTEGER ::= 7

maxNoPath INTEGER ::= 2

maxNrOfPosSImessage INTEGER ::= 32

maxnoAssistInfoFailureListItems INTEGER ::= 32

maxNrOfSegments INTEGER ::= 64

maxNrOfPosSIBs INTEGER ::= 32

maxNoOfMeasTRPs INTEGER ::= 64

maxnoTRPs INTEGER ::= 65535

maxnoTRPInfoTypes INTEGER ::= 64

maxnoofAngleInfo INTEGER ::= 65535

maxnolcs-gcs-translation INTEGER ::= 3

maxnoBcastCell INTEGER ::= 16384

maxnoSRSTriggerStates INTEGER ::= 3

maxnoSpatialRelations INTEGER ::= 64

maxnoPosMeas INTEGER ::= 16384

maxnoSRS-Carriers INTEGER ::= 32

maxnoSCSs INTEGER ::= 5

maxnoSRS-Resources INTEGER ::= 64

maxnoSRS-PosResources INTEGER ::= 64

maxnoSRS-ResourceSets INTEGER ::= 16

maxnoSRS-ResourcePerSet INTEGER ::= 16

maxnoSRS-PosResourceSets INTEGER ::= 16

maxnoSRS-PosResourcePerSet INTEGER ::= 16

maxPRS-ResourceSets INTEGER ::= 2

maxPRS-ResourcesPerSet INTEGER ::= 64

maxNoSSBs INTEGER ::= 255

maxnoofPRSresourceSet INTEGER ::= 8

maxnoofPRSresource INTEGER ::= 64

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IEs

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

id-Cause ProtocolIE-ID ::= 0

id-CriticalityDiagnostics ProtocolIE-ID ::= 1

id-LMF-UE-Measurement-ID ProtocolIE-ID ::= 2

id-ReportCharacteristics ProtocolIE-ID ::= 3

id-MeasurementPeriodicity ProtocolIE-ID ::= 4

id-MeasurementQuantities ProtocolIE-ID ::= 5

id-RAN-UE-Measurement-ID ProtocolIE-ID ::= 6

id-E-CID-MeasurementResult ProtocolIE-ID ::= 7

id-OTDOACells ProtocolIE-ID ::= 8

id-OTDOA-Information-Type-Group ProtocolIE-ID ::= 9

id-OTDOA-Information-Type-Item ProtocolIE-ID ::= 10

id-MeasurementQuantities-Item ProtocolIE-ID ::= 11

id-RequestedSRSTransmissionCharacteristics ProtocolIE-ID ::= 12

id-Cell-Portion-ID ProtocolIE-ID ::= 14

id-OtherRATMeasurementQuantities ProtocolIE-ID ::= 15

id-OtherRATMeasurementQuantities-Item ProtocolIE-ID ::= 16

id-OtherRATMeasurementResult ProtocolIE-ID ::= 17

id-WLANMeasurementQuantities ProtocolIE-ID ::= 19

id-WLANMeasurementQuantities-Item ProtocolIE-ID ::= 20

id-WLANMeasurementResult ProtocolIE-ID ::= 21

id-TDD-Config-EUTRA-Item ProtocolIE-ID ::= 22

id-Assistance-Information ProtocolIE-ID ::= 23

id-Broadcast ProtocolIE-ID ::= 24

id-AssistanceInformationFailureList ProtocolIE-ID ::= 25

id-SRSConfiguration ProtocolIE-ID ::= 26

id-MeasurementResult ProtocolIE-ID ::= 27

id-TRP-ID ProtocolIE-ID ::= 28

id-TRPInformationTypeList ProtocolIE-ID ::= 29

id-TRPInformationList ProtocolIE-ID ::= 30

id-MeasurementBeamInfoRequest ProtocolIE-ID ::= 31

id-ResultSS-RSRP ProtocolIE-ID ::= 32

id-ResultSS-RSRQ ProtocolIE-ID ::= 33

id-ResultCSI-RSRP ProtocolIE-ID ::= 34

id-ResultCSI-RSRQ ProtocolIE-ID ::= 35

id-AngleOfArrivalNR ProtocolIE-ID ::= 36

id-GeographicalCoordinates ProtocolIE-ID ::= 37

id-PositioningBroadcastCells ProtocolIE-ID ::= 38

id-LMF-Measurement-ID ProtocolIE-ID ::= 39

id-RAN-Measurement-ID ProtocolIE-ID ::= 40

id-TRP-MeasurementRequestList ProtocolIE-ID ::= 41

id-TRP-MeasurementResponseList ProtocolIE-ID ::= 42

id-TRP-MeasurementReportList ProtocolIE-ID ::= 43

id-SRSType ProtocolIE-ID ::= 44

id-ActivationTime ProtocolIE-ID ::= 45

id-SRSResourceSetID ProtocolIE-ID ::= 46

id-TRPList ProtocolIE-ID ::= 47

id-SRSSpatialRelation ProtocolIE-ID ::= 48

id-SystemFrameNumber ProtocolIE-ID ::= 49

id-SlotNumber ProtocolIE-ID ::= 50

id-SRSResourceTrigger ProtocolIE-ID ::= 51

id-TRPMeasurementQuantities ProtocolIE-ID ::= 52

id-AbortTransmission ProtocolIE-ID ::= 53

id-SFNInitialisationTime ProtocolIE-ID ::= 54

id-ResultNR ProtocolIE-ID ::= 55

id-ResultEUTRA ProtocolIE-ID ::= 56

END

-- ASN1STOP

### 9.3.8 Container definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Container definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

NRPPA-Containers {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-access (22) modules (3) nrppa (4) version1 (1) nrppa-Containers (5)}

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IE parameter types from other modules.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

IMPORTS

maxPrivateIEs,

maxProtocolExtensions,

maxProtocolIEs,

Criticality,

Presence,

PrivateIE-ID,

ProtocolIE-ID

FROM NRPPA-CommonDataTypes;

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Class Definition for Protocol IEs

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

NRPPA-PROTOCOL-IES ::= CLASS {

&id ProtocolIE-ID UNIQUE,

&criticality Criticality,

&Value,

&presence Presence

}

WITH SYNTAX {

ID &id

CRITICALITY &criticality

TYPE &Value

PRESENCE &presence

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Class Definition for Protocol Extensions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

NRPPA-PROTOCOL-EXTENSION ::= CLASS {

&id ProtocolIE-ID UNIQUE,

&criticality Criticality,

&Extension,

&presence Presence

}

WITH SYNTAX {

ID &id

CRITICALITY &criticality

EXTENSION &Extension

PRESENCE &presence

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Class Definition for Private IEs

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

NRPPA-PRIVATE-IES ::= CLASS {

&id PrivateIE-ID,

&criticality Criticality,

&Value,

&presence Presence

}

WITH SYNTAX {

ID &id

CRITICALITY &criticality

TYPE &Value

PRESENCE &presence

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Container for Protocol IEs

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ProtocolIE-Container { NRPPA-PROTOCOL-IES : IEsSetParam} ::=

SEQUENCE (SIZE (0..maxProtocolIEs)) OF

ProtocolIE-Field {{IEsSetParam}}

ProtocolIE-Single-Container { NRPPA-PROTOCOL-IES : IEsSetParam} ::=

ProtocolIE-Field {{IEsSetParam}}

ProtocolIE-Field { NRPPA-PROTOCOL-IES : IEsSetParam} ::= SEQUENCE {

id NRPPA-PROTOCOL-IES.&id ({IEsSetParam}),

criticality NRPPA-PROTOCOL-IES.&criticality ({IEsSetParam}{@id}),

value NRPPA-PROTOCOL-IES.&Value ({IEsSetParam}{@id})

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Container Lists for Protocol IE Containers

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ProtocolIE-ContainerList {INTEGER : lowerBound, INTEGER : upperBound, NRPPA-PROTOCOL-IES : IEsSetParam} ::=

SEQUENCE (SIZE (lowerBound..upperBound)) OF

ProtocolIE-Container {{IEsSetParam}}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Container for Protocol Extensions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ProtocolExtensionContainer { NRPPA-PROTOCOL-EXTENSION : ExtensionSetParam} ::=

SEQUENCE (SIZE (1..maxProtocolExtensions)) OF

ProtocolExtensionField {{ExtensionSetParam}}

ProtocolExtensionField { NRPPA-PROTOCOL-EXTENSION : ExtensionSetParam} ::= SEQUENCE {

id NRPPA-PROTOCOL-EXTENSION.&id ({ExtensionSetParam}),

criticality NRPPA-PROTOCOL-EXTENSION.&criticality ({ExtensionSetParam}{@id}),

extensionValue NRPPA-PROTOCOL-EXTENSION.&Extension ({ExtensionSetParam}{@id})

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Container for Private IEs

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PrivateIE-Container { NRPPA-PRIVATE-IES : IEsSetParam} ::=

SEQUENCE (SIZE (1..maxPrivateIEs)) OF

PrivateIE-Field {{IEsSetParam}}

PrivateIE-Field { NRPPA-PRIVATE-IES : IEsSetParam} ::= SEQUENCE {

id NRPPA-PRIVATE-IES.&id ({IEsSetParam}),

criticality NRPPA-PRIVATE-IES.&criticality ({IEsSetParam}{@id}),

value NRPPA-PRIVATE-IES.&Value ({IEsSetParam}{@id})

}

END

-- ASN1STOP

**END OF CHANGES**