**3GPP TSG RAN Meeting #89e RP-20xxxx**

**Electronic Meeting, September 14 - 18, 2020**

**Source: Nokia, Nokia Shanghai Bell**

**Title: New WID on introduction of lower 6GHz NR unlicensed operation for Europe**

**Document for: Approval**

**Agenda Item: 9.1.1**

3GPP™ Work Item Description

Information on Work Items can be found at <http://www.3gpp.org/Work-Items>   
See also the [3GPP Working Procedures](http://www.3gpp.org/specifications-groups/working-procedures), article 39 and the TSG Working Methods in [3GPP TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm)

# Title: Introduction of lower 6GHz NR unlicensed operation for Europe

## Acronym: xxxx

## Unique identifier: *{A number to be provided by MCC at the plenary}*

NOTE: For new WIs/SIs leave the Unique identifier empty and make a proposal for an Acronym.

For a revised WI/SI: Take Unique identifier and acronym as shown in 3GPP workplan.

If this is a RAN WID including Core and Perf. part, then Title, Acronym and Unique identifier refer to the feature WI.

Please tick (X) the applicable box(es) in the table below:

Either:

|  |  |
| --- | --- |
| **This WID includes a Core part** | **X** |
| **This WID includes a Performance part** | **X** |

or:

|  |  |  |
| --- | --- | --- |
| **This WID includes a Testing part** | |  |
| **and it addresses the following 3GPP work area:** | **Radio Access** |  |
| **Core Network** |  |
| **Services** |  |

Potential target Release: Rel-17.

Note that this field above indicates the proposed Release at the time of submission of the WID to TSG approval. It can later be changed without a need to revise the WID. The updated target Release is indicated in the Work Plan. NOTE: In case of contradiction with the target dates of clause 5, clause 5 determines the target release.

## 1 Impacts

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Affects:** | UICC apps | ME | AN | CN | Others (specify) |
| **Yes** |  | X | X |  |  |
| **No** | X |  |  | X | X |
| **Don't know** |  |  |  |  |  |

## 2 Classification of the Work Item and linked work items

### 2.1 Primary classification

This work item is a … *{Tick one box. "***Feature** */* **Building Block** */ Work Task" form a hierarchical structure. E.g. no Building Block can be proposed without a corresponding parent Feature. The full structure of all existing Work Items is shown in the 3GPP Work Plan in* [*ftp://ftp.3gpp.org/Information/WORK\_PLAN*](ftp://ftp.3gpp.org/Information/WORK_PLAN) *}*

|  |  |
| --- | --- |
|  | Feature |
| X | Building Block |
|  | *Work Task* |
|  | Study Item |

NOTE: Normally, Core/Perf./Testing parts in RAN WIDs are Building Blocks. Only if they are under an SA or CT umbrella, they are defined as work tasks. If you are in doubt, please contact MCC.

### 2.2 Parent Work Item

|  |  |  |  |
| --- | --- | --- | --- |
| Parent Work / Study Items | | | |
| Acronym | Working Group | Unique ID | Title (as in 3GPP Work Plan) |
|  |  |  |  |

NOTE: RAN agreed some time ago, that it describes the feature WI + Core/Perf. part WI or Testing part WI in one WID. Therefore the table above should just include the feature WI data (In case the feature covers Core and Perf. part, please list under Working Group the leading WG of the Core part).

### 2.3 Other related Work Items and dependencies

*{List here other Work Items which relate to the proposed one, such as preceding SI or a preceding WI (e.g. if further enhancing a feature).}*

|  |  |  |
| --- | --- | --- |
| Other related Work Items (if any) | | |
| Unique ID | Title | Nature of relationship |
|  |  | *{optional free text}* |

NOTE: Also related or dependent WIs/SIs in other TSGs should be indicated.

**Dependency on non-3GPP (draft) specification**: none

## 3 Justification

NR-Unlicensed is being standardized in Rel-16 with the definition of band n96 covering the spectrum range 5925-7125 MHz which is currently applicable in the USA only subject to FCC Report and Order [FCC 20-51].

Administrations in Europe are working on regulations for unlicensed operation in the range 5925-6425 MHz, and this work item addresses this range.

## 4 Objective

### 4.1 Objective of SI or Core part WI or Testing part WI

The objectives of the core part work item are:

* Depending on the details of the European regulatory requirements, determine whether they are best handled by relevant updates (if any) of band n96 or whether a new band is needed.
  + If a new band is needed, determine the band plan for unlicensed operation in the range 5925-6425 MHz
* Define or update (if needed) system parameters such as channel bandwidths and channel arrangements
* Define or update (if needed) transmitter and receiver characteristics requirements for the UE
* Define or update (if needed) transmitter and receiver characteristics requirements for the BS

### 4.2 Objective of Performance part WI

NOTE: Leave empty if the WI proposal does not contain a RAN performance part.

The objective of the performance part work item is to define or update (if needed) conformance requirements for BS testing.

Changes are to be made in a release-independent manner.

### 4.3 RAN time budget request (not applicable to RAN5 WIs/SIs)

NOTE: For all new RAN related WIs/SIs which are not led by RAN WG5 the WI/SI rapporteur has to fill out the attached Excel table to request time budgets for corresponding RAN WG meetings.  
The Excel table has to be filled out for all affected RAN WGs and up to the target date of the WI/SI.  
One time unit (TU) corresponds to ~ 2 hours in the meeting.  
If no TU is needed, then leave the field empty otherwise enter a number >0 in the field.

For revisions of already approved WI/SI descriptions: Please remove the Excel table from the WID/SID's zip file. The time budgets are already recorded. If you want to modify them, then this has to be done via the status report and not via a revised WID/SID.

If this WID is covering Core and Performance part, then please fill out one line for each part in the attached Excel table.

**additional comments to the time budget request in the attached Excel table:**

## 5 Expected Output and Time scale

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **New specifications** *{One line per specification. Create/delete lines as needed}* | | | | | |
| Type | TS/TR number | Title | For info  at TSG# | For approval at TSG# | Remarks |
|  |  |  |  |  |  |

NOTE: If this is a RAN WI including Core and Perf. part, then all new Core part specs have to be listed first and then all new Perf. part specs. Indicate "Core part" or "Perf. part" under Remarks for each spec.  
By default a new specs can only be new for one of both parts.

The work shall start immediately after new regional regulatory requirements are available for the 5925-6425 MHz frequency range. TSG RAN is to review the availability of regulatory requirements at each TSG meeting.

|  |  |  |  |
| --- | --- | --- | --- |
| **Impacted existing TS/TR** *{One line per specification. Create/delete lines as needed}* | | | |
| TS/TR No. | Description of change | Target completion plenary# | Remarks |
| 38.101-1 | NR; UE Radio transmission and reception | 6 months after the start of the work | Core UE part |
| 38.133 | NR; Requirements for support of radio resource management | 6 months after the start of the work | Core UE part |
| 38.104 | NR; BS Radio transmission and reception | 6 months after the start of the work | Core BS part |
| 38.141-1 | NR; Base Station (BS) conformance testing Part 1: Conducted conformance testing | 9 months after the start of the work | Perf. BS part |
| 38.141-2 | NR; Base Station (BS) conformance testing Part 2: Radiated conformance testing | 9 months after the start of the work | Perf. BS part |
| 36.104 | E-UTRA; BS Radio transmission and reception | 6 months after the start of the work | Core BS part |
| 36.141 | E-UTRA; BS conformance testing | 9 months after the start of the work | Perf. BS part |
| 37.104 | E-UTRA, UTRA and GSM/EDGE; Multi-Standard Radio (MSR) Base Station (BS) radio transmission and reception | 6 months after the start of the work | Core BS part |
| 37.141 | E-UTRA, UTRA and GSM/EDGE; Multi-Standard Radio (MSR) Base Station (BS) conformance testing | 9 months after the start of the work | Perf. BS part |
| 37.105 | Active Antenna System (AAS) Base Station (BS) transmission and reception | 6 months after the start of the work | Core BS part |
| 37.145-1 | Active Antenna System (AAS) Base Station (BS) conformance testing; Part 1: conducted conformance testing | 9 months after the start of the work | Perf. BS part |
| 37.145-2 | Active Antenna System (AAS) Base Station (BS) conformance testing; Part 2: radiated conformance testing | 9 months after the start of the work | Perf. BS part |
|  |  |  |  |

NOTE: If this is a RAN WI including Core and Perf. part, then all new Core part specs have to be listed first and then all new Perf. part specs. Indicate "Core part" or "Perf. part" under Remarks for each spec.  
If an existing spec is affected by both (Core part and Perf. part), then it has to be listed twice with appropriate approval dates.

## 6 Work item Rapporteur(s)

Johannes Hejselbaek, Nokia, johannes.hejselbaek@nokia.com

## 7 Work item leadership

RAN4

## 8 Aspects that involve other WGs

NOTE: For RAN WIs: Section 8 applies only toWGs outside of TSG RAN because RAN WG aspects have to be covered in section 4.

## 9 Supporting Individual Members

|  |
| --- |
| Supporting IM name |
| Nokia |
| Nokia Shanghai Bell |
| BT |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |