**3GPP TSG-RAN Meeting #90e *RP-202878***

**Electronic Meeting, December 7 – 11, 2020**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.0* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.101-2** | **CR** | **0312** | **rev** | **1** | **Current version:** | **16.5.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | CR to 38.101-2 on handling of fallbacks for FR2 CA | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | - | | | | | | | | | |
| ***Source to TSG:*** | Apple Inc. | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_newRAT-Core | | | | |  | ***Date:*** | | | 2020-12-07 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **A** |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12)* *Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | This specification is not aligned with other specifications (38.331 and 38.306) with regards to which fallback band combinations are supported for the class of EN-DC combinations which include CA combinations consist of mixed contiguous and non-contiguous intra-band CA within FR2. In an effort to reconcile this issue, it has been recognized that mandating additional in-gap requirements for all possible mixed contiguous and non-contiguous fallback band combinations results in a high number of requirements and is a burden on UE development. Together with per-UE capability signaling, this CR aligns the RAN4 specification with RAN2 specifications. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | For FR2 intra-band CA combinations with multiple sub-blocks, where at least one of the sub-blocks consists of a contiguous CA combination, the following two changes are implemented:  1. Remove the requirement of direct fallback to single FR2 carrier  2. Based on UE signaling a capability bit, introduce an applicability rule for Rx requirements (impacting clauses 7.5A, 7.5D, 7.6A, 7.6D) for fallbacks with multiple sub-blocks, where at least one of the sub-blocks consists of a contiguous CA combination  Changes to RAN2 specifications on UE capabilities (38.306) and RRC (38.331) are needed to introduce per-UE capability.  **Impact analysis**  Impacted functionality:  Requirements for band combinations.  Inter-operability:  No inter-operability issues are foreseen. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | This specification is not aligned with other specifications (38.331 and 38.306) with regards to which fallback band combinations are supported. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 4.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | | **X** |  | Other core specifications | | | | TS38.306, TS38.331 | | |
| ***affected:*** | | **X** |  | Test specifications | | | | TS38.521-2 | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | |  | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR implements the principles for handling the FR2 fallback issue as described in RP-202556 | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | RP-201873 was postponed during the RAN #89e meeting. This CR is a revision of RP-202576. | | | | | | | | |

## **<Start of Changes>**

## 4.2 Applicability of minimum requirements

a) In this specification the Minimum Requirements are specified as general requirements and additional requirements. Where the Requirement is specified as a general requirement, the requirement is mandated to be met in all scenarios

b) For specific scenarios for which an additional requirement is specified, in addition to meeting the general requirement, the UE is mandated to meet the additional requirements.

c) The spurious emissions power requirements are for the long-term average of the power. For the purpose of reducing measurement uncertainty it is acceptable to average the measured power over a period of time sufficient to reduce the uncertainty due to the statistical nature of the signal

d) All the requirements for intra-band contiguous and non-contiguous CA apply under the assumption of the same slot format indicated by *TDD-UL-DL-ConfigurationCommon and TDD-UL-DL-ConfigurationDedicated* in the PCell and SCells for NR SA.

For FR2 intra-band CA configurations with multiple sub-blocks, where at least one of the sub-blocks is a contiguous CA configuration:

- If the field *partialFR2-FallbackRX-Req* is not present, the UE shall meet all applicable UE RF requirements for the highest order CA configuration and all associated fallback CA configurations;

- If the field *partialFR2-FallbackRX-Req* is present, for each FR2 intra-band CA configuration with multiple sub-blocks that the UE indicates support for explicitly, in-gap UE RF requirements of the highest order CA configuration in clauses 7.5A, 7.5D, 7.6A, 7.6D apply as the equivalent requirements for fallback CA configurations with the same number of sub-blocks, where at least one of the sub-blocks consists of a contiguous CA configuration. The UE shall meet all applicable UE RF requirements for fallback CA configurations with a lesser number of sub-blocks and of the highest order;

- Regardless of the field *partialFR2-FallbackRX-Req*, the UE shall meet all DL out-of-gap requirements for all lower order fallback CA configurations.

## **<End of Changes>**