**3GPP TSG-RAN Meeting #93-e RP-21xxxx**

**Electronic Meeting, September 13-17, 2021**

**Agenda item:** 9.3.4.3

**Source:** Moderator (China Telecom)

**Title:** Moderator's summary for discussion [93e-25-CRSIntfHandling]

**Document for:** Discussion

# Introduction

This document is the summary of email discussion [93e-25-CRSIntfHandling] on CRS interference handling for NR PDSCH in scenarios with overlapping spectrum for LTE and NR, and the discussion outcome (if any) will be reflected in the revised WID on “Rel-17 Further enhancement on NR demodulation performance”.

All the following 5 tdocs recommend to define NR PDSCH demodulation requirements for neighbouring cell LTE CRS-IM in Rel-17, and the main discussion point is whether network assistance signalling for CRS-IM is needed or not.

|  |  |  |
| --- | --- | --- |
| Tdoc | Title | Source |
| [RP‑211835](file:///D:\0_Work\Standardization\RAN\RAN%2093%20(Sep%202021)\Tdoc%20list\docs\RP-211835.zip) | Revised WID: Further enhancement on NR demodulation performance | China Telecom |
| [RP‑211950](file:///D:\0_Work\Standardization\RAN\RAN%2093%20(Sep%202021)\Tdoc%20list\docs\RP-211950.zip) | CRS interference handling in NR | Apple, MediaTek |
| [RP‑212199](file:///D:\0_Work\Standardization\RAN\RAN%2093%20(Sep%202021)\Tdoc%20list\docs\RP-212199.zip) | Views on LTE CRS interference handling for NR UE | Nokia, Nokia Shanghai Bell |
| [RP‑212226](file:///D:\0_Work\Standardization\RAN\RAN%2093%20(Sep%202021)\Tdoc%20list\docs\RP-212226.zip) | Views on Rel-17 CRS-IM requirements in scenarios with overlapping spectrum for LTE and NR | Intel Corporation |
| [RP‑212490](file:///D:\0_Work\Standardization\RAN\RAN%2093%20(Sep%202021)\Tdoc%20list\docs\RP-212490.zip) | LS on RAN4 evaluation for LTE CRS interference handling for NR UE (R4-2115741; to: RAN; cc: -; contact: China Telecom) | RAN4 |

# Initial round

## Open issues and companies views’ collection

**Issue #1**: Except the network assistance signalling part (which is discussed separately in Issue #2), any comments on the other parts of RAN4 recommendations in LS RP-212490?

*RAN4 recommends to define NR PDSCH demodulation requirements for neighbouring cell LTE CRS-IM in scenarios with overlapping spectrum for LTE and NR in Rel-17:*

*• Use LLR weighting as baseline reference receiver, and further discuss the feasibility of CRS-IC receiver taking into account the UE complexity and PDSCH processing time.*

*• Synchronous network scenario is prioritized. The asynchronous network scenario will be discussed after RAN #93e meeting.*

*• 15 kHz SCS for NR is prioritized. The 30 kHz SCS scenario will be discussed after RAN #93e meeting.*

*• RAN4 will further discuss the necessity of ~~network assistance signaling and~~ UE capability signaling during requirements definition phase.*

|  |  |
| --- | --- |
| Company | Comment |
| Huawei | We are fine with the RAN4 recommendation part shown above. |
| OPPO | Fine with the recommendations as above. |
| MTK | The recommendation is fine to us. But we want to clarify that removing network assistance in the last bullet does not mean network assistance information is out of scope, even if we do not reach the conclusion in **Issue #2**. |
| ZTE | RAN4 recommendations are fine with us. |
| Apple | We would like to understand the reason for deleting network assistance signalling part. We think network assistance might still be in the scope pending the outcome of discussion on Issue #2. |
| China Telecom | Support to add the RAN4 recommendations in the WID, unless any technical errors are found. For the network signalling part, if additional agreements can be achieved, it can be updated; otherwise, the original wording can be kept. |
| Samsung | We support RAN4 recommendations as a package in original LS |
| Qualcomm | We agree to take the LLR weighting as baseline to define the requirements. We think that the scenarios which are deprioritized should be left out for now due to lack of time in RAN4. They could be further discussed after the requirements for the “baseline scenario” are finalized. Our understanding that assistance data is discussed separately and the fact that it was erased does not mean it is out. |
| CMCC | We are fine with the recommendation. |
| Ericsson | The recommendations are OK for us in general. Regarding the receiver assumption, we would have some preference to ease the RAN4 workload to derive the requirements based on LLR weighting and deprioritize or take out of scope CRS-IC. Regarding network signalling, we add our view for the second issue; the objectives should be aligned with the end decision for that issue. |
| Intel | Support recommendation from LS.  In our paper we suggest the following wording change for the last three bullets:   * Synchronous network scenario is prioritized. The asynchronous network scenario will be discussed further. * 15 kHz SCS for NR is prioritized. 30 kHz SCS scenario will be discussed further. * Study and if necessary, define network assistance signaling and UE capability signaling.   However, wording from LS is also fine for us.  The wording on network assistance can be updated based on conclusions on Issue #2. |
| Nokia, Nokia Shanghai Bell | In view of the RAN4 workload and timeframe of Rel-17, we do not consider it necessary to discuss further the CRS-IC receiver in Rel-17. It makes sense to use the LLR weighting receiver as the baseline reference receiver in Rel-17.  In view of the Rel-17 schedule, we should also limit the work to the synchronous network scenario only.  Otherwise, we are fine with the RAN4 recommendations shown above. It is OK to discuss the need for UE capability signalling in a later phase. |
| Vodafone | We are fine with the recommendation. |
| BT | We are fine to proceed with the recommendations captured above |
| KDDI | We are fine with the above RAN4 recommendation. |

**Issue #2:** Whether to assume network assistance information for PDSCH CRS-IM?

* Option 1: Yes (Apple, MediaTek)
* Option 2: No (Nokia - for Rel-17)
* Option 3: Task RAN4 to further discuss the necessity of network assistance signaling during requirements definition phase. (Intel, China Telecom)

|  |  |
| --- | --- |
| Company | Comment |
| Huawei | Option 2.  From RAN4 discussion, companies have common understanding that it is feasible for UE to acquire the related CRS configuration information by blind detection and PBCH decoding. Also to speed up the feature application in the real network as early as possible and avoid network and UE upgrade to support any additional signalling, it is more valuable not to introduce any network assistance signalling. |
| OPPO | Prefer option 1.  Considering UE complexity and realistic network deployment, we support to include network assistance information, along with other signalling/capabilities for Rel-17 UEs. We do not see that much of overhead. Besides, since this NW assistance will only be supported by Rel-17 UEs, there still exists enough time period for BSs to implement this before Rel-17 UEs will be launched in the market. |
| MTK | Support Option 1  UE complexity needs to be considered. As we mentioned during GTW, UE complexity cannot be seen from the throughput simulation results. The observation of similar UE performance between with and without assistance information should not be used as an argument to preclude network assistance information.  We also want to take this chance to discuss a bit about the definition of network assistance information. In our view, it is impossible for UE to do CRS-IM if network does not provide any piece of information (not even provide the LTE MO for UE to do cell search). Without MO, UE has no idea about the LTE center frequency and will need to blindly scan all possible LTE PSS/SSS frequency locations. The process is time-consuming, and the complexity is huge. With this understanding, we believe that the network assistance information is anyway needed. The discussion point is only about its content. |
| ZTE | We support Option 2.  RAN4 has confirmed that LLR weighting without network assistance can achieve better performance, thus for the time being RAN4 can focus on specifying enhanced PDSCH demodulation requirements based on LLR weighting receiver without network assistance for synchronous scenarios with 15kSCS. After that, RAN4 can work with asynchronous cases and other SCSs. In such a way, the performance improvement demands can be satisfied under the current stage.  Further potential optimization with network assistance can be deferred to a later stage. |
| Apple | We support option 1.  We would like to understand why it would be difficult for network to implement this assistance information in Rel-17, while UEs are expected to implement CRS-IM. The time frame this will be deployed would be when Rel-17 UEs and gNBs are available. To speed up the feature application in real network, rate matching schemes can be used without additional impact to UE processing.  RAN4 has not confirmed that LLR weighting without network assistance can achieve better performance.  During the GTW discussion, companies expressed their views that LLR weighting doesn’t need network assistance and that NR UE can get all the information from inter-RAT measurements. Firstly, we would like to understand if UE would always be configured with inter-RAT measurements for the LTE cells with overlapping NR spectrum. For inter-RAT measurements, the UE doesn’t need to do PBCH/MIB decoding which is necessary to know number of CRS ports and bandwidth for CRS-IM. Also, additional information like MBSFN subframe configuration, CRS muting information are not known unless this information is provided. In case UE is supposed to do CRS-IM on cell(s) other than those configured for inter-RAT measurements, there is an additional level of complexity as pointed out by MTK above and also in our paper RP-211950.  Also, there is no way to assess the the UE processing or complexity and just comparing simulation results with and without network assistance doesn’t sufficiently reflect the additional UE complexity involved without network assistance.  Given the above, we think it is necessary to have network assistance for CRS-IM and the content of such assistance information should be further discussed. |
| China Telecom | Option 2 or Option 3.  As several companies commented on Monday GTW, the network signalling aspect can be discussed separately for the two implementations of CRS-IM, i.e., LLR weighting and CRS-IC.  1) For LLR weighting  Only the power level of interference CRS needs to be estimated and UE can estimate the power of all REs in the OFDM symbols containing CRS, assuming the same number of CRS ports in the serving and neighbouring cells. So, CRS location is not needed to be signalled. For the presence of the CRS interference, it can be known by the ON/OFF of serving cell CRS-RM in DSS scenario.  If needed, we are also fine to limit the requirements to the typical scenarios, e.g., without CRS muting (i.e., network based CRS interference mitigation), and aligned MBSFN configuration among the serving and neighbouring cells, instead of considering all the scenarios supported in the specs but not used in the network.  2) For CRS-IC  For CRS-IC, in order to obtain the CRS sequence, UE may need to perform inter-RAT neighbouring cell detection and PBCH reading. The feasibility can be discussed separately.  In summary, we suggest:  1) Discuss the network signalling for LLR weighting and CRS-IC separately  2) Further align which parameters are needed to be known at UE for LLR weighting and CRS-IC respectively  3) Then discuss whether these parameters can be obtained by any means at UE |
| Samsung | We support option 3.  RAN shall respect WG decision on the recommendations including both baseline as well as further study on network assistance signalling as a package. RAN do not need to re-confirmed the baseline receiver and further discuss the network signalling necessity for baseline receiver and other receiver type which has been well/extensive discussed in RAN4. We do not need to repeat the discussions in RAN.  We suggest to follow what RAN4 recommended in the next quarter discussions. |
| Qualcomm | We support Option 1. Even though implementation of the feature without assistance data is feasible, there will be a clear increase in complexity(and consequently power consumption). The UE will have to do inter-RAT measurements and decoding of PBCH with the NR modem. Also, there will be a performance degradation because because of errors associated with detection and PBCH decoding of neighbor cells. Also, it is possible that PBCH decoding is not possible at certain levels (PBCH will always be colliding) even though interference mitigation could provide performance gains. Nokia’s proposal to consider assistance information in the future does not make much sense since Rel.17 UEs will carry the burden of additional complexity anyway.  Option 3 implies that RAN4 will have further discussion which will likely take a long time. performance evaluation without assistance data will be difficult and cumbersome because it will imply making certain assumptions about whether a cell is detectable or not, after how much delay, etc.  Irrespective of what the decision will be, there will be a loss in performance in the field if assistance data is not provided to UEs. |
| CMCC | Option 2 for LLR weighting and Option 3 for CRS-IC.  Firstly, based on the simulation results from companies, when using CRS-IM without network assistance, the performance gain can be achieved.  Secondly, only the power level of interference CRS needs to be estimated for LLR weighting, UE does not need to know the CRS location or sequence to do the mitigation. It is feasible for UE to do the blind detection without too much complexity. And the presence of interference can also be obtained from existing signalling, e.g. CRS-RM, 7.5KHz shift, inter-RAT MO configuration…  Considering of the companies’ concerns about processing timeline and UE complexity for CRS-IC receiver, we are open to further discuss the necessity of network assistance signaling during requirements definition phase. |
| Ericsson | We support option 2. We are fine to base the requirements on LLR weighting to reduce the complexity burden on the UE. Lack of a need for network signalling will widen the scenarios in which there is a benefit form the feature. Considering that CRS-IM is useful when the UE is in connected mode and receiving data anyhow, we would like to understand just how much incremental UE complexity detecting the co-channel neighbour PBCH is in these circumstances. |
| Intel | Support Option 3, which is aligned with RAN4 WG recommendation.  Same time, we see clearly two camps supporting and not supporting definition of network assistance and an alternative option, which can be further discussed in RAN4, is to define two sets of requirements for the cases with and without network assistance.  As for separate discussion on network assistance signalling for different CRS-IM receivers. Based on our understanding, same information is required for CRS-IC and LLR weighting receivers and UE needs information on CRS REs positions for both types of receivers. |
| Nokia, Nokia Shanghai Bell | Option 2. Especially with LLR-weighting receiver, there is no need for NWA. We agree with the comments from Huawei. Furthermore, it would be too late in Rel-17 to start debating the network assistance. |
| Vodafone | We prefer option 2 but can consider option 3. It seems the complexity of LLR without network assistance is manageable and this would speed up the feature application within the network as per Huawei’s comments. |
| BT | Option 2  As a result of the study, we consider it is a good compromise select LLR weighting over CRS-IC based on performance vs complexity.  LLR weighting without network assistance is the best compromise between time to market and complexity.  We are facing the end of Rel-17 and WGs are still overloaded. The introduction of network assistance will impact several WGs and due to the severity of the problem observed in real networks by different operators, it is not possible to wait until Rel-18. In addition, with network signalling, more elements of the networks need to implement the solution and the IOT/IODT will require extra time.  It is accepted that without network assistance, the UE complexity will increase but as many other things in 3GPP, the fact that PDSCH CRS-IM works without network assistance will be a good differentiator among vendors. In that sense, this is business as usual. More complexity does not mean it is broken or it will not work. Once the problem is solved, we are open to further enhancements if required.  Therefore, by adding network assistance, we are putting in severe risk the completion of the work in Rel-17 and therefore NR SA will be delayed in countries where refarming is not an option. |
| KDDI | Option2  Nokia’s proposal makes sense considering the current WGs situation. We are reluctant to impose additional work on RAN4 and other WGs to develop the network assistance feature within Rel-17 time frame. We think that we should identify advantages and disadvantages of having the enhancement for network assistance in next Rel-18. |

## Initial round summary

**Issue #1**: Phase II objective (excepting the network assistance signalling part)

Except the network assistance signalling part (which is discussed separately in Issue #2), any comments on the other parts of RAN4 recommendations in LS RP-212490?

*RAN4 recommends to define NR PDSCH demodulation requirements for neighbouring cell LTE CRS-IM in scenarios with overlapping spectrum for LTE and NR in Rel-17:*

*• Use LLR weighting as baseline reference receiver, and further discuss the feasibility of CRS-IC receiver taking into account the UE complexity and PDSCH processing time.*

*• Synchronous network scenario is prioritized. The asynchronous network scenario will be discussed after RAN #93e meeting.*

*• 15 kHz SCS for NR is prioritized. The 30 kHz SCS scenario will be discussed after RAN #93e meeting.*

*• RAN4 will further discuss the necessity of ~~network assistance signaling and~~ UE capability signaling during requirements definition phase.*

**Summary of initial round discussion:**

1. All companies support to proceed with the above recommendations, with additional clarification on the network signalling part: if further agreements for Issue #2 can be reached, the signalling part can be updated accordingly; otherwise the original RAN4 recommendation will be added back.
2. Majority companies agree to keep the RAN4 recommendation without any additional update, while there are also some suggestions on the deprioritized scenarios or FFS part in order to reduce the RAN4 workload:

* One company (QC) suggests to discuss the deprioritized scenarios (asynchronous network, 30 kHz SCS) after the requirements for the baseline scenario (synchronous network and 15 kHz SCS) are finalized.
* One company (Nokia) suggests to only focus on synchronous network scenario.
* Two companies (E///, Nokia) suggest to only focus on LLR weighting.

**Issue #2:** Whether to assume network assistance information for PDSCH CRS-IM?

**Summary of initial round discussion:**

* Option 1: Yes (Apple, MediaTek, OPPO, QC)
* Option 2: No (Nokia, HW, ZTE, China Telecom, CMCC for LLR weighting, E///, VDF, BT, KDDI)
* Option 3: Task RAN4 to further discuss the necessity of network assistance signaling during requirements definition phase (Intel, China Telecom, Samsung, CMCC for CRS-IC, Intel, VDF)
* Option 4 (NEW): Define two sets of requirements for the cases with and without network assistance. (Intel)

The need of network signalling has been debated repeatedly, and companies’ positions are not changed since RAN #91e. For the intermediate round, it might be helpful to first align the understanding on:

* 1) Which parameters are needed to be known for LLR and CRS-IC respectively?
* 2) How could UE obtain the information if not signalled by the network?
* 3) Deadline to make the decision on the need of network signalling

# Intermediate round

## Open issues and companies views’ collection

**Issue #1**: Phase II objective (excepting the network assistance signalling part)

*RAN4 recommends to define NR PDSCH demodulation requirements for neighbouring cell LTE CRS-IM in scenarios with overlapping spectrum for LTE and NR in Rel-17:*

*• Use LLR weighting as baseline reference receiver, and further discuss the feasibility of CRS-IC receiver taking into account the UE complexity and PDSCH processing time.*

*• Synchronous network scenario is prioritized. The asynchronous network scenario will be discussed after RAN #93e meeting.*

*• 15 kHz SCS for NR is prioritized. The 30 kHz SCS scenario will be discussed after RAN #93e meeting.*

*• RAN4 will further discuss the necessity of ~~network assistance signaling and~~ UE capability signaling during requirements definition phase.*

*Note: if further agreements for Issue #2 can be reached, the signalling part can be updated accordingly; otherwise the original RAN4 recommendation will be added back.*

**On top of the RAN4 recommendation, if any of the following additional updates are acceptable?**

* 1) Discuss the deprioritized scenarios (asynchronous network, 30 kHz SCS) after the requirements for the baseline scenario (synchronous network and 15 kHz SCS) are finalized.
* 2) Only focus on synchronous network scenario.
* 3) Only focus on LLR weighting.

|  |  |
| --- | --- |
| Company | Comment |
| Intel | 1. We think it is rather reasonable to focus on scenario with synchronous network and 15 kHz SCS to balance the workload. Performance benefits and feasibility of CRS-IM processing is already analysed and confirmed for this scenario. The proposed prioritization (i.e., handle asynchronous network and 30 kHz SCS scenarios after completion of work on 15kHz SCS) is acceptable for us. 2. Based our understanding, CRS-IM for async case may require multi-FFT processing and leads to complicated Rx processing. Therefore, we think that only sync case should be considered for requirements definition. Taking into account that we didn’t have a detailed discussion on CRS-IM for async case in RAN4, we are fine to keep it for further discussion. 3. We prefer to keep both receiver candidates open since CRS-IC provides better performance comparing to LLR weighting (based on results from TR 38.833). Also, CRS-IC is the baseline CRS-IM method for LTE UE. |
| Nokia, Nokia Shanghai Bell | It is very important to manage the workload in RAN4. Therefore we should focus on the synchronous network scenario and on only LLR-weighting receivers. |
| Qualcomm | We agree with the additional updates to better focus the work. |
| Apple | 1. Given the remaining time, it would be good to focus on defining requirements for synchronous and 15KHz SCS scenario and discuss deprioritized scenarios later. 2. Asynchronous (and also 30KHz SCS) requires multiple FFT for CRS-IM which would further impact UE processing and complexity. We support to focus only on synchronous network. 3. We support to only focus on LLR weighting as it is less complex than CRS-IC for interference mitigation. |
|  | 1. OK to start from 15KHz first. 2. OK to only focus on sync network. The complexity for CRS-IC is too high for asynchronous case, because UE has to go back to time domain for cancellation. Whether LLR weighting can work is still unclear.   OK to focus on LLR weighting only |
| OPPO | Agree with all 3 additional updates. Also, OK to focus on sync network and LLR weighting only. |
| Samsung | For both initial round and intermediate round discussion, unfortunately, we are just repeating the discussions in RAN4. The recommendation agreed in RAN4 is the best we can do. We do not see big difference if discussion happened in RAN4 and RAN. Overall, in our understanding, RAN4 can continue the discussion based on recommendation agreed in last RAN4 meeting without any further RAN guideline. |
| CMCC | 1. Discuss the deprioritized scenarios (asynchronous network, 30 kHz SCS) after the requirements for the baseline scenario (synchronous network and 15 kHz SCS) are finalized.   From CMCC perspective, we have 160MHz spectrum in total in 2.6GHz (n41 and b41). Both NR and LTE deployed and shared the 160MHz spectrum. We already observed the interference caused by LTE CRS in our network. This is a practical scenario that needs to be resolved. Considering the workload, we are fine to prioritize 15KHz SCS. However, we should have clear understanding on when to start the 30KHz since this is the very critical scenario for us. In previous RAN4 discussion, we had the agreement that 30KHz discussion will start after RAN#93. How the bullet said “after the requirements for the baseline scenario are finalized”. What is the meaning of “finalized”? Does it mean the final CRs been approved? And what if we had no time to discuss 30KHz in Rel-17 if the finalization is too late? We cannot accept to preclude 30KHz in Rel-17 WI considering the importance of this scenario to us.  So if companies still have concern to start 30KHz discussion after RAN#93, we can make further compromise:   * 1) Discuss the 30KHz scenarios after RAN#94.  1. Only focus on synchronous network scenario.   We are OK to focus on synchronous network scenario.  3) Only focus on LLR weighting.  The feasibility of CRS-IC is still under discussion in RAN4. We prefer to continue the discussion in RAN4. |
| China Telecom | On whether to ‘*Only focus on LLR weighting*’:  According to the companies’ simulation results as summarized in the LS, both CRS-IC and LLR weighting receivers can achieve good performance gain compared with the reference scheme, and CRS-IC can provide larger performance gain compared with LLR weighting, so we prefer not to exclude any of the 2 candidate receivers.  At the same time, if consensus can be reached on Issue#2 below that LLR weighting does not need NW assistance signalling and CRS-IC may need NW assistance signalling, we can give our compromise to only focus on LLR weighting without considering NW assistance signalling. |
| ZTE | P1 can be revisited after 2) and 3) are completed. At this stage, it is better to focus on 2) and 3). |
| Ericsson | In our view, the work can be focussed to LLR weighting only and 15kHz SCS, as we do not see that CRS-IC provides a significant incremental gain.  Asynchronous operation is complex for CRS-IC, but may be more straightforward for LLR weighting. Asynchronous operation will extend the range of scenarios in which the CRS-IM/LLR weighting can be applied, since it will also then provide gain for non-synchronized FDD scenarios. Considering that the use case is DSS and that LTE will be more prevalent in the near time frame, it would be useful to enable asynchronous operation earlier rather than later. Therefore, we would prefer to keep asynchronous operation based on LLR weighting in as a second priority (addressed if workload permits). |
| Huawei | 1) It is reasonable to start with 15kHz SCS first,  2) Agree to focus on synchronous network scenario  3) Focus on LLR weighting is enough. Lots of estimations on CRS-RM, LLR weighting and CRS-IC were conducted in last RAN4#100-e, considering the achieved performance and complexity balance, the performance achieved by LLR weighting is enough to cope with the LTE interference to NR, also LLR weighting is acceptable for all companies. |
| KDDI | 1. We are fine with starting from 15KHz, after that move on to 30KHz. 2. We are fine with only focusing on synchronous network. 3. We prefer to continue the RAN4 discussion, the same view CMCC |
| Vodafone | 1) Agree to initially focus on establishing requirements for 15 kHz synchronous as baseline scenario given workload and available time. Not opposed to discussing deprioritized scenarios (30 kHz, async) following this.  2) Agree to only focus on synchronous network scenario.  3) In line with China Telecom’s comments, we are ok with LLR as a baseline but we would prefer not to exclude CRS-IC considering the larger performance gain it could offer. As LLR already provides a complexity reduction over CRS-IC for the handset, it would seem reasonable to focus on LLR operation without network assistance. |
| BT | We are ok with proposals 1) and 2). Focus the work in SCS 15 kHz and synchronous network scenarios.  About point 3) Only focus on LLR weighting, we slightly prefer to allow RAN4 to continue its work with CRS-IC. |

**Issue #2:** Whether to assume network assistance information for PDSCH CRS-IM?

Further discuss the 3 points below:

* 1) Which parameters are needed to be known for LLR and CRS-IC respectively?
  + For LLR weighting:
    - Option 1: presence and location of interference CRS
    - Option 2: presence of interference CRS
  + For CRS-IC:
    - Option 1: presence, location and sequence of interference CRS
  + Note: the presence information includes the presence of LTE cell, MBSFN configuration, CRS muting information, and the CRS location information includes LTE carrier frequency, bandwidth, v-shift, CRS port number.
* 2) How could UE obtain the information if not signalled by the network?
  + For LLR weighting:
    - Option 1: By inter-RAT measurement and PBCH decoding
    - Option 2: By the configuration of serving cell CRS-RM, 7.5KHz shift, inter-RAT MO
  + For CRS-IC:
    - Option 1: By inter-RAT measurement and PBCH decoding
* 3) Deadline to make the decision on the need of network signalling

|  |  |
| --- | --- |
| Company | Comment |
| Intel | 1. Based on our understanding, the set of information required for LLR weighting and CRS-IC receivers is same (i.e., presence, location and sequence of interference CRS). We assume that UE needs to know CRS sequence, number of CRS APs, CRS shift, MBSFN pattern, and CRS bandwidth.   For LLR weighting receiver we assume that UE needs to estimate the power of CRS interference and one of the ways is to make it based on channel estimation for which CRS sequence is required.   1. Based on our understanding, for most parameters inter-RAT measurement and PBCH decoding should be sufficient except MBSFN configuration and CRS muting information. The latter information can be obtained via SIB reading or via CRS presence detection. 2. Taking into account that Rel-17 ASN.1 freeze is in June 2022, we think that the final deadline to define the signalling and provide information to RAN2 should be February 2022. The decision on whether signalling should be introduced needs to be made in November 2021 or January 2022 RAN4 meetings.   In addition, we prefer to handle the discussion on specific required information and how UE can obtain it in RAN4. RAN can task RAN4 to identify required information for different reference receivers. |
| Nokia, Nokia Shanghai Bell | 1) No parameters are strictly needed for either LLR-weighting or CRS-IC, though the impact of not having signalling might be greater with a CRS-IC receiver.  2) The UE can obtain what is needed by blind detection. As already mentioned by other companies, the timing and MBSFN subframe configuration could be inferred from the serving cell, leaving only the v-shift and number of CRS ports to be detected, which should be straightforward.  (As a compromise, if any signalling were to be provided, it should be confined to reusing the Rel-15/16 semi-static signalling of LTE CRS RM patterns that can be used inform the UE of the locations of the CRS REs.)  3) The decision should be made at RAN#93e. |
| Qualcomm | 1) Our understanding is that the same information is needed for LLR weighting or CRS-IC. Knowing the actual sequence could be useful for LLR weighting as well.  2) Option 1 for both.  3) we would prefer to make a decision as soon as possible or at least have a clear criteria for making a decision(if the decision is left to RAN4, how to evaluate the impact).  Infra vendors have not explained why is it so difficult to provide the assistance information. This entire work was triggered by the need to improve the performance with DSS. In order to maximize the gains in the field, assistance information is clearly useful so everyone should do their part and contribute to the possible improvements. |
| Apple | 1. For both CRS-IC and LLR weighting the same set of LTE parameters are needed for interference mitigation: LTE cell ID, number of CRS ports, LTE center frequency, CBW, MBSFN configuration. For both presence CRS-IC and LLR weighting presence, location and sequence of interference CRS information is needed. 2. In case no information on LTE interferer is available to the UE, the UE would need to rely on LTE inter-RAT measurement and would only be aware of the frequency layers configured in the LTE-MO. Also, inter-RAT measurements are restricted to measurement gaps and might be limited to single CRS port measurements. For additional information on CRS ports and LTE BW PBCH decoding is needed. For information on MBSFN configuration SIB decoding is needed. If LTE-MO is not configured, then it is very complex since a frequency scan is needed to detect LTE center frequency first. For DSS scenario even if the same configuration as serving cell is assumed for number of CRS ports, BW and center frequency and MBSFN c config, cell detection is still needed for LTE interferer to obtain the cell ID. In scenario 2 there is no such LTE serving cell information. 3. There is a necessity for network assistance as already expressed by UE vendors and propose not to continue the discussion on whether NWA is necessary or not, otherwise we would continue to hear the same arguments. We propose to start the work in RAN4 for demod requirements for CRS-IM with the assumption of network assistance information and discuss the details of what NWA information is included as part of RAN4 work. We would also like to understand why providing NWA is not feasible for R17 when UEs are expected to implement CRS-IM. If UEs don’t support this feature due to additional complexity with no NWA, then there would be no benefit in the end. |
| MTK | 1. Similar view as QC and Intel, same information is needed for LLR weighting and CRS-IC receivers, e.g., CRS sequence, CRS AP #, v\_shift, MBSFN pattern, and CRS bandwidth, center frequency, muting pattern. In our view, even for LLR weighting, UE still need to do a rough assessment on how strong the interference is in order to better determine the weighting coefficient. 2. As we mentioned in initial round, UE still need the measurement object configuration in order to do inter-RAT measurement. Otherwise, UE need to do blind scan on all possible frequency location for LTE PSS/SSS. Furthermore, measurement gap should be configured according to current RRM spec. 3. The deadline is the same as the ASN.1 frozen. Early decision is welcomed of course. We have similar question to network vendor on the difficulty to provide assistance information. |
| OPPO | 1. Presence, location and sequence of interference CRS are needed for both CRS-IC and LLR weighting. Agree that the same information is required. 2. Agree with MTK that UE can rely on LTE inter-RAT measurements and obtain the information of frequency layers configured in the LTE-MOs. Otherwise, blind detection on all possible LTE cells could be quite difficult and complex for UE. 3. Early decision before ASN.1 frozen is fine. Also share the similar concern why providing network assistance information is not feasible for R17 when UEs are expected to implement CRS-IM. |
| Samsung | Our view is to respect RAN4 recommendations to continue discussions on network assistance signalling even for LLR weighting baseline receiver. |
| CMCC | For Q1, the questions is that which information is needed for LLR and CRS-IC respectively, not strictly related to NWA. From our understanding, LLR weighting may needs to know the presence of interference CRS (option 2), CRS-IC needs to know the presence, location and sequence (option 1).  For Q2, we think all the options of existing information are feasible for UE to obtain the information. And UE can also obtain the information that needed by blind detection.  For Q3, if it is possible, we prefer to make decision in this RAN plenary meeting. However, based on the comment so far, we think it might be more practical to continue to discuss the NWA in RAN4. |
| China Telecom | 1. On which parameters are needed to be known for LLR and CRS-IC respectively   For LLR weighting, we think only the presence of neighbour LTE (Option 2) will be enough for the UE to do CRS-IM. Based on our simulation, with LLR weighting the UE only needs to estimate the interference CRS power, which is quite similar as the estimation of noise power.  For CRS-IC, UE may additionally need the exact interference CRS sequence to do the interference cancellation.  Same time, from practical NW configuration perspective, UE can assume that no CRS muting is configured and MBSFN configuration is aligned among the cells, which we think is the most common configuration in the real NW.   1. How could UE obtain the information if not signalled by the network?   For LLR weighting, UE would know the presence of interference LTE cell by the configuration of serving cell CRS-RM for DSS scenarios, i.e., option 2 will be enough for LLR weighting.  For CRS-IC, since UE may need to know the exact neighbour LTE CRS sequence, neighbour cell PCI, slot & symbol index, neighbour CBW may be necessary. So, we think option 1 may be needed for CRS-IC. |
| ZTE | 1. The question here seems a bit vague, what can be regarded as “known”? Can it be obtained via estimation, or notified/configured without need of estimation? In our view, this is completely up to UE implementation. For example, for LLR weighting, it can be done if there is only information on interfering CRS presence, but it also can be done if there is information on both presence and location of the interfering CRS. 2. As comments on 1), can be obtained with or without the need of estimation. 3. Since the current focus is on LLR weighting without network assistance, we are fine to continue discussion in RAN4 in a later stage. |
| Ericsson | 1 and 2: For CRS-IC, the indicated presence and location information needs to be known by the UE and if not provided by the network would need to be obtained by means of either reading the PBCH or inter-RAT mobility information if provided. As commented earlier, since CRS-IM is relevant when the UE is connected and receiving data, it is not obvious why additionally reading neighbour cell PBCH is a huge incremental complexity though.  For LLR weighting, the UE needs to know the locations in the RE grid of the LTE CRS (and that they are present). Of course, this information could be obtained by the same means as described for CRS-IC. On the other hand, the UE could infer DSS presence from configuration with serving cell RM pattern etc. (i.e. option 2), could use serving cell quality to determine whether it is in a position for which LLR weighting could give gain (see 38.304 5.2.4.9.2) and could use RE level power estimation to identify CRS positions. |
| Huawei | 1) We do not think that the same information is needed for LLR weighting and CRS-IC. At least sequence of interference CRS is not mandatory for LLR weighting to achieve better performance.  2) As discussed in the initial round, all companies agreed that it is feasible and manageable for UE to acquire the related necessary information for both LLR weighting and CRS-IC by blind detection and PBCH decoding even if no any additional information is provided, the key issue is the complexity as argued by proponent of the network assistant signalling, but it is still manageable. By using of the configuration of serving CRS-RM, 7.5 kHz shift and inter-RAT MO as listed in Option 2, it is more convenient for UE to do the LLR weighing. Also like many operators said in the initial round, it is very necessary to speed up the application in the real network due to the severity of the problem observed in real networks by different operators. The additional upgrade of the introduction of network assistance will also affect other WGs and real IOT/IODT testing, all these will seriously delay the application in the real network.  3) It is better to make decision in this RAN plenary meeting, but also fine to continue the discussion in the following RAN4 meetings if still no consensus can be reached. |
| KDDI | If we continue to discuss the details of network assistance information, then it should be discussed in RAN4 rather than RAN plenary, so that more RAN4 experts can join the discussion. |
|  |  |
|  |  |

## Intermediate round summary

**Issue #1**: Phase II objective (excepting the network assistance signalling part)

*RAN4 recommends to define NR PDSCH demodulation requirements for neighbouring cell LTE CRS-IM in scenarios with overlapping spectrum for LTE and NR in Rel-17:*

*• Use LLR weighting as baseline reference receiver, and further discuss the feasibility of CRS-IC receiver taking into account the UE complexity and PDSCH processing time.*

*• Synchronous network scenario is prioritized. The asynchronous network scenario will be discussed after RAN #93e meeting.*

*• 15 kHz SCS for NR is prioritized. The 30 kHz SCS scenario will be discussed after RAN #93e meeting.*

*• RAN4 will further discuss the necessity of ~~network assistance signaling and~~ UE capability signaling during requirements definition phase.*

*Note: if further agreements for Issue #2 can be reached, the signalling part can be updated accordingly; otherwise the original RAN4 recommendation will be added back.*

Summary of initial round discussion:

1. All companies support to proceed with the above recommendations, with additional clarification on the network signalling part: if further agreements for Issue #2 can be reached, the signalling part can be updated accordingly; otherwise the original RAN4 recommendation will be added back.
2. Majority companies agree to keep the RAN4 recommendation without any additional update, while there are also some suggestions on the deprioritized scenarios or FFS part in order to reduce the RAN4 workload:

* One company (QC) suggests to discuss the deprioritized scenarios (asynchronous network, 30 kHz SCS) after the requirements for the baseline scenario (synchronous network and 15 kHz SCS) are finalized.
* One company (Nokia) suggests to only focus on synchronous network scenario.
* Two companies (E///, Nokia) suggest to only focus on LLR weighting.

Summary of intermediate round discussion:

On top of the RAN4 recommendation, any further down-prioritization is acceptable?

* For asynchronous network scenario:
  + - Option 1: Keep the recommendation in RAN4 LS (Samsung, E///)
    - Option 2: Discuss after the requirements for the baseline scenario (synchronous network and 15 kHz SCS) are finalized. (Intel, QC)
    - Option 3: Only focus on synchronous network scenario. (Nokia, QC, Apple, MTK, OPPO, CMCC, ZTE, HW, KDDI, BT, Vodafone)
* For NR 30kHz SCS scenario:
  + - Option 1: Keep the recommendation in RAN4 LS (Samsung)
    - Option 2: Discuss after the requirements for the baseline scenario (synchronous network and 15 kHz SCS) are finalized. (Intel, QC, Apple, MTK, OPPO, E///, HW, KDDI, BT)
    - Option 3: Discuss the 30KHz scenario later than 15kHz, e.g., after RAN #94 (CMCC, Vodafone)
* For Reference receiver:
  + - Option 1: Keep the recommendation in RAN4 LS (Intel, Samsung, CMCC, China Telecom, KDDI, Vodafone, BT)
    - Option 2: Only focus on LLR weighting (Nokia, QC, Apple, MTK, OPPO, China Telecom - if no network signalling, ZTE, E///, HW, Vodafone - if no network signaling)

Moderator’s observation:

For asynchronous network and 30 kHz SCS scenarios, there is no consensus on whether to do further down-prioritization on top of the RAN4 recommendation. Meanwhile, considering the RAN4 workload, it is proposed to start the discussion later than the prioritized scenario, i.e., start after RAN #94e.

For the reference receiver, further down-scoping is not agreeable, and it is proposed to keep the RAN4 recommendation.

**Moderator’s proposal:**

**Proposal 1:** Add the following phase II objective in Rel-17 WID on “Further enhancement on NR demodulation performance”:

*Define NR PDSCH demodulation requirements for neighbouring cell LTE CRS-IM in scenarios with overlapping spectrum for LTE and NR:*

*• Use LLR weighting as baseline reference receiver, and further discuss the feasibility of CRS-IC receiver taking into account the UE complexity and PDSCH processing time.*

*• Synchronous network scenario is prioritized. The asynchronous network scenario will be discussed after RAN #94e meeting.*

*• 15 kHz SCS for NR is prioritized. The 30 kHz SCS scenario will be discussed after RAN #94e meeting.*

*• RAN4 will further discuss the necessity of ~~network assistance signaling and~~ UE capability signaling during requirements definition phase.*

*Note: if further agreements for Issue #2 can be reached, the signalling part can be updated accordingly; otherwise the original RAN4 recommendation will be added back.*

**Issue #2:** Whether to assume network assistance information for PDSCH CRS-IM?

Summary of initial round discussion:

* Option 1: Yes (Apple, MediaTek, OPPO, QC)
* Option 2: No (Nokia, HW, ZTE, China Telecom, CMCC for LLR weighting, E///, VDF, BT, KDDI)
* Option 3: Task RAN4 to further discuss the necessity of network assistance signaling during requirements definition phase (Intel, China Telecom, Samsung, CMCC for CRS-IC, Intel, VDF)
* Option 4 (NEW): Define two sets of requirements for the cases with and without network assistance. (Intel)

The need of network signalling has been debated repeatedly, and companies’ positions are not changed since RAN #91e.

Summary of intermediate round discussion:

For the intermediate round, further discuss the 3 points:

* 1) Which parameters are needed ~~to be known~~ for LLR and CRS-IC respectively?
  + For LLR weighting:
    - Option 1: presence and location of interference CRS (HW, E///)
    - Option 2: presence of interference CRS (CMCC, China Telecom, ZTE, HW)
    - Option 3: presence, location and sequence of interference CRS (Intel, QC, Apple, OPPO, MTK)
  + For CRS-IC:
    - Option 1: presence, location and sequence of interference CRS (Intel, QC, Apple, OPPO, CMCC, China Telecom, HW, MTK)
  + Note: the presence information includes the presence of LTE cell, MBSFN configuration, CRS muting information, and the CRS location information includes LTE carrier frequency, bandwidth, v-shift, CRS port number.
* 2) How could UE obtain the information if not signalled by the network?
  + For LLR weighting:
    - Option 1: By inter-RAT measurement and PBCH decoding (Intel, QC, Apple, MTK, OPPO)
    - Option 2: By the configuration of serving cell CRS-RM, 7.5KHz shift, [inter-RAT MO] (i.e., no need to do inter-RAT measurement and PBCH decoding) (Nokia, CMCC, China Telecom, HW, E///)
      * Note: proponents of option 2 think option 1 is also feasible to obtain the related information
  + For CRS-IC:
    - Option 1: By inter-RAT measurement and PBCH decoding (Intel, QC, Apple, MTK, OPPO, CMCC, China Telecom, HW)
* 3) Deadline to make the decision on the need of network signalling
  + Option 1: RAN #93e (Nokia, QC, Apple, HW)
  + Option 2: Continue discussion in RAN4, and make decision in Q4 2021 or Q1 2022 RAN4 meeting considering the ASN.1 frozen time (Intel, OPPO, CMCC, ZTE, Samsung, KDDI, QC, HW, MTK)

Moderator’s observation:

For LLR weighting, companies have different views on which parameters are needed, e.g., whether interference CRS sequence related information is needed for the purpose of estimating interference CRS power. Consequently, different views are shown on how to obtain the information at UE if not signalled by the network.

For CRS-IC, all companies agree that the presence, location and sequence of interference CRS are needed for UE by either blind detection or network signalling. These information can be obtained by inter-RAT measurement and PBCH decoding if not signalled by the network, but companies have different views on whether it is doable by UE considering the UE complexity.

There are also comments from UE & chipset side on why is it so difficult for infra vendors to provide the assistance information.

On the deadline to conclude the need of network signalling, some companies hope to make decision as soon as possible, meanwhile several companies commented that there are still some technical details to be further discussed at WG level.

**Moderator’s proposal:**

**Proposal 2:** Task RAN4 to further discuss the necessity of network assistance signalling in Phase II.

# Final round

## Open issues and companies views’ collection

**Issue #1**: Phase II objective (excepting the network assistance signalling part)

**Proposal 1 (after intermediate round):** Add the following phase II objective in Rel-17 WID on “Further enhancement on NR demodulation performance”:

*Define NR PDSCH demodulation requirements for neighbouring cell LTE CRS-IM in scenarios with overlapping spectrum for LTE and NR:*

*• Use LLR weighting as baseline reference receiver, and further discuss the feasibility of CRS-IC receiver taking into account the UE complexity and PDSCH processing time.*

*• Synchronous network scenario is prioritized. The asynchronous network scenario will be discussed after RAN #94e meeting.*

*• 15 kHz SCS for NR is prioritized. The 30 kHz SCS scenario will be discussed after RAN #94e meeting.*

*• RAN4 will further discuss the necessity of ~~network assistance signaling and~~ UE capability signaling during requirements definition phase.*

*Note: if further agreements for Issue #2 can be reached, the signalling part can be updated accordingly; otherwise the original RAN4 recommendation will be added back.*

**Continue discussion on Proposal 1:**

* Is it agreeable to exclude asynchronous network scenario?

|  |  |
| --- | --- |
| Company | Comment |
| Nokia, Nokia Shanghai Bell | We support excluding the asynchronous network scenario, in order to reduce the workload in RAN4.  We also believe it is not necessary to further discuss the feasibility of CRS-IC receivers. We therefore propose to modify the first bullet as follows: *Use LLR weighting as baseline reference receiver~~, and further discuss the feasibility of CRS-IC receiver taking into account the UE complexity and PDSCH processing time~~.* |
| Apple | Yes, we support to exclude async scenario.  We would like to understand why network assistance signalling part is struck out when we have Proposal 2 below. We should add a separate bullet in the WID based on Proposal #2. |
| MTK | We support to exclude the async scenario (and also 30KHz) from the WID.  We are also fine to remove CRS-IC receiver in the WID as long as we already have a baseline which is LLR weighting. |
| Qualcomm | We support to exclude async scenario. At least on this part it seems there is consensus 😊 |
| OPPO | We support to exclude the async scenario. For the last bullet, we prefer to keep the original RAN4 recommendation as stated in LS. |
| Ericsson | We would prefer to consider further the potential for applying LLR weighting to the async scenario, however since we are alone in this view, we can compromise to remove it.  However, even after it is removed, removing the asynchronous scenario does not make any reduction in the RAN4 workload in the next meeting since anyhow it was not prioritized and would only have been discussed after RAN#94. Considering discussons so far and to manage RAN4 workload, the scope should be limited to LLR weighting and the further discussion of CRS-IC removed. We support the proposal by Nokia. |
| KDDI | We are fine with the proposal. We generally prefer to have some discussion on CRS-IC receivers but it is not feasible considering RAN4 workload, we are also fine to remove it. |
| CMCC | Thanks for considering our proposal. 30KHz is the most important scenario for us. We can compromise to remove the async scenario. |
| Intel | Yes, it is agreeable to exclude asynchronous scenario. CRS-IM processing for asynchronous network scenario requires extensive studies. In addition, we note that async scenario is out of scope of LTE CRS-IM requirements and we do not consider this as a typical one. Same time, we are also ok to keep it in WID and continue discussion in RAN4 as a part of requirements definition phase with a lower priority. |
| China Telecom | We are neutral on the async scenario.  For companies’ additional comment on CRS-IC, we think it is too premature to preclude CRS-IC for now, and we should review the RAN4 recommendation on reference receiver already as a compromise among different options.  For the last bullet, we also prefer to keep the original RAN4 recommendation as stated in LS. |
| ZTE | Yes, excluding async scenario explicitly and removing CRS-IC from the WID will make RAN4 more focused in this WI. |
| Huawei | We agree to exclude asynchronous scenario. If the asynchronous network refers to network just has larger timing offset between cell, the timing offset is already considered in the initial simulation for sync network scenario evaluation. If the asynchronous network refers to asynchronous network with time-varying timing offset, it is impractical to emulate it for performance requirements definition.  Similar to Ericsson, we would like to support Nokia proposal to consider LLR weighting as baseline reference receiver with no further CRS-IC considerations, to further reduce the workload in RAN4. |
| Samsung | We support to exclude async scenario to save RAN4 work load since no strong demand foreseen from operators. |
| BT | We consider the proposal is reasonable.  In order to complete the work in Rel-17, the work should be focus on conclude the baseline scenario, LLR weighting, and its prioritizations, synchronous network and 15 kHz. Once the essential work is concluded, 30 kHz SCS and CRS-IC can be further discussed. |

**Issue #2:** Whether to assume network assistance information for PDSCH CRS-IM?

**Proposal 2 (after intermediate round):** Task RAN4 to further discuss the necessity of network assistance signalling in Phase II.

**Proposal 3:** The information needed for LLR weighting and CRS-IC include (FFS how UE could obtain these information):

* For LLR weighting: presence of interference CRS, FFS on the location and sequence of interference CRS
* For CRS-IC: presence, location and sequence of interference CRS
* Note 1: the above information is for per interference cell
* Note 2:
  + The presence information includes the presence of LTE cell, MBSFN configuration, CRS muting information
  + The CRS location information includes LTE carrier frequency, bandwidth, v-shift, CRS port number
  + The CRS sequence related information includes physical cell id, slot number and symbol number

**Review of proposal 3:**

* Encourage review and feedback on proposal 3

|  |  |
| --- | --- |
| Company | Comment |
| Nokia, Nokia Shanghai Bell | In the light of proposal 2, we do not believe that proposal 3 is necessary in RAN.  On the other hand, it would be useful to clarify proposal 2 as follows:  *Task RAN4 to further discuss the necessity of network assistance signalling in Phase II, where consideration of network assistance signalling is confined to reusing the Rel-15/16 semi-static signalling of LTE CRS RM patterns that can be used inform the UE of the locations of the CRS REs.* |
| Apple | It is unclear as to where this proposal is going to be captured. If proposal #2 is to task RAN4 to discuss NWA, we might discuss this in RAN4 as well.  For LLR weighting, only presence of interfering CRS is not sufficient, the location and sequence is also needed from our understanding. Based on intermediate round responses from companies there seem to be different understanding and implementation. For any of the implementations the location of CRS REs is needed at a minimum, so both presence and location are needed. Hence propose to change is as:   * For LLR weighting: presence and location of interference CRS, FFS on the sequence of interference CRS |
| MTK | In our view, the information needed for LLR weighting and CRS-IC is the same. We are fine to task RAN4 to study it for one more quarter. |
| Qualcomm | We are fine to go back to RAN4 to discuss the needed assistance information in more detail. We disagree with Nokia’s proposal to artificially limit the assistance information to something from previous releases. |
| OPPO | Though sharing the similar view on the same information for LLR weighting and CRS-IC, we are also fine to task RAN4 to further discuss the details of network assistance signalling in Phase II. |
| Ericsson | Regarding proposal 3, we generally agree although for LLR weighting it is not obvious why sequence information would be needed. |
| KDDI | We prefer to postpone the discussion on the network assistance signalling to Rel-18, but if some RAN4 time is available, then we are fine to discuss it in Rel-17 time frame. |
| CMCC | We are OK with proposal 2 and 3. |
| Intel | 1) We are ok with proposal 2, but suggest minor update to request RAN4 WG to discuss the required information: “*Task RAN4 to further identify the required network assistance and discuss its necessity*  2) For Proposal 3 our overall preference is to keep this discussion up to RAN4 and task RAN4 to identify the information. We don’t think that the information shall be captured in the WID at this point.  Meantime, please see our comments on the specific questions.   * LLR weighting receiver: we think that UE needs information on CRS presence, location and sequence. We would like to ask proponents to clarify how LLR weighting can work without location and sequence of interference CRS. * We agree with information from Note 2. |
| China Telecom | For Nokia’s updated proposal#2:  On the one hand, from workload perspective, we think it may be good to reuse the existing signalling to avoid some extensive discussion on details while introducing new RRC signalling, in case it is agreed for CRS-IM.  On the other hand, however, we have following questions on reusing the existing Rel-15/16 signalling for CRS-IM:   * Q#1: For the proposed Rel-15 RM pattern, is it means the Rel-15 symbol level RM pattern or the Rel-15 serving cell CRS RM pattern? * Q#2: Rel-16 RM pattern can only handle 1 CRS pattern for the serving cell and 1 interference CRS pattern in DSS scenarios. But in our simulation work in RAN4, 2 interference cells are modelled in the agreed simulation assumption. We wonder whether it is feasible to only reuse the existing Rel-16 RM pattern for CRS-IM? * Q#3: The existing Rel-15/16 RM signalling does not contain LTE cell ID, which means UE will not know the interference CRS sequence by NW assistance signalling. Although from CTC’s perspective, the CRS sequence is not needed for LLR weighting, it seems companies have not reached consensus yet.   Considering the above, we prefer the original wording of Proposal#2.  For the Proposal#3:  As commented in the intermediate round, we think it is also feasible to do LLR weighting only based on the presence of interference LTE CRS, and CRS-IC needs the presence, location and sequence of interference CRS. However, according to more companies’ views, it appears we cannot reach consensus on all these details for this RAN meeting, so we also prefer leaving this issue to RAN4 meetings for further discussion. |
| ZTE | For P2, RAN4 can of course continue discussing the necessity of network assistance after the baseline requirements (based on the current agreed LLR weighting receiver without network assistance) are completed, but an explicit task from RAN plenary on this point seems distractive at this moment. And for P3, if CRS-IC is agreed to be removed from the WI, then the further improvement on the baseline receiver can be deferred until the baseline requirements are completed.  In one word, RAN4 better to focus on specifying the agreed baseline requirements. |
| Huawei | For Proposal 2: Lots of repeated debates happened in RAN4#100-e and at this RAN#93-e. To be honest, we do not observe any benefits to postpone to RAN4 for further discussion. No conclusion on the network assistance has been reached and it will delay all the following evaluations and discussions and may delay the whole work item completion, and delay the application in the real network eventually.  The DSS scenario and NR with neighboring LTE cell deployment are popular in the current networks, serious interference issues have been observed by several operators, with LTE refarming, the related deployments is diminishing, finally the commercial benefits to introduce CRS-IM in the real network will be seriously decreased. So based on the current discussion, we prefer to make decision in this RAN plenary meeting to make the CRS-IM more meaningful in the real network as early as possible.  For Proposal 3: It is better to discuss all information after we conclude the introduction of network assistance. Like we stated in the Intermediate round, it is feasible and manageable to do PBCH decoding considering that UE needs to support cell reselection in idle state and handover in connected state from NR to LTE, so UE should support inter-RAT measurements and PBCH decoding anyway even if inter-RAT measurement and PBCH decoding are needed for certain implementations, we did not observe any additional new implementation complexity to be introduced. |
| Ericsson | We agree with Huawei that it would be very much preferable to agree to make the assumption of no network signalling in this meeting in order to save RAN4 time and on the basis that it enables a consistent, fast and effective roll-out.  One comment on the Nokia proposal; re-using the RM should in our view be a maximum on what is considered in RAN4; if there really needs to be a discussion in RAN4 we think also the possibility of a simpler signalling (e.g. presence/absence of LTE) should be in scope.  *Task RAN4 to further discuss the necessity of network assistance signalling in Phase II, where consideration of network assistance signalling is confined to a maximum of reusing the Rel-15/16 semi-static signalling of LTE CRS RM patterns that can be used inform the UE of the locations of the CRS REs (or more simple signalling).* |
| Samsung | In last RAN4 meeting, companies were focused to drive the conclusion for the evaluation as this task by RAN. Given current situation, it’s hard to make conclusion on assistant signalling part without further thorough technical discussion in WG level.  In general, we support proposal 2 to discuss the NWA signalling in RAN4. Such technical discussion should include at least below factors:   1. Performance comparison between with and without NWA signalling 2. The UE complexity impact 3. NW impact i.e. whether existing Rel-15/16 signalling can be reused 4. Details on signalling information and corresponding assumption i.e. whether signalling always needed or not   For proposal 3, we are open to further discuss in RAN4 with this as starting point.  For the signalling part, considering the potential impact on RAN2, and deadline for Rel-17 ASN.1 frozen, the conclusion should be made no later than March RAN-P. |

## Final round summary

# Summary of proposals

## Outcome after intermediate round

**Issue #1**: Phase II objective (excepting the network assistance signalling part)

**Proposal 1:** Add the following phase II objective in Rel-17 WID on “Further enhancement on NR demodulation performance”:

*Define NR PDSCH demodulation requirements for neighbouring cell LTE CRS-IM in scenarios with overlapping spectrum for LTE and NR:*

*• Use LLR weighting as baseline reference receiver, and further discuss the feasibility of CRS-IC receiver taking into account the UE complexity and PDSCH processing time.*

*• Synchronous network scenario is prioritized. The asynchronous network scenario will be discussed after RAN #94e meeting.*

*• 15 kHz SCS for NR is prioritized. The 30 kHz SCS scenario will be discussed after RAN #94e meeting.*

*• RAN4 will further discuss the necessity of ~~network assistance signaling and~~ UE capability signaling during requirements definition phase.*

*Note: if further agreements for Issue #2 can be reached, the signalling part can be updated accordingly; otherwise the original RAN4 recommendation will be added back.*

**Issue #2:** Whether to assume network assistance information for PDSCH CRS-IM?

**Proposal 2:** Task RAN4 to further discuss the necessity of network assistance signalling in Phase II.

# Annex: Contacts

Please provide a company contact that the email discussion moderator can contact if required.

|  |  |
| --- | --- |
| **Company** | **Contact name and email** |
| Huawei | Michal Szydelko, [michal.szydelko@huawei.com](mailto:michal.szydelko@huawei.com) |
| OPPO | Roy Hu, hurongyi@oppo.com |
| ZTE | Aijun CAO, cao.aijun@zte.com.cn |
| Apple | Manasa Raghavan, manasa.raghavan@apple.com |
| China Telecom | Jingzhou Wu, wujingzhou@chinatelecom.cn |
| Qualcomm | Valentin Gheorghiu, vgheorgh@qti.qualcomm.com |
| Ericsson | Thomas.chapman@ericsson.com |
| BT | Johnny Dixon, johnny.dixon@bt.com |
|  |  |
|  |  |
|  |  |