**3GPP TSG-RAN Meeting #93 Electronic *R2-21xxxx***

**Online, 13 – 17 September 2021**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **38.101-1** | **CR** | **0926** | **rev** | **2** | **Current version:** | **16.8.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Introduction of extended range and NS-value for n77 |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** | Ericsson, Nokia, Nokia Shanghai Bell, Verizon, Qualcomm Incorporated |
|  |  |
| ***Work item code:*** | NR\_RF\_FR1-Core |  | ***Date:*** | 2021-09-13 |
|  |  |  |  |  |
| ***Category:*** | **C** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | In March 2021, the FCC has released new rules for the frequency range 3450-3550 MHz. The range 3450-3550 MHz is covered by band n77. Due to high demand of 3.5 GHz spectrum in the USA, enabling the use of the new frequency range within band n77 as quickly as possible is a priority for the entire cellular ecosystem. To ensure the network can properly deal with legacy n77 UEs that do not support 3.45-3.55 GHz operation in USA, UE’s information to indicate 3450-3550 MHz can handle the issues in initial access and handover between serving cell and target cell.Introduce an NS value to be used in combination with the UE *modifiedMPR-Behavior* for handling existing UEs when extending Band n77 operation in the USA to include 3450-3550 MHz in addition to 3700-3980.The NS value is only applicable in the range 3450-3550 MHz in the USA and used for barring existing devices from accessing a cell in 3450-3550 MHz from IDLE mode. From a network standpoint, these UEs are not supposed to be in the said cell and would be rejected by a network using standard UE-capability handling. Therefore these existing UEs should be barred to prevent that they make multiple attempts at coming back to this cell. |
|  |  |
| ***Summary of change:*** | Sub-clause 2:Added references to 38.306 and 36.306Sub-clause 5.2:Modify NOTE 12 to capture the new range for n77 in USA.Sub-clause 6.2.3:An NS value “NS\_55” is introduced for n77 in Table 6.2.3.1-1 and Table 6.2.3.1-2 (NS\_55 is available in both Rel-16 and Rel-17 specifications).The requirements applicable when the “NS\_55” is indicated in a cell is specified in Table 6.2.3.1-1 by a table note. The note is specified as follows:NOTE 5: This NS value is applicable for cells in the range 3450-3550 MHz for operations in the USA. **Isolated impact analysis:** existing UEs not comprehending the new NS value and not limited to the range 3700-3980 MHz when operated in the USA cannot access the 3450-3500 MHz range from IDLE mode.  |
|  |  |
| ***Consequences if not approved:*** | The new range 3450-3550 MHz cannot be applied to band n77 for USA operation.  |
|  |  |
| ***Clauses affected:*** | 2, 5.2, 6.2.3, 6.5.5.3, L.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **X** |  |  Other core specifications  | TS 36.306 CR 1824r2TS 36.331 CR 4723r2 |
| ***affected:*** |  | **X** |  Test specifications |   |
| ***(show related CRs)*** |  | **X** |  O&M Specifications |   |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | Revision 1:NOTE 12 in 5.2 is changed to capture the new range of n77 in the US and the note now captures relation to the capability bit.NS\_55 was used instead of NS\_52. NS\_55 is used since available in both Rel-16 and Rel-17 (NS\_52 for V2X, NS\_53 and N\_54 for shared spectrum access in Rel-16, NS\_56 defined from Rel-17).Revision 2:Updated NOTE 12 in clause 5.2Updated NOTE 5 in clause 6.2.3.1Added changes to clause 2 to add references to 38.306 and 36.306.Changed "US" to "USA" on the cover page.Updated the revision-number of the CRs listed in "Other specs affected"-field.Added sub-clause 6.5.3.3.26 for additional spurious emission requirement for NS\_55.Update Table L.1-1 to include n77 with *modifiedMPR-Behavior* bit to indicate the support of NS\_55. |

*< start of changes >*

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

For a specific reference, subsequent revisions do not apply.

For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document in the same Release as the present document.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 38.101-2: "NR; User Equipment (UE) radio transmission and reception; Part 2: Range 2 Standalone".

[3] 3GPP TS 38.101-3: "NR; User Equipment (UE) radio transmission and reception; Part 3: Range 1 and Range 2 Interworking operation with other radios".

[4] 3GPP TS 38.521-1: "NR; User Equipment (UE) conformance specification; Radio transmission and reception; Part 1: Range 1 Standalone".

[5] Recommendation ITU-R M.1545: "Measurement uncertainty as it applies to test limits for the terrestrial component of International Mobile Telecommunications-2000".

[6] 3GPP TS 38.211: "NR; Physical channels and modulation".

[7] 3GPP TS 38.331: "Radio Resource Control (RRC) protocol specification".

[8] 3GPP TS 38.213: "NR; Physical layer procedures for control".

[9] ITU-R Recommendation SM.329-10, "Unwanted emissions in the spurious domain".

[10] 3GPP TS 38.214: "NR; Physical layer procedures for data".

[11] 3GPP TS 36.101: Evolved Universal Terrestrial Radio Access (E-UTRA); User Equipment (UE) radio transmission and reception;

[12] ETSI TS 102 792: "Intelligent Transport Systems (ITS); Mitigation techniques to avoid interference between European CEN Dedicated Short Range Communication (CEN DSRC) equipment and Intelligent Transport Systems (ITS) operating in the 5 GHz frequency range".

[13] 3GPP TS 38.133: "NR; Requirements for support of radio resource management".

[14] 3GPP TS 37.213: “Physical layer procedures for shared spectrum channel access”.

[X] 3GPP TS 38.306: "NR; User Equipment (UE) radio access capabilities".

[Y] 3GPP TS 36.306: "Evolved Universal Terrestrial Radio Access (E-UTRA); User Equipment (UE) radio access capabilities".

*< Next change >*

## 5.2 Operating bands

NR is designed to operate in the FR1 operating bands defined in Table 5.2-1.

Table 5.2-1: NR operating bands in FR1

|  |  |  |  |
| --- | --- | --- | --- |
| NR operating band | Uplink (UL) *operating band*BS receive / UE transmitFUL\_low  – FUL\_high | Downlink (DL) *operating band*BS transmit / UE receiveFDL\_low – FDL\_high | Duplex Mode |
| n1 | 1920 MHz – 1980 MHz | 2110 MHz – 2170 MHz | FDD |
| n2 | 1850 MHz – 1910 MHz | 1930 MHz – 1990 MHz | FDD |
| n3 | 1710 MHz – 1785 MHz | 1805 MHz – 1880 MHz | FDD |
| n5 | 824 MHz – 849 MHz | 869 MHz – 894 MHz | FDD |
| n7 | 2500 MHz – 2570 MHz | 2620 MHz – 2690 MHz | FDD |
| n8 | 880 MHz – 915 MHz | 925 MHz – 960 MHz | FDD |
| n12 | 699 MHz – 716 MHz | 729 MHz – 746 MHz | FDD |
| n14 | 788 MHz – 798 MHz | 758 MHz – 768 MHz | FDD |
| n18 | 815 MHz – 830 MHz | 860 MHz – 875 MHz | FDD |
| n20 | 832 MHz – 862 MHz | 791 MHz – 821 MHz | FDD |
| n25 | 1850 MHz – 1915 MHz | 1930 MHz – 1995 MHz | FDD |
| n26 | 814 MHz – 849 MHz | 859 MHz – 894 MHz | FDD |
| n28 | 703 MHz – 748 MHz | 758 MHz – 803 MHz | FDD |
| n29 | N/A | 717 MHz – 728 MHz | SDL |
| n303 | 2305 MHz – 2315 MHz | 2350 MHz – 2360 MHz | FDD |
| n34 | 2010 MHz – 2025 MHz | 2010 MHz – 2025 MHz | TDD |
| n3810 | 2570 MHz – 2620 MHz | 2570 MHz – 2620 MHz | TDD |
| n39 | 1880 MHz – 1920 MHz | 1880 MHz – 1920 MHz | TDD |
| n40 | 2300 MHz – 2400 MHz | 2300 MHz – 2400 MHz | TDD |
| n41 | 2496 MHz – 2690 MHz | 2496 MHz – 2690 MHz | TDD |
| n46 | 5150 MHz – 5925 MHz | 5150 MHz – 5925 MHz | TDD13 |
| n4711 | 5855 MHz – 5925 MHz | 5855 MHz – 5925 MHz | TDD |
| n48 | 3550 MHz – 3700 MHz | 3550 MHz – 3700 MHz | TDD |
| n50 | 1432 MHz – 1517 MHz | 1432 MHz – 1517 MHz | TDD1 |
| n51 | 1427 MHz – 1432 MHz | 1427 MHz – 1432 MHz | TDD |
| n53 | 2483.5 MHz – 2495 MHz | 2483.5 MHz – 2495 MHz | TDD |
| n65 | 1920 MHz – 2010 MHz | 2110 MHz – 2200 MHz | FDD4 |
| n66 | 1710 MHz – 1780 MHz | 2110 MHz – 2200 MHz | FDD |
| n70 | 1695 MHz – 1710 MHz | 1995 MHz – 2020 MHz | FDD |
| n71 | 663 MHz – 698 MHz | 617 MHz – 652 MHz | FDD |
| n74 | 1427 MHz – 1470 MHz | 1475 MHz – 1518 MHz | FDD |
| n75 | N/A | 1432 MHz – 1517 MHz | SDL |
| n76 | N/A | 1427 MHz – 1432 MHz | SDL |
| n7712 | 3300 MHz – 4200 MHz | 3300 MHz – 4200 MHz | TDD |
| n78 | 3300 MHz – 3800 MHz | 3300 MHz – 3800 MHz | TDD |
| n79 | 4400 MHz – 5000 MHz | 4400 MHz – 5000 MHz | TDD |
| n80 | 1710 MHz – 1785 MHz | N/A | SUL  |
| n81 | 880 MHz – 915 MHz | N/A | SUL  |
| n82 | 832 MHz – 862 MHz | N/A | SUL  |
| n83 | 703 MHz – 748 MHz | N/A | SUL |
| n84 | 1920 MHz – 1980 MHz | N/A | SUL |
| n86 | 1710 MHz – 1780 MHz | N/A | SUL |
| n89 | 824 MHz – 849 MHz | N/A | SUL |
| n90 | 2496 MHz – 2690 MHz | 2496 MHz – 2690 MHz | TDD5 |
| n91 | 832 MHz – 862 MHz | 1427 MHz – 1432 MHz | FDD9 |
| n92 | 832 MHz – 862 MHz | 1432 MHz – 1517 MHz | FDD9 |
| n93 | 880 MHz – 915 MHz | 1427 MHz – 1432 MHz | FDD9 |
| n94 | 880 MHz – 915 MHz | 1432 MHz – 1517 MHz | FDD9 |
| n958 | 2010 MHz – 2025 MHz | N/A | SUL |
| n9614 | 5925 MHz – 7125 MHz | 5925 MHz – 7125 MHz | TDD13 |
| NOTE 1: UE that complies with the NR Band n50 minimum requirements in this specification shall also comply with the NR Band n51 minimum requirements.NOTE 2: UE that complies with the NR Band n75 minimum requirements in this specification shall also comply with the NR Band n76 minimum requirements.NOTE 3: Uplink transmission is not allowed at this band for UE with external vehicle-mounted antennas.NOTE 4: A UE that complies with the NR Band n65 minimum requirements in this specification shall also comply with the NR Band n1 minimum requirements.NOTE 5: Unless otherwise stated, the applicability of requirements for Band n90 is in accordance with that for Band n41; a UE supporting Band n90 shall meet the requirements for Band n41. A UE supporting Band n90 shall also support band n41.NOTE 6: A UE that supports NR Band n66 shall receive in the entire DL operating band.NOTE 7: A UE that supports NR Band n66 and CA operation in any CA band shall also comply with the minimum requirements specified for the DL CA configurations CA\_n66B and CA\_n66(2A) in the current version of the specification.NOTE 8: This band is applicable in China only.NOTE 9: Variable duplex operation does not enable dynamic variable duplex configuration by the network, and is used such that DL and UL frequency ranges are supported independently in any valid frequency range for the band. NOTE 10: When this band is used for V2X SL service, the band is exclusively used for NR V2X in particular regions.NOTE 11: This band is unlicensed band used for V2X service. There is no expected network deployment in this band.NOTE 12: In the USA this band is restricted to 3450 – 3550 MHz and 3700 – 3980 MHz.NOTE 13: This band is restricted to operation with shared spectrum channel access as defined in 37.213.NOTE 14: This band is applicable in the USA only subject to FCC Report and Order FCC 20-51 |

*< Next change >*

### 6.2.3 UE additional maximum output power reduction

#### 6.2.3.1 General

Additional emission requirements can be signalled by the network. Each additional emission requirement is associated with a unique network signalling (NS) value indicated in RRC signalling by an NR frequency band number of the applicable operating band and an associated value in the field *additionalSpectrumEmission.* Throughout this specification, the notion of indication or signalling of an NS value refers to the corresponding indication of an NR frequency band number of the applicable operating band, the IE field *freqBandIndicatorNR* and an associated value of *additionalSpectrumEmission* in the relevant RRC information elements [7]*.*

To meet the additional requirements, additional maximum power reduction (A-MPR) is allowed for the maximum output power as specified in Table 6.2.1-1. Unless stated otherwise, the total reduction to UE maximum output power is max(MPR, A-MPR) where MPR is defined in clause 6.2.2. Outer and inner allocation notation used in clause 6.2.3 is defined in clause 6.2.2 In absence of modulation and waveform types the A-MPR applies to all modulation and waveform types.

Table 6.2.3.1-1 specifies the additional requirements with their associated network signalling values and the allowed A-MPR and applicable operating band(s) for each NS value. In case of a power class 3 UE, when IE *powerBoostPi2BPSK* is set to 1, power class 2 A-MPR values apply. The mapping of NR frequency band numbers and values of the *additionalSpectrumEmission* to network signalling labels is specified in Table 6.2.3.1-1A.

For almost contiguous allocations in CP-OFDM waveforms in power class 3, the allowed A-MPR defined in clause 6.2.3 is increased by CEIL{ 10 log10(1 + NRB\_gap / NRB\_alloc), 0.5 } dB, where NRB\_gap is the total number of unallocated RBs between allocated RBs and NRB\_alloc is the total number of allocated RBs, and the parameter LCRB is replaced by NRB\_alloc + NRB\_gap in specifying the RB allocation regions.

Unless otherwise specified, pi/2 BPSK in following A-MPR tables refers to both variants of pi/2 BPSK referenced in 6.2.2 tables 6.2.2-1.

Table 6.2.3.1-1: Additional maximum power reduction (A-MPR)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Network signalling label | Requirements (clause) | NR Band | Channel bandwidth (MHz) | Resources blocks (*N*RB) | A-MPR (dB) |
| NS\_01 |  | Table 5.2-1 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | Table 5.3.2-1 | N/A |
| NS\_03 | 6.5.2.3.3 | n2, n25, n66,n70, n86 |  |  | Clause 6.2.3.7 |
| NS\_03U | 6.5.2.3.3, 6.5.2.4.2 | n2, n25, n66, n86 |  |  | Clause 6.2.3.7 |
| NS\_04 | 6.5.2.3.2, 6.5.3.3.1 | n41 | 10, 15, 20, 30, 40, 50, 60 80, 90, 100 |  | Clause 6.2.3.2 |
| NS\_05 | 6.5.3.3.4 | n1, n65, n84 | 5, 10, 15, 20(NOTE 2) |  | Clause 6.2.3.4 |
| NS\_05U | 6.5.3.3.4, 6.5.2.4.2 | n1, n65, n84 | 5, 10, 15, 20 |  | Clause 6.2.3.4 |
| NS\_06 | 6.5.2.3.4 | n12 | 5, 10, 15 |  | N/A |
| n14 | 5,10 |
| NS\_10 |  | n20 | 15, 20 | Table 6.2.3.3-1 | Table6.2.3.3-1 |
| NS\_12 | 6.5.3.3.17 | n26 | 5,10 | Table 6.2.3.21-1 | Table 6.2.3.21-2 |
| NS\_13 | 6.5.3.3.18 | n26 | 5 | Table 6.2.3.22-1 | Table 6.2.3.22-2 |
| NS\_14 | 6.5.3.3.19 | n26 | 10,15,20 | Table 6.2.3.23-1 | Table 6.2.3.23-2 |
| NS\_15 | 6.5.3.3.20 | n26 | 5,10,15,20 | Table 6.2.3.24-1 | Table 6.2.3.24-2 |
| NS\_17 | 6.5.3.3.2 | n28, n83 | 5,10 | Table 5.3.2-1 | N/A |
| NS\_18 | 6.5.3.3.3 | n28, n83 | 5 |  | Table 6.2.3.13-1, A1 |
|  |  |  | 10, 15, 20 |  | Table 6.2.3.13-1, A2 |
|  |  |  | 30 |  | Table 6.2.3.13-1, A3, A4, A5 |
| NS\_21 | 6.5.3.3.12 | n30 | 5, 10 |  | Clause 6.2.3.14 |
| NS\_24 | 6.5.3.3.13 | n65 (NOTE 4) | 5, 10, 15, 20 | Table 6.2.3.15-1 | Clause 6.2.3.15 |
| NS\_27 | 6.5.2.3.86.5.3.3.14 | n48 | 5, 10, 15, 20, 40 | Table 6.2.3.16-1 | Table 6.2.3.16-2 |
| NS\_35 | 6.5.2.3.1 | n71 | 5, 10, 15, 20 | Table 5.3.2-1 | N/A |
| NS\_37 | 6.5.3.3.6 | n74(NOTE 3) | 10, 15 | Table 6.2.3.8-1 | Table6.2.3.8-1 |
| NS\_38 | 6.5.3.3.7 | n74 | 5, 10, 15, 20 | Table 6.2.3.9-1 | Table6.2.3.9-1 |
| NS\_39 | 6.5.3.3.8 | n74 | 10, 15, 20 | Table 6.2.3.10-1 | Table 6.2.3.10-1 |
| NS\_40 | 6.5.3.3.9 | n51 | 5 |  | Table6.2.3.5-1 |
| NS\_41 | 6.5.3.3.10 | n50 | 5, 10, 15, 20, 30, 40, 50, 60 |  | Table 6.2.3.11-1 |
| NS\_42 | 6.5.3.3.11 | n50 | 5, 10, 15, 20, 30, 40, 50, 60 |  | Table 6.2.3.12-1 |
| NS\_43 | 6.5.3.3.5 | n8, n81 | 5, 10, 15 |  | Clause 6.2.3.6 |
| NS\_43U | 6.5.3.3.5, 6.5.2.4.2 | n8, n81 | 5, 10, 15 |  | Clause 6.2.3.6 |
| NS\_44 | 6.5.3.3.24 | n38 | 25, 30, 40 | Table 6.2.3.20-1 | Table 6.2.3.20-1 |
| NS\_45 | 6.5.3.3.21 | n53 | 5, 10 |  | Clause 6.2.3.25 |
| NS\_46 | 6.5.3.3.25 | n7 | 25, 30, 40, 50 | Table 6.2.3.17-1 | Table 6.2.3.17-2 |
| NS\_47 | 6.5.3.3.15 | n41 (Note 5) | 30 | Table 6.2.3.18-1 | Table 6.2.3.18-2 |
| NS\_48 | 6.5.3.3.22 | n1 | 25, 30, 40, 50 | Table 6.2.3.26-1 | Table 6.2.3.26-1 |
| NS\_49 | 6.5.3.3.23 | n1 | 25, 30, 40, 50 | Table 6.2.3.27-1 | Table 6.2.3.27-1 |
| NS\_50 | 6.5.3.3.16 | n39 | 25, 30, 40 |  | Clause 6.2.3.19 |
| NS\_51 | 6.5.3.3.22 | n65 | 50 | Table 6.2.3.28-1 | Table 6.2.3.28-2 |
| NS\_55 | 6.5.3.3.26NOTE 5 | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  | N/A |
| NS\_100 | 6.5.2.4.2 | n1, n2, n3, n5, n8, n18, n25, n26, n65, n66, n80, n81, n84, n86, n89(NOTE 1) |  |  | Table6.2.3.1-2 |
| NOTE 1: This NS can be signalled for NR bands that have UTRA services deployedNOTE 2: No A-MPR is applied for 5 MHz BWChannel where the lower channel edge is ≥ 1930 MHz,10 MHz BWChannel where the lower channel edge is ≥ 1950 MHz and 15 MHz BWChannel where the lower channel edge is ≥ 1955 MHz.NOTE 3: Applicable when the NR carrier is within 1447.9 – 1462.9 MHzNOTE 4: Applicable when the upper edge of the channel bandwidth frequency is greater than 1980 MHNOTE 5: Applicable when the NR carrier is within 2545 – 2575 MHzNOTE 5: This NS value is applicable for cells in the range 3450-3550 MHz for operations in the USA.  |

[The NS\_01 label with the field *additionalPmax* [7] absent is default for all NR bands.]

Table 6.2.3.1-1A: Mapping of network signalling label

|  |  |
| --- | --- |
| NR band | Value of additionalSpectrumEmission |
|  | **0** | **1** | **2** | **3** | **4** | **5** | **6** | **7** |
| n1 | NS\_01 | NS\_100 | NS\_05 | NS\_05U | NS\_48 | NS\_49 |  |  |
| n2 | NS\_01 | NS\_100 | NS\_03 | NS\_03U |  |  |  |  |
| n3 | NS\_01 | NS\_100 |  |  |  |  |  |  |
| n5 | NS\_01 | NS\_100 |  |  |  |  |  |  |
| n7 | NS\_01 | NS\_46 |  |  |  |  |  |  |
| n8 | NS\_01 | NS\_100 | NS\_43 | NS\_43U |  |  |  |  |
| n12 | NS\_01 | NS\_06 |  |  |  |  |  |  |
| n14 | NS\_01 | NS\_06 |  |  |  |  |  |  |
| n18 | NS\_01 | NS\_100 |  |  |  |  |  |  |
| n20 | NS\_01 | Void | NS\_10 |  |  |  |  |  |
| n25 | NS\_01 | NS\_100 | NS\_03 | NS\_03U |  |  |  |  |
| n26 | NS\_01 | NS\_100 | NS\_12 | NS\_13 | NS\_14 | NS\_15 |  |  |
| n28 | NS\_01 | NS\_17 | NS\_18 |  |  |  |  |  |
| n30 | NS\_01 | NS\_21 |  |  |  |  |  |  |
| n34 | NS\_01 |  |  |  |  |  |  |  |
| n38 | NS\_01 | NS\_44 |  |  |  |  |  |  |
| n39 | NS\_01 | NS\_50 |  |  |  |  |  |  |
| n40 | NS\_01 |  |  |  |  |  |  |  |
| n41 | NS\_01 | NS\_04 | NS\_47 |  |  |  |  |  |
| n48 | NS\_01 | NS\_27 |  |  |  |  |  |  |
| n50 | NS\_01 | NS\_41 | NS\_42 |  |  |  |  |  |
| n51 | NS\_01 | NS\_40 |  |  |  |  |  |  |
| n53 | NS\_01 | NS\_45 |  |  |  |  |  |  |
| n65 | NS\_01 | NS\_24 | NS\_100 | NS\_05 | NS\_05U | NS\_51 |  |  |
| n66 | NS\_01 | NS\_100 | NS\_03 | NS\_03U |  |  |  |  |
| n70 | NS\_01 | NS\_03 |  |  |  |  |  |  |
| n71 | NS\_01 | NS\_35 |  |  |  |  |  |  |
| n74 | NS\_01 | NS\_37 | NS\_38 | NS\_39 |  |  |  |  |
| n77 | NS\_01 | NS\_55 |  |  |  |  |  |  |
| n78 | NS\_01 |  |  |  |  |  |  |  |
| n79 | NS\_01 |  |  |  |  |  |  |  |
| n80 | NS\_01 | NS\_100 |  |  |  |  |  |  |
| n81 | NS\_01 | NS\_100 | NS\_43 | NS\_43U |  |  |  |  |
| n82 | NS\_01 | Void |  |  |  |  |  |  |
| n83 | NS\_01 | NS\_17 | NS\_18 |  |  |  |  |  |
| n84 | NS\_01 | NS\_100 | NS\_05 | NS\_05U |  |  |  |  |
| n86 | NS\_01 | NS\_100 | NS\_03 | NS\_03U |  |  |  |  |
| n89 | NS\_01 | NS\_100 |  |  |  |  |  |  |
| n91 | NS\_01 |  |  |  |  |  |  |  |
| n92 | NS\_01 |  |  |  |  |  |  |  |
| n93 | NS\_01 |  |  |  |  |  |  |  |
| n94 | NS\_01 |  |  |  |  |  |  |  |
| n95 | NS\_01 |  |  |  |  |  |  |  |
| NOTE: *additionalSpectrumEmission* corresponds to an information element of the same name defined in clause 6.3.2 of TS 38.331 [7]. |

*< Unchanged sections omitted >*

#### 6.5.3.3 Additional spurious emissions

These requirements are specified in terms of an additional spectrum emission requirement. Additional spurious emission requirements are signalled by the network to indicate that the UE shall meet an additional requirement for a specific deployment scenario as part of the cell handover/broadcast message.

*< Unchanged sections omitted >*

##### 6.5.3.3.26 Requirement for network signalling value "NS\_55"

When "NS\_55" is indicated in the cell, the power of any UE emission shall not exceed the levels specified in Table 6.5.3.3.7-1. This requirement does not apply for the frequency ranges that are less than FOOB (MHz) in Table 6.5.3.1-1 from the edge of the channel bandwidth.

**Table 6.5.3.3.26-1: Additional requirements for NR channels assigned within 3450-3550MHz for "NS\_55"**

|  |  |  |
| --- | --- | --- |
| **Frequency band****(MHz)** | **Channel bandwidth (MHz) /** **Spectrum emission limit (dBm)** | **Measurement bandwidth** |
| **10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100** |
| 3550 ≤ f ≤ 3700 | -25 | 1 MHz |

*< Unchanged sections omitted >*

# L.1 Indication of modified MPR behavior

This annex contains the definitions of the bits in the field *modifiedMPR-Behavior* indicated per supported NR band in the IE *RF-Parameters* [7] by a UE supporting an MPR or A-MPR modified in a given version of this specification. A modified MPR or A-MPR behaviour can apply to a supported NR band in stand-alone operation (including CA and NN-DC operation) or in non-standalone operation with the said NR band as part of an EN-DC or NE-DC band combination.

NOTE 1: In the present release, the *modifiedMPR-Behavior* is indicated [7] by an 8-bit bitmap per supported NR band.

Table L.1-1: Definitions of the bits in the field *modifiedMPR-Behavior*

|  |  |  |  |
| --- | --- | --- | --- |
| NR Band | Index of field(bit number) | Definition(description of the supported functionality if indicator set to one) | Notes |
| n41 | 0 (leftmost bit) | - EN-DC contiguous intraband MPR as defined in clause 6.2B.2.1 of 38.101-3 v15.5.0 | - This bit shall be set to 1 by a UE supporting DC\_(n)41AA UE EN-DC  |
|  | 1 | - EN-DC non-contiguous intraband MPR as defined in clause 6.2B.2.2 of 38.101-3 v15.5.0 | - This bit shall be set to 1 by a UE supporting DC\_41A\_n41A EN-DC  |
|  | 2 | - EN-DC contiguous and non-contiguous intraband MPR and A-MPR as defined in 38.101-3 v16.4.0. If this bit is not set the UE uses Rel-15 MPR or A-MPR for EN-DC contiguous and non-contiguous intraband MPR and A-MPR  | -This bit may be set to 1 by a UE supporting DC\_(n)41AA or DC\_41A\_n41A EN-DC  |
| n71 | 0 (leftmost bit) | - EN-DC contiguous intraband MPR as defined in clause 6.2B.2.1 of 38.101-3 v15.5.0 | - This bit shall be set to 1 by a UE supporting DC\_(n)71AA UE EN-DC  |
| n77 | 0 (leftmost bit) | - Support of the 3450-3550 MHz range and NS\_55 in addition to the 3700-3980 MHz for US operation | - This bit shall be set to 1 by a UE supporting the 3450-3550 MHz range in addition to the 3700-3980 MHz within band n77 in the USA |