**3GPP TSG RAN Meeting #94e Rev2 of RP-212713**

**Electronic Meeting, Dec. 6 - 17, 2021** (revision of RP-21xxxx)

**Source: RAN Vice-Chair (AT&T)**

**Title: New WI: NR NTN (Non-Terrestrial Networks) enhancements**

**Document for: Approval**

**Agenda Item: xxx**

3GPP™ Work Item Description

Information on Work Items can be found at <http://www.3gpp.org/Work-Items>   
See also the [3GPP Working Procedures](http://www.3gpp.org/specifications-groups/working-procedures), article 39 and the TSG Working Methods in [3GPP TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm)

# Title: New WI: NR NTN (Non-Terrestrial Networks) enhancements

## Acronym: NR\_NTN\_enh

## Unique identifier:

NOTE: For new WIs/SIs leave the Unique identifier empty and make a proposal for an Acronym.

For a revised WI/SI: Take Unique identifier and acronym as shown in 3GPP workplan.

If this is a RAN WID including Core and Perf. part, then Title, Acronym and Unique identifier refer to the feature WI.

Please tick (X) the applicable box(es) in the table below:

Either:

|  |  |
| --- | --- |
| **This WID includes a Core part** | **X** |
| **This WID includes a Performance part** | **X** |

or:

|  |  |  |
| --- | --- | --- |
| **This WID includes a Testing part** | |  |
| **and it addresses the following 3GPP work area:** | **Radio Access** |  |
| **Core Network** |  |
| **Services** |  |

Potential target Release: Rel-18

Note that this field above indicates the proposed Release at the time of submission of the WID to TSG approval. It can later be changed without a need to revise the WID. The updated target Release is indicated in the Work Plan. NOTE: In case of contradiction with the target dates of clause 5, clause 5 determines the target release.

## 1 Impacts

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Affects:** | UICC apps | ME | AN | CN | Others (specify) |
| **Yes** |  | X | X | X |  |
| **No** |  |  |  |  | X |
| **Don't know** | X |  |  |  |  |

## 2 Classification of the Work Item and linked work items

### 2.1 Primary classification

This work item is a …

|  |  |
| --- | --- |
| X | Feature |
|  | Building Block |
|  | *Work Task* |
|  | Study Item |

NOTE: Normally, Core/Perf./Testing parts in RAN WIDs are Building Blocks. Only if they are under an SA or CT umbrella, they are defined as work tasks. If you are in doubt, please contact MCC.

### 2.2 Parent Work Item

|  |  |  |  |
| --- | --- | --- | --- |
| Parent Work / Study Items | | | |
| Acronym | Working Group | Unique ID | Title (as in 3GPP Work Plan) |
|  |  |  |  |

NOTE: RAN agreed some time ago, that it describes the feature WI + Core/Perf. part WI or Testing part WI in one WID. Therefore the table above should just include the feature WI data (In case the feature covers Core and Perf. part, please list under Working Group the leading WG of the Core part).

### 2.3 Other related Work Items and dependencies

|  |  |  |
| --- | --- | --- |
| Other related Work Items (if any) | | |
| Unique ID | Title | Nature of relationship |
| 750040 | Study on NR to support non-terrestrial networks (FS\_NR\_nonterr\_nw) | The proposed WID will make use of the channel model defined by the FS\_NR\_nonterr\_nw study |
| 800099 | Study on solutions for NR to support non-terrestrial networks (FS\_NR\_NTN\_solutions) | The proposed WID will leverage solutions identified in FS\_NR\_NTN\_solutions to address some of the key issues associated to NTN |
| 890034 | Integration of satellite systems in the 5G architecture (5GSAT\_ARCH) | The proposed WID can consider the QoS management and Satellite NG-RAN global identities solutions identified in 5GSAT\_ARCH. |
| 860046 | solutions for NR to support non-terrestrial networks (NR\_NTN\_solutions) | The proposed WID will use this WID as basis for the evolution. |

NOTE: Also related or dependent WIs/SIs in other TSGs should be indicated.

## 3 Justification

In Release 17, a work item was carried out to define solutions enabling New Radio and NG-RAN to support Non-Terrestrial Networks (NTN):

* Transparent payload based GEO and NGEO network scenarios addressing at least 3GPP power class 3 UE with GNSS capability in both Earth fixed and/or moving cell configurations

As part of Release 18, a new work item is proposed to define enhancements for NG-RAN based Non-Terrestrial Networks in order to:

* Support new scenarios to cover deployments in frequency bands above 10 GHz
* Offer optimized performance especially when addressing handset terminals (including smartphones with more realistic assumptions on antenna gains, e.g., -5dBi instead of 0 dBi antenna gain with the specific realistic antenna gain assumption to be determined at the working group level) w.r.t. coverage considering the NTN characteristics such as large propagation delay and satellite movement.
* Address requirements, if needed based on the study outcome, which mandate the network operator to cross check the UE location reported by the UE, which needs to be carried out in order to fulfil the regulatory requirements (e.g., Lawful intercept, emergency call, Public Warning System, …) regarding a network verified UE location i.e., to be able to check the UE reported location information and specify if needed mechanisms to fulfil the regulatory requirements.

## 4 Objective

### 4.1 Objective of SI or Core part WI or Testing part WI

The work item aims at specifying enhancements for NG-RAN based NTN (non-terrestrial networks) according to the following assumptions [with implicit compatibility to support HAPS (high altitude platform station) and ATG (air to ground) scenarios]:

* GEO and NGEO (LEO and MEO) with transparent payload.
* Earth fixed tracking area. Earth fixed & Earth moving cells for NGEO
* FDD mode
* UEs with GNSS capabilities
* Both “VSAT” devices with directive antenna (including fixed and moving platform mounted devices and commercial handset terminals (e.g. Power class 3) are supported in FR1
* Only “VSAT” devices with directive antenna (including fixed and moving platform mounted devices) are supported in above 10 GHz bands.

Note: In Rel-17 WID, “VSAT” device with external antenna on moving platform is equivalent to a device that operate on platforms in motion, and this is referred to as ESIM.

The detailed objectives are to specify enhancing features to Rel-15, 16 & 17’s NR radio interface & NG-RAN as follows:

4.1.1 Coverage enhancement

The Rel-18 NTN objectives are focused on the applicability of the solutions developed by general NR coverage enhancement to NTN, and identifying potential issues and enhancements if necessary, considering the NTN characteristics including large propagation delay and satellite movement. Only NTN-specific characteristics are to be included in this coverage enhancement work, otherwise it should be part of another WI (e.g., UL enhancement of coverage). The work needs to cover the use case of voice and low-data rate services using commercial smartphones with more realistic assumptions on antenna gains, e.g., -5dBi instead of 0dBi currently assumed for link budget analysis for non-terrestrial networks. The specific realistic antenna gain assumption will be determined at the working group level.

Have a 1-TU [6]-month study phase focusing on the following (to derive clear & limited scope):

* Evaluate the coverage performance and identify the candidate physical radio channels that have coverage issues specific to NTN with following target services taking into account the studies in TR38.830 where appropriate, as well as general coverage enhancement techniques specified in Rel-18 [RAN1]
  + VoIP and low-data rate services for commercial handset terminals
* Study, and if justified, specify NTN-specific repetitions enhancements beyond techniques covered in Rel-17 CovEnh WI for the relevant channels [RAN1,RAN2]
* Study, and if justified, specify NTN-specific techniques for improved diversity and/or reduced polarization loss [RAN1]
* Study, and if justified, improve the performance of low-rate codecs in link budget limited situation including reducing RAN protocol overhead for VoNR [RAN2,RAN1] [Liaise with SA2/SA4 as necessary]
  + NOTE: Intent is to optimize the NTN-based NG-RAN to work with the lowest rate codec currently available and will not introduce a new codec.

RAN to determine by RAN#97 (for RAN1 items) and RAN#98 (for RAN2 items) whether the study phase has identified any need for NTN-specific coverage enhancements in Rel-18. After conclusion of the study phase above, the set of NTN-specific objectives may need to be updated/refined.

4.1.2 NR-NTN deployment in above 10 GHz bands

The following assumptions are taken a baseline for this work:

* GEO and NGEO (e.g. LEO, MEO, HEO) based satellite access to be considered
  + NGEO is not applicable for ESIM scenarios in Ka band.
* Targeted UE types: fixed and mobile VSAT. VSAT UE characteristics from TR38.821 to be considered in priority but additional NTN UE classes may be considered if justified
  + Regarding mobile VSAT, three types of terminal and scenario exist; airborne, maritime and land based ESIM.
* FDD mode is assumed for satellite operation above 10 GHz, while TDD mode is assumed for terrestrial operation in FR2
* The harmonized Ka band frequency range (17.7-20.2 and 27.5-30.0) as common across all regions will serve as reference

The following covers the objectives for NR-NTN deployment in above 10 GHz bands. In accordance with the WF in RP-211596, this work would start after March 2022 once FR1 NTN coexistence study is stable enough.

* Study and identify NTN bands (example band(s)?): Analysis of regulations and adjacent channel co-existence scenarios. The example band(s) shall be identified early in the WI. Additional bands can be introduced in a release-independent manner. [RAN4]
  + Consider at least a portion of the Ka band as the example band, according to ITU allocation; identify which parts of the Ka band are suitable as 3GPP bands [RAN4]
  + Study implications of FDD operation in FR2 and derive requirements for the identified part(s) of the Ka band appropriately. Satellite bands introduced in 3GPP for NTN for FDD shall not impact the existing 3GPP TDD specifications for terrestrial bands (see note 3 of the approved way forward RP-211596 in RAN#92-e). [RAN4]
  + For airborne and maritime ESIM terminals and scenarios, a large geographical separation to TN is assumed. This assumption shall be captured in the specification [RAN4].
  + For land based ESIM scenarios and terminals, appropriate co-existence scenarios need to be identified taking into account the regulatory condition of no interference towards terrestrial networks [RAN4]. The assumed scenarios need to be captured in the specification.
  + For non-mobile VSAT, appropriate co-existence scenarios need to be identified [RAN4].
  + Relevant coexistence scenarios and analysis to be considered in RAN4, if and where applicable, to ensure that satellite bands introduced in 3GPP for NTN shall neither impact the existing specifications of nor cause degradation (in the sense of RAN4 co-existence studies) to present and future networks in 3GPP specified terrestrial bands. [RAN4]
  + Definition of NTN band(s) above 10 GHz does not change the current FR1/FR2 definition, nor automatically apply to future terrestrial bands defined in this frequency region; (see proposal 2 of the approved way forward RP-211596 in RAN#92-e) [RAN4]
* Specify Rx/Tx requirements for satellite access node and different VSAT UE class (not only 60 cm aperture) as appropriate for the identified example band [RAN4]
* Identify values for physical layer parameters chosen from the existing FR1 and FR2 sets. The following set of parameters to specify, but not necessarily limited to, are listed.as follows [RAN4]:
  + time relationship related enhancement (e.g. K\_offset)
  + subcarrier spacing for different UL/DL signals/channels
  + PRACH configuration index for FDD above 10 GHz.

4.1.3 Network verified UE location

Have a 1-TU [6]-month study phase focusing on the following (to derive clear & limited scope):

* Study detailed regulatory requirement for network-verified UE location, e.g. accuracy requirement (at RAN plenary, from RAN#95 to RAN#96). [RAN]
* Study and evaluate, if needed, solutions for network to verify UE reported location information [RAN2,RAN1,RAN3]
  + For verification of Network based UE location, re-use of Rel-17 UE-specific Timing Advance report can be considered as baseline

RAN to determine by RAN#98 whether the study has identified any need for Network verified UE location specification support in Rel-18.

NOTE: The objectives for Network Verified UE Location will be moved to a separate SID or possibly to the Expanded and Improved Positioning WI depending on the outcome of the RAN#94e discussions.

### 4.2 Objective of Performance part WI

NOTE: Leave empty if the WI proposal does not contain a RAN performance part.

The performance part objectives are applicable to the NR-NTN deployment in above 10 GHz bands objective.

* Specify RRM performance requirements and test cases [RAN4]
* Specify UE demodulation and CSI reporting requirements [RAN4]
* Specify satellite access node demodulation requirements [RAN4]
* Specify satellite access node conformance tests [RAN4]

The RAN4 performance part for the remaining objectives needs to be further discussed once the scope is stabilized.

### 4.3 RAN time budget request (not applicable to RAN5 WIs/SIs)

NOTE: For all new RAN related WIs/SIs which are not led by RAN WG5 the WI/SI rapporteur has to fill out the attached Excel table to request time budgets for corresponding RAN WG meetings.  
The Excel table has to be filled out for all affected RAN WGs and up to the target date of the WI/SI.  
One time unit (TU) corresponds to ~ 2 hours in the meeting.  
If no TU is needed, then leave the field empty otherwise enter a number >0 in the field.

For revisions of already approved WI/SI descriptions: Please remove the Excel table from the WID/SID's zip file. The time budgets are already recorded. If you want to modify them, then this has to be done via the status report and not via a revised WID/SID.

If this WID is covering Core and Performance part, then please fill out one line for each part in the attached Excel table.

**additional comments to the time budget request in the attached Excel table:**

## 5 Expected Output and Time scale

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **New specifications** *{One line per specification. Create/delete lines as needed}* | | | | | |
| Type | TS/TR number | Title | For info  at TSG# | For approval at TSG# | Remarks |
| TS | 38.XXX | NR; User Equipment (UE) radio transmission and reception, part X: VSAT |  |  | Whether a specific VSAT TS is required is pending RAN decision. A unified specification may also be required. |
| TR | 38.XXX | NR; Network verified UE location for NTN |  |  | Applicabilty is pending the outcome of the RAN study. |

*{Note 1: Only TSs may contain normative provisions. Study Items shall create or impact only TRs.  
"Internal TR" is intended for 3GPP internal use only whereas "External TR" may be transposed by OPs.}*

NOTE: If this is a RAN WI including Core and Perf. part, then all new Core part specs have to be listed first and then all new Perf. part specs. Indicate "Core part" or "Perf. part" under Remarks for each spec.  
By default a new specs can only be new for one of both parts.

| **Impacted existing TS/TR** | | | |
| --- | --- | --- | --- |
| TS/TR No. | Description of change | Target completion plenary# | Remarks |
| 38.211 | NR; Physical channels and modulation  Enhancement on the PRACH sequence and/or format (in the case pre-compensation of timing and frequency offset is not done at UE side) |  | Core part |
| 38.213 | NR; Physical layer procedures for control  Enhancements to Timing Advance, control procedures signalling |  | Core part |
| 38.214 | NR; Physical layer procedures for data  Timing relationship enhancements, Enhancements on UL time and frequency synchronization, |  | Core part |
| 38.300 | NR; Overall description; Stage-2:  NTN stage 2 description |  | Core part |
| 38.304 | NR; User Equipment (UE) procedures in idle mode and in RRC Inactive state  Enhance the idle mobility trigger conditions |  | Core part |
| 38.305 | NG Radio Access Network (NG-RAN); Stage 2 functional specification of User Equipment (UE) positioning in NG-RAN  NTN UEs with GNSS capabilities |  | Core part |
| 38.306 | NR; User Equipment (UE) radio access capabilities  Support of NTN UE capabilities |  | Core part |
| 38.307 | NR; Requirements on User Equipments (UEs) supporting a release-independent frequency band  NTN release-independent frequency bands |  | Core part |
| 38.321 | NR; Medium Access Control (MAC) protocol specification: Enhance Random access, timing advance, DRX, Scheduling Request, HARQ |  | Core part |
| 38.322 | NR; Radio Link Control (RLC) protocol specification  Enhance Status reporting and Sequence Number and Window Size |  | Core part |
| 38.323 | NR; Packet Data Convergence Protocol (PDCP) specification  Enhance Status reporting and Sequence Number and SDU discard |  | Core part |
| 38.331 | NR; Radio Resource Control (RRC); Protocol specification  Enhance idle and connected mode mobility, NTN specific system information and RRC signalling |  | Core part |
| 38.401 | NG-RAN; Architecture description  NTN specific features |  | Core part |
| 38.410 | NG-RAN; NG general aspects and principles  NTN specific features |  | Core part |
| 38.413 | NG-RAN; NG Application Protocol (NGAP)  NTN specific features |  | Core part |
| 38.423 | NG-RAN; NG-RAN; Xn Application Protocol (XnAP)  NTN specific features |  | Core part |
| 38.108 | NR; Satellite Node radio transmission and reception  NTN specific characteristics |  |  |
| 38.181 | NR; Satellite Node conformance testing  NTN specific characteristics |  |  |
| 38.863 | NR; Solutions for NR to support non-terrestrial networks (NTN):  Non-terrestrial networks (NTN) related RF and co-existence aspects |  |  |

NOTE: If this is a RAN WI including Core and Perf. part, then all new Core part specs have to be listed first and then all new Perf. part specs. Indicate "Core part" or "Perf. part" under Remarks for each spec.  
If an existing spec is affected by both (Core part and Perf. part), then it has to be listed twice with appropriate approval dates.

## 6 Work item Rapporteur(s)

Chuberre, Nicolas, Thales, [nicolas.chuberre@thalesaleniaspace.com](mailto:nicolas.chuberre@thalesaleniaspace.com)

Hidekazu, Shimodaira, NTT DOCOMO, hidekazu.shimodaira.sa@nttdocomo.com

## 7 Work item leadership

Leading working group: RAN2

Secondary working groups: RAN1, RAN3, RAN4

## 8 Aspects that involve other WGs

Possible cooperation/alignment with:

SA2, SA3 and SA3-LI with respect to ‘Network verified UE location’ and the possible impact on regulatory requirements (e.g. LI, PWS,…).

* SA2 & SA4 with respect to ‘coverage enhancement’ and in particular the potential low-rate codecs performance enhancements for in link budget limited context.

NOTE: For RAN WIs: Section 8 applies only to WGs outside of TSG RAN because RAN WG aspects have to be covered in section 4.

## 9 Supporting Individual Members

*{At least 4 supporting Individual Members are needed. There is an expectation that these companies will provide resources to progress the work. Note that having 4 supporting companies is a necessary but not sufficient condition: the usual TSG approval process by consensus is needed for the WID approval.}*

|  |
| --- |
| Supporting IM name |
|  |
|  |
|  |
|  |
|  |
|  |