**3GPP TSG RAN WG1 Meeting #100bis-e *R1-200xxxx***

**E-Meeting, April 20 - April 30, 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **DRAFT CHANGE REQUEST** |
|  |
|  | **36.213** | **CR** | **xxxx** | **rev** | **-** | **Current version:** | **V14.14.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network | **x** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Correction on NPDCCH monitoring for NB-IoT |
|  |  |
| ***Source to WG:*** | Huawei, HiSilicon |
| ***Source to TSG:*** | R1 |
|  |  |
| ***Work item code:*** | NB\_IOTenh-Core |  | ***Date:*** | 2020-04-20 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-14 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | UE should not monitor DCI format N2 in a NPDCCH UE-specific search space. |
|  |  |
| ***Summary of change:*** | Remove “DCI N1” from UE-spceific search space and two HARQ processes case. |
|  |  |
| ***Consequences if not approved:*** | Without the first change, specification may cause confusion on whether DCI format N2 is intended to be valid or not. |
|  |  |
| ***Clauses affected:*** | 16.6 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  |  |
| ***affected:*** |  | **X** |  Test specifications |   |
| ***(show related CRs)*** |  | **X** |  O&M Specifications |   |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

< Unchanged parts are omitted >

## 16.6 Narrowband physical downlink control channel related procedures

< Unchanged parts are omitted >

For a NPDCCH UE-specific search space, if a NB-IoT UE is configured with higher layer parameter *twoHARQ-ProcessesConfig*

- and if the NB-IoT UE detects NPDCCH with DCI Format N1 ending in subframe *n*, and if a NPDSCH transmission starts from *n+k*, the UE is not required to monitor an NPDCCH candidate in any subframe starting from subframe *n+k-2* to subframe *n+k-1*;

otherwise

- if the NB-IoT UE detects NPDCCH with DCI Format N1 or N2 ending in subframe *n*, and if the corresponding NPDSCH transmission starts from *n+k*, the UE is not required to monitor NPDCCH in any subframe starting from subframe *n+1* to subframe *n+k-1*.

< Unchanged parts are omitted >