**3GPP TSG RAN WG1 #100bis R1-** **200xxxx**

**e-Meeting, April 20th – 30th, 2020**

**Agenda item:** 6.2.4

**Source:** Moderator (Qualcomm Incorporated)

**Title:** Email discussion [100b-e-LTE-TerrBcast-01]

**Document for:** Discussion and Decision

# Summary of issues

This document contains the discussion for the following:

[100b-e-LTE-TerrBcast-01] Email discussion/approval on reference signal aspects for 0.37 kHz numerology (antenna port definition; presence of RS; correction to MBSFN-RS generation) by 4/23; if necessary, followed by endorsing the corresponding TPs by 4/28 - Alberto (Qualcomm)

# Issue #1: Antenna port definition

In x1635, it is proposed to modify the text in TS 36.211 on antenna port definition as follows:

**<TP-1, TS 36.211, 6.2.1>**

- MBSFN reference signals are transmitted on antenna port. The channel over which a symbol on antenna portis conveyed can be inferred from the channel over which another symbol on the same antenna port is conveyed only if the two symbols correspond to subframes of the same MBSFN area. For MBSFN reference signal pattern type 1 of 0.37 kHz subcarrier spacing, the channel over which a symbol on antenna port  is conveyed can be inferred from the channel over which another three symbols on the same port is conveyed only if the four symbols correspond to slots of the same MBSFN area. For MBSFN reference signal pattern type 2 of 0.37 kHz subcarrier spacing, the channel over which a symbol on antenna port  is conveyed can be inferred from the channel over which another symbol on the same port is conveyed only if the two symbols correspond to slots of the same MBSFN area.

This introduces the following changes:

* Use “slots” instead of subframes.
* Limit the coherency for four symbols / two symbols depending on the RS pattern.

|  |  |
| --- | --- |
| **Company name** | **Comment** |
| Qualcomm | In general, the current specification should be enough, since the spec says “two symbols correspond to subframes of the same MBSFN area”, and, in the end, the 3 subframes of a slot belong to the same MBSFN area. If this needs to be made more clear, we suggest the following revision:For subcarrier spacing other than 0.37kHz, the channel over which a symbol on antenna portis conveyed can be inferred from the channel over which another symbol on the same antenna port is conveyed only if the two symbols correspond to subframes of the same MBSFN area. For subcarrier spacing of 0.37kHz, the channel over which a symbol on antenna portis conveyed can be inferred from the channel over which another symbol on the same antenna port is conveyed only if the two symbols correspond to slots of the same MBSFN areaWhat we do not support is the limitation of another three symbols. In theory, if the channel is completely static, the UE should be able to run an infinite filter to keep improving the channel estimation. |

# Issue #2: Presence of RS

In x2626 and x2179, it is recommended to discuss the assumptions the UE can make regarding the presence of reference symbols outside a given PMCH slot. More precisely, the following observations are made:

* In x2626***: A UE implementing frequency-only channel interpolation for the PMCH numerology with Δf = 0.37 kHz and RS pattern with Dt = 4/2 only achieves a theoretical equalisation interval of 225/450µs.***
* In x2179: The following TP is proposed, along with some additional observations on the proposals:

**<TP-2, 36.211 6.10.2>**

6.10.2 MBSFN reference signals

MBSFN reference signals shall be transmitted in the MBSFN region of MBSFN subframes only when the PMCH is transmitted. MBSFN reference signals are transmitted on antenna port 4.

For a PMCH transmitted with 0.37 kHz subcarrier spacing in slot ,

 - for MBSFN reference signal pattern type 1, the UE may assume that MBSFN reference signals associated with the same are present in the three preceding slots to slot .

- for MBSFN reference signal pattern type 2, the UE may assume that MBSFN reference signals associated with the same are present in the preceding slot to slot .

MBSFN reference signals are defined for extended cyclic prefix only.

**</TP-2>**

|  |  |
| --- | --- |
| **Company name** | **Comment** |
| Qualcomm | Support this change. |

# Issue #3: Correction to MBSFN-RS generation

In x2179, a potential issue with the MBSFN-RS generation for 0.37kHz SCS is presented. The current equation gives the following pattern for Td=4:



A TP is presented in x2179 as follows:

**<TP-3, 6.10.2.2.4>**

The reference-signal sequence in OFDM symbol shall be mapped to complex-valued modulation symbols with according to

where is the 3ms absolute slot number, defined as is the 3 ms slot number as defined in clause 4.1 and

- for MBSFN reference signal pattern type 1

* + For odd
	+ For even

- for MBSFN reference signal pattern type 2

**</TP-3>**

|  |  |
| --- | --- |
| **Company name** | **Comment** |
| Qualcomm | Support this change. If other companies find an easier way to write the equations, we would also be OK. |

# References

|  |  |  |
| --- | --- | --- |
| [R1-2001635](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_100b_e/Docs/R1-2001635.zip) | Corrections to TS 36.211 for the 0.37kHz subcarrier spacing MBSFN | ZTE |
| [R1-2002179](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_100b_e/Docs/R1-2002179.zip) | Support of longer numerologies for rooftop reception | Qualcomm Incorporated |
| [R1-2002626](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_100b_e/Docs/R1-2002626.zip) | UE assumptions of MBSFN-RS for new PMCH numerology for support of rooftop reception | EBU, BBC, IRT |