**3GPP TSG RAN WG1 Meeting #100bis-E R1-200xxxx**

**e-Meeting, April 20th – 30th, 2020**

**Source: Moderator (Intel Corporation)**

**Title: Email Discussion #3 [100b-e-NR-5G\_V2X\_NRSL-Mode-2-03]**

**Agenda item: 7.2.4.2.2**

**Document for:** **Discussion and Decision**

Introduction

This document provides discussion on issues in the third email discussion on V2X Mode-2 during RAN1#100bis-e.

[100b-e-NR-5G\_V2X\_NRSL-Mode-2-03] Email discussion/approval w.r.t. step2 including aspects:

* Whether to support HARQ retransmissions on unreserved resources
* Early in time initial resource selection
* Relation of selected number of resources and signalled number of resources, including number of outstanding reservations

till 4/27, with potential TPs till 4/30 (Intel, Sergey)

Discussion

The first aspect “Whether to support HARQ retransmissions on unreserved resources” has been touched in the last meeting in the context of maximum timing restriction between selected resources. There was no conclusion. This time, a more general question is asked first, and the solution to it, if needed, is expected to be decided right after a consensus.

From the contributions, the following options with respect to reserved/unreserved HARQ retransmissions are discussed:

* Allow unreserved HARQ retransmissions and do not introduce any condition/restriction to do that. Some companies think this is undesirable, and confirm it by evaluation results [13][27].
* Allow unreserved HARQ retransmissions if resource selection does not provide resources which can be signalled in one SCI, without changes to resource selection procedure. Some companies think this is undesirable, and confirm it by evaluation results [13][27].
  + When reservation of HARQ retransmission resources is not possible, there are two options:
    - Stop HARQ retransmissions
    - Continue HARQ retransmissions on unreserved resources. [8] shows that continuation is better than dropping in this case.
* Do not allow unreserved HARQ retransmissions, but introduce exceptions due to events external to the resource selection procedure, i.e. dropping due to prioritization after Uu-SL competition or congestion control
  + If this option is formulated using resource selection terms, then the dropping due to prioritization after Uu-SL competition or congestion control is automatically accounted. The pre-emption event may need to be discussed separately, subject to the outcome of Mode2-02 discussion.
  + If this option is formulated using signalling/reservation terms, then the dropping due to prioritization after Uu-SL competition or congestion control should be explicitly listed as an exception. The pre-emption event may need to be discussed separately, subject to the outcome of Mode2-02 discussion.

**Q1: Which of the following options related to HARQ retransmission resource reservation is preferred? General support can be expressed, while the detailed proposal can be worked out in the second phase.**

* Option 1: Support/allow unreserved HARQ retransmissions
  + Option 1a: Completely up to UE implementation to do that.
  + Option 1b: Only when resource selection does not provide resources which can be signalled in one SCI (without changes to the resource selection procedure)
* Option 2: Do not allow unreserved HARQ retransmissions
  + Option 2a: capture this in terms of Step 2 resource selection restriction as a maximum allowed logical slot distance, so that at least two resources can be signalled in one SCI
  + Option 2b: capture this as a signalling restriction, without direct impact on resource selection. At least Uu-SL competition and congestion control are exceptions to this
* Option 3: Configure between allowed / not allowed
  + One option was proposed in the last meeting

|  |  |  |  |
| --- | --- | --- | --- |
| Source | Option | Comment |  |
| Ericsson | See comments | None of the alternatives is good.  We think that a UE should make use of reservations whenever the signalling allows for it (e.g., 32 slots) and always make use of reserved resources (except if HARQ-ACK is received). However, preventing “unreserved HARQ retransmissions” altogether does not sound reasonable. There are many cases in which the UE may need to transmit on unreserved resources. Capturing the exceptions in a list may be hard. The following proposal is a way of capturing these points.  **Proposal**:   * The UE indicates max(Nselected, Nmax) resources when setting the values of frequency resource assignment and time resource assignment in SCI format 0\_1, where Nselected is the number of outstanding resources selected by MAC within 32 slots (including the current one). * The UE does not transmit a TB on unreserved resources if it has one or more reservations for transmission for that TB.   We do not think that this issue can be solved with a restriction on the slot distance (2a). |  |
| Intel | Option 2a | In case of re-evaluation in order to meet signalling window constraints (chain integrity):   1. UE can check if there are appropriate resources in candidate set and pick one 2. UE can ignore re-evaluation result and transmit if there is no available candidate resource satisfying chain integrity condition |  |
| Panasonic | Similar to Option 2a | (Re-)transmission of a TB should be reserved by a prior SCI unless some exceptions (pre-emption, Uu-SL priority competition, congestion control, etc.).  For option 2a, just to limit logical slot distance would not be sufficient in order not to allow unreserved HARQ retransmissions as frequency domain also needs to be restricted |  |
| NTT DOCOMO | Option 2a | Support Option 2. Capturing appropriate exceptions may be hard in 2b. |  |
| vivo | Option 2a-like | Agree with Panasonic. | vivo |
| Xiaomi | Option 1 | Can add constraints that only allow when UE does not have reserved resource to transmit. |  |

The second aspect is related to the first one, and intends to cover UE behaviour to signal resources in SCI depending on configured Nmax, the number of intended retransmissions M, etc. The following points have been identified from contributions:

* What is UE signalling behaviour for resources t0, t1, …tM-1 for a given configured Nmax value
  + For example, if Nmax = 2, whether UE signals first {t0, t1}, then {t1, t2}, then {t2, t3}, …, {tM-2, tM-1}, and finally {tM-1}, subject to the aspects of reserved/unreserved HARQ retransmissions in Q1
  + For example, if Nmax = 3, whether UE signals first {t0, t1, t2}, then {t1, t2, t3}, then {t2, t3, t4}, …, {tM-3, tM-2, tM-1}, then {tM-2, tM-1}, and finally {tM-1} etc., subject to the aspects of reserved/unreserved HARQ retransmissions in Q1
  + Whether a UE maximizes the number of signalled resources subject to configured Nmax
* How many unused resources can be allowed for FB-based retransmissions?
  + E.g. even if Nmax=3, whether a UE only reserves N=2, so that only one resource is at most left unreserved
* Number of outstanding reservations
  + Similar to the first bullet, current specification may allow reservation in the following un-ordered manner: {t0, t1, t2}, {t1, t3, t4}, {t3, t5, t6} etc. Whether it needs to be disallowed or not. In FL understanding, if the firs bullet aspect is resolved, this aspect is also automatically resolved

**Q2: Whether to support maximization of signaled number of resources in one SCI subject to configured Nmax value. General support can be expressed, while the detailed proposal can be worked out in the second phase.**

* Option 1: Support maximization of signaled number of resources in one SCI subject to configured Nmax value and logical slot distance between resources after the resource selection
  + Subject to fulfilled logical distance condition of 32 slots, the sequence of SCI signaling in different time instances for resources t0, t1, …tM-1 where M is the number of intended (re-)transmissions, can look like
    - N = 2: {t0, t1}, {t1, t2}, {t2, t3}, … {tM-2, tM-1}, {tM-1}
    - N = 3: {t0, t1, t2}, {t1, t2}, {t2, t3, t4}, …, {tM-3, tM-2, tM-1}, {tM-2, tM-1}, {tM-1}
      * here t1 and t3 are not within 32 slots, and thus {t1, t2} signals two resources
* Option 2: Leave the number of signalled resources up to UE implementation w/o any restriction

|  |  |  |  |
| --- | --- | --- | --- |
| Source | Option | Comment |  |
| Ericsson | 1 |  |  |
| Intel | Option 1 | We think the following UE behavior should be supported   * Case 1: Two resources dynamically signalled by SCI (NMAX ≤ 3):   + If any given SCI reserves one future resource - R1, the next SCI transmission, associated with the same resource selection process, should occur in the reserved resource - R1, subject to congestion control, in-device coexistence, HARQ feedback conditions * Case 2: Three resources dynamically signalled by SCI (NMAX = 3):   + If any given SCI reserves two future resources R1 and R2, the next SCI transmission, associated with the same resource selection process, should occur in the first in time reserved resource - R1, indicate the second reserved resource – R2 and possibly new resource reservation - R3 following the second reserved resource – R2, subject to congestion control, in-device coexistence, HARQ feedback conditions   Number of resources signaled by each SCI is up to UE implementation, subject to Nmax configuration |  |
| Panasonic | Option 1 | To maximize the benefit of the reservation of Nmax resources |  |
| NTT DOCOMO | Option 1 | Agree with Panasonic. |  |
| vivo | Option 1 |  |  |
| Xiaomi | Option 1 | If N=3, it is not clear whether it is allowed to signal resources which is not the nearest in time domain. For example, {t0, t1, t2}, {t1, t3, t4}, …, assuming that t1 and t4 are within 32 slots. Earlier signaling may be helpful for resource reservation purpose. |  |

The third aspect relates to so called “Early in time initial resource selection”. Companies, discussing this issue, argue that the initial resource should be selected as close as possible to the resource (re-)selection trigger. This may allow lower latency access to channel, earlier reservation announcement, and in some cases more HARQ retransmissions. Some companies show SLS results of latency and/or PRR benefits [13][27].

**Q3: Whether the initial resource can be selected in random non-uniform manner by prioritization of earlier candidate resources? General support can be expressed, while the detailed proposal can be worked out in the second phase.**

* Option 1
  + Do not support modifications to Step 2 resource selection that provide earlier in time initial resource selection
* Option 2
  + Support a modification to Step 2 resource selection that provides earlier in time initial resource selection
    - Option 2a: by picking the earliest identified resource after Step 1
    - Option 2b: by picking one resource from M\_earliest identified resources after Step 1. M\_earliest can be a 1/M part of the total identified resource set, where M is the intended number of retransmissions
    - Option 2c: by introducing a separate resource selection window for the initial resource with reduced maximum length

|  |  |  |  |
| --- | --- | --- | --- |
| Source | Option | Comment |  |
| Ericsson | Option 2c | Feature and window size can be configurable. |  |
| Intel | Option 2 | Prefer Option 2b for implementation. Evaluation results have shown stable and improved system performance with reduced latency. |  |
| Panasonic | Similar to Option 2b | We support that the earlier resources should be more prioritized. We think more weightage should be given to the earlier resources with randomization considered, instead of limiting to single resource (as in Option 2a).  We also think that the later resource should able be selected with lower weightage (as a modified Option 2b). |  |
| NTT DOCOMO | 2a | Support Option 2. In 2c, a resource with bad condition can be selected as candidate resource set due to narrower resource selection window. |  |
| vivo | Option 1 | We are not sure about the benefit of the so-called early in time selection in current situation. Since UE will select all resource for potential retransmission of a TB in one resource selection procedure, UE can decide the exact timing of each selected resource, this is totally up to UE implementation.  In our understanding, early in time selection maybe helpful if HARQ feedback can trigger resource selection. Then, for a given TB multiple resource selection process can be triggered, of course, the initial transmission is better at beginning of the PDB. |  |
| Xiaomi | Option 1 | The first selected resource may not be the first resource transmitted in time domain. Do not see the benefit of the modification |  |

Summary of proposals on the relevant issues

Although Step 2 was discussed last meeting, there are still remaining issues identified as follows:

1. Whether to support HARQ retransmissions on unreserved resources
   * Allowed w/o conditions: [19]
   * Allowed if chain is broken: [8][16]
     + Note: [8] shows results that HARQ process dropping is worse than unreserved retransmissions
   * Not allowed with exceptions
     + Formulated using HARQ retransmissions: [4][10][24][27]
     + Formulated using resource selection: [5][6][13][15][21]
     + Note: [13] and [27] show results in support if it
2. Early in time initial resource selection
   * [3][13][15][24][27]
     + Note: [13] and [27] show results in support if it
3. Relation of selected number of resources and signalled number of resources, including number of outstanding reservations
   * [6][13][17][21][23]

References

1. [R1-2001552](file:///C:\\Users\\wanshic\\OneDrive%20-%20Qualcomm\\Documents\\Standards\\3GPP%20Standards\\Meeting%20Documents\\TSGR1_100b\\Docs\\R1-2001552.zip) Remaining details of sidelink resource allocation mode 2 Huawei, HiSilicon

1. [R1-2001661](file:///C:\\Users\\wanshic\\OneDrive%20-%20Qualcomm\\Documents\\Standards\\3GPP%20Standards\\Meeting%20Documents\\TSGR1_100b\\Docs\\R1-2001661.zip) Remaining issues on mode 2 resource allocation mechanism vivo

1. [R1-2001749](file:///C:\\Users\\wanshic\\OneDrive%20-%20Qualcomm\\Documents\\Standards\\3GPP%20Standards\\Meeting%20Documents\\TSGR1_100b\\Docs\\R1-2001749.zip) Discussion on remaining open issue for mode 2 OPPO

1. [R1-2001793](file:///C:\\Users\\wanshic\\OneDrive%20-%20Qualcomm\\Documents\\Standards\\3GPP%20Standards\\Meeting%20Documents\\TSGR1_100b\\Docs\\R1-2001793.zip) Remaining Issues on Sidelink Mode 2 Resource Allocation Panasonic Corporation

1. [R1-2001805](file:///C:\\Users\\wanshic\\OneDrive%20-%20Qualcomm\\Documents\\Standards\\3GPP%20Standards\\Meeting%20Documents\\TSGR1_100b\\Docs\\R1-2001805.zip) Remaining details of Resource allocation for sidelink - Mode 2 Nokia, Nokia Shanghai Bell

1. [R1-2001877](file:///C:\\Users\\wanshic\\OneDrive%20-%20Qualcomm\\Documents\\Standards\\3GPP%20Standards\\Meeting%20Documents\\TSGR1_100b\\Docs\\R1-2001877.zip) Remaining details on mode 2 resource allocation for NR V2X Fujitsu

1. [R1-2001886](file:///C:\\Users\\wanshic\\OneDrive%20-%20Qualcomm\\Documents\\Standards\\3GPP%20Standards\\Meeting%20Documents\\TSGR1_100b\\Docs\\R1-2001886.zip) Discussion on resource allocation for Mode 2 LG Electronics

1. [R1-2001896](file:///C:\\Users\\wanshic\\OneDrive%20-%20Qualcomm\\Documents\\Standards\\3GPP%20Standards\\Meeting%20Documents\\TSGR1_100b\\Docs\\R1-2001896.zip) Remaining issues of mode 2 operation on sidelink ZTE, Sanechips

1. [R1-2001907](file:///C:\\Users\\wanshic\\OneDrive%20-%20Qualcomm\\Documents\\Standards\\3GPP%20Standards\\Meeting%20Documents\\TSGR1_100b\\Docs\\R1-2001907.zip) Sidelink mode-2 resource allocation MediaTek Inc.

1. [R1-2001964](file:///C:\\Users\\wanshic\\OneDrive%20-%20Qualcomm\\Documents\\Standards\\3GPP%20Standards\\Meeting%20Documents\\TSGR1_100b\\Docs\\R1-2001964.zip) Resource allocation for NR sidelink Mode 2 TCL Communication Ltd.

1. [R1-2001969](file:///C:\\Users\\wanshic\\OneDrive%20-%20Qualcomm\\Documents\\Standards\\3GPP%20Standards\\Meeting%20Documents\\TSGR1_100b\\Docs\\R1-2001969.zip) Discussion on resource allocation for NR sidelink Mode 2 Lenovo, Motorola Mobility

1. [R1-2001978](file:///C:\\Users\\wanshic\\OneDrive%20-%20Qualcomm\\Documents\\Standards\\3GPP%20Standards\\Meeting%20Documents\\TSGR1_100b\\Docs\\R1-2001978.zip) Remaining Issues in Resource Allocation for Mode 2 NR V2X Fraunhofer HHI, Fraunhofer IIS

1. [R1-2001994](file:///C:\\Users\\wanshic\\OneDrive%20-%20Qualcomm\\Documents\\Standards\\3GPP%20Standards\\Meeting%20Documents\\TSGR1_100b\\Docs\\R1-2001994.zip) Solutions to remaining opens of resource allocation mode-2 for NR V2X sidelink design Intel Corporation
2. [R1-2002041](file:///C:\Users\wanshic\OneDrive%20-%20Qualcomm\Documents\Standards\3GPP%20Standards\Meeting%20Documents\TSGR1_100b\Docs\R1-2002041.zip) Remianing details on mode-2 resource allocation Futurewei

1. [R1-2002078](file:///C:\\Users\\wanshic\\OneDrive%20-%20Qualcomm\\Documents\\Standards\\3GPP%20Standards\\Meeting%20Documents\\TSGR1_100b\\Docs\\R1-2002078.zip) Remaining issues on Mode 2 resource allocation in NR V2X CATT

1. [R1-2002126](file:///C:\\Users\\wanshic\\OneDrive%20-%20Qualcomm\\Documents\\Standards\\3GPP%20Standards\\Meeting%20Documents\\TSGR1_100b\\Docs\\R1-2002126.zip) On Mode 2 for NR Sidelink Samsung

1. [R1-2002234](file:///C:\\Users\\wanshic\\OneDrive%20-%20Qualcomm\\Documents\\Standards\\3GPP%20Standards\\Meeting%20Documents\\TSGR1_100b\\Docs\\R1-2002234.zip) Resource allocation Mode 2 for NR SL Ericsson

1. [R1-2002267](file:///C:\\Users\\wanshic\\OneDrive%20-%20Qualcomm\\Documents\\Standards\\3GPP%20Standards\\Meeting%20Documents\\TSGR1_100b\\Docs\\R1-2002267.zip) Remaining issues in NR sidelink mode 2 resource allocation Spreadtrum Communications

1. [R1-2002301](file:///C:\\Users\\wanshic\\OneDrive%20-%20Qualcomm\\Documents\\Standards\\3GPP%20Standards\\Meeting%20Documents\\TSGR1_100b\\Docs\\R1-2002301.zip) Remaining Issues on NR Sidelink Mode 2 Resource Allocation InterDigital, Inc.

1. [R1-2002325](file:///C:\\Users\\wanshic\\OneDrive%20-%20Qualcomm\\Documents\\Standards\\3GPP%20Standards\\Meeting%20Documents\\TSGR1_100b\\Docs\\R1-2002325.zip) On Remaining Details of Mode 2 Resource Allocation Apple

1. [R1-2002362](file:///C:\\Users\\wanshic\\OneDrive%20-%20Qualcomm\\Documents\\Standards\\3GPP%20Standards\\Meeting%20Documents\\TSGR1_100b\\Docs\\R1-2002362.zip) Remaining issues on resource allocation Mode 2 NEC

1. [R1-2002388](file:///C:\\Users\\wanshic\\OneDrive%20-%20Qualcomm\\Documents\\Standards\\3GPP%20Standards\\Meeting%20Documents\\TSGR1_100b\\Docs\\R1-2002388.zip) Remaining issues on resource allocation mode 2 for NR sidelink Sharp

1. [R1-2002402](file:///C:\\Users\\wanshic\\OneDrive%20-%20Qualcomm\\Documents\\Standards\\3GPP%20Standards\\Meeting%20Documents\\TSGR1_100b\\Docs\\R1-2002402.zip) On resource reservation in Mode 2 resource allocation Xiaomi Communications

1. [R1-2002439](file:///C:\\Users\\wanshic\\OneDrive%20-%20Qualcomm\\Documents\\Standards\\3GPP%20Standards\\Meeting%20Documents\\TSGR1_100b\\Docs\\R1-2002439.zip) Remaining issues on resource allocation mechanism mode 2 NTT DOCOMO, INC.
2. [R1-2002487](file:///C:\Users\wanshic\OneDrive%20-%20Qualcomm\Documents\Standards\3GPP%20Standards\Meeting%20Documents\TSGR1_100b\Docs\R1-2002487.zip) Remain details on mode-2 resource allocation for NR V2X ITL
3. [R1-2002489](file:///C:\Users\wanshic\OneDrive%20-%20Qualcomm\Documents\Standards\3GPP%20Standards\Meeting%20Documents\TSGR1_100b\Docs\R1-2002489.zip) Remaining issue for Mode 2 resource allocation in NR V2X ASUSTeK

1. [R1-2002539](file:///C:\\Users\\wanshic\\OneDrive%20-%20Qualcomm\\Documents\\Standards\\3GPP%20Standards\\Meeting%20Documents\\TSGR1_100b\\Docs\\R1-2002539.zip) Sidelink Resource Allocation Mechanism for NR V2X Qualcomm Incorporated