Rel-16 5G V2X maintenance email discussion topics

* Thread 1: Remaining issues for PT-RS design
  + Issue PS-1-1: For PT-RS sequence generation, when r(m) is defined, which DM-RS symbol is used for reference is not clear.
  + Issue PS-1-2: Removal of duplication for PT-RS mapping
* Thread 2: Location of PSFCH/PSSCH/PSCCH/2nd SCI mapping
  + Issue PS-2-1: To clarify starting symbol and location for PSFCH
  + Issue PS-2-2: To clarify time-domain location of PSSCH
  + Issue PS-2-3: To clarify time-domain and frequency-domain location of PSCCH
  + Issue PS-2-4: To modify the amount of resources for 2nd SCI rate matching
* Thread 3: The outstanding agreement from RAN1#102-e on the minimum gap between PSFCH and next SL retransmission.
  + Issue M1-1-1: Conditions for applicability
  + Issue M1-1-2: Value of delta
* Thread 4: Re-evaluation procedure for periodic resource reservations
  + Issue M2-1: Fix undefined UE behaviour for the case of re-evaluation performed during periodic reservation process
* Thread 5: Indication/derivation of TDD configuration.
  + Issue SY-1-1: TDD configuration derivation
  + Issue SY-1-2: TDD configuration for OoC UEs
  + Issue SY-1-3: Indication of the non-TDD case in sl-TDD-config
  + Also include Issue SY-3 Timing determination for NR V2X when the CR is prepared
* Thread 6: Remaining issues in prioritization between SL and UL
  + Issue PP-2: Prioritization rule between PSCCH/PSSCH and PUCCH without SL HARQ reports/PUSCH without UL-SCH/SRS
  + Issue PP-3: Prioritization rule between PSFCH/S-SSB reception(s) and UL transmission(s)
  + Issue PP-4: MsgA PUSCH is prioritized over SL transmission
* Thread 7: Clarification on the sidelink slot index
  + Issue PP-7: Clarification on the logical slot set for resource allocation procedure
  + Issue M2-6: Logical slot index vs physical slot index for slots where candidate set is determined