3GPP TSG RAN WG1 #104-e R1-21xxxxx

e-Meeting, January 25th – February 5th, 2021

**Agenda item: 7.2.10**

**Source: Moderator (Nokia)**

**Title: [104-e-NR-MRDC-CA-02] Email discussion/approval on cross-carrier triggering scheduling and A-CSI RS triggering, and unaligned**

**Document for: Discussion and Decision**

Table of Contents

[1 Introduction 1](#_Toc62485352)

[2 Summary of issues addressed in the Tdocs 2](#_Toc62485353)

[2.1 Cross-carrier scheduling and A-CSI RS triggering 2](#_Toc62485354)

[2.2 Unaligned CA 2](#_Toc62485355)

[3 Conclusions 3](#_Toc62485356)

# 1 Introduction

The RAN1#104-e preparation for Rel-16 MR-DC/CA work item conclusion is captured in R1-2101792. Based on that the email thread #2 was kicked off as follows:

[104-e-NR-MRDC-CA-02] Email discussion/approval on cross-carrier triggering scheduling and A-CSI RS triggering, and unaligned CA until 10/29 – Karri (Nokia)

* XCC-1: Proposal 1 in R1-2100585
* XCC-2: Proposal 3 in R1-2100585
* XCC-3 (could be discussed with XCC-1): Proposal 2 in R1-2101443
* CA-1: Proposal (for conclusion) in R1-2101553 and Proposals 2 and 3 in R1-2100420
* CA-2: Proposals 4 and 5 in R1-2100420

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **TDoc** | **Title** | **Source** | **X-CC** | **Unal. CA** | **Issue tags** |
| [R1-2100420](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_104-e/Docs/R1-2100420.zip) | Maintenance on MR-DC and CA enhancements | vivo |  | x | CA-1, CA-2 |
| [R1-2100585](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_104-e/Docs/R1-2100585.zip) | Remaining issues on Rel-16 carrier aggregation | MediaTek | x |  | XCC-1, XCC-2 |
| [R1-2101443](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_104-e/Docs/R1-2101443.zip) | Remaining issues on SCell dormancy and cross-carrier scheduling | Qualcomm | x |  | XCC-3 |
| [R1-2101553](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_104-e/Docs/R1-2101553.zip) | Maintenance for Rel-16 MR-DC and CA enhancements | Ericsson |  | x | CA-1 |

# 2 Summary of issues addressed in the Tdocs

# 2.1 Cross-carrier scheduling and A-CSI RS triggering

|  |  |  |  |
| --- | --- | --- | --- |
| **Issue** | **TDoc** | **Issue** | **Moderator comment** |
| XCC-1 | [R1-2100585](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_104-e/Docs/R1-2100585.zip) | Proposal 1: To align the RAN1 #99 agreement for cross-carrier scheduling as mentioned above, adopt the following TP to 38.214 Section 5.1.5 where the additional beam switching timing (d) is added without connection to the default beam behavior: | Both documents address the same issue. TP in ‘0585 seems to be based on the old version of the specification and is more intrusive that the one in ‘1443 |
| XCC-3 | [R1-2101443](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_104-e/Docs/R1-2101443.zip) | Proposal 2: Adopt a TP for cross-carrier beam switching time for TS 38.214 subclause 5.1.5 moving the “the UE is configured with *enableDefaultBeam-ForCCS*“ condition to a sub-bullet |
| XCC-2 | [R1-2100585](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_104-e/Docs/R1-2100585.zip) | Proposal 3: Add the following two sentences from R15 38.214 5.2.1.5.1 to the R16 newly added sections in 38.214 5.2.1.5.1a, since they are general behaviour defined for “Aperiodic CSI Reporting”/”Aperiodic CSI-RS triggering”:   * A UE is not expected to receive more than one DCI with non-zero CSI request per slot. * A UE is not expected to receive more than one aperiodic CSI report request for transmission in a given slot. | The restriction is already covered by 5.2.1.5.1a as it specifically starts with this sentence:  *When the triggering PDCCH and the triggered aperiodic CSI-RS are of different numerologies, the behavior defined in 5.2.1.5.1 for the case where the numerologies are the same applies with the following exceptions:*  And there are no exceptions made on these points. Hence they apply as is, and there is no need to replicate them in 5.2.1.5.1a |

**Moderator proposal:**

* For XCC-1/XCC-3: Agree that a change is needed, develop a TP using the proposal in R1-2101443 as the starting point.
* For XCC-2: The suggested change is not needed as the indicated text is already inherited as-is from 5.2.1.5.1 to 5.2.1.5.1a.

Please add company comments on the proposal above

|  |  |  |
| --- | --- | --- |
| **Company** | **Issue** | **Comment** |
| ZTE | **XCC-1,2,3** | OK with the moderator’s proposal. |
| Huawei | **all** | Support moderator proposal |
| NTT DOCOMO | **XCC-1/3**  **XCC-2** | We are fine with moderator proposal. |
| vivo | **XCC-1, 2, and 3** | Ok with moderator’s proposal. |
| MTK | **All** | Support moderator proposal |

# 2.2 Unaligned CA

|  |  |  |  |
| --- | --- | --- | --- |
| **Issue** | **TDoc** | **Issue** | **Moderator comment** |
| CA-1 | [R1-2101553](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_104-e/Docs/R1-2101553.zip) | Proposal (for conclusion):   * It is RAN1 understanding that, at most single non-zero offset duration (independent on SCS) can be configured among CCs of a CG in the unaligned CA configuration. | The two contributions are in disagreement on whether the limitation to a single offset should apply across all CCs, or across CCs per CG. |
| CA-1 | [R1-2100420](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_104-e/Docs/R1-2100420.zip) | Proposal 2: RAN1 should clarify that at most one non-zero CA offset across cell groups can be configured for a UE supporting capability 18-7.  Proposal 3: If more than one non-zero offsets are required, a separate UE capability from 18-7 should be introduced for such kind of Ues. |
| CA-2 | [R1-2100420](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_104-e/Docs/R1-2100420.zip) | Proposal 4: NR DC is considered synchronous with slot offset if all the cells are slot boundary aligned and the number of slot offsets between cells are not more than one.  Proposal 5: NR DC is considered asynchronous with slot offset if MCG and SCG are not slot boundary aligned and the number of slot offsets between cells are not more than one, or all the cells are slot boundary aligned with two non-zero slot offsets among cells. | Proposal 4 seems clear, but is this needed in addition to what is already said after CA-1 is resolved?  Proposal 5: this would seem redundant if there is a resolution to the CA-1. Further, it is not clear if the proponent means that the “two non-zero offsets” can be different. |

**Moderator proposal:** (taking the discussion of RAN1#103-e into consideration, see R1-2009810)

* For CA-1:
  + Agree that the CA configuration applies per CG, i.e. adopt proposal 1 of R1-2101553
  + Discuss if there is a strong need to split the capability 18-7 to differentiate between one offset over all CCs and one offset over CCs per CG
* For CA-2:
  + Agree to capture proposal 4 of R1-2100420 in the chairman’s notes.

Please add company comments on the proposal above

|  |  |  |
| --- | --- | --- |
| **Company** | **Issue** | **Comment** |
| ZTE  CMCC | **CA-1**  **CA-2**  **CA-1**  **CA-2** | We are fine with the proposal for CA-1. From our perspective, a UE feature to split the capability 18-7 to differentiate between one offset over all CCs and one offset over CCs per CG is necessary.  For CA-2, we have a different understanding. Since the synchronous and asynchronous NR-DC requirements are specified before the introduction of unaligned frame boundary, it is preferred to determine synchronous or asynchronous NR-DC before applying the slot offset in MCG and SCG. In other words, synchronous and asynchronous NR-DC is determined assuming there is no slot offset introduced by unaligned frame boundary.  We are fine the further clarification for the application of single non-zero offset as the proposal for CA-1, but on how to split the capability 18-7, to avoid intertangling the offsets of CA and DC, we are inclined to split the capability to differentiate between single CG with one non-zero offset and multiple CGs with individual non-zero offset.  For CA-2, we share the same understanding as ZTE in general, we should not mix the offset for CA and DC, however, we are open to further clarify the slot offset and non-slot offset capability of DC on top which the unaligned CA can be configured. |
| Huawei | **CA-1** | Support moderator proposal about CA-1. |
|  | **CA-2** | As for the DC consideration, we have different understanding from the proponent of CA-2. We think unaligned CA is only about sync-DC (but of course it can also be configured in async-DC), since no slot alignment between MCG and SCG is required for async-DC, and for sync-DC, misaligned frame boundary is ok and unknown/non-indicated to UE (only slot offset within a CG can be indicated to a UE). Thus the slot alignment requirements for unaligned CA naturally meet sync-DC requirement, and is not relevant for determining whether DC is sync-ed or not. |
| NTT DOCOMO | **CA-1**  **CA-2** | We are fine with the moderator proposal for CA-1.  For CA-2, our understanding is that sync or async DC is defined based on MTTD/MRTD conditions specified in TS38.133, i.e., irrespective of slot offset within a CG, if the case which cannot meet MTTD/MRTD condition for sync NR-DC can happen for the NR-DC, it would be async NR-DC and UE needs to support asyncNRDC-r16. |
| vivo | **CA-1** | We can agree the per-CG CA offset together with a UE capability. We are open to how to define the UE capability. |
| MTK | **CA-2**  **CA-1**  **CA-2** | We think the definition of synchronous and asynchronous in the case of unaligned CA should be clarified (clearly the companies’ views here are divergent according to the comments). Proposal 4 is one trial that may be acceptable in our view. But we are open on how to clarify.  For CA-1, we share the same view with vivo, that basic feature (18-7) is one offset across CG, and additional feature is required to split the capability 18-7 to differentiate between one offset over all CCs and one offset over CCs per CG  For CA-2, we tend to agree that sync or async DC is defined based on MTTD/MRTD conditions specified in TS38.133, i.e., irrespective of slot offset within a CG. We are open to further clarification. |

# 3 Conclusions

TBD