**3GPP TSG RAN WG1 #104-e R1-2101412**

**e-Meeting, January 25 – February 05, 2021**

**Source: Moderator (OPPO)**

**Title: FL summary for AI 8.11.1.1 – resource allocation for power saving**

**Agenda item: 8.11.1.1**

**Document for:** **Discussion and Decision**

Introduction

In the latest revised Rel-17 WID for NR sidelink enhancement [1], the objective for enhancing RA to reduce UE power consumption in mode 2 has been updated as followed.

|  |
| --- |
| 2. Resource allocation enhancement:* Specify resource allocation to reduce power consumption of the UEs [RAN1, RAN2]
	+ Baseline is to introduce the principle of Rel-14 LTE sidelink random resource selection and partial sensing to Rel-16 NR sidelink resource allocation mode 2.
	+ Note: Taking Rel-14 as the baseline does not preclude introducing a new solution to reduce power consumption for the cases where the baseline cannot work properly.
	+ This work should consider the impact of sidelink DRX, if any.
 |

This contribution provides a summary of the submitted contributions, email discussion topics and outcomes during RAN1#104-e meeting.

Collection of agreements / conclusion in RAN1#104-e

Agreements**:**

* Random resource selection is applicable to both periodic and aperiodic transmissions
	+ FFS conditions for random resource selection

**Conclusion:**

* PSFCH reception is not included for Type A UE
* S-SSB reception is not included for Type A UE
* SL reception Type B is additionally added
	+ Type B: Same as Type A with an exception of performing PSFCH and S-SSB reception
* Note: the same conditions as in RAN1#103-e regarding the context of the discussion of Type A and Type D still apply (also applicable to type B)

Topics for email discussion

[104-e-NR-R17-SL-01] Email discussion on resource allocation for power saving– Kevin (OPPO)

* 1st check point: Jan 28
* 2nd check point: Feb 2
* 3rd check point: Feb 4

## Topic #1: PSFCH and S-SSB reception for Type A UE

**Background**: In the last meeting RAN1#103-e, there was an FFS item on whether a Type A UE should be capable of performing PSFCH and S-SSB reception as an exception.

|  |
| --- |
| * + Type A: UE is not capable of performing reception of any SL signals and channels, FFS with exception of performing PSFCH and S-SSB reception (aim to conclude in RAN1#104-e)
 |

From reviewing contributions submitted to this meeting,

* Main reasons for not to support PSFCH reception for Type A UEs:
	+ Minimum reception capability, same as PUE in LTE-V
	+ Likely only perform broadcast transmissions as it cannot receive any data, and receiving HARQ feedback is not required in SL broadcast
* Main reason to support PSFCH reception was mainly to improve communication reliability
* The main reason not to support S-SSB reception was that the UE can always sync to network or GNSS timing, same as in LTE-V
* The main reason to support S-SSB reception was that S-SSB transmitted from UE synchronized to eNB/gNB is prioritized over GNSS

### Proposals before 1st check point (Jan 28)

**Proposal 1 (for conclusion):**

* PSFCH reception is not supported for Type A UE
* S-SSB reception is not supported for Type A UE
* SL reception Type B is additionally added
	+ Type B: Same as Type A with an exception of performing PSFCH and S-SSB reception

|  |  |
| --- | --- |
| **Company** | **Comments** |
| OPPO | Agree |
| Fraunhofer | Agree  |
| Apple | Agree |
| Ericsson | First of all, we would like to remark that the UE Type definition, i.e., A, D (or B), are not related to UE capabilities but just as a reference for evaluation and designing the power saving features.We do not think that having S-SSB reception support but not having PSFCH reception support is justified from a product perspective. If companies think that there should be a UE that is not capable of receiving any signal, we can be fine with an additional UE Type where neither S-SSB nor PSFCH can be received. Therefore, we are OK to define two types of UE, i.e., Type A and Type B as in proposal 1, to be used as a baseline to define and design power saving features. |
| CATT | Since these types are used as the reference for evaluation and designing of SL power saving features in R17, it’s better to add another type( B1 )which supports S-SSB reception but not PSFCH reception. |
| Qualcomm | We agree with the proposal and would like to reiterate that these types are only for evaluation and to facilitate discussion but do not define UE capabilities. |
| Lenovo&MM | Agree |
| CMCC | We are basically fine with this proposal. As per the conclusion made in the last meeting, these UE types were defined as the reference for evaluation, and have nothing to do with the UE capability covered by UE feature. From this perspective, we are ok to define Type A UE without any reception capability to obtain the lower bound of the power consumption level and the system performance level. On the other hand, it is mentioned that supporting the reception of PSFCH is beneficial for higher reliability, and supporting the reception of S-SSB allows the UE to synchronized to a cell or other reference UEs when GNSS is not available or reliable. To our understanding, this Type B UE is a special case of Type D UE. It seems optional to us; however, we do not have strong objections to define the Type B UE as a trade-off. |
| NEC | Agree |
| vivo | Agree with FL’s proposal |
| FUTUREWEI | Agree with proposals. The types discussed are for evaluations not for defining UE capabilities. For clarification, is the Type B listed above different from the Type B discussed in the previous meeting? |
| ETRI | Agree only for design of power saving features |
| Panasonic  | Agree with FL’s proposal for the purpose of evaluation.  |
| Sony | Agree with the proposal. |
| NTT DOCOMO | We are fine with the FL’s proposal, based on discussions in the last GTW session. From actual device perspective, no reception unit seems feasible for a P-UE. |
| CAICT | Agree  |
| Sharp | Agree with FL’s proposal. |
| Xiaomi | We are fine with FL’s proposal. |
| ZTE | Agree with FL’s proposal. |
| LGE | We’re fine with the FL proposal to separate Type A and Type B UE. Type A UE may represent the operation of LTE-V2X P-UE. For Type B UE, continual full S-SSB search may require significant power consumption. So we need to study more how to minimize the power consumption for S-SSB reception. The recommended proposal is as follows.**Proposal 1*** Type A UE supports neither PSFCH nor S-SSB reception
* Type B UE supports both PSFCH and S-SSB reception
	+ FFS whether/how to minimize power consumption for S-SSB reception
 |
| Samsung | Agree with FL’s proposal. |
| Fujitsu | Agree |
| MediaTek | We agree with FL’s proposal. |
| Intel | Agree with the first two bulletsFor the last bullet we disagree that Type-B is the same as Type A. In our opinion type B can also be viewed as a Type D UE that is configured to only receive PSFCH and S-SSB. Therefore we propose to replace the last bullet with the following text:FFS if Type B UE, that is capable to receive only PSFCH and SSB is needed, or this functionality can be considered as a part of Type-D UE operation |
| Huawei, HiSilicon | We wish to emphasise that the UE’s here are only “*reference UEs for the purpose of evaluation and design*” as agreed in 103e, and thus are *not* real UEs. The capabilities of real UEs will be decided at the end of the release. What we are discussing here is with reference to what the evaluations and designs will be considered, not what is inside any particular real UE. Thus the word “supported” leads to incorrect understandings. And the statement in the 3rd bullet that these are already SL reception types (seeming to write 38.202 already) leads to similar incorrect understandings. The structure of the proposal should be such as:For reference UEs:* PSFCH reception is not included for Type A UE
* S-SSB reception is not included for Type A UE
* Type B is additionally defined.
	+ Type B: Same as Type A with addition of PSFCH and S-SSB reception

We are OK with the basis of the proposal. Type A refers to the reception type which costs minimal power consumption, i.e. no reception behaviour at all. This serves as a lower bound for power consumption, which is informative. And this is also aligned with LTE-V. Introducing of Type B is fine, although we think Type-D UE has already covered Type-B UE reception behaviour. |
| Convida Wireless | We are generally ok with the FL’s proposal. |
| Bosch | We also see that it should not take us too long to discuss UE capability at this point. For the reference UE (for evaluation purpose), we support the FL proposal. We also prefer Huawei’s suggestion to replace “supported” 🡪 “included”. This will let us clearly focus on the actual role of these reference Types A, B, & D. |
| Nokia, NSB | Ok. |

## Topic #2: Periodic-based partial sensing (determination of Y candidate slots for periodic transmission)

**Background**:



Figure 1

In R14 LTE sidelink, the partial sensing scheme is optimized for periodic traffic type only, where

* UE performs monitoring of subframes in sensing occasions according to $t\_{y-k×P\_{step}}^{SL}$ for a set of Y candidate subframes determined within the resource selection window
* The smallest denominator was set to 100ms for Pstep and 20/50ms reservation periodicities were not taken into consideration.
* Period sensing occasions within the sensing window are determined by the kth bit of the higher layer parameter *gapCandidateSensing*.

From reviewing contributions submitted in this meeting, the above Rel-14 LTE sidelink partial sensing scheme can be taken as the baseline, but some enhancements are needed for a power constrained UE configured with partial sensing to perform periodic transmission in NR sidelink mode 2. First of all, it is aimed to confirm the same principle as in LTE-V that a UE first determines a set of Y candidate slots within the resource selection window when resource selection is triggered in slot n.

### Proposal before 1st check point (Jan 28)

**Proposal 2**: If UE is configured to perform partial sensing and provided with a resource reservation interval ($P\_{rsvp\\_TX}$) from higher layer, it is up to UE implementation to determine Y candidate slots within a resource selection window, where

* The resource selection window $[n+T\_{1},n+T\_{2}]$ is defined in the same way as in R16 NR-V2X according to step 1 [TS 38.214 Sec. 8.1.4].
* UE determination of Y candidate slots should exclude slots in which its own SL and UL transmissions occur in the resource selection window.
* Due to integer multiple of resource reservation periods, UE determination of Y candidate slots should exclude slots that would coincide with its own SL and UL transmissions within the corresponding periodic sensing occasions.
* Periodic sensing occasions that correspond to the set of Y candidate slots should align with the SL-DRX ON duration as much as possible (if configured) and/or as early as possible to maximize number of contiguous sensing slots before the resource selection trigger in slot n.
* FFS min and max Y candidate slots should be applied (e.g., a range of Y values per priority level)

|  |  |
| --- | --- |
| **Company** | **Comments** |
| OPPO | We are OK with the 1st sub-bullet. Not support for the other bullets* For the 2nd and 3rd bullet: UE should not exclude the slot that is used for UL transmission. Whether to prioritize between UL and SL is up to UE hardware implementation. If there are two sets of RF, UE can transmit UL and SL (if they are in different carrier) at the same time, in that case, there is no necessary to exclude the slots for UL transmission. In legacy resource exclusion procedure of sensing, only the slots for SL transmission is considered, not for UL transmission. We suggest to follow legacy behaviour.
* For the 4th bullet: the relationship between DRX and sensing is discussing in another email thread [104-e-NR-R17-SL-LS-01], it is not necessary to discuss that here again.
* For the last bullet: in LTE-V2X, only min Y slots was applied. We are not convinced to apply max Y slots. No intension to introduce additional feature unless performance gain can be justified.
 |
| Fraunhofer | For the determination of the selection window for periodic transmissions, we prefer to stick to the same procedure as defined in Rel-16. Exclusions based on UL transmissions can be left out.We agree that the candidate slots should align with the DRX ON duration as much as possible. |
| Apple | We are fine with the main bullet and the first sub-bullet. For the second and third sub-bullets, we share the views from OPPO that only SL transmissions slots should be considered. The prioritization between SL and UL can be handled separately with the existing R-16 rule. For the fourth sub-bullet, we are fine in general. But some clarification is needed, such as how to quantify “as much as possible”, “as early as possible”?For the fifth sub-bullet, we think only the lower bound on Y can be applied, and we do not mention the example that range of Y is per priority level.  |
| Ericsson | We do not see the need to introduce a new scheme for periodic transmissions. We propose to reuse the LTE mechanism (where the 2nd and 3rd sub-bullets do not need to be specified and can be left to UE implementation) and discuss the potential enhancements needed to address the periodicities introduced in NR (see Section 3.3.1) and any other potential issue.We have two comments regarding the sub-bullet on DRX. First, it is probably a good idea to leave the discussion for later, when more about the DRX procedure is known. In general, a wider discussion on the connection between SL DRX and partial sensing has to take place. Besides that, we believe that aspects may be left to UE implementation, like for the other bullets. |
| InterDigital | When SL DRX is not configured, we agree that determination of Y can be UE’s implementation. But when SL DRX is configured, Y should be selected based on the DRX ON duration of the reception UE(s) which is the target of the transmission, instead of the UE itself. * For the 2nd and 3rd, we prefer to reuse the R16 procedure, in which SL Tx slots can be considered but not UL slots.
* We agree with the principle of the 4th bullet that periodic sensing should align with the SL DRX ON duration as much as possible (if configured).
* For the 5th bullet, we do not see the motivation to consider Y max.

We assume that this proposal is applicable to the first TB of periodic traffic.* $P\_{rsvp\\_TX}$ should be greater than 0ms.
 |
| CATT | In principle we should reuse Rel-16 procedure as much as possible. For this particular proposal, we don’t agree with the sub-bullet regarding DRX alignment. In fact, it’s more efficient that sensing operation is allowed in SL DRX inaction duration without the restriction of its own SL DRX configuration. We should discuss the details related to DRX issue. |
| Qualcomm | We think that we need to discuss the different scenarios (Tx UE doing power savings, Rx UE doing power savings, or both UEs) and then discuss the general design(s) with evaluation results prior to discussing this level of detail.For example, if the transmitter isn’t receiving data, e.g. P2V-only application, then it isn’t clear why some of the points would apply, e.g. the one about DRX.Similarly, when both UEs are doing power savings, it is more efficient to fully align their DRX and partial sensing windows.We should also consider whether some aspects need to specified or can be left up to UE implementation. |
| Lenovo&MM | Rel-14 LTE sidelink partial sensing scheme can be taken as the baseline and select the resource(s) for periodic transmission. FFS, the sensing scheme for aperiodic transmissionThe relationship between partial sensing and SL DRX on duration should be further clarified such that the partial sensing slots are defined by the partial sensing configuration or SL DRX on duration.  |
| CMCC | We have concerns regarding the 2nd, 4th and last bullets. For the 2nd bullet, in LTE-V, the determination of Y candidate slots is up to UE implementation as long as Y is higher than the (pre-)configured higher layer parameter *minNumCandidateSlot*. The intention of introducing additional rules is not clear to us.For the 4th bullet, regarding the alignment of DRX ON duration and the sensing occasion, we think that the relationship of SL DRX pattern with the sensing window and resource selection window, e.g., whether they are configured and performed independently, or configured independently but the sensing and selection should be performed during ON duration, or aligned as much as possible by configuration, should be separately discussed.For the last bullet, we are ok to discuss per priority level configured Y value, however, we still think that the principle of minimum values should be kept.  |
| NEC | Main bullet: Fine, as the main bullet is reusing the principle of LTE, we are OK with it.* 1st sub-bullet: OK
* 2nd and 3rd sub-bullet: Are the intention to exclude slots that will be used for UE's future transmissions? Besides, as an exclusion set, we think Y should also exclude the resources reserved by hypothetical SCI in non-monitored slots, because these resources will not be excluded if they are selected as candidate slots in legacy Rel.14 partial sensing (step 5 is not performed).
* 4th sub-bullet: we are not sure whether "periodic sensing occasions" will exist in NR partial sensing. Periodic sensing occasions apply to LTE partial because the allowed periods are in periodic manner e.g., 100,200…1000. But for NR, as explained in the background of next topic, if the considered periods include e.g., 99ms, 97ms, etc., the whole sensing occasions will not be periodic.

5th sub-bullet: min Y candidate slots configured from higher layer is enough and we can FFS the details for Y's configuration |
| vivo | 1. Same view as OPPO. UE may perform priority comparison between UL and SL, and may drop the UL transmission in some cases, there is no need to exclude the UL slots from the window in advance.
2. We agree that the periodic sensing occasion should align with the DRX ON duration as much as possible, however, how to achieve this should not be up UE implementation and needs further discussion. so we would like to remove ‘up to UE implementation’ from the main bullet and add a FFS point on the determination of Y
3. minY is to avoid high collision probability, the benefit of setting a maximum value for Y is not clear.

**Proposal 2**: If UE is configured to perform partial sensing and provided with a resource reservation interval ($P\_{rsvp\\_TX}$) from higher layer, ~~it is up to UE implementation to~~ UE should determine Y candidate slots within a resource selection window, where* The resource selection window $[n+T\_{1},n+T\_{2}]$ is defined in the same way as in R16 NR-V2X according to step 1 [TS 38.214 Sec. 8.1.4].
* UE determination of Y candidate slots should exclude slots in which its own SL ~~and UL transmissions~~ occur in the resource selection window.
* Due to integer multiple of resource reservation periods, UE determination of Y candidate slots should exclude slots that would coincide with its own SL ~~and UL transmissions~~ within the corresponding periodic sensing occasions.
* Periodic sensing occasions that correspond to the set of Y candidate slots should align with the SL-DRX ON duration as much as possible (if configured) and/or as early as possible to maximize number of contiguous sensing slots before the resource selection trigger in slot n.
* FFS min ~~and max~~ Y candidate slots should be applied (e.g., a range of Y values per priority level)

FFS how to determine the Y candidate slots |
| FUTUREWEI | * First bullet: ok
* Second bullet: ok. A question about the wording. In 38.214, step 2 of clause 8.1.4 states “…The UE shall monitor slots which can belong to a sidelink resource pool within the sensing window except for those in which its own transmissions occur. …” To be consistent with the spec, perhaps the adjectives “SL and UL” can be removed
* Third bullet: unclear if needed. Its wording effectively encompasses the wording of the second bullet
* Fourth bullet: ok.
 |
| ETRI | We agree with other companies’ concerns, i.e., no need to exclude UL transmission and define max Y. Rel-14 LTE sidelink partial sensing scheme can be reused as much as possible with additional consideration of SL DRX. |
| Panasonic | We agree the main and the 1st sub-bullet. For the 2nd and the 3rd sub-bullets, we think these can up to implementation.For the 4th sub-bullet, we are generally fine with the principle and we think it should be separately discussed. Also, it’s hard to understand how to determine “as much as possible (if configured) and/or as early as possible”For the 5th sub-bullet, we propose to reword as “FFS details of Y candidate slots (e.g., …)” |
| Sony | We think we should reuse the existing scheme for periodic traffic basically. For the 2nd and 3rd sub-bullet, only SL transmission should be excluded from the candidate slots.On the sidelink DRX in 4th sub-bullet, we are basically OK with aligning sensing operation with the sidelink DRX configuration. But “as much as possible” and “as early as possible” are unclear. We need to further discuss the details. |
| NTT DOCOMO | * Main bullet: intention of ‘provided with a resource reservation interval ($P\_{rsvp\\_TX}$) from higher layer’ is unclear for us. Only for periodic transmission from the UE performing partial sensing? If correct, one comment: $P\_{rsvp\\_TX}$ = 0 means aperiodic transmission. Is it OK to include this case?
* 1st bullet: OK
* 2nd bullet: ‘UL’ is unnecessary as some companies mentioned above.
* 3rd bullet: ‘UL’ is unnecessary as some companies mentioned above. In addition, ‘Due to integer multiple of resource reservation periods’ is unclear for us. ‘resource reservation periods’ means resource reservation periods configured to the resource pool, right? This should be clarified. At last, ‘the corresponding periodic sensing occasion’ is completely FFS and discussed in the next section, right? If correct, this FFS should be added as sub-bullet.
* 4th bullet: ‘as much as possible’ is unclear for us. RAN1 will discuss further for this or up to UE? Similarly, ‘as early as possible’ is also. Postponing discussion for DRX is fine for us.
* 5th bullet: range restriction of Y value should be the same as LTE. Different mechanism would be unnecessary.
 |
| CAICT | Generally we agree with the proposal. For the 2nd and 3rd sub-bullets, the prioritization between the SL and UL transmissions should be considered when to exclude the occasions colliding with the candidate resources.  |
| Sharp | In our view it is possible that the use of partial sensing is not “semi-static” (for example, it may depend on whether partial sensing is enabled in the selected resource pool), so the first sentence in the main bullet should simply say “For partial sensing, …”. And this comment applies to other proposals in this document as well.Details in sub-bullets 2, 3, and 4 are premature at the moment. For sub-bullet 5, it may be better to just say “FFS restriction on values of Y”.Besides, considering both pre-emption check and re-evaluation are supported for partial sensing, selecting Y slots only by UE implementation is not enough, the selected Y slots should include at least $(r\_{0},r\_{1},r\_{2},…) $and $(r\_{0}^{'},r\_{1}^{'},r\_{2}^{'},…)$ subject to re-evaluation and pre-emption check respectively, instead of up to UE implementation only. |
| Xiaomi | In LTE V2x partial sensing treats periodic and aperiodic traffic in the same way. Therefore, we would like to clarify why only periodic traffic is considered in the main bullet.In addition, in LTE V2x, the determined Y candidate subframes must satisfy the corresponding sensing requirement, i.e. UE must guarantee that it has sensed in the corresponding subframes for each candidate subframe. However, from the current wording of main bullet, it seems that the Y candidate slots can be arbitrarily selected. Therefore we suggest to clarify this in the main bullet.In subbullet 1 there is n but it is not defined. In main bullet it should state “when resource selection is triggered in slot n, ……”Sub-bullet 2,3,4 propose some additional constraints on determining Y candidate slot. A word “periodic sensing occasion” appears in 3rd and 4th sub-bullet, but it has not been defined in LTE V2x or previous agreement. If it is related to the discussion of what kind of sensing requirement should be satisfied, we suggest to delay the discussion after making decision in that topic, or use some other words to replace it.For subbullet 4, it is not clear whether SL-DRX on duration is of Tx UE or Rx UE. We understand the motivation if it is of Rx UE, but still think it can be discussed after we define the sensing requirement for partial sensing.  |
| ZTE | For the second and third bullet, from our understanding, UE is not capable to know when its uplink transmission scheduling would be when performing sensing. Thus, it is hard for UE to exclude uplink slot during sensing duration. However, the collision between sidelink transmission and uplink transmission should be solved by other approaches. For the forth bullet, we should firstly discuss the relationship between sidelink DRX and partial sensing, and then go into such detailed discussion. |
| LGE | We think the resource selection procedure based on partial sensing can be improved for power saving. For example, if short-term sensing is used for resource re-evaluation or pre-emption checking, the longer interval between the selected resources, the more STS power is consumed due to longer sensing duration. If the intervals between the selected resources are short, the overall STS duration becomes shorter and the power consumption is minimized. Therefore, the adjacent resources are prioritized for resource selection over the distributed resources. For this, the selection window length needs to be (pre-)configured as short.In this sense, the following modifications are proposed for the bullets.* 1st bullet is modified as follows.

The resource selection window [n+T1, n+T2] is randomly selected by UE while satisfying:* + T1 ≥ 0 and T2 *≤* remaining PDB
	+ T2-T1 *≤* (pre-)configured threshold
* Clarifications on 2nd and 3rd bullet are need. Any slots not monitored by UE due to SL transmission are excluded from Y candidate slots.
* 4th bullet is removed. DRX operation and sensing are independent operation, and they don’t need to be correlated. According to main sentence, as candidate slots thereby partial sensing slots are determined by UE implementation, the alignment between partial sensing slot and DRX on duration cannot be specified.
* 5th bullet is modified as follows.

FFS whether min and max Y candidate slots are applied (e.g., a range of Y values per priority level) |
| Samsung | For the determination of selection window and candidate slots, we prefer to reuse legacy LTE and NR Rel-16 procedure as much as possible. Therefore 1st bullet seems OK for us, but for 2nd and 3rd bullets, we agree with other companies’ concern on excluding UL transmission.We agree with 4th bullet in principle, but current wording may lead to ambiguity. We suggest to discuss DRX related details as a separate issue. |
| Fujitsu | We think that we need to discuss firstly which is the base to design the sensing scheme: the traffic type that the UE is about to transmit or the traffic type(s) that is ongoing in the resource pool. We prefer to design the sensing scheme based on the ongoing traffic type(s) in the resource pool. To sense other UE’s periodic reservations, Rel.14 LTE partial sensing mechanism can be reused.* For the 2nd and 3rd bullet, it is not necessary to exclude UL slots from the Y candidate slots.
* Regarding the 4th bullet, it is not relevant with the determination of Y candidate slots. It seems that it is overlapped with section 3.3. In addition, clarification of “as early as possible” is needed. For the alignment of sensing occasions and DRX on duration, we share the same view as OPPO that it is under discussion in another email thread [104-e-NR-R17-SL-LS-01], we do not need to discuss it here.
* For the 5th bullet, we are fine to configure min Y values per priority level. In addition of priority level, other factors can also be considered, such as whether HARQ feedback is enabled or disabled.
 |
| MediaTek | We are OK with the 1st, 2nd, and 3rd sub-bullets. NR-SL partial sensing should follow LTE-SL design. We also agree with the 4th sub-bullet in principal.For the 5th sub-bullet, we don’t see a need to include max of Y. As mentioned in the main bullet of the proposal, it’s up to UE implementation to select Y slots. In LTE-SL, UE can select a minimum of Y subframes, but max is not needed. We suggest the following change:**Proposal 2**: If UE is configured to perform partial sensing and provided with a resource reservation interval ($P\_{rsvp\\_TX}$) from higher layer, it is up to UE implementation to determine at least Y candidate slots within a resource selection window, where* The resource selection window $[n+T\_{1},n+T\_{2}]$ is defined in the same way as in R16 NR-V2X according to step 1 [TS 38.214 Sec. 8.1.4].
* UE determination of Y candidate slots should exclude slots in which its own SL and UL transmissions occur in the resource selection window.
* Due to integer multiple of resource reservation periods, UE determination of Y candidate slots should exclude slots that would coincide with its own SL and UL transmissions within the corresponding periodic sensing occasions.
* Periodic sensing occasions that correspond to the set of Y candidate slots should align with the SL-DRX ON duration as much as possible (if configured) and/or as early as possible to maximize number of contiguous sensing slots before the resource selection trigger in slot n.
* ~~FFS min and max Y candidate slots should be applied (e.g., a range of Y values per priority level)~~
 |
| Intel | We propose following modifications to FL proposal:**Proposal 2**: If UE ~~is configured to~~ performs partial sensing and provided with a resource reservation interval ($P\_{rsvp\\_TX}$) from higher layer, ~~it is up to UE implementation to determine Y candidate slots within a resource selection window, where~~* The resource selection window $[n+T\_{1},n+T\_{2}]$ is defined and determined by UE in the same way as in R16 NR-V2X according to step 1 [TS 38.214 Sec. 8.1.4].
* ~~UE determination of Y candidate slots should exclude slots in which its own SL and UL transmissions occur in the resource selection window.~~
* In our view the bullet above is a separate discussion topic and procedures defined in Rel.16 can be reused at least as a starting point.
* ~~Due to integer multiple of resource reservation periods, UE determination of Y candidate slots should exclude slots that would coincide with its own SL and UL transmissions within the corresponding periodic sensing occasions.~~
* In our view the bullet above is a separate discussion topic and procedures defined in Rel.16 can be used at least as a starting point.
* ~~Periodic sensing occasions that correspond to the set of Y candidate slots should align with the SL-DRX ON duration as much as possible (if configured) and/or as early as possible to maximize number of contiguous sensing slots before the resource selection trigger in slot n.~~
* We prefer to finalize details of partial sensing operation first and then discuss impact/interaction w/ SL-DRX .
* ~~FFS min and max Y candidate slots should be applied (e.g., a range of Y values per priority level)~~
* In our view, above bullet relates to resource selection window size determination which is not supposed to change comparing to Rel.16
 |
| Huawei, HiSilicon | For the main bullet, it can be understood that if the UE is configured to perform partial sensing in a resource pool, a UE can select resources based on the limited Y sensing slots. However, it is not clear the relationship between the provision of resource reservation interval and monitoring behaviour. A UE cannot predict the service type, aperiodic or periodic, for future packets, and so cannot know which slots would be part of partial monitoring. Although the procedure is not defined yet, this does mean the UE cannot know what to sense in the past for this periodic transmission to select resources. However, this part of the proposals does not seem to depend on needing any knowledge of Prsvp\_TX, so there is no need to use “provided with a resource reservation interval ($P\_{rsvp\\_TX}$)) from higher layer” as a condition for monitoring. The first sub-bullet is OK, as mode 2 RA sensing in Rel-16 should be reused as much as possible, and this includes resource selection window.For the second sub-bullet, the candidate slots should be the slots in a resource pool which has already excluded by applying the bitmap. It does not relate to UL transmission. How to choose Y candidate slots can be left to UE implementation, same as in LTE-V, e.g. exclude slots of its own SL transmissions and/or slots would coincide with its own SL transmissions due to resource reservation periods. Hence, both second and third sub-bullets can be up to UE implementation which is already covered by main bullet. These two sub-bullets are not needed.For the fourth sub-bullet, at this stage, RAN1 does not have a clear understanding on SL DRX (re-)configuration, of which design is under RAN2 discussion, as well as the relation between SL DRX and partial sensing configuration. RAN1 should focus on the basic and critical designs for partial sensing first and then consider the coordination of SL DRX and partial sensing. Taking this bullet later would allow a more meaningful agreement than “as much as possible”.We are OK with the fifth bullet. Therefore, the proposal should be modified as follows:**Proposal 2**: If UE is configured to perform partial sensing ~~and provided with a resource reservation interval (~~$P\_{rsvp\\_TX}$~~) from higher layer~~, it is up to UE implementation to determine Y candidate slots within a resource selection window, where* The resource selection window $[n+T\_{1},n+T\_{2}]$ is defined in the same way as in R16 NR-V2X according to step 1 [TS 38.214 Sec. 8.1.4].
* ~~The resource selection window~~ $[n+T\_{1},n+T\_{2}]$ ~~is defined in the same way as in R16 NR-V2X according to step 1 [TS 38.214 Sec. 8.1.4].~~
* ~~The resource selection window~~ $[n+T\_{1},n+T\_{2}]$ ~~is defined in the same way as in R16 NR-V2X according to step 1 [TS 38.214 Sec. 8.1.4].~~
* ~~Periodic sensing occasions that correspond to the set of Y candidate slots should align with the SL-DRX ON duration as much as possible (if configured) and/or as early as possible to maximize number of contiguous sensing slots before the resource selection trigger in slot n.~~
* FFS min and max Y candidate slots should be applied (e.g., a range of Y values per priority level)
 |
| Convida Wireless | The same procedure that are defined in Rel-16 should be reused. SL Tx slots can be considered but UL slots may not be considered. In addition, our view is that the candidate slots should align with the DRX ON duration as much as possible. |
| Bosch | We are fine with the main-bullet. If the proposal targets periodic resource /SPS sensing only, then we do not need to repeat Rel-16 sensing procedure again (i.e., Prsvp\_TX). We are also fine to remove this sentence completely to fit periodic and aperiodic sensing: “~~and provided with a resource reservation interval (~~$P\_{rsvp\\_TX}$~~) from higher layer~~” We agree with the 1st and the 5th sub-bullet. We agree with the majority of companies to delete 2nd, 3rd sub-bullets. We would like to postpone 4th sub-bullet until we discuss and agree on DRX design. |
| Nokia, NSB | For main bullet, suggest modification as shown below. *Proposal 2: If UE is configured to perform partial sensing ~~and provided with a resource reservation interval (~~*$P\_{rsvp\\_TX}$*~~) from higher layer~~, it is up to UE implementation to determine Y candidate slots within a resource selection window, …*We support the first sub-bullet and the 5th sub-bullet.We are not agreed with the 2nd, 3rd, and the 4th sub-bullets. For the 2nd and 3rd sub-bullets, there is no need to exclude the UL slots. The DRX issue in the 4th sub-bullet shall be discussed in somewhere else.  |

**Proposal 2’**: If UE is configured to perform partial sensing and provided with a resource reservation interval ($P\_{rsvp\\_TX}\ne 0$) from higher layer in slot n, it is up to UE implementation to determine Y candidate slots within a resource selection window, where

* The resource selection window $[n+T\_{1},n+T\_{2}]$ is defined in the same way as in R16 NR-V2X according to step 1 [TS 38.214 Sec. 8.1.4].
* FFS whether a range of minimum Y values is (pre-)configured per priority level as in LTE-V

|  |  |
| --- | --- |
| **Company** | **Comments** |
| OPPO | We are fine with main bullet and 1st sub-bullet. For the 2nd sub-bullet, we want to clarify that in LTE-V, the minimum Y is configured as follows, not configured per priority level. The intension to configure minimum Y per priority level is not clear. We prefer to take LTE-V mechanism as baseline. Then we suggest to remove “per priority level” in the sub-bullet.p2x-SensingConfig-r14 SEQUENCE { minNumCandidateSF-r14 INTEGER (1..13), gapCandidateSensing-r14 BIT STRING (SIZE (10)) } OPTIONAL, -- Need OR**Proposal 2’**: If UE is configured to perform partial sensing and provided with a resource reservation interval ($P\_{rsvp\\_TX}\ne 0$) from higher layer in slot n, it is up to UE implementation to determine Y candidate slots within a resource selection window, where* The resource selection window $[n+T\_{1},n+T\_{2}]$ is defined in the same way as in R16 NR-V2X according to step 1 [TS 38.214 Sec. 8.1.4].
* ~~FFS whether a~~ A range of minimum Y values is (pre-)configured ~~per priority level~~ as in LTE-V
 |
| LGE | R16 resource selection can be enhanced for power saving when partial sensing and additional short-term sensing (STS) to avoid collision with aperiodic traffic are used. The problem of R16 procedure to determine Y candidate slots is depicted in Fig 1. UE determines a selection window [n+T1, n+T2] within PDB and Y candidate slots. After identifying the idle resources among the candidate resources based on sensing, the idle resources are reported to MAC layer for final resource selection.If the selection window is chosen as wide, and the candidate resources are determined so that the interval between candidate resources is long (e.g. more than STS window length), the resultant total short-term sensing duration over the selected resources becomes quite long, as shown in Fig 1, which requires high power consumption. This is problematic for power saving UE.This high power consumption due to short-term sensing can be solved at the stage of determining the selection window and the Y candidate resources. If UE choose a shorter selection window, the candidate resources can also be determined within the short selection window. Then the STS windows prior to the selected resources significantly overlap each other, thus the total sensing duration will be very short, as shown in Fig 2. This will greatly save power in performing short-term sensing, compared to that required in the procedure depicted in Fig 1.With the observation above, we strongly recommend the group to consider the power saving benefit of this ‘burst-type’ resource selection for P-UE. Following the claimed advantage, we propose the following and hope FL to capture it for further discussion.**Proposal 2’**: If UE is configured to perform partial sensing and provided with a resource reservation interval ($P\_{rsvp\\_TX}\ne 0$) from higher layer in slot n, it is up to UE implementation to determine Y candidate slots within a resource selection window, where* The resource selection window [n+T1, n+T2] is randomly selected by UE while satisfying:
	+ T1 ≥ 0 and T2 *≤* remaining PDB
	+ T2-T1 *≤* (pre-)configured threshold
* FFS whether a range of minimum Y values is (pre-)configured per priority level as in LTE-V
 |
| NEC | Regarding determination of Y, we think if it’s totally up to UE implementation will cause resource collision due to non-monitored slots and thus waste power for partial sensing UE. At this early stage of Rel.17, we have chance to do some enhancements just like want we done for full sensing in step 5.For the non-monitored slots, the specified way in LTE/NR full sensing is to exclude all the possible reserved resources with allowed reservation periods of the resource pool. i.e., step 5 is captured in full sensing to exclude the hypothetical reserved resources. However, step 5 is not performed in Rel.14 partial sensing. The selection of Y candidate resources within the selection window is up to UE implementation in current Rel.14 partial sensing specification. If we reuse the legacy procedure, as a consequence, UE has possibility to select all the slot as the candidate resources and will not exclude the collided slots reserved by others due to the non-monitored slots.Hence, we propose to add one sub bullet as * FFS any restrictions to determine Y candidate slots.

1st sub-bullet: ok2nd sub-bullet: We didn't observe that min Y is configured per priority in LTE-V and propose to delete "~~as in LTE-V~~". In addition, In LTE-V, the min selection window is [n+4,n+20] which contains at least 17 subframes, considering some subframes which the UE cannot monitor, it's feasible to set *minNumCandidateSF* as [1, 13] because even the largest candidate value 13 is less than the minimum resource selection window 17. In NR sidelink, the resource selection window size depends on subcarrier spacing configuration μ, RRC parameter T2\_min, remaining PDB and UE implementation. The minimum window size it’s no longer a fixed value as LTE sidelink. So we think the range of *minNumCandidateSF* in NR should be carefully designed and propose:FFS how to (pre-) configure the range of minimum Y values. e.g., consider priority level, resource selection window size, etc. |
| NTT DOCOMO | We support the proposal. Regarding how to determine Y, it is OK with up to UE implementation. UE can select Y slots so that power saving performance gets better if the UE want to do so. Even in any case of Y slot selection, resource collision is avoided by re-evaluation/pre-emption check. |
| Apple  | We think in LTE V2X, the minimum Y values is (pre-)configured independent of priority level. Here, we prefer to keep the same design as LTE V2X, i.e., removal of “per priority level”. Otherwise, we are fine with the proposal.  |
| ETRI | We prefer Apple’s modification. |
| Qualcomm | The proposal seems too restrictive at such an early stage and could limit communications between two power savings UEs. Evaluations and analysis of different scenarios (Tx/Rx/Interferer, power saving/non-power saving) are needed before agreeing on the scheme. |
| Fujitsu | For the main bullet, we think it is too early to conclude that the Y candidate slots can be determined up to UE implementation. Unlike Rel.14 LTE-V2X, Rel.16 NR-V2X supports HARQ-ACK feedback. When the HARQ-ACK feedback is enabled, the UE should ensure the HARQ RTT related minimum time gap between any two selected resources of a TB. In such circumstance, if the Y candidate slots are determined totally up to UE implementation, it is possible that there are many un-selectable resources considering that the resources within the HARQ RTT minimum time gap cannot be selected. As a result, reliability performance may be impacted due to the limited number of selectable resources.We are fine with the 1st sub-bullet.For the 2nd sub-bullet, we are fine in general. Since per priority configured min Y is not supported in LTE-V2X, we propose to remove “as in LTE-V”. From our understanding, the intention is to FFS whether “a minimum Y value” is (pre-)configured per priority level, but not “a range of minimum Y values” is (pre-)configured per priority level. Therefore, we propose to change “a range of minimum Y values” into “a minimum Y value”.  |
| Xiaomi | Our question on why only periodic traffic is considered is not yet answered. Also we prefer to clearly stating that UE is triggered to perform partial sensing based resource selection in slot n. Except this, we are generally fine with the proposal. We support to remove “as in LTE-V” in the 2nd subbullet FFS. |
| Panasonic | We are fine with the 1st sub-bullet.For the 2nd sub-bullet, we are ok with NEC’s modification.  |
| CMCC | Support. Regarding the 2nd bullet, in LTE-V partial sensing, the parameter is fixed regardless of the data priority and UE by implementation selects Y slots that meets the (pre-)configured minimum parameter, in such a case, it is possible that the determined set of slots may not meet the requirement of remaining PDB, or the number of determined set of slots that satisfy the PDB may be limited, then the data transmission will be interfered and the transmission reliability is decreased. We think that (pre-)configuring the minimum Y values per priority level is one potential solution to solve the problem. |
| Samsung | We’re OK with the main bullet and 1st sub-bullet. For 2nd sub-bullet, we also prefer to remove “pre priority level”. |
| Ericsson | We are supportive of the main bullet and the first sub-bullet. For the second sub-bullet, we think it is too early to include any parameter (priority-level) in order to define the range. We can include an FFS for the parameters to be considered. |
| Sony | We also think that a range of minimum Y values is not (pre-)configured “per priority level” for the second sub-bullet. So we are OK with FL’s proposal with removing “as in LTE-V” in the second sub-bullet. |
| ZTE | Can agree the main bullet and 1st sub-bullet. For 2nd sub-bullet, ‘per priority level’ is removed since the priority is not considered in LTE V2X. On the other hand, the minimum Y values may be related to sub-carrier spacing. So the 2nd sub-bullet is suggested as following:* FFS whether a range of minimum Y values is (pre-)configured per sub-carrier spacing. The (pre-)configuration in LTE-V can be seen as reference.
 |
| Vivo | Regarding how to determine Y, it would be too early to conclude that Y is up to UE implementation as new NR SL features such as DRX on-off can have impact on resource selection process, we share the same view as NEC that restrictions on Y should be studied.We are not convinced to introduce min Y per priority level. We suggest removing ‘per priority level’. |
| Huawei, Hisilicon | Repeatedly, the ambiguity of timing relationship between a resource reservation interval delivery and Y candidate slots determination has not been clarified by the updated the proposal.As explained by our first round reply, a TB along with a reservation interval is delivered at slot n, if at slot n, a UE starts to determine the candidate slots, which slots are used to monitor before slot n and what sensing results are applied to select resource in the selection window? We note similar comments from other companies in the following proposals.For the second sub-bullet, we do not recall in LTE-V, the minimum number of Y is determined as per priority value, so we suggest to remove “as in LTE-V”. It does seem to make sense to have a range of minimum values without clarification of their use by UE, because the practical minimum would simply be the smallest value in the range.  A further update to the proposal 2’ is as follows:**Proposal 2’**: If UE is configured to perform partial sensing ~~and provided with a resource reservation interval (~~$P\_{rsvp\\_TX}\ne 0$~~) from higher layer in slot n~~, it is up to UE implementation to determine Y candidate slots within a resource selection window, where* The resource selection window $[n+T\_{1},n+T\_{2}]$ is defined in the same way as in R16 NR-V2X according to step 1 [TS 38.214 Sec. 8.1.4].

FFS whether a ~~range of~~ minimum Y value~~s~~ is (pre-)configured per priority level ~~as in LTE-V~~ |
| Fraunhofer | We agree with the main bullet and first sub-bullet.Regarding the second sub-bullet, we also feel that it is premature to agree to a single parameter to define the (pre-)configured range. |
| Interdigital | Relying purely on UE’s implementation to determine the set of candidate slots Y is risky at this stage since the partial sensing UEs in NR should support HARQ and SL DRX and we haven’t investigated the potential impacts at this point. Therefore, we prefer to check whether a restriction of selecting Y candidate slots is needed or not. In addition, in LTE-V, Y was not configured per priority.We propose the following update of Proposal 2’:**Proposal 2’**: If a UE is configured to perform partial sensing and provided with a resource reservation interval ($P\_{rsvp\\_TX}\ne 0$) from higher layer in slot n, the UE determines Y candidate slots within a resource selection, ~~it is up to UE implementation to determine Y candidate slots within a resource selection window~~, where* The resource selection window $[n+T\_{1},n+T\_{2}]$ is defined in the same way as in R16 NR-V2X according to step 1 [TS 38.214 Sec. 8.1.4].
* FFS whether a range of minimum Y values is (pre-)configured per priority level ~~as in LTE-V~~
* FFS any further restriction of determining Y candidate slots
 |
| CATT | Regarding the second bullet , we think ‘per priority level’ should be removed, and we would prefer the following wording: FFS Restrictions to determine Y candidate slots. |
| Nokia, NSB | We are okay with the main bullet and the 1st sub-bullet.For 2nd sub-bullet, please remove “as in LTE-V” since the per-priority level configuration of minimum Y is not specified before. |

### Proposals before 2nd check point (Feb 2)

FL observations and comments based on inputs received in Sec. 3.2.1:

* Please check the background description in at the beginning of Section 3.2 and also the accompany email sent for discussion before the 2nd check point.
* In short, this proposal targets a scenario where resource (re)selection is triggered by higher layer in slot n for periodic transmission in a resource pool that allows partial sensing and periodic transmission, the UE uses LTE-V like partial sensing for resource (re)selection.
* In this version, a new term (periodic-based partial sensing) is used to aid with the discussion
* Main differences from the last version
	+ An additional option is added based on LGE’s request.
	+ The last FFS is included based on comments mainly from Qualcomm and vivo.

**Proposal 2’’**: In a resource pool (pre-)configured with at least partial sensing, if UE is configured to perform periodic-based partial sensing (i.e., provided with a resource reservation interval $P\_{rsvp\\_TX}\ne 0$) by higher layer in slot n, it is up to UE implementation to determine Y candidate slots within a resource selection window, where

* Down select to one:
	+ Option 1: The resource selection window $[n+T\_{1},n+T\_{2}]$ is defined in the same way as in R16 NR-V2X according to step 1 [TS 38.214 Sec. 8.1.4]
	+ Option 2: The resource selection window [n+T1, n+T2] is randomly selected by UE while satisfying:
		- T1 ≥ 0 and T2 *≤* remaining PDB
		- T2-T1 *≤* (pre-)configured threshold
* A range of minimum Y values is (pre-)configured
* FFS any restriction to determine Y candidate slots
* FFS whether the resource selection window [n+T1, n+T2] should be confined within a set of periodic set of resources and its relationship with SL-DRX

|  |  |
| --- | --- |
| **Company** | **Comments** |
| OPPO | We are OK with the proposal |
| LGE | According to the FL clarification, the resource selection window can depend on the timing of periodic transmission and the number of retransmissions. Therefore we’d like to slightly modify option 2 as below.* + Option 2: The resource selection window [n+T1, n+T2] is ~~randomly~~ selected by UE while satisfying:
		- T1 ≥ 0 and T2 *≤* remaining PDB
		- T2-T1 *≤* (pre-)configured threshold

In addition, we need further clarification what “a set of periodic set of resources” means in the last FFT bullet. Does it mean the resources available within SL-DRX on-duration? If it’s the case, we may discuss this topic later and separately as SL-DRX issue. |
| NTT DOCOMO | We are OK with the proposal. |
| Apple | * + - 1. We do not see the reason of using “A range of” in the second sub-bullet. Maybe, “The minimum Y value is (pre-)configured” is better wording.
			2. From the main bullet, it reads as “if UE is configured to perform periodic-based partial sensing … in slot n”. Actually, UE has resource selection trigger in slot n, rather than performing sensing in slot n. Maybe, we could modify it as

“… by higher layer, **when UE receives resource selection request from higher layers in slot n**, it is up to UE implementation…” * + - 1. We would like to mention that a UE is configured to perform periodic-based partial sensing is not equivalent to UE itself has periodic traffic. Specifically, UE with aperiodic traffic may still perform periodic-based partial sensing to avoid the resource collision with other UE’s periodic resource reservation. In this sense, we may consider one of the following two options:

Change to “(e.g., at least for the case of provided with a resource reservation interval $P\_{rsvp\\_TX}\ne 0$)” in the main bullet.Change to “(i.e., at least for the case of resource reservation period configured by resource pool including non-zero values)” in the main bullet. |
| Fujitsu | We are fine with the main bullet and the first three sub-bullets. For the 4th sub-bullet, we share the same view as LGE that the clarification of “a set of periodic set of resources” is needed and the issue related to SL-DRX should be discussed separately. |
| CAICT | We are generally OK with the proposal. Since UE might not know when the resource selection trigger “n” will occur in the partial sensing and need to determine the sensing resources related to the candidate resources in the resource selection window, we suggest to change the wording in the main bullet as “it is up to UE implementation to determine Y candidate slots within a resource selection window which might be hypothetical”. |
| vivo | As there is an FFS on restrictions on the determination of Y, ‘up to UE implementation’ in the main bullet should be removed, otherwise the main bullet and the sub-bullet are contradictory. ‘a set of periodic set of resources’ in the last bullet refers, in my understanding, to a set of slots in [n+T1, n+T2] that are **potential** periodic reservations corresponding to slots in periodic sensing window.Regarding whether to keep the SL DRX in the last bullet, if moderator is **not** planning to have a separate discussion/proposal for SL DRX case this meeting, we prefer to keep the SL DRX thing in the FFS. First of all, TX UE must ensure that the selected resource in within the DRX on duration of the RX UE otherwise the RX UE will miss the transmission, we think it is natural that the SL DRX must have some constraints on [n+T1, n+T2] and/or Y. Originally we expected to discuss the interaction between resource selection/sensing and DRX first, but now the group has moved directly into the details related to resource selection/sensing, we are concerned that making agreements without consideration of DRX (e.g., DRX for TX UE, DRX for RX UE) may result in frequent updates or reversals of agreements already reached in the follow-up meetings or delayed discussion for the case with SL DRX. Thus, we prefer to keep the ‘its relationship with SL-DRX’ if we don’t have time to discuss SL DRX separately in this meeting, companies can further study this aspect and provides their observations in the future meeting**Proposal 2’’**: In a resource pool (pre-)configured with at least partial sensing, if UE is configured to perform periodic-based partial sensing (i.e., provided with a resource reservation interval $P\_{rsvp\\_TX}\ne 0$) by higher layer in slot n, ~~it is up to UE implementation to~~ UE determine Y candidate slots within a resource selection window, where* Down select to one:
	+ Option 1: The resource selection window $[n+T\_{1},n+T\_{2}]$ is defined in the same way as in R16 NR-V2X according to step 1 [TS 38.214 Sec. 8.1.4]
	+ Option 2: The resource selection window [n+T1, n+T2] is randomly selected by UE while satisfying:
		- T1 ≥ 0 and T2 *≤* remaining PDB
		- T2-T1 *≤* (pre-)configured threshold
* A range of minimum Y values is (pre-)configured
* FFS any restriction to determine Y candidate slots
	+ if no restriction is identified, it is up to UE implementation to determine Y candidate slots
* FFS whether the resource selection window [n+T1, n+T2] and/or Y should be confined within a set of periodic set of resources and its relationship with SL-DRX
 |
| ZTE, Sanechips | Agree proposal for option 1. For option 2, the motivation of ‘randomly selected’ is not clearly. It is better to change the wording to ‘The resource selection window [n+T1, n+T2] is selected by UE implementation while satisfying:’In addition, for the main bullet, we suggest to change ‘(i.e., provided with a resource reservation interval $P\_{rsvp\\_TX}\ne 0$)’ to ‘(e.g., provided with a resource reservation interval $P\_{rsvp\\_TX}\ne 0$)’ since it is just one possible example. |
| Fraunhofer | We agree with the FL’s proposals.For option 2, we prefer the wording from ZTE.With regards to the DRX, we agree with Vivo, and maybe to simplify it further and alleviate the wording concerns raised by other companies, the last bullet can be phrased “FFS relationship with SL-DRX”, similar to how its done in proposal 5”. |
| Nokia, NSB | Support the proposal with Option 1. For Option 2, it is not clear what the “random selection” of selection window means. R16 specified the selection of $T\_{1}$ and $T\_{2}$ is up to UE’s implementation with certain restrictions. Not sure why the random selection of the resource selection window is needed.For the “slot n” in the main bullet, we need to clarify the slot-n is the time of resource selection trigger, not the time of performing sensing, which may be implied in the current text. |
| Quaclomm | RAN1 hasn’t agreed yet that a UE is configured to perform a specific type of sensing, only that the resource pool is configured to allow certain types of sensing. This can be addressed by removing “is configured to”. In the proposal, it isn’t clear that slot n is where resource (re)selection is triggered:In a resource pool (pre-)configured with at least partial sensing, if UE ~~is configured to~~ performs periodic-based partial sensing (i.e., provided with a resource reservation interval $P\_{rsvp\\_TX}\ne 0$) and resource (re)selection is triggered by higher layers in slot n, it is up to UE implementation to determine a set Y candidate slots within a resource selection window, whereWe agree with the FL’s wording in the last FFS since isn’t only about DRX. It could also apply to cases where the UEs are both transmitters for example. |
| NEC | Fine with the proposal |
| Huawei, HiSilicon | $P\_{rsvp\\_TX}\ne 0$ does not mean the UE is configured for partial sensing, nor vice-versa. The condition in this main bullet, and of other proposals, is not correct. The periodicity of the reservation is time-varying, provided in trigger-slot n from MAC, and is not known to PHY before that time. Therefore, the UE cannot predict the traffic type of its next transmission, and decide if/how to perform (partial) sensing at any slot before n, based on the knowledge of Prsvp\_TX which is delivered only in slot n. This means “*i.e., provided with a resource reservation interval*$ P\_{rsvp\\_TX}\ne 0$” and the “*configured to perform periodic-based partial sensing*” is not equivalent, and therefore should be removed.One thing needs to be emphasized that in LTE-V, the request from MAC received in slot n is only to trigger the resource selection in the PHY layer and ask to report the resource set SB to the MAC layer. The partial sensing is performing continuously once it is configured on the resource pool, rather than starting at the moment of the request reception for the resource selection, i.e. the slot n. We also see other companies, such as Apple and Qualcomm, share the similar views, the slot n is the moment to trigger resource selction, rather than partial sensing.Furthermore, the configuration on UE performing partial sensing RA is intend to detect resource reservations from other UEs, based on reduced number of monitoring slots compared to full-sensing RA. This behaviour, and that it is necessary to perform, does not depend on what traffic type (periodic or aperiodic) is the UE’s own transmission. No matter which traffic type it is, the UE could select the resources based on the sensing results from periodical sensing occasions, once partial sensing is configured, and the short sensing window.For the first sub-bullet, both options are derived based on the Rel-16 resource selection window$[n+T\_{1},n+T\_{2}]$, so these options can be merged to a single one with leaving some FFS.For the second sub-bullet, it does not seem to make sense to have a range of minimum values without clarification of their use by UE, because the practical minimum would simply be the smallest value in the range.For the last sub-bullet, the meaning and the necessity to confine resource selection window it is a second level issue, the relevant of which may depend on other details, and can be discussed separately in the future meetingsWe suggest following changes:In a resource pool (pre-)configured with at least partial sensing, if UE ~~is configured to~~ performs ~~periodic-based~~ partial sensing ~~(i.e., provided with a resource reservation interval~~ $P\_{rsvp\\_TX}\ne 0$~~)~~ ~~by higher layer~~, when resource (re-)selection is triggered in slot n, it is up to UE implementation to determine Y candidate slots within a resource selection window, where* ~~Down select to one:~~
	+ The resource selection window $[n+T\_{1},n+T\_{2}]$ is defined in the same way as in R16 NR-V2X according to step 1 [TS 38.214 Sec. 8.1.4]
		- ~~T1 ≥ 0 and T2~~ *~~≤~~* ~~remaining PDB~~
		- FFS: whether T2-T1 *≤* (pre-)configured threshold
* A ~~range of~~ minimum Y value~~s~~ is (pre-)configured
* FFS any restriction to determine Y candidate slots
* FFS ~~whether the resource selection window [n+T1, n+T2] should be confined within a set of periodic set of resources and its~~ the relationship of selection window $[n+T\_{1},n+T\_{2}]$ with SL-DRX,
 |
| Sharp | Agree with QC on removing “is configured to” (and this comment applies to 3’’ and 5’’ as well). |
| Spreadtrum | Agree proposal generally.For “in slot n” in the main bullet , we agree with QC, Nokia and Apple. In slot n, UE is triggered to do resource (re)selection instead of being configured to perform periodic-based partial sensing by higher layer. So it canbe modified as “…when resource (re)selection is triggered by higher layers in slot n, …” in the main bullet. |

### Proposals before 3rd check point (Feb 4)

FL observations and comments based on inputs received in Sec. 3.2.2:

* TBD

## Topic #3: Periodic-based partial sensing (determination of periodic sensing occasions for periodic transmission)

**Background**: Continuation from Topic #2, as it is mentioned that in R14 LTE-V a common divisor was set to 100ms for Pstep and 20/50ms reservation periodicities were not taken into consideration, the R14 partial sensing was based on an assumption that the reservation periodicity of PUE’s transmission will always be in an integer multiple of 100ms. And k (*gapCandidateSensing*) is (pre-)configured according to the set of possible resource reservation periods allowed in the resource pool. In R16 NR sidelink, the set of up to 16 (pre-)configured possible resource reservation periodicities can be much smaller ([1:99], 0, 100, 200, …, 1000) to cater for wider range of traffic patterns especially ones with short latency requirement. As such, it would be very difficult and dangerous to continue assuming a common divisor can be used in periodic-based partial sensing for NR sidelink. As such, the k value will no longer need to be based on a bitmap which identifies a set of periodic sensing occasions that are integer multiple of 100ms to cover other allowed reservation periodicities in the resource pool.

### Proposals before 1st check point (Jan 28)



Figure 2

**Proposal 3**: If UE is configured to perform partial sensing and provided with a resource reservation interval ($P\_{rsvp\\_TX}$) from higher layer, the UE monitors slots of a set of periodic sensing occasions, where a periodic sensing occasion is a set of slots according to $t\_{y-k×P\_{reserve}}^{SL}$ if $t\_{y}^{SL}$ is included in the set of Y candidate slots.

* $P\_{reserve}$ is a periodicity value from the configured set of possible resource reservation periods allowed in the resource pool (*sl-ResourceReservePeriodList*)
	+ Option 1: $ P\_{reserve}$ corresponds to all values from *sl-ResourceReservePeriodList*
	+ Option 2: $ P\_{reserve}$ corresponds to a subset of values from *sl-ResourceReservePeriodList*
		- FFS how to determine the subset
* k equals to
	+ Option 1: Only the most recent sensing occasion for a reservation period (k=1)
	+ Option 2: The two most recent sensing occasions for a reservation period (k = [1, 2])
	+ Option 3: All possible sensing occasions before $n –T\_{0}$
	+ Option 4: FFS others

|  |  |
| --- | --- |
| **Company** | **Comments and option selection for** $P\_{reserve}$ **and k** |
| OPPO | We are OK with the proposal in principle. While it needs to clarify that down selection from these options should be considered later.  |
| Fraunhofer | We agree with the proposal as such, with the option to decide on the $P\_{reserve}$ and k values as FFS. |
| Apple | We are fine with the proposal with modification.For Preserve, we support Option 2. If Option 1 is selected, then the sensing efforts will be large especially with small resource reservation periods. For example, if the resource reservation period is 1 ms, then no power saving gain can be achieved at all. Here, we may configure a resource reservation period threshold, and only apply the configured resource reservation periods which are larger than the threshold. For k, we prefer to add an option that the k is by (resource pool) configuration. Any integer value between 1 and a configured value is used to determine the number of sensing occasions. This is restricted within the sensing window [n-T0, n-Tproc,0). |
| Ericsson | Regarding Preserve, we think that the easiest thing is to have full configurability (from the values in *sl-ResourceReservePeriodList*), avoid a fruitless discussion, and focus on more important issues.Moreover, for the values of k only Option 1 should be considered. That is aligned with the procedure in 8.1.4. |
| InterDigital | We are OK with the proposal |
| CATT | We are OK to discuss the selection of $P\_{reserve}$ and k values later. |
| Qualcomm | Similar to Proposal 2, we think we need to consider the general principle prior to discussing the details. |
| Lenovo&MM | For $P\_{reserve}$, option 1 is our preference. For k, option 1 is our preference. |
| CMCC | We are OK with the 2 options, and meanwhile, we would like to add a third option that $P\_{reserve}$ corresponds to the common devisor of all values from *sl-ResourceReservePeriodList.* In our views, by supporting option 3, both options in the proposal can be achieved by setting specific *gapCandidateSensing* bitmap indications, which can be up to implementation. In addition, by supporting option 3, the k value should be modified to be the ratio of sensing window size and the derived $P\_{reserve}$. |
| NEC | **Preserve: Option 1/option 2.** Option 1 is preferred because we should exclude all the reservations. Option 2 contains more flexibility (including option 1) which we can also accept.**K: Option 1.** Concerns: for a small $P\_{reserve}$ and large index of slot y, when we take k = 1, it's possible that y-$P\_{reserve}$ doesn't belong to the sensing window, e.g., later than n-Tproc. K-1 may make the occasion out of sensing window. Or, as alternative, we just define sensing occasions based on k and $P\_{reserve}$ for Rel.17 partial sensing because we're also trying to define additional sensing occasions out of legacy sensing window in other topics.Considering figure 2 above, we think only option 1 is aligned with existing sensing procedure. According to legacy SPS scaling mechanism and spec, only reservation received in the last Preserve will be scaled to the resource selection window. The other reservations (k=2,3,…) except the last one(k=1) will not be scaled according to the legacy method and will have no impact to the resource exclusion in selection window (due to Q = 1 in step 6 (c)). |
| vivo | * Regarding $P\_{reserve}$

We are ok with both options, but option2 is preferred from the perspective of power saving. For example, if two periods are configured in a pool, one period is an integer multiple of the other, $P\_{reserve}$ can be set to the larger one of the two periods, which not only reduces the time instances of periodic sensing but also ensures that the UE can detect packets of both periodicities. We suggest adding a FFS on the conditions on using option1 or option2.* Regarding the value of k

I think we need to discuss some basic principles for determining the location of sensing occasions before choosing one or more options. For example, whether the periodic sensing occasions can be after slot n or $n –T\_{0}$. whether a (pre-)configured bitmap like *gapCandidateSensing* in LTE V2X will be reused to determine the k values. |
| FUTUREWEI | We agree with the proposal. FFS for the values of *P*reserve and k |
| ETRI | We are generally fine with FL’s proposal. Regarding $P\_{reserve}$ and k values, it can be discussed further. |
| Panasonic | We are ok with the proposals.  |
| Sony | We are OK with the proposal and down-selecting later. |
| NTT DOCOMO | Support the proposal’s direction and prefer option 1 + option 1. |
| CAICT | For $P\_{reserve}$, we prefer option1 since it would lead to a serious conflict between SL TXs if a subset of values from *sl-ResourceReservePeriodList* is configured for partial sensing. Besides, it is hard to determine which subset to configure for option2.For k, we prefer option3 considering it seems to have higher reliability than option1 and option2. |
| Sharp | Regarding the values of k, since the UE cannot predict where slot n is before it comes, it has to monitor the slots in a periodic manner anyway, so it is unclear why restricting the values of k here helps.Besides, we have 2 further clarifications. 1) Considering the topic#4 and #5, we suggest to add “at least the UE monitors…”, since probably in partial sensing, the periodic slots are not the only monitored slots. 2) the issue related to periodic reservation in SCI format 1-A has not been decided yet, thus, $P\_{reserve}$ should be a value with conversion from ‘ms’ to logical slot (of a resource pool), since the terminology $t\_{y}^{SL}$ is used in the proposal. |
| Xiaomi | As shown in Figure 2, the resource selection happens at slot n, and UE sensing behaviour happens before slot n. Y candidate slots are determined at slot n, but not before slot n. Therefore, we suggest to rewording the main bullet such as “When resource selection is triggered in slot n, given a slot in the set of Y candidate slots, UE should have monitored in slots …”.  |
| ZTE | For the first bullet, we agree with option 1. For the second bullet, we understands that all options are under the assumption that the bitmap is set with all “1”, or there is no such bitmap mechanism for sensing indication anymore. But we think firstly, we should discuss whether to reuse legacy bitmap mechanism for partial sensing. |
| LGE | The main sentence of the proposal is generally ok.* For $P\_{reserve}$, option 2 is preferred for power saving purpose. Actually option 1 is a special case of option 2.
* For value k, sensing over multiple slots for the same reservation period is redundant so not necessary. In this sense, sensing only one slot for each reservation period is reasonable. We propose option 4 as follows.
	+ Only one sensing occasion for one reservation period. A value k for a specific sensing occasion is UE implementation. Max value k is (pre-)configured.
 |
| Samsung | We are OK with the proposal if down-selection will be made later. Otherwise we prefer full configurability for both $P\_{reserve}$ and k. |
| Fujitsu | * Regarding $P\_{reserve}$, we prefer option 2. Since the periodicities ranging from 100 ms to 1000 ms are integer multiples of 100 ms, it is not necessary to take all the values from *sl-ResourceReservePeriodList.*
* Regarding *k*, the earliest sensing occasion should be equal to the maximum periodicity in the current resource pool. On the other hand, for some extreme short periodicities (e.g., 1 ms ~ 3 ms), since the processing time needs to be guaranteed for resource selection, the UE cannot perform sensing for the most recent sensing occasions. Considering the above points, we propose the following for *k.*
	+ For the reservation period ≧a certain value (e.g., 100 ms), *k*=1.
	+ For the reservation period < a certain value (e.g., 100 ms), *k* is the minimum integer which makes $t\_{y-k×P\_{reserve}}^{SL}$ falling into the sensing window.
 |
| MediaTek | We are fine with the proposal with $P\_{reserve}$ and k as FFS. Downselection should be done later. |
| Intel | Agree with modification aiming to support coexistence with dynamic transmissions that will require sensing in a window of size max(resource selection window, SCI signaling window) prior to resource reselection time instance.Our preferred option for “Preserve” – make it fully configurableOur preferred option for “k” is k = 1. Other k values seem overcomplicate design and do not serve power saving purpose. |
| Huawei, HiSilicon | For the main bullet, same comments as that for proposal 2, i.e., “and provided with a resource reservation interval ($P\_{rsvp\\_TX}$) from higher layer” should be removed.Please could the FL clarify if the proposal is to support all the options under Preserve and k, or to down-select now or later? We assume downselection is intended.On $P\_{reserve}$, Option 1. Support all values that were already supported in Rel-16, since it should be backward compatible for Rel-16 design in Rel-17.On k, Option 4 (k is a configurable set). We doubt that all options should be supported individually, but configuration could cover all or most.Unlike in LTE-V where partial sensing deals with periodic traffic only, NR partial sensing would suffer more collisions due to aperiodic traffic, hence restriction on k =1 only would more likely result in un-reliable decision on corresponding candidate slot due to failure of a SCI decoding at a given periodicity, e.g. caused by aperiodic transmission. We do not see much more value in option 2 than option 1. The value of k can be configurable to provide flexibility.  |
| Convida Wireless | We are fine with the proposal with down selection for options. |
| Bosch | In principle, we are fine with the FL proposal. If we are going to down select, then our preference is to be able to (pre-)configure both P\_reserve and k. |
| Nokia, NSB | We shall agree with some general principles to support various periodicities for partial sensing, before we discuss this detailed proposal. |

**Proposal 3’**: If UE is configured to perform partial sensing and provided with a resource reservation interval ($P\_{rsvp\\_TX}\ne 0$) from higher layer, the UE monitors slots of a set of periodic sensing occasions, where a periodic sensing occasion is a set of slots according to $t\_{y-k×P\_{reserve}}^{SL}$ if $t\_{y}^{SL}$ is included in the set of Y candidate slots.

* $P\_{reserve}$ is a periodicity value from the configured set of possible resource reservation periods allowed in the resource pool (*sl-ResourceReservePeriodList*). Down select among:
	+ Option 1: $ P\_{reserve}$ corresponds to all values from *sl-ResourceReservePeriodList*
	+ Option 2: $ P\_{reserve}$ corresponds to a subset of values from *sl-ResourceReservePeriodList*
		- FFS how to determine the subset
	+ Option 3: $P\_{reserve}$ is (pre-)configurable from values in *sl-ResourceReservePeriodList*
	+ Option 4: $P\_{reserve}$ is a common devisor among values in *sl-ResourceReservePeriodList*
* k equals to (down select to one)
	+ Option 1: Only the most recent sensing occasion for a reservation period (k=1)
	+ Option 2: The two most recent sensing occasions for a reservation period (k = [1, 2])
	+ Option 3: All possible sensing occasions after $n –T\_{0}$
	+ Option 4: Only one periodic sensing occasion for one reservation period. The k value is up to UE implementation. Max value for k is (pre-)configured.
	+ Option 5: FFS others

|  |  |
| --- | --- |
| **Company** | **Comments** |
| OPPO | We support FL’s proposal.  |
| NEC | As they are down-select options, we're ok with current proposal. One clarification for the "down select among" is the intention to down select at least one option for Preserve? We think "down select to one" is applicable to Preserve too. |
| NTT DOCOMO | Agree with the current proposal keeping options for future down-selection. |
| LGE | Support FL’s proposal. For $P\_{reserve}$, option 1 always requires max power consumption. Option 4 is unclear as value 1 is always a common divisor, which means monitoring all slots. From power consumption perspective, a subset of values are preferred. But rather than making a rule for decision by UE, network can (pre-)configured the required values. As a result, option 3 is preferred.For k value, as we commented earlier, sensing over multiple slots for the same reservation period is redundant, so not necessary. In this sense, sensing only one slot for each reservation period is reasonable. Option 4 is preferred as it is a superset including the option 1. |
| Apple | We prefer to add “k is (pre-)configured” as a more reliable sensing option. At this moment, we may include all possible options and down-select later. For $P\_{reserve}$, we think Option 2 covers Option 3, since Option 3 can be considered as one way (i.e., configuration) of determining the subset. |
| ETRI | We support FL’s proposal. As commented by NEC, it might be better to modify into “Down select to one” instead of “Down select among”.  |
| Qualcomm | Similar to our comment on Proposal 2’, it’s too early to restrict the design of the partial sensing scheme. Different combinations of Tx/Rx UEs need to be investigated first. |
| Fujitsu | We are fine with the main bullet and the 2nd sub-bullet.For $P\_{reserve}$, we think that the FFS in option 2 includes the subset determination methods provided by option 3 and option 4.  |
| Xiaomi | We are generally fine with the intention of the proposal. As our last comment, UE can determine the set of Y slots no earlier than slot n, and UE has already finished sensing operation in the slots corresponding to the Y slots. We prefer to describing the main bullet in a requirement way for example:If UE is configured to perform partial sensing and provided with a resource reservation interval ($P\_{rsvp\\_TX}\ne 0$) from higher layer, and determines Y candidate slots in slot n, the ~~UE monitors~~ slots of a set of periodic sensing occasions shall be monitored by the UE, where a periodic sensing occasion is a set of slots according to $t\_{y-k×P\_{reserve}}^{SL}$ if $t\_{y}^{SL}$ is included in the set of Y candidate slots. |
| Panasonic | We support FL’s proposals for future down selection.  |
| CMCC | Support the FL’s proposal.For $P\_{reserve}$, let us elaborate more on the intention of Option 4. Option 4 does not indicate to always set 1 as the common divisor, and the value should be dependent on the (pre-)configured reservation period of a given RP. For instance, a RP allows reservation periods of 5ms, 15ms, and 20ms, then the $P\_{reserve}$ = 5ms. Even if we consider some special case that a RP allows reservation periods of 15ms and 16ms, the common divisor is 1; however, it does not intend to monitor all the slots. In such a case, by setting the 15th and 16th bit of the higher layer parameter *gapCandidateSensing* to be 1, and all the other bits to be 0, it would be the same as Option 1 with k=1. |
| Samsung | We are fine with the main bullet and 2nd sub-bullet.For $P\_{reserve}$, it’s unclear for us why Option 4 of using a common divisor have gain compared with Option 2. In addition, Option 3 can be one possible manner of Option 2. However since it’s for down-selection, we can accept the current version.  |
| Ericsson | We support the FL proposal for further down-selection. We would like to get some clarification on whether Option 3 as written includes a pre-configured set or if this can be included in the FFS of Option 2. Moreover, in our view for the second point the value that should be considered is Option 1 which is aligned with the current procedure in 38.314. |
| Sony | We can support the FL’s proposal basically. But regarding the periodicity value, we think option 3 and 4 could be included in the FFS in option 2. |
| ZTE | Agree FL’s proposal.As down-select, for $P\_{reserve}$, we support option 1 and option 3 is acceptable.For k value, suggest to add ‘ from ’ into option 1 and option 2 for more understandable, such as following:* + Option 1: Only the most recent sensing occasion from  for a reservation period (k=1)
	+ Option 2: The two most recent sensing occasions from  for a reservation period (k = [1, 2])

As down-select, prefer to option 4. It seems that the resource reservation interval ($P\_{rsvp\\_TX}\ne 0$) is not related to the proposal, so I am wonder whether it can be removed.  |
| vivo | Support the FL’s proposal. |
| Huawei, HiSilicon | The main bullet can be corrected as what we suggest in question 2.For the first sub-bullet, option 2 takes the same effect of option 3, once the FFS is resolved. The FFS allows a subset of values are used by (pre-)configuration. So the option 3 can be removed.For the k determination, another option could be added which “k is (pre-) configured”. We also see others have similar understanding.**Proposal 3’**: If UE is configured to perform partial sensing ~~and provided with a resource reservation interval (~~$P\_{rsvp\\_TX}\ne 0$~~) from higher layer~~, the UE monitors slots of a set of periodic sensing occasions, where a periodic sensing occasion is a set of slots according to $t\_{y-k×P\_{reserve}}^{SL}$ if $t\_{y}^{SL}$ is included in the set of Y candidate slots.* $P\_{reserve}$ is a periodicity value from the configured set of possible resource reservation periods allowed in the resource pool (*sl-ResourceReservePeriodList*). Down select among:
	+ Option 1: $ P\_{reserve}$ corresponds to all values from *sl-ResourceReservePeriodList*
	+ Option 2: $ P\_{reserve}$ corresponds to a subset of values from *sl-ResourceReservePeriodList*
		- FFS how to determine the subset
	+ ~~Option 3:~~ $P\_{reserve}$ ~~is (pre-)configurable from values in~~ *~~sl-ResourceReservePeriodList~~*
	+ Option 4: $P\_{reserve}$ is a common devisor among values in *sl-ResourceReservePeriodList*
* k equals to (down select to one)
	+ Option 1: Only the most recent sensing occasion for a reservation period (k=1)
	+ Option 2: The two most recent sensing occasions for a reservation period (k = [1, 2])
	+ Option 3: All possible sensing occasions after $n –T\_{0}$
	+ Option 4: Only one periodic sensing occasion for one reservation period. The k value is up to UE implementation. Max value for k is (pre-)configured.
	+ Option 5: k is (pre-) configured
	+ Option ~~5~~6: FFS others
 |
| Fraunhofer | We agree with the FL’s proposal with the option to down-select at a later stage. |
| Interdigital | We support FL’s proposals |
| CATT | For the first bullet, not sure we need all the three options, we think options 3 already incudes option 1 and option2. No need to have the first two to options. |
| Convida Wireless | We support FL’s proposal with down-selection. |
| Nokia, NSB | This proposal is only applied for periodic traffic, and the UE with aperiodic traffic shall use another partial sensing scheme (such as in Proposal 5). Please clarify that we are going to define two partial sensing schemes, one for periodic traffic and anther one for aperiodic traffic. How about mixed traffic?For this proposal, using a parameter $P\_{reserve}$ might resolve the problem to support these periodicities ([1:99], 100, 200, …, 1000)ms. Can we clarify whether $P\_{reserve}$ is UE specific or resource pool specific? Support to keep these options of $P\_{reserve}$ open.For k options, support to add another option “pre-configured” for k. |

### Proposals before 2nd check point (Feb 2)

FL observations and comments based on inputs received in Sec. 3.3.1:

* Please check the background description in at the beginning of Section 3.3, Fig. 2 and also the accompany email sent for discussion before the 2nd check point.
* In short, this proposal targets a scenario where resource (re)selection is triggered by higher layer in slot n for periodic transmission in a resource pool that allows partial sensing and periodic transmission, the UE uses LTE-V like partial sensing for resource (re)selection.
* In this version, a new term (periodic-based partial sensing) is used to aid with the discussion.

**Proposal 3’’**: In a resource pool (pre-)configured with at least partial sensing, if UE is configured to perform periodic-based partial sensing (i.e., provided with a resource reservation interval $P\_{rsvp\\_TX}\ne 0$) by higher layer, the UE monitors slots of a set of periodic sensing occasions, where a periodic sensing occasion is a set of slots according to $t\_{y-k×P\_{reserve}}^{SL}$ if $t\_{y}^{SL}$ is included in the set of Y candidate slots.

* $P\_{reserve}$ is a periodicity value from the configured set of possible resource reservation periods allowed in the resource pool (*sl-ResourceReservePeriodList*). Down select to one:
	+ Option 1: $ P\_{reserve}$ corresponds to all values from *sl-ResourceReservePeriodList*
	+ Option 2: $ P\_{reserve}$ corresponds to a subset of values from *sl-ResourceReservePeriodList*
		- FFS how to determine the subset (e.g., by (pre-)configuration, UE determination, whether to include all values)
	+ Option 3: $P\_{reserve}$ is a common divisor among values in *sl-ResourceReservePeriodList*
* k equals to (down select to one)
	+ Option 1: Only the most recent sensing occasion for a reservation period (k=1)
	+ Option 2: The two most recent sensing occasions for a reservation period (k = [1, 2])
	+ Option 3: All possible sensing occasions after $n –T\_{0}$
	+ Option 4: Only one periodic sensing occasion for one reservation period. The k value is up to UE implementation. Max value for k is (pre-)configured.
	+ Option 5: k is (pre-)configured
	+ Option 6: FFS others

|  |  |
| --- | --- |
| **Company** | **Comments** |
| OPPO | We are OK with the proposal |
| LGE | Option 1 of the second bullet is a special case of option 4 in that only one (the most recent) periodic sensing occasion per reservation period is selected. We can merge two options like this.* + Option 1: Only one periodic sensing occasion for one reservation period.
		- FFS whether the one occasion is the most recent one, UE implementation, or (pre-)configuration
		- FFS whether max k value is (pre-)configured
 |
| NTT DOCOMO | We are OK with the proposal. |
| Apple | Fine with the proposal in general.For $P\_{reserve}$ , it seems that in Option 2, “whether to include all values” covers Option 1. Hence, we wonder if Option 1 could be removed, as it already merged to Option 2? As our comment in Proposal 2’’, a UE is configured to perform periodic-based partial sensing is not equivalent to UE itself has periodic traffic. Specifically, UE with aperiodic traffic may still perform periodic-based partial sensing to avoid the resource collision with other UE’s periodic resource reservation. In this sense, we may consider either one of the options:Change to “(e.g., at least for the case of provided with a resource reservation interval $P\_{rsvp\\_TX}\ne 0$)” in the main bullet.Change to “(i.e., at least for the case of resource reservation period configured by resource pool including non-zero values)” in the main bullet. |
| Fujitsu | We are fine with the proposal in general.For option 1 and option 2 of *k*, considering that UE can only perform sensing within the sensing window, the most recent sensing occasion refers to the most recent periodic occasion that falls into the sensing window. If *k* is restricted to 1 or [1,2], some determined periodic occasion may be outside the sensing window and cannot be sensed. Hence, we propose to remove k=1 and k=[1,2] from option 1 and option 2, respectively.* Option 1: Only the most recent sensing occasion for a reservation period ~~(k=1)~~
* Option 2: The two most recent sensing occasions for a reservation period ~~(k = [1, 2])~~
 |
| CAICT | For Option5, it is better to clarify that whether multiple k can be pre-configured or not.  |
| vivo | Fine with the proposal in principle.UE configured with periodic sensing also needs to do continuous sensing to exclude aperiodic reservation from other UE from the candidate resource set, so UE should ‘at least’ perform the periodic sensing on the periodic occasions.Besides, we have a similar comment as that we made last Friday and in 3.2.2, we would like to add FFS points on the SL DRX in case SL-DRX might affect the sensing slot.**Proposal 3’’**: In a resource pool (pre-)configured with at least partial sensing, if UE is configured to perform periodic-based partial sensing (i.e., provided with a resource reservation interval $P\_{rsvp\\_TX}\ne 0$) by higher layer, the UE monitors slots ~~of~~ at least including a set of periodic sensing occasions, where a periodic sensing occasion is a set of slots according to $t\_{y-k×P\_{reserve}}^{SL}$ if $t\_{y}^{SL}$ is included in the set of Y candidate slots.* $P\_{reserve}$ is a periodicity value from the configured set of possible resource reservation periods allowed in the resource pool (*sl-ResourceReservePeriodList*). Down select to one:
	+ Option 1: $ P\_{reserve}$ corresponds to all values from *sl-ResourceReservePeriodList*
	+ Option 2: $ P\_{reserve}$ corresponds to a subset of values from *sl-ResourceReservePeriodList*
		- FFS how to determine the subset (e.g., by (pre-)configuration, UE determination, whether to include all values)
	+ Option 3: $P\_{reserve}$ is a common divisor among values in *sl-ResourceReservePeriodList*
* k equals to (down select to one)
	+ Option 1: Only the most recent sensing occasion for a reservation period (k=1)
	+ Option 2: The two most recent sensing occasions for a reservation period (k = [1, 2])
	+ Option 3: All possible sensing occasions after $n –T\_{0}$
	+ Option 4: Only one periodic sensing occasion for one reservation period. The k value is up to UE implementation. Max value for k is (pre-)configured.
	+ Option 5: k is (pre-)configured
	+ Option 6: FFS others
* FFS$ $Interaction between k and/or $P\_{reserve}$ with SL-DRX
 |
| ZTE, Sanechips | For the second bullet to define k, we think one more option should be added, which is to use legacy bitmap to configure. |
| Fraunhofer | We are fine with the FL’s proposal. |
| Nokia, NSB | This proposal defines perodic sensing occations for partial sensing. We are fine with the main bullet and the 1st sub-bullet. For the 2nd sub-bullet on k, we are also okay to keep all options open. Suggest to delete “(down selection to one)”, because some of the options can be combined together. |
| Qualcomm | We have the same comment about sensing type and configuration as Proposal 2’’. We also propose to use the wording “UE shall monitor” from LTE SL spec instead of “UE monitors” to avoid any confusion about causality:In a resource pool (pre-)configured with at least partial sensing, if UE ~~is configured to~~ performs periodic-based partial sensing (i.e., provided with a resource reservation interval $P\_{rsvp\\_TX}\ne 0$) by higher layer, the UE shall monitor~~s~~ slots of a set of periodic sensing occasions, where a periodic sensing occasion is a set of slots according to $t\_{y-k×P\_{reserve}}^{SL}$ if $t\_{y}^{SL}$ is included in the set of Y candidate slots.We also share vivo’s view on introducing an FFS for DRX* FFS relation relationship between sensing occasions and SL-DRX
 |
| NEC | We're agree with the proposal to down select. |
| Huawei, HiSilicon | Same comment for the main bullet as Question 2.The RP-level allowed/dis-allowed (pre-)configuration (RRC signalling) on periodic reservation is NOT same as $P\_{rsvp\\_TX}\ne 0$/$P\_{rsvp\\_TX}=0$ in slot n, where the latter is provided by MAC layer and is time-varying in different slot “n” per UE. Hence the provision of resource reservation interval in the parentheses in the main bullet should be removed as follows: In a resource pool (pre-)configured with at least partial sensing, if UE ~~is configured to~~ performs ~~periodic-based~~ partial sensing ~~(i.e., provided with a resource reservation interval~~ $P\_{rsvp\\_TX}\ne 0$~~)~~ by higher layer, the UE monitors slots of a set of periodic sensing occasions, where a periodic sensing occasion is a set of slots according to $t\_{y-k×P\_{reserve}}^{SL}$ if $t\_{y}^{SL}$ is included in the set of Y candidate slots.For determination, it seems there is an overlap between option 1 and option 2, using all values or a subset of values are different considerations for design at this stage and can be down select in future meeting, “whether to include all values” is better to be removed in the FFS of FFS.* + Option 2: $ P\_{reserve}$ corresponds to a subset of values from *sl-ResourceReservePeriodList*
		- FFS how to determine the subset (e.g., by (pre-)configuration, UE determination~~, whether to include all values~~)

We are ok for the sub bullets which aim to down-select to one in future meetings. |
| Spreadtrum | We are OK with the FL’s proposal. |

### Proposals before 3rd check point (Feb 4)

FL observations and comments based on inputs received in Sec. 3.3.2:

* TBD

## Topic #4: Contiguous-based partial sensing (when $P\_{rsvp\\_TX}$ is provided by higher layer) – re-evaluation and pre-emption checking for periodic transmission

**Background**: Continuation from Topic #3, partial sensing for a periodic transmission in a resource pool that allows aperiodic transmissions (which is all SL Tx pools), should also take into consideration of resource reservation by aperiodic transmissions. In various submitted contributions to this meeting, it is proposed that an additional sensing (short-term sensing/extended partial sensing) should be performed by the UE for periodic transmissions to take into account of aperiodic resource reservations.

Furthermore, it was agreed in the last meeting (RAN1#103-e) that “re-evaluation and pre-emption checking are supported by UEs that perform sensing”, it is also proposed in contributions that the additional sensing can also be used for the purpose of re-evaluation and pre-emption checking.

### Proposals before 1st check point (Jan 28)



Figure 3

**Proposal 4:** If UE is configured to perform partial sensing and provided with a resource reservation interval ($P\_{rsvp\\_TX}$) from higher layer, the UE additionally monitors slots

* Option 1: from slot ty0 -32, where ty0 is the first slot in the set of Y candidate slots, until $m –T\_{3}$ before the last transmission for the TB, except for slots in which its own SL and UL transmissions occur
* Option 2: from slot n-32 until $m –T\_{3}$ before the last transmission for the TB, except for slots in which its own SL and UL transmissions occur

|  |  |  |
| --- | --- | --- |
| **Company** | **Option 1, 2 or others** | **Comments** |
| OPPO |  | Firstly, it needs to clarify in the main bullet that this proposal targets for period traffic. For aperiodic traffic, UE cannot predict the arriving time of the packet so that it cannot sense the slots before slot n (packet arrival time). In our view, considering the aperiodic traffic in the RP, UE should do short term sensing (e.g., 32 slots) before slot n. furthermore, UE should do short term sensing (e.g., 32 slots) before each selected resource for re-evaluation/pre-emption check. For option 1 and 2, as we commented in proposal 2, UL transmission should be removed. Furthermore, for option 1, whether the UE should monitor from ty0 -32 depends on whether the time position of the corresponding slot is before or after slot n. For option 2, if the time gap between slot n and the first selected resource is > 32 slots, UE does not need to sense the slots between [n+1, ty0 -32]. |
| Fraunhofer |  | We prefer to retain the procedure used in Rel-16 for re-evaluation/pre-emption. Based on the proposal, exclusions based on UL transmissions can be removed. |
| Apple |  | We have the following comments about the proposal:1. We assume this is for resource re-evaluation and pre-emption checking. We may mention it in the proposal.
2. Why “resource reservation interval” is mentioned in the main bullet? Do you intend to mean the periodic resource reservation? Note that for aperiodic resource reservation, the resource reservation interval of 0 ms is also provided by higher layer.
3. In the figure, why a UE starts the contiguous-based sensing for resource re-evaluation before n (slot for resource selection) in the case of partial sensing? A UE is not supposed to perform sensing for resource re-evaluation until the resource is selected. Here, is the slot n the initial periodic data arrival time or the data arrival time after one period?
4. We should consider another option that the sensing for resource re-evaluation could start from m-32 until m-T3 to avoid collision with aperiodic reservation from another UE, where m is the slot of the selected resource.
 |
| Ericsson |  | We do not agree with this proposal. First, we should anchor the behaviour of the sensing mechanism for aperiodic transmissions (see 3.5) and once it has been agreed, we can revisit the issue defined in this proposal.  |
| InterDigital |  | For resource (re)selection, the UE should perform short-term sensing before slot n. For pre-emption and re-evaluation, the UE should perform short-term sensing from slot n+1 to m-T3. |
| CATT |  | The intended use case of the proposal should be further clarified. Also, we think It’s better to discuss this proposal after detail mechanism of sensing has been decided. |
| Qualcomm |  | We prefer to discuss this issue after Proposals 4 and 5 are settled. |
| Lenovo&MM | Option 1 | Option 1 is acceptable to us. |
| CMCC |  | The intention of this proposal is not quite clear to us:* Does this proposal intend to solve the case when a resource pool which is shared by both periodic and aperiodic transmissions, and to introduce an additional sensing window on top of the partial sensing slots to avoid the potential collision caused by the aperiodic transmissions?
* Or, it is intended to study the re-evaluation and pre-emption mechanism for the partial sensing?
 |
| NEC | Option 1 | If this proposal is intended for UE's periodic traffic, $P\_{rsvp\\_TX}=0$ should be excluded.Partial sensing cares about candidate resources Y, so we think ty0 -32 could be the starting sensing time in this proposal. |
| vivo | Option1 | 1. UL transmission should be removed.
2. Option2 may introduce unnecessary sensing occasion compared with option1 when n-32< ty0 -32
 |
| ETRI |  | We slightly prefer option 1. However as mentioned by several companies, this proposal should be limited for periodic traffic. |
| Sony |  | We need to make agreement for the other topics and then we can revisit this topic later. |
| NTT DOCOMO | Option 1 with update | * UL transmission is unnecessary.
* Option 2 includes unrequired slot for sensing for aperiodic reservation.
* Option 1 should be updated as ‘ty0 -31’ since SCI in ty0 -32 cannot reserve resource in ty0.
 |
| CAICT |  | It is better to separate the issues on sensing to avoid the conflict with aperiodic traffic and sensing for pre-emption and re-evaluation apart. 1. To avoid the conflict with aperiodic traffic, slots from ty0-32 to ty0 shall be sensing, except the slots for its own SL/UL transmissions.
2. For pre-emption and re-evaluation, slots from n-32 until $m –T\_{3}$ before the last transmission for the TB shall be sensing, except the slots for its own SL/UL transmissions.
 |
| Sharp |  | We agree with Ericsson and Qualcomm that the issue is discussed after proposal 5 concluded. |
| Xiaomi | Option1 | The sensing behaviour before n and after n should be distinguished. From our understanding, what we are discussing in the behaviour of resource selection, which happens at slot n. Sensing before slot n cannot be determined at slot n, as you cannot go back to sense; you can only determine whether sensing requirement is satisfied or not. But sensing after slot n can be determined at slot n. Therefore, sensing before slot n should be discussed together with sensing requirement issue; while sensing after slot n can be discussed in pre-emption and pre-evaluation issue. |
| ZTE | neither | Firstly, we share the same view with OPPO that if n is defined as packet arrival time, it is not capable for UE to predict the packet arrival timer. Then if n is defined as resource (re-)selection trigger time indicated by MAC, we think the example shown in proposal 5 is a more reasonable solution that short term sensing is triggered after n. So firstly, we should give a clear definition of n. |
| LGE | See comments | We need to separate two operations.1) short-term sensing (STS) for resource (re)selection Before resource (re)selection, STS is performed over [n-TA, n–Tproc,0] to detect any possible periodic traffic, where TA = max interval between reserved resources that can be indicated by a SCI.We didn’t make any decision on the content of SCI, so it’s safer at this stage to say TA is based on the SCI content. If Rel.16 SCI rule is reused, TA is 31 slots.2) STS for resource re-evaluation/pre-emption checking After resource (re)selection, STS is performed over [STSk, mk-T3] for k=0,…,K, where mk is the timing of the k-th reserved resource and K is the number of reserved resources, and STSk is determined as max(n+1, mk - TA).If the candidate slots are apart from each other more than 31 slots, sensing over a duration exceeding 31 slots is not performed for power saving. |
| Samsung |  | We also prefer to clarify the intention of this proposal. If that’s common understanding that resource reservation interval provided by higher layer corresponds to periodic traffic, then we’re fine. In addition, UL transmission should be removed similarly as in topic#3.We slightly prefer option 1. |
| Fujitsu |  | There should be two windows with different functions. One is short sensing window which is defined as $[t\_{y0}-32,t\_{y0}-T\_{proc,0}]$. It is used for sensing aperiodic reservations. The other is defined as re-evaluation/pre-emption sensing window, used for re-evaluation/pre-emption check. If pre-emption is disabled in current resource pool, the re-evaluation/pre-emption sensing window is from the slot $t\_{y0}-T\_{proc,0}$ until $m –T\_{3}-T\_{proc,0}$ before the first-in-time selected resource. If pre-emption check is enabled in current resource pool, the re-evaluation/pre-emption sensing window is from the slot $t\_{y0}-T\_{proc,0}$ until $m –T\_{3}-T\_{proc,0}$ before the last-in-time selected resource. |
| MediaTek |  | We do not support this. Sensing for re-evaluation/pre-emption can be performed separately from the sensing for aperiodic traffic detection in the pool. That is, sensing can be performed in [n-32,n] and [m-32, m-T3]. We should also add this as another option. |
| Intel |  | We prefer Option 2 but are open to discuss it later. |
| Huawei, HiSilicon  | Principles of option 1, but needs modifications  | First of all, it seems the current proposals ignore an essential issue when a UE will report SA to the high layer and how to use the sensing results in the short sensing window by the UE to detect aperiodic reservations from other UEs.Before ty0, a short sensing window is defined for the purpose to handle aperiodic reservations from other UEs, and therefore the sensing results obtained from the short sensing window and partial sensing slots can be used to determine and report the candidate resources set SA to the high layer. Considering the largest gap resource reservation by a single SCI and UE processing time, the time interval should be from ty0 – 31 to ty0 - tproc,0 –T1 to cover the most relevant 32 slots.After ty0, if the re-evaluation is triggered based on specific conditions for the selected resource by MAC, additional slots can be monitored for re-evaluating the resources. If the re-evaluation is not triggered, no more monitoring is needed after ty0.Thus the problem in the proposal is that there is no distinction between sensing before ty0 and re-evaluation after ty0. This structure needs to be reflected in the proposal before it is possible to consider the whole procedure.The SL and UL part should be deleted, as mentioned above for proposal 2. Similar with other proposals, the dependence on Prsvp\_TX needs to be removed, because the UE is performing this procedure to detect traffic from other UEs, without depending on the periodic or aperiodic nature of its own traffic. |
| Convida Wireless |  | The proposal 4 could be discussed later. |
| Bosch |  | In our understanding, if “resource reservation interval ($P\_{rsvp\\_TX}$)” is stated in the main bullet, then we are targeting periodic reservation. In this case, option 2 works well. However, we are open for discussions. |
| Nokia, NSB |  | This proposal can be discussed later after we made some progress on the design. |

### Proposals before 2nd check point (Feb 2)

FL observations and comments based on inputs received in Sec. 3.4.1:

* TBD

### Proposals before 3rd check point (Feb 4)

FL observations and comments based on inputs received in Sec. 3.4.2:

* TBD

## Topic #5: Contiguous-based partial sensing (when $P\_{rsvp\\_TX}$ is NOT provided by higher layer) – re-evaluation and pre-emption checking for aperiodic transmission

**Background**: For UE with aperiodic traffic, data packets could arrive at any time for SL transmission without any prior knowledge. Therefore, it is not possible for a power constrained UE to predict and perform monitoring of slots before the resource selection trigger. From reviewing the contributions submitted to this meeting, in general, there are two partial sensing schemes, but both based on sensing in a contiguous manner.

### Proposals before 1st check point (Jan 28)

|  |  |
| --- | --- |
| Option 1 | Option 2 |

**Proposal 5:**

* When resource selection is triggered in slot n and resource reservation interval ($P\_{rsvp\\_TX}$) is NOT provided from higher layer,
	+ Option 1: In slot n, UE performs random resource selection
		- For a UE that performs sensing and for the purpose of re-evaluation and pre-emption checking, the UE monitors slots starting from n+1 until $m –T\_{3}$ before the last transmission for the TB, except for slots in which its own SL and UL transmissions occur
	+ Option 2: In slot $n+T\_{A}-T\_{proc,1}^{SL}$, UE reports a set of candidate single-slot resources (*SA*) to the higher layer after performing resource exclusion based on sensing results obtained during $[n+1,n+T\_{A}-T\_{proc,1}^{SL}-T\_{proc,0}^{SL}]$ for resource selection within the resource selection window $[n+T\_{A},n+T\_{2}]$.
		- Alt. 1: $T\_{A}=32$ is fixed
		- Alt. 2: $T\_{A}$ is dependent on the remaining PDB
		- Alt. 3: FFS $T\_{A}$
		- Alt. 4: $T\_{A}$ is based on received HARQ feedback
		- For re-evaluation and pre-emption checking, the UE monitors slots starting from n+1 until $m –T\_{3}$ before the last transmission for the TB, except for slots in which its own SL and UL transmissions occur
* Option 1 and Option 2 are both supported, or only one option is supported
	+ FFS how UE selects Option 1 or 2 when both are supported

|  |  |  |
| --- | --- | --- |
| **Company** | **Option 1, 2 or both** | **Comments** |
| OPPO | Option 1 and option 2 | We are OK with these two options in principle. While we suggest to discuss the details later.  |
| Fraunhofer | Both | We are fine with the proposal, since both option 1 and 2 are possible actions that can be done by type D UEs.  |
| Apple | Both with modifications | In both options, the sensing for resource re-evaluation could be starting from m-32 to m-T3 just to avoid the collision with aperiodic resource reservation. Specifically, In Option 1, the sensing does not start at n+1, rather start from m-32. In Option 2, the sensing for resource selection is from n+1 to n+TA-Tproc,1 and the sensing for resource re-evaluation is from m-32 to m-T3. |
| Ericsson | Option 1 and Option 2 | We are OK to support both options and the conditions to trigger each of them when supported by the UE, but at this point further discussion on $T\_{A}$ is necessary. Thus, our proposal is to include Alt. 4 in in the Proposal 5. (Alt. 4: T\_A is based on received HARQ feedback) |
| InterDigital | Both | We are ok with the proposal and support both options. |
| CATT | Both (but details needs to further modified) | Details needs to be further discussed. Particularly, for option 1 we think it should be FFS on whether to support re-evaluation and pre-emption for UEs perform sensing but operate random selection. This incurs more power consumption with no performance gain. |
| Qualcomm | Both options | We observed that both schemes provide significant performance for the power saving UE over random selection only. We also note that Option 1 could be viewed as a special case of Option 2 where TA = 0.We share the view that details should be discussed later and suggest a more general proposal to agree on the principle without yet defining the precise timeline. That discussion would also include what can be left up to UE implementation.  |
| Lenovo&MM | Both options | Both options should be considered at this stage. |
| CMCC | Both | We are ok with both options.  |
| NEC | Both are ok | Firstly, in the main bullet, for aperiodic traffic, $P\_{rsvp\\_TX}$ may be provided by higher layer with 0ms. Secondly, in the first option, the monitoring window can be FFS between [n-1, m-T3] or [m-32, m-T3], because if the first selected resources m is in later of the selection window, it's possible that m-32 > n – 1, then UE can start to monitor from m-32 to save power. |
| vivo | Both (but needs more discussion and clarifications on details) | Just to make sure if we understand correctly. Option1 is to perform resource selection first and then re-evaluate the resources being selected. Option 2 is to do sensing first, use the sensing results for resource selection, and possibly also re-evaluate the selected resources. If so, then we are fine with the principle of two options. But more clarifications on the start/end of sensing and details such as the value of $T\_{A}$ are needed.‘UL’ transmission should be removed. |
| ETRI | OK with Both | At this point, we are OK with both. Details should be discussed further. |
| Panasonic | Both |  |
| Sony | Both options | We are OK with both options. |
| NTT DOCOMO | Option 1 as random selectionOption 2 as partial sensing | We are OK with directions of both options. Two comments below.* Option 1 does random selection first and then re-evaluation/pre-emption check will be performed, right? If correct, this option 1 is one of random selection mechanism, not partial sensing in my understanding based on the agreements at the last meeting. Clarification is preferred.
* For option 2, Alt 3 is preferred. In this meeting, details can be FFS.
 |
| CAICT | Option1 and Option2 | Both options can be supported and FFS the details of the two options. |
| Sharp | Both | Basically, we share similar view as vivo. Besides, the last transmission seems not clear enough to us, since MAC layer provides the selected SL grant and the UE is not able to know which resource within the grant would be the last transmission when doing the re-evaluation/pre-emption check. Thus, we propose to define m as the last resource within a period. |
| Xiaomi |  | From our point of view, if T2 is large enough, e.g. 100ms, UE can change the start of selection window to T+32. Any collision from aperiodic traffic can be thus avoided. |
| ZTE | Option 2 | We agree with option 2 but we think re-evalution/pre-emption is an independent issue which is irrespective to short term sensing discussion. |
| LGE | Option 2 with modification | Option 2 is generally ok, but the following modifications are necessary.* TA = max interval between resources that can be indicated by a SCI.

We didn’t make any decision on the content of SCI, so it’s safer at this stage to say TA is based on the SCI content. If Rel.16 SCI rule is reused, TA is 31 slots.* TA < T2 < remaining PDB
	+ Otherwise resource re-evaluation and pre-emption checking are not performed.
* Short-term sensing is performed over [mk-TA, mk-T3] for k=0,…,K, where mk is the timing of the k-th reserved resource and K is the number of reserved resources.

If the selected resources are apart from each other more than TA, sensing over a duration exceeding TA is not performed for power saving. |
| Samsung | Both | We are OK with both options at high level and the details can be discussed later. We agree with QC’s comment that use a more general proposal to agree on principle without touch exact timing. |
| Fujitsu | Option 2 | For re-evaluation and pre-emption checking, as we commented in proposal 4, the range of sensing slots depends on whether pre-emption is enabled or not in current resource pool. |
| MediaTek | Option 2 | We support Option2. |
| Intel | Please see comments | In our understanding, RAN1 needs to decide on start time for partial sensing window (e.g. time instance ‘n+1’) and end time of partial sensing window that may be dependent on ether time instance of last retransmission or HARQ ACK feedback. Other details are already covered by Rel.16 procedure for resource selection. Separately RAN1 can discuss whether min bound on partial sensing window size needs to be introduced or can be left up to UE implementation.In addition, in resource pools with disabled semi-persistent reservations UE may still have periodic traffic with predictable arrival time and thus resource reselection trigger time instances. In such cases UE can start partial sensing at time instance [n-32] i.e. before resource reselection trigger. **We ask feature lead to add this option for RAN1 discussion/consideration**. |
| Huawei,HiSilicon | Both options could work with modifications. Only one of them would be chosen. | For the main bullet, similar as our comments above in proposal 2, a UE cannot predict the next transmission is periodic or aperiodic before a TB reception in PHY. So the provision of resource reservation interval which is transported along with the TB cannot be a judgement for traffic type, periodic or aperiodic.The proposal should have an applicability to partial sensing being configured.For option 1 and option 2, it should be clarified what the scenario is under discussing. The whole issue of 3.5 is under partial sensing agenda which means all the options should take the partial sensing procedure into account. Specifically, for option 1, we think the random selection is different from what is defined in Rel-14. Considering the partial sensing procedure which Y candidate slots are selected in PHY as SA and reported to MAC, MAC would only randomly select a set of resources among the reported SA and instruct the PHY to re-evaluate the set of resources. So the starting point of sensing window would not relate to slot n+1 only but involve ty0, the first candidate resource. That is the window should start from max (ty0-31, n+1) to $m –T\_{3}$.Similarly, for option 2, the windows for resource selection and re-evaluation should be designed separately. A UE in PHY needs to report candidate resource set to MAC before the first slot among Y candidate slots. Therefore, the window for resource selection should start from max (ty0-31, n+1) until ty0 - tproc,0 –T1.Option 2 has a problem that sensing from before the defined interval appears not to be considered. On the other hand, as we explained in other questions, it is no need to consider UL transmission to determine candidate slots, and SL transmission impact can be handled by UE implementation. Therefore, we suggest two options are changed as following.* + Option 1: In slot n, UE performs random resource selection
		- For a UE that performs sensing and for the purpose of re-evaluation and pre-emption checking, the UE monitors slots starting from ~~n+1~~ max (ty0-31, n+1) until $m –T\_{3}$ before the last transmission for the TB, except for slots in which its own SL and UL transmissions occur
	+ Option 2: In slot $n+T\_{A}-T\_{proc,1}^{SL}$, $t\_{y0}-T\_{1} $UE reports a set of candidate single-slot resources (*SA*) to the higher layer after performing resource exclusion also taking into account ~~based on~~ sensing results obtained during $[n+1,n+T\_{A}-T\_{proc,1}^{SL}-T\_{proc,0}^{SL}]$ $[max⁡(t\_{y0}-31,n+1),t\_{y0}-T\_{proc,0}^{SL}-T\_{1}]$ for resource selection within the resource selection window $[n+T\_{A},n+T\_{2}] [n+T\_{1},n+T\_{2}]$.
		- For re-evaluation and pre-emption checking, the UE monitors slots starting from ~~n+1~~ $t\_{y0}$ until $m –T\_{3}$ before the last transmission for the TB, except for slots in which its own SL and UL transmissions occur
 |
| Convida Wireless | Both options 1 and 2 | We are fine with both option 1 and option 2. |
| Bosch | Both, Option 1 & 2 | We are also fine with both options. |
| Nokia, NSB | Both options | Both option 1 and option 2 shall be supported in general for partial sensing. We shall agree the general principle and then work out the details, especially for option 2.  |

**Proposal 5’:**

* When resource (re-)selection is triggered in slot n and resource reservation interval ($P\_{rsvp\\_TX}$) is NOT provided from higher layer,
	+ Option 1: In slot n, UE performs random resource selection
		- For re-evaluation and pre-emption checking, the UE monitors slots after the random resource selection
			* FFS details of the monitoring, including timing, duration and exceptions
	+ Option 2: For the purpose of resource (re-)selection, the UE monitors slots between $[n+1,n+T\_{A}]$ and performs resource selection based on sensing results.
		- FFS $T\_{A}$ and remaining details
		- For re-evaluation and pre-emption checking, the UE monitors additional slots.
			* FFS details of the additional monitoring, including timing, duration and exceptions
	+ Other options are not precluded
	+ FFS which one or multiple option(s) to be supported

|  |  |
| --- | --- |
| **Company** | **Comments** |
| OPPO | We support FL’s proposal. |
| NEC | We support the proposal 5' with following suggestions.* Resource reservation interval ($P\_{rsvp\\_TX}$) = 0 ms is preclude in 3.2, 3.3 and 3.5, we think $P\_{rsvp\\_TX}$ = 0 ms is the aperiodic case and should added in the main bullet of this proposal.

In Option 1: For re-evaluation and pre-emption checking, the UE monitors slots after the resource selection trigger. |
| NTT DOCOMO | We support the proposal with update in main bullet as* When resource (re-)selection is triggered in slot n and resource reservation interval ($P\_{rsvp\\_TX}$) is NOT provided from higher layer or resource reservation interval ($P\_{rsvp\\_TX}$) = 0 is provided from higher layer,
 |
| LGE | We support FL’s proposal and both options.Option 1 can be used as a random resource selection if e.g. remaining PDB is not sufficient for constructing a sensing window [n+1, n+TA] followed by a resource selection window.If the remaining PDB is sufficient, option 2 can be used rather than random resource selection as it guarantees the sensing duration [n+1, n+TA] before resource (re)selection. |
| Apple | We think this proposal discusses two different parts: resource selection and resource re-evaluation/pre-emption checking. Option 1 and Option 2 are differentiated at resource selection, while the sub-bullets of Option 1 and Option 2 are targeted for resource re-evaluation/pre-emption checking. We suggest removing the resource re-evaluation/pre-emption checking part in this proposal (i.e., sub-bullet of Option 1 and the second sub-bullet of Option 2) to make the proposal focusing on resource selection only. A separate proposal could be made on resource re-evaluation/pre-emption checking.  |
| ETRI | We support FL’s proposal with including ‘0 ms’ case. |
| Qualcomm | We support the general direction and would like to propose the following change to Option 2 so that it remains general at this point, similar to Option 1:* + Option 2: For the purpose of resource (re-)selection, the UE monitors slots between $[n+1T\_{B},n+T\_{A}]$ and performs resource selection based on sensing results.
		- FFS $T\_{A}$, $T\_{B}$ and remaining details
		- For re-evaluation and pre-emption checking, the UE monitors additional slots.
			* FFS details of the additional monitoring, including timing, duration and exceptions

For re-evaluation and pre-emption checking in Option 1, we agree with the feature-lead’s wording of sensing after resource selection.We’d like to add a sentence to clarify that these options are in addition to random selection without any sensing or re-evaluation/pre-emption checking:* + FFS which one or multiple option(s) to be supported
	+ These options are in addition to random selection only without sensing or re-evaluation and pre-emption checking.
 |
| Fujitsu | We are generally fine with the proposal but with the following concerns:For option 2, if both periodic and aperiodic traffics are ongoing in the resource pool, the UE also needs to monitor the slots in the sensing occasions corresponding to the Y candidate slots. Otherwise, collision(s) between the UE’s aperiodic transmission and other UE’s periodic transmission may happen.  |
| Xiaomi | We support the changes proposed by QC. |
| Panasonic | We support FL’s proposals.  |
| CMCC | Support the FL’s proposal. |
| Samsung | We agree with the proposal in principle. In addition, we have similar view with QC on modifying n+1 to n+TB. |
| Ericsson | We are supportive of the current proposal from the FL and our position is to support both Option 1 and Option 2 and study the conditions that trigger them. |
| Sony | We support FL’s proposal. |
| ZTE | Agree FL’s proposal with another option added.We think the re-evaluation and pre-emption checking is independent of the short term based monitoring. After resource (re)selection based on short term sensing, whether perform re-evaluation and pre-emption checking can be based on (pre-)configuration or up to UE implementation. So we suggest to add option 3 as following: * + Option 3: For the purpose of resource (re-)selection, the UE monitors slots between $[n+1,n+T\_{A}]$ and performs resource selection based on sensing results.
		- FFS $T\_{A}$ and remaining details
 |
| Vivo | support the changes proposed by Qualcomm |
| Huawei, HiSilicon | First of all, the proposal should have an applicability to partial sensing being configured, and then a UE can perform this RA for resource selection based on either options. Both options can work, However, specification does not necessarily need to define two options in parallel.On the other hand, the proposal should separate resource selection and revaluation/pre-emption checking. We have the sympathy with others that RAN1 could focus the resource selection design, because it is still under FFS on conditions(s) in which re-evaluation and pre-emption checking can be performed, i.e. a UE with reduced-sensing RA may not always perform re-evaluation/pre-emption checking. The specification should aim to have a unified solution for a UE performing partial sensing RA regardless of its own traffic is aperiodic or periodic, because the sensing procedure is intended to detect other UE’s resource reservation, which can be aperiodic and/or periodic. The short sensing window, which was introduced to cover aperiodic reservation made by other UEs, should be same for both aperiodic and periodic service. For option 2, the starting point of the short sensing window may be not always slot n+1. Considering partial sensing, a UE should report the candidate resource set to MAC layer before $t\_{y0}$, and first resource for transmission might be $t\_{y0}$ . To cover the most relevant 31 slots just before $t\_{y0}$, the starting point could be $t\_{y0}-31$. In addition, the ending point may be not only associated with slot n, but also with $t\_{y0}$. Therefore, we suggest the proposal is changed as following.**Proposal 5’:** * If UE is configured to perform partial sensing, and when resource (re-)selection is triggered in slot n ~~and resource reservation interval (~~$P\_{rsvp\\_TX}$~~) is NOT provided from higher layer~~,
	+ Option 1: In slot n, UE performs random resource selection in physical layer
		- ~~For re-evaluation and pre-emption checking, the UE monitors slots after the random resource selection~~
			* FFS details of the monitoring (if any), including timing, duration and exceptions
	+ Option 2: For the purpose of resource (re-)selection, the UE monitors slots between $[max⁡(n+1, t\_{y0}-31),n+T\_{A}]$ and performs resource selection based on sensing results, $t\_{y0}$ is the first slot in the set of Y candidate slots.
		- FFS $T\_{A}$ and remaining details
		- ~~For re-evaluation and pre-emption checking, the UE monitors additional slots.~~
			* ~~FFS details of the additional monitoring, including timing, duration and exceptions~~
	+ Other options are not precluded
	+ FFS which one or multiple option(s) to be supported
 |
| Fraunhofer | We support the FL’s proposal. |
| Interdigital | We are ok with the proposal and support both options. |
| CATT | For option 1, we are not sure if ‘re-evaluation and pre-emption checking’ is needed here. From our evaluation, it does not have much gain and is negative for power consumption. We would prefer to remove the corresponding words:Option 1: In slot n, UE performs random resource selection FFS details of monitoring |
| Convida Wireless | We are fine with FL’s proposal. |
| Nokia, NSB | We support Option 1 and Option 2 in principle. Suggest removing the “re-evaluation and pre-emption checking” part for both Option 1 and Option 2. We shall focus on the resource selection in this proposal. The “re-evaluation and pre-emption check” can be another proposal for further discussion.On QC’s proposal to modify the sensing window from $[n+1, n+T\_{A}]$ to $[n+T\_{B}, n+T\_{A}]$ for Option 2, not sure whether this is necessary. If power saving is a concern to limit the sensing window, UE can choose Option 1 with random selection. |

### Proposals before 2nd check point (Feb 2)

FL observations and comments based on inputs received in Sec. 3.5.1:

* Please check the background description in at the beginning of Section 3.5 and also the accompany email sent for discussion before the 2nd check point.
* In short, this proposal targets a scenario where resource (re)selection is triggered by higher layer in slot n for aperiodic transmission in a resource pool that allows partial sensing and/or random resource selection, where
	+ resource pool is (pre-)configured for either periodic + aperiodic, or aperiodic transmissions only,
	+ resource pool is (pre-)configured with partial sensing and/or random resource selection

The UE performs contiguous partial sensing and/or random resource selection for resource (re)selection.

* This version is based on the latest text we discussed during Friday’s GTW session (Jan 29), and a new term (contiguous partial sensing) is added to aid with the discussion.
* During the last Friday GTW session,
	+ A comment was made on not needing any other partial sensing scheme beside a LTE-V like partial sensing for aperiodic traffic. Do you think the above is a valid operating scenario that requires a contiguous partial sensing solution for aperiodic transmission?
	+ There was a hint of suggestion or wish to combine the discussion between contiguous partial sensing for periodic transmission and contiguous sensing for aperiodic transmission. Do you agree to combine the discussion together or to discuss separately?

**Proposal 5’’:**

* In a resource pool (pre-)configured with at least partial sensing and/or random resource selection, if UE is configured to perform contiguous partial sensing (i.e., at least for the case of resource reservation interval is NOT provided or $P\_{rsvp\\_TX}=0$) by higher layer, when resource (re-)selection is triggered in slot n, support the following option:
	+ Option 1: For the purpose of resource (re-)selection, the UE monitors slots between $[n+T\_{A},n+T\_{B}]$ and performs resource (re)selection based on sensing results.
		- FFS $T\_{A}$, $T\_{B}$ (including the possibility of equal to zero) and remaining details
			* When both $T\_{A}$ and $T\_{B}$ are equal to zero, random resource selection is performed
	+ FFS interaction with SL-DRX
	+ Other options are not precluded
	+ This option is in addition to random resource selection only without sensing or re-evaluation and pre-emption checking

|  |  |
| --- | --- |
| **Company** | **Comments** |
| OPPO | Firstly, We would like to add a sub-bullet as follows since the re-evaluation and pre-emption checking should be combined with the contiguous partial sensing. Especially for the case of $T\_{A}$, $T\_{B}$ equal to 0, in that case, random resource selection is performed and re-evaluation and pre-emption checking is the only way to avoid collision. * + FFS re-evaluation and pre-emption checking in addition to the contiguous partial sensing

Secondly, we would like to clarify that the resource (re)selection is based on all available sensing results. * + Option 1: For the purpose of resource (re-)selection, the UE monitors slots between $[n+T\_{A},n+T\_{B}]$ and performs resource (re)selection based on all available sensing results.

The sensing results can include the contiguous partial sensing and periodic-based partial sensing. If the RP allows periodic and aperiodic traffic, the UE can do periodic-based partial sensing for periodic transmission all the time. If an aperiodic traffic arrives at slot n, the UE can additionally do contiguous partial sensing. Then the resource selection can be based on all the available sensing results.  |
| LGE | We agree with OPPO’s second point. As we commented on Friday GTW, UE can have both periodic traffic and aperiodic traffic depending on the services of UE interest. In this case, UE can perform in parallel the periodic-based partial sensing for periodic traffic, and the contiguous partial sensing for aperiodic traffic. At slot n, when UE is triggered to transmit an aperiodic traffic, UE can perform contiguous partial sensing as in Proposal 5”. But at the time of resource (re)selection, there could be available periodic-based partial sensing results due to other periodic transmission. Then, it’s reasonable to use those periodic-based partial sensing results if available, in addition to the contiguous partial sensing results. In this way, UE can avoid any collision with periodic traffic allowed in resource pool, for its aperiodic transmission. Therefore, we propose the following modification for option 1.* + Option 1: For the purpose of resource (re-)selection, the UE monitors slots between $[n+T\_{A},n+T\_{B}]$ ($T\_{A}\geq 0$, $T\_{B}\geq 0$) and performs resource (re)selection based on all available sensing results at the time of resource (re)selection.
		- When both $T\_{A}$ and $T\_{B}$ are equal to zero,
			* if there is no available sensing results at all, random resource selection is performed
			* otherwise, resource (re)selection is performed based on the available sensing results
		- FFS whether all or part of $[n+T\_{A},n+T\_{B}]$ is used for contiguous partial sensing
		- FFS remaining details

In this sense, as long as UE is capable of sensing, even if $T\_{A}$ and $T\_{B}$ are equal to zero, resource (re)selection can be based on periodic-based sensing results if available. If there are no sensing results available at all for UE, UE can do random selection.Clarification added for TA and TB, which can be positive or zero. |
| NTT DOCOMO | * Regarding OPPO’s second point and relative LGE’s comment,

we think their point is that:some other sensing results may be available, may not. If available, the results should also be used. The FL’s proposal is made under the assumption that periodic-based partial sensing for aperiodic transmission is impossible since UE cannot know when the traffic comes. Under the assumption, the UE may do periodic-based partial sensing for other periodic traffic, or may do contiguous partial sensing for other aperiodic traffic in the past. In this case, the sensing results (if any) can be used as well.If the above is correct understanding, we are OK with the direction but mandatory/optional should be mentioned clearly. In my understanding, the sensing results of $[n+T\_{A},n+T\_{B}]$ is mandatorily used but other sensing results are up to UE since the monitoring is up to UE. For example, \*\*\** + Option 1: For the purpose of resource (re-)selection, the UE monitors slots between $[n+T\_{A},n+T\_{B}]$ and performs resource (re)selection based on at least the sensing results.
		- If other sensing results are available, UE can use the results for resource (re)selection.

\*\*\** Regarding OPPO’s first comment, we agree with it. At least FFS for re-evaluation/pre-emption should be added; otherwise, TA=TB=0 is completely same as just random selection, which has already been agreed.
* For limitation of aperiodic traffic to be transmitted from the UE, we think it is reasonable one. For periodic traffic, UE should monitor slots before slot n even for contiguous partial sensing, while for aperiodic traffic, n=0 or after is possible only for contiguous partial sensing.

If still joint discussion is preferable, minus values of TA, TB can be used: for example, (update from FL’s proposal for easy discussions,)\*\*\** In a resource pool (pre-)configured with at least partial sensing and/or random resource selection, ~~if UE is configured to perform contiguous partial sensing (i.e., at least for the case of resource reservation interval is NOT provided or~~ $P\_{rsvp\\_TX}=0$~~) by higher layer,~~ when resource (re-)selection is triggered in slot n, support the following option:
	+ Option 1: For the purpose of resource (re-)selection, the UE monitors slots between $[n+T\_{A},n+T\_{B}]$ and performs resource (re)selection based on sensing results.
		- FFS $T\_{A}$, $T\_{B}$ (including the possibility of equal to zero or minus) and remaining details
			* When both $T\_{A}$ and $T\_{B}$ are equal to zero, random resource selection is performed
			* $T\_{A}<0$ is applicable only when resource (re-)selection is triggered in slot n and resource reservation interval ($P\_{rsvp\\_TX}$) is provided from higher layer and $P\_{rsvp\\_TX}\ne 0$
 |
| Apple | Overall, we are fine with this proposal, i.e., contiguous partial sensing is needed to avoid the collision from aperiodic resource reservation. We have two clarification questions related to “contiguous partial sensing”: Can a UE be configured with “contiguous partial sensing” and “periodic-based partial sensing” simultaneously? We know a resource pool is configured to support “partial sensing”, “full sensing” and “random selection”. How could UE’s configuration of “contiguous partial sensing” or “periodic-based partial sensing” be aligned with resource pool’s configuration?  |
| Fujitsu | We are fine with the proposal in general with some concerns regarding the first sub-bullet.* For the first sub-bullet, we share the similar view as OPPO and LGE. The current wording sounds like that resource (re-)selection for aperiodic transmission is purely based on sensing results of the monitored slots between $[n+T\_{A},n+T\_{B}]$. However, if both periodic and aperiodic traffics are configured to be transmitted in the same resource pool, the sensing results of periodic occasions should also be taken into account. We are fine with the wording suggested by OPPO.
 |
| CAICT | We are OK with the proposal in general. In our understanding, if this type of continuous partial sensing is co-existing with LTE-V based partial sensing where slots before “n” might have been sensed, resource selection can be carried out based on the available sensing results in the sensing window *[t-T0, t]* where *t* stands for the starting time of the resource selection window. There is no necessity to include all the available sensing results and we think the sensing window definition in the full sensing scenario can be re-used here.  |
| vivo | We share a similar view as DOCOMO that if the resource (re)selection is triggered for aperiodic TX at slot n, the sensing results of contiguous partial sensing within $[n+T\_{A},n+T\_{B}]$ should be mandatorily used. If there are other available sensing results for other periodic/aperiodic TX purposes, whether to use these sensing results can be up to UE implementation. We suggest some refinements on top of DOCOMO’s wording.* In a resource pool (pre-)configured with at least partial sensing and/or random resource selection, if UE is configured to perform contiguous partial sensing (i.e., at least for the case of resource reservation interval is NOT provided or $P\_{rsvp\\_TX}=0$) by higher layer, when resource (re-)selection is triggered in slot n, support the following option:
	+ Option 1: For the purpose of resource (re-)selection, the UE monitors slots between $[n+T\_{A},n+T\_{B}]$ and performs resource (re)selection based on at least the sensing results within $[n+T\_{A},n+T\_{B}]$.
		- If other sensing results are available, it is up to UE implementation to ~~UE can~~ use the results for resource (re)selection.
 |
| ZTE, Sanechips | We are fine with this proposal except the last bullet, we suggest to change to:* + FFS for random resource selection only without sensing or re-evaluation and pre-emption checking
 |
| Fraunhofer | We are supportive of the proposal in general, and agree with LG and and Docomo that the UE should be able to use any sensing information available for resource (re-)selection. |
| Nokia, NSB | To the FL’s question on the need of continuous partial sensing for aperiodic traffic, we think that there is need. A UE may have periodic/aperiodic traffic. The aperodic traffic may use the perodic sensing and the continuous partisl sensing.We are generally fine with this proposal with some minor suggestions. i) support companies’ proposal to add “all available” before the “sensing results in Option 1. ii) When $T\_{A}=0$ and $T\_{B}=0$, random selection is performed when there is no other resource sensing results.  |
| Qualcomm | We propose the same change about sensing and configuration and we agree with OPPO’s addition on using all available sensing information. Finally, T\_A and T\_B could be negative and we’d like to clarify this. This is for the case when a packet arrives and the UE has to base its transmission on prior sensing results only, e.g. due to PDB constraints or DRX considerations.In a resource pool (pre-)configured with at least partial sensing and/or random resource selection, if UE ~~is configured to~~ performs contiguous partial sensing (i.e., at least for the case of resource reservation interval is NOT provided or $P\_{rsvp\\_TX}=0$) by higher layer, when resource (re-)selection is triggered in slot n, support the following option:* Option 1: For the purpose of resource (re-)selection, the UE monitors slots between $[n+T\_{A},n+T\_{B}]$ and performs resource (re)selection based on all available sensing results.
	+ FFS $T\_{A}$, $T\_{B}$ (including the possibility of equal to zero or negative values) and remaining details
		- ~~When both~~ $T\_{A}$ ~~and~~ $T\_{B}$ ~~are equal to zero, random resource selection is performed~~

We also think it’s important to capture that re-evaluation checking is still FFS and hasn’t been precluded:* FFS Applicability and details of re-evaluation checking.
 |
| NEC | 1. We are OK to add the re-evaluation checking for FFS.2. For the posibble sensing results for periodic transmission, we're fine to add FFS point like "FFS usage of other avaible sensing results besides results from [n+TA, n+TB]", in other words, details can be FFS next meeting. |
| Huawei, HiSilicon | First of all, we suggest to focus on the partial sensing functionality in this proposal. As commented in the last GTW, whether/how to perform random selection when partial sensing is configured should have more investigations, and the necessity or conditions of switching between partial sensing and random selection is not clear and needs further discussion. So the sub-bullet “*When both T\_A and T\_B are equal to zero, random resource selection is performed*” in option 1 should be removed.For the main bullet, same as our comments for proposal 2’’ and proposal 3’’, the condition assuming different $P\_{rsvp\\_TX}$ values in slot n can trigger how/when to perform partial sensing is not correct. It is not reasonable to clarify the resource allocations schemes by the traffic type, a unified design, which no matter which traffic type it is, the UE could select the resources based on the sensing results in slots $t\_{y-k×P\_{reserve}}^{SL}$ and the short sensing window should be adopted. At this point, we share the similar views with OPPO, LGE and others, all availiable sensing results can be used for resource selection regardless of its traffic type and the content in the parentheses needs to be removed. As DCM explained, the sensing results from the sensing window is mandatory to be used, however, it is not necessary. Sensing results from both the short sensing window and periodic sensing oaccassions can be used for resource selection, how to use them can be up to UE implementation, not need to specify which part is mandatory. Since a uniform design and common sensing procedure for both aperiodic and periodic traffic, it is not necessary either to define the window starting from slot n, as others comments, T\_A and T\_B may be negative values. For simplicity, window size could define as $[T\_{A},T\_{B}]$, how to define T\_A and T\_B including reference starting point can be discussed in the next meeting.We suggest the proposal to have following changes:* In a resource pool (pre-)configured with at least partial sensing ~~and/or random resource selection~~, if UE ~~is configured to~~ performs ~~contiguous~~ partial sensing ~~(i.e., at least for the case of resource reservation interval is NOT provided or~~ $P\_{rsvp\\_TX}=0$~~) by higher layer~~, when resource (re-)selection is triggered in slot n, support the following option:
	+ Option 1: For the purpose of resource (re-)selection, the UE monitors slots between $[n+T\_{A},n+T\_{B}]$ and performs resource (re)selection based on sensing results from $[n+T\_{A},n+T\_{B}]$ and $t\_{y-k×P\_{reserve}}^{SL}$ if any.
		- FFS $T\_{A}$, $T\_{B}$ ~~(including the possibility of equal to zero)~~ and remaining details
			* ~~When both~~ $T\_{A}$ ~~and~~ $T\_{B}$ ~~are equal to zero, random resource selection is performed~~
	+ FFS interaction with SL-DRX
	+ Other options are not precluded
	+ ~~This option is in addition to random resource selection only without sensing or re-evaluation and pre-emption checking~~
 |
| Sharp | To answer FL’s questions above, we think contiguous partial sensing solution for aperiodic transmission is needed and we support to consider contiguous partial sensing for aperiodic and periodic transmission together, as HW commented during GTW and the above.We are fine with OPPO’s second point that sensing results on periodic reservation are also considered. On top of that, we share similar view as Docomo and Qualcomm that $T\_{A}$, $T\_{B}$ can be negative and should be clarified. Regarding the re-evaluation and pre-emption check, since in our understanding, , $T\_{B}$ is related to both, we propose to add both re-evaluation and pre-emption check as OPPO commented for the first point. |
| Spreadtrum | Agree with some conpany’s comments for adding “all available” in the first sub-bullet. It canbe modified as the following:* + Option 1: For the purpose of resource (re-)selection, the UE monitors slots between $[n+T\_{A},n+T\_{B}]$ and performs resource (re)selection based on all available sensing results.
		- FFS $T\_{A}$, $T\_{B}$ (including the possibility of equal to zero) and remaining details
			* When both $T\_{A}$ and $T\_{B}$ are equal to zero and there are no other resource sensing results, random resource selection is performed
 |

### Proposals before 3rd check point (Feb 4)

FL observations and comments based on inputs received in Sec. 3.5.2:

* TBD

Contribution summary

## Partial sensing for periodic transmissions

* Selection of Y candidate slots
	+ LTE-V based selection of Y ≥ min candidate slots according to Tx priority, CBR level, HARQ enabling, subcarrier spacing or re-evaluation/pre-emption enabling: [2][5][8][9][14][17][20][21][22, multiple sets of Y][25][29]
	+ Same as resource selection window, which size is left up to UE implementation, subject to T2min constrain on minimum size [13]
	+ If HARQ feedback is enabled, HARQ RTT related timing restriction should be considered when determining the candidate slots [17]
* Determination of sensing slots
	+ Slots that belong to (y – k\*reservation period), where y is included in Y candidate slots [2][3][4][8][11][12][13][14][28][22][25][29][34][35][6]
		- K=1, multiple, or by configuration
		- Reservation period according to the configured set of periodicity in the resource pool, or a subset
* X% of candidate resources is based on the total number candidate resources only within the Y candidate slots [2][25]
* X% for partial sensing UE is separately configured from that for full sensing UE [9]
* A short-term / extended sensing / continuous sensing (e.g., 32 slots) to account for aperiodic traffic [2][3][4][6][10][11][12][13][17][18][19][21][22][24][25][27][28][30][33][34][35][29]
	+ Option 1: before 1st candidate slot
	+ Option 2: before the resource selection in slot n
* Introduce reduced adaptive sensing windows with varying sensing intervals across time to enhance the UE's capability to save power as well as achieve adequate sensing results [16]

## Partial sensing for aperiodic transmissions

* Scheme 1: At packet arrival in slot n, UE performs random selection as well as sensing for re-evaluation and pre-emption checking until the last retransmission of a TB [2][9][10][13][14][22][32]
* Scheme 2: At packet arrival in slot n, UE performs sensing for a short period (e.g., 32 slots), then select resources based on sensing results. UE continue sensing for re-evaluation and pre-emption checking until the last retransmission of a TB [2][4][9][12][13, UE implement][14][29][32][35]
* Selection between scheme 1 and 2 (or adaptive sensing window) is based on HARQ feedback [14][30]

## Random resource selection

* When random selection is performed, re-evaluation and pre-emption checking is disabled [3][5]
* Higher priority is assigned to the resources which is randomly selected by a UE, to preserve these selected resources from being pre-empted by UEs performing sensing [6][12]
* When a resource is randomly selected, the same resource is reused periodically based on the SPS resource reservation procedure [9]
* Random resource selection should be applicable to both periodic and aperiodic transmissions [13]
	+ random resource selection is applied for initial transmission and all retransmissions of a TB
* Conditions in which random resource selection can be applied
	+ Random resource selection is enabled in a SL resource pool [13][22]
	+ One of the following criteria is met [13]:
		- UE does not have sidelink RX chain to perform sensing (i.e. sidelink TX only UE)
		- Battery level is below preconfigured threshold [22]
	+ Tx priority is within a preconfigured range of values [24]
	+ Sensing accuracy [22]
	+ Selection between random resource selection and partial sensing according to the system load [7]
	+ Selection between random resource selection and partial sensing based on a pre-configured condition, such as SL congestion, packet reliability [12][22][27]
* UE performing random resource selection should respect PSSCH to PSFCH HARQ time gap, if UE monitors PSFCH and requests for sidelink HARQ feedback, otherwise the gap can be ignored [13]
	+ UE ensures a minimum time gap Z between any two selected resources of a TB where a HARQ feedback for the first of these resources is expected
* Random resource selection preserves sidelink resource reservation signalling principle as defined for sidelink transmissions in Rel.16 [13]
	+ Maximum distance in logical slots for the first and last sidelink transmissions in a SCI is less than 32
* For random resource selection, the resources are selected among the partial sensing slots [9]
* PSFCH resources associated with the randomly selected resources are separately configured from those for full/partial sensing based selected resources [9]
* Pseudo-random frequency hopping for periodic reservation based on CRC bits of the associated PSCCH [10]
* The frequency that a UE performs random resource selection should be restricted [27]
* For random resource selection, consider partitioning of candidate SL resources to reduce collision probability [28]
* Enhancements for random resource selection [35]:
	+ Option 1: Restrict priority level for transmissions
	+ Option 2: sensing UE excludes random selection UE’s reserved resources regardless of priority
	+ Option 3: random selection based on a resource pattern

## Re-evaluation and pre-emption checking

* For the UE performing sensing, support re-evaluation for random selection resources [24] [29]
* Conditions for performing re-evaluation and pre-emption checking
	+ When multiple NACKs are received [3]
	+ ACK/NACK ratio is below a threshold [9]
	+ Re-evaluation or pre-emption checking is (pre-)configured [9]
	+ Number of partial sensing slots before resource (re)selection triggering is below a threshold [9]
	+ TX priority value is higher than the pre-emption priority value [9][24]
	+ Interference/congestion level is above a threshold [9]
* Re-valuation/pre-emption is configurable for Type D UEs [8]
* The pre-emption priority used by power saving UE is separately (pre-)configured from that used by full-sensing UE [9]
* When performing resource re-evaluation or pre-emption, burst type of resources are prioritized in resource (re)selection [9]
* The transmission resources reserved by power saving UEs are not pre-empted. Transmission resources reserved for transmissions destined to power saving sidelink UEs are not pre-empted [11]
* Due to re-evaluation and pre-emption, UE can re-select resources in noncandidate slots if aperiodic resource sensing is performed [2]
* For semi-persistent reservation, the UE can skip pre-emption for certain reservation periods. The number of skip periods is (pre-)configured per priority [24]
* UE is only required to sense in the slots in which the SL transmission may reserve a resource overlapping with the resource to be pre-empted or re-evaluated [27]
* Re-evaluation and pre-emption is based on reduced sensing performed between the UE’s resource selection time and resource re-evaluation/pre-emption checking time [29]
* Supports re-evaluation and pre-emption at least on subsequent periods [30]

## Type A UE performing PSFCH and S-SSB reception

* PSFCH (no) / S-SSB (no): [3][6][15][21][26]
	+ Reasons: maximum power saving, same as in LTE-V,
* PSFCH (no) / S-SSB (yes): [7][35]
	+ Reasons: support only broadcast which does not require HARQ feedback, S-SSB from UE synchronized to eNB/gNB is prioritized over GNSS
* PSFCH (yes) / S-SSB (yes): [9][12][14][22, S-SSB not considered][31]
	+ Reasons: reliable communication, power saving from less retransmissions, essential for communicating with others,

## Impact of SL-DRX on partial or full sensing

* SL-DRX parameters should be exchanged between Tx and Rx UEs for the purpose of aligning resource selection of Tx UE and the DRX ON period of Rx UE [2][5][6][9][11][18][27][29][30]
* If sensing is limited within DRX ON period, sensing accuracy and resource collision will be affected [2][3]
* PSCCH monitoring for sensing should be allowed during SL-DRX inactive period [2][3][5]
* DRX may increase latency for full sensing UEs [7]
* SL DRX and partial sensing are independent operation. SL DRX and partial sensing operation are specified separately from each other in Rel.17 [9][21][24]
* If the sensing is not restricted by DRX operation, then there will be no impacts on the resource selection [10]
* The full-time SL sync search should be avoided during SL DRX operation for power saving [12]
* The design of SL DRX cycle needs to ensure that UE partial sensing behavior is respected (i.e. UE wake up time intervals for the purpose of partial sensing need to be aligned with On duration intervals, as well as traffic characteristics) [13][17][21][22]
* No separate TX/RX alignment procedure is specified in RAN1 for partial sensing [14]
* The (partial) sensing operation and the resource selection performed by a UE takes into account the active time defined by SL DRX configuration, if (pre-)configured [14][16][17][20][21][29][30]
* The very initial transmission should be within the current “Active Time” of the Rx UE [17]
* It should be left to the UE’s implementation to decide whether sensing is limited to its DRX active time interval or it can also be performed outside of the active time [32]
* Consider PSCCH is used to align sidelink DRX wake-up time between TX UE and RX UE(s) [28]
* Sensing slots corresponding to selection target shall be included in DRX on-duration of the TX-UE [35]
	+ If a sensing slot is not included in DRX on-duration, the corresponding selection target is excluded from identified resource set of the resource allocation
	+ If a selection candidate is not included in DRX on-duration of RX-UE, the candidate is excluded from identified resource set of the resource allocation
	+ If PSFCH occasion corresponding to a selection candidate is not included in DRX on-duration of PSCCH/PSSCH TX-UE, the candidate is excluded from identified resource set of the resource allocation
* UE can perform sensing during the part of sensing window within the DRX active time only, in case of periodic traffic with PDB ≥ 100ms [38]

## Resource pool configuration with mixed RA

* A priority threshold is configured for a resource pool, at which reduced sensing UEs can select resources in a pool configured for mixed types of RA [3]
* Power constrained UEs occupy a sub-pool of the shared resource pool [7][11]
* Separation of resources is (pre-)configured where a specific portion of resource pool is allocated for each resource allocation mechanism (e.g., smaller bandwidth/frequency resource) [14][15][16][20][24]
* Different RSRP thresholds or increased RSRP threshold value is (pre-)configured for different resource selection scheme [25][29]
* UE reports whether one candidate resource overlaps with resources reserved by random resource selection UE to higher layer for further resource selection [25]
* A non-sensing UE sharing a resource pool with sensing UEs shall select/reserve resources for consecutive transmissions with a separation/gap large enough so that the sensing UE can react accordingly if a collision happens [14][24]
* Resource pool should not be shared among random selection UE and UEs configured with other RA schemes, unless random selection UE can reserve resources by sending reservation indication [21]

## Wake-up / go-to-sleep signals for SL-DRX

* Introduce wake up / go to sleep indication on sidelink (or keep sleep / keep awake indication) signals/triggers for UE power saving management [2][12][13][18][23]
	+ Reuse the existing R16 WUS/GTS principle [2]

## Congestion control for partial sensing

* CBR could be measured with fewer OFDM symbols in a slot to save power [3]
* Calculation of CBR/CR should take the reception time (e.g., DRX ON duration) into account [6][22]
* For UE with no PSCCH/PSSCH reception capability or number of sensing slots is less than a threshold, a (pre-)configured CBR value is used for PHY parameter selection [9]
* CBR measurement calculation is based on number of sub-channels of the partial sensing slots within the measurement window [9]
* Restriction of transmission parameter based on the CBR measurement is performed per active period of a DRX cycle [18]
* The evaluation of CR and the definition of CR\_limit for power saving resource allocation schemes reuse the design for full sensing resource allocation schemes [29]

## Inter-UE coordination for power saving

* Inter-UE coordination should be used for power saving as well, where a UE selects resources based on coordination / assistance information from another UE [3][7][16][18][19][20][22][31]
* Inter-UE signaling to negotiate sidelink resources (e.g. PSCCH monitoring intervals) where UE(s) are expected to monitor PSCCH resources and perform sensing for sidelink communication [13]
* The resource allocation for power saving considers new aspects introduced in Rel-17 NR sidelink such as inter-UE coordination, sidelink DRX and so on [28]
* Support a UE informing other UEs of its reception and transmission availability [32]

## Indication of power-saving UE transmissions

* Using a reserved bit in SCI to indicate the type of UE or RA scheme [9][10][11][24]

## Other techniques for power saving

* Power control
	+ SL pathloss based OLPC for PSFCH [6]
* UL/SL prioritization procedure
	+ A (pre)configured offset value can be added to the priority value of P-UE’s SL TX to avoid the frequent dropping [9]
* SL processing and transmission capability
	+ Support of PSSCH TX with 2 layers, high modulation order, and SL-SSB TX can be reduced [9]
* Power saving in SL data reception
	+ A monitoring interval and a retransmission interval in a period are (pre-)configured. The first transmission of a TB is always limited in the monitoring interval. Only the retransmissions of a TB are allowed in the retransmission interval. Thus, a receiving UE only receives/decodes PSCCHs/PSSCHs in the monitoring interval and then determines whether to turn on in the retransmission interval [10]
* Longer PSFCH period for power limited UE [6][4]
* The CSI reporting procedure and HARQ-ACK based (re)transmission should be enhanced to ensure that the CSI report/retransmission can be received by the CSI requesting UE with discontinuous reception [6]
* Reserved bits of SCI format 1-A can be used to transmit some bits of the destination ID (shortened destination ID) [7][16]
* The second stage SCI contains a field to indicate when the UE is expected to receive the next transmission [7]
* NR supports adaptation(switching) of sidelink power saving resource allocation schemes in time (i.e. b/w random, partial or full sensing-based resource selection) [13][12][22][8]
* Introduce the notion of sidelink power saving states / modes and associate with these states / modes certain set of sidelink power saving features developed in Rel.17 [13]
* Sidelink bandwidth / slot adaptation for transmission / reception is supported as a power saving feature [13]
* To utilize the geographical location of group UEs and destination-L2 ID, as the reference parameters for partial sensing, in the application layer connection-less group. And to utilize the destination-L2 ID, as the reference parameter for partial sensing, in the application layer managed group [17]
* Cross-slot scheduling enhancement for power saving purpose [18]
* Dedicated BWP can be configured for power saving UEs and S-SSB BW should be (pre-)configured within the dedicated BWP [21]
* Reduced max number of retransmission per TB for power saving UEs [22]
* Support different initial RSRP thresholds for resources reserved by PUE [24]
* An upper limit of the number of RSRP threshold increments or the maximum value of increased RSRP threshold can be configured. When the upper limit or the maximum value is reached, UE increases the number of determined set of slots [25]
* Support an adaptive frequency search space based on the channel activity, VRU traffic conditions [30]
* Support sidelink cross-slot scheduling allowing only decoding 2nd and/or 3rd retransmission(s) after a minimum configured time gap [30]

References

1. [RP-202846](http://www.3gpp.org/ftp/tsg_ran/TSG_RAN/TSGR_90e/Docs/RP-202846.zip) WID revision: NR sidelink enhancement LG Electronics
2. [R1-2100141](file:///C%3A%5C3GPP%5CRAN1_Meetings%5CTdocs%5C2021%5CR1-2100141.zip) Power saving mechanism in NR sidelink OPPO
3. [R1-2100205](file:///C%3A%5C3GPP%5CRAN1_Meetings%5CTdocs%5C2021%5CR1-2100205.zip) Sidelink resource allocation to reduce power consumption Huawei, HiSilicon
4. [R1-2100309](file:///C%3A%5C3GPP%5CRAN1_Meetings%5CTdocs%5C2021%5CR1-2100309.zip) Considerations on partial sensing in NR V2X CAICT
5. [R1-2100351](file:///C%3A%5C3GPP%5CRAN1_Meetings%5CTdocs%5C2021%5CR1-2100351.zip) Discussion on resource allocation for power saving CATT, GOHIGH
6. [R1-2100466](file:///C%3A%5C3GPP%5CRAN1_Meetings%5CTdocs%5C2021%5CR1-2100466.zip) Resource allocation for sidelink power saving vivo
7. [R1-2100486](file:///C%3A%5C3GPP%5CRAN1_Meetings%5CTdocs%5C2021%5CR1-2100486.zip) Power consumption reduction for sidelink resource allocation FUTUREWEI
8. [R1-2100492](file:///C%3A%5C3GPP%5CRAN1_Meetings%5CTdocs%5C2021%5CR1-2100492.zip) Discussion on resource allocation for power saving Zhejiang Lab
9. [R1-2100517](file:///C%3A%5C3GPP%5CRAN1_Meetings%5CTdocs%5C2021%5CR1-2100517.zip) Discussion on resource allocation for power saving LG Electronics
10. [R1-2100538](file:///C%3A%5C3GPP%5CRAN1_Meetings%5CTdocs%5C2021%5CR1-2100538.zip) Sidelink resource allocation for power saving Nokia, Nokia Shanghai Bell
11. [R1-2100546](file:///C%3A%5C3GPP%5CRAN1_Meetings%5CTdocs%5C2021%5CR1-2100546.zip) Resource allocation for power saving TCL Communication Ltd.
12. [R1-2100612](file:///C%3A%5C3GPP%5CRAN1_Meetings%5CTdocs%5C2021%5CR1-2100612.zip) Resource allocation for sidelink power saving MediaTek Inc.
13. [R1-2100672](file:///C%3A%5C3GPP%5CRAN1_Meetings%5CTdocs%5C2021%5CR1-2100672.zip) Design of sidelink power saving solutions Intel Corporation
14. [R1-2100687](file:///C%3A%5C3GPP%5CRAN1_Meetings%5CTdocs%5C2021%5CR1-2100687.zip) Resource allocation mechanisms for power saving Ericsson
15. [R1-2100696](file:///C%3A%5C3GPP%5CRAN1_Meetings%5CTdocs%5C2021%5CR1-2100696.zip) Discussion on Sidelink Resource Allocation for Power Saving Panasonic Corporation
16. [R1-2100701](file:///C%3A%5C3GPP%5CRAN1_Meetings%5CTdocs%5C2021%5CR1-2100701.zip) NR Sidelink Resource Allocation for UE Power Saving Fraunhofer HHI, Fraunhofer IIS
17. [R1-2101788](file:///C%3A%5C3GPP%5CRAN1_Meetings%5CTdocs%5C2021%5CR1-2101788.zip) Considerations on partial sensing and DRX in NR V2X Fujitsu
18. [R1-2100766](file:///C%3A%5C3GPP%5CRAN1_Meetings%5CTdocs%5C2021%5CR1-2100766.zip) Sidelink resource allocation for Power saving Lenovo, Motorola Mobility
19. [R1-2100801](file:///C%3A%5C3GPP%5CRAN1_Meetings%5CTdocs%5C2021%5CR1-2100801.zip) Discussion on sidelink resource allocation for power saving Spreadtrum Communications
20. [R1-2100870](file:///C%3A%5C3GPP%5CRAN1_Meetings%5CTdocs%5C2021%5CR1-2100870.zip) Discussion on sidelink resource allocation for power saving Sony
21. [R1-2100924](file:///C%3A%5C3GPP%5CRAN1_Meetings%5CTdocs%5C2021%5CR1-2100924.zip) Discussion on sidelink power saving ZTE, Sanechips
22. [R1-2100946](file:///C%3A%5C3GPP%5CRAN1_Meetings%5CTdocs%5C2021%5CR1-2100946.zip) Discussion on resource allocation for power saving NEC
23. [R1-2100962](file:///C%3A%5C3GPP%5CRAN1_Meetings%5CTdocs%5C2021%5CR1-2100962.zip) Discussion on resource allocation for power saving Hyundai Motors
24. [R1-2100981](file:///C%3A%5C3GPP%5CRAN1_Meetings%5CTdocs%5C2021%5CR1-2100981.zip) Resource allocation for power saving InterDigital, Inc.
25. [R1-2101060](file:///C%3A%5C3GPP%5CRAN1_Meetings%5CTdocs%5C2021%5CR1-2101060.zip) Discussion on resource allocation for power saving CMCC
26. [R1-2101086](file:///C%3A%5C3GPP%5CRAN1_Meetings%5CTdocs%5C2021%5CR1-2101086.zip) Discussion on resource allocation for power saving ETRI
27. [R1-2101097](file:///C%3A%5C3GPP%5CRAN1_Meetings%5CTdocs%5C2021%5CR1-2101097.zip) Discussion on sidelink resource allocation for power saving Xiaomi
28. [R1-2101231](file:///C%3A%5C3GPP%5CRAN1_Meetings%5CTdocs%5C2021%5CR1-2101231.zip) On Resource Allocation for Power Saving Samsung
29. [R1-2101357](file:///C%3A%5C3GPP%5CRAN1_Meetings%5CTdocs%5C2021%5CR1-2101357.zip) Sidelink Resource Allocation for Power Saving Apple
30. [R1-2101400](file:///C%3A%5C3GPP%5CRAN1_Meetings%5CTdocs%5C2021%5CR1-2101400.zip) Discussion on Reduce Power Consumption for Sidelink ROBERT BOSCH GmbH
31. [R1-2101422](file:///C%3A%5C3GPP%5CRAN1_Meetings%5CTdocs%5C2021%5CR1-2101422.zip) On NR Sidelink Resource Allocation for Power Saving Convida Wireless
32. [R1-2101485](file:///C%3A%5C3GPP%5CRAN1_Meetings%5CTdocs%5C2021%5CR1-2101485.zip) Power Savings for Sidelink Qualcomm Incorporated
33. [R1-2101550](file:///C%3A%5C3GPP%5CRAN1_Meetings%5CTdocs%5C2021%5CR1-2101550.zip) Discussion on resource allocation for power saving Sharp
34. [R1-2101572](file:///C%3A%5C3GPP%5CRAN1_Meetings%5CTdocs%5C2021%5CR1-2101572.zip) Discussion on partial sensing and SL DRX impact ASUSTeK
35. [R1-2101630](file:///C%3A%5C3GPP%5CRAN1_Meetings%5CTdocs%5C2021%5CR1-2101630.zip) Discussion on sidelink resource allocation for power saving NTT DOCOMO, INC.
36. [R1-2101663](file:///C%3A%5C3GPP%5CRAN1_Meetings%5CTdocs%5C2021%5CR1-2101663.zip) Resource allocation for power saving with partial sensing in NR sidelink enhancement ITL
37. [R1-2100021](file:///C%3A%5C3GPP%5CRAN1_Meetings%5CTdocs%5C2021%5CR1-2100021.zip) LS to RAN1 on SL DRX design RAN2
38. R1-2101790 Resource allocation for sidelink power saving vivo

Appendix (past meeting outcomes)

## RAN1#103-e (26/Oct – 13/Nov 2020)

**Conclusion**

* SL reception Type A and Type D should be used as the reference for evaluation and designing of SL power saving features in R17.
	+ Type A: UE is not capable of performing reception of any SL signals and channels, FFS with exception of performing PSFCH and S-SSB reception (aim to conclude in RAN1#104-e)
	+ Type D: UE is capable of performing reception of all SL signals and channels defined in R16. It does not preclude UE to perform reception of a subset of SL signals/channels
	+ If there are evaluations with assumptions other than the above reference, the detailed assumptions need to be reported
	+ Note: the types and the associated capability defined here are not intended to be defined as Rel-17 UE features as is.

Agreements**:**

* Partial sensing based RA is supported as a power saving RA scheme
	+ FFS details
* Random resource selection is supported as a power saving RA scheme
	+ FFS any changes or enhancement
	+ FFS on conditions to apply random resource selection

Agreements:

* In R17, a SL Mode 2 Tx resource pool can be (pre-)configured to enable full sensing only, partial sensing only, random resource selection only, or any combination(s) thereof
	+ FFS details, including usage, potential restrictions, whether/how any enhancement or condition is needed for the coexistence of full sensing and power saving RA scheme(s) in a same resource pool, etc.

Agreements:

* Re-evaluation and pre-emption checking are not supported by UEs that do not perform any sensing (i.e. PSCCH reception)
* Re-evaluation and pre-emption checking are supported by UEs that perform sensing
	+ FFS details and any conditions(s) in which re-evaluation and pre-emption can be performed
* FFS whether/how re-evaluation and pre-emption can be supported by UEs performing random resource selection that do perform sensing
* Note: details about sensing in this context, including when it is performed, are not decided yet.

Agreements:

* Further study congestion control based on CBR and CR for power saving RA schemes
	+ Identify necessary changes from R16 CBR/CR (if any), including transmission resource selection and transmission parameters that can be adjusted and applicable to power savings RA schemes
	+ Note: this is not intended to require all UEs to perform sensing for the purpose of CBR measurement