**3GPP TSG RAN WG1 Meeting #104bis-e R1-200xxxx**

**April 12th – April 20th, 2020**

**Agenda item: 7.2.2**

**Source: Moderator (Qualcomm Incorporated)**

**Title: Preparation phase email discussion for NR-U**

**Document for: Discussion and Decision**

# Introduction

The paper summarizes the preparation phase email discussion for contribution submitted to 7.2.2 on NR-U CR.

# Issues identified

## 2.1 Initial access signals and channels

For initial access signals and channels [1], the following issues have been identified, but it can be captured in IA discussion

|  |  |  |
| --- | --- | --- |
| Issue # | Issue summary | # Contributions |
| ~~Init-1~~ | ~~Invalid SSB by SSB positions in burst for FBE~~ | ~~1~~ |
|  |  |  |

FL recommendations

* Captured in IA as well. Discuss it there.

## 2.2 DL signals and channels

For DL signals and channels [2], the following issues have been identified

|  |  |  |
| --- | --- | --- |
| Issue # | Issue summary | # Contributions |
| DL-A1 | Maximum size of switchTriggerToAddModList-r16 and switchTriggerToReleaseList-r16 | 1 |
| DL-B1 | Action when an inapplicable value for HARQ-ACK feedback timing is provided in the DCI scheduling the PDSCH (K1=-1) | 1 |
| DL-B2 | Measurement during SCell activation | 4 |
| DL-B3 | CSI measurement across DL bursts | 1 |
| DL-C1 | Processing time for at least l\_d=5 | 2 |
| DL-D1 | Missing description of PDCCH features for shared spectrum in TS38.300 | 1 |
|  |  |  |
|  |  |  |
|  |  |  |

FL recommendations:

## 2.3 UL signals and channels

For UL signals and channels [3], the following issues have been identified

|  |  |  |
| --- | --- | --- |
| **Issue #** | **Issue summary** | **# Contribution(s)** |
| UL-01 | Clarification on DCI size matching rules for DCI 0\_0 | 1 |
|  |  |  |
|  |  |  |
|  |  |  |

FL recommendations (see further details in [3]): Already discussed multiple times and no consensus to change.

## 2.4 Channel access

For channel access [4], the following issues have been identified

|  |  |  |
| --- | --- | --- |
| Issue # | Issue summary | # Contributions |
| CA-1 | Clarifying the conditions for indicating Type 2 LBT for wideband scheduled PUSCH | 1 |
| CA-2 | China-specific aspects related to CCA time and gaps | 1 |
| CA-3 | Correction to SR reporting due to consistent LBT failure recovery | 1 |
| CA-4 | Clarifications on applicability of Type 2A DL Channel Access | 2 |
| CA-5 | UL contention window adjustment procedures | 1 |
| CA-6 | DL COT Detection in Semi-static Channel Access | 1 |
|  |  |  |
|  |  |  |

FL recommendations:

## 2.5 Initial access procedures

For initial access procedures [5], the following issues have been identified

|  |  |  |
| --- | --- | --- |
| Issue # | Issue summary | # Contributions |
| IA 2-1 | PDSCH rate matching over SSB partially overlapping with idle | 1 |
| IA 3-1 | Terminology clarification for “operation” | 1 |
| IA 3-2 | MsgA PUSCH in FBE idle | 1 |

## 2.6 HARQ enhancements

For HARQ enhancements [6], the following issues have been identified

|  |  |  |
| --- | --- | --- |
| Issue # | Issue summary | # Contributions |
| Type3CB#1 | Type-3 HARQ-ACK codebook size ambiguity | 2 |
| Type3CB#2 | Correction on multiplexing timeline definition for Type-3 HARQ-ACK codebook | 4 |
| Type2CB#3 | Assumption on NFI value for a PDSCH group not received at UE side when the UL DAI indicates a value not equal to 4 for that group | 1 |
|  |  |  |
|  |  |  |

FL recommendations:

* Type2CB#3 discussed before

## 2.7 CG enhancements

For CG enhancements [7], the following issues have been identified

|  |  |  |
| --- | --- | --- |
| Issue # | Issue summary | # Contributions |
| CG-1 | Freq hopping for NR-U CG | 1 |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

FL recommendations:

## 2.8 Wideband operation

On wideband operation enhancements, no issue identified.

# Preparation phase discussion

We have identified many issues and we have limited email thread to discuss them. In the next tables, please provide your view on issues with the following notations

* “Y” if you believe the issue is important and needs email discussion
* “E” if you believe the issue is agreeable but editorial in nature. Potentially we can take all the editorial issues out for a separate fast track email approval.
* Empty if you believe the issue is not necessary to fix or low priority

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Company | DL-A1 | DL-B1 | DL-B2 | DL-B3 | DL-C1 | DL-D1 | UL-01 |
| Ericsson | Y |  | Y |  |  | E |  |
| LG | Y |  | Y | E |  | E |  |
| Samsung | Y |  | Y |  |  |  |  |
| Sharp |  |  | Y |  |  |  |  |
| Nokia, NSB | Y/E |  | Y | E |  | E |  |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Company | CA-1 | CA-2 | CA-3 | CA-4 | CA-5 | CA-6 |
| Ericsson | Yes | **No.**  Longer sensing always possible due to e.g. implementation or regional regulatory | Yes | Yes | -  Agree w FL recommendation | **No.**  CR is not correct. UE can detect DL anywhere in COT. |
| Samsung | Y |  |  | Y |  |  |
| Sharp |  |  | Y | Y |  |  |
| DOCOMO | Y |  | Y | Y |  |  |
| Nokia, NSB | Y |  | Y | Y |  | Y |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Company | IA 2-1 | IA 3-1 | IA 3-2 | Type3CB#1 | Type3CB#2 | Type2CB#3 | CG-1 |
| Ericsson |  |  | E | Yes | Yes | - | - |
| Samsung |  |  | E | Y | E |  |  |
| Sharp | Y |  | Y | Y | E |  |  |
| Nokia, NSB |  |  | Y | Y | Y |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |

Please provide additional company views below

|  |  |
| --- | --- |
| **Company** | **View** |
| Ericsson | Regarding **DL-B1**, we don't think this is a valid scenario. The point of specifying the MAC action times in 38.214 (e.g., activation/deactivation of sp-CSI reporting, SCell activation/deactivation, TCI state activation, etc., etc.) is to that there can be aligned understanding between gNB and UE on exactly when the MAC actions are applied. It is in the gNB's interest to know this precisely, hence it does not make sense that for important PDSCH transmissions carrying such MAC-CEs that the gNB would also choose to indicate NNK1. Rather, the gNB should schedule in a way that it is able to indicate a valid K1. With this understanding, there is no need for a spec change. Moreover, this is quite a large spec change.  Regarding **DL-B3**, we are okay with the (editorial) correction of the typo ('PDDCH' 🡺 'PDCCH'); however, we don't agree with the rest of the TP. We don't agree that the current spec text can be interpreted that there could be a gap between two sets of symbols. According to the current spec text, there is only one set of symbols, and the "instances" (note the plurality) of the p/sp-CSI-RS occur "in a set of symbols" (note the singularity). The spec text then says that if this set of symbols is not all occupied by one or more PDSCHs and/or one or more CSI-RS(s), then the UE is not allowed to average across the instances of the p/sp-CSI-RS resources. Hence, the current spec text is in line with the agreement on which it is based.  Regarding **IA 3-1**, there are many instances of the phrase "for operation with shared spectrum channel access," and it is already clear what this means. It applies to the case when any one or more of the cells on which the UE is configured to transmit/receive is in shared spectrum. We do not need to clarify for every use of this phrase exactly which cell is in shared spectrum.  Regarding **IA 3-2**. We agree that this correction is needed. A similar correction was made some time ago in Section 8.1 for PRACH occasion validation, and the same applies for a PUSCH occasion for 2-step RACH. This should be easy to agree as an editorial correction. |
| LG | For **DL-B3**, there are 3 corrections.   * Clarification of “a set of symbols”: At least Ericsson seems to have a view that “a set of symbols” corresponds to symbols without any gaps in between. However, we understand that “a set of symbols” can be discontinuous. Different understanding between companies should be resolved. * For cross-carrier triggering/scheduling, triggering/scheduling DCI cannot affect P/SP-CSI-RS validation. * Typo: PDDCH 🡪 PDCCH   To deal with above issues, it should be handled by email discussion, but seems to fall into ‘editorial’ category in nature. |
| Samsung | For IA 3-1, we think if a cell either of DL or UL is operated in unlicensed, UE should regard this as operation with shared spectrum. |
| Sharp | Regarding **UL-01**, the issue doesn’t occur since the size of FDRA field in DCI format 0\_0 is determined based on active UL BWP in a case of interlace scheduling.  Regarding **IA 3-1**, the spec. is clear enough. The UE determines whether or not the serving cell is “for operation in a cell with shared spectrum channel access” or not by referring to PCell even when the UE transmits a PRACH in a SCell. However, if companies have different understanding, we are OK to discuss.  Regarding **CA-6**, we understand the intention, however it is too late to change Rel-16 behaviours for forward compatibility. Backward compatibility has to be ensured by Rel-17 if necessary. |
| Nokia, NSB | For **CA-2**, the change seems to imply that the existing equipment (e.g. LAA and Wi-Fi is not compliant anymore. We would like to first study the related regulation to see isf this was really intended. In that respect, a reference to the updated regulation would be useful.  For **CA-6**, we feel that the companies may not have understood the motivation correctly, so let me reiterate it here:   * According to the current specs, a Rel-16 UE may assume that any DL transmission occurs in a gNB initiated FFP/COT, which as such is correct up to Rel-16. * However, we have agreed to introduce UE initiated FFP, and UE-gNB COT sharing in the Rel-17 WI on URLLC enhancements. Once UE-gNB COT sharing is enabled, a Rel-16 UE may erroneously assume that a COT initiated by another UE is a gNB initiated COT. * To avoid this, we propose to limit the gNB FFP detection to the start of the gNB COT only. Note that it is too late to address this in Rel-17 since the Rel-16 UEs will already have a different understanding.   One might rightfully argue that this change is actually triggered by the Rel-17 WI, and should be treated there. However, as described above, the Rel-16 UE will already see the issue, and hence it is preferred to solve this as soon as possible before there are issues in the field. |

# Reference

[1]. R1-20xxxxx, FL summary for initial access signals and channels, Qualcomm

[2]. R1-20xxxxx, FL summary for DL signals and channels, Lenovo

[3]. R1-20xxxxx, FL summary for UL signals and channels, Ericsson

[4]. R1-20xxxxx, FL summary for channel access procedures for NR-U, Nokia

[5]. R1-20xxxxx, FL summary for initial access procedure enhancements, Charter Communications

[6]. R1-20xxxxx, FL summary on NR-U HARQ maintenance, Huawei

[7]. R1-20xxxxx, FL summary for on NRU configured grant enhancement, Vivo

[8]. Reserved