3GPP TSG RAN WG1 #105-e R1-21xxxxx

**e-Meeting, May 10th – 27th, 2021**

**Agenda item: 7.2.12**

**Source: Moderator (China Telecom)**

**Title: [105-e-NR-R16-TxSwitching-01] Summary of email discussion on maintenance of Rel-16 uplink Tx switching**

**Document for: Discussion and Decision**

# Introduction

In [1], maintenance issues are summarized for Rel-16 uplink Tx switching. As per the guidance of Chairman, following issues are identified for email discussion/approval during RAN1 #105 e-meeting:

[105-e-NR-R16-TxSwitching-01] Email discussion/approval regarding issues #1 and #2 as in the summary, till 5/24 – Jianchi (China Telecom)

This contribution is the summary of email discussion/approval on maintenance of Rel-16 uplink Tx switching.

# Email discussion (1st round)

## Issue #1: Correction on RRC parameter “*tdm-PatternConfig-r15*” and “*tdm-PatternConfig-r16*” in TS 38.214

R1-2104731 mentioned that in RAN1#104bis-e meeting, it was agreed to update RRC parameter as below [R1-2104019 (TS38.213, CR0216, Rel-16)]

|  |
| --- |
| RAN1#104bis-e output for power control [R1-2104019 (TS38.213, CR0216, Rel-16)]* *tdm-PatternConfig-r15* is updated to *tdm-PatternConfig*
* *tdm-PatternConfig-r16* is updated to *tdm-PatternConfig2*
 |

However, the above modification/CR approved by NR CA/DC session is only applicable for the power control part of TS 38.213, and not applicable for the UL Tx switching part of TS 38.214. Thus, the same issue still exists for UL Tx switching.

**Proposal:**

* Adopt the following TP to TS 38.214.

|  |
| --- |
| **< unchanged text omitted>**1. 6.1.6.1 Uplink switching for EN-DC

For a UE indicating a capability for uplink switching with *BandCombination-UplinkTxSwitch* for a band combination, and if it is for that band combination configured with a MCG using E-UTRA radio access and with a SCG using NR radio access (EN-DC), if the UE is configured with uplink switching with parameter *uplinkTxSwitching*,- for the UE configured with *switchedUL* by the parameter *uplinkTxSwitchingOption*, when the UE is to transmit in the uplink based on DCI(s) received before $T\_{0}-T\_{offset}$or based on a higher layer configuration(s):- when the UE is to transmit an NR uplink that takes place after an E-UTRA uplink on another uplink carrier then the UE is not expected to transmit for the duration of $N\_{Tx1-Tx2}$ on any of the two carriers.- when the UE is to transmit an E-UTRA uplink that takes place after an NR uplink on another uplink carrier then the UE is not expected to transmit for the duration of $N\_{Tx1-Tx2}$ on any of the two carriers.- the UE is not expected to transmit simultaneously on the NR uplink and the E-UTRA uplink. If the UE is scheduled or configured to transmit any NR uplink transmission overlapping with an E-UTRA uplink transmission, the NR uplink transmission is dropped, - for the UE configured with *uplinkTxSwitchingOption* set to 'dualUL'*,* when the UE is to transmit in the uplink based on DCI(s) received before $T\_{0}-T\_{offset}$or based on a higher layer configuration(s):- when the UE is to transmit an NR two-port uplink that takes place after an E-UTRA uplink on another uplink carrier then the UE is not expected to transmit for the duration of $N\_{Tx1-Tx2}$ on any of the two carriers.- when the UE is to transmit an E-UTRA uplink that takes place after an NR two-port uplink on another uplink carrier then the UE is not expected to transmit for the duration of $N\_{Tx1-Tx2}$ on any of the two carriers.- the UE is not expected to transmit simultaneously a two- port transmission on the NR uplink and the E-UTRA uplink.- in all other cases the UE is expected to transmit normally all uplink transmissions without interruptions.- when the UE is configured with *tdm-PatternConfig~~-r15~~* or by *~~tdm-PatternConfig-r16~~ tdm-PatternConfig2*- for the E-UTRA subframes designated as uplink by the configuration, the UE assumes the operation state in which one-port E-UTRA uplink can be transmitted. - for the E-UTRA subframes other than the ones designated as uplink by the configuration, the UE assumes the operation state in which two-port NR uplink can be transmitted. **< unchanged text omitted>** |

Companies are encouraged to provide views on the above TP.

|  |  |
| --- | --- |
| **Company** | **Comments** |
|  |  |
|  |  |
|  |  |

## Issue #2: Clarification on CA based SRS carrier switching

SRS carrier switching was intensively discussed in RAN1 #104e and RAN1 #104b-e. Companies acknowledged that some clarification is needed, but no consensus has been achieved. R1-2104325, R1-2105925 proposed to further discuss this issue in Rel-16, while R1-2104653 proposed to conclude that the combination of SRS carrier switching and UL Tx switching is not supported in R16 and suggested solving the issues in R17 for the combined feature of SRS carrier switching and UL Tx switching. Based on the views from companies, we have following alternatives:

* Alt 1: Conclude that the combination of SRS carrier switching and UL Tx switching is not supported in R16.
* Alt 2: Further discuss SRS carrier switching and UL Tx switching in Rel-16.
	+ Alt 2-1: focus on clarification on UE behavior of suspension.
	+ Alt 2-2: clarification on both dropping rule and suspension.
* Alt 3: Suspend the discussion until Rel-15 CR on SRS carrier switching has been finalized.

Companies are encouraged to provide views on the above alternatives.

|  |  |
| --- | --- |
| **Company** | **Comments** |
|  |  |
|  |  |
|  |  |
|  |  |

For Alt 2-1: focus on clarification on UE behavior of suspension, R1-2105925 proposed the following TP to TS 38.214.

|  |
| --- |
| **<Unchanged parts are omitted – 38.214>**A UE can be configured with SRS resource(s) on a carrier *c1* with slot formats comprised of DL and UL symbols and not configured for PUSCH/PUCCH transmission. For carrier *c1*, the UE is configured with higher layer parameter *srs-SwitchFromServCellIndex* and *srs-SwitchFromCarrier* the switching from carrier *c2* which is configured for PUSCH/PUCCH transmission. During SRS transmission on carrier *c1* (including any interruption due to uplink or downlink RF retuning time [11, TS 38.133] as defined by higher layer parameters *switchingTimeUL* and *switchingTimeDL* of *SRS-SwitchingTimeNR*), the UE temporarily suspends the uplink transmission on carrier *c2*, and also the uplink transmission on carrier *c3* if the UE is configured with *uplinkTxSwitching-r16* for uplink switching between uplink carrier *c2* and *c3*.**<Unchanged parts are omitted – 38.214>** |

Companies are encouraged to provide views on the above TP.

|  |  |
| --- | --- |
| **Company** | **Comments** |
|  |  |
|  |  |
|  |  |
|  |  |

Alt 2-2: clarification on both dropping rule and suspension, R1-2104325 proposed the following TP to TS 38.214.

|  |
| --- |
| For an aperiodic SRS triggered in DCI format 2\_3 and if the UE is configured with higher layer parameter *srs-TPC-PDCCH-Group* set to 'typeB' without PUSCH/PUCCH transmission, the order of the triggered SRS transmission on the serving cells follow the order of the serving cells with aperiodic SRS triggered in the DCI, and the UE in each serving cell transmits the configured one or two SRS resource set(s) with higher layer parameter *usage* set to 'antennaSwitching' and higher layer parameter *resourceType* in *SRS-ResourceSet* set to 'aperiodic'.A UE can be configured with SRS resource(s) on a carrier *c1* with slot formats comprised of DL and UL symbols and not configured for PUSCH/PUCCH transmission. For carrier *c1*, the UE is configured with higher layer parameter *srs-SwitchFromServCellIndex* and *srs-SwitchFromCarrier* the switching from carrier *c2* which is configured for PUSCH/PUCCH transmission. ~~During SRS transmission on carrier~~ *~~c~~~~1~~* ~~(including any interruption due to uplink or downlink RF retuning time [11, TS 38.133] as defined by higher layer parameters~~ *~~switchingTimeUL~~* ~~and~~ *~~switchingTimeDL~~* ~~of~~ *~~SRS-SwitchingTimeNR~~*~~), the UE temporarily suspends the uplink transmission on carrier~~ *~~c~~~~2.~~*After applying the prioritization/dropping rules in this subclause in case of collision between a transmission of SRS over a carrier *c1* and transmission of a physical signal/channel over a carrier *c2*, during [2-port] SRS transmission on carrier *c1* (including any interruption due to uplink or downlink RF retuning time [11, TS 38.133] as defined by higher layer parameters *switchingTimeUL* and *switchingTimeDL* of *SRS-SwitchingTimeNR*), the UE temporarily suspends the uplink transmission on carrier *c3* if the UE is configured with *uplinkTxSwitching-r16* for uplink switching between uplink carrier *c2* and *c3*.If the UE is not configured for PUSCH/PUCCH transmission on carrier *c1* with slot formats comprised of DL and UL symbols, and if the UE is not capable of simultaneous reception and transmission on carrier *c1*and serving cell *c2*, the UE is not expected to be configured or indicated with SRS resource(s) such that SRS transmission on carrier *c1* (including any interruption due to uplink or downlink RF retuning time [11, TS 38.133] as defined by higher layer parameters *switchingTimeUL* and *switchingTimeDL* of *SRS-SwitchingTimeNR*) would collide with the REs corresponding to the SS/PBCH blocks configured for the UE or the slots belonging to a control resource set indicated by *MIB* or *SIB1* on serving cell *c2*. |

Companies are encouraged to provide views on the above TP.

|  |  |
| --- | --- |
| **Company** | **Comments** |
|  |  |
|  |  |
|  |  |
|  |  |

# References

1. R1-2104858, Summary of Rel-16 uplink Tx switching, Moderator (China Telecom), RAN1#105-e, May 10th – 27th, 2021.
2. R1-2104325, Remaining Issues of Rel-16 UL Tx Switching, ZTE, RAN1#105-e, May 10th – 27th, 2021.
3. R1-2104653, Remaining issues for 1Tx-2Tx switching, Qualcomm Incorporated, RAN1#105-e, May 10th – 27th, 2021.
4. R1-2104731, Text Proposals for Tx Switching between Two Uplink Carriers, OPPO, RAN1#105-e, May 10th – 27th, 2021.
5. R1-2105925, Discussion on the remaining problems of supporting Tx switching between two uplink carriers, Huawei, HiSilicon, RAN1#105-e, May 10th – 27th, 2021.