**3GPP TSG RAN WG1 #105-e R1-210xxxx**

**e-Meeting, May 10 – 27, 2021**

**Agenda Item: 8.11**

**Source: Moderator (ZTE)**

**Title: Moderator summary of Email Discussion/approval to rely LS in R1-2100021**

**Document for: Discussion and Decision**

# Introduction

The reply LS to R1-2100021 was discussed during two previous RAN1 meetings. Given the reply is closely related to whether UE is allowed to perform sensing operations including PSCCH monitoring and RSRP measurement during SL DRX inactive time, this document will try to collect companies' views on this topic. Discussion on this topic captured in [2] during RAN1#104b-e is used as a starting point to facilitate smooth progress.

# Discussions

## Round 1 discussion

It's moderator's understanding that the scope of this discussion is limited to the topic whether UE is allowed to perform PSCCH monitoring and RSRP measurement during SL DRX inactive time, while the details should be up to the progress of RAN2 discussion on DRX configuration and RAN1 discussion on 8.11.1.1 resource allocation for power saving if the majority is UE is allowed to perform such operations. Under this consideration, we would like to ask for companies' views on their preference over the following three alternatives on the proposed possible agreement. Alt 1 and Alt 2 were raised as FL proposal from 8.11.1.1 to this topic. Alt 3 is consolidated based on a contribution submitted to this meeting under AI 5 on this topic.

* Alt 1 A UE can perform SL reception of PSCCH and RSRP measurement for sensing during its SL DRX inactive time. FFS details
* Alt 2 It is up to UE implementation to perform SL reception of PSCCH and RSRP measurement for sensing during its SL DRX inactive time.
* Alt 3 A UE is not required to perform sensing out of the DRX active time

|  |  |
| --- | --- |
| Company | View |
| ZTE, Sanechips | Alt 1. Based on RAN2’s progress, we can get the following observations on SL DRX:1. The granularity of SL DRX operation could be per a pair of source/destination, or per cast type, or per L2 destination ID.
2. The SL DRX configurations can be obtained from pre-configuration ,SIB ,dedicated-RRC or PC5-RRC.
3. For one UE, more than one SL DRX configurations would be configured.
4. For unicast, the SL DRX for both Tx UE and RX UE can be acquired by one UE.

In case the sensing window or the slots which are expected to be sensed in sensing window (for partial sensing), overlaps the off-duration of SL DRX, the UE is not expected to perform sensing on those slots during the off-duration of SL DRX. This could lead to performance degradation and impact on sensing procedure.Apart from the concerns of performance/sensing procedure, the following issues should be considered too.Issue 1: Based on observation 1, which granularity of SL DRX should be applied in current partial sensing?Issue 2: Based on observation 4, in unicast, whether SL DRX of Tx UE or RX UE should be applied? Which UE is the target RX UE for the current partial sensing?Issue 3: Based on observation 2, in groupcast/broadcast, for an OoC UE, if its pre-configured SL DRX is applied to sensing, is it feasible for a target RX UE which is in coverage?Issue 4: Based on observation 3, if more than one SL DRX configurations are configured, one or all of configured SL DRX should be applied for partial sensing?In addition, according to Rel-16 sensing procedure, PHY doesn’t know the sensed resources would be used for which HARQ process, which destination ID, which cast-type, HARQ enable/disable, etc. And for V2X, safety is the first priority, the sensing reliability and collision detection are the key points for sensing. Power saving can be mostly obtained by setting sensing parameters reasonably. Thus it's sensible that UE can perform SL reception of PSCCH and RSRP measurement for sensing during its SL DRX inactive time. |

Outcome of round 1 discussion

From the email replies received from HW/HiSilicon, Ericsson, Samsung, DoCoMo, vivo, Futurewei, Qualcomm, the following categorization received support from 3 companies(HW/HiSilicon, DoCoMo, Futurewei)

   Alt 1 A UE can perform SL reception of PSCCH and RSRP measurement for sensing during its SL DRX inactive time.

1. FFS: Whether when such reception is performed is subject to specification, or is up to UE implementation

2. FFS: Other details

 Alt 2 A UE cannot perform sensing out of the DRX active time

The following categorization received support from 2 companies (vivo/Qualcomm)

-       Option 1: UE shall perform sensing during its SL DRX inactivity time.

-       Option 2: UE should~~can~~perform sensing during its SL DRX inactivity time, based on specified rule(s). FFS the rule(s).

-       Option 3: It is up to UE whether to perform sensing during its SL DRX inactivity time.

-       Option 4: UE does not perform sensing during its SL DRX inactivity time.

The following categorization received support from 2 companies (DoCoMo/Qualcomm)

-       Option 1: UE shall perform sensing during its SL DRX inactive time.

-       Option 2: UE can perform sensing during its SL DRX inactive time, based on a rule. FFS what is the rule.

-       Option 3: UE can perform sensing during its SL DRX inactive time, but up to UE implementation.

-       Option 4: UE does not perform sensing during its SL DRX inactive time.

One company (Futurewei) prefer some additional change to option 2 as following as starting point

Option 2: UE can perform sensing during its SL DRX inactive time, based on specified rules and configurations. FFS  the rules and configurations.

The first categorization with modification by vivo is adopted as the additional question asked to collect companies’ views after they provided answer to the preference of the alternatives proposed by HW/HiSilicon because:

The modification has better distinction between UE implementation and specification work by replacing the wording ‘can’.

Companies’ are kindly invited to provide answers to the following questions, we will see whether we can agree to any alternative, or future progress on given option under an alternative with companies’ feedback.

## Round 2 discussion

Question 1: Out of the two alternatives, which one do you prefer as the direction for agreement to the topic.

   Alt 1 A UE can perform SL reception of PSCCH and RSRP measurement for sensing during its SL DRX inactive time.

1. FFS: Whether when such reception is performed is subject to specification, or is up to UE implementation

2. FFS: Other details

 Alt 2 A UE cannot perform sensing out of the DRX active time

|  |  |
| --- | --- |
| Company | View |
| Samsung | We support Alt 2 in order to achieve the power saving by prohibiting sensing (SL reception of PSCCH and RSRP measurement) during the SL DRX inactive time. Like Alt 1, additional UE behavior should be discussed for Alt 2. For example, for UE with SL DRX, sensing window can be adjusted into DRX active time within configured sensing window and if the sensing window is not available, UE can perform random selection without sensing. So, we suggest to add “FFS other details” also for Alt 2.  |
| OPPO | Support Alt 1.In our view, if sensing cannot performed out of DRX active time, there will be the following issues:* + Issue 1: The sensing results is not accurate since in some cases the most recent sensing occasion is within inactive time

The most recent sensing occasion carries the more accurate sensing results. That is why when we discussing partial sensing, at least k=1 should be monitored. If the period corresponding to k=1 is not monitored, that will degrade PRR performance.* + Issue 2: Re-evaluation/pre-emption is not applicable in case the resource selection window (which is determined by the packet arriving time of TX UE) is within TX UE’s inactive time.

Re-evaluation and pre-emption is important feature introduced in R16 to avoid collision with aperiodic traffic. It is more important in R17 considering mix RA including random resource selection. If sensing cannot be performed out of active time which result in re-evaluation/pre-emption cannot be performed either, the collision with aperiodic traffic, especially the UE with RS, is hardly to be avoided which will degrade the PRR performance greatly.  |
| CATT, GOHIGH | We support Alt 1.In RAN2 #113-e meeting, the following agreement was achieved on SL DRX:*“4: For data reception, RAN2 defines the behaviour for monitoring the SCI reception (i.e., PSCCH and 2nd SCI on PSSCH) during the SL active time for SL DRX. For data reception, the UE may skip monitoring of PSCCH and 2nd SCI on PSSCH during inactive time for SL DRX. Sensing aspect is not considered in this agreement.”*It is clear that RAN2 defines SL DRX active time as the duration during which the UE performs SCI reception (i.e., PSCCH and 2nd SCI on PSSCH) for the purpose of data reception. Since DRX is entirely a receive behavior, it should not be confused with sensing (PSCCH reception and SL-RSRP measurement) which is a transmission behavior.From RAN1’s perspective, if Tx UE is restricted to performing sensing only during its DRX active time, sensing performance cannot be guaranteed. Tx UE should either give up the sensing occasions which fall into the DRX inactive time or configure the DRX active time to include all the sensing occasions. However, the former may cause a loss of resource selection performance due to insufficient sensing results, while the latter is difficult to implement and may prolong the DRX active time, leading to increased power consumption.Thus, in order to achieve a trade-off between PRR performance and power consumption, sensing operation should be allowed in SL DRX inactive time without the restriction of UE’s own SL DRX configuration, i.e. Alt 1 is a more reasonable alternative. |

Question 2: If your answer to the first question is alternative 1, please indicate which option from option 1 – 3 is your preference, please indicate any other detail you would like to share. If your preference to the first question is alternative 2, please indicate whether option 4 is your preference and any other detail you would like to share.

|  |  |
| --- | --- |
| Company | View |
| Samsung | For Option 4, we need to discuss about detailed UE behavior. Please see our comment in Q1 above. |
| OPPO | The LS from RAN2 just ask whether RAN1 has concern on the following WA. The selection between Alt1 or Alt 2 in Q1 is enough to answer to the LS from RAN2. The details for the sensing, corresponding to option 1-3, is not related to the LS and can be discussed later in RAN1. Working assumption: SL DRX should take PSCCH monitoring also for sensing (in addition to data reception) into account if SL DRX is used. |
| CATT, GOHIGH | We support option 1 with following modification:Option 1: UE shall perform sensing in every sensing occasion during its SL DRX inactivity time.As our comments in Q1, DRX is entirely a receive behavior and should not have direct impact on sensing. That is to say, once the sensing occasion is determined by the sensing and resource selection procedure, UE shall perform sensing in every sensing occasion, whether during its DRX active time or inactive time.The above-mentioned behavior should not be up to UE implementation and no more specified rule(s) is(are) needed. Thus, we do not support option 2 and option 3. |

# Conclusion

TBD

# References

1. Chair's Notes RAN1#104b-e v012
2. R1-2104093, FL summary for AI 8.11.1.1 – resource allocation for power saving (final), Moderator(OPPO)