**3GPP TSG RAN WG1 #106-e R1-21abcde**

**e-Meeting, August 16th – August 27th, 2021**

**Agenda item:** 7.1

**Source:** Moderator **(**Qualcomm Incorporated)

**Title:** Summary of [106-e-NR-7.1CRs-08]

**Document for:** Discussion/Decision

# Introduction

In Rel-15 Type II CSI, a precoding matrix on a subband is obtained as linear combination of 2L spatial beams. Each linear combination coefficients are quantized by wideband amplitude (i.e., ), subband amplitude (i.e., ) and subband phase (i.e., ). The wideband amplitudes are reported following the order of beam index, while the reporting order of subband amplitude/phase is unclear in current spec. In this contribution, we discuss possible understandings of the reporting order and propose potential text change.

# Discussion (Round 1)

In Rel-15 Type II CSI, a precoding matrix on a subband is obtained as linear combination of 2L spatial beams. Each linear combination coefficients are quantized by wideband amplitude (i.e., ), subband amplitude (i.e., ) and subband phase (i.e., ). For wideband amplitude, though not explicitly written in the spec, it seems that the only possible reporting order is following the beam indices. That is, the elements of are applied to the 1st, 2nd, …, the (2L-1)-th beam, respectively, where the beam indices are in increasing order. However, for subband amplitude and subband phase, there are two possible understandings.

* Alt1: the elements of and are mapped following the same order as (i.e., based on beam indices).
* Alt2: the elements of and are mapped based on the beam strength, i.e., the value reported in wideband amplitude indicator .

Detailed analysis can be found in R1-2107314**.**

**Companies please provide views on coefficient mapping order, either Alt1 or Alt2.**

|  |  |
| --- | --- |
| Company | Comments |
| Qualcomm | Slightly prefer Alt1, can go with majority view.  |
|  |  |

# Text proposal (round 2, to be decided after round 1)

**In R1-2107314, following text proposal is provided for Alt1 and Alt2.**

**Following spec change is proposed if following beam index:**

### 5.2.3 CSI reporting on PUSCH

>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>> unchanged text omitted <<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<

For Type I and Type II CSI feedback on PUSCH, a CSI report comprises of two parts. Part 1 has a fixed payload size and is used to identify the number of information bits in Part 2. Part 1 shall be transmitted in its entirety before Part 2.

- For Type I CSI feedback, Part 1 contains RI (if reported), CRI (if reported), CQI for the first codeword (if reported). Part 2 contains PMI (if reported) and contains the CQI for the second codeword (if reported) when RI (if reported) is larger than 4.

- For Type II CSI feedback, Part 1 contains RI (if reported), CQI, and an indication of the number of non-zero wideband amplitude coefficients per layer for the Type II CSI (see clause 5.2.2). The fields of Part 1 – RI (if reported), CQI, and the indication of the number of non-zero wideband amplitude coefficients for each layer – are separately encoded. Part 2 contains the PMI of the Type II CSI. The elements of , and are reported in the increasing order of their indices, where the lowest index is mapped to the most significant bits and the last index to be reported is mapped to the least significant bits. Part 1 and 2 are separately encoded.

>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>> unchanged text omitted <<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<

**Following spec change is proposed if following beam strength reported in wideband amplitude:**

### 5.2.3 CSI reporting on PUSCH

>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>> unchanged text omitted <<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<

For Type I and Type II CSI feedback on PUSCH, a CSI report comprises of two parts. Part 1 has a fixed payload size and is used to identify the number of information bits in Part 2. Part 1 shall be transmitted in its entirety before Part 2.

- For Type I CSI feedback, Part 1 contains RI (if reported), CRI (if reported), CQI for the first codeword (if reported). Part 2 contains PMI (if reported) and contains the CQI for the second codeword (if reported) when RI (if reported) is larger than 4.

- For Type II CSI feedback, Part 1 contains RI (if reported), CQI, and an indication of the number of non-zero wideband amplitude coefficients per layer for the Type II CSI (see clause 5.2.2). The fields of Part 1 – RI (if reported), CQI, and the indication of the number of non-zero wideband amplitude coefficients for each layer – are separately encoded. Part 2 contains the PMI of the Type II CSI. The elements of and are reported in the decreasing order of their wideband amplitude reported in , where the element with strongest wideband amplitude is mapped to the most significant bits and the element with weakest wideband ampltidue to be reported is mapped to the least significant bits. Part 1 and 2 are separately encoded.

>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>> unchanged text omitted <<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<

**Companies please provide comments on the proposed spec change**

|  |  |
| --- | --- |
| Company | Comments |
|  |  |
|  |  |

# Conclusion

TBD